**3GPP TSG-RAN WG2 Meeting #123bis *R2-231xxxx***

**Xiamen, China, October 9th – 13th, 2023**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.331** | **CR** | **DraftCR** | **rev** | **-** | **Current version:** | **17.6.0** |  |
|  | | | | | | | | |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | RRC running CR for subsequent CPAC in NR-DC | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | OPPO | | | | | | | | | |
| ***Source to TSG:*** | R2 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_Mob\_enh2-Core | | | | |  | ***Date:*** | | | 2023-10-17 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | This CR is to introduce the functionality of subsequent CPAC in NR-DC.  The related agreements:  **RAN2#119 meeting**   * The selective activation of cell groups should correspond to support of subsequent conditional changes (CPC) after a cell group change (normal or conditional). CPA FFS. * Initial focus on SCG * There is interest to support delta configuration, to reduce the signalling overhead (FFS if some other objective should be achieved) * FFS how many subsequent conditional changes are targeted (and what is the impact of such assumption). * FFS whether there is a security issue: e.g. to determine vertical or horizontal key derivation, e.g. security parameters re-used as part of subsequent CG switch (for the case when UE goes back to a previous cell, maybe in another SN), and FFS on the procedure/method with which the UE derives the SN security, e.g. based on a prior MN config (without RRC CPC config at the time of SN switch).   **RAN2#119bis**   * Baseline procedure to support subsequent secondary cell group change (FFS if UE keeps all configurations or if those are indicated by the network, FFS support of nested configs): * a. Step 1: when the execution condition of a CPC candidate PScell is met, a UE performs the execution of CPC towards this candidate PScell. * b. Step 2: After finishing the PSCell addition or change, the UE doesn’t release conditional configuration of other candidate PSCells for subsequent CPC, the UE continues evaluating the execution conditions of other candidate PScells. * c. Step 3: When the execution condition of a candidate PScell is met, the UE performs the execution of CPC towards this candidate PSCell. * Confirm that “CPA” selective activation of cell groups will be supported for this WI objective * Confirm that we aim to support delta configuration, i.e. that there need to be a known reference. * RAN2 aim to support selective activation of cell groups without RRC reconfiguration with respect to security (FFS, need to consult with SA3 at some point in time).   **RAN2#120**  Delta configuration   * A UE stores the reference configuration as a separate configuration. * The reference configuration is managed separately   **RAN2#121**   * Assume to support the following scenarios of SCG selective activation:   -SN initiated intra-SN SCG selective activation  -MN initiated inter-SN SCG selective activation  -SN initiated inter-SN SCG selective activation   * It is assumed that if the UE need to be able to return to a current SCG by conditional procedure, then the network could explicitly configure a candidate configuration for that cell. * In SCG selective activation, the CPC/CPA configurations of the UE should be released after Pcell change, at least for inter MN (by explicit indication from network, FFS other case). * R2 assumes that a CPA conditional configuration can be used for CPC (but with different triggering conditions) * For inter-SN CPC, MN should provide the reference configuration to all candidate T-SNs (in order to generate the T-SN candidate configuration). * R2 understands that A target SN may include an indication in SN Addition Request Ack for each candidate target PSCell, denoting whether the associated SCG configuration is a delta with respect to the reference SCG configuration.   **RAN2#121bis**   * For the reference configuration for SCG Selective Activation, aim at following similar design as LTM. * For inter-SN SCG Selective Activation, the RRC reconfiguration message containing the Rel-18 CPC configurations provided to the UE is in MN format. * For MN initiated inter-SN SCG selective activation, source MN generates the execution conditions for the initial CPAC. * FFS on the following options for subsequent CPC: * Option 1: Source MN generates the execution conditions for all subsequent CPC. * Option 2: Candidate SN may generate execution conditions for subsequent CPC. * For SN initiated inter-SN SCG selective activation, source SN generates the execution conditions for the initial CPC. * FFS if Candidate SN may generate/modify execution conditions for subsequent CPC * Assume for now that there is only one reference configuration. * The following may be included in the initial RRC reconfiguration message containing the Rel-18 CPC configurations: * Reference SCG configuration (Optionality FFS). Assume as for LTM Reference configuration may be empty. * FFS whether MCG configuration is included. * FFS RRC model for the reference configuration. * Initial List of candidate target PSCells (this list can be updated by the network, e.g., cells may be added or removed) with associated target SCG configurations. FFS whether the MCG configurations associated with the target SCG configurations are included. * 3. The execution conditions associated with each candidate target PSCell. * a. For MN initiated procedure, execution conditions based on event A4 are supported. FFS whether A3/A5 are supported. * b. For SN initiated procedure, execution conditions based on events A3/A5 are supported. * UE will keep R18 CPC configurations after CPC execution. It should be possible to release a CPC candidate explicitly by RRC reconfiguration procedure.   **RAN2#122**   * For SN-initiated SCG selective activation, candidate SN generates execution conditions for subsequent CPC. * FFS if it shall be possible to do something like MN-initiated CPA/CPC where Candidate SN generate execution conditions for subsequent CPC * The UE shall skip the condition evaluation for a candidate which is a current PScell. * The reference configuration is provided to all candidates involved in preparation, FFS which node initially generates it. Assume it can be provided in MN initiated and in SN initiated procedures. * Will not spend specific efforts for supporting nested configurations for candidate cell configuration. * Rapporteur take initiative on naming offline * Terminology is “Subsequent CPAC”   **RAN2#123**   * For subsequent CPAC it is useful to support use of A3 A5 * A3 A5 is supported with SN-initiated subsequent CPAC * Proposal 1: For MN-initiated subsequent CPAC, MN initially triggers the candidate cell preparation of subsequent CPAC procedure, i.e. MN triggers the procedure as defined in Section 10.5.2 and Section 10.2.2 of TS 37.340 in the endorsed running CR. * Proposal 2: For SN-initiated inter-SN subsequent CPAC, SN initially triggers the candidate cell preparation of subsequent CPAC procedure, i.e. source SN triggers the procedure as defined in Section 10.5.2 of TS 37.340 in the endorsed running CR. * Proposal 3 (option2): For MN-initiated subsequent CPAC, the execution condition configuration is provided as following: * MN generates the execution conditions (A4 event) for initial CPAC execution, and the measID refers to the measurement configuration associated with MCG; * candidate SN generates the execution conditions (A3/A5 event) for subsequent CPC execution, and the measID refers to the measurement configuration associated with SCG. * UE autonomously releases the subsequent CPAC configurations in the following cases: upon RRC re-establishment and RRC release (to RRC\_IDLE and/or RRC\_INACTIVE) * No need for an optimized single-indication-release of CPAC configuration. Can rely on explicit release for other cases. * Will support the SA3 solution, i.e. update of Sk-counter at inter-SN-mobility, based on pre-configured multiple Sk-counter. UE need to know when Sk counter need to change.   **RAN2#123bis**   * P1a: Upon SCG release, RAN2 confirms that the UE shall release the subsequent CPAC configuration within SCG VarConditionalReconfig autonomously. * P1b: Upon SCG release, it’s up to the NW decision to maintain or release the subsequent CPAC configuration within MCG VarConditionalReconfig. * P2: Upon intra-MN PCell change, it’s up to the NW decision to maintain/modify/release the subsequent CPAC configuration. * P3: If there are maintained subsequent CPAC configurations with CPA execution conditions after SCG release, the maintained configurations can be used for the subsequent CPA execution. * P4: The coexistence of subsequent CPAC and SCG deactivation is not supported in Rel-18, i.e. follow the same principle as legacy CPAC. * P5: The candidate and reference configuration for subsequent CPAC can include both MCG and SCG part configurations. It can be up to the NW implementation whether to include the MCG part. * P6: The MN generates the MCG part of the reference configuration (if any), while the SN (source or candidate) generates the SCG part of the reference configuration. * P8: The MN is responsible for the reference configuration generation for MN/SN initiated inter-SN SCPAC. * P10: The MN can request an SCG reference configuration from any of the involved SNs. * P11: Candidate SN prepares the execution conditions for subsequent CPC when the candidate SN prepares the candidate SCG configuration(s) for candidate PSCell(s). * P12: For SN initiated inter-SN subsequent CPAC, in SN Change Required message, the source SN includes the following information to the MN: * - A list of candidate SNs (can also include source SN) for the initial and subsequent CPC, and for each candidate SN in the list, a list of PSCells suggested to be prepared by the candidate SN. * - Execution conditions associated with each suggested PSCell of the initial CPC. * P14: In SN Addition Request Acknowledge message, the candidate SN includes the following information to the MN: * 1) List of prepared candidate PSCells and associated candidate SCG configurations, which include the candidate SCG measurement configurations, i.e. as legacy; * 2) For each cell in 1), a list of proposed candidate PSCells for the subsequent CPC (e.g., the neighbour PSCells), and associated execution conditions (events A3/A5, based on the candidate SCG measurement configurations). * Note: The proposed candidate PSCells are selected from the recommended cell list provided by the MN, as the legacy. * P15: The MN checks whether the proposed candidate PSCells for subsequent CPC have been prepared by other candidate SNs, and the MN may initiate an SN Modification procedure to the candidate SN, e.g. when not all proposed candidate PSCells for subsequent CPC have been prepared. * P16a: In SN Modification Request message, the MN includes the following information to the candidate SN: * Candidate PSCells for subsequent CPC that have been prepared by other candidate SNs. * P16b: In SN Modification Request Acknowledge message, the candidate SN includes the following information to the MN: * Updated candidate SCG configurations and/or the execution conditions for subsequent CPC, if needed. The detailed signaling is similar to that in SN Addition Request Acknowledge message. * P17: RAN2 assumes that the coexistence of subsequent CPAC and legacy CPAC is supported. [Check with RAN3] * P18: RAN2 assumes that the existing signalling flow charts and procedural texts for Rel-17 CPA/CPC procedures can be reused for subsequent CPAC procedure with some modifications. [Check with RAN3] * For one UE, for CPC only either MN format or SN format (only intra-SN case is possible) is used * MN format is supported for intra-SN (in addition to SN format) * P13a: For MN initiated inter-SN subsequent CPAC, in SN Addition Request message, the MN includes the following information to each candidate SN: * A list of candidate SNs, and for each candidate SN in the list, a list of cells recommended by MN (assume format as legacy) * P13b: For SN initiated inter-SN subsequent CPAC, in SN Addition Request message, the MN includes the following information to each candidate SN: * A list of candidate SNs, and for each candidate SN in the list, a list of PSCells suggested to be prepared by the candidate SN. * Rel-18 Conditional-Reconfiguration Information element may include * - List of Group-ID (mapping to SN) and associated SK-counter values outside the candidate conditional configurations. * - The Group-ID parameter is included within each candidate conditional configuration(CondConfigAddMod) marked for subsequent CPAC. * Mod P3: UE include the selected SK-counter value in the MN RRC Reconfiguration Complete message when UE selects new SK-counter value as part of S-CPAC execution. * Mod P4: For Pcell-change /PSCell-change /SCG Release scenarios, if the SCPAC configuration is maintained, UE also maintains the unused SK-counter values. * RAN2 Understanding: The NW configuration ensures that The SK-counter lists assigned for SCPAC configurations and the SK-counter value assigned for CPAC configurations are uniquely different. No specification changes are needed in this regard. * No specification changes needed for UE behaviour for the Scenario where free SK-Counter not available at the time of execution. This scenario can be avoided by NW configuration. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Necessary procedures and ASN.1 changes in order to support the subsequent CPAC feature in NR are introduced. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | If the CR is not approved the subsequent CPAC in NR-DC feature will not be supported in NR. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.3.5, 5.3.7, 5.3.8.3, 5.3.11, 5.5.3, 6.2.2, 6.3.2, 6.4, 7.4, 11.2.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | R2-2309336 | | | | | | | | |

*START OF CHANGES*

## 3.2 Abbreviations

For the purposes of the present document, the abbreviations given in TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in TR 21.905 [1].

5GC 5G Core Network

ACK Acknowledgement

AM Acknowledged Mode

ARQ Automatic Repeat Request

AS Access Stratum

ASN.1 Abstract Syntax Notation One

BAP Backhaul Adaptation Protocol

BCD Binary Coded Decimal

BFD Beam Failure Detection

BH Backhaul

BLER Block Error Rate

BWP Bandwidth Part

CA Carrier Aggregation

CAG Closed Access Group

CAG-ID Closed Access Group Identifier

CAPC Channel Access Priority Class

CBR Channel Busy Ratio

CCCH Common Control Channel

CFR Common Frequency Resources

CG Cell Group

CHO Conditional Handover

CLI Cross Link Interference

CMAS Commercial Mobile Alert Service

CP Control Plane

CPA Conditional PSCell Addition

CPC Conditional PSCell Change

CPAC Conditional PSCell Addition or Change

C-RNTI Cell RNTI

CSI Channel State Information

DAPS Dual Active Protocol Stack

DC Dual Connectivity

DCCH Dedicated Control Channel

DCI Downlink Control Information

DCP DCI with CRC scrambled by PS-RNTI

DFN Direct Frame Number

DL Downlink

DL-PRS Downlink Positioning Reference Signal

DL-SCH Downlink Shared Channel

DM-RS Demodulation Reference Signal

DRB (user) Data Radio Bearer

DRX Discontinuous Reception

DTCH Dedicated Traffic Channel

ECEF Earth-Centered, Earth-Fixed

ECI Earth-Centered Inertial

EN-DC E-UTRA NR Dual Connectivity with E-UTRA connected to EPC

EPC Evolved Packet Core

EPS Evolved Packet System

ETWS Earthquake and Tsunami Warning System

E-UTRA Evolved Universal Terrestrial Radio Access

E-UTRA/5GC E-UTRA connected to 5GC

E-UTRA/EPC E-UTRA connected to EPC

E-UTRAN Evolved Universal Terrestrial Radio Access Network

FDD Frequency Division Duplex

FFS For Further Study

G-CS-RNTI Group Configured Scheduling RNTI

GERAN GSM/EDGE Radio Access Network

GIN Group ID for Network selection

GNSS Global Navigation Satellite System

G-RNTI Group RNTI

GSM Global System for Mobile Communications

HARQ Hybrid Automatic Repeat Request

HRNN Human Readable Network Name

HSDN High Speed Dedicated Network

H-SFN Hyper SFN

IAB Integrated Access and Backhaul

IAB-DU IAB-node DU

IAB-MT IAB Mobile Termination

IDC In-Device Coexistence

IE Information element

IMSI International Mobile Subscriber Identity

kB Kilobyte (1000 bytes)

L1 Layer 1

L2 Layer 2

L3 Layer 3

LBT Listen Before Talk

LEO Low Earth Orbit

MAC Medium Access Control

MBS Multicast/Broadcast Service

MBS FSAI MBS Frequency Selection Area Identity

MCCH MBS Control Channel

MCG Master Cell Group

MDT Minimization of Drive Tests

MIB Master Information Block

MPE Maximum Permissible Exposure

MRB MBS Radio Bearer

MR-DC Multi-Radio Dual Connectivity

MTCH MBS Traffic Channel

MTSI Multimedia Telephony Service for IMS

MUSIM Multi-Universal Subscriber Identity Module

N/A Not Applicable

NE-DC NR E-UTRA Dual Connectivity

(NG)EN-DC E-UTRA NR Dual Connectivity (covering E-UTRA connected to EPC or 5GC)

NGEN-DC E-UTRA NR Dual Connectivity with E-UTRA connected to 5GC

NID Network Identifier

NPN Non-Public Network

NR-DC NR-NR Dual Connectivity

NR/5GC NR connected to 5GC

NSAG Network Slice AS Group

NTN Non-Terrestrial Network

PCell Primary Cell

PDCP Packet Data Convergence Protocol

PDU Protocol Data Unit

PEI Paging Early Indication

PEI-O Paging Early Indication-Occasion

PLMN Public Land Mobile Network

PNI-NPN Public Network Integrated Non-Public Network

posSIB Positioning SIB

PPW PRS Processing Window

PRS Positioning Reference Signal

PSCell Primary SCG Cell

PTM Point to Multipoint

PTP Point to Point

PWS Public Warning System

QoE Quality of Experience

QoS Quality of Service

RAN Radio Access Network

RAT Radio Access Technology

RLC Radio Link Control

RLM Radio Link Monitoring

RMTC RSSI Measurement Timing Configuration

RNA RAN-based Notification Area

RNTI Radio Network Temporary Identifier

ROHC Robust Header Compression

RPLMN Registered Public Land Mobile Network

RRC Radio Resource Control

RS Reference Signal

SBAS Satellite Based Augmentation System

SCell Secondary Cell

SCG Secondary Cell Group

SCS Subcarrier Spacing

SD-RSRP Sidelink Discovery RSRP

SDT Small Data Transmission

SFN System Frame Number

SFTD SFN and Frame Timing Difference

SI System Information

SIB System Information Block

SL Sidelink

SLSS Sidelink Synchronisation Signal

SNPN Stand-alone Non-Public Network

SpCell Special Cell

SRAP Sidelink Relay Adaptation Protocol

SRB Signalling Radio Bearer

SRS Sounding Reference Signal

SSB Synchronization Signal Block

TAG Timing Advance Group

TDD Time Division Duplex

TEG Timing Error Group

TM Transparent Mode

TMGI Temporary Mobile Group Identity

U2N UE-to-Network

UDC Uplink Data Compression

UE User Equipment

UL Uplink

UM Unacknowledged Mode

UP User Plane

VR Virtual Reality

In the ASN.1, lower case may be used for some (parts) of the above abbreviations e.g. c-RNTI.

### 5.3.5 RRC reconfiguration

#### 5.3.5.3 Reception of an *RRCReconfiguration* by the UE

The UE shall perform the following actions upon reception of the *RRCReconfiguration,* or upon execution of the conditional reconfiguration (CHO, CPA or CPC):

1> if the *RRCReconfiguration* is applied due to a conditional reconfiguration execution upon cell selection performed while timer T311 was running, as defined in 5.3.7.3:

2> remove all the entries within the MCG and the SCG *VarConditionalReconfig*, if any;

1> if the *RRCReconfiguration* is applied due to a conditional reconfiguration execution in accordance with 5.3.5.13.5 and the *subsequentCondReconfig* and the *securityCellSetID* are included in the entry in *VarConditionalReconfig* containing the *RRCReconfiguration* message:

2> if the value of *SecurityCellSetID* associated with the selected cell is not equal to the value of *servingSecurityCellSetID* within *VarServingSecurityCellSetID*:

3> consider the first unused *SK-Counter* value in the *SK-CounterList* associated with the *SecurityCellSetID* within the *VarConditionalReconfig* as the selected *SK-Counter* value, and perform security key update procedure as specified in 5.3.5.7;

3> replace the value of *servingSecurityCellSetID* within *VarServingSecurityCellSetID* with the value of *SecurityCellSetID* associated with the selected cell;

*Editor note: whether to remove the slelcted SK-Counter upon security update.*

1> if the *RRCReconfiguration* includes the *daps-SourceRelease*:

2> reset the source MAC and release the source MAC configuration;

2> for each DAPS bearer:

3> release the RLC entity or entities as specified in TS 38.322 [4], clause 5.1.3, and the associated logical channel for the source SpCell;

3> reconfigure the PDCP entity to release DAPS as specified in TS 38.323 [5];

2> for each SRB:

3> release the PDCP entity for the source SpCell;

3> release the RLC entity as specified in TS 38.322 [4], clause 5.1.3, and the associated logical channel for the source SpCell;

2> release the physical channel configuration for the source SpCell;

2> discard the keys used in the source SpCell (the KgNB key, the KRRCenc key, the KRRCint key, the KUPint key and the KUPenc key), if any;

1> if the *RRCReconfiguration* is received via other RAT (i.e., inter-RAT handover to NR):

2> if the *RRCReconfiguration* does not include the *fullConfig* and the UE is connected to 5GC (i.e., delta signalling during intra 5GC handover):

3> re-use the source RAT SDAP and PDCP configurations if available (i.e., current SDAP/PDCP configurations for all RBs from source E-UTRA RAT prior to the reception of the inter-RAT HO *RRCReconfiguration* message);

1> else:

2> if the RRCReconfiguration includes the fullConfig:

3> perform the full configuration procedure as specified in 5.3.5.11;

1> if the *RRCReconfiguration* includes the *masterCellGroup*:

2> perform the cell group configuration for the received *masterCellGroup* according to 5.3.5.5;

1> if the *RRCReconfiguration* includes the *masterKeyUpdate*:

2> perform AS security key update procedure as specified in 5.3.5.7;

1> if the *RRCReconfiguration* includes the *sk-Counter*:

2> perform security key update procedure as specified in 5.3.5.7;

1> if the *RRCReconfiguration* includes the *secondaryCellGroup*:

2> perform the cell group configuration for the SCG according to 5.3.5.5;

1> if the *RRCReconfiguration* includes the *mrdc-SecondaryCellGroupConfig:*

2> if the *mrdc-SecondaryCellGroupConfig* is set to *setup*:

3> if the *mrdc-SecondaryCellGroupConfig* includes *mrdc-ReleaseAndAdd*:

4> perform MR-DC release as specified in clause 5.3.5.10;

3> if the received *mrdc-SecondaryCellGroup* is set to *nr-SCG*:

4> perform the RRC reconfiguration according to 5.3.5.3 for the *RRCReconfiguration* message included in *nr-SCG*;

3> if the received *mrdc-SecondaryCellGroup* is set to *eutra-SCG*:

4> perform the RRC connection reconfiguration as specified in TS 36.331 [10], clause 5.3.5.3 for the *RRCConnectionReconfiguration* message included in *eutra-SCG*;

2> else (*mrdc-SecondaryCellGroupConfig* is set to *release*):

3> perform MR-DC release as specified in clause 5.3.5.10;

1> if the *RRCReconfiguration* message includes the *radioBearerConfig*:

2> perform the radio bearer configuration according to 5.3.5.6;

1> if the *RRCReconfiguration* message includes the *radioBearerConfig2*:

2> perform the radio bearer configuration according to 5.3.5.6;

1> if the *RRCReconfiguration* message includes the *measConfig*:

2> perform the measurement configuration procedure as specified in 5.5.2;

1> if the *RRCReconfiguration* message includes the *dedicatedNAS-MessageList*:

2> forward each element of the *dedicatedNAS-MessageList* to upper layers in the same order as listed;

1> if the *RRCReconfiguration* message includes the *dedicatedSIB1-Delivery*:

2> perform the action upon reception of *SIB1* as specified in 5.2.2.4.2;

NOTE 0: If this *RRCReconfiguration* is associated to the MCG and includes *reconfigurationWithSync* in *spCellConfig* and *dedicatedSIB1-Delivery*, the UE initiates (if needed) the request to acquire required SIBs, according to clause 5.2.2.3.5, only after the random access procedure towards the target SpCell is completed.

1> if the *RRCReconfiguration* message includes the *dedicatedSystemInformationDelivery*:

2> perform the action upon reception of System Information as specified in 5.2.2.4;

2> if all the SIB(s) and/or posSIB(s) requested in *DedicatedSIBRequest* message have been acquired:

3> stop timer T350, if running;

1> if the *RRCReconfiguration* message includes the *dedicatedPosSysInfoDelivery*:

2> perform the action upon reception of the contained posSIB(s), as specified in clause 5.2.2.4.16;

2> if all the SIB(s) and/or posSIB(s) requested in *DedicatedSIBRequest* message have been acquired:

3> stop timer T350, if running;

1> if the *RRCReconfiguration* message includes the *otherConfig*:

2> perform the other configuration procedure as specified in 5.3.5.9;

1> if the *RRCReconfiguration* message includes the *bap-Config*:

2> perform the BAP configuration procedure as specified in 5.3.5.12;

1> if the *RRCReconfiguration* message includes the *iab-IP-AddressConfigurationList*:

2> if *iab-IP-AddressToReleaseList* is included:

3> perform release of IP address as specified in 5.3.5.12a.1.1;

2> if *iab-IP-AddressToAddModList* is included:

3> perform IAB IP address addition/update as specified in 5.3.5.12a.1.2;

1> if the *RRCReconfiguration* message includes the *conditionalReconfiguration*:

2> perform conditional reconfiguration as specified in 5.3.5.13;

1> if the *RRCReconfiguration* message includes the *needForGapsConfigNR*:

2> if *needForGapsConfigNR* is set to *setup*:

3> consider itself to be configured to provide the measurement gap requirement information of NR target bands;

2> else:

3> consider itself not to be configured to provide the measurement gap requirement information of NR target bands;

1> if the *RRCReconfiguration* message includes the *needForGapNCSG-ConfigNR*:

2> if *needForGapNCSG-ConfigNR* is set to *setup*:

3> consider itself to be configured to provide the measurement gap and NCSG requirement information of NR target bands;

2> else:

3> consider itself not to be configured to provide the measurement gap and NCSG requirement information of NR target bands;

1> if the *RRCReconfiguration* message includes the *needForGapNCSG-ConfigEUTRA*:

2> if *needForGapNCSG-ConfigEUTRA* is set to *setup*:

3> consider itself to be configured to provide the measurement gap and NCSG requirement information of E‑UTRA target bands;

2> else:

3> consider itself not to be configured to provide the measurement gap and NCSG requirement information of E‑UTRA target bands;

1> if the *RRCReconfiguration* message includes the *onDemandSIB-Request*:

2> if *onDemandSIB-Request* is set to *setup*:

3> consider itself to be configured to request SIB(s) or posSIB(s) in RRC\_CONNECTED in accordance with clause 5.2.2.3.5;

2> else:

3> consider itself not to be configured to request SIB(s) or posSIB(s) in RRC\_CONNECTED in accordance with clause 5.2.2.3.5;

3> stop timer T350, if running;

1> if the *RRCReconfiguration* message includes the *sl-ConfigDedicatedNR*:

2> perform the sidelink dedicated configuration procedure as specified in 5.3.5.14;

NOTE 0a: If the *sl-ConfigDedicatedNR* was received embedded within an E-UTRA *RRCConnectionReconfiguration* message, the UE does not build an NR *RRCReconfigurationComplete* message for the received *sl-ConfigDedicatedNR*.

1> if the *RRCReconfiguration* message includes the *sl-L2RelayUE-Config*:

2> perform the L2 U2N Relay UE configuration procedure as specified in 5.3.5.15;

1> if the *RRCReconfiguration* message includes the *sl-L2RemoteUE-Config*:

2> perform the L2 U2N Remote UE configuration procedure as specified in 5.3.5.16;

1> if the *RRCReconfiguration* message includes the *dedicatedPagingDelivery*:

2> perform the *Paging* message reception procedure as specified in 5.3.2.3;

1> if the *RRCReconfiguration* message includes the *sl-ConfigDedicatedEUTRA-Info*:

2> perform related procedures for V2X sidelink communication in accordance with TS 36.331 [10], clause 5.3.10 and clause 5.5.2;

1> if the *RRCReconfiguration* message includes the *ul-GapFR2-Config*:

2> perform the FR2 UL gap configuration procedure as specified in 5.3.5.13c;

1> if the *RRCReconfiguration* message includes the *musim-GapConfig*:

2> perform the MUSIM gap configuration procedure as specified in 5.3.5.9a;

1> if the *RRCReconfiguration* message includes the *appLayerMeasConfig*:

2> perform the application layer measurement configuration procedure as specified in 5.3.5.13d;

1> if the *RRCReconfiguration* message includes the *ue-TxTEG-RequestUL-TDOA-Config*:

2> if *ue-TxTEG-RequestUL-TDOA-Config* is set to *setup*:

3> perform the UE positioning assistance information procedure as specified in 5.7.14;

2> else:

3> release the configuration of UE positioning assistance information;

1> set the content of the *RRCReconfigurationComplete* message as follows:

2> if the *RRCReconfiguration* includes the *masterCellGroup* containing the *reportUplinkTxDirectCurrent*:

3> include the *uplinkTxDirectCurrentList* for each MCG serving cell with UL;

3> include *uplinkDirectCurrentBWP-SUL* for each MCG serving cell configured with SUL carrier, if any, within the *uplinkTxDirectCurrentList*;

2> if the *RRCReconfiguration* includes the *masterCellGroup* containing the *reportUplinkTxDirectCurrentTwoCarrier*:

3> include in the *uplinkTxDirectCurrentTwoCarrierList* the list of uplink Tx DC locations for the configured intra-band uplink carrier aggregation in the MCG;

2> if the *RRCReconfiguration* includes the *masterCellGroup* containing the *reportUplinkTxDirectCurrentMoreCarrier*:

3> include in the *uplinkTxDirectCurrentMoreCarrierList* the list of uplink Tx DC locations for the configured intra-band uplink carrier aggregation in the MCG;

2> if the *RRCReconfiguration* includes the *secondaryCellGroup* containing the *reportUplinkTxDirectCurrent*:

3> include the *uplinkTxDirectCurrentList* for each SCG serving cell with UL;

3> include *uplinkDirectCurrentBWP-SUL* for each SCG serving cell configured with SUL carrier, if any, within the *uplinkTxDirectCurrentList*;

2> if the *RRCReconfiguration* includes the *secondaryCellGroup* containing the *reportUplinkTxDirectCurrentTwoCarrier*:

3> include in the *uplinkTxDirectCurrentTwoCarrierList* the list of uplink Tx DC locations for the configured intra-band uplink carrier aggregation in the SCG;

2> if the *RRCReconfiguration* includes the *secondaryCellGroup* containing the *reportUplinkTxDirectCurrentMoreCarrier*:

3> include in the *uplinkTxDirectCurrentMoreCarrierList* the list of uplink Tx DC locations for the configured intra-band uplink carrier aggregation in the SCG;

NOTE 0b: The UE does not expect that the *reportUplinkTxDirectCurrentTwoCarrier* or *reportUplinkTxDirectCurrentMoreCarrier* is received in both *masterCellGroup* and in *secondaryCellGroup*. Network only configures at most one of *reportUplinkTxDirectCurrent, reportUplinkTxDirectCurrentTwoCarrier* or *reportUplinkTxDirectCurrentMoreCarrier* in one RRC message*.*

2> if the *RRCReconfiguration* message includes the *mrdc-SecondaryCellGroupConfig* with *mrdc-SecondaryCellGroup* set to *eutra-SCG*:

3> include in the *eutra-SCG-Response* the E-UTRA *RRCConnectionReconfigurationComplete* message in accordance with TS 36.331 [10] clause 5.3.5.3;

2> if the *RRCReconfiguration* message includes the *mrdc-SecondaryCellGroupConfig* with *mrdc-SecondaryCellGroup* set to *nr-SCG*:

3> include in the *nr-SCG-Response* the SCG *RRCReconfigurationComplete* message;

3> if the *RRCReconfiguration* message is applied due to conditional reconfiguration execution and the *RRCReconfiguration* message does not include the *reconfigurationWithSync* in the *masterCellGroup*:

4> include in the *selectedCondRRCReconfig* the *condReconfigId* for the selected cell of conditional reconfiguration execution;

4> if a new *SK-Counter* value has been selected due to the conditional reconfiguration execution:

5> include in the *selectedSK-Counter* the selected *SK-Counter* for the selected cell of conditional reconfiguration execution;

2> if the *RRCReconfiguration* includes the *reconfigurationWithSync* in *spCellConfig* of an MCG:

3> if the UE has logged measurements available for NR and if the RPLMN is included in *plmn-IdentityList* stored in *VarLogMeasReport*:

4> include the *logMeasAvailable* in the *RRCReconfigurationComplete* message;

4> if Bluetooth measurement results are included in the logged measurements the UE has available for NR:

5> include the *logMeasAvailableBT* in the *RRCReconfigurationComplete* message;

4> if WLAN measurement results are included in the logged measurements the UE has available for NR:

5> include the *logMeasAvailableWLAN* in the *RRCReconfigurationComplete* message;

3> if the *sigLoggedMeasType* in *VarLogMeasReport* is included:

4> if T330 timer is running and the logged measurements configuration is for NR:

5> set *sigLogMeasConfigAvailable* to *true* in the *RRCReconfigurationComplete* message;

4> else:

5> if the UE has logged measurements available for NR:

6> set *sigLogMeasConfigAvailable* to *false* in the *RRCReconfigurationComplete* message;

3> if the UE has connection establishment failure or connection resume failure information available in *VarConnEstFailReport* or *VarConnEstFailReportList* and if the RPLMN is equal to *plmn-Identity* stored in *VarConnEstFailReport* orin at least one of the entries of *VarConnEstFailReportList*:

4> include *connEstFailInfoAvailable* in the *RRCReconfigurationComplete* message;

3> if the UE has radio link failure or handover failure information available in *VarRLF-Report* and if the RPLMN is included in *plmn-IdentityList* stored in *VarRLF-Report*; or

3> if the UE has radio link failure or handover failure information available in *VarRLF-Report* of TS 36.331 [10] and if the UE is capable of cross-RAT RLF reporting and if the RPLMN is included in *plmn-IdentityList* stored in *VarRLF-Report* of TS 36.331 [10]:

4> include *rlf-InfoAvailable* in the *RRCReconfigurationComplete* message;

3> if the UE was configured with *successHO-Config* when connected to the source PCell; and

3> if the applied *RRCReconfiguration* is not due to a conditional reconfiguration execution upon cell selection performed while timer T311 was running, as defined in 5.3.7.3:

4> perform the actions for the successful handover report determination as specified in clause 5.7.10.6, upon successfully completing the Random Access procedure triggered for the *reconfigurationWithSync* in *spCellConfig* of the MCG;

3> if the UE has successful handover information available in *VarSuccessHO-Report* and if the RPLMN is included in *plmn-IdentityList* stored in *VarSuccessHO-Report*:

4> include *successHO-InfoAvailable* in the *RRCReconfigurationComplete* message;

2> if the *RRCReconfiguration* message was received via SRB1, but not within *mrdc-SecondaryCellGroup* or E-UTRA *RRCConnectionReconfiguration* or E-UTRA *RRCConnectionResume*:

3> if the UE is configured to provide the measurement gap requirement information of NR target bands:

4> if the *RRCReconfiguration* message includes the *needForGapsConfigNR*; or

4> if the *NeedForGapsInfoNR* information is changed compared to last time the UE reported this information:

5> include the *NeedForGapsInfoNR* and set the contents as follows:

6> include *intraFreq-needForGap* and set the gap requirement information of intra-frequency measurement for each NR serving cell;

6> if *requestedTargetBandFilterNR* is configured:

7> for each supported NR band that is also included in *requestedTargetBandFilterNR*, include an entry in *interFreq-needForGap* and set the gap requirement information for that band;

6> else:

7> include an entry in *interFreq-needForGap* and set the corresponding gap requirement information for each supported NR band;

3> if the UE is configured to provide the measurement gap and NCSG requirement information of NR target bands:

4> if the *RRCReconfiguration* message includes the *needForGapNCSG-ConfigNR*; or

4> if the *needForGapNCSG-InfoNR* information is changed compared to last time the UE reported this information:

5> include the *NeedForGapNCSG-InfoNR* and set the contents as follows:

6> include *intraFreq-needForNCSG* and set the gap and NCSG requirement information of intra-frequency measurement for each NR serving cell;

6> if *requestedTargetBandFilterNCSG-NR* is configured:

7> for each supported NR band included in *requestedTargetBandFilterNCSG-NR*, include an entry in *interFreq-needForNCSG* and set the NCSG requirement information for that band;

6> else:

7> include an entry for each supported NR band in *interFreq-needForNCSG* and set the corresponding NCSG requirement information;

3> if the UE is configured to provide the measurement gap and NCSG requirement information of E‑UTRA target bands:

4> if the *RRCReconfiguration* message includes the *needForGapNCSG-ConfigEUTRA*; or

4> if the *needForGapNCSG-InfoEUTRA* information is changed compared to last time the UE reported this information:

5> include the *NeedForGapNCSG-InfoEUTRA* and set the contents as follows:

6> if *requestedTargetBandFilterNCSG-EUTRA* is configured, for each supported E-UTRA band included in *requestedTargetBandFilterNCSG-EUTRA*, include an entry in *needForNCSG-EUTRA* and set the NCSG requirement information for that band; otherwise, include an entry for each supported E-UTRA band in *needForNCSG-EUTRA* and set the corresponding NCSG requirement information;

1> if the UE is configured with E-UTRA *nr-SecondaryCellGroupConfig* (UE in (NG)EN-DC):

2> if the *RRCReconfiguration* message was received via E-UTRA SRB1 as specified in TS 36.331 [10]; or

2> if the *RRCReconfiguration* message was received via E-UTRA RRC message *RRCConnectionReconfiguration* within *MobilityFromNRCommand* (handover from NR standalone to (NG)EN-DC);

3> if the *RRCReconfiguration* is applied due to a conditional reconfiguration execution for CPC which is configured via *conditionalReconfiguration* contained in *nr-SecondaryCellGroupConfig* specified in TS 36.331 [10]:

4> submit the *RRCReconfigurationComplete* message via the E-UTRA MCG embedded in E-UTRA RRC message *ULInformationTransferMRDC* as specified in TS 36.331 [10], clause 5.6.2a.

3> else if the *RRCReconfiguration* message was included in E-UTRA *RRCConnectionResume* message:

4> submit the *RRCReconfigurationComplete* message via E-UTRA embedded in E-UTRA RRC message *RRCConnectionResumeComplete* as specified in TS 36.331 [10], clause 5.3.3.4a;

3> else:

4> submit the *RRCReconfigurationComplete* via E-UTRA embedded in E-UTRA RRC message *RRCConnectionReconfigurationComplete* as specified in TS 36.331 [10], clause 5.3.5.3/5.3.5.4/5.4.2.3;

3> if the *scg-State* is not included in the E-UTRA message (*RRCConnectionReconfiguration* or *RRCConnectionResume*) containing the *RRCReconfiguration* message:

4> perform SCG activation as specified in 5.3.5.13a;

4> if *reconfigurationWithSync* was included in *spCellConfig* of an SCG:

5> initiate the Random Access procedure on the PSCell, as specified in TS 38.321 [3];

4> else if the SCG was deactivated before the reception of the E-UTRA RRC message containing the *RRCReconfiguration* message:

5> if *bfd-and-RLM* was not configured to *true* before the reception of the E-UTRA *RRCConnectionReconfiguration* or *RRCConnectionResume* message containing the *RRCReconfiguration* message or if lower layers indicate that a Random Access procedure is needed for SCG activation:

6> initiate the Random Access procedure on the SpCell, as specified in TS 38.321 [3];

5> else the procedure ends;

4> else the procedure ends;

3> else:

4> perform SCG deactivation as specified in 5.3.5.13b;

4> the procedure ends;

2> if the *RRCReconfiguration* message was received within *nr-SecondaryCellGroupConfig* in *RRCConnectionReconfiguration* message received via SRB3 within *DLInformationTransferMRDC*:

3> submit the *RRCReconfigurationComplete* via E-UTRA embedded in E-UTRA RRC message *RRCConnectionReconfigurationComplete* as specified in TS 36.331 [10], clause 5.3.5.3/5.3.5.4;

3> if the *scg-State* is not included in the *RRCConnectionReconfiguration*:

4> if *reconfigurationWithSync* was included in *spCellConfig* of an SCG:

5> initiate the Random Access procedure on the SpCell, as specified in TS 38.321 [3];

4> else the procedure ends;

3> else:

4> perform SCG deactivation as specified in 5.3.5.13b;

4> the procedure ends;

NOTE 1: The order the UE sends the *RRCConnectionReconfigurationComplete* message and performs the Random Access procedure towards the SCG is left to UE implementation.

2> else (*RRCReconfiguration* was received via SRB3) but not within *DLInformationTransferMRDC*:

3> submit the *RRCReconfigurationComplete* message via SRB3 to lower layers for transmission using the new configuration;

NOTE 2: In (NG)EN-DC and NR-DC, in the case *RRCReconfiguration* is received via SRB1 or within *DLInformationTransferMRDC* via SRB3, the random access is triggered by RRC layer itself as there is not necessarily other UL transmission. In the case *RRCReconfiguration* is received via SRB3 but not within *DLInformationTransferMRDC*, the random access is triggered by the MAC layer due to arrival of *RRCReconfigurationComplete*.

1> else if the *RRCReconfiguration* message was received via SRB1 within the *nr-SCG* within *mrdc-SecondaryCellGroup* (UE in NR-DC, *mrdc-SecondaryCellGroup* was received in *RRCReconfiguration* or *RRCResume* via SRB1):

2> if the *RRCReconfiguration* is applied due to a conditional reconfiguration execution for CPC which is configured via *conditionalReconfiguration* contained in *nr-SCG* within *mrdc-SecondaryCellGroup*:

3> submit the *RRCReconfigurationComplete* message via the NR MCG embedded in NR RRC message *ULInformationTransferMRDC* as specified in clause 5.7.2a.3.

2> if the *scg-State* is not included in the *RRCReconfiguration* or *RRCResume* message containing the *RRCReconfiguration* message:

3> perform SCG activation as specified in 5.3.5.13a;

3> if *reconfigurationWithSync* was included in *spCellConfig* in nr-SCG:

4> initiate the Random Access procedure on the PSCell, as specified in TS 38.321 [3];

3> else if the SCG was deactivated before the reception of the NR RRC message containing the *RRCReconfiguration* message:

4> if *bfd-and-RLM* was not configured to *true* before the reception of the *RRCReconfiguration* or *RRCResume* message containing the *RRCReconfiguration* message; or

4> if lower layers indicate that a Random Access procedure is needed for SCG activation:

5> initiate the Random Access procedure on the PSCell, as specified in TS 38.321 [3];

4> else the procedure ends;

3> else the procedure ends;

2> else

3> perform SCG deactivation as specified in 5.3.5.13b;

3> the procedure ends;

NOTE 2a: The order in which the UE sends the *RRCReconfigurationComplete* message and performs the Random Access procedure towards the SCG is left to UE implementation.

1> else if the *RRCReconfiguration* message was received via SRB3 (UE in NR-DC):

2> if the *RRCReconfiguration* message was received within *DLInformationTransferMRDC*:

3> if the *RRCReconfiguration* message was received within the *nr-SCG* within *mrdc-SecondaryCellGroup* (NR SCG RRC Reconfiguration):

4> if the *scg-State* is not included in the *RRCReconfiguration* message containing the *RRCReconfiguration* message:

5> if *reconfigurationWithSync* was included in spCellConfig in nr-SCG:

6> initiate the Random Access procedure on the PSCell, as specified in TS 38.321 [3];

5> else:

6> the procedure ends;

4> else:

5> perform SCG deactivation as specified in 5.3.5.13b;

5> the procedure ends;

3> else:

4> if the *RRCReconfiguration* does not include the *mrdc-SecondaryCellGroupConfig*:

5> if the *RRCReconfiguration* includes the *scg-State*:

6> perform SCG deactivation as specified in 5.3.5.13b;

4> submit the *RRCReconfigurationComplete* message via SRB1 to lower layers for transmission using the new configuration;

2> else:

3> submit the *RRCReconfigurationComplete* message via SRB3 to lower layers for transmission using the new configuration;

1> else(*RRCReconfiguration* was received via SRB1):

2> if the UE is in NR-DC and;

2> if the *RRCReconfiguration* does not include the *mrdc-SecondaryCellGroupConfig*:

3> if the *RRCReconfiguration* includes the *scg-State*:

4> perform SCG deactivation as specified in 5.3.5.13b;

3> else:

4> perform SCG activation without SN message as specified in 5.3.5.13b1;

2> if the *reconfigurationWithSync* was included in *spCellConfig* of an MCG:

3> if *ta-Report* is configured with value *enabled* and the UE supports TA reporting:

4> indicate TA report initiation to lower layers;

2> submit the *RRCReconfigurationComplete* message via SRB1 to lower layers for transmission using the new configuration;

2> if this is the first *RRCReconfiguration* message after successful completion of the RRC re-establishment procedure:

3> resume SRB2, SRB4, DRBs, multicast MRB, and BH RLC channels for IAB-MT, and Uu Relay RLC channels for L2 U2N Relay UE, that are suspended;

1> if *reconfigurationWithSync* was included in *spCellConfig* of an MCG or SCG and when MAC of an NR cell group successfully completes a Random Access procedure triggered above; or,

1> if *sl-PathSwitchConfig* was included in *reconfigurationWithSync* included in *spCellConfig* of an MCG, and when successfully sending *RRCReconfigurationComplete* message (i.e., PC5 RLC acknowledgement is received from target L2 U2N Relay UE):

2> stop timer T304 for that cell group if running;

2> if *sl-PathSwitchConfig* was included in *reconfigurationWithSync*:

3> stop timer T420;

3> release all radio resources, including release of the RLC entities and the MAC configuration at the source side;

3> reset MAC used in the source cell;

NOTE 2b: PDCP and SDAP configured by the source prior to the path switch that are reconfigured and re-used by target when delta signalling is used, are not released as part of this procedure.

2> stop timer T310 for source SpCell if running;

2> apply the parts of the CSI reporting configuration, the scheduling request configuration and the sounding RS configuration that do not require the UE to know the SFN of the respective target SpCell, if any;

2> apply the parts of the measurement and the radio resource configuration that require the UE to know the SFN of the respective target SpCell (e.g. measurement gaps, periodic CQI reporting, scheduling request configuration, sounding RS configuration), if any, upon acquiring the SFN of that target SpCell;

2> for each DRB configured as DAPS bearer, request uplink data switching to the PDCP entity, as specified in TS 38.323 [5];

2> if the *reconfigurationWithSync* was included in *spCellConfig* of an MCG:

3> if T390 is running:

4> stop timer T390 for all access categories;

4> perform the actions as specified in 5.3.14.4.

3> if T350 is running:

4> stop timer T350;

3> if *RRCReconfiguration* does not include *dedicatedSIB1-Delivery* and

3> if the active downlink BWP, which is indicated by the *firstActiveDownlinkBWP-Id* for the target SpCell of the MCG, has a common search space configured by *searchSpaceSIB1*:

4> acquire the *SIB1*, which is scheduled as specified in TS 38.213 [13], of the target SpCell of the MCG;

4> upon acquiring *SIB1*, perform the actions specified in clause 5.2.2.4.2;

2> if the *reconfigurationWithSync* was included in *spCellConfig* of an MCG; or

2> if the *reconfigurationWithSync* was included in *spCellConfig* of an SCG and the CPA or CPC was configured:

3> remove all the entries in the *condReconfigList* within the MCG and the SCG *VarConditionalReconfig* except for the entries in which *subsequentCondReconfig* is present, if any;

3> remove all the entries within *VarConditionalReconfiguration* as specified in TS 36.331 [10], clause 5.3.5.9.6, if any;

3> for each *measId* of the MCG *measConfig*, if configured, and for each *measId* of the SCG *measConfig*, if configured, if the associated *reportConfig* has a *reportType* set to *condTriggerConfig*：

4> if the *reportConfigId* is not associated with any *measId* indicated by the *condExecutionCond* or the *condExecutionCondSCG* in an entry of *condReconfigList* in *VarConditionalReconfig* in which *subsequentCondReconfig* is included; and

4> if the *reportConfigId* is not associated with any *measId* indicated by the *condExecutionCond* or the *condExecutionCondSCG* in an entry of *subsequentCondReconfig* in an entry of *condReconfigList* in *VarConditionalReconfig*:

5> remove the entry with the matching *reportConfigId* from the *reportConfigList* within the *VarMeasConfig*;

4> if the associated *measObjectId* is only associated to a *reportConfig* with *reportType* set to *condTriggerConfig*; and

4> if the *measObjectId* is not associated with any *measId* indicated by the *condExecutionCond* or the *condExecutionCondSCG* in an entry of *condReconfigList* in *VarConditionalReconfig* in which *subsequentCondReconfig* is included; and

4> if the *measObjectId* is not associated with any *measId* indicated by the *condExecutionCond* or the *condExecutionCondSCG* in an entry of *subsequentCondReconfig* in an entry of *condReconfigList* in *VarConditionalReconfig*:

5> remove the entry with the matching *measObjectId* from the *measObjectList* within the *VarMeasConfig*;

4> remove the entry with the matching *measId* from the *measIdList* within the *VarMeasConfig*;

2> if the *RRCReconfiguration* message is applied due to a conditional reconfiguration execution and the *subsequentCondReconfig* is included in the entry in *VarConditionalReconfig* containing the *RRCReconfiguration* message:

3> for each *condReconfigId* included in *condExecutionCondToAddModList* within *subsequentCondReconfig*:

4> replace *condExecutionCond* or *condExecutionCondSCG* within the *VarConditionalReconfig* with the value received for this *condReconfigId*;

3> initiate the conditional reconfiguration evaluation procedure, as specified in 5.3.5.13.4;

*Editor’s Note: FFS on how to start conditional reconfiguration evaluation for subsequent CPAC for the following cases: after SCG is release；upon pscell change/addition completion；upon pcell change completion.*

2> if *reconfigurationWithSync* was included in *masterCellGroup* or *secondaryCellGroup*:

3> if the UE initiated transmission of a *UEAssistanceInformation* message for the corresponding cell group during the last 1 second, and the UE is still configured to provide the concerned UE assistance information for the corresponding cell group; or

3> if the *RRCReconfiguration* message is applied due to a conditional reconfiguration execution, and the UE is configured to provide UE assistance information for the corresponding cell group, and the UE has initiated transmission of a *UEAssistanceInformation* message for the corresponding cell group since it was configured to do so in accordance with 5.7.4.2:

4> initiate transmission of a *UEAssistanceInformation* message for the corresponding cell group in accordance with clause 5.7.4.3 to provide the concerned UE assistance information;

4> start or restart the prohibit timer (if exists) or the leave without response timer for the MUSIM associated with the concerned UE assistance information with the timer value set to the value in corresponding configuration;

3> if *SIB12* is provided by the target PCell, and the UE initiated transmission of a *SidelinkUEInformationNR* message indicating a change of NR sidelink communication/discovery related parameters relevant in target PCell (i.e. change of *sl-RxInterestedFreqList* or *sl-TxResourceReqList*) during the last 1 second preceding reception of the *RRCReconfiguration* message including *reconfigurationWithSync* in *spCellConfig* of an MCG; or

3> if the *RRCReconfiguration* message is applied due to a conditional reconfiguration execution and the UE is capable of NR sidelink communication/discovery and *SIB12* is provided by the target PCell, and the UE has initiated transmission of a *SidelinkUEInformationNR* message since it was configured to do so in accordance with 5.8.3.2:

4> initiate transmission of the *SidelinkUEInformationNR* message in accordance with 5.8.3.3;

2> if *reconfigurationWithSync* was included in *masterCellGroup*:

3> if configured with application layer measurements and if application layer measurement report container has been received from upper layers for which the successful transmission of the message or at least one segment of the message has not been confirmed by lower layers:

4> re-submit the *MeasurementReportAppLayer* message or all segments of the *MeasurementReportAppLayer* message to lower layers for transmission via SRB4;

2> if *reconfigurationWithSync* was included in *masterCellGroup* and the target cell provides *SIB21*:

3> if the UE initiated transmission of an *MBSInterestIndication*message during the last 1 second preceding reception of this *RRCReconfiguration* message; or

3> if the *RRCReconfiguration* message is applied due to a conditional reconfiguration execution, and the UE has initiated transmission of an *MBSInterestIndication* message after having received this *RRCReconfiguration* message:

4> initiate transmission of an *MBSInterestIndication*message in accordance with clause 5.9.4;

2> the procedure ends.

NOTE 3: The UE is only required to acquire broadcasted *SIB1* if the UE can acquire it without disrupting unicast or MBS multicast data reception, i.e. the broadcast and unicast/MBS multicast beams are quasi co-located.

NOTE 4: The UE sets the content of *UEAssistanceInformation* according to latest configuration (i.e. the configuration after applying the *RRCReconfiguration* message) and latest UE preference. The UE may include more than the concerned UE assistance information within the *UEAssistanceInformation* according to 5.7.4.2. Therefore, the content of *UEAssistanceInformation* message might not be the same as the content of the previous *UEAssistanceInformation* message.

#### 5.3.5.4 Secondary cell group release

The UE shall:

1> as a result of SCG release triggered by E-UTRA (i.e. (NG)EN-DC case) or NR (i.e. NR-DC case):

2> reset SCG MAC, if configured;

2> for each RLC bearer that is part of the SCG configuration:

3> perform RLC bearer release procedure as specified in 5.3.5.5.3;

2> for each BH RLC channel that is part of the SCG configuration:

3> perform BH RLC channel release procedure as specified in 5.3.5.5.10;

2> release the SCG configuration;

2> remove all the entries within the SCG *VarConditionalReconfig*, if any;

2> if SCG release was triggered by NR (i.e. NR-DC case):

3> remove all the entries in the *condReconfigList* within the MCG *VarConditionalReconfig* for which the *RRCReconfiguration* within *condRRCReconfig* does not include the *masterCellGroup* with *reconfigurationWithSync* except for the entries in which *subsequentCondReconfig* is present, if any;

2> else (i.e. EN-DC case):

3> perform *VarConditionalReconfiguration* CPC removal as specified in TS 36.331 [10] clause 5.3.5.9.7;

2> stop timer T310 for the corresponding SpCell, if running;

2> stop timer T312 for the corresponding SpCell, if running;

2> stop timer T304 for the corresponding SpCell, if running.

NOTE: Release of cell group means only release of the lower layer configuration of the cell group but the *RadioBearerConfig* may not be released.

#### 5.3.5.7 AS Security key update

The UE shall:

1> if UE is connected to E-UTRA/EPC or E-UTRA/5GC:

2> upon reception of *sk-Counter* as specified in TS 36.331 [10]:

3> update the S-KgNB key based on the KeNB key and using the received *sk-Counter* value, as specified in TS 33.401 [30] for EN-DC, or TS 33.501 [11] for NGEN-DC;

3> derive the KRRCenc and KUPenc keys as specified in TS 33.401 [30] for EN-DC, or TS 33.501 [11] for NGEN-DC;

3> derive the KRRCint and KUPint keys as specified in TS 33.401 [30] for EN-DC or TS 33.501 [11] for NGEN-DC.

1> else if this procedure was initiated due to reception of the *masterKeyUpdate*:

2> if the *nas-Container* is included in the received *masterKeyUpdate*:

3> forward the *nas-Container* to the upper layers;

2> if the *keySetChangeIndicator* is set to *true*:

3> derive or update the KgNB key based on the KAMF key, as specified in TS 33.501 [11];

2> else:

3> derive or update the KgNB key based on the current KgNB key or the NH, using the *nextHopChainingCount* value indicated in the received *masterKeyUpdate*, as specified in TS 33.501 [11];

2> store the *nextHopChainingCount* value;

2> derive the keys associated with the KgNB key as follows:

3> if the *securityAlgorithmConfig* is included in *SecurityConfig*:

4> derive the KRRCenc and KUPenc keys associated with the *cipheringAlgorithm* indicated in the *securityAlgorithmConfig,* as specified in TS 33.501 [11];

4> derive the KRRCint and KUPint keys associated with the *integrityProtAlgorithm* indicated in the *securityAlgorithmConfig,* as specified in TS 33.501 [11];

3> else:

4> derive the KRRCenc and KUPenc keys associated with the current *cipheringAlgorithm,* as specified in TS 33.501 [11];

4> derive the KRRCint and KUPint keys associated with the current *integrityProtAlgorithm,* as specified in TS 33.501 [11].

NOTE 1: Ciphering and integrity protection are optional to configure for the DRBs.

1> else if this procedure was initiated due to reception of the *sk-Counter* or upon selection of *sk-Counter* for the conditional reconfiguration execution for subsequent CPAC (UE is in NE-DC, or NR-DC, or is configured with SN terminated bearer(s)):

2> derive or update the secondary key (S-KgNB or S-KeNB) based on the KgNB key and using the received/selected *sk-Counter* value, as specified in TS 33.501 [11];

2> derive the KRRCenc key and the KUPenc key as specified in TS 33.501 [11] using the ciphering algorithms indicated in the *RadioBearerConfig* associated with the secondary key (S-KgNB or S-KeNB) as indicated by *keyToUse*;

2> derive the KRRCint key and the KUPint key as specified in TS 33.501 [11] using the integrity protection algorithms indicated in the *RadioBearerConfig* associated with the secondary key (S-KgNB or S-KeNB) as indicated by *keyToUse*;

NOTE 2: If the UE has no radio bearer configured with *keyToUse* set to *secondary* and receives the *sk-Counter* without any *RadioBearerConfig* with *keyToUse* set to *secondary*, the UE does not consider it as an invalid reconfiguration.

#### 5.3.5.13 Conditional Reconfiguration

##### 5.3.5.13.1 General

The network configures the UE with one or more candidate target SpCells in the conditional reconfiguration. The UE evaluates the condition of each configured candidate target SpCell. The UE applies the conditional reconfiguration associated with one of the target SpCells which fulfils associated execution condition. The network provides the configuration parameters for the target SpCell in the *condRRCReconfig*.

In NR-DC, the UE may receive two independent *conditionalReconfiguration*:

- a *conditionalReconfiguration* associated with MCG, that is included in the *RRCReconfiguration* message received via SRB1; and

- a *conditionalReconfiguration*, associated with SCG, that is included in the *RRCReconfiguration* message received via SRB3, or, alternatively, included within a *RRCReconfiguration* message embedded in a *RRCReconfiguration* message received via SRB1.

In this case:

- the UE maintains two independent *VarConditionalReconfig*, one associated with each *conditionalReconfiguration*;

- the UE independently performs all the procedures in clause 5.3.5.13 for each *conditionalReconfiguration* and the associated *VarConditionalReconfig*, unless explicitly stated otherwise;

- the UE performs the procedures in clause 5.5 for the *VarConditionalReconfig* associated with the same cell group like the *measConfig*.

In EN-DC, the *VarConditionalReconfig* is associated with the SCG.

In NE-DC and when no SCG is configured, the *VarConditionalReconfig* is associated with the MCG.

The UE performs the following actions based on a received *ConditionalReconfiguration* IE:

1> if the *ConditionalReconfiguration* contains the *condReconfigToRemoveList*:

2> perform conditional reconfiguration removal procedure as specified in 5.3.5.13.2;

1> if the *ConditionalReconfiguration* contains the *condReconfigToAddModList*:

2> perform conditional reconfiguration addition/modification as specified in 5.3.5.13.3;

1> if the *ConditionalReconfiguration* contains the *scpac-ReferenceConfiguration*:

2> perform reference configuration addition/removal as specified in 5.3.5.13.x1;1> if the *ConditionalReconfiguration* contains the *sk-CounterConfiguration*:

2> perform sk-CounterList addition/modification/removal as specified in 5.3.5.13.x2;

*Editor’s Note: Wait for LTM on the complete configuration generation/application related part.*

##### 5.3.5.13.2 Conditional reconfiguration removal

The UE shall:

1> for each *condReconfigId* value included in the *condReconfigToRemoveList* that is part of the current UE conditional reconfiguration in *VarConditionalReconfig*:

2> remove the entry with the matching *condReconfigId* from the *VarConditionalReconfig*;

NOTE: The UE does not consider the message as erroneous if the *condReconfigToRemoveList* includes any cond*ReconfigId* value that is not part of the current UE configuration.

*Editor’s Note: FFS on how to remove the entries within the VarServingSecurityCellSetID when NW explicitly removes all the SCPAC configurations.*

##### 5.3.5.13.3 Conditional reconfiguration addition/modification

For each *condReconfigId* received in the *condReconfigToAddModList* IE the UE shall:

1> if an entry with the matching *condReconfigId* exists in the *condReconfigToAddModList* within the *VarConditionalReconfig*:

2> if the entry in *condReconfigToAddModList* includes an *condExecutionCond* or *condExecutionCondSCG*;

3> replace *condExecutionCond* or *condExecutionCondSCG* within the *VarConditionalReconfig* with the value received for this *condReconfigId*;

2> if the entry in *condReconfigToAddModList* includes *subsequentCondReconfig* containing *condExecutionCondToAddModList*:

3> for each *condReconfigId* received in *condExecutionCondToAddModList*:

4> if there is an entry with the matching *condReconfigId* exists in the *condExecutionCondToAddModList;*

5> replace the entry with the value received for this *condReconfigId*;

4> else:

5> add a new entry for the received *condReconfigId* to the *condExecutionCondToAddModList*;

3> for each *condReconfigId* received in *condExecutionCondToReleaseList* that is part of current stored *condExecutionCondToAddModList*:

4> remove the entry with the matching *condReconfigId* from the *condExecutionCondToAddModList*;

2> if the entry in *condReconfigToAddModList* includes an *condRRCReconfig*;

3> replace *condRRCReconfig* within the *VarConditionalReconfig* with the value received for this *condReconfigId*;

1> else:

2> add a new entry for this *condReconfigId* within the *VarConditionalReconfig*;

1> perform conditional reconfiguration evaluation as specified in 5.3.5.13.4;

##### 5.3.5.13.4 Conditional reconfiguration evaluation

The UE shall:

1> for each *condReconfigId* within the *VarConditionalReconfig*:

2> if the *RRCReconfiguration* within *condRRCReconfig* includes the *masterCellGroup* including the *reconfigurationWithSync*:

3> consider the cell which has a physical cell identity matching the value indicated in the *ServingCellConfigCommon* included in the *reconfigurationWithSync* within the *masterCellGroup* in the received *condRRCReconfig* to be applicable cell;

2> else if the *RRCReconfiguration* within *condRRCReconfig* includes the *secondaryCellGroup* including the *reconfigurationWithSync*:

3> if the cell which has a physical cell identity matching the value indicated in the *ServingCellConfigCommon* included in the *reconfigurationWithSync* within the *secondaryCellGroup* within the received *condRRCReconfig* is not the PSCell:

4> consider the cell to be applicable cell;

2> if *condExecutionCondSCG* is configured:

3> in the remainder of the procedure, consider each *measId* indicated in the *condExecutionCondSCG* as a *measId* in the *VarMeasConfig* associated with the SCG *measConfig*;

2> if *condExecutionCond* is configured:

3> if it is configured via SRB3 or configured within *nr-SCG* or within *nr-SecondaryCellGroupConfig* (specified in TS 36.331[10]) via SRB1:

4> in the remainder of the procedure, consider each *measId* indicated in the *condExecutionCond* as a *measId* in the *VarMeasConfig* associated with the SCG *measConfig*;

3> else:

4> in the remainder of the procedure, consider each *measId* indicated in the *condExecutionCond* as a *measId* in the *VarMeasConfig* associated with the MCG *measConfig*;

2> for each *measId* included in the *measIdList* within *VarMeasConfig* indicated in the *condExecutionCond* or *condExecutionCondSCG* associated to *condReconfigId:*

3> if the *condEventId* is associated with *condEventT1*, and if the entry condition applicable for this event associated with the *condReconfigId*, i.e. the event corresponding with the *condEventId(s)* of the corresponding *condTriggerConfig* within *VarConditionalReconfig*, is fulfilled for the applicable cell; or

3> if the *condEventId* is associated with *condEventD1*, and if the entry conditions applicable for this event associated with the *condReconfigId*, i.e. the event corresponding with the *condEventId(s)* of the corresponding *condTriggerConfig* within *VarConditionalReconfig*, is fulfilled for the applicable cell during the corresponding *timeToTrigger* defined for this event within the *VarConditionalReconfig*; or

3> if the *condEventId* is associated with *condEventA3*, *condEventA4* or *condEventA5*, and if the entry condition(s) applicable for this event associated with the *condReconfigId*, i.e. the event corresponding with the *condEventId(s)* of the corresponding *condTriggerConfig* within *VarConditionalReconfig*, is fulfilled for the applicable cells for all measurements after layer 3 filtering taken during the corresponding *timeToTrigger* defined for this event within the *VarConditionalReconfig*:

4> consider the event associated to that *measId* to be fulfilled;

3> if the *measId* for this event associated with the *condReconfigId* has been modified; or

3> if the *condEventId* is associated with *condEventT1*, and if the leaving condition applicable for this event associated with the *condReconfigId*, i.e. the event corresponding with the *condEventId(s)* of the corresponding *condTriggerConfig* within *VarConditionalReconfig*, is fulfilled for the applicable cell; or

3> if the *condEventId* is associated with *condEventD1*, and if the leaving condition(s) applicable for this event associated with the *condReconfigId*, i.e. the event corresponding with the *condEventId(s)* of the corresponding *condTriggerConfig* within *VarConditionalReconfig*, is fulfilled for the applicable cell during the corresponding *timeToTrigger* defined for this event within the *VarConditionalReconfig*; or

3> if the *condEventId* is associated with *condEventA3*, *condEventA4* or *condEventA5*, and if the leaving condition(s) applicable for this event associated with the *condReconfigId*, i.e. the event corresponding with the *condEventId(s)* of the corresponding *condTriggerConfig* within *VarConditionalReconfig*, is fulfilled for the applicable cells for all measurements after layer 3 filtering taken during the corresponding *timeToTrigger* defined for this event within the *VarConditionalReconfig*:

4> consider the event associated to that *measId* to be not fulfilled;

2> if event(s) associated to all *measId*(s) within *condTriggerConfig* for the applicable cell are fulfilled:

3> consider the applicable cell, associated to that *condReconfigId*, as a triggered cell;

3> initiate the conditional reconfiguration execution, as specified in 5.3.5.13.5;

NOTE 1: Up to 2 *MeasId* can be configured for each *condReconfigId.* The conditional reconfiguration event of the 2 *MeasId* may have the same or different event conditions, triggering quantity, time to trigger, and triggering threshold.

NOTE 2: Void.

##### 5.3.5.13.4a Conditional reconfiguration evaluation of SN initiated inter-SN CPC for EN-DC

The UE shall:

1> for each *condReconfigurationId* within the *VarConditionalReconfiguration* specified in TS 36.331[10]:

2> for each *measId* included in the *measIdList* within *VarMeasConfig* indicated in the *CondReconfigExecCondSCG* contained in the *triggerConditionSN* associated to the *condReconfigurationId* as specified in TS 36.331[10]:

3> if the entry condition(s) applicable for the event associated with that *measId*, is fulfilled for the applicable cells for all measurements after layer 3 filtering taken during the corresponding *timeToTrigger* defined for this event associated with that *measId*:

4> consider this event to be fulfilled;

3> if the *measId* for this event has been modified; or

3> if the leaving condition(s) applicable for this event associated with that *measId*, is fulfilled for the applicable cells for all measurements after layer 3 filtering taken during the corresponding *timeToTrigger* defined for this event associated with that *measId*:

4> consider this event associated to that *measId* to be not fulfilled;

2> if trigger conditions for all events associated with the *measId(s)* indicated in the *CondReconfigExecCondSCG* contained in the *triggerConditionSN* as specified in TS 36.331[10]), are fulfilled:

3> consider the target cell candidate within the *RRCReconfiguration* message contained in *nr-SecondaryCellGroupConfig* in the *RRCConnectionReconfiguration* message, as specified in TS 36.331[10], contained in the stored *condReconfigurationToApply*, associated to that *condReconfigurationId* as specified in TS 36.331[10]), clause 5.3.5.9.4, as a triggered cell;

3> initiate the conditional reconfiguration execution, as specified in TS 36.331[10]), clause 5.3.5.9.5;

NOTE: Void.

##### 5.3.5.13.5 Conditional reconfiguration execution

The UE shall:

1> if more than one triggered cell exists:

2> select one of the triggered cells as the selected cell for conditional reconfiguration execution;

1> else:

2> consider the triggered cell as the selected cell for conditional reconfiguration execution;

1> for the selected cell of conditional reconfiguration execution:

2> apply the stored *condRRCReconfig* of the selected cell and perform the actions as specified in 5.3.5.3;

NOTE: If multiple NR cells are triggered in conditional reconfiguration execution, it is up to UE implementation which one to select, e.g. the UE considers beams and beam quality to select one of the triggered cells for execution.

*Editor’s Note: FFS on whether to rely on the full configuration procedure as specified in 5.3.5.11 or new complete configuration procedure when the UE applies a complete configuration.*

*Editor’s Note: FFS whether to restrict full configuration flag for subsequent CPAC candidate configuration if complete configuration procedure is used.*

*Editor’s Note: FFS whether to have separate handling on execution for MN configured and SN configured subsequent CPAC.*

##### 5.3.5.13.x1 Reference configuration addition/removal

The UE shall:

1> if the *scpac-ReferenceConfiguration* is set to *setup*:

2> if *SCPAC-ReferenceConfiguration* exists within the *VarConditionalReconfig*:

3> replace the *SCPAC-ReferenceConfiguration* within the *VarConditionalReconfig*;

2> else:

3> store the *SCPAC-ReferenceConfiguration* within the *VarConditionalReconfig*;

1> else:

2> remove the *SCPAC-ReferenceConfiguration* within the *VarConditionalReconfig*;

##### 5.3.5.13.x2 sk-CounterList addition/modification/removal

The UE shall:

1> for each *securityCellSetID* received in the *sk-CounterConfigToAddModList* IE:

2> if an entry with the matching *securityCellSetID* exists in the *sk-CounterConfigToAddModList* within the *VarConditionalReconfig*:

3> replace the *sk-CounterList* within the *VarConditionalReconfig* with the value received for this *securityCellSetID*;

2> else:

3> add a new entry for this *securityCellSetID* within the *VarConditionalReconfig*;

1> for each *securityCellSetID* value included in the *sk-CounterConfigToRemoveList* that is part of the current *sk-CounterConfigToAddModList* in *VarConditionalReconfig*:

2> remove the entry with the matching *securityCellSetID* from the *sk-CounterConfigToAddModList*;

*Editor’s Note: FFS on the how to update/release the sk-counters.*

### 5.3.7 RRC connection re-establishment

#### 5.3.7.1 General



Figure 5.3.7.1-1: RRC connection re-establishment, successful



Figure 5.3.7.1-2: RRC re-establishment, fallback to RRC establishment, successful

The purpose of this procedure is to re-establish the RRC connection. A UE in RRC\_CONNECTED, for which AS security has been activated with SRB2 and at least one DRB/multicast MRB setup or, for IAB, SRB2, may initiate the procedure in order to continue the RRC connection. The connection re-establishment succeeds if the network is able to find and verify a valid UE context or, if the UE context cannot be retrieved, and the network responds with an *RRCSetup* according to clause 5.3.3.4.

The network applies the procedure e.g as follows:

- When AS security has been activated and the network retrieves or verifies the UE context:

- to re-activate AS security without changing algorithms;

- to re-establish and resume the SRB1;

- When UE is re-establishing an RRC connection, and the network is not able to retrieve or verify the UE context:

- to discard the stored AS Context and release all RBs and BH RLC channels and Uu Relay RLC channels;

- to fallback to establish a new RRC connection.

If AS security has not been activated, the UE shall not initiate the procedure but instead moves to RRC\_IDLE directly, with release cause 'other'. If AS security has been activated, but SRB2 and at least one DRB or multicast MRB or, for IAB, SRB2, are not setup, the UE does not initiate the procedure but instead moves to RRC\_IDLE directly, with release cause 'RRC connection failure'.

#### 5.3.7.2 Initiation

The UE initiates the procedure when one of the following conditions is met:

1> upon detecting radio link failure of the MCG and *t316* is not configured, in accordance with 5.3.10; or

1> upon detecting radio link failure of the MCG while SCG transmission is suspended, in accordance with 5.3.10; or

1> upon detecting radio link failure of the MCG while PSCell change or PSCell addition is ongoing, in accordance with 5.3.10; or

1> upon detecting radio link failure of the MCG while the SCG is deactivated, in accordance with 5.3.10; or

1> upon re-configuration with sync failure of the MCG, in accordance with clause 5.3.5.8.3; or

1> upon mobility from NR failure, in accordance with clause 5.4.3.5; or

1> upon integrity check failure indication from lower layers concerning SRB1 or SRB2, except if the integrity check failure is detected on the *RRCReestablishment* message; or

1> upon an RRC connection reconfiguration failure, in accordance with clause 5.3.5.8.2; or

1> upon detecting radio link failure for the SCG while MCG transmission is suspended, in accordance with clause 5.3.10.3 in NR-DC or in accordance with TS 36.331 [10] clause 5.3.11.3 in NE-DC; or

1> upon reconfiguration with sync failure of the SCG while MCG transmission is suspended in accordance with clause 5.3.5.8.3; or

1> upon SCG change failure while MCG transmission is suspended in accordance with TS 36.331 [10] clause 5.3.5.7a; or

1> upon SCG configuration failure while MCG transmission is suspended in accordance with clause 5.3.5.8.2 in NR-DC or in accordance with TS 36.331 [10] clause 5.3.5.5 in NE-DC; or

1> upon integrity check failure indication from SCG lower layers concerning SRB3 while MCG is suspended; or

1> upon T316 expiry, in accordance with clause 5.7.3b.5; or

1> upon detecting sidelink radio link failure by L2 U2N Remote UE in RRC\_CONNECTED, in accordance with clause 5.8.9.3; or

1> upon reception of *NotificationMessageSidelink* including *indicationType* by L2 U2N Remote UE in RRC\_CONNECTED, in accordance with clause 5.8.9.10; or

1> upon PC5 unicast link release indicated by upper layer at L2 U2N Remote UE in RRC\_CONNECTED while T301 is not running.

NOTE 0: It is up to UE implementation whether to initiate the procedure while T346g is running.

Upon initiation of the procedure, the UE shall:

1> stop timer T310, if running;

1> stop timer T312, if running;

1> stop timer T304, if running;

1> start timer T311;

1. stop timer T316, if running;

1> for each *measId* of the MCG *measConfig*, if configured, and for each *measId* of the SCG *measConfig*, if configured, if the associated *reportConfig* has a *reportType* set to *condTriggerConfig*:

2> if the *reportConfigId* is associated the *measId* indicated by the *condExecutionCond* or the *condExecutionCondSCG* in an entry of *condReconfigList* in *VarConditionalReconfig* in which *subsequentCondReconfig* is included; or

2> if the *reportConfigId* is associated with the *measId* indicated by the *condExecutionCond* or the *condExecutionCondSCG* in an entry of *subsequentCondReconfig* in an entry of *condReconfigList* in *VarConditionalReconfig*:

3> remove the entry with the matching *reportConfigId* from the *reportConfigList* within the *VarMeasConfig*;

2> if the associated *measObjectId* is only associated to a *reportConfig* with *reportType* set to *condTriggerConfig*:

3> if the *measObjectId* is associated with the *measId* indicated by the *condExecutionCond* or the *condExecutionCondSCG* in an entry of *condReconfigList* in *VarConditionalReconfig* in which *subsequentCondReconfig* is included; or

3> if the *measObjectId* is associated with the *measId* indicated by the *condExecutionCond* or the condExecutionCondSCG in an entry of *subsequentCondReconfig* in an entry of *condReconfigList* in *VarConditionalReconfig*:

4> remove the entry with the matching *measObjectId* from the *measObjectList* within the *VarMeasConfig*;

2> remove the entry with the matching *measId* from the *measIdList* within the *VarMeasConfig*;

1> remove all the entries within the *VarServingSecurityCellSetID*, if any;

1> if UE is not configured with *attemptCondReconfig*:

2> reset MAC;

2> release *spCellConfig*, if configured;

2> suspend all RBs, and BH RLC channels for IAB-MT, and Uu Relay RLC channels for L2 U2N Relay UE, except SRB0 and broadcast MRBs;

2> release the MCG SCell(s), if configured;

2> if MR-DC is configured:

3> perform MR-DC release, as specified in clause 5.3.5.10;

2> release *delayBudgetReportingConfig*, if configured and stop timer T342, if running;

2> release *overheatingAssistanceConfig*, if configured and stop timer T345, if running;

2> release *idc-AssistanceConfig*, if configured;

2> release *btNameList*, if configured;

2> release *wlanNameList*, if configured;

2> release *sensorNameList*, if configured;

2> release *drx-PreferenceConfig* for the MCG, if configured and stop timer T346a associated with the MCG, if running;

2> release *maxBW-PreferenceConfig* for the MCG, if configured and stop timer T346b associated with the MCG, if running;

2> release *maxCC-PreferenceConfig* for the MCG, if configured and stop timer T346c associated with the MCG, if running;

2> release *maxMIMO-LayerPreferenceConfig* for the MCG, if configured and stop timer T346d associated with the MCG, if running;

2> release *minSchedulingOffsetPreferenceConfig* for the MCG, if configured stop timer T346e associated with the MCG, if running;

2> release *rlm-RelaxationReportingConfig* for the MCG, if configured and stop timer T346j associated with the MCG, if running;

2> release *bfd-RelaxationReportingConfig* for the MCG, if configured and stop timer T346k associated with the MCG, if running;

2> release *releasePreferenceConfig*, if configured stop timer T346f, if running;

2> release *onDemandSIB-Request* if configured, and stop timer T350, if running;

2> release *referenceTimePreferenceReporting*, if configured;

2> release *sl-AssistanceConfigNR*, if configured;

2> release *obtainCommonLocation*, if configured;

2> release *musim-GapAssistanceConfig*, if configured and stop timer T346h, if running;

2> release *musim-LeaveAssistanceConfig*, if configured;

2> release*ul-GapFR2-PreferenceConfig*, if configured;

2> release *scg-DeactivationPreferenceConfig*, if configured, and stop timer T346i, if running;

2> release *propDelayDiffReportConfig*, if configured;

2> release *rrm-MeasRelaxationReportingConfig*, if configured;

2> release *maxBW-PreferenceConfigFR2-2*, if configured;

2> release *maxMIMO-LayerPreferenceConfigFR2-2*, if configured;

2> release *minSchedulingOffsetPreferenceConfigExt*, if configured;

1> release *successHO-Config*, if configured;

1> if any DAPS bearer is configured:

2> reset the source MAC and release the source MAC configuration;

2> for each DAPS bearer:

3> release the RLC entity or entities as specified in TS 38.322 [4], clause 5.1.3, and the associated logical channel for the source SpCell;

3> reconfigure the PDCP entity to release DAPS as specified in TS 38.323 [5];

2> for each SRB:

3> release the PDCP entity for the source SpCell;

3> release the RLC entity as specified in TS 38.322 [4], clause 5.1.3, and the associated logical channel for the source SpCell;

2> release the physical channel configuration for the source SpCell;

2> discard the keys used in the source SpCell (the KgNB key, the KRRCenc key, the KRRCint key, the KUPint key and the KUPenc key), if any;

1> release *sl-L2RelayUE-Config*, if configured;

1> release *sl-L2RemoteUE-Config*, if configured;

1> release the SRAP entity, if configured;

1> if the UE is acting as L2 U2N Remote UE:

2> if the PC5-RRC connection with the U2N Relay UE is determined to be released:

3> indicate upper layers to trigger PC5 unicast link release;

3> perform either cell selection in accordance with the cell selection process as specified in TS 38.304 [20], or relay selection as specified in clause 5.8.15.3, or both;

2> else (i.e., maintain the PC5 RRC connection):

3> consider the connected L2 U2N Relay UE as suitable and perform actions as specified in clause 5.3.7.3a;

NOTE 1: It is up to Remote UE implementation whether to release or keep the current PC5 unicast link.

1> else:

2> if the UE is capable of L2 U2N Remote UE:

3> perform either cell selection as specified in TS 38.304 [20], or relay selection as specified in clause 5.8.15.3, or both;

2> else:

3> perform cell selection in accordance with the cell selection process as specified in TS 38.304 [20].

NOTE 2: For L2 U2N Remote UE, if both a suitable cell and a suitable relay are available, the UE can select either one based on its implementation.

#### 5.3.7.3 Actions following cell selection while T311 is running

Upon selecting a suitable NR cell, the UE shall:

1> ensure having valid and up to date essential system information as specified in clause 5.2.2.2;

1> stop timer T311;

1> if T390 is running:

2> stop timer T390 for all access categories;

2> perform the actions as specified in 5.3.14.4;

1> stop the relay (re)selection procedure, if ongoing;

1> if the cell selection is triggered by detecting radio link failure of the MCG or re-configuration with sync failure of the MCG or mobility from NR failure, and

1> if *attemptCondReconfig* is configured; and

1> if the selected cell is not configured with *CondEventT1*, or the selected cell is configured with *CondEventT1* and leaving condition has not been fulfilled; and

1> if the selected cell is one of the candidate cells for which the *reconfigurationWithSync* is included in the *masterCellGroup* in the MCG *VarConditionalReconfig*:

2> if the UE supports RLF-Report for conditional handover, set the *choCellId* in the *VarRLF-Report* to the global cell identity, if available, otherwise to the physical cell identity and carrier frequency of the selected cell;

2> apply the stored *condRRCReconfig* associated to the selected cell and perform actions as specified in 5.3.5.3;

NOTE 1: It is left to network implementation to how to avoid keystream reuse in case of CHO based recovery after a failed handover without key change.

1> else:

2> if UE is configured with *attemptCondReconfig*:

3> reset MAC;

3> release *spCellConfig*, if configured;

3> release the MCG SCell(s), if configured;

3> release *delayBudgetReportingConfig*, if configured and stop timer T342, if running;

3> release *overheatingAssistanceConfig* , if configured and stop timer T345, if running;

3> if MR-DC is configured:

4> perform MR-DC release, as specified in clause 5.3.5.10;

3> release *idc-AssistanceConfig*, if configured;

3> release *btNameList*, if configured;

3> release *wlanNameList*, if configured;

3> release *sensorNameList*, if configured;

3> release *drx-PreferenceConfig* for the MCG, if configured and stop timer T346a associated with the MCG, if running;

3> release *maxBW-PreferenceConfig* for the MCG, if configured and stop timer T346b associated with the MCG, if running;

3> release *maxCC-PreferenceConfig* for the MCG, if configured and stop timer T346c associated with the MCG, if running;

3> release *maxMIMO-LayerPreferenceConfig* for the MCG, if configured and stop timer T346d associated with the MCG, if running;

3> release *minSchedulingOffsetPreferenceConfig* for the MCG, if configured and stop timer T346e associated with the MCG, if running;

3> release *rlm-RelaxationReportingConfig* for the MCG, if configured and stop timer T346j associated with the MCG, if running;

3> release *bfd-RelaxationReportingConfig* for the MCG, if configured and stop timer T346k associated with the MCG, if running;

3> release *releasePreferenceConfig*, if configured and stop timer T346f, if running;

3> release *onDemandSIB-Request* if configured, and stop timer T350, if running;

3> release referenceTimePreferenceReporting, if configured;

3> release *sl-AssistanceConfigNR*, if configured;

3> release *obtainCommonLocation*, if configured;

3> release *scg-DeactivationPreferenceConfig*, if configured, and stop timer T346i, if running;

3> release *musim-GapAssistanceConfig*, if configured and stop timer T346h, if running;

3> release *musim-LeaveAssistanceConfig*, if configured;

3> release *propDelayDiffReportConfig*, if configured;

3> release *ul-GapFR2-PreferenceConfig*, if configured;

3> release *rrm-MeasRelaxationReportingConfig*, if configured;

3> release *maxBW-PreferenceConfigFR2-2*, if configured;

3> release *maxMIMO-LayerPreferenceConfigFR2-2*, if configured;

3> release *minSchedulingOffsetPreferenceConfigExt*, if configured;

3> suspend all RBs, and BH RLC channels for the IAB-MT, except SRB0 and broadcast MRBs;

2> remove all the entries within the MCG *VarConditionalReconfig*, if any;

2> for each *measId*, if the associated *reportConfig* has a *reportType* set to *condTriggerConfig*:

3> for the associated *reportConfigId*:

4> remove the entry with the matching *reportConfigId* from the *reportConfigList* within the *VarMeasConfig*;

3> if the associated *measObjectId* is only associated to a *reportConfig* with *reportType* set to *condTriggerConfig*:

4> remove the entry with the matching *measObjectId* from the *measObjectList* within the *VarMeasConfig*;

3> remove the entry with the matching *measId* from the *measIdList* within the *VarMeasConfig*;

2> release the PC5 RLC entity for SL-RLC0, if any;

2> start timer T301;

2> apply the default L1 parameter values as specified in corresponding physical layer specifications except for the parameters for which values are provided in *SIB1*;

2> apply the default MAC Cell Group configuration as specified in 9.2.2;

2> apply the CCCH configuration as specified in 9.1.1.2;

2> apply the *timeAlignmentTimerCommon* included in *SIB1*;

2> initiate transmission of the *RRCReestablishmentRequest* message in accordance with 5.3.7.4;

NOTE 2: This procedure applies also if the UE returns to the source PCell.

Upon selecting an inter-RAT cell, the UE shall:

1> perform the actions upon going to RRC\_IDLE as specified in 5.3.11, with release cause 'RRC connection failure'.

5.3.8.3 Reception of the *RRCRelease* by the UE

The UE shall:

1> delay the following actions defined in this clause 60 ms from the moment the *RRCRelease* message was received or optionally when lower layers indicate that the receipt of the *RRCRelease* message has been successfully acknowledged, whichever is earlier;

1> stop timer T380, if running;

1> stop timer T320, if running;

1> if timer T316 is running;

2> stop timer T316;

2> clear the information included in *VarRLF-Report,* if any;

1> stop timer T350, if running;

1> stop timer T346g, if running;

1> if theAS security is not activated:

2> ignore any field included in *RRCRelease* message except *waitTime*;

2> perform the actions upon going to RRC\_IDLE as specified in 5.3.11 with the release cause 'other' upon which the procedure ends;

1> if the *RRCRelease* message includes *redirectedCarrierInfo* indicating redirection to *eutra*:

2> if *cnType* is included:

3> after the cell selection, indicate the available CN Type(s) and the received *cnType* to upper layers;

NOTE 1: Handling the case if the E-UTRA cell selected after the redirection does not support the core network type specified by the *cnType,* is up to UE implementation.

2> if *voiceFallbackIndication* is included:

3> consider the RRC connection release was for EPS fallback for IMS voice (see TS 23.502 [43]);

1> if the *RRCRelease* message includes the *cellReselectionPriorities*:

2> store the cell reselection priority information provided by the *cellReselectionPriorities*;

2> if the *t320* is included:

3> start timer T320, with the timer value set according to the value of *t320*;

1> else:

2> apply the cell reselection priority information broadcast in the system information;

1> if *deprioritisationReq* is included and the UE supports RRC connection release with deprioritisation:

2> start or restart timer T325 with the timer value set to the *deprioritisationTimer* signalled;

2> store the *deprioritisationReq* until T325 expiry;

NOTE 1a: The UE stores the deprioritisation request irrespective of any cell reselection absolute priority assignments (by dedicated or common signalling) and regardless of RRC connections in NR or other RATs unless specified otherwise.

1> if the *RRCRelease* includes the *measIdleConfig*:

2> if T331 is running:

3> stop timer T331;

3> perform the actions as specified in 5.7.8.3;

2> if the *measIdleConfig* is set to *setup*:

3> store the received *measIdleDuration* in *VarMeasIdleConfig*;

3> start timer T331 with the value set to *measIdleDuration*;

3> if the *measIdleConfig* contains *measIdleCarrierListNR*:

4> store the received *measIdleCarrierListNR* in *VarMeasIdleConfig*;

3> if the *measIdleConfig* contains *measIdleCarrierListEUTRA*:

4> store the received *measIdleCarrierListEUTRA* in *VarMeasIdleConfig*;

3> if the *measIdleConfig* contains *validityAreaList*:

4> store the received *validityAreaList* in *VarMeasIdleConfig*;

1> if the *RRCRelease* includes *suspendConfig*:

2> reset MAC and release the default MAC Cell Group configuration, if any;

2> apply the received *suspendConfig* except the received *nextHopChainingCount*;

2> if the *sdt-Config* is configured:

3> for each of the DRB in the *sdt-DRB-List*:

4> consider the DRB to be configured for SDT;

3> if *sdt-SRB2-Indication* is configured:

4> consider the SRB2 to be configured for SDT;

3> for each RLC bearer (except those associated with broadcast MRBs) that is not suspended:

4> re-establish the RLC entity as specified in TS 38.322 [4];

3> for SRB2 (if it is resumed) and for SRB1:

4> trigger the PDCP entity to perform SDU discard as specified in TS 38.323 [5];

3> if *sdt-MAC-PHY-CG-Config* is configured:

4> configure the PCell with the configured grant resources for SDT and instruct the MAC entity to start the *cg-SDT-TimeAlignmentTimer*;

2> if *srs-PosRRC-Inactive* is configured:

3> apply the configuration and instruct MAC to start the *inactivePosSRS-TimeAlignmentTimer*;

NOTE 1b: The Network should provide full configuration to UE for SRS for Positioning in RRC\_INACTIVE.

2> remove all the entries within the MCG and the SCG *VarConditionalReconfig*, if any;

2> remove all the entries within the *VarServingSecurityCellSetID*, if any;

2> for each *measId* of the MCG *measConfig* and for each *measId* of the SCG *measConfig*, if configured, if the associated *reportConfig* has a *reportType* set to *condTriggerConfig*:

3> for the associated *reportConfigId*:

4> remove the entry with the matching *reportConfigId* from the *reportConfigList* within the *VarMeasConfig*;

3> if the associated *measObjectId* is only associated to a *reportConfig* with *reportType* set to *condTriggerConfig*:

4> remove the entry with the matching *measObjectId* from the *measObjectList* within the *VarMeasConfig*;

3> remove the entry with the matching *measId* from the *measIdList* within the *VarMeasConfig*;

2> if the UE is acting as L2 U2N Remote UE:

3> if the PC5-RRC connection with the U2N Relay UE is determined to be released:

4> indicate upper layers to trigger PC5 unicast link release;

3> else (i.e., maintain the PC5 RRC connection):

4> establish or re-establish (e.g. via release and add) SL RLC entity for SRB1;

2> else:

3> re-establish RLC entities for SRB1;

2> if the *RRCRelease* message with *suspendConfig* was received in response to an *RRCResumeRequest* or an *RRCResumeRequest1*:

3> stop the timer T319 if running;

3> in the stored UE Inactive AS context:

4> replace the KgNB and KRRCint keys with the current KgNB and KRRCint keys;

4> replace the *nextHopChainingCount* with the value of *nextHopChainingCount* received in the *RRCRelease* message*;*

4> replace the *cellIdentity* with the *cellIdentity* of the cell the UE has received the *RRCRelease* message;

4> if the *suspendConfig* contains the *sl-UEIdentityRemote* (i.e. the UE is a L2 U2N Remote UE):

5> replace the C-RNTI with the value of the *sl-UEIdentityRemote*;

5> replace the physical cell identitywith the value of the *sl-PhysCellId* in *sl-ServingCellInfo* contained in the discovery message received from the connected L2 U2N Relay UE;

4> else:

5> replace the C-RNTI with the C-RNTI used in the cell (see TS 38.321 [3]) the UE has received the *RRCRelease* message;

5> replace the physical cell identitywith the physical cell identity of the cell the UE has received the *RRCRelease* message;

3> replace the *nextHopChainingCount* with the value associated with the current KgNB;

3> stop the timer T319a if running and consider SDT procedure is not ongoing;

2> else:

3> store in the UE Inactive AS Context the *nextHopChainingCount* received in the *RRCRelease* message*,* the current KgNB and KRRCint keys, the ROHC state, the EHC context(s), the UDC state, the stored QoS flow to DRB mapping rules, the application layer measurement configuration, the C-RNTI used in the source PCell, the *cellIdentity* and the physical cell identity of the source PCell, the *spCellConfigCommon* within *ReconfigurationWithSync* of the NR PSCell (if configured) and all other parameters configured except for:

- parameters within *ReconfigurationWithSync* of the PCell;

- parameters within *ReconfigurationWithSync* of the NR PSCell, if configured;

- parameters within *MobilityControlInfoSCG* of the E-UTRA PSCell, if configured;

- *servingCellConfigCommonSIB*;

- *sl-L2RelayUE-Config*, if configured;

- *sl-L2RemoteUE-Config*, if configured;

NOTE 1c: *suspendConfig* is not stored as part of UE Inactive AS Context, except for the fields explicitly specified.

3> store any previously or subsequently received application layer measurement report containers for which no segment, or full message, has been submitted to lower layers for transmission;

NOTE 2: NR sidelink communication/discovery related configurations and logged measurement configuration are not stored as UE Inactive AS Context, when UE enters RRC\_INACTIVE.

2> suspend all SRB(s) and DRB(s) and multicast MRB(s), except SRB0 and broadcast MRBs;

2> indicate PDCP suspend to lower layers of all DRBs and multicast MRBs;

2> release Uu Relay RLC channel(s), if configured;

2> release PC5 Relay RLC channel(s), if configured;

2> release the SRAP entity, if configured;

NOTE 2a: A L2 U2N Relay UE may re-establish the SL-RLC0, SL-RLC1 and SRAP entity after release.

2> if the *t380* is included:

3> start timer T380, with the timer value set to *t380*;

2> if the *RRCRelease* message is including the *waitTime*:

3> start timer T302 with the value set to the *waitTime*;

3> inform upper layers that access barring is applicable for all access categories except categories '0' and '2';

2> if T390 is running:

3> stop timer T390 for all access categories;

3> perform the actions as specified in 5.3.14.4;

2> indicate the suspension of the RRC connection to upper layers;

2> if the UE is capable of L2 U2N Remote UE:

3> enter RRC\_INACTIVE, and perform either cell selection as specified in TS 38.304 [20], or relay selection as specified in clause 5.8.15.3, or both;

2> else:

3> enter RRC\_INACTIVE and perform cell selection as specified in TS 38.304 [20];

1> else:

2> perform the actions upon going to RRC\_IDLE as specified in 5.3.11, with the release cause 'other'.

NOTE 3: Whether to release the PC5 unicast link is left to L2 U2N Remote UE's implementation.

NOTE 4: It is left to UE implementation whether to stop T430, if running, when going to RRC\_INACTIVE.

5.3.11 UE actions upon going to RRC\_IDLE

The UE shall:

1> reset MAC;

1> set the variable *pendingRNA-Update* to *false*, if that is set to *true*;

1> if going to RRC\_IDLE was triggered by reception of the *RRCRelease* message including a *waitTime*:

2> if T302 is running:

3> stop timer T302;

2> start timer T302 with the value set to the *waitTime*;

2> inform upper layers that access barring is applicable for all access categories except categories '0' and '2'.

1> else:

2> if T302 is running:

3> stop timer T302;

3> perform the actions as specified in 5.3.14.4;

1> if T390 is running:

2> stop timer T390 for all access categories;

2> perform the actions as specified in 5.3.14.4;

1> if the UE is leaving RRC\_INACTIVE:

2> if going to RRC\_IDLE was not triggered by reception of the *RRCRelease message*:

3> if stored, discard the cell reselection priority information provided by the *cellReselectionPriorities*;

3> stop the timer T320, if running;

2> if T319a is running:

3> stop timer T319a;

3> consider SDT procedure is not ongoing;

1> stop all timers that are running except T302, T320, T325, T330, T331, T400 and T430;

1> discard the UE Inactive AS context, if any;

1> release the *suspendConfig*, if configured;

1> remove all the entries within the MCG and the SCG *VarConditionalReconfig*, if any;

1> remove all the entries within the *VarServingSecurityCellSetID*, if any;

1> for each *measId*, if the associated *reportConfig* has a *reportType* set to *condTriggerConfig*:

2> for the associated *reportConfigId*:

3> remove the entry with the matching *reportConfigId* from the *reportConfigList* within the *VarMeasConfig*;

2> if the associated *measObjectId* is only associated to a *reportConfig* with *reportType* set to *condTriggerConfig*:

3> remove the entry with the matching *measObjectId* from the *measObjectList* within the *VarMeasConfig*;

2> remove the entry with the matching *measId* from the *measIdList* within the *VarMeasConfig*;

1> discard the KgNB key, the S-KgNB key, the S-KeNB key, the KRRCenc key, the KRRCint key, the KUPint key and the KUPenc key, if any;

1> release all radio resources, including release of the RLC entity, the BAP entity, the MAC configuration and the associated PDCP entity and SDAP for all established RBs (except for broadcast MRBs), BH RLC channels, Uu Relay RLC channels, PC5 Relay RLC channels and SRAP entity;

NOTE 0: A L2 U2N Relay UE may re-establish the SL-RLC0, SL-RLC1 and SRAP entity after release.

1> indicate the release of the RRC connection to upper layers together with the release cause;

1> inform upper layers about the release of all application layer measurement configurations;

1> discard any application layer measurement reports which were not yet submitted to lower layers for transmission;

1> discard any segments of segmented RRC messages stored according to 5.7.6.3;

1> except if going to RRC\_IDLE was triggered by inter-RAT cell reselection while the UE is in RRC\_INACTIVE or RRC\_IDLE or when selecting an inter-RAT cell while T311 was running or when selecting an E-UTRA cell for EPS fallback for IMS voice as specified in 5.4.3.5:

2> if the UE is capable of L2 U2N Remote UE:

3> enter RRC\_IDLE, and perform either cell selection as specified in TS 38.304 [20], or relay selection as specified in clause 5.8.15.3, or both;

2> else:

3> enter RRC\_IDLE and perform cell selection as specified in TS 38.304 [20];

NOTE 1: Whether to release the PC5 unicast link is left to L2 U2N Remote UE's implementation.

NOTE 2: It is left to UE implementation whether to stop T430, if running, when going to RRC\_IDLE.

### 5.5.3 Performing measurements

5.5.3.1 General

An RRC\_CONNECTED UE shall derive cell measurement results by measuring one or multiple beams associated per cell as configured by the network, as described in 5.5.3.3. For all cell measurement results, except for RSSI, and CLI measurement results in RRC\_CONNECTED, the UE applies the layer 3 filtering as specified in 5.5.3.2, before using the measured results for evaluation of reporting criteria, measurement reporting or the criteria to trigger conditional reconfiguration execution. For cell measurements, the network can configure RSRP, RSRQ, SINR, RSCP or EcN0 as trigger quantity. For CLI measurements, the network can configure SRS-RSRP or CLI-RSSI as trigger quantity. For cell and beam measurements, reporting quantities can be any combination of quantities (i.e. only RSRP; only RSRQ; only SINR; RSRP and RSRQ; RSRP and SINR; RSRQ and SINR; RSRP, RSRQ and SINR; only RSCP; only EcN0; RSCP and EcN0), irrespective of the trigger quantity, and for CLI measurements, reporting quantities can be either SRS-RSRP or CLI-RSSI. For conditional reconfiguration execution, the network can configure up to 2 quantities, both using same RS type. The UE does not apply the layer 3 filtering as specified in 5.5.3.2 to derive the CBR measurements. The UE does not apply the layer 3 filtering as specified in 5.5.3.2 to derive the Rx-Tx time difference measurements.

The network may also configure the UE to report measurement information per beam (which can either be measurement results per beam with respective beam identifier(s) or only beam identifier(s)), derived as described in 5.5.3.3a. If beam measurement information is configured to be included in measurement reports, the UE applies the layer 3 beam filtering as specified in 5.5.3.2. On the other hand, the exact L1 filtering of beam measurements used to derive cell measurement results is implementation dependent.

The UE shall:

1> whenever the UE has a *measConfig*, perform RSRP and RSRQ measurements for each serving cell for which *servingCellMO* is configured as follows:

2> if the *reportConfig* associated with at least one *measId* included in the *measIdList* within *VarMeasConfig* contains an *rsType* set to *ssb* and *ssb-ConfigMobility* is configured in the *measObject* indicated by the *servingCellMO*:

3> if the *reportConfig* associated with at least one *measId* included in the *measIdList* within *VarMeasConfig* contains a *reportQuantityRS-Indexes* and *maxNrofRS-IndexesToReport* and contains an *rsType* set to *ssb*:

4> derive layer 3 filtered RSRP and RSRQ per beam for the serving cell based on SS/PBCH block, as described in 5.5.3.3a;

3> derive serving cell measurement results based on SS/PBCH block, as described in 5.5.3.3;

2> if the *reportConfig* associated with at least one *measId* included in the *measIdList* within *VarMeasConfig* contains an *rsType* set to *csi-rs* and *CSI-RS-ResourceConfigMobility* is configured in the *measObject* indicated by the *servingCellMO*:

3> if the *reportConfig* associated with at least one *measId* included in the *measIdList* within *VarMeasConfig* contains a *reportQuantityRS-Indexes* and *maxNrofRS-IndexesToReport* and contains an *rsType* set to *csi-rs*:

4> derive layer 3 filtered RSRP and RSRQ per beam for the serving cell based on CSI-RS, as described in 5.5.3.3a;

3> derive serving cell measurement results based on CSI-RS, as described in 5.5.3.3;

1> for each serving cell for which *servingCellMO* is configured, if the *reportConfig* associated with at least one *measId* included in the *measIdList* within *VarMeasConfig* contains SINR as trigger quantity and/or reporting quantity:

2> if the *reportConfig* contains *rsType* set to *ssb* and *ssb-ConfigMobility* is configured in the *servingCellMO*:

3> if the *reportConfig*contains a *reportQuantityRS-Indexes* and *maxNrofRS-IndexesToReport*:

4> derive layer 3 filtered SINR per beam for the serving cell based on SS/PBCH block, as described in 5.5.3.3a;

3> derive serving cell SINR based on SS/PBCH block, as described in 5.5.3.3;

2> if the *reportConfig* contains *rsType* set to *csi-rs* and *CSI-RS-ResourceConfigMobility* is configured in the *servingCellMO*:

3> if the *reportConfig*contains a *reportQuantityRS-Indexes* and *maxNrofRS-IndexesToReport*:

4> derive layer 3 filtered SINR per beam for the serving cell based on CSI-RS, as described in 5.5.3.3a;

3> derive serving cell SINR based on CSI-RS, as described in 5.5.3.3;

1> for each *measId* included in the *measIdList* within *VarMeasConfig*:

2> if the *reportType* for the associated *reportConfig* is set to *reportCGI* and timer T321 is running:

3> if *useAutonomousGaps* is configured for the associated *reportConfig*:

4> perform the corresponding measurements on the frequency and RAT indicated in the associated *measObject* using autonomous gaps as necessary;

3> else:

4> perform the corresponding measurements on the frequency and RAT indicated in the associated *measObject* using available idle periods;

3> if the cell indicated by *reportCGI* field for the associated *measObject* is an NR cell and that indicated cell is broadcasting *SIB1* (see TS 38.213 [13], clause 13):

4> try to acquire *SIB1* in the concerned cell;

3> if the cell indicated by *reportCGI* field is an E-UTRA cell:

4> try to acquire *SystemInformationBlockType1* in the concerned cell;

2> if the *ul-DelayValueConfig* is configured for the associated *reportConfig*:

3> ignore the *measObject;*

3> for each of the configured DRBs*,* configure the PDCP layer to perform corresponding average UL PDCP packet delay measurement per DRB;

2> if the *ul-ExcessDelayConfig* is configured for the associated *reportConfig*:

3> ignore the *measObject;*

3> for each of the configured DRBs*,* configure the PDCP layer to perform corresponding UL PDCP Excess Packet Delay delay measurement according to the configured threshold per DRB;

2> if the *reportType* for the associated *reportConfig* is *periodical*, *eventTriggered*; or

2> if the *reportType* for the associated *reportConfig* is *condTriggerConfig,* the *measId* is within the MCG *VarMeasConfig* and is indicated in the *condExecutionCond* associated to a *condReconfigId* in the MCG *VarConditionalReconfig* (for CHO, CPA or MN-initiated inter-SN CPC in NR-DC); or

2> if the *reportType* for the associated *reportConfig* is *condTriggerConfig*, the *measId* is within the SCG *VarMeasConfig* and is indicated in the *condExecutionCond* associated to a *condReconfigId* in the SCG *VarConditionalReconfig* (for intra-SN CPC); or

2> if the *reportType* for the associated *reportConfig* is *condTriggerConfig*, the *measId* is within the SCG *VarMeasConfig* and is indicated in the *condExecutionCondSCG* associated to a *condReconfigId* in the MCG *VarConditionalReconfig* (for SN-initiated inter-SN CPC in NR-DC); or

2> if the *reportType* for the associated *reportConfig* is *condTriggerConfig*, the *measId* is within the SCG *VarMeasConfig* and is indicated in the *triggerConditionSN* associated to a *condReconfigurationId* in *VarConditionalReconfiguration* as specified in TS 36.331 [10] (for SN-initiated inter-SN CPC in EN-DC):

3> if a measurement gap configuration is setup, or

3> if the UE does not require measurement gaps to perform the concerned measurements:

4> if *s-MeasureConfig* is not configured, or

4> if *s-MeasureConfig* is set to *ssb-RSRP* and the NR SpCell RSRP based on SS/PBCH block, after layer 3 filtering, is lower than *ssb-RSRP,* or

4> if *s-MeasureConfig* is set to *csi-RSRP* and the NR SpCell RSRP based on CSI-RS, after layer 3 filtering, is lower than *csi-RSRP*:

5> if the *measObject* is associated to NR and the *rsType* is set to *csi-rs*:

6> if reportQuantityRS-Indexes and maxNrofRS-IndexesToReport for the associated reportConfig are configured:

7> derive layer 3 filtered beam measurements only based on CSI-RS for each measurement quantity indicated in *reportQuantityRS-Indexes*, as described in 5.5.3.3a;

6> derive cell measurement results based on CSI-RS for the trigger quantity and each measurement quantity indicated in *reportQuantityCell* using parameters from the associated *measObject*, as described in 5.5.3.3;

5> if the *measObject* is associated to NR and the *rsType* is set to *ssb*:

6> if reportQuantityRS-Indexes and maxNrofRS-IndexesToReport for the associated reportConfig are configured:

7> derive layer 3 beam measurements only based on SS/PBCH block for each measurement quantity indicated in *reportQuantityRS-Indexes*, as described in 5.5.3.3a;

6> derive cell measurement results based on SS/PBCH block for the trigger quantity and each measurement quantity indicated in *reportQuantityCell* using parameters from the associated *measObject*, as described in 5.5.3.3;

5> if the *measObject* is associated to E-UTRA:

6> perform the corresponding measurements associated to neighbouring cells on the frequencies indicated in the concerned *measObject*, as described in 5.5.3.2;

5> if the measObject is associated to UTRA-FDD:

6> perform the corresponding measurements associated to neighbouring cells on the frequencies indicated in the concerned *measObject*, as described in 5.5.3.2;

5> if the measObject is associated to L2 U2N Relay UE:

6> perform the corresponding measurements associated to candidate Relay UEs on the frequencies indicated in the concerned *measObject*, as described in 5.5.3.4;

4> if the *measRSSI-ReportConfig* is configured in the associated *reportConfig*:

5> perform the RSSI and channel occupancy measurements on the frequency configured by *rmtc-Frequency* in the associated *measObject*;

NOTE 0: The network avoids configuring UEs supporting only CHO and/or Rel-16 CPC with measurements not referred to by any execution condition.

2> if the *reportType* for the associated *reportConfig* is set to *reportSFTD* and the *numberOfReportsSent* as defined within the *VarMeasReportList* for this *measId* is less than one:

3> if the *reportSFTD-Meas* is set to *true:*

4> if the *measObject* is associated to E-UTRA:

5> perform SFTD measurements between the PCell and the E-UTRA PSCell;

5> if the *reportRSRP* is set to *true*;

6> perform RSRP measurements for the E-UTRA PSCell;

4> else if the *measObject* is associated to NR:

5> perform SFTD measurements between the PCell and the NR PSCell;

5> if the *reportRSRP* is set to *true*;

6> perform RSRP measurements for the NR PSCell based on SSB;

3> else if the *reportSFTD-NeighMeas* is included*:*

4> if the *measObject* is associated to NR:

5> if the *drx-SFTD-NeighMeas* is included:

6> perform SFTD measurements between the PCell and the NR neighbouring cell(s) detected based on parameters in the associated *measObject* using available idle periods;

5> else:

6> perform SFTD measurements between the PCell and the NR neighbouring cell(s) detected based on parameters in the associated *measObject*;

5> if the *reportRSRP* is set to *true*:

6> perform RSRP measurements based on SSB for the NR neighbouring cell(s) detected based on parameters in the associated *measObject*;

2> if the *reportType* for the associated *reportConfig* is *cli-Periodical* or *cli-EventTriggered*:

3> perform the corresponding measurements associated to CLI measurement resources indicated in the concerned *measObjectCLI*;

2> perform the evaluation of reporting criteria as specified in 5.5.4, except if *reportConfig* is *condTriggerConfig*.

The UE acting as a L2 U2N Remote UE whenever configured with *measConfig* shall:

1> perform the corresponding measurements associated to the serving L2 U2N Relay UE, as described in 5.5.3.4;

NOTE 1: The evaluation of conditional reconfiguration execution criteria is specified in 5.3.5.13.

The UE capable of Rx-Tx time difference measurement when configured with *measObjectRxTxDiff* shall:

1> perform the corresponding Rx-Tx time difference measurements associated with downlink reference signals indicated in the concerned *measObjectRxTxDiff*.

The UE capable of CBR measurement when configured to transmit NR sidelink communication/discovery shall:

1> If the frequency used for NR sidelink communication/discovery is included in *sl-FreqInfoToAddModList* in *sl-ConfigDedicatedNR* within *RRCReconfiguration* message or includedin *sl-ConfigCommonNR* within *SIB12*:

2> if the UE is in RRC\_IDLE or in RRC\_INACTIVE:

3> if configured with NR sidelink communication and the cell chosen for NR sidelink communication provides *SIB12* which includes *sl-TxPoolSelectedNormal* or *sl-TxPoolExceptional* forthe concerned frequency; or

3> if configured with NR sidelink discovery and the cell chosen for NR sidelink discovery provides *SIB12* which includes *sl-TxPoolSelectedNormal* or *sl-TxPoolExceptional* but does not include *sl-DiscTxPoolSelected* forthe concerned frequency:

4> perform CBR measurement on pool(s) in *sl-TxPoolSelectedNormal* or *sl-TxPoolExceptional* for the concerned frequency in *SIB12*;

3> if configured with NR sidelink discovery and the cell chosen for NR sidelink discovery provides *SIB12* which includes *sl-DiscTxPoolSelected* forthe concerned frequency:

4> perform CBR measurement on pools in *sl-DiscTxPoolSelected* and *sl-TxPoolExceptional* for the concerned frequency in *SIB12*;

2> if the UE is in RRC\_CONNECTED:

3> if *tx-PoolMeasToAddModList* is included in *VarMeasConfig*:

4> perform CBR measurements on each transmission resource pool indicated in the *tx-PoolMeasToAddModList*;

3> if *sl-DiscTxPoolSelected*, *sl-TxPoolSelectedNormal*, *sl-TxPoolScheduling* or *sl-TxPoolExceptional* is included in *sl-ConfigDedicatedNR* for the concerned frequency within *RRCReconfiguration*:

4> perform CBR measurement on pool(s) in *sl-DiscTxPoolSelected*, *sl-TxPoolSelectedNormal*, *sl-TxPoolScheduling* and *sl-TxPoolExceptional* if included in *sl-ConfigDedicatedNR* for the concerned frequency within *RRCReconfiguration*;

3> else:

4> if configured with NR sidelink communication and the cell chosen for NR sidelink communication provides *SIB12* which includes *sl-TxPoolSelectedNormal* or *sl-TxPoolExceptional* forthe concerned frequency; or

4> if configured with NR sidelink discovery and the cell chosen for NR sidelink discovery provides *SIB12* which includes *sl-TxPoolSelectedNormal* or *sl-TxPoolExceptional* but does not provide *sl-DiscTxPoolSelected* forthe concerned frequency:

5> perform CBR measurement on pool(s) in *sl-TxPoolSelectedNormal* or *sl-TxPoolExceptional* for the concerned frequency in *SIB12*;

4> if configured with NR sidelink discovery and the cell chosen for NR sidelink discovery provides *SIB12* which includes *sl-DiscTxPoolSelected* forthe concerned frequency:

5> perform CBR measurement on pools in *sl-DiscTxPoolSelected* and *sl-TxPoolExceptional* for the concerned frequency in *SIB12*;

1> else:

2> if configured with NR sidelink communication and *sl-TxPoolSelectedNormal* is included in *SidelinkPreconfigNR* for the concerned frequency; or

2> if configured with NR sidelink discovery and *sl-TxPoolSelectedNormal* is included in *SidelinkPreconfigNR* but *sl-DiscTxPoolSelected* is not included in *SidelinkPreconfigNR* for the concerned frequency:

3> perform CBR measurement on pool(s) in *sl-TxPoolSelectedNormal* in *SidelinkPreconfigNR* for the concerned frequency.

2> if configured with NR sidelink discovery and *sl-DiscTxPoolSelected* is included in *SidelinkPreconfigNR* for the concerned frequency:

3> perform CBR measurement on pools in *sl-DiscTxPoolSelected* if included in *SidelinkPreconfigNR*.

NOTE 2: In case the configurations for NR sidelink communication and CBR measurement are acquired via the E-UTRA, configurations for NR sidelink communication in *SIB12*, *sl-ConfigDedicatedNR* within *RRCReconfiguration* used in this clause are provided by the configurations in *SystemInformationBlockType28*, *sl-ConfigDedicatedForNR* within *RRCConnectionReconfiguration* as specified in TS 36.331[10], respectively.

NOTE 3: If a UE that is configured by upper layers to transmit V2X sidelink communication is configured by NR with transmission resource pool(s) and the measurement objects concerning V2X sidelink communication (i.e. by *sl-ConfigDedicatedEUTRA-Info*), it shall perform CBR measurement as specified in clause 5.5.3 of TS 36.331 [10], based on the transmission resource pool(s) and the measurement object(s) concerning V2X sidelink communication configured by NR.

NOTE 4: For V2X sidelink communication, each of the CBR measurement results is associated with a resource pool, as indicated by the *poolReportId* (see TS 36.331 [10]), that refers to a pool as included in *sl-ConfigDedicatedEUTRA-Info* or *SIB13*.

### 

6.2.2 Message definitions

*– RRCReconfigurationComplete*

The *RRCReconfigurationComplete* message is used to confirm the successful completion of an RRC connection reconfiguration.

Signalling radio bearer: SRB1 or SRB3

RLC-SAP: AM

Logical channel: DCCH

Direction: UE to Network

***RRCReconfigurationComplete message***

-- ASN1START

-- TAG-RRCRECONFIGURATIONCOMPLETE-START

RRCReconfigurationComplete ::= SEQUENCE {

rrc-TransactionIdentifier RRC-TransactionIdentifier,

criticalExtensions CHOICE {

rrcReconfigurationComplete RRCReconfigurationComplete-IEs,

criticalExtensionsFuture SEQUENCE {}

}

}

RRCReconfigurationComplete-IEs ::= SEQUENCE {

lateNonCriticalExtension OCTET STRING OPTIONAL,

nonCriticalExtension RRCReconfigurationComplete-v1530-IEs OPTIONAL

}

RRCReconfigurationComplete-v1530-IEs ::= SEQUENCE {

uplinkTxDirectCurrentList UplinkTxDirectCurrentList OPTIONAL,

nonCriticalExtension RRCReconfigurationComplete-v1560-IEs OPTIONAL

}

RRCReconfigurationComplete-v1560-IEs ::= SEQUENCE {

scg-Response CHOICE {

nr-SCG-Response OCTET STRING (CONTAINING RRCReconfigurationComplete),

eutra-SCG-Response OCTET STRING

} OPTIONAL,

nonCriticalExtension RRCReconfigurationComplete-v1610-IEs OPTIONAL

}

RRCReconfigurationComplete-v1610-IEs ::= SEQUENCE {

ue-MeasurementsAvailable-r16 UE-MeasurementsAvailable-r16 OPTIONAL,

needForGapsInfoNR-r16 NeedForGapsInfoNR-r16 OPTIONAL,

nonCriticalExtension RRCReconfigurationComplete-v1640-IEs OPTIONAL

}

RRCReconfigurationComplete-v1640-IEs ::= SEQUENCE {

uplinkTxDirectCurrentTwoCarrierList-r16 UplinkTxDirectCurrentTwoCarrierList-r16 OPTIONAL,

nonCriticalExtension RRCReconfigurationComplete-v1700-IEs OPTIONAL

}

RRCReconfigurationComplete-v1700-IEs ::= SEQUENCE {

needForGapNCSG-InfoNR-r17 NeedForGapNCSG-InfoNR-r17 OPTIONAL,

needForGapNCSG-InfoEUTRA-r17 NeedForGapNCSG-InfoEUTRA-r17 OPTIONAL,

selectedCondRRCReconfig-r17 CondReconfigId-r16 OPTIONAL,

nonCriticalExtension RRCReconfigurationComplete-v1720-IEs OPTIONAL

}

RRCReconfigurationComplete-v1720-IEs ::= SEQUENCE {

uplinkTxDirectCurrentMoreCarrierList-r17 UplinkTxDirectCurrentMoreCarrierList-r17 OPTIONAL,

nonCriticalExtension RRCReconfigurationComplete-v1800-IEs OPTIONAL

}

RRCReconfigurationComplete-v1800-IEs ::= SEQUENCE {

selectedSK-Counter-r18 SK-Counter OPTIONAL,

nonCriticalExtension SEQUENCE {} OPTIONAL

}

-- TAG-RRCRECONFIGURATIONCOMPLETE-STOP

-- ASN1STOP

|  |
| --- |
| ***RRCReconfigurationComplete-IEs* field descriptions** |
| ***needForGapsInfoNR***  This field is used to indicate the measurement gap requirement information of the UE for NR target bands. |
| ***needForGapNCSG-InfoEUTRA***  This field is used to indicate the measurement gap and NCSG requirement information of the UE for E‑UTRA target bands. |
| ***needForGapNCSG-InfoNR***  This field is used to indicate the measurement gap and NCSG requirement information of the UE for NR target bands. |
| ***scg-Response***  In case of NR-DC (*nr-SCG-Response*), this field includes the *RRCReconfigurationComplete* message. In case of NE-DC (*eutra-SCG-Response*), this field includes the E-UTRA *RRCConnectionReconfigurationComplete* message as specified in TS 36.331 [10]*.* |
| ***selectedCondRRCReconfig***  This field indicates the ID of the selected conditional reconfiguration the UE applied upon the execution of CPA or inter-SN CPC. |
| ***selectedSK-Counter***  This field includes the selected *SK-counter* value for security key update upon the execution of subsequent CPAC. |
| ***uplinkTxDirectCurrentList***  The Tx Direct Current locations for the configured serving cells and BWPs if requested by the NW (see *reportUplinkTxDirectCurrent* in *CellGroupConfig*). |
| ***uplinkTxDirectCurrentMoreCarrierList***  The Tx Direct Current locations for the configured intra-band CA requested by *reportUplinkTxDirectCurrentMoreCarrier-r17*. |
| ***uplinkTxDirectCurrentTwoCarrierList***  The Tx Direct Current locations for the configured uplink intra-band CA with two carriers if requested by the NW (see *reportUplinkTxDirectCurrentTwoCarrier-r16* in *CellGroupConfig*). |

### 6.3.2 Radio resource control information elements

#### *– CondReconfigId*

The IE *CondReconfigId* is used to identify a CHO, CPA or CPC configuration.

*CondReconfigId* information element

-- ASN1START

-- TAG-CONDRECONFIGID-START

CondReconfigId-r16 ::= INTEGER (1.. maxNrofCondCells-r16)

-- TAG-CONDRECONFIGID-STOP

-- ASN1STOP

#### *– CondReconfigToAddModList*

The IE *CondReconfigToAddModList* concerns a list of conditional reconfigurations to add or modify, with for each entry the *condReconfigId* and the associated *condExecutionCond/condExecutionCondSCG/subsequentCondReconfig* and *condRRCReconfig*.

*CondReconfigToAddModList* information element

-- ASN1START

-- TAG-CONDRECONFIGTOADDMODLIST-START

CondReconfigToAddModList-r16 ::= SEQUENCE (SIZE (1.. maxNrofCondCells-r16)) OF CondReconfigToAddMod-r16

CondReconfigToAddMod-r16 ::= SEQUENCE {

condReconfigId-r16 CondReconfigId-r16,

condExecutionCond-r16 SEQUENCE (SIZE (1..2)) OF MeasId OPTIONAL, -- Need M

condRRCReconfig-r16 OCTET STRING (CONTAINING RRCReconfiguration) OPTIONAL, -- Cond condReconfigAdd

...,

[[

condExecutionCondSCG-r17 OCTET STRING (CONTAINING CondReconfigExecCondSCG-r17) OPTIONAL -- Need M

]]

[[

subsequentCondReconfig-r18 SubsequentCondReconfig-r18 OPTIONAL -- Cond SCPAC

securityCellSetID-r18 SecurityCellSetID-r18 OPTIONAL -- Need M

]]

}

CondReconfigExecCondSCG-r17 ::= SEQUENCE (SIZE (1..2)) OF MeasId

SubsequentCondReconfig-r18 ::= SEQUENCE {

condExecutionCondToReleaseList-r18 CondExecutionCondToReleaseList-r18 OPTIONAL, -- Need N

condExecutionCondToAddModList-r18 CondExecutionCondToAddModList-r18 OPTIONAL -- Need N

}

CondExecutionCondToAddModList-r18 ::= SEQUENCE (SIZE (1.. maxNrofCondCells-r16)) OF CondExecutionCondToAddMod-r18

CondExecutionCondToAddMod-r18 ::= SEQUENCE {

condReconfigId-r16 CondReconfigId-r16,

condExecutionCond-r16 ::= SEQUENCE (SIZE (1..2)) OF MeasId OPTIONAL, -- Need M

CondReconfigExecCondSCG-r17 ::= SEQUENCE (SIZE (1..2)) OF MeasId OPTIONAL -- Need M

}

CondExecutionCondToReleaseList-r18 ::= SEQUENCE (SIZE (1.. maxNrofCondCells-r16)) OF condReconfigId-r16

-- TAG-CONDRECONFIGTOADDMODLIST-STOP

-- ASN1STOP

| *CondReconfigToAddMod* field descriptions |
| --- |
| ***condExecutionCond***  The execution condition that needs to be fulfilled in order to trigger the execution of a conditional reconfiguration for CHO, CPA, intra-SN CPC without MN involvement, MN initiated inter-SN CPC or SN initiated intra-SN subsequent CPC. When configuring 2 triggering events (Meas Ids) for a candidate cell, the network ensures that both refer to the same *measObject.* For CHO, if the network configures *condEventD1* or *condEventT1* for a candidate cell, the network configures a second triggering event *condEventA3, condEventA4* or *condEventA5* for the same candidate cell. The network does not configure both *condEventD1* and *condEventT1* for the same candidate cell. For CHO in terrestrial networks, the network does not indicate a *MeasId* associated with *condEventA4*. For CPA and for MN-initiated inter-SN CPC, the network only indicates *MeasId*(s) associated with *condEventA4*. For intra-SN CPC and intra-SN subsequent CPC, the network only indicates *MeasId*(s) associated with *condEventA3* or *condEventA5*. |
| ***condExecutionCondSCG***  Contains execution condition that needs to be fulfilled in order to trigger the execution of a conditional reconfiguration for SN initiated inter-SN CPC or SN initiated inter-SN subsequent CPC or MN initiated inter-SN subsequent CPC. The Meas Ids refer to the *measConfig* associated with the SCG. When configuring 2 triggering events (Meas Ids) for a candidate cell, network ensures that both refer to the same *measObject*. For each *condReconfigId*, the network always configures either *condExecutionCond* or *condExecutionCondSCG* (not both). The network only indicates *MeasId*(s) associated with *condEventA3* or *condEventA5*. |
| ***condRRCReconfig***  The *RRCReconfiguration* message to be applied when the condition(s) are fulfilled. The *RRCReconfiguration* message contained in *condRRCReconfig* cannot contain the field *conditionalReconfiguration* or the field *daps-Config*. |
| ***subsequentCondReconfig***  Contains the execution conditions for subsequent CPAC execution. If the field is present, the configuration of candidate PSCells for subsequent CPAC is supported. The subsequent execution condition is used for conditional reconfiguration evaluation for other candidate cells when the *RRCReconfiguration* message contained in *condRRCReconfig* has been applied. |

|  |  |
| --- | --- |
| Conditional Presence | Explanation |
| *condReconfigAdd* | The field is mandatory present when a *condReconfigId* is being added. Otherwise the field is optional, need M. |
| *condSCPAC* | This field is mandatory present when a *condReconfigId* support subsequent CPAC is being added. Otherwise the field is optional, need M. |

#### *– ConditionalReconfiguration*

The IE *ConditionalReconfiguration* is used to add, modify and release the configuration of conditional reconfiguration.

*ConditionalReconfiguration* information element

-- ASN1START

-- TAG-CONDITIONALRECONFIGURATION-START

ConditionalReconfiguration-r16 ::= SEQUENCE {

attemptCondReconfig-r16 ENUMERATED {true} OPTIONAL, -- Cond CHO

condReconfigToRemoveList-r16 CondReconfigToRemoveList-r16 OPTIONAL, -- Need N

condReconfigToAddModList-r16 CondReconfigToAddModList-r16 OPTIONAL, -- Need N

... ,

[[

scpac-ReferenceConfiguration-r18 SetupRelease (SCPAC-ReferenceConfiguration-r18) OPTIONAL, -- Need M

servingSecurityCellSetID-r18 SecurityCellSetID-r18 OPTIONAL, -- Cond InitialSCPAC

sk-CounterConfiguration-r18 SK-CounterConfiguration-r18 OPTIONAL -- Need M

]]

}

SCPAC-ReferenceConfiguration-r18 ::= OCTET STRING (CONTAINING RRCReconfiguration)

SK-CounterConfiguration-r18 ::= SEQUENCE {

sk-CounterConfigToReleaseList-r18 SK-CounterConfigToReleaseList-r18 OPTIONAL, -- Need N

sk-CounterConfigToAddModList-r18 SK-CounterConfigToAddModList-r18 OPTIONAL -- Need N

}

SK-CounterConfigToAddModList-r18 ::= SEQUENCE (SIZE (1..maxSecurityCellSet-r18)) OF SK-CounterConfigToAddMod-r18

SK-CounterConfigToAddMod-r18 ::= SEQUENCE {

securityCellSetID-r18 SecurityCellSetID-r18

sk-CounterList-r18 SK-CounterList-r18

}

SecurityCellSetID-r18 ::= INTEGER (1.. maxSecurityCellSet-r18)

SK-CounterList-r18 ::= SEQUENCE (SIZE (1..maxSK-Counter)) OF SK-Counter

sk-CounterConfigToRemoveList-r16 ::= SEQUENCE (SIZE (1.. maxSecurityCellSet-r18)) OF SecurityCellSetID-r18

CondReconfigToRemoveList-r16 ::= SEQUENCE (SIZE (1.. maxNrofCondCells-r16)) OF CondReconfigId-r16

-- TAG-CONDITIONALRECONFIGURATION-STOP

-- ASN1STOP

*Editor’s Note: FFS on how to guarantee the validity of sourceSecurityCellSetID after normal PSCell change, i.e. leave to NW implementation.*

| *ConditionalReconfiguration* field descriptions |
| --- |
| ***attemptCondReconfig***  If present, the UE shall perform conditional reconfiguration if selected cell is a target candidate cell and it is the first cell selection after failure as described in clause 5.3.7.3. |
| ***condReconfigToAddModList***  List of the configuration of candidate SpCells to be added or modified for CHO, CPA or CPC. |
| ***condReconfigToRemoveList***  List of the configuration of candidate SpCells to be removed. |
| ***scpac-ReferenceConfiguration***  Includes the reference configuration for the candidate supporting subsequent CPAC. |
| ***securityCellSetID***  This field is used to determine whether UE should perform security update when conditional reconfiguration containing *subsequentCondReconfig* is executed. |
| ***sk-counterConfiguration***  Includes SK-counters for security update for inter-SN subsequent CPAC. |
| ***servingSecurityCellSetID***  This field identifies the security cell set for serving PSCell. |

|  |  |
| --- | --- |
| Conditional Presence | Explanation |
| *CHO* | The field is optional present, Need R, if the UE is configured with at least a candidate SpCell for CHO. Otherwise the field is not present. |
| *condInitialSCPAC* | This field is mandatory present upon the initial conditional reconfiguration which includes at least one candidate PSCell supporting subsequent CPAC. Otherwise the field is optional, need N. |

## 6.4 RRC multiplicity and type constraint values

### – Multiplicity and type constraint definitions

-- ASN1START

-- TAG-MULTIPLICITY-AND-TYPE-CONSTRAINT-DEFINITIONS-START

maxAdditionalRACH-r17 INTEGER ::= 256 -- Maximum number of additional RACH configurations.

maxAI-DCI-PayloadSize-r16 INTEGER ::= 128 --Maximum size of the DCI payload scrambled with ai-RNTI

maxAI-DCI-PayloadSize-1-r16 INTEGER ::= 127 --Maximum size of the DCI payload scrambled with ai-RNTI minus 1

maxBandComb INTEGER ::= 65536 -- Maximum number of DL band combinations

maxBandsUTRA-FDD-r16 INTEGER ::= 64 -- Maximum number of bands listed in UTRA-FDD UE caps

maxBH-RLC-ChannelID-r16 INTEGER ::= 65536 -- Maximum value of BH RLC Channel ID

maxBT-IdReport-r16 INTEGER ::= 32 -- Maximum number of Bluetooth IDs to report

maxBT-Name-r16 INTEGER ::= 4 -- Maximum number of Bluetooth name

maxCAG-Cell-r16 INTEGER ::= 16 -- Maximum number of NR CAG cell ranges in SIB3, SIB4

maxTwoPUCCH-Grp-ConfigList-r16 INTEGER ::= 32 -- Maximum number of supported configuration(s) of {primary PUCCH group

-- config, secondary PUCCH group config}

maxTwoPUCCH-Grp-ConfigList-r17 INTEGER ::= 16 -- Maximum number of supported configuration(s) of {primary PUCCH group

-- config, secondary PUCCH group config} for PUCCH cell switching

maxCBR-Config-r16 INTEGER ::= 8 -- Maximum number of CBR range configurations for sidelink communication

-- congestion control

maxCBR-Config-1-r16 INTEGER ::= 7 -- Maximum number of CBR range configurations for sidelink communication

-- congestion control minus 1

maxCBR-Level-r16 INTEGER ::= 16 -- Maximum number of CBR levels

maxCBR-Level-1-r16 INTEGER ::= 15 -- Maximum number of CBR levels minus 1

maxCellExcluded INTEGER ::= 16 -- Maximum number of NR exclude-listed cell ranges in SIB3, SIB4

maxCellGroupings-r16 INTEGER ::= 32 -- Maximum number of cell groupings for NR-DC

maxCellHistory-r16 INTEGER ::= 16 -- Maximum number of visited PCells reported

maxPSCellHistory-r17 INTEGER ::= 16 -- Maximum number of visited PSCells across all reported PCells

maxCellInter INTEGER ::= 16 -- Maximum number of inter-Freq cells listed in SIB4

maxCellIntra INTEGER ::= 16 -- Maximum number of intra-Freq cells listed in SIB3

maxCellMeasEUTRA INTEGER ::= 32 -- Maximum number of cells in E-UTRAN

maxCellMeasIdle-r16 INTEGER ::= 8 -- Maximum number of cells per carrier for idle/inactive measurements

maxCellMeasUTRA-FDD-r16 INTEGER ::= 32 -- Maximum number of cells in FDD UTRAN

maxCellNTN-r17 INTEGER ::= 4 -- Maximum number of NTN neighbour cells for which assistance information is

-- provided

maxCarrierTypePairList-r16 INTEGER ::= 16 -- Maximum number of supported carrier type pair of (carrier type on which

-- CSI measurement is performed, carrier type on which CSI reporting is

-- performed) for CSI reporting cross PUCCH group

maxCellAllowed INTEGER ::= 16 -- Maximum number of NR allow-listed cell ranges in SIB3, SIB4

maxEARFCN INTEGER ::= 262143 -- Maximum value of E-UTRA carrier frequency

maxEUTRA-CellExcluded INTEGER ::= 16 -- Maximum number of E-UTRA exclude-listed physical cell identity ranges

-- in SIB5

maxEUTRA-NS-Pmax INTEGER ::= 8 -- Maximum number of NS and P-Max values per band

maxFeatureCombPreamblesPerRACHResource-r17 INTEGER ::= 256 -- Maximum number of feature combination preambles.

maxLogMeasReport-r16 INTEGER ::= 520 -- Maximum number of entries for logged measurements

maxMultiBands INTEGER ::= 8 -- Maximum number of additional frequency bands that a cell belongs to

maxNARFCN INTEGER ::= 3279165 -- Maximum value of NR carrier frequency

maxNR-NS-Pmax INTEGER ::= 8 -- Maximum number of NS and P-Max values per band

maxFreqIdle-r16 INTEGER ::= 8 -- Maximum number of carrier frequencies for idle/inactive measurements

maxNrofServingCells INTEGER ::= 32 -- Max number of serving cells (SpCells + SCells)

maxNrofServingCells-1 INTEGER ::= 31 -- Max number of serving cells (SpCells + SCells) minus 1

maxNrofAggregatedCellsPerCellGroup INTEGER ::= 16

maxNrofAggregatedCellsPerCellGroupMinus4-r16 INTEGER ::= 12

maxNrofDUCells-r16 INTEGER ::= 512 -- Max number of cells configured on the collocated IAB-DU

maxNrofAppLayerMeas-r17 INTEGER ::= 16 -- Max number of simultaneous application layer measurements

maxNrofAppLayerMeas-1-r17 INTEGER ::= 15 -- Max number of simultaneous application layer measurements minus 1

maxNrofAvailabilityCombinationsPerSet-r16 INTEGER ::= 512 -- Max number of AvailabilityCombinationId used in the DCI format 2\_5

maxNrofAvailabilityCombinationsPerSet-1-r16 INTEGER ::= 511 -- Max number of AvailabilityCombinationId used in the DCI format 2\_5 minus 1

maxNrofIABResourceConfig-r17 INTEGER ::= 65536 -- Max number of IAB-ResourceConfigID used in MAC CE

maxNrofIABResourceConfig-1-r17 INTEGER ::= 65535 -- Max number of IAB-ResourceConfigID used in MAC CE minus 1

maxNrofSCellActRS-r17 INTEGER ::= 255 -- Max number of RS configurations per SCell for SCell activation

maxNrofSCells INTEGER ::= 31 -- Max number of secondary serving cells per cell group

maxNrofCellMeas INTEGER ::= 32 -- Maximum number of entries in each of the cell lists in a measurement object

maxNrofCRS-IM-InterfCell-r17 INTEGER ::= 8 -- Maximum number of LTE interference cells for CRS-IM per UE

maxNrofRelayMeas-r17 INTEGER ::= 32 -- Maximum number of L2 U2N Relay UEs to measure for each measurement object

-- on sidelink frequency

maxNrofCG-SL-r16 INTEGER ::= 8 -- Max number of sidelink configured grant

maxNrofCG-SL-1-r16 INTEGER ::= 7 -- Max number of sidelink configured grant minus 1

maxSL-GC-BC-DRX-QoS-r17 INTEGER ::= 16 -- Max number of sidelink DRX configurations for NR

-- sidelink groupcast/broadcast communication

maxNrofSL-RxInfoSet-r17 INTEGER ::= 4 -- Max number of sidelink DRX configuration sets in sidelink DRX assistant

-- information

maxNrofSS-BlocksToAverage INTEGER ::= 16 -- Max number for the (max) number of SS blocks to average to determine cell measurement

maxNrofCondCells-r16 INTEGER ::= 8 -- Max number of conditional candidate SpCells

maxNrofCondCells-1-r17 INTEGER ::= 7 -- Max number of conditional candidate SpCells minus 1

maxNrofCSI-RS-ResourcesToAverage INTEGER ::= 16 -- Max number for the (max) number of CSI-RS to average to determine cell measurement

maxNrofDL-Allocations INTEGER ::= 16 -- Maximum number of PDSCH time domain resource allocations

maxNrofDL-AllocationsExt-r17 INTEGER ::= 64 -- Maximum number of PDSCH time domain resource allocations for multi-PDSCH

-- scheduling

maxNrofPDU-Sessions-r17 INTEGER ::= 256 -- Maximum number of PDU Sessions

maxNrofSR-ConfigPerCellGroup INTEGER ::= 8 -- Maximum number of SR configurations per cell group

maxLCG-ID INTEGER ::= 7 -- Maximum value of LCG ID

maxLCG-ID-IAB-r17 INTEGER ::= 255 -- Maximum value of LCG ID for IAB-MT

maxLC-ID INTEGER ::= 32 -- Maximum value of Logical Channel ID

maxLC-ID-Iab-r16 INTEGER ::= 65855 -- Maximum value of BH Logical Channel ID extension

maxLTE-CRS-Patterns-r16 INTEGER ::= 3 -- Maximum number of additional LTE CRS rate matching patterns

maxNrofTAGs INTEGER ::= 4 -- Maximum number of Timing Advance Groups

maxNrofTAGs-1 INTEGER ::= 3 -- Maximum number of Timing Advance Groups minus 1

maxNrofBWPs INTEGER ::= 4 -- Maximum number of BWPs per serving cell

maxNrofCombIDC INTEGER ::= 128 -- Maximum number of reported MR-DC combinations for IDC

maxNrofSymbols-1 INTEGER ::= 13 -- Maximum index identifying a symbol within a slot (14 symbols, indexed from 0..13)

maxNrofSlots INTEGER ::= 320 -- Maximum number of slots in a 10 ms period

maxNrofSlots-1 INTEGER ::= 319 -- Maximum number of slots in a 10 ms period minus 1

maxNrofPhysicalResourceBlocks INTEGER ::= 275 -- Maximum number of PRBs

maxNrofPhysicalResourceBlocks-1 INTEGER ::= 274 -- Maximum number of PRBs minus 1

maxNrofPhysicalResourceBlocksPlus1 INTEGER ::= 276 -- Maximum number of PRBs plus 1

maxNrofControlResourceSets INTEGER ::= 12 -- Max number of CoReSets configurable on a serving cell

maxNrofControlResourceSets-1 INTEGER ::= 11 -- Max number of CoReSets configurable on a serving cell minus 1

maxNrofControlResourceSets-1-r16 INTEGER ::= 15 -- Max number of CoReSets configurable on a serving cell extended in minus 1

maxNrofCoresetPools-r16 INTEGER ::= 2 -- Maximum number of CORESET pools

maxCoReSetDuration INTEGER ::= 3 -- Max number of OFDM symbols in a control resource set

maxNrofSearchSpaces-1 INTEGER ::= 39 -- Max number of Search Spaces minus 1

maxNrofSearchSpacesLinks-1-r17 INTEGER ::= 39 -- Max number of Search Space links minus 1

maxNrofBFDResourcePerSet-r17 INTEGER ::= 64 -- Max number of reference signal in one BFD set

maxSFI-DCI-PayloadSize INTEGER ::= 128 -- Max number payload of a DCI scrambled with SFI-RNTI

maxSFI-DCI-PayloadSize-1 INTEGER ::= 127 -- Max number payload of a DCI scrambled with SFI-RNTI minus 1

maxIAB-IP-Address-r16 INTEGER ::= 32 -- Max number of assigned IP addresses

maxINT-DCI-PayloadSize INTEGER ::= 126 -- Max number payload of a DCI scrambled with INT-RNTI

maxINT-DCI-PayloadSize-1 INTEGER ::= 125 -- Max number payload of a DCI scrambled with INT-RNTI minus 1

maxNrofRateMatchPatterns INTEGER ::= 4 -- Max number of rate matching patterns that may be configured

maxNrofRateMatchPatterns-1 INTEGER ::= 3 -- Max number of rate matching patterns that may be configured minus 1

maxNrofRateMatchPatternsPerGroup INTEGER ::= 8 -- Max number of rate matching patterns that may be configured in one group

maxNrofCSI-ReportConfigurations INTEGER ::= 48 -- Maximum number of report configurations

maxNrofCSI-ReportConfigurations-1 INTEGER ::= 47 -- Maximum number of report configurations minus 1

maxNrofCSI-ResourceConfigurations INTEGER ::= 112 -- Maximum number of resource configurations

maxNrofCSI-ResourceConfigurations-1 INTEGER ::= 111 -- Maximum number of resource configurations minus 1

maxNrofAP-CSI-RS-ResourcesPerSet INTEGER ::= 16

maxNrOfCSI-AperiodicTriggers INTEGER ::= 128 -- Maximum number of triggers for aperiodic CSI reporting

maxNrofReportConfigPerAperiodicTrigger INTEGER ::= 16 -- Maximum number of report configurations per trigger state for aperiodic reporting

maxNrofNZP-CSI-RS-Resources INTEGER ::= 192 -- Maximum number of Non-Zero-Power (NZP) CSI-RS resources

maxNrofNZP-CSI-RS-Resources-1 INTEGER ::= 191 -- Maximum number of Non-Zero-Power (NZP) CSI-RS resources minus 1

maxNrofNZP-CSI-RS-ResourcesPerSet INTEGER ::= 64 -- Maximum number of NZP CSI-RS resources per resource set

maxNrofNZP-CSI-RS-ResourceSets INTEGER ::= 64 -- Maximum number of NZP CSI-RS resource sets per cell

maxNrofNZP-CSI-RS-ResourceSets-1 INTEGER ::= 63 -- Maximum number of NZP CSI-RS resource sets per cell minus 1

maxNrofNZP-CSI-RS-ResourceSetsPerConfig INTEGER ::= 16 -- Maximum number of resource sets per resource configuration

maxNrofNZP-CSI-RS-ResourcesPerConfig INTEGER ::= 128 -- Maximum number of resources per resource configuration

maxNrofZP-CSI-RS-Resources INTEGER ::= 32 -- Maximum number of Zero-Power (ZP) CSI-RS resources

maxNrofZP-CSI-RS-Resources-1 INTEGER ::= 31 -- Maximum number of Zero-Power (ZP) CSI-RS resources minus 1

maxNrofZP-CSI-RS-ResourceSets-1 INTEGER ::= 15

maxNrofZP-CSI-RS-ResourcesPerSet INTEGER ::= 16

maxNrofZP-CSI-RS-ResourceSets INTEGER ::= 16

maxNrofCSI-IM-Resources INTEGER ::= 32 -- Maximum number of CSI-IM resources

maxNrofCSI-IM-Resources-1 INTEGER ::= 31 -- Maximum number of CSI-IM resources minus 1

maxNrofCSI-IM-ResourcesPerSet INTEGER ::= 8 -- Maximum number of CSI-IM resources per set

maxNrofCSI-IM-ResourceSets INTEGER ::= 64 -- Maximum number of NZP CSI-IM resource sets per cell

maxNrofCSI-IM-ResourceSets-1 INTEGER ::= 63 -- Maximum number of NZP CSI-IM resource sets per cell minus 1

maxNrofCSI-IM-ResourceSetsPerConfig INTEGER ::= 16 -- Maximum number of CSI IM resource sets per resource configuration

maxNrofCSI-SSB-ResourcePerSet INTEGER ::= 64 -- Maximum number of SSB resources in a resource set

maxNrofCSI-SSB-ResourceSets INTEGER ::= 64 -- Maximum number of CSI SSB resource sets per cell

maxNrofCSI-SSB-ResourceSets-1 INTEGER ::= 63 -- Maximum number of CSI SSB resource sets per cell minus 1

maxNrofCSI-SSB-ResourceSetsPerConfig INTEGER ::= 1 -- Maximum number of CSI SSB resource sets per resource configuration

maxNrofCSI-SSB-ResourceSetsPerConfigExt INTEGER ::= 2 -- Maximum number of CSI SSB resource sets per resource configuration

-- extended

maxNrofFailureDetectionResources INTEGER ::= 10 -- Maximum number of failure detection resources

maxNrofFailureDetectionResources-1 INTEGER ::= 9 -- Maximum number of failure detection resources minus 1

maxNrofFailureDetectionResources-1-r17 INTEGER ::= 63 -- Maximum number of the enhanced failure detection resources minus 1

maxNrofFreqSL-r16 INTEGER ::= 8 -- Maximum number of carrier frequency for NR sidelink communication

maxNrofSL-BWPs-r16 INTEGER ::= 4 -- Maximum number of BWP for NR sidelink communication

maxFreqSL-EUTRA-r16 INTEGER ::= 8 -- Maximum number of EUTRA anchor carrier frequency for NR sidelink communication

maxNrofSL-MeasId-r16 INTEGER ::= 64 -- Maximum number of sidelink measurement identity (RSRP) per destination

maxNrofSL-ObjectId-r16 INTEGER ::= 64 -- Maximum number of sidelink measurement objects (RSRP) per destination

maxNrofSL-ReportConfigId-r16 INTEGER ::= 64 -- Maximum number of sidelink measurement reporting configuration(RSRP) per destination

maxNrofSL-PoolToMeasureNR-r16 INTEGER ::= 8 -- Maximum number of resource pool for NR sidelink measurement to measure for

-- each measurement object (for CBR)

maxFreqSL-NR-r16 INTEGER ::= 8 -- Maximum number of NR anchor carrier frequency for NR sidelink communication

maxNrofSL-QFIs-r16 INTEGER ::= 2048 -- Maximum number of QoS flow for NR sidelink communication per UE

maxNrofSL-QFIsPerDest-r16 INTEGER ::= 64 -- Maximum number of QoS flow per destination for NR sidelink communication

maxNrofObjectId INTEGER ::= 64 -- Maximum number of measurement objects

maxNrofPageRec INTEGER ::= 32 -- Maximum number of page records

maxNrofPCI-Ranges INTEGER ::= 8 -- Maximum number of PCI ranges

maxPLMN INTEGER ::= 12 -- Maximum number of PLMNs broadcast and reported by UE at establishment

maxTAC-r17 INTEGER ::= 12 -- Maximum number of Tracking Area Codes to which a cell belongs to

maxNrofCSI-RS-ResourcesRRM INTEGER ::= 96 -- Maximum number of CSI-RS resources per cell for an RRM measurement object

maxNrofCSI-RS-ResourcesRRM-1 INTEGER ::= 95 -- Maximum number of CSI-RS resources per cell for an RRM measurement object

-- minus 1.

maxNrofMeasId INTEGER ::= 64 -- Maximum number of configured measurements

maxNrofQuantityConfig INTEGER ::= 2 -- Maximum number of quantity configurations

maxNrofCSI-RS-CellsRRM INTEGER ::= 96 -- Maximum number of cells with CSI-RS resources for an RRM measurement object

maxNrofSL-Dest-r16 INTEGER ::= 32 -- Maximum number of destination for NR sidelink communication and discovery

maxNrofSL-Dest-1-r16 INTEGER ::= 31 -- Highest index of destination for NR sidelink communication and discovery

maxNrofSLRB-r16 INTEGER ::= 512 -- Maximum number of radio bearer for NR sidelink communication per UE

maxSL-LCID-r16 INTEGER ::= 512 -- Maximum number of RLC bearer for NR sidelink communication per UE

maxSL-SyncConfig-r16 INTEGER ::= 16 -- Maximum number of sidelink Sync configurations

maxNrofRXPool-r16 INTEGER ::= 16 -- Maximum number of Rx resource pool for NR sidelink communication and

-- discovery

maxNrofTXPool-r16 INTEGER ::= 8 -- Maximum number of Tx resource pool for NR sidelink communication and

-- discovery

maxNrofPoolID-r16 INTEGER ::= 16 -- Maximum index of resource pool for NR sidelink communication and

-- discovery

maxNrofSRS-PathlossReferenceRS-r16 INTEGER ::= 64 -- Maximum number of RSs used as pathloss reference for SRS power control.

maxNrofSRS-PathlossReferenceRS-1-r16 INTEGER ::= 63 -- Maximum number of RSs used as pathloss reference for SRS power control

-- minus 1.

maxNrofSRS-ResourceSets INTEGER ::= 16 -- Maximum number of SRS resource sets in a BWP.

maxNrofSRS-ResourceSets-1 INTEGER ::= 15 -- Maximum number of SRS resource sets in a BWP minus 1.

maxNrofSRS-PosResourceSets-r16 INTEGER ::= 16 -- Maximum number of SRS Positioning resource sets in a BWP.

maxNrofSRS-PosResourceSets-1-r16 INTEGER ::= 15 -- Maximum number of SRS Positioning resource sets in a BWP minus 1.

maxNrofSRS-Resources INTEGER ::= 64 -- Maximum number of SRS resources.

maxNrofSRS-Resources-1 INTEGER ::= 63 -- Maximum number of SRS resources minus 1.

maxNrofSRS-PosResources-r16 INTEGER ::= 64 -- Maximum number of SRS Positioning resources.

maxNrofSRS-PosResources-1-r16 INTEGER ::= 63 -- Maximum number of SRS Positioning resources minus 1.

maxNrofSRS-ResourcesPerSet INTEGER ::= 16 -- Maximum number of SRS resources in an SRS resource set

maxNrofSRS-TriggerStates-1 INTEGER ::= 3 -- Maximum number of SRS trigger states minus 1, i.e., the largest code point.

maxNrofSRS-TriggerStates-2 INTEGER ::= 2 -- Maximum number of SRS trigger states minus 2.

maxRAT-CapabilityContainers INTEGER ::= 8 -- Maximum number of interworking RAT containers (incl NR and MRDC)

maxSimultaneousBands INTEGER ::= 32 -- Maximum number of simultaneously aggregated bands

maxULTxSwitchingBandPairs INTEGER ::= 32 -- Maximum number of band pairs supporting dynamic UL Tx switching in a band

-- combination.

maxNrofSlotFormatCombinationsPerSet INTEGER ::= 512 -- Maximum number of Slot Format Combinations in a SF-Set.

maxNrofSlotFormatCombinationsPerSet-1 INTEGER ::= 511 -- Maximum number of Slot Format Combinations in a SF-Set minus 1.

maxNrofTrafficPattern-r16 INTEGER ::= 8 -- Maximum number of Traffic Pattern for NR sidelink communication.

maxNrofPUCCH-Resources INTEGER ::= 128

maxNrofPUCCH-Resources-1 INTEGER ::= 127

maxNrofPUCCH-ResourceSets INTEGER ::= 4 -- Maximum number of PUCCH Resource Sets

maxNrofPUCCH-ResourceSets-1 INTEGER ::= 3 -- Maximum number of PUCCH Resource Sets minus 1.

maxNrofPUCCH-ResourcesPerSet INTEGER ::= 32 -- Maximum number of PUCCH Resources per PUCCH-ResourceSet

maxNrofPUCCH-P0-PerSet INTEGER ::= 8 -- Maximum number of P0-pucch present in a p0-pucch set

maxNrofPUCCH-PathlossReferenceRSs INTEGER ::= 4 -- Maximum number of RSs used as pathloss reference for PUCCH power control.

maxNrofPUCCH-PathlossReferenceRSs-1 INTEGER ::= 3 -- Maximum number of RSs used as pathloss reference for PUCCH power control

-- minus 1.

maxNrofPUCCH-PathlossReferenceRSs-r16 INTEGER ::= 64 -- Maximum number of RSs used as pathloss reference for PUCCH power control

-- extended.

maxNrofPUCCH-PathlossReferenceRSs-1-r16 INTEGER ::= 63 -- Maximum number of RSs used as pathloss reference for PUCCH power control

-- minus 1 extended.

maxNrofPUCCH-PathlossReferenceRSs-1-r17 INTEGER ::= 7 -- Maximum number of RSs used as pathloss reference for PUCCH power control

-- minus 1.

maxNrofPUCCH-PathlossReferenceRSsDiff-r16 INTEGER ::= 60 -- Difference between the extended maximum and the non-extended maximum

maxNrofPUCCH-ResourceGroups-r16 INTEGER ::= 4 -- Maximum number of PUCCH resources groups.

maxNrofPUCCH-ResourcesPerGroup-r16 INTEGER ::= 128 -- Maximum number of PUCCH resources in a PUCCH group.

maxNrofPowerControlSetInfos-r17 INTEGER ::= 8 -- Maximum number of PUCCH power control set infos

maxNrofMultiplePUSCHs-r16 INTEGER ::= 8 -- Maximum number of multiple PUSCHs in PUSCH TDRA list

maxNrofP0-PUSCH-AlphaSets INTEGER ::= 30 -- Maximum number of P0-pusch-alpha-sets (see TS 38.213 [13], clause 7.1)

maxNrofP0-PUSCH-AlphaSets-1 INTEGER ::= 29 -- Maximum number of P0-pusch-alpha-sets minus 1 (see TS 38.213 [13], clause 7.1)

maxNrofPUSCH-PathlossReferenceRSs INTEGER ::= 4 -- Maximum number of RSs used as pathloss reference for PUSCH power control.

maxNrofPUSCH-PathlossReferenceRSs-1 INTEGER ::= 3 -- Maximum number of RSs used as pathloss reference for PUSCH power control

-- minus 1.

maxNrofPUSCH-PathlossReferenceRSs-r16 INTEGER ::= 64 -- Maximum number of RSs used as pathloss reference for PUSCH power control

-- extended

maxNrofPUSCH-PathlossReferenceRSs-1-r16 INTEGER ::= 63 -- Maximum number of RSs used as pathloss reference for PUSCH power control

-- extended minus 1

maxNrofPUSCH-PathlossReferenceRSsDiff-r16 INTEGER ::= 60 -- Difference between maxNrofPUSCH-PathlossReferenceRSs-r16 and

-- maxNrofPUSCH-PathlossReferenceRSs

maxNrofPathlossReferenceRSs-r17 INTEGER ::= 64 -- Maximum number of RSs used as pathloss reference for PUSCH, PUCCH, SRS

-- power control for unified TCI state operation

maxNrofPathlossReferenceRSs-1-r17 INTEGER ::= 63 -- Maximum number of RSs used as pathloss reference for PUSCH, PUCCH, SRS

-- power control for unified TCI state operation minus 1

maxNrofNAICS-Entries INTEGER ::= 8 -- Maximum number of supported NAICS capability set

maxBands INTEGER ::= 1024 -- Maximum number of supported bands in UE capability.

maxBandsMRDC INTEGER ::= 1280

maxBandsEUTRA INTEGER ::= 256

maxCellReport INTEGER ::= 8

maxDRB INTEGER ::= 29 -- Maximum number of DRBs (that can be added in DRB-ToAddModList).

maxFreq INTEGER ::= 8 -- Max number of frequencies.

maxFreqLayers INTEGER ::= 4 -- Max number of frequency layers.

maxFreqPlus1 INTEGER ::= 9 -- Max number of frequencies for Slicing.

maxFreqIDC-r16 INTEGER ::= 128 -- Max number of frequencies for IDC indication.

maxCombIDC-r16 INTEGER ::= 128 -- Max number of reported UL CA for IDC indication.

maxFreqIDC-MRDC INTEGER ::= 32 -- Maximum number of candidate NR frequencies for MR-DC IDC indication

maxNrofCandidateBeams INTEGER ::= 16 -- Max number of PRACH-ResourceDedicatedBFR in BFR config.

maxNrofCandidateBeams-r16 INTEGER ::= 64 -- Max number of candidate beam resources in BFR config.

maxNrofCandidateBeamsExt-r16 INTEGER ::= 48 -- Max number of PRACH-ResourceDedicatedBFR in the CandidateBeamRSListExt

maxNrofPCIsPerSMTC INTEGER ::= 64 -- Maximum number of PCIs per SMTC.

maxNrofQFIs INTEGER ::= 64

maxNrofResourceAvailabilityPerCombination-r16 INTEGER ::= 256

maxNrOfSemiPersistentPUSCH-Triggers INTEGER ::= 64 -- Maximum number of triggers for semi persistent reporting on PUSCH

maxNrofSR-Resources INTEGER ::= 8 -- Maximum number of SR resources per BWP in a cell.

maxNrofSlotFormatsPerCombination INTEGER ::= 256

maxNrofSpatialRelationInfos INTEGER ::= 8

maxNrofSpatialRelationInfos-plus-1 INTEGER ::= 9

maxNrofSpatialRelationInfos-r16 INTEGER ::= 64

maxNrofSpatialRelationInfosDiff-r16 INTEGER ::= 56 -- Difference between maxNrofSpatialRelationInfos-r16 and maxNrofSpatialRelationInfos

maxNrofIndexesToReport INTEGER ::= 32

maxNrofIndexesToReport2 INTEGER ::= 64

maxNrofSSBs-r16 INTEGER ::= 64 -- Maximum number of SSB resources in a resource set.

maxNrofSSBs-1 INTEGER ::= 63 -- Maximum number of SSB resources in a resource set minus 1.

maxNrofS-NSSAI INTEGER ::= 8 -- Maximum number of S-NSSAI.

maxNrofTCI-StatesPDCCH INTEGER ::= 64

maxNrofTCI-States INTEGER ::= 128 -- Maximum number of TCI states.

maxNrofTCI-States-1 INTEGER ::= 127 -- Maximum number of TCI states minus 1.

maxUL-TCI-r17 INTEGER ::= 64 -- Maximum number of TCI states.

maxUL-TCI-1-r17 INTEGER ::= 63 -- Maximum number of TCI states minus 1.

maxNrofAdditionalPCI-r17 INTEGER ::= 7 -- Maximum number of additional PCI

maxMPE-Resources-r17 INTEGER ::= 64 -- Maximum number of pooled MPE resources

maxNrofUL-Allocations INTEGER ::= 16 -- Maximum number of PUSCH time domain resource allocations.

maxQFI INTEGER ::= 63

maxRA-CSIRS-Resources INTEGER ::= 96

maxRA-OccasionsPerCSIRS INTEGER ::= 64 -- Maximum number of RA occasions for one CSI-RS

maxRA-Occasions-1 INTEGER ::= 511 -- Maximum number of RA occasions in the system

maxRA-SSB-Resources INTEGER ::= 64

maxSCSs INTEGER ::= 5

maxSecondaryCellGroups INTEGER ::= 3

maxNrofServingCellsEUTRA INTEGER ::= 32

maxMBSFN-Allocations INTEGER ::= 8

maxNrofMultiBands INTEGER ::= 8

maxCellSFTD INTEGER ::= 3 -- Maximum number of cells for SFTD reporting

maxReportConfigId INTEGER ::= 64

maxNrofCodebooks INTEGER ::= 16 -- Maximum number of codebooks supported by the UE

maxNrofCSI-RS-ResourcesExt-r16 INTEGER ::= 16 -- Maximum number of codebook resources supported by the UE for eType2/Codebook combo

maxNrofCSI-RS-ResourcesExt-r17 INTEGER ::= 8 -- Maximum number of codebook resources for fetype2R1 and fetype2R2

maxNrofCSI-RS-Resources INTEGER ::= 7 -- Maximum number of codebook resources supported by the UE

maxNrofCSI-RS-ResourcesAlt-r16 INTEGER ::= 512 -- Maximum number of alternative codebook resources supported by the UE

maxNrofCSI-RS-ResourcesAlt-1-r16 INTEGER ::= 511 -- Maximum number of alternative codebook resources supported by the UE minus 1

maxNrofSRI-PUSCH-Mappings INTEGER ::= 16

maxNrofSRI-PUSCH-Mappings-1 INTEGER ::= 15

maxSIB INTEGER::= 32 -- Maximum number of SIBs

maxSI-Message INTEGER::= 32 -- Maximum number of SI messages

maxSIB-MessagePlus1-r17 INTEGER::= 33 -- Maximum number of SIB messages plus 1

maxPO-perPF INTEGER ::= 4 -- Maximum number of paging occasion per paging frame

maxPEI-perPF-r17 INTEGER ::= 4 -- Maximum number of PEI occasion per paging frame

maxAccessCat-1 INTEGER ::= 63 -- Maximum number of Access Categories minus 1

maxBarringInfoSet INTEGER ::= 8 -- Maximum number of access control parameter sets

maxCellEUTRA INTEGER ::= 8 -- Maximum number of E-UTRA cells in SIB list

maxEUTRA-Carrier INTEGER ::= 8 -- Maximum number of E-UTRA carriers in SIB list

maxPLMNIdentities INTEGER ::= 8 -- Maximum number of PLMN identities in RAN area configurations

maxDownlinkFeatureSets INTEGER ::= 1024 -- (for NR DL) Total number of FeatureSets (size of the pool)

maxUplinkFeatureSets INTEGER ::= 1024 -- (for NR UL) Total number of FeatureSets (size of the pool)

maxEUTRA-DL-FeatureSets INTEGER ::= 256 -- (for E-UTRA) Total number of FeatureSets (size of the pool)

maxEUTRA-UL-FeatureSets INTEGER ::= 256 -- (for E-UTRA) Total number of FeatureSets (size of the pool)

maxFeatureSetsPerBand INTEGER ::= 128 -- (for NR) The number of feature sets associated with one band.

maxPerCC-FeatureSets INTEGER ::= 1024 -- (for NR) Total number of CC-specific FeatureSets (size of the pool)

maxFeatureSetCombinations INTEGER ::= 1024 -- (for MR-DC/NR)Total number of Feature set combinations (size of the pool)

maxInterRAT-RSTD-Freq INTEGER ::= 3

maxGIN-r17 INTEGER ::= 24 -- Maximum number of broadcast GINs

maxHRNN-Len-r16 INTEGER ::= 48 -- Maximum length of HRNNs

maxNPN-r16 INTEGER ::= 12 -- Maximum number of NPNs broadcast and reported by UE at establishment

maxNrOfMinSchedulingOffsetValues-r16 INTEGER ::= 2 -- Maximum number of min. scheduling offset (K0/K2) configurations

maxK0-SchedulingOffset-r16 INTEGER ::= 16 -- Maximum number of slots configured as min. scheduling offset (K0)

maxK2-SchedulingOffset-r16 INTEGER ::= 16 -- Maximum number of slots configured as min. scheduling offset (K2)

maxK0-SchedulingOffset-r17 INTEGER ::= 64 -- Maximum number of slots configured as min. scheduling offset (K0)

maxK2-SchedulingOffset-r17 INTEGER ::= 64 -- Maximum number of slots configured as min. scheduling offset (K2)

maxDCI-2-6-Size-r16 INTEGER ::= 140 -- Maximum size of DCI format 2-6

maxDCI-2-7-Size-r17 INTEGER ::= 43 -- Maximum size of DCI format 2-7

maxDCI-2-6-Size-1-r16 INTEGER ::= 139 -- Maximum DCI format 2-6 size minus 1

maxNrofUL-Allocations-r16 INTEGER ::= 64 -- Maximum number of PUSCH time domain resource allocations

maxNrofP0-PUSCH-Set-r16 INTEGER ::= 2 -- Maximum number of P0 PUSCH set(s)

maxOnDemandSIB-r16 INTEGER ::= 8 -- Maximum number of SIB(s) that can be requested on-demand

maxOnDemandPosSIB-r16 INTEGER ::= 32 -- Maximum number of posSIB(s) that can be requested on-demand

maxCI-DCI-PayloadSize-r16 INTEGER ::= 126 -- Maximum number of the DCI size for CI

maxCI-DCI-PayloadSize-1-r16 INTEGER ::= 125 -- Maximum number of the DCI size for CI minus 1

maxUu-RelayRLC-ChannelID-r17 INTEGER ::= 32 -- Maximum value of Uu Relay RLC channel ID

maxWLAN-Id-Report-r16 INTEGER ::= 32 -- Maximum number of WLAN IDs to report

maxWLAN-Name-r16 INTEGER ::= 4 -- Maximum number of WLAN name

maxRAReport-r16 INTEGER ::= 8 -- Maximum number of RA procedures information to be included in the RA report

maxTxConfig-r16 INTEGER ::= 64 -- Maximum number of sidelink transmission parameters configurations

maxTxConfig-1-r16 INTEGER ::= 63 -- Maximum number of sidelink transmission parameters configurations minus 1

maxPSSCH-TxConfig-r16 INTEGER ::= 16 -- Maximum number of PSSCH TX configurations

maxNrofCLI-RSSI-Resources-r16 INTEGER ::= 64 -- Maximum number of CLI-RSSI resources for UE

maxNrofCLI-RSSI-Resources-1-r16 INTEGER ::= 63 -- Maximum number of CLI-RSSI resources for UE minus 1

maxNrofCLI-SRS-Resources-r16 INTEGER ::= 32 -- Maximum number of SRS resources for CLI measurement for UE

maxCLI-Report-r16 INTEGER ::= 8

maxNrofCC-Group-r17 INTEGER ::= 16 -- Maximum number of CC groups for DC location report

maxNrofConfiguredGrantConfig-r16 INTEGER ::= 12 -- Maximum number of configured grant configurations per BWP

maxNrofConfiguredGrantConfig-1-r16 INTEGER ::= 11 -- Maximum number of configured grant configurations per BWP minus 1

maxNrofCG-Type2DeactivationState INTEGER ::= 16 -- Maximum number of deactivation state for type 2 configured grants per BWP

maxNrofConfiguredGrantConfigMAC-1-r16 INTEGER ::= 31 -- Maximum number of configured grant configurations per MAC entity minus 1

maxNrofSPS-Config-r16 INTEGER ::= 8 -- Maximum number of SPS configurations per BWP

maxNrofSPS-Config-1-r16 INTEGER ::= 7 -- Maximum number of SPS configurations per BWP minus 1

maxNrofSPS-DeactivationState INTEGER ::= 16 -- Maximum number of deactivation state for SPS per BWP

maxNrofPPW-Config-r17 INTEGER ::= 4 -- Maximum number of Preconfigured PRS processing windows per DL BWP

maxNrofPPW-ID-1-r17 INTEGER ::= 15 -- Maximum number of Preconfigured PRS processing windows minus 1

maxNrOfTxTEGReport-r17 INTEGER ::= 256 -- Maximum number of UE Tx Timing Error Group Report

maxNrOfTxTEG-ID-1-r17 INTEGER ::= 7 -- Maximum number of UE Tx Timing Error Group ID minus 1

maxNrofPagingSubgroups-r17 INTEGER ::= 8 -- Maximum number of paging subgroups per paging occasion

maxNrofPUCCH-ResourceGroups-1-r16 INTEGER ::= 3

maxNrofReqComDC-Location-r17 INTEGER ::= 128 -- Maximum number of requested carriers/BWPs combinations for DC location

-- report

maxNrofServingCellsTCI-r16 INTEGER ::= 32 -- Maximum number of serving cells in simultaneousTCI-UpdateList

maxNrofTxDC-TwoCarrier-r16 INTEGER ::= 64 -- Maximum number of UL Tx DC locations reported by the UE for 2CC uplink CA

maxNrofRB-SetGroups-r17 INTEGER ::= 8 -- Maximum number of RB set groups

maxNrofRB-Sets-r17 INTEGER ::= 8 -- Maximum number of RB sets

maxNrofEnhType3HARQ-ACK-r17 INTEGER ::= 8 -- Maximum number of enhanced type 3 HARQ-ACK codebook

maxNrofEnhType3HARQ-ACK-1-r17 INTEGER ::= 7 -- Maximum number of enhanced type 3 HARQ-ACK codebook minus 1

maxNrofPRS-ResourcesPerSet-r17 INTEGER ::= 64 -- Maximum number of PRS resources for one set

maxNrofPRS-ResourcesPerSet-1-r17 INTEGER ::= 63 -- Maximum number of PRS resources for one set minus 1

maxNrofPRS-ResourceOffsetValue-1-r17 INTEGER ::= 511

maxNrofGapId-r17 INTEGER ::= 8 -- Maximum number of measurement gap ID is FFS

maxNrofPreConfigPosGapId-r17 INTEGER ::= 16 -- Maximum number of preconfigured positioning measurement gap

maxNrOfGapPri-r17 INTEGER ::= 16 -- Maximum number of gap priority level

maxCEFReport-r17 INTEGER ::= 4 -- Maximum number of CEF reports by the UE

maxNrofMultiplePDSCHs-r17 INTEGER ::= 8 -- Maximum number of PDSCHs in PDSCH TDRA list

maxSliceInfo-r17 INTEGER ::= 8 -- Maximum number of NSAGs

maxCellSlice-r17 INTEGER ::= 16 -- Maximum number of cells supporting the NSAG

maxNrofTRS-ResourceSets-r17 INTEGER ::= 64 -- Maximum number of TRS resource sets

maxNrofSearchSpaceGroups-1-r17 INTEGER ::= 2 -- Maximum number of search space groups minus 1

maxNrofRemoteUE-r17 INTEGER ::= 32 -- Maximum number of connected L2 U2N Remote UEs

maxDCI-4-2-Size-r17 INTEGER ::= 140 -- Maximum size of DCI format 4-2

maxFreqMBS-r17 INTEGER ::= 16 -- Maximum number of MBS frequencies reported in MBSInterestIndication

maxNrofDRX-ConfigPTM-r17 INTEGER ::= 64 -- Max number of DRX configuration for PTM provided in MBS broadcast in a

-- cell

maxNrofDRX-ConfigPTM-1-r17 INTEGER ::= 63 -- Max number of DRX configuration for PTM provided in MBS broadcast in a

-- cell minus 1

maxNrofMBS-ServiceListPerUE-r17 INTEGER ::= 16 -- Maximum number of services which the UE can include in the MBS interest

-- indication

maxNrofMBS-Session-r17 INTEGER ::= 1024 -- Maximum number of MBS sessions provided in MBS broadcast in a cell

maxNrofMTCH-SSB-MappingWindow-r17 INTEGER ::= 16 -- Maximum number of MTCH to SSB beam mapping pattern

maxNrofMTCH-SSB-MappingWindow-1-r17 INTEGER ::= 15 -- Maximum number of MTCH to SSB beam mapping pattern minus 1

maxNrofMRB-Broadcast-r17 INTEGER ::= 4 -- Maximum number of broadcast MRBs configured for one MBS broadcast service

maxNrofPageGroup-r17 INTEGER ::= 32 -- Maximum number of paging groups in a paging message

maxNrofPDSCH-ConfigPTM-r17 INTEGER ::= 16 -- Maximum number of PDSCH configuration groups for PTM

maxNrofPDSCH-ConfigPTM-1-r17 INTEGER ::= 15 -- Maximum number of PDSCH configuration groups for PTM minus 1

maxG-RNTI-r17 INTEGER ::= 16 -- Maximum number of G-RNTI that can be configured for a UE.

maxG-RNTI-1-r17 INTEGER ::= 15 -- Maximum number of G-RNTI that can be configured for a UE minus 1.

maxG-CS-RNTI-r17 INTEGER ::= 8 -- Maximum number of G-CS-RNTI that can be configured for a UE.

maxG-CS-RNTI-1-r17 INTEGER ::= 7 -- Maximum number of G-CS-RNTI that can be configured for a UE minus 1.

maxMRB-r17 INTEGER ::= 32 -- Maximum number of multicast MRBs (that can be added in MRB-ToAddModLIst)

maxFSAI-MBS-r17 INTEGER ::= 64 -- Maximum number of MBS frequency selection area identities

maxNeighCellMBS-r17 INTEGER ::= 8 -- Maximum number of MBS broadcast neighbour cells

maxNrofPdcch-BlindDetectionMixed-1-r16 INTEGER ::= 7 -- Maximum number of combinations of mixed Rel-16 and Rel-15 PDCCH

-- monitoring capabilities minus 1

maxNrofPdcch-BlindDetection-r17 INTEGER ::= 16 -- Maximum number of combinations of PDCCH blind detection monitoring

-- capabilities

maxSecurityCellSet-r18 INTEGER ::= FFS -- Maximum number of cell sets for subsequent CPAC.

maxSK-Counter-r18 INTEGER ::= FFS -- Maximum number of SK-counters configured for a cell set for subsequent CPAC.

-- TAG-MULTIPLICITY-AND-TYPE-CONSTRAINT-DEFINITIONS-STOP

-- ASN1STOP

*Editor’s Note: FFS on the maximum number of maxSecurityCellSet-r18 and maxSK-Counter-r18.*

## 7.4 UE variables

NOTE: To facilitate the specification of the UE behavioural requirements, UE variables are represented using ASN.1. Unless explicitly specified otherwise, it is however up to UE implementation how to store the variables. The optionality of the IEs in ASN.1 is used only to indicate that the values may not always be available.

#### – *NR-UE-Variables*

This ASN.1 segment is the start of the NR UE variable definitions.

-- ASN1START

-- NR-UE-VARIABLES-START

NR-UE-Variables DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

IMPORTS

AreaConfiguration-v1700,

ARFCN-ValueNR,

CellIdentity,

EUTRA-PhysCellId,

maxCEFReport-r17,

MeasId,

MeasIdToAddModList,

MeasIdleCarrierEUTRA-r16,

MeasIdleCarrierNR-r16,

MeasResultIdleEUTRA-r16,

MeasResultIdleNR-r16,

MeasObjectToAddModList,

PhysCellId,

RNTI-Value,

ReportConfigToAddModList,

RSRP-Range,

SL-MeasId-r16,

SL-MeasIdList-r16,

SL-MeasObjectList-r16,

SL-ReportConfigList-r16,

SL-QuantityConfig-r16,

Tx-PoolMeasList-r16,

QuantityConfig,

maxNrofCellMeas,

maxNrofMeasId,

maxFreqIdle-r16,

PhysCellIdUTRA-FDD-r16,

ValidityAreaList-r16,

CondReconfigToAddModList-r16,

ConnEstFailReport-r16,

LoggingDuration-r16,

LoggingInterval-r16,

LogMeasInfoList-r16,

LogMeasInfo-r16,

RA-Report-r16,

RLF-Report-r16,

TraceReference-r16,

WLAN-Identifiers-r16,

WLAN-NameList-r16,

BT-NameList-r16,

PLMN-Identity,

maxNrofRelayMeas-r17,

maxPLMN,

RA-ReportList-r16,

VisitedCellInfoList-r16,

AbsoluteTimeInfo-r16,

LoggedEventTriggerConfig-r16,

LoggedPeriodicalReportConfig-r16,

Sensor-NameList-r16,

SL-SourceIdentity-r17,

SuccessHO-Report-r17,

PLMN-IdentityList2-r16,

AreaConfiguration-r16,

maxNrofSL-MeasId-r16,

maxNrofFreqSL-r16,

maxNrofCLI-RSSI-Resources-r16,

maxNrofCLI-SRS-Resources-r16,

RSSI-ResourceId-r16,

SRS-ResourceId,

VisitedPSCellInfoList-r17,

VarServingSecurityCellSetID-r18

FROM NR-RRC-Definitions;

-- NR-UE-VARIABLES-STOP

-- ASN1STOP

#### – *VarConditionalReconfig*

The UE variable *VarConditionalReconfig* includes the accumulated configuration of the conditional handover, conditional PSCell addition or conditional PSCell change configurations including the pointers to conditional handover, conditional PSCell addition or conditional PSCell change or subsequent CPAC execution condition (associated *measId*(s)), the stored target candidate SpCell *RRCReconfiguration*, the stored reference configuration and the stored *SK-Counter* configuration.

*VarConditionalReconfig UE variable*

-- ASN1START

-- TAG-VARCONDITIONALRECONFIG-START

VarConditionalReconfig ::= SEQUENCE {

condReconfigList CondReconfigToAddModList-r16 OPTIONAL,

SCPAC-ReferenceConfiguration-r18 OCTET STRING (CONTAINING RRCReconfiguration) OPTIONAL,

sk-CounterConfiguration-r18 SK-CounterConfiguration-r18 OPTIONAL

}

-- TAG-VARCONDITIONALRECONFIG-STOP

-- ASN1STOP

#### – *VarServingSecurityCellSetID*

The UE variable *VarServingSecurityCellSetID includes the security cell set ID of serving PSCell.*

*VarServingSecurityCellSetID UE variable*

-- ASN1START

-- TAG-VARCONDITIONALRECONFIG-START

VarServingSecurityCellSetID ::= SEQUENCE {

servingSecurityCellSetID-r18 SecurityCellSetID-r18 OPTIONAL

}

-- TAG-VARCONDITIONALRECONFIG-STOP

-- ASN1STOP

### 11.2.2 Message definitions

#### – *CG-CandidateList*

This message is used to transfer the SCG radio configuration for one or more candidate cells for Conditional PSCell Addition (CPA) or Conditional PSCell Change (CPC) as generated by the candidate target SgNB.

Direction: Secondary gNB to master gNB or eNB.

*CG-CandidateList* message

-- ASN1START

-- TAG-CG-CANDIDATELIST-START

CG-CandidateList ::= SEQUENCE {

criticalExtensions CHOICE {

c1 CHOICE{

cg-CandidateList-r17 CG-CandidateList-r17-IEs,

spare3 NULL, spare2 NULL, spare1 NULL

},

criticalExtensionsFuture SEQUENCE {}

}

}

CG-CandidateList-r17-IEs ::= SEQUENCE {

cg-CandidateToAddModList-r17 SEQUENCE (SIZE (1..maxNrofCondCells-r16)) OF CG-CandidateInfo-r17 OPTIONAL,

cg-CandidateToReleaseList-r17 SEQUENCE (SIZE (1..maxNrofCondCells-r16)) OF CG-CandidateInfoId-r17 OPTIONAL,

nonCriticalExtension SEQUENCE {} OPTIONAL

}

CG-CandidateInfo-r17 ::= SEQUENCE {

cg-CandidateInfoId-r17 CG-CandidateInfoId-r17,

candidateCG-Config-r17 OCTET STRING (CONTAINING CG-Config)

}

CG-CandidateInfoId-r17::= SEQUENCE {

ssbFrequency-r17 ARFCN-ValueNR,

physCellId-r17 PhysCellId

}

-- TAG-CG-CANDIDATELIST-STOP

-- ASN1STOP

|  |
| --- |
| *CG-CandidateList* field descriptions |
| ***cg-CandidateToAddModList***  Contains information regarding candidate target cells to be added or modified for Conditional PSCell Addition (CPA) or Conditional PSCell Change (CPC) from the candidate target secondary node to the master node. |
| ***cg-CandidateToReleaseList***  Contains information regarding candidate target cells for CPA or CPC to be removed from the candidate target secondary node to the master node. This list is not used in CPA or CPC preparation. |

|  |
| --- |
| *CG-CandidateInfo* field descriptions |
| ***cg-CandidateInfoId***  SSB frequency and Physical Cell Identity of the candidate target cell. |
| ***candidateCG-Config***  *CG-Config* message corresponding to the cell indicated by *cg-CandidateInfoId*. |

– *CG-Config*

This message is used to transfer the SCG radio configuration as generated by the SgNB or SeNB. It can also be used by a CU to request a DU to perform certain actions, e.g. to request the DU to perform a new lower layer configuration.

Direction: Secondary gNB or eNB to master gNB or eNB, alternatively CU to DU.

***CG-Config* message**

-- ASN1START

-- TAG-CG-CONFIG-START

CG-Config ::= SEQUENCE {

criticalExtensions CHOICE {

c1 CHOICE{

cg-Config CG-Config-IEs,

spare3 NULL, spare2 NULL, spare1 NULL

},

criticalExtensionsFuture SEQUENCE {}

}

}

CG-Config-IEs ::= SEQUENCE {

scg-CellGroupConfig OCTET STRING (CONTAINING RRCReconfiguration) OPTIONAL,

scg-RB-Config OCTET STRING (CONTAINING RadioBearerConfig) OPTIONAL,

configRestrictModReq ConfigRestrictModReqSCG OPTIONAL,

drx-InfoSCG DRX-Info OPTIONAL,

candidateCellInfoListSN OCTET STRING (CONTAINING MeasResultList2NR) OPTIONAL,

measConfigSN MeasConfigSN OPTIONAL,

selectedBandCombination BandCombinationInfoSN OPTIONAL,

fr-InfoListSCG FR-InfoList OPTIONAL,

candidateServingFreqListNR CandidateServingFreqListNR OPTIONAL,

nonCriticalExtension CG-Config-v1540-IEs OPTIONAL

}

CG-Config-v1540-IEs ::= SEQUENCE {

pSCellFrequency ARFCN-ValueNR OPTIONAL,

reportCGI-RequestNR SEQUENCE {

requestedCellInfo SEQUENCE {

ssbFrequency ARFCN-ValueNR,

cellForWhichToReportCGI PhysCellId

} OPTIONAL

} OPTIONAL,

ph-InfoSCG PH-TypeListSCG OPTIONAL,

nonCriticalExtension CG-Config-v1560-IEs OPTIONAL

}

CG-Config-v1560-IEs ::= SEQUENCE {

pSCellFrequencyEUTRA ARFCN-ValueEUTRA OPTIONAL,

scg-CellGroupConfigEUTRA OCTET STRING OPTIONAL,

candidateCellInfoListSN-EUTRA OCTET STRING OPTIONAL,

candidateServingFreqListEUTRA CandidateServingFreqListEUTRA OPTIONAL,

needForGaps ENUMERATED {true} OPTIONAL,

drx-ConfigSCG DRX-Config OPTIONAL,

reportCGI-RequestEUTRA SEQUENCE {

requestedCellInfoEUTRA SEQUENCE {

eutraFrequency ARFCN-ValueEUTRA,

cellForWhichToReportCGI-EUTRA EUTRA-PhysCellId

} OPTIONAL

} OPTIONAL,

nonCriticalExtension CG-Config-v1590-IEs OPTIONAL

}

CG-Config-v1590-IEs ::= SEQUENCE {

scellFrequenciesSN-NR SEQUENCE (SIZE (1.. maxNrofServingCells-1)) OF ARFCN-ValueNR OPTIONAL,

scellFrequenciesSN-EUTRA SEQUENCE (SIZE (1.. maxNrofServingCells-1)) OF ARFCN-ValueEUTRA OPTIONAL,

nonCriticalExtension CG-Config-v1610-IEs OPTIONAL

}

CG-Config-v1610-IEs ::= SEQUENCE {

drx-InfoSCG2 DRX-Info2 OPTIONAL,

nonCriticalExtension CG-Config-v1620-IEs OPTIONAL

}

CG-Config-v1620-IEs ::= SEQUENCE {

ueAssistanceInformationSCG-r16 OCTET STRING (CONTAINING UEAssistanceInformation) OPTIONAL,

nonCriticalExtension CG-Config-v1630-IEs OPTIONAL

}

CG-Config-v1630-IEs ::= SEQUENCE {

selectedToffset-r16 T-Offset-r16 OPTIONAL,

nonCriticalExtension CG-Config-v1640-IEs OPTIONAL

}

CG-Config-v1640-IEs ::= SEQUENCE {

servCellInfoListSCG-NR-r16 ServCellInfoListSCG-NR-r16 OPTIONAL,

servCellInfoListSCG-EUTRA-r16 ServCellInfoListSCG-EUTRA-r16 OPTIONAL,

nonCriticalExtension CG-Config-v1700-IEs OPTIONAL

}

CG-Config-v1700-IEs ::= SEQUENCE {

candidateCellInfoListCPC-r17 CandidateCellInfoListCPC-r17 OPTIONAL,

twoPHRModeSCG-r17 ENUMERATED {enabled} OPTIONAL,

nonCriticalExtension CG-Config-v1730-IEs OPTIONAL

}

CG-Config-v1730-IEs ::= SEQUENCE {

fr1-Carriers-SCG-r17 INTEGER (1..32) OPTIONAL,

fr2-Carriers-SCG-r17 INTEGER (1..32) OPTIONAL,

nonCriticalExtension CG-Config-v1800-IEs OPTIONAL

}

CG-Config-v1800-IEs ::= SEQUENCE {

candidateCellInfoListCPC-v18xy CandidateCellInfoListCPCExt-v18xy OPTIONAL,

SCPAC-ReferenceConfigurationSCG-r18 OCTET STRING (CONTAINING RRCReconfiguration) OPTIONAL,

nonCriticalExtension SEQUENCE{} OPTIONAL

}

ServCellInfoListSCG-NR-r16 ::= SEQUENCE (SIZE (1.. maxNrofServingCells)) OF ServCellInfoXCG-NR-r16

ServCellInfoXCG-NR-r16 ::= SEQUENCE {

dl-FreqInfo-NR-r16 FrequencyConfig-NR-r16 OPTIONAL,

ul-FreqInfo-NR-r16 FrequencyConfig-NR-r16 OPTIONAL, -- Cond FDD

...

}

FrequencyConfig-NR-r16 ::= SEQUENCE {

freqBandIndicatorNR-r16 FreqBandIndicatorNR,

carrierCenterFreq-NR-r16 ARFCN-ValueNR,

carrierBandwidth-NR-r16 INTEGER (1..maxNrofPhysicalResourceBlocks),

subcarrierSpacing-NR-r16 SubcarrierSpacing

}

ServCellInfoListSCG-EUTRA-r16 ::= SEQUENCE (SIZE (1.. maxNrofServingCellsEUTRA)) OF ServCellInfoXCG-EUTRA-r16

ServCellInfoXCG-EUTRA-r16 ::= SEQUENCE {

dl-CarrierFreq-EUTRA-r16 ARFCN-ValueEUTRA OPTIONAL,

ul-CarrierFreq-EUTRA-r16 ARFCN-ValueEUTRA OPTIONAL, -- Cond FDD

transmissionBandwidth-EUTRA-r16 TransmissionBandwidth-EUTRA-r16 OPTIONAL,

...

}

TransmissionBandwidth-EUTRA-r16 ::= ENUMERATED {rb6, rb15, rb25, rb50, rb75, rb100}

PH-TypeListSCG ::= SEQUENCE (SIZE (1..maxNrofServingCells)) OF PH-InfoSCG

PH-InfoSCG ::= SEQUENCE {

servCellIndex ServCellIndex,

ph-Uplink PH-UplinkCarrierSCG,

ph-SupplementaryUplink PH-UplinkCarrierSCG OPTIONAL,

...,

[[

twoSRS-PUSCH-Repetition-r17 ENUMERATED{enabled} OPTIONAL

]]

}

PH-UplinkCarrierSCG ::= SEQUENCE{

ph-Type1or3 ENUMERATED {type1, type3},

...

}

MeasConfigSN ::= SEQUENCE {

measuredFrequenciesSN SEQUENCE (SIZE (1..maxMeasFreqsSN)) OF NR-FreqInfo OPTIONAL,

...

}

NR-FreqInfo ::= SEQUENCE {

measuredFrequency ARFCN-ValueNR OPTIONAL,

...

}

ConfigRestrictModReqSCG ::= SEQUENCE {

requestedBC-MRDC BandCombinationInfoSN OPTIONAL,

requestedP-MaxFR1 P-Max OPTIONAL,

...,

[[

requestedPDCCH-BlindDetectionSCG INTEGER (1..15) OPTIONAL,

requestedP-MaxEUTRA P-Max OPTIONAL

]],

[[

requestedP-MaxFR2-r16 P-Max OPTIONAL,

requestedMaxInterFreqMeasIdSCG-r16 INTEGER(1..maxMeasIdentitiesMN) OPTIONAL,

requestedMaxIntraFreqMeasIdSCG-r16 INTEGER(1..maxMeasIdentitiesMN) OPTIONAL,

requestedToffset-r16 T-Offset-r16 OPTIONAL

]],

[[

reservedResourceConfigNRDC-r17 ResourceConfigNRDC-r17 OPTIONAL

]]

}

BandCombinationIndex ::= INTEGER (1..maxBandComb)

BandCombinationInfoSN ::= SEQUENCE {

bandCombinationIndex BandCombinationIndex,

requestedFeatureSets FeatureSetEntryIndex

}

FR-InfoList ::= SEQUENCE (SIZE (1..maxNrofServingCells-1)) OF FR-Info

FR-Info ::= SEQUENCE {

servCellIndex ServCellIndex,

fr-Type ENUMERATED {fr1, fr2}

}

CandidateServingFreqListNR ::= SEQUENCE (SIZE (1.. maxFreqIDC-MRDC)) OF ARFCN-ValueNR

CandidateServingFreqListEUTRA ::= SEQUENCE (SIZE (1.. maxFreqIDC-MRDC)) OF ARFCN-ValueEUTRA

T-Offset-r16 ::= ENUMERATED {ms0dot5, ms0dot75, ms1, ms1dot5, ms2, ms2dot5, ms3, spare1}

CandidateCellInfoListCPC-r17 ::= SEQUENCE (SIZE (1..maxFreq)) OF CandidateCellInfo-r17

CandidateCellInfo-r17 ::= SEQUENCE {

ssbFrequency-r17 ARFCN-ValueNR,

candidateList-r17 SEQUENCE (SIZE (1..maxNrofCondCells-r16)) OF CandidateCell-r17

}

CandidateCell-r17 ::= SEQUENCE {

physCellId-r17 PhysCellId,

condExecutionCondSCG-r17 OCTET STRING (CONTAINING CondReconfigExecCondSCG-r17) OPTIONAL

}

CandidateCellInfoListCPCExt-v18xy ::= SEQUENCE (SIZE (1..maxFreq)) OF CandidateCellInfoExt-v18xy

CandidateCellInfoExt-v18xy ::= SEQUENCE {

ssbFrequency-r17 ARFCN-ValueNR,

candidateList-v18xy SEQUENCE (SIZE (1..maxNrofCondCells-r16)) OF CandidateCellExt-v18xy

CandidateCellExt-v18xy ::= SEQUENCE {

physCellId-r17 PhysCellId,

subsequentExecCondConfig-r18 OCTET STRING (CONTAINING CondReconfigExecCondSCG-r17) OPTIONAL

}

-- TAG-CG-CONFIG-STOP

-- ASN1STOP

|  |
| --- |
| ***CG-Config* field descriptions** |
| ***candidateCellInfoListCPC,*** ***candidateCellInfoListCPCExt***  Contains information regarding candidate target cells for Conditional PSCell Change (CPC) or subsequent CPC that the source master gNB or secondary gNB suggests the target secondary gNB to consider configuring for CPC or subsequent CPC. |
| ***candidateCellInfoListSN***  Contains information regarding cells that the source secondary node suggests the target secondary gNB to consider configuring. |
| ***candidateCellInfoListSN-EUTRA***  Includes the *MeasResultList3EUTRA* as specified in TS 36.331 [10]. Contains information regarding cells that the source secondary node suggests the target secondary eNB to consider configuring. This field is only used in NE-DC. |
| ***candidateServingFreqListNR, candidateServingFreqListEUTRA***  Indicates frequencies of candidate serving cells for In-Device Co-existence Indication (see TS 36.331 [10]). |
| ***configRestrictModReq***  Used by SN to request changes to SCG configuration restrictions previously set by MN to ensure UE capabilities are respected. E.g. can be used to request configuring an NR band combination whose use MN has previously forbidden. SN only includes this field in SN-initiated procedures. |
| ***drx-ConfigSCG***  This field contains the complete DRX configuration of the SCG. This field is only used in NR-DC. |
| ***drx-InfoSCG***  This field contains the DRX long and short cycle configuration of the SCG. This field is used in (NG)EN-DC and NE-DC. |
| ***drx-InfoSCG2***  This field contains the drx-onDurationTimer configuration of the SCG. This field is only used in (NG)EN-DC. |
| ***fr-InfoListSCG***  Contains information of FR information of serving cells that include PScell and SCells configured in SCG. |
| ***fr1-Carriers-SCG, fr2-Carriers-SCG***  Indicates the number of FR1 or FR2 serving cells configured in SCG. |
| ***measuredFrequenciesSN***  Used by SN to indicate a list of frequencies measured by the UE. |
| ***needForGaps***  In NE-DC, indicates whether the SN requests gNB to configure measurements gaps. |
| ***ph-InfoSCG***  Power headroom information in SCG that is needed in the reception of PHR MAC CE of MCG |
| ***ph-SupplementaryUplink***  Power headroom information for supplementary uplink. In the case of (NG)EN-DC and NR-DC, this field is only present when two UL carriers are configured for a serving cell and one UL carrier reports type1 PH while the other reports type 3 PH. |
| ***ph-Type1or3***  Type of power headroom for a certain serving cell in SCG (PSCell and activated SCells). Value *type1* refers to type 1 power headroom, value *type3* refers to type 3 power headroom. (See TS 38.321 [3]). |
| ***ph-Uplink***  Power headroom information for uplink. |
| ***pSCellFrequency, pSCellFrequencyEUTRA***  Indicates the frequency of PSCell in NR (i.e., *pSCellFrequency*) or E-UTRA (i.e., *pSCellFrequencyEUTRA*). In this version of the specification, *pSCellFrequency* is not used in NE-DC whereas *pSCellFrequencyEUTRA* is only used in NE-DC. *pSCellFrequency* indicates the *absoluteFrequencySSB*. |
| ***reportCGI-RequestNR, reportCGI-RequestEUTRA***  Used by SN to indicate to MN about configuring *reportCGI* procedure. The request may optionally contain information about the cell for which SN intends to configure *reportCGI* procedure. In this version of the specification, the *reportCGI-RequestNR* is used in (NG)EN-DC and NR-DC whereas *reportCGI-RequestEUTRA* is used only for NE-DC. |
| ***requestedBC-MRDC***  Used to request configuring a band combination and corresponding feature sets which are forbidden to use by MN (i.e. outside of the *allowedBC-ListMRDC*) to allow re-negotiation of the UE capabilities for SCG configuration. |
| ***reservedResourceConfigNRDC***  Used to request or indicate the maximum number of resources reserved for the SCG. This field is only used in NR-DC. |
| ***requestedMaxInterFreqMeasIdSCG***  Used to request the maximum number of allowed measurement identities to configure for inter-frequency measurement. This field is only used in NR-DC. |
| ***requestedMaxIntraFreqMeasIdSCG***  Used to request the maximum number of allowed measurement identities to configure for intra-frequency measurement on each serving frequency. |
| ***requestedPDCCH-BlindDetectionSCG***  Requested value of the reference number of cells for PDCCH blind detection allowed to be configured for the SCG. |
| ***requestedP-MaxEUTRA***  Requested value for the maximum power for the serving cells the UE can use in E-UTRA SCG. This field is only used in NE-DC. |
| ***requestedP-MaxFR1***  Requested value for the maximum power for the serving cells on frequency range 1 (FR1) in this secondary cell group (see TS 38.104 [12]) the UE can use in NR SCG. |
| ***requestedP-MaxFR2***  Requested value for the maximum power for the serving cells on frequency range 2 (FR2) in this secondary cell group the UE can use in NR SCG. This field is only used in NR-DC. |
| ***requestedToffset***  Requests the new value for the time offset restriction used by the SN for scheduling SCG transmissions (i.e. see TS 38.213 [13]). This field is used in NR-DC only when the fields *nrdc-PC-mode-FR1-r16* or *nrdc-PC-mode-FR2-r16* are set to dynamic. Value ms0dot5 corresponds to 0.5 ms, value ms0dot75 corresponds to 0.75 ms, value ms1 corresponds to 1ms and so on. |
| ***scellFrequenciesSN-EUTRA, scellFrequenciesSN-NR***  Indicates the frequency of all SCells with SSB configured in SCG. The field *scellFrequenciesSN-EUTRA* is used in NE-DC; the field *scellFrequenciesSN-NR* is used in (NG)EN-DC and NR-DC. In (NG)EN-DC, the field is optionally provided to the MN. *scellFrequenciesSN-NR* indicates *absoluteFrequencySSB*. |
| ***scg-CellGroupConfig***  Contains the *RRCReconfiguration* message (containing only *secondaryCellGroup* and/or *measConfig* and/or *otherConfig* and/or *conditionalReconfiguration* and/or *bap-Config* and/or *iab-IP-AddressConfigurationList*):  - to be sent to the UE, used upon SCG establishment or modification (only when the SCG is not released by the SN), as generated (entirely) by the (target) SgNB. In this case, the SN sets the *RRCReconfiguration* message in accordance with clause 6 e.g. regarding the "Need" or "Cond" statements.  or  - including the current SCG configuration of the UE, when provided in response to a query from MN, or in SN triggered SN change in order to enable delta signaling by the target SN, or in SN triggered modification procedure in order to coordinate CHO or MN-initiated CPC with SCG reconfigurations (see TS 38.423 [35]). In this case, the SN sets the *RRCReconfiguration* message in accordance with clause 11.2.3.  The field is absent if neither SCG (re)configuration nor SCG configuration query nor SN triggered modification procedure in order to coordinate CHO or MN-initiated CPC with SCG reconfigurations (see TS 38.423 [35]) nor SN triggered SN change is performed, e.g. at inter-node capability/configuration coordination which does not result in SCG (re)configuration towards the UE. The field is also absent upon an SCG release triggered by the SN. This field is not applicable in NE-DC. |
| ***scg-CellGroupConfigEUTRA***  Includes the E-UTRA *RRCConnectionReconfiguration* message as specified in TS 36.331 [10]. In this version of the specification, the E-UTRA RRC message can only include the field *scg-Configuration*:  - to be sent to the UE, used to (re-)configure the SCG configuration upon SCG establishment or modification (only when the SCG is not released by the SN), as generated (entirely) by the (target) SeNB. In this case, the SN sets the *scg-Configuration* within the EUTRA *RRCConnectionReconfiguration* message in accordance with clause 6 in TS 36.331 [10] e.g. regarding the "Need" or "Cond" statements.  or  - including the current SCG configuration of the UE, when provided in response to a query from MN, or in SN triggered SN change in order to enable delta signalling by the target SN.  The field is absent if neither SCG (re)configuration nor SCG configuration query nor SN triggered SN change is performed, e.g. at inter-node capability/configuration coordination which does not result in SCG (re)configuration towards the UE. The field is also absent upon an SCG release triggered by the SN. This field is only used in NE-DC. |
| ***scg-RB-Config***  Contains the IE *RadioBearerConfig*:  - to be sent to the UE, used to (re-)configure the SCG RB configuration upon SCG establishment or modification, as generated (entirely) by the (target) SgNB or SeNB. In this case, the SN sets the *RadioBearerConfig* in accordance with clause 6, e.g. regarding the "Need" or "Cond" statements.  or  - including the current SCG RB configuration of the UE, when provided in response to a query from MN or in SN triggered SN change or in SN triggered SN release or bearer type change between SN terminated bearer to MN terminated bearer in order to enable delta signaling by the MN or target SN. In this case, the SN sets the *RadioBearerConfig* in accordance with clause 11.2.3.  The field is absent if neither SCG (re)configuration nor SCG configuration query nor SN triggered SN change nor SN triggered SN release is performed, e.g. at inter-node capability/configuration coordination which does not result in SCG RB (re)configuration. |
| ***selectedBandCombination***  Indicates the band combination selected by SN in (NG)EN-DC, NE-DC, and NR-DC. The SN should inform the MN with this field whenever the band combination and/or feature set it selected for the SCG changes (i.e. even if the new selection concerns a band combination and/or feature set that is allowed by the *allowedBC-ListMRDC*) |
| ***selectedToffset***  Indicates the value used by the SN for scheduling SCG transmissions (i.e. see TS 38.213 [13]). This field is used in NR-DC only when the fields *nrdc-PC-mode-FR1-r16* or *nrdc-PC-mode-FR2-r16* are set to dynamic. The SN can only indicate a value that is less than or equal to *maxToffset* received from MN. This field is used in NR-DC only when MN has included the field *maxToffset* in *CG-ConfigInfo*. Value *ms0dot5* corresponds to 0.5 ms, value *ms0dot75* corresponds to 0.75 ms, value *ms1* corresponds to 1ms and so on. |
| ***servCellInfoListSCG-EUTRA***  Indicates the carrier frequency and the transmission bandwidth of the serving cell(s) in the SCG in intra-band NE-DC. The field is needed when MN and SN operate serving cells in the same band for either contiguous or non-contiguous intra-band band combination or LTE NR inter-band band combinations where the frequency range of the E-UTRA band is a subset of the frequency range of the NR band (as specified in Table 5.5B.4.1-1 of TS 38.101-3 [34]) in NE-DC. |
| ***servCellInfoListSCG-NR***  Indicates the frequency band indicator, carrier center frequency, UE specific channel bandwidth and SCS of the serving cell(s) in the SCG in intra-band (NG)EN-DC. The field is needed when MN and SN operate serving cells in the same band for either contiguous or non-contiguous intra-band band combination or LTE NR inter-band band combinations where the frequency range of the E-UTRA band is a subset of the frequency range of the NR band (as specified in Table 5.5B.4.1-1 of TS 38.101-3 [34]) in (NG)EN-DC. |
| ***subsequentExecCondConfig***  Includes the the execution conditions for subsequent CPC when the candidate SN prepares the candidate SCG configuration(s) for candidate PSCell(s). |
| ***twoPHRModeSCG***  Indicates if the power headroom for SCG shall be reported as two PHRs (each PHR associated with a SRS resource set) is enabled or not. |
| ***twoSRS-PUSCH-Repetition***  Indicates whether the indicated serving cell is configured for PUSCH repetition corresponding to two SRS resource sets configured in either *srs-ResourceSetToAddModList* or *srs-ResourceSetToAddModListDCI-0-2* with usage 'codebook' or 'noncodebook'. |
| ***transmissionBandwidth-EUTRA***  Indicates the transmission bandwidth on an E-UTRA carrier frequency as defined by the parameter Transmission Bandwidth Configuration "NRB" TS 36.104 [33]. The values rb6, rb15, rb25, rb50, rb75, rb100 indicate 6, 15, 25, 50, 75 and 100 resource blocks respectively. |
| ***ueAssistanceInformationSCG***  Includes for each UE assistance feature associated with the SCG, the information last reported by the UE in the NR *UEAssistanceInformation* message for the SCG, if any. |

|  |
| --- |
| ***BandCombinationInfoSN* field descriptions** |
| ***bandCombinationIndex***  In case of NR-DC, this field indicates the position of a band combination in the *supportedBandCombinationList*. In case of NE-DC, this field indicates the position of a band combination in the *supportedBandCombinationList* and/or *supportedBandCombinationListNEDC-Only*. In case of (NG)EN-DC, this field indicates the position of a band combination in the *supportedBandCombinationList* and/or *supportedBandCombinationList-UplinkTxSwitch*. Band combination entries in *supportedBandCombinationList* are referred by an index which corresponds to the position of a band combination in the *supportedBandCombinationList*. Band combination entries in *supportedBandCombinationListNEDC-Only* are referred by an index which corresponds to the position of a band combination in the *supportedBandCombinationListNEDC-Only* increased by the number of entries in *supportedBandCombinationList*. Band combination entries in *supportedBandCombinationList-UplinkTxSwitch* are referred by an index which corresponds to the position of a band combination in the *supportedBandCombinationList-UplinkTxSwitch* increased by the number of entries in *supportedBandCombinationList*. |
| ***requestedFeatureSets***  The position in the *FeatureSetCombination* which identifies one *FeatureSetUplink*/*Downlink* for each band entry in the associated band combination |

|  |  |
| --- | --- |
| **Conditional Presence** | **Explanation** |
| *FDD* | This field is mandatory present if dl-FreqInfo-NR is included and concerns an FDD carrier; otherwise the field is absent. |

#### *– CG-ConfigInfo*

This message is used by master eNB or gNB to request the SgNB or SeNB to perform certain actions e.g. to establish, modify or release an SCG. The message may include additional information e.g. to assist the SgNB or SeNB to set the SCG configuration. It can also be used by a CU to request a DU to perform certain actions, e.g. to establish, or modify an MCG or SCG.

Direction: Master eNB or gNB to secondary gNB or eNB, alternatively CU to DU.

*CG-ConfigInfo* message

-- ASN1START

-- TAG-CG-CONFIG-INFO-START

CG-ConfigInfo ::= SEQUENCE {

criticalExtensions CHOICE {

c1 CHOICE{

cg-ConfigInfo CG-ConfigInfo-IEs,

spare3 NULL, spare2 NULL, spare1 NULL

},

criticalExtensionsFuture SEQUENCE {}

}

}

CG-ConfigInfo-IEs ::= SEQUENCE {

ue-CapabilityInfo OCTET STRING (CONTAINING UE-CapabilityRAT-ContainerList) OPTIONAL,-- Cond SN-AddMod

candidateCellInfoListMN MeasResultList2NR OPTIONAL,

candidateCellInfoListSN OCTET STRING (CONTAINING MeasResultList2NR) OPTIONAL,

measResultCellListSFTD-NR MeasResultCellListSFTD-NR OPTIONAL,

scgFailureInfo SEQUENCE {

failureType ENUMERATED { t310-Expiry, randomAccessProblem,

rlc-MaxNumRetx, synchReconfigFailure-SCG,

scg-reconfigFailure,

srb3-IntegrityFailure},

measResultSCG OCTET STRING (CONTAINING MeasResultSCG-Failure)

} OPTIONAL,

configRestrictInfo ConfigRestrictInfoSCG OPTIONAL,

drx-InfoMCG DRX-Info OPTIONAL,

measConfigMN MeasConfigMN OPTIONAL,

sourceConfigSCG OCTET STRING (CONTAINING RRCReconfiguration) OPTIONAL,

scg-RB-Config OCTET STRING (CONTAINING RadioBearerConfig) OPTIONAL,

mcg-RB-Config OCTET STRING (CONTAINING RadioBearerConfig) OPTIONAL,

mrdc-AssistanceInfo MRDC-AssistanceInfo OPTIONAL,

nonCriticalExtension CG-ConfigInfo-v1540-IEs OPTIONAL

}

CG-ConfigInfo-v1540-IEs ::= SEQUENCE {

ph-InfoMCG PH-TypeListMCG OPTIONAL,

measResultReportCGI SEQUENCE {

ssbFrequency ARFCN-ValueNR,

cellForWhichToReportCGI PhysCellId,

cgi-Info CGI-InfoNR

} OPTIONAL,

nonCriticalExtension CG-ConfigInfo-v1560-IEs OPTIONAL

}

CG-ConfigInfo-v1560-IEs ::= SEQUENCE {

candidateCellInfoListMN-EUTRA OCTET STRING OPTIONAL,

candidateCellInfoListSN-EUTRA OCTET STRING OPTIONAL,

sourceConfigSCG-EUTRA OCTET STRING OPTIONAL,

scgFailureInfoEUTRA SEQUENCE {

failureTypeEUTRA ENUMERATED { t313-Expiry, randomAccessProblem,

rlc-MaxNumRetx, scg-ChangeFailure},

measResultSCG-EUTRA OCTET STRING

} OPTIONAL,

drx-ConfigMCG DRX-Config OPTIONAL,

measResultReportCGI-EUTRA SEQUENCE {

eutraFrequency ARFCN-ValueEUTRA,

cellForWhichToReportCGI-EUTRA EUTRA-PhysCellId,

cgi-InfoEUTRA CGI-InfoEUTRA

} OPTIONAL,

measResultCellListSFTD-EUTRA MeasResultCellListSFTD-EUTRA OPTIONAL,

fr-InfoListMCG FR-InfoList OPTIONAL,

nonCriticalExtension CG-ConfigInfo-v1570-IEs OPTIONAL

}

CG-ConfigInfo-v1570-IEs ::= SEQUENCE {

sftdFrequencyList-NR SFTD-FrequencyList-NR OPTIONAL,

sftdFrequencyList-EUTRA SFTD-FrequencyList-EUTRA OPTIONAL,

nonCriticalExtension CG-ConfigInfo-v1590-IEs OPTIONAL

}

CG-ConfigInfo-v1590-IEs ::= SEQUENCE {

servFrequenciesMN-NR SEQUENCE (SIZE (1.. maxNrofServingCells-1)) OF ARFCN-ValueNR OPTIONAL,

nonCriticalExtension CG-ConfigInfo-v1610-IEs OPTIONAL

}

CG-ConfigInfo-v1610-IEs ::= SEQUENCE {

drx-InfoMCG2 DRX-Info2 OPTIONAL,

alignedDRX-Indication ENUMERATED {true} OPTIONAL,

scgFailureInfo-r16 SEQUENCE {

failureType-r16 ENUMERATED { scg-lbtFailure-r16, beamFailureRecoveryFailure-r16,

t312-Expiry-r16, bh-RLF-r16,

beamFailure-r17, spare3, spare2, spare1},

measResultSCG-r16 OCTET STRING (CONTAINING MeasResultSCG-Failure)

} OPTIONAL,

dummy1 SEQUENCE {

failureTypeEUTRA-r16 ENUMERATED { scg-lbtFailure-r16, beamFailureRecoveryFailure-r16,

t312-Expiry-r16, spare5,

spare4, spare3, spare2, spare1},

measResultSCG-EUTRA-r16 OCTET STRING

} OPTIONAL,

sidelinkUEInformationNR-r16 OCTET STRING (CONTAINING SidelinkUEInformationNR-r16) OPTIONAL,

sidelinkUEInformationEUTRA-r16 OCTET STRING OPTIONAL,

nonCriticalExtension CG-ConfigInfo-v1620-IEs OPTIONAL

}

CG-ConfigInfo-v1620-IEs ::= SEQUENCE {

ueAssistanceInformationSourceSCG-r16 OCTET STRING (CONTAINING UEAssistanceInformation) OPTIONAL,

nonCriticalExtension CG-ConfigInfo-v1640-IEs OPTIONAL

}

CG-ConfigInfo-v1640-IEs ::= SEQUENCE {

servCellInfoListMCG-NR-r16 ServCellInfoListMCG-NR-r16 OPTIONAL,

servCellInfoListMCG-EUTRA-r16 ServCellInfoListMCG-EUTRA-r16 OPTIONAL,

nonCriticalExtension CG-ConfigInfo-v1700-IEs OPTIONAL

}

CG-ConfigInfo-v1700-IEs ::= SEQUENCE {

candidateCellListCPC-r17 CandidateCellListCPC-r17 OPTIONAL,

twoPHRModeMCG-r17 ENUMERATED {enabled} OPTIONAL,

lowMobilityEvaluationConnectedInPCell-r17 ENUMERATED {enabled} OPTIONAL,

nonCriticalExtension CG-ConfigInfo-v1730-IEs OPTIONAL

}

CG-ConfigInfo-v1730-IEs ::= SEQUENCE {

fr1-Carriers-MCG-r17 INTEGER (1..32) OPTIONAL,

fr2-Carriers-MCG-r17 INTEGER (1..32) OPTIONAL,

nonCriticalExtension CG-ConfigInfo-v1800-IEs OPTIONAL

}

CG-ConfigInfo-v1800-IEs ::= SEQUENCE {

SCPAC-ReferenceConfiguration-r18 OCTET STRING (CONTAINING RRCReconfiguration) OPTIONAL,

nonCriticalExtension SEQUENCE {} OPTIONAL

}

ServCellInfoListMCG-NR-r16 ::= SEQUENCE (SIZE (1.. maxNrofServingCells)) OF ServCellInfoXCG-NR-r16

ServCellInfoListMCG-EUTRA-r16 ::= SEQUENCE (SIZE (1.. maxNrofServingCellsEUTRA)) OF ServCellInfoXCG-EUTRA-r16

SFTD-FrequencyList-NR ::= SEQUENCE (SIZE (1..maxCellSFTD)) OF ARFCN-ValueNR

SFTD-FrequencyList-EUTRA ::= SEQUENCE (SIZE (1..maxCellSFTD)) OF ARFCN-ValueEUTRA

ConfigRestrictInfoSCG ::= SEQUENCE {

allowedBC-ListMRDC BandCombinationInfoList OPTIONAL,

powerCoordination-FR1 SEQUENCE {

p-maxNR-FR1 P-Max OPTIONAL,

p-maxEUTRA P-Max OPTIONAL,

p-maxUE-FR1 P-Max OPTIONAL

} OPTIONAL,

servCellIndexRangeSCG SEQUENCE {

lowBound ServCellIndex,

upBound ServCellIndex

} OPTIONAL, -- Cond SN-AddMod

maxMeasFreqsSCG INTEGER(1..maxMeasFreqsMN) OPTIONAL,

dummy INTEGER(1..maxMeasIdentitiesMN) OPTIONAL,

...,

[[

selectedBandEntriesMNList SEQUENCE (SIZE (1..maxBandComb)) OF SelectedBandEntriesMN OPTIONAL,

pdcch-BlindDetectionSCG INTEGER (1..15) OPTIONAL,

maxNumberROHC-ContextSessionsSN INTEGER(0.. 16384) OPTIONAL

]],

[[

maxIntraFreqMeasIdentitiesSCG INTEGER(1..maxMeasIdentitiesMN) OPTIONAL,

maxInterFreqMeasIdentitiesSCG INTEGER(1..maxMeasIdentitiesMN) OPTIONAL

]],

[[

p-maxNR-FR1-MCG-r16 P-Max OPTIONAL,

powerCoordination-FR2-r16 SEQUENCE {

p-maxNR-FR2-MCG-r16 P-Max OPTIONAL,

p-maxNR-FR2-SCG-r16 P-Max OPTIONAL,

p-maxUE-FR2-r16 P-Max OPTIONAL

} OPTIONAL,

nrdc-PC-mode-FR1-r16 ENUMERATED {semi-static-mode1, semi-static-mode2, dynamic} OPTIONAL,

nrdc-PC-mode-FR2-r16 ENUMERATED {semi-static-mode1, semi-static-mode2, dynamic} OPTIONAL,

maxMeasSRS-ResourceSCG-r16 INTEGER(0..maxNrofCLI-SRS-Resources-r16) OPTIONAL,

maxMeasCLI-ResourceSCG-r16 INTEGER(0..maxNrofCLI-RSSI-Resources-r16) OPTIONAL,

maxNumberEHC-ContextsSN-r16 INTEGER(0..65536) OPTIONAL,

allowedReducedConfigForOverheating-r16 OverheatingAssistance OPTIONAL,

maxToffset-r16 T-Offset-r16 OPTIONAL

]],

[[

allowedReducedConfigForOverheating-r17 OverheatingAssistance-r17 OPTIONAL,

maxNumberUDC-DRB-r17 INTEGER(0..2) OPTIONAL,

maxNumberCPCCandidates-r17 INTEGER(0..maxNrofCondCells-1-r17) OPTIONAL

]],

[[

allowedResourceConfigNRDC-r17 ResourceConfigNRDC-r17 OPTIONAL

]]

}

SelectedBandEntriesMN ::= SEQUENCE (SIZE (1..maxSimultaneousBands)) OF BandEntryIndex

BandEntryIndex ::= INTEGER (0.. maxNrofServingCells)

PH-TypeListMCG ::= SEQUENCE (SIZE (1..maxNrofServingCells)) OF PH-InfoMCG

PH-InfoMCG ::= SEQUENCE {

servCellIndex ServCellIndex,

ph-Uplink PH-UplinkCarrierMCG,

ph-SupplementaryUplink PH-UplinkCarrierMCG OPTIONAL,

...,

[[

twoSRS-PUSCH-Repetition-r17 ENUMERATED{enabled} OPTIONAL

]]

}

PH-UplinkCarrierMCG ::= SEQUENCE{

ph-Type1or3 ENUMERATED {type1, type3},

...

}

BandCombinationInfoList ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombinationInfo

BandCombinationInfo ::= SEQUENCE {

bandCombinationIndex BandCombinationIndex,

allowedFeatureSetsList SEQUENCE (SIZE (1..maxFeatureSetsPerBand)) OF FeatureSetEntryIndex

}

FeatureSetEntryIndex ::= INTEGER (1.. maxFeatureSetsPerBand)

DRX-Info ::= SEQUENCE {

drx-LongCycleStartOffset CHOICE {

ms10 INTEGER(0..9),

ms20 INTEGER(0..19),

ms32 INTEGER(0..31),

ms40 INTEGER(0..39),

ms60 INTEGER(0..59),

ms64 INTEGER(0..63),

ms70 INTEGER(0..69),

ms80 INTEGER(0..79),

ms128 INTEGER(0..127),

ms160 INTEGER(0..159),

ms256 INTEGER(0..255),

ms320 INTEGER(0..319),

ms512 INTEGER(0..511),

ms640 INTEGER(0..639),

ms1024 INTEGER(0..1023),

ms1280 INTEGER(0..1279),

ms2048 INTEGER(0..2047),

ms2560 INTEGER(0..2559),

ms5120 INTEGER(0..5119),

ms10240 INTEGER(0..10239)

},

shortDRX SEQUENCE {

drx-ShortCycle ENUMERATED {

ms2, ms3, ms4, ms5, ms6, ms7, ms8, ms10, ms14, ms16, ms20, ms30, ms32,

ms35, ms40, ms64, ms80, ms128, ms160, ms256, ms320, ms512, ms640, spare9,

spare8, spare7, spare6, spare5, spare4, spare3, spare2, spare1 },

drx-ShortCycleTimer INTEGER (1..16)

} OPTIONAL

}

DRX-Info2 ::= SEQUENCE {

drx-onDurationTimer CHOICE {

subMilliSeconds INTEGER (1..31),

milliSeconds ENUMERATED {

ms1, ms2, ms3, ms4, ms5, ms6, ms8, ms10, ms20, ms30, ms40, ms50, ms60,

ms80, ms100, ms200, ms300, ms400, ms500, ms600, ms800, ms1000, ms1200,

ms1600, spare8, spare7, spare6, spare5, spare4, spare3, spare2, spare1 }

}

}

MeasConfigMN ::= SEQUENCE {

measuredFrequenciesMN SEQUENCE (SIZE (1..maxMeasFreqsMN)) OF NR-FreqInfo OPTIONAL,

measGapConfig SetupRelease { GapConfig } OPTIONAL,

gapPurpose ENUMERATED {perUE, perFR1} OPTIONAL,

...,

[[

measGapConfigFR2 SetupRelease { GapConfig } OPTIONAL

]],

[[

interFreqNoGap-r16 ENUMERATED {true} OPTIONAL

]]

}

MRDC-AssistanceInfo ::= SEQUENCE {

affectedCarrierFreqCombInfoListMRDC SEQUENCE (SIZE (1..maxNrofCombIDC)) OF AffectedCarrierFreqCombInfoMRDC,

...,

[[

overheatingAssistanceSCG-r16 OCTET STRING (CONTAINING OverheatingAssistance) OPTIONAL

]],

[[

overheatingAssistanceSCG-FR2-2-r17 OCTET STRING (CONTAINING OverheatingAssistance-r17) OPTIONAL

]]

}

AffectedCarrierFreqCombInfoMRDC ::= SEQUENCE {

victimSystemType VictimSystemType,

interferenceDirectionMRDC ENUMERATED {eutra-nr, nr, other, utra-nr-other, nr-other, spare3, spare2, spare1},

affectedCarrierFreqCombMRDC SEQUENCE {

affectedCarrierFreqCombEUTRA AffectedCarrierFreqCombEUTRA OPTIONAL,

affectedCarrierFreqCombNR AffectedCarrierFreqCombNR

} OPTIONAL

}

VictimSystemType ::= SEQUENCE {

gps ENUMERATED {true} OPTIONAL,

glonass ENUMERATED {true} OPTIONAL,

bds ENUMERATED {true} OPTIONAL,

galileo ENUMERATED {true} OPTIONAL,

wlan ENUMERATED {true} OPTIONAL,

bluetooth ENUMERATED {true} OPTIONAL

}

AffectedCarrierFreqCombEUTRA ::= SEQUENCE (SIZE (1..maxNrofServingCellsEUTRA)) OF ARFCN-ValueEUTRA

AffectedCarrierFreqCombNR ::= SEQUENCE (SIZE (1..maxNrofServingCells)) OF ARFCN-ValueNR

CandidateCellListCPC-r17 ::= SEQUENCE (SIZE (1..maxFreq)) OF CandidateCellCPC-r17

CandidateCellCPC-r17 ::= SEQUENCE {

ssbFrequency-r17 ARFCN-ValueNR,

candidateCellList-r17 SEQUENCE (SIZE (1..maxNrofCondCells-r16)) OF PhysCellId

}

-- TAG-CG-CONFIG-INFO-STOP

-- ASN1STOP

*Editor’s Note: FFS on the IE/message to transfer the reference configuration.*

|  |
| --- |
| *CG-ConfigInfo* field descriptions |
| ***alignedDRX-Indication***  This field is signalled upon MN triggered CGI reporting by the UE that requires aligned DRX configurations between the MCG and the SCG (i.e. same DRX cycle and on-duration configured by MN completely contains on-duration configured by SN). |
| ***allowedBC-ListMRDC***  A list of indices referring to band combinations in MR-DC capabilities from which SN is allowed to select the SCG band combination. Each entry refers to:  - a band combination numbered according to *supportedBandCombinationList* and *supportedBandCombinationList-UplinkTxSwitch* in the *UE-MRDC-Capability* (in case of (NG)EN-DC), or according to *supportedBandCombinationList* and *supportedBandCombinationListNEDC-Only* in the *UE-MRDC-Capability* (in case of NE-DC), or according to *supportedBandCombinationList* in the UE-NR-Capability (in case of NR-DC),  - and the Feature Sets allowed for each band entry. All MR-DC band combinations indicated by this field comprise the MCG band combination, which is a superset of the MCG band(s) selected by MN. |
| ***allowedReducedConfigForOverheating***  Indicates the reduced configuration that the SCG is allowed to configure.  *reducedMaxCCs* in *allowedReducedConfigForOverheating* indicates the maximum number of downlink/uplink PSCell/SCells that the SCG is allowed to configure. This field is used in (NG)EN-DC and NR-DC.  *reducedMaxBW-FR1* and *reducedMaxBW-FR2* in *allowedReducedConfigForOverheating* indicates the maximum aggregated bandwidth across all downlink/uplink carriers of FR1 and FR2-1, respectively that the SCG is allowed to configure. *reducedMaxBW-FR2-2* in *allowedReducedConfigForOverheating-r17* indicates the maximum aggregated bandwidth across all downlink/uplink carriers of FR2-2 that the SCG is allowed to configure. This field is only used in NR-DC.  *reducedMaxMIMO-LayersFR1* and *reducedMaxMIMO-LayersFR2* in *allowedReducedConfigForOverheating* indicates the maximum number of downlink/uplink MIMO layers of each serving cell operating on FR1 and FR2-1, respectively that the SCG is allowed to configure. *reducedMaxMIMO-LayersFR2-2* in *allowedReducedConfigForOverheating-r17* indicates the maximum number of downlink/uplink MIMO layers of each serving cell operating on FR2-2 that the SCG is allowed to configure. This field is only used in NR-DC. |
| ***allowedResourceConfigNRDC***  Used to indicate the maximum number of resources reserved for the SCG. This field is only used in NR-DC. |
| ***candidateCellInfoListMN***, ***candidateCellInfoListSN***  Contains information regarding cells that the master node or the source node suggests the target gNB or DU to consider configuring. In case of MN initiated CPA or CPC, the field *candidateCellInfoListMN* contains information regarding cells that the MN suggests the candidate target secondary node to consider configuring for MN initiated CPA or CPC.  For (NG)EN-DC, including CSI-RS measurement results in *candidateCellInfoListMN* is not supported in this version of the specification. For NR-DC, including SSB and/or CSI-RS measurement results in *candidateCellInfoListMN* is supported. |
| ***candidateCellInfoListMN-EUTRA***, ***candidateCellInfoListSN-EUTRA***  Includes the *MeasResultList3EUTRA* as specified in TS 36.331 [10]. Contains information regarding cells that the master node or the source node suggests the target secondary eNB to consider configuring. These fields are only used in NE-DC. |
| ***candidateCellListCPC***  Contains information regarding cells that the source secondary node suggests the candidate target secondary node to consider configuring for SN initiated Conditional PSCell Change (CPC). |
| ***configRestrictInfo***  Includes fields for which SgNB is explicitly indicated to observe a configuration restriction. |
| ***drx-ConfigMCG***  This field contains the complete DRX configuration of the MCG. This field is only used in NR-DC. |
| ***drx-InfoMCG***  This field contains the DRX long and short cycle configuration of the MCG. This field is used in (NG)EN-DC and NE-DC. |
| ***drx-InfoMCG2***  This field contains the *drx-onDurationTimer* configuration of the MCG. This field is only used in (NG)EN-DC. |
| ***dummy, dummy1***  These fields are not used in the specification and SN ignores the received value(s). |
| ***fr-InfoListMCG***  Contains information of FR information of serving cells that include PCell and SCell(s) configured in MCG. |
| ***fr1-Carriers-MCG, fr2-Carriers-MCG***  Indicates the number of FR1 or FR2 serving cells configured in MCG. |
| ***interFreqNoGap***  Indicates that the field *interFrequencyConfig-NoGap-r16* has been included within the *MeasConfig* IE generated by the MN. |
| ***lowMobilityEvaluationConnectedInPCell***  Indicates if low mobility criterion has been configured in NR PCell. |
| ***maxInterFreqMeasIdentitiesSCG***  Indicates the maximum number of allowed measurement identities that the SCG is allowed to configure for inter-frequency measurement. The maximum value for this field is 10. If the field is absent, the SCG is allowed to configure inter-frequency measurements up to the maximum value. This field is only used in NR-DC. |
| ***maxIntraFreqMeasIdentitiesSCG***  Indicates the maximum number of allowed measurement identities that the SCG is allowed to configure for intra-frequency measurement on each serving frequency. The maximum value for this field is 9 (in case of (NG)EN-DC or NR-DC) or 10 (in case of NE-DC). If the field is absent, the SCG is allowed to configure intra-frequency measurements up to the maximum value on each serving frequency. |
| ***maxMeasCLI-ResourceSCG***  Indicates the maximum number of CLI RSSI resources that the SCG is allowed to configure. |
| ***maxMeasFreqsSCG***  Indicates the maximum number of NR inter-frequency carriers the SN is allowed to configure with PSCell for measurements. |
| ***maxMeasSRS-ResourceSCG***  Indicates the maximum number of SRS resources that the SCG is allowed to configure for CLI measurement. |
| ***maxNumberCPCCandidates***  Indicates the maximum numbers of conditional reconfigurations the SN is allowed to configure for SN initiated CPC. Value 0 indicates that the SN is not allowed to configure SN initiated CPC. If the field is absent, the SN is allowed to configure up to *maxNrofCondCells-r16* conditional reconfigurations for SN-initiated CPC. |
| ***maxNumberROHC-ContextSessionsSN***  Indicates the maximum number of ROHC context sessions allowed to SN terminated bearer, excluding context sessions that leave all headers uncompressed. |
| ***maxNumberEHC-ContextsSN***  Indicates the maximum number of EHC contexts allowed to the SN terminated bearer. The field indicates the number of contexts in addition to CID = "all zeros", as specified in TS 38.323 [5]. |
| ***maxNumberUDC-DRB***  Indicates the maximum number of UDC DRBs allowed to SN terminated bearer. This field is used in NGEN-DC, NR-DC and NE-DC. |
| ***maxToffset***  Indicates the maximum Toffset value the SN is allowed to use for scheduling SCG transmissions (see TS 38.213 [13]). This field is used in NR-DC only when the fields *nrdc-PC-mode-FR1-r16* or *nrdc-PC-mode-FR2-r16* are set to dynamic. Value *ms0dot5* corresponds to 0.5 ms, value *ms0dot75* corresponds to 0.75 ms, value *ms1* corresponds to 1 ms and so on. |
| ***measuredFrequenciesMN***  Used by MN to indicate a list of frequencies measured by the UE. |
| ***measGapConfig***  Indicates the FR1 and perUE measurement gap configuration configured by MN. |
| ***measGapConfigFR2***  Indicates the FR2 measurement gap configuration configured by MN. |
| ***mcg-RB-Config***  Contains all of the fields in the IE *RadioBearerConfig* used in MN, used by the SN to support delta configuration to UE (i.e. when MN does not use full configuration option), for bearer type change between MN terminated bearer with NR PDCP to SN terminated bearer. It is also used to indicate the PDCP duplication related information for MN terminated split bearer (whether duplication is configured and if so, whether it is initially activated) in SN Addition/Modification procedure. Otherwise, this field is absent. |
| ***measResultReportCGI, measResultReportCGI-EUTRA***  Used by MN to provide SN with CGI-Info for the cell as per SN′s request. In this version of the specification, the *measResultReportCGI* is used for (NG)EN-DC and NR-DC and the *measResultReportCGI-EUTRA* is used only for NE-DC. |
| ***measResultSCG-EUTRA***  This field includes the *MeasResultSCG-FailureMRDC* IE as specified in TS 36.331 [10]. This field is only used in NE-DC. |
| ***measResultSFTD-EUTRA***  SFTD measurement results between the PCell and the E-UTRA PScell in NE-DC. This field is only used in NE-DC. |
| ***mrdc-AssistanceInfo***  Contains the IDC assistance information for MR-DC reported by the UE (see TS 36.331 [10]). |
| ***nrdc-PC-mode-FR1***  Indicates the uplink power sharing mode that the UE uses in NR-DC FR1 (see TS 38.213 [13], clause 7.6). |
| ***nrdc-PC-mode-FR2***  Indicates the uplink power sharing mode that the UE uses in NR-DC FR2 (see TS 38.213 [13], clause 7.6). |
| ***overheatingAssistanceSCG***  Contains the UE's preference on reduced configuration for NR SCG to address overheating. This field is only used in (NG)EN-DC. |
| ***overheatingAssistanceSCG-FR2-2***  Contains the UE's preference on reduced configuration for NR SCG on FR2-2 to address overheating. This field is only used in (NG)EN-DC. |
| ***p-maxEUTRA***  Indicates the maximum total transmit power to be used by the UE in the E-UTRA cell group (see TS 36.104 [33]). This field is used in (NG)EN-DC and NE-DC. |
| ***p-maxNR-FR1***  For (NG)EN-DC and NE-DC, the field indicates the maximum total transmit power to be used by the UE in the NR cell group across all serving cells in frequency range 1 (FR1) (see TS 38.104 [12]). For NR-DC, it indicates the maximum total transmit power to be used by the UE in the NR cell group across all serving cells in frequency range 1 (FR1) (see TS 38.104 [12]) the UE can use in NR SCG. |
| ***p-maxUE-FR1***  Indicates the maximum total transmit power to be used by the UE across all serving cells in frequency range 1 (FR1). |
| ***p-maxNR-FR1-MCG***  Indicates the maximum total transmit power to be used by the UE in the NR cell group across all serving cells in frequency range 1 (FR1) (see TS 38.104 [12]) the UE can use in NR MCG. This field is only used in NR-DC. |
| ***p-maxNR-FR2-SCG***  Indicates the maximum total transmit power to be used by the UE in the NR cell group across all serving cells in frequency range 2 (FR2) (see TS 38.104 [12]) the UE can use in NR SCG. |
| ***p-maxUE-FR2***  Indicates the maximum total transmit power to be used by the UE across all serving cells in frequency range 2 (FR2). |
| ***p-maxNR-FR2-MCG***  Indicates the maximum total transmit power to be used by the UE in the NR cell group across all serving cells in frequency range 2 (FR2) (see TS 38.104 [12]) the UE can use in NR MCG. |
| ***pdcch-BlindDetectionSCG***  Indicates the maximum value of the reference number of cells for PDCCH blind detection allowed to be configured for the SCG. |
| ***ph-InfoMCG***  Power headroom information in MCG that is needed in the reception of PHR MAC CE in SCG. |
| ***ph-SupplementaryUplink***  Power headroom information for supplementary uplink. For UE in (NG)EN-DC, this field is absent. |
| ***ph-Type1or3***  Type of power headroom for a serving cell in MCG (PCell and activated SCells). *type1* refers to type 1 power headroom, *type3* refers to type 3 power headroom. (See TS 38.321 [3]). |
| ***ph-Uplink***  Power headroom information for uplink. |
| ***powerCoordination-FR1***  Indicates the maximum power that the UE can use in FR1. |
| ***powerCoordination-FR2***  Indicates the maximum power that the UE can use in frequency range 2 (FR2). This field is only used in NR-DC. |
| ***scgFailureInfo***  Contains SCG failure type and measurement results. In case the sender has no measurement results available, the sender may include one empty entry (i.e. without any optional fields present) in *measResultPerMOList*. This field is used in (NG)EN-DC and NR-DC. |
| ***scg-RB-Config***  Contains all of the fields in the IE RadioBearerConfig used in SN, used to allow the target SN to use delta configuration to the UE, e.g. during SN change. The field is signalled upon change of SN unless MN uses full configuration option. Otherwise, the field is absent. |
| ***scpac-ReferenceConfiguration***  Includes the reference configuration for the candidate supporting subsequent CPAC. |
| ***selectedBandEntriesMNList***  A list of indices referring to the position of a band entry selected by the MN, in each band combination entry in *allowedBC-ListMRDC* IE. *BandEntryIndex* 0 identifies the first band in the *bandList* of the *BandCombination*, *BandEntryIndex* 1 identifies the second band in the *bandList* of the *BandCombination*, and so on. This *selectedBandEntriesMNList* includes the same number of entries, and listed in the same order as in *allowedBC-ListMRDC*. The SN uses this information to determine which bands out of the NR band combinations in *allowedBC-ListMRDC* it can configure in SCG in NR-DC. The SN can use this information to determine for which band pair(s) it should check *SimultaneousRxTxPerBandPair*. |
| ***servCellIndexRangeSCG***  Range of serving cell indices that SN is allowed to configure for SCG serving cells. |
| ***servCellInfoListMCG-EUTRA***  Indicates the carrier frequency and the transmission bandwidth of the serving cell(s) in the MCG in intra-band (NG)EN-DC. The field is needed when MN and SN operate serving cells in the same band for either contiguous or non-contiguous intra-band band combination or LTE NR inter-band band combinations where the frequency range of the E-UTRA band is a subset of the frequency range of the NR band (as specified in Table 5.5B.4.1-1 of TS 38.101-3 [34]) in (NG)EN-DC. |
| ***servCellInfoListMCG-NR***  Indicates the frequency band indicator, carrier center frequency, UE specific channel bandwidth and SCS of the serving cell(s) in the MCG in intra-band NE-DC. The field is needed when MN and SN operate serving cells in the same band for either contiguous or non-contiguous intra-band band combination or LTE NR inter-band band combinations where the frequency range of the E-UTRA band is a subset of the frequency range of the NR band (as specified in Table 5.5B.4.1-1 of TS 38.101-3 [34]) in NE-DC. |
| ***servFrequenciesMN-NR***  Indicates the frequency of all serving cells that include PCell and SCell(s) with SSB configured in MCG. This field is only used in NR-DC. servFrequenciesMN-NR indicates absoluteFrequencySSB. |
| ***sftdFrequencyList-NR***  Includes a list of SSB frequencies. Each entry identifies the SSB frequency of a PSCell, which corresponds to one *MeasResultCellSFTD-NR* entry in the *MeasResultCellListSFTD-NR*. |
| ***sftdFrequencyList-EUTRA***  Includes a list of E-UTRA frequencies. Each entry identifies the carrier frequency of a PSCell, which corresponds to one *MeasResultSFTD-EUTRA* entry in the *MeasResultCellListSFTD-EUTRA*. |
| ***sidelinkUEInformationEUTRA***  This field contains the E-UTRA *SidelinkUEInformation* message as specified in TS 36.331 [10]. |
| ***sidelinkUEInformationNR***  This field contains the NR *SidelinkUEInformationNR* message. |
| ***sourceConfigSCG***  Includes all of the current SCG configurations used by the target SN to build delta configuration to be sent to UE, e.g. during SN change. The field contains the *RRCReconfiguration* message, i.e. including *secondaryCellGroup* and *measConfig*. The field is signalled upon change of SN, unless MN uses full configuration option. Otherwise, the field is absent. |
| ***sourceConfigSCG-EUTRA***  Includes the E-UTRA *RRCConnectionReconfiguration* message as specified in TS 36.331 [10]. In this version of the specification, the E-UTRA RRC message can only include the field *scg-Configuration.* In this version of the specification, this field is absent when master gNB uses full configuration option. This field is only used in NE-DC. |
| ***twoPHRModeMCG***  Indicates if the power headroom for MCG shall be reported as two PHRs (each PHR associated with a SRS resource set) is enabled or not. |
| ***twoSRS-PUSCH-Repetition***  Indicates whether the indicated serving cell is configured for PUSCH repetition corresponding to two SRS resource sets configured in either *srs-ResourceSetToAddModList* or *srs-ResourceSetToAddModListDCI-0-2* with usage 'codebook' or 'noncodebook'. |
| ***ueAssistanceInformationSourceSCG***  Includes for each UE assistance feature associated with the SCG, the information last reported by the UE in the NR *UEAssistanceInformation* message for the source SCG, if any. |
| ***ue-CapabilityInfo***  Contains the IE *UE-CapabilityRAT-ContainerList* supported by the UE (see NOTE 3). A gNB that retrieves MRDC related capability containers ensures that the set of included MRDC containers is consistent w.r.t. the feature set related information. |

|  |
| --- |
| *BandCombinationInfo* field descriptions |
| ***allowedFeatureSetsList***  Defines a subset of the entries in a *FeatureSetCombination*. Each index identifies a position in the *FeatureSetCombination*, which corresponds to one *FeatureSetUplink*/*Downlink* for each band entry in the associated band combination. |
| ***bandCombinationIndex***  In case of NR-DC, this field indicates the position of a band combination in the *supportedBandCombinationList*. In case of NE-DC, this field indicates the position of a band combination in the *supportedBandCombinationList* and/or *supportedBandCombinationListNEDC-Only*. In case of (NG)EN-DC, this field indicates the position of a band combination in the *supportedBandCombinationList* and/or *supportedBandCombinationList-UplinkTxSwitch*. Band combination entries in *supportedBandCombinationList* are referred by an index which corresponds to the position of a band combination in the *supportedBandCombinationList*. Band combination entries in *supportedBandCombinationListNEDC-Only* are referred by an index which corresponds to the position of a band combination in the *supportedBandCombinationListNEDC-Only* increased by the number of entries in *supportedBandCombinationList*. Band combination entries in *supportedBandCombinationList-UplinkTxSwitch* are referred by an index which corresponds to the position of a band combination in the *supportedBandCombinationList-UplinkTxSwitch* increased by the number of entries in *supportedBandCombinationList*. |

|  |  |
| --- | --- |
| Conditional Presence | Explanation |
| *SN-AddMod* | The field is mandatory present upon SN addition and SN change. It is optionally present upon SN modification and inter-MN handover without SN change. Otherwise, the field is absent. |

NOTE 3: The following table indicates per MN RAT and SN RAT whether RAT capabilities are included or not in *ue-CapabilityInfo*.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| MN RAT | SN RAT | NR capabilities | E-UTRA capabilities | MR-DC capabilities |
| E-UTRA | NR | Need not be included if the UE Radio Capability ID as specified in 23.502 [43] is used. Included otherwise | Not included | Need not be included if the UE Radio Capability ID as specified in 23.502 [43] is used. Included otherwise |
| NR | E-UTRA | Not included | Need not be included if the UE Radio Capability ID as specified in 23.502 [43] is used. Included otherwise | Need not be included if the UE Radio Capability ID as specified in 23.502 [43] is used. Included otherwise |
| NR | NR | Need not be included if the UE Radio Capability ID as specified in 23.502 [43] is used. Included otherwise | Not included | Not included |

*END OF CHANGES*