**3GPP TSG-RAN WG2 Meeting #124 *R2-231xxxx***

**Chicago, US, 13 – 17 November, 2023**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **38.331** | **CR** | **4435** | **rev** | **-** | **Current version:** | **17.6.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Introduction of RRCRelease with resume indication for SDT [SDT\_ReleaseEnh] |
|  |  |
| ***Source to WG:*** | Huawei, HiSilicon, China Telecom, Qualcomm, CATT, Lenovo, Orange, Vodafone, CMCC, China Unicom |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | TEI18, NR\_SmallData\_INACTIVE-Core |  | ***Date:*** | 2023-11-XX |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | In the “LS on SDT signalling optimization for partial context transfer” (R3-234589), RAN3 indicates that the signalling procedure for the DL non-SDT data arrival in case of SDT without UE anchor relocation (as described in TS 38.300 section 18.3) may be optimised for the scenario where currently, it requires to move the UE to RRC INACTIVE state and afterwards send RAN Paging messages in the cells of the RNA. This imposes additional signalling overhead in the RAN and increases the delay to trigger transition into RRC\_CONNECTED state.  |
|  |  |
| ***Summary of change:*** | A *resumeIndication* is introduced in *suspendConfig* included in the RRCRelease message. After receiving such indication, the UE triggers RRC connection resume procedure automatically, i.e. without waiting for Paging from the network. |
|  |  |
| ***Consequences if not approved:*** | The signalling optimization for the DL non-SDT data arrival in case of SDT without UE anchor relocation as indicated in R3-234589 is not supported. |
|  |  |
| ***Clauses affected:*** | 5.3.8.3, 5.3.13.2, 6.2.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...TS/TR ... CR ... |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ... |
| ***(show related CRs)*** |  | **X** |  O&M Specifications |  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

#### 5.3.8.3 Reception of the *RRCRelease* by the UE

The UE shall:

1> delay the following actions defined in this clause 60 ms from the moment the *RRCRelease* message was received or optionally when lower layers indicate that the receipt of the *RRCRelease* message has been successfully acknowledged, whichever is earlier;

1> stop timer T380, if running;

1> stop timer T320, if running;

1> if timer T316 is running;

2> stop timer T316;

2> clear the information included in *VarRLF-Report,* if any;

1> stop timer T350, if running;

1> stop timer T346g, if running;

1> if theAS security is not activated:

2> ignore any field included in *RRCRelease* message except *waitTime*;

2> perform the actions upon going to RRC\_IDLE as specified in 5.3.11 with the release cause 'other' upon which the procedure ends;

1> if the *RRCRelease* message includes *redirectedCarrierInfo* indicating redirection to *eutra*:

2> if *cnType* is included:

3> after the cell selection, indicate the available CN Type(s) and the received *cnType* to upper layers;

NOTE 1: Handling the case if the E-UTRA cell selected after the redirection does not support the core network type specified by the *cnType,* is up to UE implementation.

2> if *voiceFallbackIndication* is included:

3> consider the RRC connection release was for EPS fallback for IMS voice (see TS 23.502 [43]);

1> if the *RRCRelease* message includes the *cellReselectionPriorities*:

2> store the cell reselection priority information provided by the *cellReselectionPriorities*;

2> if the *t320* is included:

3> start timer T320, with the timer value set according to the value of *t320*;

1> else:

2> apply the cell reselection priority information broadcast in the system information;

1> if *deprioritisationReq* is included and the UE supports RRC connection release with deprioritisation:

2> start or restart timer T325 with the timer value set to the *deprioritisationTimer* signalled;

2> store the *deprioritisationReq* until T325 expiry;

NOTE 1a: The UE stores the deprioritisation request irrespective of any cell reselection absolute priority assignments (by dedicated or common signalling) and regardless of RRC connections in NR or other RATs unless specified otherwise.

1> if the *RRCRelease* includes the *measIdleConfig*:

2> if T331 is running:

3> stop timer T331;

3> perform the actions as specified in 5.7.8.3;

2> if the *measIdleConfig* is set to *setup*:

3> store the received *measIdleDuration* in *VarMeasIdleConfig*;

3> start timer T331 with the value set to *measIdleDuration*;

3> if the *measIdleConfig* contains *measIdleCarrierListNR*:

4> store the received *measIdleCarrierListNR* in *VarMeasIdleConfig*;

3> if the *measIdleConfig* contains *measIdleCarrierListEUTRA*:

4> store the received *measIdleCarrierListEUTRA* in *VarMeasIdleConfig*;

3> if the *measIdleConfig* contains *validityAreaList*:

4> store the received *validityAreaList* in *VarMeasIdleConfig*;

1> if the *RRCRelease* includes *suspendConfig*:

2> reset MAC and release the default MAC Cell Group configuration, if any;

2> apply the received *suspendConfig* except the received *nextHopChainingCount*;

2> if the *sdt-Config* is configured:

3> for each of the DRB in the *sdt-DRB-List*:

4> consider the DRB to be configured for SDT;

3> if *sdt-SRB2-Indication* is configured:

4> consider the SRB2 to be configured for SDT;

3> for each RLC bearer (except those associated with broadcast MRBs) that is not suspended:

4> re-establish the RLC entity as specified in TS 38.322 [4];

3> for SRB2 (if it is resumed) and for SRB1:

4> trigger the PDCP entity to perform SDU discard as specified in TS 38.323 [5];

3> if *sdt-MAC-PHY-CG-Config* is configured:

4> configure the PCell with the configured grant resources for SDT and instruct the MAC entity to start the *cg-SDT-TimeAlignmentTimer*;

2> if *srs-PosRRC-Inactive* is configured:

3> apply the configuration and instruct MAC to start the *inactivePosSRS-TimeAlignmentTimer*;

NOTE 1b: The Network should provide full configuration to UE for SRS for Positioning in RRC\_INACTIVE.

2> remove all the entries within the MCG and the SCG *VarConditionalReconfig*, if any;

2> for each *measId* of the MCG *measConfig* and for each *measId* of the SCG *measConfig*, if configured, if the associated *reportConfig* has a *reportType* set to *condTriggerConfig*:

3> for the associated *reportConfigId*:

4> remove the entry with the matching *reportConfigId* from the *reportConfigList* within the *VarMeasConfig*;

3> if the associated *measObjectId* is only associated to a *reportConfig* with *reportType* set to *condTriggerConfig*:

4> remove the entry with the matching *measObjectId* from the *measObjectList* within the *VarMeasConfig*;

3> remove the entry with the matching *measId* from the *measIdList* within the *VarMeasConfig*;

2> if the UE is acting as L2 U2N Remote UE:

3> if the PC5-RRC connection with the U2N Relay UE is determined to be released:

4> indicate upper layers to trigger PC5 unicast link release;

3> else (i.e., maintain the PC5 RRC connection):

4> establish or re-establish (e.g. via release and add) SL RLC entity for SRB1;

2> else:

3> re-establish RLC entities for SRB1;

2> if the *RRCRelease* message with *suspendConfig* was received in response to an *RRCResumeRequest* or an *RRCResumeRequest1*:

3> stop the timer T319 if running;

3> in the stored UE Inactive AS context:

4> replace the KgNB and KRRCint keys with the current KgNB and KRRCint keys;

4> replace the *nextHopChainingCount* with the value of *nextHopChainingCount* received in the *RRCRelease* message*;*

4> replace the *cellIdentity* with the *cellIdentity* of the cell the UE has received the *RRCRelease* message;

4> if the *suspendConfig* contains the *sl-UEIdentityRemote* (i.e. the UE is a L2 U2N Remote UE):

5> replace the C-RNTI with the value of the *sl-UEIdentityRemote*;

5> replace the physical cell identitywith the value of the *sl-PhysCellId* in *sl-ServingCellInfo* contained in the discovery message received from the connected L2 U2N Relay UE;

4> else:

5> replace the C-RNTI with the C-RNTI used in the cell (see TS 38.321 [3]) the UE has received the *RRCRelease* message;

5> replace the physical cell identitywith the physical cell identity of the cell the UE has received the *RRCRelease* message;

3> replace the *nextHopChainingCount* with the value associated with the current KgNB;

3> stop the timer T319a if running and consider SDT procedure is not ongoing;

2> else:

3> store in the UE Inactive AS Context the *nextHopChainingCount* received in the *RRCRelease* message*,* the current KgNB and KRRCint keys, the ROHC state, the EHC context(s), the UDC state, the stored QoS flow to DRB mapping rules, the application layer measurement configuration, the C-RNTI used in the source PCell, the *cellIdentity* and the physical cell identity of the source PCell, the *spCellConfigCommon* within *ReconfigurationWithSync* of the NR PSCell (if configured) and all other parameters configured except for:

- parameters within *ReconfigurationWithSync* of the PCell;

- parameters within *ReconfigurationWithSync* of the NR PSCell, if configured;

- parameters within *MobilityControlInfoSCG* of the E-UTRA PSCell, if configured;

- *servingCellConfigCommonSIB*;

- *sl-L2RelayUE-Config*, if configured;

- *sl-L2RemoteUE-Config*, if configured;

NOTE 1c: *suspendConfig* is not stored as part of UE Inactive AS Context, except for the fields explicitly specified.

3> store any previously or subsequently received application layer measurement report containers for which no segment, or full message, has been submitted to lower layers for transmission;

NOTE 2: NR sidelink communication/discovery related configurations and logged measurement configuration are not stored as UE Inactive AS Context, when UE enters RRC\_INACTIVE.

2> suspend all SRB(s) and DRB(s) and multicast MRB(s), except SRB0 and broadcast MRBs;

2> indicate PDCP suspend to lower layers of all DRBs and multicast MRBs;

2> release Uu Relay RLC channel(s), if configured;

2> release PC5 Relay RLC channel(s), if configured;

2> release the SRAP entity, if configured;

NOTE 2a: A L2 U2N Relay UE may re-establish the SL-RLC0, SL-RLC1 and SRAP entity after release.

2> if the *t380* is included:

3> start timer T380, with the timer value set to *t380*;

2> if the *RRCRelease* message is including the *waitTime*:

3> start timer T302 with the value set to the *waitTime*;

3> inform upper layers that access barring is applicable for all access categories except categories '0' and '2';

2> if T390 is running:

3> stop timer T390 for all access categories;

3> perform the actions as specified in 5.3.14.4;

2> indicate the suspension of the RRC connection to upper layers;

2> if the UE is capable of L2 U2N Remote UE:

3> enter RRC\_INACTIVE, and perform either cell selection as specified in TS 38.304 [20], or relay selection as specified in clause 5.8.15.3, or both;

2> else:

3> enter RRC\_INACTIVE and perform cell selection as specified in TS 38.304 [20];

2> if the *suspendConfig* includes *resumeIndication*:

3> perform the actions as if the UE received *Paging* message with the *ue-Identity* included in the *PagingRecord* matching the UE's stored *fullI-RNTI*, as specified in clause 5.3.2.3;

1> else:

2> perform the actions upon going to RRC\_IDLE as specified in 5.3.11, with the release cause 'other'.

NOTE 3: Whether to release the PC5 unicast link is left to L2 U2N Remote UE's implementation.

NOTE 4: It is left to UE implementation whether to stop T430, if running, when going to RRC\_INACTIVE.

**<TEXT OMITTED>**

### 5.3.13 RRC connection resume

**<TEXT OMITTED>**

#### 5.3.13.2 Initiation

The UE initiates the procedure when upper layers or AS (when responding to RAN paging, upon triggering RNA updates while the UE is in RRC\_INACTIVE, for NR sidelink communication/discovery/V2X sidelink communication as specified in clause 5.3.13.1a, upon receiving *RRCRelease* message including *resumeIndication*) requests the resume of a suspended RRC connection or requests the resume for initiating SDT as specified in clause 5.3.13.1b.

The UE shall ensure having valid and up to date essential system information as specified in clause 5.2.2.2 before initiating this procedure.

Upon initiation of the procedure, the UE shall:

1> if the resumption of the RRC connection is triggered by response to NG-RAN paging; or

1> if the resumption of the RRC connection is triggered by receiving *RRCRelease* message including *resumeIndication*:

2> select '0' as the Access Category;

2> perform the unified access control procedure as specified in 5.3.14 using the selected Access Category and one or more Access Identities provided by upper layers;

3> if the access attempt is barred, the procedure ends;

1> else if the resumption of the RRC connection is triggered by upper layers:

2> if the upper layers provide an Access Category and one or more Access Identities:

3> perform the unified access control procedure as specified in 5.3.14 using the Access Category and Access Identities provided by upper layers;

4> if the access attempt is barred, the procedure ends;

2> if the upper layers provide NSAG information and one or more S-NSSAI(s) triggering the access attempt (TS 23.501 [32] and TS 24.501 [23]):

3> apply the NSAG with highest NSAG priority among the NSAGs that are included in *SIB1* (i.e., in *FeatureCombination* and/or in *RA-PrioritizationSliceInfo*), and that are associated with the S-NSSAI(s) triggering the access attempt, in the Random Access procedure (TS 38.321 [3], clause 5.1);

NOTE: If there are multiple NSAGs with the same highest NAS-provided NSAG priority identified for access attempt as above, it is left to UE implementation to select the NSAG to be applied in the Random Access procedure.

2> if the resumption occurs after release with redirect with *mpsPriorityIndication*:

3> set the *resumeCause* to *mps-PriorityAccess*;

2> else:

3> set the *resumeCause* in accordance with the information received from upper layers;

1> else if the resumption of the RRC connection is triggered due to an RNA update as specified in 5.3.13.8:

2> if an emergency service is ongoing:

NOTE 1: How the RRC layer in the UE is aware of an ongoing emergency service is up to UE implementation.

3> select '2' as the Access Category;

3> set the *resumeCause* to *emergency*;

2> else:

3> select '8' as the Access Category;

2> perform the unified access control procedure as specified in 5.3.14 using the selected Access Category and one or more Access Identities to be applied as specified in TS 24.501 [23];

3> if the access attempt is barred:

4> set the variable *pendingRNA-Update* to *true*;

4> the procedure ends;

NOTE 2: In case the L2 U2N Relay UE initiates RRC connection resume triggered by reception of message from a L2 U2N Remote UE via SL-RLC0 or SL-RLC1 as specified in 5.3.13.1a, the L2 U2N Relay UE sets the *resumeCause* by implementation, but it can only set the *emergency*, *mps-PriorityAccess*, or *mcs-PriorityAccess* as *resumeCause*, if the same cause value in the message received from the L2 U2N Remote UE via SL-RLC0.

1> if the UE is in NE-DC or NR-DC:

2> if the UE does not support maintaining SCG configuration upon connection resumption:

3> release the MR-DC related configurations (i.e., as specified in 5.3.5.10) from the UE Inactive AS context, if stored;

1> if the UE does not support maintaining the MCG SCell configurations upon connection resumption:

2> release the MCG SCell(s) from the UE Inactive AS context, if stored;

1> if the UE is acting as L2 U2N Remote UE:

2> establish a SRAP entity as specified in TS 38.351 [66], if no SRAP entity has been established;

2> apply the default configuration of SL-RLC1 as defined in 9.2.4 for SRB1;

2> apply the default PDCP configuration as defined in 9.2.1 for SRB1;

2> apply the default configuration of SRAP as defined in 9.2.5 for SRB1;

1> else:

2> apply the default L1 parameter values as specified in corresponding physical layer specifications, except for the parameters for which values are provided in *SIB1*;

2> apply the default SRB1 configuration as specified in 9.2.1;

2> apply the default MAC Cell Group configuration as specified in 9.2.2;

1> release *delayBudgetReportingConfig* from the UE Inactive AS context, if stored;

1> stop timer T342, if running;

1> release *overheatingAssistanceConfig* from the UE Inactive AS context, if stored;

1> stop timer T345, if running;

1> release *idc-AssistanceConfig* from the UE Inactive AS context, if stored;

1> release *drx-PreferenceConfig* for all configured cell groups from the UE Inactive AS context, if stored;

1> stop all instances of timer T346a, if running;

1> release *maxBW-PreferenceConfig* and *maxBW-PreferenceConfigFR2-2* for all configured cell groups from the UE Inactive AS context, if stored;

1> stop all instances of timer T346b, if running;

1> release *maxCC-PreferenceConfig* for all configured cell groups from the UE Inactive AS context, if stored;

1> stop all instances of timer T346c, if running;

1> release *maxMIMO-LayerPreferenceConfig* and *maxMIMO-LayerPreferenceConfigFR2-2* for all configured cell groups from the UE Inactive AS context, if stored;

1> stop all instances of timer T346d, if running;

1> release *minSchedulingOffsetPreferenceConfig* and *minSchedulingOffsetPreferenceConfigExt* for all configured cell groups from the UE Inactive AS context, if stored;

1> stop all instances of timer T346e, if running;

1> release *rlm-RelaxationReportingConfig* for all configured cell groups from the UE Inactive AS context, if stored;

1> stop all instances of timer T346j, if running;

1> release *bfd-RelaxationReportingConfig* for all configured cell groups from the UE Inactive AS context, if stored;

1> stop all instances of timer T346k, if running;

1> release *releasePreferenceConfig* from the UE Inactive AS context, if stored;

1> release *wlanNameList* from the UE Inactive AS context, if stored;

1> release *btNameList* from the UE Inactive AS context, if stored;

1> release *sensorNameList* from the UE Inactive AS context, if stored;

1> release *obtainCommonLocation* from the UE Inactive AS context, if stored;

1> stop timer T346f, if running;

1> stop timer T346i, if running;

1> release *referenceTimePreferenceReporting* from the UE Inactive AS context, if stored;

1> release *sl-AssistanceConfigNR* from the UE Inactive AS context, if stored;

1> release *musim-GapAssistanceConfig* from the UE Inactive AS context, if stored and stop timer T346h, if running;

1> release *musim-GapConfig* from the UE Inactive AS context, if stored;

1> release *musim-LeaveAssistanceConfig* from the UE Inactive AS context, if stored;

1> release *propDelayDiffReportConfig* from the UE Inactive AS context, if stored;

1> release *ul-GapFR2-PreferenceConfig*, if configured;

1> release *rrm-MeasRelaxationReportingConfig* from the UE Inactive AS context, if stored;

1> if the UE is acting as L2 U2N Remote UE:

2> apply the specified configuration of SL-RLC0 used for the delivery of RRC message over SRB0 as specified in 9.1.1.4;

2> apply the SDAP configuration and PDCP configuration as specified in 9.1.1.2 for SRB0;

1> else:

2> apply the CCCH configuration as specified in 9.1.1.2;

2> apply the *timeAlignmentTimerCommon* included in *SIB1*;

1> if *sdt-MAC-PHY-CG-Config* is configured:

2> if the resume procedure is initiated in a cell that is different to the PCell in which the UE received the stored *sdt-MAC-PHY-CG-Config*:

3> release the stored *sdt-MAC-PHY-CG-Config*;

3> instruct the MAC entity to stop the *cg-SDT-TimeAlignmentTimer*, if it is running;

1> if *ncd-SSB-RedCapInitialBWP-SDT* is configured:

2> if the resume procedure is initiated in a cell that is different to the PCell in which the UE received the stored *ncd-SSB-RedCapInitialBWP-SDT*:

3> release the stored *ncd-SSB-RedCapInitialBWP-SDT;*

1> if conditions for initiating SDT in accordance with 5.3.13.1b are fulfilled:

2> consider the resume procedure is initiated for SDT;

2> start timer T319a when the lower layers first transmit the CCCH message;

2> consider SDT procedure is ongoing;

1> else:

2> start timer T319;

2> instruct the MAC entity to stop the *cg*-*SDT*-*TimeAlignmentTimer*, if it is running;

1> if *ta-Report* is configured with value *enabled* and the UE supports TA reporting:

2> indicate TA report initiation to lower layers;

1> set the variable *pendingRNA-Update* to *false*;

1> release *successHO-Config* from the UE Inactive AS context, if stored;

1> initiate transmission of the *RRCResumeRequest* message or *RRCResumeRequest1* in accordance with 5.3.13.3.

**<TEXT OMITTED>**

### 6.2.2 Message definitions

**<TEXT OMITTED>**

#### – *RRCRelease*

The *RRCRelease* message is used to command the release of an RRC connection or the suspension of the RRC connection.

Signalling radio bearer: SRB1

RLC-SAP: AM

Logical channel: DCCH

Direction: Network to UE

*RRCRelease* message

-- ASN1START

-- TAG-RRCRELEASE-START

RRCRelease ::= SEQUENCE {

 rrc-TransactionIdentifier RRC-TransactionIdentifier,

 criticalExtensions CHOICE {

 rrcRelease RRCRelease-IEs,

 criticalExtensionsFuture SEQUENCE {}

 }

}

RRCRelease-IEs ::= SEQUENCE {

 redirectedCarrierInfo RedirectedCarrierInfo OPTIONAL, -- Need N

 cellReselectionPriorities CellReselectionPriorities OPTIONAL, -- Need R

 suspendConfig SuspendConfig OPTIONAL, -- Need R

 deprioritisationReq SEQUENCE {

 deprioritisationType ENUMERATED {frequency, nr},

 deprioritisationTimer ENUMERATED {min5, min10, min15, min30}

 } OPTIONAL, -- Need N

 lateNonCriticalExtension OCTET STRING OPTIONAL,

 nonCriticalExtension RRCRelease-v1540-IEs OPTIONAL

}

RRCRelease-v1540-IEs ::= SEQUENCE {

 waitTime RejectWaitTime OPTIONAL, -- Need N

 nonCriticalExtension RRCRelease-v1610-IEs OPTIONAL

}

RRCRelease-v1610-IEs ::= SEQUENCE {

 voiceFallbackIndication-r16 ENUMERATED {true} OPTIONAL, -- Need N

 measIdleConfig-r16 SetupRelease {MeasIdleConfigDedicated-r16} OPTIONAL, -- Need M

 nonCriticalExtension RRCRelease-v1650-IEs OPTIONAL

}

RRCRelease-v1650-IEs ::= SEQUENCE {

 mpsPriorityIndication-r16 ENUMERATED {true} OPTIONAL, -- Cond Redirection2

 nonCriticalExtension RRCRelease-v1710-IEs OPTIONAL

}

RRCRelease-v1710-IEs ::= SEQUENCE {

 noLastCellUpdate-r17 ENUMERATED {true} OPTIONAL, -- Need S

 nonCriticalExtension SEQUENCE {} OPTIONAL

}

RedirectedCarrierInfo ::= CHOICE {

 nr CarrierInfoNR,

 eutra RedirectedCarrierInfo-EUTRA,

 ...

}

RedirectedCarrierInfo-EUTRA ::= SEQUENCE {

 eutraFrequency ARFCN-ValueEUTRA,

 cnType ENUMERATED {epc,fiveGC} OPTIONAL -- Need N

}

CarrierInfoNR ::= SEQUENCE {

 carrierFreq ARFCN-ValueNR,

 ssbSubcarrierSpacing SubcarrierSpacing,

 smtc SSB-MTC OPTIONAL, -- Need S

 ...

}

SuspendConfig ::= SEQUENCE {

 fullI-RNTI I-RNTI-Value,

 shortI-RNTI ShortI-RNTI-Value,

 ran-PagingCycle PagingCycle,

 ran-NotificationAreaInfo RAN-NotificationAreaInfo OPTIONAL, -- Need M

 t380 PeriodicRNAU-TimerValue OPTIONAL, -- Need R

 nextHopChainingCount NextHopChainingCount,

 ...,

 [[

 sl-UEIdentityRemote-r17 RNTI-Value OPTIONAL, -- Cond L2RemoteUE

 sdt-Config-r17 SetupRelease { SDT-Config-r17 } OPTIONAL, -- Need M

 srs-PosRRC-Inactive-r17 SetupRelease { SRS-PosRRC-Inactive-r17 } OPTIONAL, -- Need M

 ran-ExtendedPagingCycle-r17 ExtendedPagingCycle-r17 OPTIONAL -- Cond RANPaging

 ]],

 [[

 ncd-SSB-RedCapInitialBWP-SDT-r17 SetupRelease {NonCellDefiningSSB-r17} OPTIONAL -- Need M

 ]],

 [[

 resumeIndication-r18 ENUMERATED {true} OPTIONAL -- Need N

 ]]

}

PeriodicRNAU-TimerValue ::= ENUMERATED { min5, min10, min20, min30, min60, min120, min360, min720}

CellReselectionPriorities ::= SEQUENCE {

 freqPriorityListEUTRA FreqPriorityListEUTRA OPTIONAL, -- Need M

 freqPriorityListNR FreqPriorityListNR OPTIONAL, -- Need M

 t320 ENUMERATED {min5, min10, min20, min30, min60, min120, min180, spare1} OPTIONAL, -- Need R

 ...,

 [[

 freqPriorityListDedicatedSlicing-r17 FreqPriorityListDedicatedSlicing-r17 OPTIONAL -- Need M

 ]]

}

PagingCycle ::= ENUMERATED {rf32, rf64, rf128, rf256}

ExtendedPagingCycle-r17 ::= ENUMERATED {rf256, rf512, rf1024, spare1}

FreqPriorityListEUTRA ::= SEQUENCE (SIZE (1..maxFreq)) OF FreqPriorityEUTRA

FreqPriorityListNR ::= SEQUENCE (SIZE (1..maxFreq)) OF FreqPriorityNR

FreqPriorityEUTRA ::= SEQUENCE {

 carrierFreq ARFCN-ValueEUTRA,

 cellReselectionPriority CellReselectionPriority,

 cellReselectionSubPriority CellReselectionSubPriority OPTIONAL -- Need R

}

FreqPriorityNR ::= SEQUENCE {

 carrierFreq ARFCN-ValueNR,

 cellReselectionPriority CellReselectionPriority,

 cellReselectionSubPriority CellReselectionSubPriority OPTIONAL -- Need R

}

RAN-NotificationAreaInfo ::= CHOICE {

 cellList PLMN-RAN-AreaCellList,

 ran-AreaConfigList PLMN-RAN-AreaConfigList,

 ...

}

PLMN-RAN-AreaCellList ::= SEQUENCE (SIZE (1.. maxPLMNIdentities)) OF PLMN-RAN-AreaCell

PLMN-RAN-AreaCell ::= SEQUENCE {

 plmn-Identity PLMN-Identity OPTIONAL, -- Need S

 ran-AreaCells SEQUENCE (SIZE (1..32)) OF CellIdentity

}

PLMN-RAN-AreaConfigList ::= SEQUENCE (SIZE (1..maxPLMNIdentities)) OF PLMN-RAN-AreaConfig

PLMN-RAN-AreaConfig ::= SEQUENCE {

 plmn-Identity PLMN-Identity OPTIONAL, -- Need S

 ran-Area SEQUENCE (SIZE (1..16)) OF RAN-AreaConfig

}

RAN-AreaConfig ::= SEQUENCE {

 trackingAreaCode TrackingAreaCode,

 ran-AreaCodeList SEQUENCE (SIZE (1..32)) OF RAN-AreaCode OPTIONAL -- Need R

}

SDT-Config-r17 ::= SEQUENCE {

 sdt-DRB-List-r17 SEQUENCE (SIZE (0..maxDRB)) OF DRB-Identity OPTIONAL, -- Need M

 sdt-SRB2-Indication-r17 ENUMERATED {allowed} OPTIONAL, -- Need R

 sdt-MAC-PHY-CG-Config-r17 SetupRelease {SDT-CG-Config-r17} OPTIONAL, -- Need M

 sdt-DRB-ContinueROHC-r17 ENUMERATED { cell, rna } OPTIONAL -- Need S

}

SDT-CG-Config-r17 ::= OCTET STRING (CONTAINING SDT-MAC-PHY-CG-Config-r17)

SDT-MAC-PHY-CG-Config-r17 ::= SEQUENCE {

 -- CG-SDT specific configuration

 cg-SDT-ConfigLCH-RestrictionToAddModList-r17 SEQUENCE (SIZE(1..maxLC-ID)) OF CG-SDT-ConfigLCH-Restriction-r17 OPTIONAL, -- Need N

 cg-SDT-ConfigLCH-RestrictionToReleaseList-r17 SEQUENCE (SIZE(1..maxLC-ID)) OF LogicalChannelIdentity OPTIONAL, -- Need N

 cg-SDT-ConfigInitialBWP-NUL-r17 SetupRelease {BWP-UplinkDedicatedSDT-r17} OPTIONAL, -- Need M

 cg-SDT-ConfigInitialBWP-SUL-r17 SetupRelease {BWP-UplinkDedicatedSDT-r17} OPTIONAL, -- Need M

 cg-SDT-ConfigInitialBWP-DL-r17 BWP-DownlinkDedicatedSDT-r17 OPTIONAL, -- Need M

 cg-SDT-TimeAlignmentTimer-r17 TimeAlignmentTimer OPTIONAL, -- Need M

 cg-SDT-RSRP-ThresholdSSB-r17 RSRP-Range OPTIONAL, -- Need M

 cg-SDT-TA-ValidationConfig-r17 SetupRelease { CG-SDT-TA-ValidationConfig-r17 } OPTIONAL, -- Need M

 cg-SDT-CS-RNTI-r17 RNTI-Value OPTIONAL, -- Need M

 ...

}

CG-SDT-TA-ValidationConfig-r17 ::= SEQUENCE {

 cg-SDT-RSRP-ChangeThreshold-r17 ENUMERATED { dB2, dB4, dB6, dB8, dB10, dB14, dB18, dB22,

 dB26, dB30, dB34, spare5, spare4, spare3, spare2, spare1}

}

BWP-DownlinkDedicatedSDT-r17 ::= SEQUENCE {

 pdcch-Config-r17 SetupRelease { PDCCH-Config } OPTIONAL, -- Need M

 pdsch-Config-r17 SetupRelease { PDSCH-Config } OPTIONAL, -- Need M

 ...

}

BWP-UplinkDedicatedSDT-r17 ::= SEQUENCE {

 pusch-Config-r17 SetupRelease { PUSCH-Config } OPTIONAL, -- Need M

 configuredGrantConfigToAddModList-r17 ConfiguredGrantConfigToAddModList-r16 OPTIONAL, -- Need N

 configuredGrantConfigToReleaseList-r17 ConfiguredGrantConfigToReleaseList-r16 OPTIONAL, -- Need N

 ...

}

CG-SDT-ConfigLCH-Restriction-r17 ::= SEQUENCE {

 logicalChannelIdentity-r17 LogicalChannelIdentity,

 configuredGrantType1Allowed-r17 ENUMERATED {true} OPTIONAL, -- Need R

 allowedCG-List-r17 SEQUENCE (SIZE (0.. maxNrofConfiguredGrantConfigMAC-1-r16)) OF ConfiguredGrantConfigIndexMAC-r16

 OPTIONAL -- Need R

}

SRS-PosRRC-Inactive-r17 ::= OCTET STRING (CONTAINING SRS-PosRRC-InactiveConfig-r17)

SRS-PosRRC-InactiveConfig-r17 ::= SEQUENCE {

 srs-PosConfigNUL-r17 SRS-PosConfig-r17 OPTIONAL, -- Need R

 srs-PosConfigSUL-r17 SRS-PosConfig-r17 OPTIONAL, -- Need R

 bwp-NUL-r17 BWP OPTIONAL, -- Need S

 bwp-SUL-r17 BWP OPTIONAL, -- Need S

 inactivePosSRS-TimeAlignmentTimer-r17 TimeAlignmentTimer OPTIONAL, -- Need M

 inactivePosSRS-RSRP-ChangeThreshold-r17 RSRP-ChangeThreshold-r17 OPTIONAL -- Need M

}

RSRP-ChangeThreshold-r17 ::= ENUMERATED {dB4, dB6, dB8, dB10, dB14, dB18, dB22, dB26, dB30, dB34, spare6, spare5, spare4, spare3, spare2, spare1}

SRS-PosConfig-r17 ::= SEQUENCE {

 srs-PosResourceSetToReleaseList-r17 SEQUENCE (SIZE(1..maxNrofSRS-PosResourceSets-r16)) OF SRS-PosResourceSetId-r16 OPTIONAL,-- Need N

 srs-PosResourceSetToAddModList-r17 SEQUENCE (SIZE(1..maxNrofSRS-PosResourceSets-r16)) OF SRS-PosResourceSet-r16 OPTIONAL,-- Need N

 srs-PosResourceToReleaseList-r17 SEQUENCE (SIZE(1..maxNrofSRS-PosResources-r16)) OF SRS-PosResourceId-r16 OPTIONAL,-- Need N

 srs-PosResourceToAddModList-r17 SEQUENCE (SIZE(1..maxNrofSRS-PosResources-r16)) OF SRS-PosResource-r16 OPTIONAL -- Need N

}

-- TAG-RRCRELEASE-STOP

-- ASN1STOP

|  |
| --- |
| *RRCRelease-IEs* field descriptions |
| ***cellReselectionPriorities***Dedicated priorities to be used for cell reselection as specified in TS 38.304 [20]*.* The maximum number of NR carrier frequencies that the network can configure through *FreqPriorityListNR* and *FreqPriorityListDedicatedSlicing* together is eight. If the same frequency is configured in both *FreqPriorityListNR* and *FreqPriorityListDedicatedSlicing*, the frequency is only counted once. |
| ***cnType***Indicate that the UE is redirected to EPC or 5GC. |
| ***deprioritisationReq***Indicates whether the current frequency or RAT is to be de-prioritised. |
| ***deprioritisationTimer***Indicates the period for which either the current carrier frequency or NR is deprioritised. Value *minN* corresponds to N minutes. |
| ***measIdleConfig***Indicates measurement configuration to be stored and used by the UE while in RRC\_IDLE or RRC\_INACTIVE. |
| ***mpsPriorityIndication***Indicates the UE can set the establishment cause to *mps-PriorityAccess* for a new connection following a redirect to NR or set the resume cause to *mps-PriorityAccess* for a resume following a redirect to NR. If the target RAT is E-UTRA, see TS 36.331 [10]. The gNB sets the indication only for UEs authorized to receive MPS treatment as indicated by ARP and/or QoS characteristics at the gNB, and it is applicable only for this instance of release with redirection to carrier/RAT included in the *redirectedCarrierInfo* field in the *RRCRelease* message. |
| ***noLastCellUpdate***Presence of the field indicates that the last used cell for PEI shall not be updated. When the field is absent, the PEI-capable UE shall update its last used cell with the current cell. The UE shall not update its last used cell with the current cell if the AS security is not activated. |
| ***srs-PosRRC-InactiveConfig***SRS for positioning configuration during RRC\_INACTIVE state. |
| ***suspendConfig***Indicates configuration for the RRC\_INACTIVE state. The network does not configure *suspendConfig* when the network redirect the UE to an inter-RAT carrier frequency or if the UE is configured with a DAPS bearer. |
| ***redirectedCarrierInfo***Indicates a carrier frequency (downlink for FDD) and is used to redirect the UE to an NR or an inter-RAT carrier frequency, by means of cell selection at transition to RRC\_IDLE or RRC\_INACTIVE as specified in TS 38.304 [20]. Based on UE capability, the network may include *redirectedCarrierInfo* in *RRCRelease* message with *suspendConfig* if this message is sent in response to an *RRCResumeRequest* or an *RRCResumeRequest1* which is triggered by the NAS layer (see 5.3.1.4 in TS 24.501 [23]). |
| ***voiceFallbackIndication***Indicates the RRC release is triggered by EPS fallback for IMS voice as specified in TS 23.502 [43]. |

|  |
| --- |
| *CarrierInfoNR* field descriptions |
| ***carrierFreq***Indicates the redirected NR frequency. |
| ***ssbSubcarrierSpacing***Subcarrier spacing of SSB in the redirected SSB frequency.Only the following values are applicable depending on the used frequency:FR1: 15 or 30 kHzFR2-1: 120 or 240 kHzFR2-2: 120, 480, or 960 kHz |
| ***smtc***The SSB periodicity/offset/duration configuration for the redirected SSB frequency. It is based on timing reference of PCell. If the field is absent, the UE uses the SMTC configured in the measObjectNR having the same SSB frequency and subcarrier spacing. |

|  |
| --- |
| *RAN-NotificationAreaInfo* field descriptions |
| ***cellList***A list of cells configured as RAN area. |
| ***ran-AreaConfigList***A list of RAN area codes or RA code(s) as RAN area. |

|  |
| --- |
| *PLMN-RAN-AreaConfig* field descriptions |
| ***plmn-Identity***PLMN Identity to which the cells in *ran-Area* belong. If the field is absent the UE not in SNPN access mode uses the ID of the registered PLMN. This field is not included for UE in SNPN access mode (for UE in SNPN access mode the *ran-Area* always belongs to the registered SNPN). |
| ***ran-AreaCodeList***The total number of RAN-AreaCodes of all PLMNs does not exceed 32. |
| ***ran-Area***Indicates whether TA code(s) or RAN area code(s) are used for the RAN notification area. The network uses only TA code(s) or both TA code(s) and RAN area code(s) to configure a UE. The total number of TACs across all PLMNs does not exceed 16. |

|  |
| --- |
| *PLMN-RAN-AreaCell* field descriptions |
| ***plmn-Identity***PLMN Identity to which the cells in *ran-AreaCells* belong. If the field is absent the UE not in SNPN access mode uses the ID of the registered PLMN. This field is not included for UE in SNPN access mode (for UE in SNPN access mode the *ran-AreaCells* always belongs to the registered SNPN). |
| ***ran-AreaCells***The total number of cells of all PLMNs does not exceed 32. |

|  |
| --- |
| *SDT-Config* field descriptions |
| ***sdt-DRB-ContinueROHC***Indicates whether the PDCP entity of the radio bearers configured for SDT continues or resets the ROHC header compression protocol during PDCP re-establishment during SDT procedure, as specified in TS 38.323 [5]. Value *cell* indicates that ROHC header compression continues when the UE resumes for SDT in the same cell as the PCell when the RRCRelease message was received. Value *rna* indicates that ROHC header compression continues when the UE resumes for SDT in a cell belonging to the same RNA as the PCell where the RRCRelease message was received. If the field is absent, the UE releases any stored value for this field and the PDCP entity of the radio bearers configured for SDT always resets the ROHC header compression protocol during PDCP re-establishment when SDT procedure is initiated, as specified in TS 38.323 [5]. |
| ***sdt-DRB-List***Indicates the ID(s) of the DRB(s) that are configured for SDT. If size of the sequence is zero, then the UE assumes that none of the DRBs are configured for SDT. The network only configures MN terminated MCG bearers for SDT. |
| ***sdt-SRB2-Indication***Indiates whether SRB2 is configured for SDT or not. |

|  |
| --- |
| *SDT-MAC-PHY-CG-Config* field descriptions |
| ***cg-SDT-ConfigInitialBWP-DL***Downlink BWP configuration for CG-SDT. If a UE is a RedCap UE and if the *initialDownlinkBWP-RedCap* is configured in *downlinkConfigCommon* in *SIB1*, this field is configured for *initialDownlinkBWP-RedCap*, otherwise it is configured for *initialDownlinkBWP*. |
| ***cg-SDT-ConfigInitialBWP-NUL***UL BWP configuration for CG-SDT on NUL carrier. If a UE is a RedCap UE and if the *initialUplinkBWP-RedCap* is configured in *uplinkConfigCommon* in *SIB1*, this field is configured for *initialUplinkBWP-RedCap*, otherwise it is configured for *initialUplinkBWP* for NUL. |
| ***cg-SDT-ConfigInitialBWP-SUL***UL BWP configuration for CG-SDT on SUL carrier configured for the *initialUplinkBWP* for SUL. |
| ***cg-SDT-CS-RNTI***The CS-RNTI value for CG-SDT as specified in TS 38.321 [3]. |
| ***cg-SDT-RSRP-ThresholdSSB***An RSRP threshold configured for SSB selection for CG-SDT as specified in TS 38.321 [3]. |
| ***cg-SDT-TA-ValidationConfig***Configuration for the RSRP based TA validation. If this field is not configured, then the UE does not perform RSRP based TA validation. |
| ***cg-SDT-timeAlignmentTimer***TAT value for CG-SDT as specified in TS 38.321 [3]. The network always configures this field when *sdt-MAC-PHY-CG-Config* is configured. |

|  |
| --- |
| *CG-SDT-ConfigLCH-Restriction* field descriptions |
| ***allowedCG-List***This restriction applies only when the UL grant is a configured grant for CG-SDT. If present, UL MAC SDUs from this logical channel can only be mapped to the indicated CG-SDT configured grant configuration. If the size of the sequence is zero, then UL MAC SDUs from this logical channel cannot be mapped to any CG-SDT configured grant configurations. If the field is not present, UL MAC SDUs from this logical channel can be mapped to any CG-SDT configured grant configurations. If the field *configuredGrantType1Allowed* is present, only those CG-SDT configured grant type 1 configurations indicated in this sequence are allowed for use by this logical channel; otherwise, this sequence shall not include any CG-SDT configured grant type 1 configuration. Corresponds to "*allowedCG*-*List*" as specified in TS 38.321 [3]. |
| ***configuredGrantType1Allowed***If present, or if the capability *lcp-Restriction* as specified in TS 38.306 [26] is not supported, UL MAC SDUs from this logical channel can be transmitted on a configured grant type 1 for CG-SDT. Otherwise, UL MAC SDUs from this logical channel cannot be transmitted on a configured grant type 1 for CG-SDT. Corresponds to "*configuredGrantType1Allowed*" in TS 38.321 [3]. |
| ***logicalChannelIdentity***ID used commonly for the MAC logical channel and for the RLC bearer associated with a *servedRadioBearer* configured for SDT. |

|  |
| --- |
| *CG-SDT-TA-ValidationConfig* field descriptions |
| ***cg-SDT-RSRP-ChangeThreshold***The RSRP threshold for TA validation for CG-SDT as specified in TS 38.321 [3]. Value *dB2* corresponds to 2 dB, value *dB4* corresponds to 4 dB and so on. |

|  |
| --- |
| *SRS-PosRRC-InactiveConfig* field descriptions |
| ***bwp-NUL***BWP configuration for SRS for Positioning during the RRC\_INACTIVE state in Normal Uplink Carrier. If the field is absent UE is configured with an SRS for Positioning associated with the initial UL BWP and transmitted, during the RRC\_INACTIVE state, inside the initial UL BWP with the same CP and SCS as configured for initial UL BWP. |
| ***bwp-SUL***BWP configuration for SRS for Positioning during the RRC\_INACTIVE state in Supplementary Uplink Carrier. If the field is absent UE is configured with an SRS for Positioning associated with the initial UL BWP and transmitted, during the RRC\_INACTIVE state, inside the initial UL BWP with the same CP and SCS as configured for initial UL BWP. |
| ***inactivePosSRS-RSRP-ChangeThreshold***RSRP threshold for the increase/decrease of RSRP for time alignment validation as specified in TS 38.321 [3]. |
| ***inactivePosSRS-TimeAlignmentTimer***TAT value for SRS for positioning transmission during RRC\_INACTIVE state as specified in TS 38.321 [3]. The network always configures this field when *srs-PosRRC-Inactive* is configured. |
| ***srs-PosConfigNUL***SRS for Positioning configuration in RRC\_INACTIVE state in Normal Uplink Carrier. |
| ***srs-PosConfigSUL***SRS for Positioning configuration in RRC\_INACTIVE state in Supplementary Uplink Carrier. |

|  |
| --- |
| *SuspendConfig* field descriptions |
| ***ncd-SSB-RedCapInitialBWP-SDT***Indicates that the UE uses the RedCap-specific initial DL BWP associated with the NCD-SSB for SDT. The network configures this field if a RedCap UE is configured with SDT in the RedCap-specific initial DL BWP not associated with CD-SSB. If configured, the NCD-SSB indicated by this field can only be used during the SDT procedure for CG-SDT or RA-SDT. |
| ***ran-ExtendedPagingCycle***The extended DRX (eDRX) cycle for RAN-initiated paging to be applied by the UE. Value *rf256* corresponds to 256 radio frames, value *rf512* corresponds to 512 radio frames and so on. Value of the field indicates an eDRX cycle which is shorter or equal to the IDLE mode eDRX cycle configured for the UE. |
| ***ran-NotificationAreaInfo***Network ensures that the UE in RRC\_INACTIVE always has a valid *ran-NotificationAreaInfo*. |
| ***ran-PagingCycle***Refers to the UE specific cycle for RAN-initiated paging. Value *rf32* corresponds to 32 radio frames, value *rf64* corresponds to 64 radio frames and so on. |
| ***resumeIndication***Indicates that the UE shall trigger the RRC connection resume procedure after receiving this *RRCRelease* message, as specified in section 5.3.8.3. The network only includes this field in the *RRCRelease* message used to terminate an ongoing SDT procedure. |
| ***sl-UEIdentityRemote***Indicates the C-RNTI to the L2 U2N Remote UE. |
| ***t380***Refers to the timer that triggers the periodic RNAU procedure in UE. Value *min5* corresponds to 5 minutes, value *min10* corresponds to 10 minutes and so on. |

|  |  |
| --- | --- |
| Conditional Presence | Explanation |
| *L2RemoteUE* | The field is mandatory present for L2 U2N Remote UE's RNAU; otherwise it is absent. |
| *RANPaging* | This field is optionally present, Need R, if the UE is configured with IDLE eDRX, see TS 24.501 [23]; otherwise the field is not present. |
| *Redirection2* | The field is optionally present, Need R, if *redirectedCarrierInfo* is included; otherwise the field is not present. |