**3GPP TSG RAN WG2 Meeting #124 R2-231xxxx
Chicago, US, 13th – 17th Nov., 2023**

**Agenda item: 7.3.1**

**Source: Apple**

**Title: Collection of comments to 38.304 CR for NES**

**WID/SID: Netw\_Energy\_NR-Core– Release 18**

**Document for: Discussion and Decision**

# 1 Introduction

This is a summary document on collection of comments to TS 38.304 CR during below running CR discussion:

* [POST124][038][NES] 38.304 CR (Apple)

 Intended outcome: Agree to CR

 Deadline: 2 weeks

# 2 Collection of comments

Please provide your comments in below table, and Rapporteur will response. Please do not insert any comments in running CR directly, which is hard for Rapporteur to follow all comments.

|  |  |  |
| --- | --- | --- |
| **Company** | **Detailed comments** | **Rapporteur response** |
| vivo | Suggest to remove the last sentence: *cellBarred* (IE type: "barred" or "not barred") Indicated in *MIB* message. In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is common for all PLMNs and NPNs. This field is ignored by UEs supporting NTN while *cellBarredNTN* is included in SIB1. This field is ignored by NES-capable UEs while *cellBarredNES* is included in SIB1.The reasons are the following:* 1)There is a NOTE in RRC Running CR, which means NES-capable UEs needs to read cellBarred in MIB and its value to determine whether the UE needs to acquire SIB1. Moreover, when cellBarredNES is included in SIB1, the UE does not need to check cellBarred in MIB again, because the value in cellBarred can only be “barred”. So, the UE actually does not ignore the bar in MIB.

NOTE 2: A UE capable of NES cell DTX/DRX should acquire SIB1 to determine the cell barring status when the *cellBarred* in MIB is set to *barred*.* 2) Having the below text is sufficient.

When *cellBarredNES* is absent and *cellBarred* is set to"barred",- The NES-capable UE shall treat this cell as if cell status is "barred". |  |
| Huawei | We prefer to change “NES-capable UE” to “UE capable of NES cell DTX/DRX” or “UE supporting NES cell DTX/DRX” and remove the NES-capable UE from the definitions section. The reasons are the following:The definitions are far from the relevant section and in my view adding a definition can lead to misunderstandings for someone that is only reading the cell barring section. Making a definition of NES capable UE is not optimal from the readability and spec clarity perspective as this term is used in various places in 38.331 and for a reader/implementer it would not be obvious to check the definitions section before analysing the NES cell barring. Therefore for 38.331 I have adopted the above wording and suggest the same for 38.304.  |  |
| Nokia | We agree with both Vivo and Huawei. Both proposals make specification clearer. |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# 3 Conclusion

TBD