3GPP TSG-RAN WG2 #124 R2-23xxxxx

**Chicago, USA, 13th – 17th November 2023**

Agenda Item: 7.2.1

Source: Ericsson

Title: [Post124][415][POS] Rel-18 Positioning 38.331 CR (Ericsson)

Document for: Discussion, Decision

# Introduction

This is to kick off the email discussion.

* [Post124][415][POS] Rel-18 Positioning 38.331 CR (Ericsson)

 Scope: Finalise and check the Rel-18 positioning 38.331 CR (including taking into account parameter list updates).

 Intended outcome: Agreed CR

 Deadline: Short (for RP)

# 2 Discussion

## 2.1 Bandwidth Aggregation CR

Please provide your comments on the CR for BWA. The changes are track marked with “BandwidthAggregation”

|  |  |
| --- | --- |
| Company Name | Comments |
| Huawei, HiSilicon | 1/ should consdier NUL and SUL in the candicate SRS configurations for linked SRS. Also need to consdier BWP configurations. Can consider to align with the SRS configurations that we introdue in R17 for RRC\_INACTIVESRS-PosResSetLinkedForAggBWInactiveList-r18 ::= SEQUENCE (SIZE(1..maxNrOfLinkedSRS-PosResourceSet-r18)) OF SRS-PosResourceSetLinkedForAggBW-r18SRS-PosRRC-AggBW-InactiveConfigList-r18 ::= SEQUENCE (SIZE (2..3)) OF SRS-PosRRC-AggBW-InactiveConfig-r18SRS-PosRRC-AggBW-InactiveConfig-r18 ::= SEQUENCE { srs-PosConfig-r18 SRS-PosConfig-r17, freqInfoAdditionalCcList-r18 ARFCN-ValueNR} |
|  |  |
|  |  |
|  |  |
|  |  |

## 2.2 RedCap

Please provide your comments on the CR. The changes are marked with “Redcap”

|  |  |
| --- | --- |
| Company Name | Comments |
| Huawei, HiSilicon | 1/ setupRelase needs to be added for need M2/ need to consdier NUL and SUL-- ASN1START-- TAG- SRS-PosTx-Hopping-STARTSRS-PosTx-Hopping-r18 ::= SEQUENCE { srs-PosConfig-r18 SRS-PosConfig-r17, bwp-18 BWP, srs-PosUplinkTransmissionWindowConfig-r18 SRS-PosUplinkTransmissionWindowConfig-r18 OPTIONAL --Need M}SRS-PosUplinkTransmissionWindowConfig-r18 ::= SEQUENCE { windowPeriodicityAndOffset-r18 CHOICE { periodicityAndOffset-r18 SRS-PeriodicityAndOffset-r16, periodicityAndOffset-Ext-r18 SRS-PeriodicityAndOffsetExt-r16 }, duration-r18 ENUMERATED {s1,s2,s4,s6}, ... }-- TAG-SRS-PosTx-Hopping-STOP-- ASN1STOP |
|  |  |
|  |  |
|  |  |
|  |  |

## 2.3 LPHAP

Please provide your comments on the CR. The changes before RAN2#124 are marked with NR\_pos\_enh2 and the changes after are track marked with RAN2#124\_LPHAP

|  |  |
| --- | --- |
| Company Name | Comments |
| Huawei, HiSilicon | 1/ Not sure why the editor’s NOTE is still here Editor’s Note: For preconfigured SRS, there is no need to start the *inactivePosSRS-ValidityAreaTAT* immediately. But for Periodic SRS the above clause would be needed. Agreement says: “Periodic SRSis supported to be configured with validity area. This agreement does not affect preconfigured SRS.” How to differentiate normal and preconfigured SRS. FFS How to start/stop the timer.2/ Not sure what is the agreement for this change?Upon receiving a positioning SRS configuration for RRC\_INACTIVE release request from lower layers, the UE shall:1> release the configured *srs-PosRRC-Inactive*, if configured;1> release the configured *srs-PosRRC-InactiveValidityArea*, if configured.3/ if the trigger is from upper layer, not sure why the RRC layer determines the access category. This can be dicsused in the future meetings."Requst for configuration" can be removed1> else if *srs-PosRRC-InactiveValidityAreaConfig* is configured and the resumption of the RRC connection is triggered due to upper layers request for configuration or activation of preconfigured SRS for positioning when the UE is camped in one of the cells indicated in *srs-PosConfigValidityArea*:2> select '8' as the Access Category;2> set the *resumeCause* to *srs-PosConfigOrActivationReq*;4/ should be "indicate to the lower layer to update TA and stored RSRP"1> else if cell reselection occurs when *srs-PosRRC-InactiveValidityAreaConfig* is configured and if the cell is included in the *srs-PosRRC-InactiveValidityAreaConfig*:2> if *autonomousTA-AdjustmentEnabled* is configured;3> autonomously adjusts the time advance value and the stored RSRP for TA validation.5/ the realed UE behavior seems to have already been covered in TS 38.213When the UE is (pre)configured to transmit SRS for positioning in a validity area, the UE shall:1> if the RS in *spatialRelationInfoPos* cannot be accurately measured:2> suspend the transmission of the SRS for positioning resource.For the power control of an SRS for positioning (pre)configuration in validity area, the UE shall:1> if pathloss RS is provided in *pathlossReferenceRS-Pos*: 2> use the provided pathloss RS;2> if pathloss RS cannot be accurately measured:3> calculate pathloss based on the RS resources obtained from SS/PBCH block of the new camping cell that the UE uses to obtain MIB.6/ The preconfigured SRS should be a list with the following agreement in the last meeting. When multiple validity areas are configured, it should also be clarified that the validity areas do not overlap. srs-PosRRC-InactiveValidityAreaConfig-r18 SetupRelease { SRS-PosRRC-InactiveValidityAreaConfig-r18 } OPTIONAL, -- Need MAlso, there should be only a single SRS-PosRRC-InactiveValidityAreaConfig that can be configured as "not-preconfigured"7/ The relase of the SRS configuration does not necessarily follow RAN paging. The network can choose to release the configuration e.g., at a periodic RNAU, or SRS configuration/activation request or even e.g., SDT procedure. No need to mention about paging here8/ When the RACH procedure is successful, the RRC layer should indicate to the lower layer the applicable SRS configuration when pre-configured is configured for activation request and for configfuation request when the UE moves ouf of the validity area. 1> else if *srs-PosRRC-InactiveValidityAreaConfig* is configured and the resumption of the RRC connection is triggered due to cell reselection to a cell that is not included in *srs-PosConfigValidityArea* and there is an on-going SRS for positioning transmission:2> select '8' as the Access Category;2> set the *resumeCause* to *srs-PosConfigOrActivationReq*;1> else if *srs-PosRRC-InactiveValidityAreaConfig* is configured and the resumption of the RRC connection is triggered due to upper layers request for configuration or activation of preconfigured SRS for positioning when the UE is camped in one of the cells indicated in *srs-PosConfigValidityArea*:2> select '8' as the Access Category;2> set the *resumeCause* to *srs-PosConfigOrActivationReq*; |
|  |  |
|  |  |
|  |  |
|  |  |

# Conclusion

In the previous sections we made the following observations:

Based on the discussion in the previous sections we propose the following:

# References