**3GPP TSG-RAN WG2 Meeting #124R2-231xxxx**

**Chicago, USA 13rd – 17th Nov, 2023**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.331** | **CR** | **4490** | **rev** | **2** | **Current version:** | **17.6.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Introduction of eMBS to RRC | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei, HiSilicon | | | | | | | | | |
| ***Source to TSG:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_MBS\_enh-Core | | | | |  | ***Date:*** | | | 2023-11-23 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | |  |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | This CR introduces the enhancements specified for MBS in Rel-18. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Introduction of multicast reception for UEs in RRC\_INACTIVE and shared processing for simultaneous reception of broadcast and unicast. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Rel-18 MBS enhancements are not supported. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 4.2.1, 5.2.2.4.2, 5.2.2.4.x(new), 5.3.2.3, 5.3.8.3, 5.3.13.2, 5.3.13.4, 5.3.13.x(new), 5.3.14.4, 5.9.4.1, 5.9.4.2, 5.9.4.3, 5.9.4.5, 5.x.1(new), 5.x.2(new), 5.x.3(new), 6.2.2, 6.3.1, 6.3.2, 6.3.6, 6.4 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | | **X** |  | Other core specifications | | | | TS 38.300 CR 0732  TS 38.321 CR 1701  TS 38.304 CR 0355  TS 38.323 CR 0130  TS 38.306 CR 1015 | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | * Compared to the endorsed version in R2-2306855 after May meeting, the CR is updated based on the latest version of RRC spec (v17.5.0). * The CR is further updated based on RAN2#123 meeting agreements. * There is no change compared to the endorsed version in R2-2309033 after August meeting * The CR is updated based on agreements from RAN2#123bis. And the CR is updated based on the latest version of RRC spec (v17.6.0). | | | | | | | | |

*Start of Change*s

4.2 Architecture

4.2.1 UE states and state transitions including inter RAT

A UE is either in RRC\_CONNECTED state or in RRC\_INACTIVE state when an RRC connection has been established. If this is not the case, i.e. no RRC connection is established, the UE is in RRC\_IDLE state. The RRC states can further be characterised as follows:

**- RRC\_IDLE**:

- A UE specific DRX may be configured by upper layers;

- At lower layers, the UE may be configured with a DRX for PTM transmission of MBS broadcast;

- UE controlled mobility based on network configuration;

- The UE:

- Monitors Short Messages transmitted with P-RNTI over DCI (see clause 6.5);

- Monitors a Paging channel for CN paging using 5G-S-TMSI, except if the UE is acting as a L2 U2N Remote UE;

- If configured by upper layers for MBS multicast reception, monitors a Paging channel for CN paging using TMGI;

- Performs neighbouring cell measurements and cell (re-)selection;

- Acquires system information and can send SI request (if configured);

- Performs logging of available measurements together with location and time for logged measurement configured UEs;

- Performs idle/inactive measurements for idle/inactive measurement configured UEs;

- If configured by upper layers for MBS broadcast reception, acquires MCCH change notification and MBS broadcast control information and data.

**- RRC\_INACTIVE**:

- A UE specific DRX may be configured by upper layers or by RRC layer;

- At lower layers, the UE may be configured with a DRX for PTM transmission of MBS broadcast and/or a DRX for PTM transmission of MBS multicast;

- UE controlled mobility based on network configuration;

- The UE stores the UE Inactive AS context;

- A RAN-based notification area is configured by RRC layer;

- Transfer of unicast data and/or signalling to/from UE over radio bearers configured for SDT.

- The UE:

- Monitors Short Messages transmitted with P-RNTI over DCI (see clause 6.5);

- During SDT procedure, monitors control channels associated with the shared data channel to determine if data is scheduled for it;

- While SDT procedure is not ongoing, monitors a Paging channel for CN paging using 5G-S-TMSI and RAN paging using fullI-RNTI, except if the UE is acting as a L2 U2N Remote UE;

- If configured by upper layers for MBS multicast reception, while SDT procedure is not ongoing, monitors a Paging channel for paging using TMGI;

- Performs neighbouring cell measurements and cell (re-)selection;

- Performs RAN-based notification area updates periodically and when moving outside the configured RAN-based notification area;

- Acquires system information and, while SDT procedure is not ongoing, can send SI request (if configured);

- While SDT procedure is not ongoing, performs logging of available measurements together with location and time for logged measurement configured UEs;

- While SDT procedure is not ongoing, performs idle/inactive measurements for idle/inactive measurement configured UEs;

- If configured by upper layers for MBS broadcast reception, acquires MCCH change notification and MBS broadcast control information and data;

- If configured for MBS multicast reception in RRC\_INACTIVE, acquires multicast MCCH change notification and MBS multicast control information and data;

- Transmits SRS for Positioning.

**- RRC\_CONNECTED:**

- The UE stores the AS context;

- Transfer of unicast data to/from UE;

- Transfer of MBS multicast data to UE;

- At lower layers, the UE may be configured with a UE specific DRX;

- At lower layers, the UE may be configured with a DRX for PTM transmission of MBS broadcast and/or a DRX for MBS multicast;

- For UEs supporting CA, use of one or more SCells, aggregated with the SpCell, for increased bandwidth;

- For UEs supporting DC, use of one SCG, aggregated with the MCG, for increased bandwidth;

- Network controlled mobility within NR, to/from E-UTRA, and to UTRA-FDD;

- Network controlled mobility (path switch) between a serving cell and a L2 U2N Relay UE, or vice versa.

- The UE:

- Monitors Short Messages transmitted with P-RNTI over DCI (see clause 6.5), if configured;

- Monitors control channels associated with the shared data channel to determine if data is scheduled for it;

- Provides channel quality and feedback information;

- Performs neighbouring cell measurements and measurement reporting;

- Acquires system information;

- Performs immediate MDT measurement together with available location reporting;

- If configured by upper layers for MBS broadcast reception, acquires MCCH change notification and MBS broadcast control information and data.

Figure 4.2.1-1 illustrates an overview of UE RRC state machine and state transitions in NR. A UE has only one RRC state in NR at one time.

****

**Figure 4.2.1-1: UE state machine and state transitions in NR**

Figure 4.2.1-2 illustrates an overview of UE state machine and state transitions in NR as well as the mobility procedures supported between NR/5GC, E-UTRA/EPC and E-UTRA/5GC.

****

**Figure 4.2.1-2: UE state machine and state transitions between NR/5GC, E-UTRA/EPC and E-UTRA/5GC**

Figure 4.2.1-3 illustrates the mobility procedure supported between NR/5GC and UTRA-FDD.

****

**Figure 4.2.1-3: Mobility procedure supported between NR/5GC and UTRA-FDD**

*Next Change*

## 5.2 System information

### 5.2.2 System information acquisition

#### 5.2.2.4 Actions upon receipt of System Information

5.2.2.4.2 Actions upon reception of the *SIB1*

Upon receiving the *SIB1* the UE shall:

1> store the acquired *SIB1*;

1> if the access is for NTN, and the *cellBarredNTN* in the acquired *SIB1* is set to *barred* or the *cellBarredNTN* is not included in the acquired *SIB1*:

2> consider the cell as barred in accordance with TS 38.304 [20];

2> perform cell re-selection to other cells on the same frequency as the barred cell as specified in TS 38.304 [20];

1> if the UE is a RedCap UE and it is in RRC\_IDLE or in RRC\_INACTIVE, or if the RedCap UE is in RRC\_CONNECTED while *T311* is running:

2> if *intraFreqReselectionRedCap* is not present in *SIB1*:

3> consider the cell as barred in accordance with TS 38.304 [20];

3> perform barring as if *intraFreqReselectionRedCap* is set to allowed;

2> else:

3> if the *cellBarredRedCap1Rx* is present in the acquired *SIB1* and is set to *barred* and the UE is equipped with 1 Rx branch; or

3> if the *cellBarredRedCap2Rx* is present in the acquired *SIB1* and is set to *barred* and the UE is equipped with 2 Rx branches; or

3> if the *halfDuplexRedCapAllowed* is not present in the acquired *SIB1* and the UE supports only half-duplex FDD operation:

4> consider the cell as barred in accordance with TS 38.304 [20];

4> perform barring based on *intraFreqReselectionRedCap* as specified in TS 38.304 [20];

1> if the *cellAccessRelatedInfo* contains an entry of a selected SNPN or PLMN and in case of PLMN the UE is either allowed or instructed to access the PLMN via a cell for which at least one CAG ID is broadcast:

2> in the remainder of the procedures use *npn-IdentityList, trackingAreaCode,* and *cellIdentity* for the cell as received in the corresponding entry of *npn-IdentityInfoList* containing the selected PLMN or SNPN;

1> else if the *cellAccessRelatedInfo* contains an entry with the *PLMN-Identity* of the selected PLMN:

2> in the remainder of the procedures use *plmn-IdentityList*, *trackingAreaCode*, *trackingAreaList,* and *cellIdentity* for the cell as received in the corresponding *PLMN-IdentityInfo* containing the selected PLMN;

1> if the UE in RRC\_INACTIVE is configured for feature(s) that it does not support in current serving cell:

2> the corresponding configuration is not used in current serving cell;

1> if in RRC\_CONNECTED while T311 is not running:

2> disregard the *frequencyBandList*, if received, while in RRC\_CONNECTED;

2> forward the *cellIdentity* to upper layers;

2> forward the *trackingAreaCode* to upper layers, if included;

2> forward the *trackingAreaList* to upper layers, if included;

2> forward the received *posSIB-MappingInfo* to upper layers, if included;

2> apply the configuration included in the *servingCellConfigCommon*;

2> if the UE has a stored valid version of a SIB or posSIB, in accordance with clause 5.2.2.2.1, that the UE requires to operate within the cell in accordance with clause 5.2.2.1:

3> use the stored version of the required SIB or posSIB;

2> else:

3> acquire the required SIB or posSIB requested by upper layer as defined in clause 5.2.2.3.5;

NOTE 1: Void.

1> else:

2> if the UE supports one or more of the frequency bands indicated in the *frequencyBandList* for downlink for TDD, or one or more of the frequency bands indicated in the *frequencyBandList* for uplink for FDD, and they are not downlink only bands, and

2> if the UE is IAB-MT or supports at least one *additionalSpectrumEmission* in the *NR-NS-PmaxList* for a supported band in the downlink for TDD, or a supported band in uplink for FDD, and

2> if the UE supports an uplink channel bandwidth with a maximum transmission bandwidth configuration (see TS 38.101-1 [15], TS 38.101-2 [39], and TS 38.101-5 [75]) which

- is smaller than or equal to the *carrierBandwidth* (indicated in *uplinkConfigCommon* for the SCS of the initial uplink BWP or, for RedCap UE, of the RedCap-specific initial uplink BWP if configured), and which

- is wider than or equal to the bandwidth of the initial uplink BWP or, for RedCap UE, of the RedCap-specific initial uplink BWP if configured, and

2> if the UE supports a downlink channel bandwidth with a maximum transmission bandwidth configuration (see TS 38.101-1 [15], TS 38.101-2 [39], and TS 38.101-5 [75]) which

- is smaller than or equal to the *carrierBandwidth* (indicated in *downlinkConfigCommon* for the SCS of the initial downlink BWP or, for RedCap UE, of the RedCap-specific initial downlink BWP if configured), and which

- is wider than or equal to the bandwidth of the initial downlink BWP or, for RedCap UE, of the RedCap-specific initial downlink BWP if configured, and

2> if *frequencyShift7p5khz* is present and the UE supports corresponding 7.5kHz frequency shift on this band; or *frequencyShift7p5khz* is not present:

3> if neither *trackingAreaCode* nor *trackingAreaList* is provided for the selected PLMN nor the registered PLMN nor PLMN of the equivalent PLMN list:

4> consider the cell as barred in accordance with TS 38.304 [20];

4> perform cell re-selection to other cells on the same frequency as the barred cell as specified in TS 38.304 [20];

3> else if UE is IAB-MT and if *iab-Support* is not provided for the selected PLMN nor the registered PLMN nor PLMN of the equivalent PLMN list nor the selected SNPN nor the registered SNPN:

4> consider the cell as barred in accordance with TS 38.304 [20];

3> else:

4> apply a supported uplink channel bandwidth with a maximum transmission bandwidth which

- is contained within the *carrierBandwidth* indicated in *uplinkConfigCommon* for the SCS of the initial uplink BWP or, for RedCap UEs, RedCap-specific initial uplink BWP, if configured, and which

- is wider than or equal to the bandwidth of the initial BWP for the uplink or, for a RedCap UE, of the RedCap-specific initial uplink BWP if configured;

4> apply a supported downlink channel bandwidth with a maximum transmission bandwidth which

- is contained within the *carrierBandwidth* indicated in *downlinkConfigCommon* for the SCS of the initial downlink BWP or, for RedCap UEs, RedCap-specific initial downlink BWP, if configured, and which

- is wider than or equal to the bandwidth of the initial BWP for the downlink or, for a RedCap UE, of the RedCap-specific initial downlink BWP if configured;

4> select the first frequency band in the *frequencyBandList*, for FDD from *frequencyBandList* for uplink, or for TDD from *frequencyBandList* for downlink,which the UE supports and for which the UE supports at least one of the *additionalSpectrumEmission* values in *nr-NS-PmaxList*, if present;

4> forward the *cellIdentity* to upper layers;

4> forward the *trackingAreaCode* to upper layers;

4> forward the *trackingAreaList* to upper layers, if included;

4> forward the received *posSIB-MappingInfo* to upper layers, if included;

4> forward the PLMN identity or SNPN identity or PNI-NPN identity to upper layers;

4> if in RRC\_INACTIVE and the forwarded information does not trigger message transmission by upper layers:

5> if the serving cell does not belong to the configured *ran-NotificationAreaInfo*:

6> initiate an RNA update as specified in 5.3.13.8;

5> if configured to receive MBS multicast in RRC\_INACTIVE and not indicated to stop monitoring G-RNTI for at least one MBS multicast session:

6> if *SIBx* is not scheduled in *SIB1* after the UE selects or reselects a different cell :

7> initiate an RRC connection resume procedure for multicast reception as specified in 5.3.13.x;

4> forward the *ims-EmergencySupport* to upper layers, if present;

4> forward the *eCallOverIMS-Support* to upper layers, if present;

4> forward the *UAC-AccessCategory1-SelectionAssistanceInfo* or *UAC-AC1-SelectAssistInfo* for the selected PLMN/SNPNto upper layers, if present and set to *a*, *b* or *c*;

4> if the UE is in SNPN access mode:

5> forward the *imsEmergencySupportForSNPN* indicators with the corresponding SNPN identities to upper layers, if present;

4> apply the configuration included in the *servingCellConfigCommon*;

4> apply the specified PCCH configuration defined in 9.1.1.3;

4> if the UE has a stored valid version of a SIB, in accordance with clause 5.2.2.2.1, that the UE requires to operate within the cell in accordance with clause 5.2.2.1:

5> use the stored version of the required SIB;

4> if the UE has not stored a valid version of a SIB, in accordance with clause 5.2.2.2.1, of one or several required SIB(s), in accordance with clause 5.2.2.1:

5> for the SI message(s) that, according to the *si-SchedulingInfo*, contain at least one required SIB and for which *si-BroadcastStatus* is set to broadcasting:

6> acquire the SI message(s) as defined in clause 5.2.2.3.2;

5> for the SI message(s) that, according to the *si-SchedulingInfo*, contain at least one required SIB and for which *si-BroadcastStatus* is set to *notBroadcasting*:

6> trigger a request to acquire the SI message(s) as defined in clause 5.2.2.3.3;

4> if the UE has a stored valid version of a posSIB, in accordance with clause 5.2.2.2.1, of one or several required posSIB(s), in accordance with clause 5.2.2.1:

5> use the stored version of the required posSIB;

4> if the UE has not stored a valid version of a posSIB, in accordance with clause 5.2.2.2.1, of one or several posSIB(s) in accordance with clause 5.2.2.1:

5> for the SI message(s) that, according to the *posSI-SchedulingInfo*, contain at least one requested posSIB and for which *posSI-BroadcastStatus* is set to *broadcasting*:

6> acquire the SI message(s) as defined in clause 5.2.2.3.2;

5> for the SI message(s) that, according to the *posSI-SchedulingInfo*, contain at least one requested posSIB for which *posSI-BroadcastStatus* is set to *notBroadcasting*:

6> trigger a request to acquire the SI message(s) as defined in clause 5.2.2.3.3a;

4> apply the first listed *additionalSpectrumEmission* which it supports among the values included in *NR-NS-PmaxList* within *frequencyBandList* in *uplinkConfigCommon* for FDD or in *downlinkConfigCommon* for TDD;

4> if the *additionalPmax* is present in the same entry of the selected *additionalSpectrumEmission* within *NR-NS-PmaxList*:

5> apply the *additionalPmax* for UL;

4> else:

5> apply the *p-Max* in *uplinkConfigCommon* for UL;

4> if *supplementaryUplink* is present in *servingCellConfigCommon*; and

4> if the UE supports one or more of the frequency bands indicated in the *frequencyBandList* for the *supplementaryUplink*; and

4> if the UE supports at least one *additionalSpectrumEmission* in the *NR-NS-PmaxList* for a supported supplementary uplink band; and

4> if the UE supports an uplink channel bandwidth with a maximum transmission bandwidth configuration (see TS 38.101-1 [15] and TS 38.101-2 [39]) which

- is smaller than or equal to the *carrierBandwidth* (indicated in *supplementaryUplink* for the SCS of the initial uplink BWP), and which

- is wider than or equal to the bandwidth of the initial uplink BWP of the SUL:

5> consider supplementary uplink as configured in the serving cell;

5> select the first frequency band in the *frequencyBandList* for the *supplementaryUplink* which the UE supports and for which the UE supports at least one of the *additionalSpectrumEmission* values in *nr-NS-PmaxList*, if present;

5> apply a supported supplementary uplink channel bandwidth with a maximum transmission bandwidth which

- is contained within the *carrierBandwidth* (indicated in *supplementaryUplink* for the SCS of the initial uplink BWP), and which

- is wider than or equal to the bandwidth of the initial BWP of the SUL;

5> apply the first listed *additionalSpectrumEmission* which it supports among the values included in *NR-NS-PmaxList* within *frequencyBandList* for the *supplementaryUplink*;

5> if the *additionalPmax* is present in the same entry of the selected *additionalSpectrumEmission* within *NR-NS-PmaxList* for the *supplementaryUplink*:

6> apply the *additionalPmax* in *supplementaryUplink* for SUL;

5> else:

6> apply the *p-Max* in *supplementaryUplink* for SUL;

NOTE 2: For an out of coverage L2 U2N Remote UE in RRC\_IDLE or RRC\_INACTIVE receiving SIB1 from its connected L2 U2N Relay UE, it is up to Remote UE implementation whether to consider and apply the following parameters: *frequencyBandList*, *carrierBandwidth*, *frequencyShift7p5khz*, frequency band, channel bandwidth, the configuration included in the *servingCellConfigCommon*, the specified PCCH configuration, *additionalSpectrumEmission*, *additionalPmax*, and *p-Max*.

2> else:

3> consider the cell as barred in accordance with TS 38.304 [20]; and

3> perform barring as if *intraFreqReselection*, or *intraFreqReselectionRedCap* for RedCap UEs, is set to *notAllowed*;

*Next Change (new)*

##### 5.2.2.4.x Actions upon reception of *SIBx*

No UE requirements related to the contents of *SIBx* apply other than those specified elsewhere e.g., within procedures using the concerned system information, and/or within the corresponding field descriptions.

*Next Change*

## 5.3 Connection control

5.3.2.3 Reception of the *Paging* *message* by the UE or *PagingRecord* by the L2 U2N Remote UE

Upon receiving the *Paging* message by the UE or receiving *PagingRecord* from its connected L2 U2N Relay UE by a L2 U2N Remote UE, the UE shall:

1> if in RRC\_IDLE, for each of the *PagingRecord*, if any, included in the *Paging* message, or

1> if in RRC\_IDLE, for the *PagingRecord*, if any, included in the *UuMessageTransferSidelink* message received from the connected L2 U2N Relay UE:

2> if the *ue-Identity* included in the *PagingRecord* matches the UE identity allocated by upper layers:

3> if upper layers indicate the support of paging cause:

4> forward the *ue-Identity,* *accessType* (if present) and paging cause (if determined) to the upper layers;

3> else:

4> forward the *ue-Identity* and *accessType* (if present) to the upper layers;

1> if in RRC\_INACTIVE, for each of the *PagingRecord*, if any, included in the *Paging* message, or

1> if in RRC\_INACTIVE, for the *PagingRecord*, if any, included in the *UuMessageTransferSidelink* message received from the connected L2 U2N Relay UE:

2> if the *ue-Identity* included in the *PagingRecord* matches the UE's stored *fullI-RNTI*:

3> if the UE is configured by upper layers with Access Identity 1:

4> initiate the RRC connection resumption procedure according to 5.3.13 with *resumeCause* set to *mps-PriorityAccess*;

3> else if the UE is configured by upper layers with Access Identity 2:

4> initiate the RRC connection resumption procedure according to 5.3.13 with *resumeCause* set to *mcs-PriorityAccess*;

3> else if the UE is configured by upper layers with one or more Access Identities equal to 11-15:

4> initiate the RRC connection resumption procedure according to 5.3.13 with *resumeCause* set to *highPriorityAccess*;

3> else:

4> initiate the RRC connection resumption procedure according to 5.3.13 with *resumeCause* set to *mt-Access*;

NOTE: A MUSIM UE may not initiate the RRC connection resumption procedure, e.g. when it decides not to respond to the *Paging* message due to UE implementation constraints as specified in TS 24.501 [23].

2> else if the *ue-Identity* included in the *PagingRecord* matches the UE identity allocated by upper layers:

3> if upper layers indicate the support of paging cause:

4> forward the *ue-Identity*, *accessType* (if present) and paging cause (if determined) to the upper layers;

3> else:

4> forward the *ue-Identity* and *accessType* (if present) to the upper layers;

3> perform the actions upon going to RRC\_IDLE as specified in 5.3.11 with release cause 'other';

1> if in RRC\_IDLE, for each *TMGI* included in *pagingGroupList*, if any, included in the *Paging* message:

2> if the UE has joined an MBS session indicated by the *TMGI* included in the *pagingGroupList*:

3> forward the *TMGI* to the upper layers;

1> if in RRC\_INACTIVE and the UE has joined one or more MBS session(s) indicated by the *TMGI(s)* included in the *pagingGroupList*:

2> if the UE is not configured to receive multicast in RRC\_INACTIVE or if *inactiveReceptionAllowed* is not included for at least one of the MBS session (s) indicated by the *TMGI(s)* that the UE has joined:

3> if *PagingRecordList* is not included in the *Paging* message; or

3> if none of the ue-Identity included in any of the PagingRecord matches the UE identity allocated by upper layers or the UE's stored fullI-RNTI:

4> initiate the RRC connection resumption procedure according to 5.3.13 with *resumeCause* set as below:

5> if the UE is configured by upper layers with Access Identity 1:

6> resumeCause is set to mps-PriorityAccess;

5> else if the UE is configured by upper layers with Access Identity 2:

6> resumeCause is set to mcs-PriorityAccess;

5> else if the UE is configured by upper layers with one or more Access Identities equal to 11-15:

6> resumeCause is set to highPriorityAccess;

5> else:

6> resumeCause is set to mt-Access;

3> else if the *ue-Identity* included in any of the *PagingRecord* matches the UE identity allocated by upper layers:

4> forward the TMGI(s) to the upper layers;

2> else:

3> start monitoring the G-RNTI(s) corresponding to the *TMGI(s),* if configured;

3> if the UE was notified to stop monitoring the G-RNTI(s) for all the joined multicast sessions that are configured for reception in RRC\_INACTIVE:

4> start monitoring the Multicast MCCH-RNTI;

4> acquire the *MBSMulticastConfiguration* message on multicast MCCH, if present;

3> else if the UE was notified to stop monitoring the G-RNTI for at least one multicast session for which the PTM configuration was not included in *RRCRelease* message:

4> acquire the *MBSMulticastConfiguration* message on multicast MCCH;

1> if the UE is acting as a L2 U2N Relay UE, for each of the *PagingRecord*, if any, included in the *Paging* message:

2> if the *ue-Identity* included in the *PagingRecord* in the *Paging* message matches the UE identity in *sl-PagingIdentityRemoteUE* included in *sl-PagingInfo-RemoteUE* received in *RemoteUEInformationSidelink* message from a L2 U2N Remote UE:

3> inititate the Uu Message transfer in sidelink to that UE as specified in 5.8.9.9;

*Next Change*

5.3.8.3 Reception of the *RRCRelease* by the UE

The UE shall:

1> delay the following actions defined in this clause 60 ms from the moment the *RRCRelease* message was received or optionally when lower layers indicate that the receipt of the *RRCRelease* message has been successfully acknowledged, whichever is earlier;

1> stop timer T380, if running;

1> stop timer T320, if running;

1> if timer T316 is running;

2> stop timer T316;

2> clear the information included in *VarRLF-Report,* if any;

1> stop timer T350, if running;

1> stop timer T346g, if running;

1> if theAS security is not activated:

2> ignore any field included in *RRCRelease* message except *waitTime*;

2> perform the actions upon going to RRC\_IDLE as specified in 5.3.11 with the release cause 'other' upon which the procedure ends;

1> if the *RRCRelease* message includes *redirectedCarrierInfo* indicating redirection to *eutra*:

2> if *cnType* is included:

3> after the cell selection, indicate the available CN Type(s) and the received *cnType* to upper layers;

NOTE 1: Handling the case if the E-UTRA cell selected after the redirection does not support the core network type specified by the *cnType,* is up to UE implementation.

2> if *voiceFallbackIndication* is included:

3> consider the RRC connection release was for EPS fallback for IMS voice (see TS 23.502 [43]);

1> if the *RRCRelease* message includes the *cellReselectionPriorities*:

2> store the cell reselection priority information provided by the *cellReselectionPriorities*;

2> if the *t320* is included:

3> start timer T320, with the timer value set according to the value of *t320*;

1> else:

2> apply the cell reselection priority information broadcast in the system information;

1> if *deprioritisationReq* is included and the UE supports RRC connection release with deprioritisation:

2> start or restart timer T325 with the timer value set to the *deprioritisationTimer* signalled;

2> store the *deprioritisationReq* until T325 expiry;

NOTE 1a: The UE stores the deprioritisation request irrespective of any cell reselection absolute priority assignments (by dedicated or common signalling) and regardless of RRC connections in NR or other RATs unless specified otherwise.

1> if the *RRCRelease* includes the *measIdleConfig*:

2> if T331 is running:

3> stop timer T331;

3> perform the actions as specified in 5.7.8.3;

2> if the *measIdleConfig* is set to *setup*:

3> store the received *measIdleDuration* in *VarMeasIdleConfig*;

3> start timer T331 with the value set to *measIdleDuration*;

3> if the *measIdleConfig* contains *measIdleCarrierListNR*:

4> store the received *measIdleCarrierListNR* in *VarMeasIdleConfig*;

3> if the *measIdleConfig* contains *measIdleCarrierListEUTRA*:

4> store the received *measIdleCarrierListEUTRA* in *VarMeasIdleConfig*;

3> if the *measIdleConfig* contains *validityAreaList*:

4> store the received *validityAreaList* in *VarMeasIdleConfig*;

1> if the *RRCRelease* includes *suspendConfig*:

2> reset MAC and release the default MAC Cell Group configuration, if any;

2> apply the received *suspendConfig* except the received *nextHopChainingCount*;

2> if the *sdt-Config* is configured:

3> for each of the DRB in the *sdt-DRB-List*:

4> consider the DRB to be configured for SDT;

3> if *sdt-SRB2-Indication* is configured:

4> consider the SRB2 to be configured for SDT;

3> for each RLC bearer (except those associated with broadcast MRBs) that is not suspended:

4> re-establish the RLC entity as specified in TS 38.322 [4];

3> for SRB2 (if it is resumed) and for SRB1:

4> trigger the PDCP entity to perform SDU discard as specified in TS 38.323 [5];

3> if *sdt-MAC-PHY-CG-Config* is configured:

4> configure the PCell with the configured grant resources for SDT and instruct the MAC entity to start the *cg-SDT-TimeAlignmentTimer*;

2> if *srs-PosRRC-Inactive* is configured:

3> apply the configuration and instruct MAC to start the *inactivePosSRS-TimeAlignmentTimer*;

NOTE 1b: The Network should provide full configuration to UE for SRS for Positioning in RRC\_INACTIVE.

2> remove all the entries within the MCG and the SCG *VarConditionalReconfig*, if any;

2> for each *measId* of the MCG *measConfig* and for each *measId* of the SCG *measConfig*, if configured, if the associated *reportConfig* has a *reportType* set to *condTriggerConfig*:

3> for the associated *reportConfigId*:

4> remove the entry with the matching *reportConfigId* from the *reportConfigList* within the *VarMeasConfig*;

3> if the associated *measObjectId* is only associated to a *reportConfig* with *reportType* set to *condTriggerConfig*:

4> remove the entry with the matching *measObjectId* from the *measObjectList* within the *VarMeasConfig*;

3> remove the entry with the matching *measId* from the *measIdList* within the *VarMeasConfig*;

2> if the UE is acting as L2 U2N Remote UE:

3> if the PC5-RRC connection with the U2N Relay UE is determined to be released:

4> indicate upper layers to trigger PC5 unicast link release;

3> else (i.e., maintain the PC5 RRC connection):

4> establish or re-establish (e.g. via release and add) SL RLC entity for SRB1;

2> else:

3> re-establish RLC entities for SRB1;

2> if the *RRCRelease* message with *suspendConfig* was received in response to an *RRCResumeRequest* or an *RRCResumeRequest1*:

3> stop the timer T319 if running;

3> in the stored UE Inactive AS context:

4> replace the KgNB and KRRCint keys with the current KgNB and KRRCint keys;

4> replace the *nextHopChainingCount* with the value of *nextHopChainingCount* received in the *RRCRelease* message*;*

4> replace the *cellIdentity* with the *cellIdentity* of the cell the UE has received the *RRCRelease* message;

4> if the *suspendConfig* contains the *sl-UEIdentityRemote* (i.e. the UE is a L2 U2N Remote UE):

5> replace the C-RNTI with the value of the *sl-UEIdentityRemote*;

5> replace the physical cell identitywith the value of the *sl-PhysCellId* in *sl-ServingCellInfo* contained in the discovery message received from the connected L2 U2N Relay UE;

4> else:

5> replace the C-RNTI with the C-RNTI used in the cell (see TS 38.321 [3]) the UE has received the *RRCRelease* message;

5> replace the physical cell identitywith the physical cell identity of the cell the UE has received the *RRCRelease* message;

3> replace the *nextHopChainingCount* with the value associated with the current KgNB;

3> stop the timer T319a if running and consider SDT procedure is not ongoing;

2> else:

3> store in the UE Inactive AS Context the *nextHopChainingCount* received in the *RRCRelease* message*,* the current KgNB and KRRCint keys, the ROHC state, the EHC context(s), the UDC state, the stored QoS flow to DRB mapping rules, the application layer measurement configuration, the C-RNTI used in the source PCell, the *cellIdentity* and the physical cell identity of the source PCell, the *spCellConfigCommon* within *ReconfigurationWithSync* of the NR PSCell (if configured) and all other parameters configured except for:

- parameters within *ReconfigurationWithSync* of the PCell;

- parameters within *ReconfigurationWithSync* of the NR PSCell, if configured;

- parameters within *MobilityControlInfoSCG* of the E-UTRA PSCell, if configured;

- *servingCellConfigCommonSIB*;

- *sl-L2RelayUE-Config*, if configured;

- *sl-L2RemoteUE-Config*, if configured;

NOTE 1c: *suspendConfig* is not stored as part of UE Inactive AS Context, except for the fields explicitly specified.

3> store any previously or subsequently received application layer measurement report containers for which no segment, or full message, has been submitted to lower layers for transmission;

NOTE 2: NR sidelink communication/discovery related configurations and logged measurement configuration are not stored as UE Inactive AS Context, when UE enters RRC\_INACTIVE.

2> suspend all SRB(s) and DRB(s), except SRB0 and broadcast MRBs;

2> suspend all multicast MRB(s) associated with multicast session(s) not configured to receive in RRC\_INACTIVE;

2> indicate PDCP suspend to lower layers of all DRBs and multicast MRBs associated with multicast session(s) not configured to receive in RRC\_INACTIVE;

2> release Uu Relay RLC channel(s), if configured;

2> release PC5 Relay RLC channel(s), if configured;

2> release the SRAP entity, if configured;

NOTE 2a: A L2 U2N Relay UE may re-establish the SL-RLC0, SL-RLC1 and SRAP entity after release.

2> if the *t380* is included:

3> start timer T380, with the timer value set to *t380*;

2> if the *RRCRelease* message is including the *waitTime*:

3> start timer T302 with the value set to the *waitTime*;

3> inform upper layers that access barring is applicable for all access categories except categories '0' and '2';

2> if T390 is running:

3> stop timer T390 for all access categories;

3> perform the actions as specified in 5.3.14.4;

2> indicate the suspension of the RRC connection to upper layers;

2> if the UE is capable of L2 U2N Remote UE:

3> enter RRC\_INACTIVE, and perform either cell selection as specified in TS 38.304 [20], or relay selection as specified in clause 5.8.15.3, or both;

2> else:

3> enter RRC\_INACTIVE and perform cell selection as specified in TS 38.304 [20];

2> if the *multicastConfigInactive* is configured:

3> if the multicast PTM configuration is provided for a multicast session for which the UE is not indicated to stop monitoring the G-RNTI and the UE selects the same cell as the one on which it received *RRCRelease*:

4> apply the multicast PTM configuration as specified in 5.x.3;

4> monitor the Multicast MCCH-RNTI as specified in 5.x.2;

1> else:

2> perform the actions upon going to RRC\_IDLE as specified in 5.3.11, with the release cause 'other'.

NOTE 3: Whether to release the PC5 unicast link is left to L2 U2N Remote UE's implementation.

NOTE 4: It is left to UE implementation whether to stop T430, if running, when going to RRC\_INACTIVE.

*Next Change*

### 5.3.13 RRC connection resume

#### 5.3.13.2 Initiation

The UE initiates the procedure when upper layers or AS (when responding to RAN paging, upon triggering RNA updates while the UE is in RRC\_INACTIVE, upon requesting multicast reception as specified in clause 5.3.13.x, for NR sidelink communication/discovery/V2X sidelink communication as specified in clause 5.3.13.1a) requests the resume of a suspended RRC connection or requests the resume for initiating SDT as specified in clause 5.3.13.1b.

The UE shall ensure having valid and up to date essential system information as specified in clause 5.2.2.2 before initiating this procedure.

Upon initiation of the procedure, the UE shall:

1> if the resumption of the RRC connection is triggered by response to NG-RAN paging; or

1> if the resumption of the RRC connection is triggered by multicast reception request as specified in clause 5.3.13.x:

2> select '0' as the Access Category;

2> perform the unified access control procedure as specified in 5.3.14 using the selected Access Category and one or more Access Identities provided by upper layers;

3> if the access attempt is barred, the procedure ends;

1> else if the resumption of the RRC connection is triggered by upper layers:

2> if the upper layers provide an Access Category and one or more Access Identities:

3> perform the unified access control procedure as specified in 5.3.14 using the Access Category and Access Identities provided by upper layers;

4> if the access attempt is barred, the procedure ends;

2> if the upper layers provide NSAG information and one or more S-NSSAI(s) triggering the access attempt (TS 23.501 [32] and TS 24.501 [23]):

3> apply the NSAG with highest NSAG priority among the NSAGs that are included in *SIB1* (i.e., in *FeatureCombination* and/or in *RA-PrioritizationSliceInfo*), and that are associated with the S-NSSAI(s) triggering the access attempt, in the Random Access procedure (TS 38.321 [3], clause 5.1);

NOTE: If there are multiple NSAGs with the same highest NAS-provided NSAG priority identified for access attempt as above, it is left to UE implementation to select the NSAG to be applied in the Random Access procedure.

2> if the resumption occurs after release with redirect with *mpsPriorityIndication*:

3> set the *resumeCause* to *mps-PriorityAccess*;

2> else:

3> set the *resumeCause* in accordance with the information received from upper layers;

1> else if the resumption of the RRC connection is triggered due to an RNA update as specified in 5.3.13.8:

2> if an emergency service is ongoing:

NOTE 1: How the RRC layer in the UE is aware of an ongoing emergency service is up to UE implementation.

3> select '2' as the Access Category;

3> set the *resumeCause* to *emergency*;

2> else:

3> select '8' as the Access Category;

2> perform the unified access control procedure as specified in 5.3.14 using the selected Access Category and one or more Access Identities to be applied as specified in TS 24.501 [23];

3> if the access attempt is barred:

4> set the variable *pendingRNA-Update* to *true*;

4> the procedure ends;

NOTE 2: In case the L2 U2N Relay UE initiates RRC connection resume triggered by reception of message from a L2 U2N Remote UE via SL-RLC0 or SL-RLC1 as specified in 5.3.13.1a, the L2 U2N Relay UE sets the *resumeCause* by implementation, but it can only set the *emergency*, *mps-PriorityAccess*, or *mcs-PriorityAccess* as *resumeCause*, if the same cause value in the message received from the L2 U2N Remote UE via SL-RLC0.

1> if the UE is in NE-DC or NR-DC:

2> if the UE does not support maintaining SCG configuration upon connection resumption:

3> release the MR-DC related configurations (i.e., as specified in 5.3.5.10) from the UE Inactive AS context, if stored;

1> if the UE does not support maintaining the MCG SCell configurations upon connection resumption:

2> release the MCG SCell(s) from the UE Inactive AS context, if stored;

1> if the UE is acting as L2 U2N Remote UE:

2> establish a SRAP entity as specified in TS 38.351 [66], if no SRAP entity has been established;

2> apply the default configuration of SL-RLC1 as defined in 9.2.4 for SRB1;

2> apply the default PDCP configuration as defined in 9.2.1 for SRB1;

2> apply the default configuration of SRAP as defined in 9.2.5 for SRB1;

1> else:

2> apply the default L1 parameter values as specified in corresponding physical layer specifications, except for the parameters for which values are provided in *SIB1*;

2> apply the default SRB1 configuration as specified in 9.2.1;

2> apply the default MAC Cell Group configuration as specified in 9.2.2;

1> release *delayBudgetReportingConfig* from the UE Inactive AS context, if stored;

1> stop timer T342, if running;

1> release *overheatingAssistanceConfig* from the UE Inactive AS context, if stored;

1> stop timer T345, if running;

1> release *idc-AssistanceConfig* from the UE Inactive AS context, if stored;

1> release *drx-PreferenceConfig* for all configured cell groups from the UE Inactive AS context, if stored;

1> stop all instances of timer T346a, if running;

1> release *maxBW-PreferenceConfig* and *maxBW-PreferenceConfigFR2-2* for all configured cell groups from the UE Inactive AS context, if stored;

1> stop all instances of timer T346b, if running;

1> release *maxCC-PreferenceConfig* for all configured cell groups from the UE Inactive AS context, if stored;

1> stop all instances of timer T346c, if running;

1> release *maxMIMO-LayerPreferenceConfig* and *maxMIMO-LayerPreferenceConfigFR2-2* for all configured cell groups from the UE Inactive AS context, if stored;

1> stop all instances of timer T346d, if running;

1> release *minSchedulingOffsetPreferenceConfig* and *minSchedulingOffsetPreferenceConfigExt* for all configured cell groups from the UE Inactive AS context, if stored;

1> stop all instances of timer T346e, if running;

1> release *rlm-RelaxationReportingConfig* for all configured cell groups from the UE Inactive AS context, if stored;

1> stop all instances of timer T346j, if running;

1> release *bfd-RelaxationReportingConfig* for all configured cell groups from the UE Inactive AS context, if stored;

1> stop all instances of timer T346k, if running;

1> release *releasePreferenceConfig* from the UE Inactive AS context, if stored;

1> release *wlanNameList* from the UE Inactive AS context, if stored;

1> release *btNameList* from the UE Inactive AS context, if stored;

1> release *sensorNameList* from the UE Inactive AS context, if stored;

1> release *obtainCommonLocation* from the UE Inactive AS context, if stored;

1> stop timer T346f, if running;

1> stop timer T346i, if running;

1> release *referenceTimePreferenceReporting* from the UE Inactive AS context, if stored;

1> release *sl-AssistanceConfigNR* from the UE Inactive AS context, if stored;

1> release *musim-GapAssistanceConfig* from the UE Inactive AS context, if stored and stop timer T346h, if running;

1> release *musim-GapConfig* from the UE Inactive AS context, if stored;

1> release *musim-LeaveAssistanceConfig* from the UE Inactive AS context, if stored;

1> release *propDelayDiffReportConfig* from the UE Inactive AS context, if stored;

1> release *ul-GapFR2-PreferenceConfig*, if configured;

1> release *rrm-MeasRelaxationReportingConfig* from the UE Inactive AS context, if stored;

1> if the UE is acting as L2 U2N Remote UE:

2> apply the specified configuration of SL-RLC0 used for the delivery of RRC message over SRB0 as specified in 9.1.1.4;

2> apply the SDAP configuration and PDCP configuration as specified in 9.1.1.2 for SRB0;

1> else:

2> apply the CCCH configuration as specified in 9.1.1.2;

2> apply the *timeAlignmentTimerCommon* included in *SIB1*;

1> if *sdt-MAC-PHY-CG-Config* is configured:

2> if the resume procedure is initiated in a cell that is different to the PCell in which the UE received the stored *sdt-MAC-PHY-CG-Config*:

3> release the stored *sdt-MAC-PHY-CG-Config*;

3> instruct the MAC entity to stop the *cg-SDT-TimeAlignmentTimer*, if it is running;

1> if *ncd-SSB-RedCapInitialBWP-SDT* is configured:

2> if the resume procedure is initiated in a cell that is different to the PCell in which the UE received the stored *ncd-SSB-RedCapInitialBWP-SDT*:

3> release the stored *ncd-SSB-RedCapInitialBWP-SDT;*

1> if conditions for initiating SDT in accordance with 5.3.13.1b are fulfilled:

2> consider the resume procedure is initiated for SDT;

2> start timer T319a when the lower layers first transmit the CCCH message;

2> consider SDT procedure is ongoing;

1> else:

2> start timer T319;

2> instruct the MAC entity to stop the *cg*-*SDT*-*TimeAlignmentTimer*, if it is running;

1> if *ta-Report* is configured with value *enabled* and the UE supports TA reporting:

2> indicate TA report initiation to lower layers;

1> set the variable *pendingRNA-Update* to *false*;

1> release *successHO-Config* from the UE Inactive AS context, if stored;

1. initiate transmission of the *RRCResumeRequest* message or *RRCResumeRequest1* in accordance with 5.3.13.3.

*Next Change*

5.3.13.4 Reception of the *RRCResume* by the UE

The UE shall:

1> stop timer T319, if running;

1> stop timer T319a, if running and consider SDT procedure is not ongoing;

1> stop timer T380, if running;

1> if T331 is running:

2> stop timer T331;

2> perform the actions as specified in 5.7.8.3;

1> if the *RRCResume* includes the *fullConfig*:

2> perform the full configuration procedure as specified in 5.3.5.11;

1> else:

2> if the *RRCResume* does not include the *restoreMCG-SCells*:

3> release the MCG SCell(s) from the UE Inactive AS context, if stored;

2> if the *RRCResume* does not include the *restoreSCG*:

3> release the MR-DC related configurations (i.e., as specified in 5.3.5.10) from the UE Inactive AS context, if stored;

2> restore the *masterCellGroup, mrdc-SecondaryCellGroup*, if stored, and *pdcp-Config* from the UE Inactive AS context;

2> configure lower layers to consider the restored MCG and SCG SCell(s) (if any) to be in deactivated state;

1> discard the UE Inactive AS context;

1> store the used *nextHopChainingCount* value associated to the current KgNB;

1> if *sdt-MAC-PHY-CG-Config* is configured:

2> instruct the MAC entity to stop the *cg-SDT-TimeAlignmentTimer*, if it is running;

2> instruct the MAC entity to start the *timeAlignmentTimer* associated with the PTAG*,* if it is not running;

1> if *srs-PosRRC-InactiveConfig* is configured:

2> instruct the MAC entity to stop *inactivePosSRS-TimeAlignmentTimer*, if it is running;

1> release the *suspendConfig* except the *ran-NotificationAreaInfo*;

1> if the *RRCResume* includes the *masterCellGroup*:

2> perform the cell group configuration for the received *masterCellGroup* according to 5.3.5.5;

1> if the *RRCResume* includes the *mrdc-SecondaryCellGroup:*

2> if the received *mrdc-SecondaryCellGroup* is set to *nr-SCG*:

3> perform the RRC reconfiguration according to 5.3.5.3 for the *RRCReconfiguration* message included in *nr-SCG*;

2> if the received *mrdc-SecondaryCellGroup* is set to *eutra-SCG*:

3> perform the RRC connection reconfiguration as specified in TS 36.331 [10], clause 5.3.5.3 for the *RRCConnectionReconfiguration* message included in *eutra-SCG*;

1> if the *RRCResume* includes the *radioBearerConfig*:

2> perform the radio bearer configuration according to 5.3.5.6;

1> if the *RRCResume* message includes the *sk-Counter*:

2> perform security key update procedure as specified in 5.3.5.7;

1> if the *RRCResume* message includes the *radioBearerConfig2*:

2> perform the radio bearer configuration according to 5.3.5.6;

1> if the *RRCResume* message includes the *needForGapsConfigNR*:

2> if *needForGapsConfigNR* is set to *setup*:

3> consider itself to be configured to provide the measurement gap requirement information of NR target bands;

2> else:

3> consider itself not to be configured to provide the measurement gap requirement information of NR target bands;

1> if the *RRCResume* message includes the *needForGapNCSG-ConfigNR*:

2> if *needForGapNCSG-ConfigNR* is set to *setup*:

3> consider itself to be configured to provide the measurement gap and NCSG requirement information of NR target bands;

2> else:

3> consider itself not to be configured to provide the measurement gap and NCSG requirement information of NR target bands;

1> if the *RRCResume* message includes the *needForGapNCSG-ConfigEUTRA*:

2> if *needForGapNCSG-ConfigEUTRA* is set to *setup*:

3> consider itself to be configured to provide the measurement gap and NCSG requirement information of E‑UTRA target bands;

2> else:

3> consider itself not to be configured to provide the measurement gap and NCSG requirement information of E‑UTRA target bands;

1> if the *RRCResume* message includes the *appLayerMeasConfig*:

2> perform the application layer measurement configuration procedure as specified in 5.3.5.13d;

1> if the *RRCResume* message includes the *sl-L2RemoteUE-Config* (i.e. the UE is a L2 U2N Remote UE):

2> perform the L2 U2N Remote UE configuration procedure as specified in 5.3.5.16;

1> if the *RRCResume* message includes the *sl-ConfigDedicatedNR*:

2> perform the sidelink dedicated configuration procedure as specified in 5.3.5.14;

1> resume SRB2 (if suspended), SRB3 (if configured), SRB4 (if configured), all DRBs (that are suspended) and multicast MRBs (that are suspended);

NOTE 1: If the SCG is deactivated, resuming SRB3 and all DRBs does not imply that PDCP or RRC PDUs can be transmitted or received on SCG RLC bearers.

1> if stored, discard the cell reselection priority information provided by the *cellReselectionPriorities* or inherited from another RAT;

1> stop timer T320, if running;

1> if the *RRCResume* message includes the *measConfig*:

2> perform the measurement configuration procedure as specified in 5.5.2;

1> resume measurements if suspended;

1> if T390 is running:

2> stop timer T390 for all access categories;

2> perform the actions as specified in 5.3.14.4;

1> if T302 is running:

2> stop timer T302;

2> perform the actions as specified in 5.3.14.4;

1> enter RRC\_CONNECTED;

1> indicate to upper layers that the suspended RRC connection has been resumed;

1> stop the cell re-selection procedure;

1> stop relay reselection procedure if any for L2 U2N Remote UE;

1> consider the current cell to be the PCell;

1> set the content of the of *RRCResumeComplete* message as follows:

2> if the upper layer provides NAS PDU, set the *dedicatedNAS-Message* to include the information received from upper layers;

2> if upper layers provides a PLMN:

3> if the UE is either allowed or instructed to access the PLMN via a cell for which at least one CAG ID is broadcast:

4> set the *selectedPLMN-Identity* from the *npn-IdentityInfoList*;

3> else:

4> set the *selectedPLMN-Identity* to the PLMN selected by upper layers from the *plmn-IdentityInfoList*;

2> if the *masterCellGroup* contains the *reportUplinkTxDirectCurrent*:

3> include the *uplinkTxDirectCurrentList* for each MCG serving cell with UL;

3> include *uplinkDirectCurrentBWP-SUL* for each MCG serving cell configured with SUL carrier, if any, within the *uplinkTxDirectCurrentList*;

2> if the *masterCellGroup* contains the *reportUplinkTxDirectCurrentTwoCarrier*:

3> include in the *uplinkTxDirectCurrentTwoCarrierList* the list of uplink Tx DC locations for the configured uplink carrier aggregation in the MCG;

2> if the *masterCellGroup* contains the *reportUplinkTxDirectCurrentMoreCarrier*:

3> include in the *uplinkTxDirectCurrentMoreCarrierList* the list of uplink Tx DC locations for the configured uplink carrier aggregation in the MCG;

2> if the UE has idle/inactive measurement information concerning cells other than the PCell available in *VarMeasIdleReport*:

3> if the *idleModeMeasurementReq* is included in the *RRCResume* message:

4> set the *measResultIdleEUTRA* in the *RRCResumeComplete* message to the value of *measReportIdleEUTRA* in the *VarMeasIdleReport,* if available;

4> set the *measResultIdleNR* in the *RRCResumeComplete* message to the value of *measReportIdleNR* in the *VarMeasIdleReport*, if available;

4> discard the *VarMeasIdleReport* upon successful delivery of the *RRCResumeComplete* message is confirmed by lower layers;

3> else:

4> if the SIB1 contains *idleModeMeasurementsNR* and the UE has NR idle/inactive measurement information concerning cells other than the PCell available in *VarMeasIdleReport*; or

4> if the SIB1 contains *idleModeMeasurementsEUTRA* and the UE has E-UTRA idle/inactive measurement information available in *VarMeasIdleReport*:

5> include the *idleMeasAvailable*;

2> if the *RRCResume* message includes *mrdc-SecondaryCellGroup* set to *eutra-SCG*:

3> include in the *eutra-SCG-Response* the E-UTRA *RRCConnectionReconfigurationComplete* message in accordance with TS 36.331 [10] clause 5.3.5.3;

2> if the *RRCResume* message includes *mrdc-SecondaryCellGroup* set to *nr-SCG*:

3> include in the *nr-SCG-Response* the SCG *RRCReconfigurationComplete* message;

2> if the UE has logged measurements available for NR and if the RPLMN is included in *plmn-IdentityList* stored in *VarLogMeasReport*:

3> include the *logMeasAvailable* in the *RRCResumeComplete* message*;*

3> if Bluetooth measurement results are included in the logged measurements the UE has available for NR:

4> include the *logMeasAvailableBT* in the *RRCResumeComplete* message;

3> if WLAN measurement results are included in the logged measurements the UE has available for NR:

4> include the *logMeasAvailableWLAN* in the *RRCResumeComplete* message;

2> if the *sigLoggedMeasType* in *VarLogMeasReport* is included:

3> if T330 timer is running and the logged measurements configuration is for NR:

4> set *sigLogMeasConfigAvailable* to *true* in the *RRCResumeComplete* message;

3> else:

4> if the UE has logged measurements available for NR:

5> set *sigLogMeasConfigAvailable* to *false* in the *RRCResumeComplete* message;

2> if the UE has connection establishment failure or connection resume failure information available in *VarConnEstFailReport* or *VarConnEstFailReportList* and if the RPLMN is equal to *plmn-Identity* stored in *VarConnEstFailReport* orin at least one of the entries of *VarConnEstFailReportList*:

3> include *connEstFailInfoAvailable* in the *RRCResumeComplete* message;

2> if the UE has radio link failure or handover failure information available in *VarRLF-Report* and if the RPLMN is included in *plmn-IdentityList* stored in *VarRLF-Report*; or

2> if the UE has radio link failure or handover failure information available in *VarRLF-Report* of TS 36.331 [10] and if the UE is capable of cross-RAT RLF reporting and if the RPLMN is included in *plmn-IdentityList* stored in *VarRLF-Report* of TS 36.331 [10]:

3> include *rlf-InfoAvailable* in the *RRCResumeComplete* message;

2> if the UE has successful handover information available in *VarSuccessHO-Report* and if the RPLMN is included in *plmn-IdentityList* stored in *VarSuccessHO-Report*:

3> include *successHO-InfoAvailable* in the *RRCResumeComplete* message;

2> if the UE supports storage of mobility history information and the UE has mobility history information available in *VarMobilityHistoryReport*:

3> include the *mobilityHistoryAvail* in the *RRCResumeComplete* message;

2> if *speedStateReselectionPars* is configured in the *SIB2*:

3> include the *mobilityState* in the *RRCResumeComplete* message and set it to the mobility state (as specified in TS 38.304 [20]) of the UE just prior to entering RRC\_CONNECTED state;

2> if the UE is configured to provide the measurement gap requirement information of NR target bands:

3> include the *NeedForGapsInfoNR* and set the contents as follows:

4> include *intraFreq-needForGap* and set the gap requirement information of intra-frequency measurement for each NR serving cell;

4> if *requestedTargetBandFilterNR* is configured, for each supported NR band that is also included in *requestedTargetBandFilterNR*, include an entry in *interFreq-needForGap* and set the gap requirement information for that band; otherwise, include an entry in *interFreq-needForGap* and set the corresponding gap requirement information for each supported NR band;

2> if the UE is configured to provide the measurement gap and NCSG requirement information of NR target bands:

3> include the *NeedForGapNCSG-InfoNR* and set the contents as follows:

4> include *intraFreq-needForNCSG* and set the gap and NCSG requirement information of intra-frequency measurement for each NR serving cell;

4> if *requestedTargetBandFilterNCSG-NR* is configured:

5> for each supported NR band included in *requestedTargetBandFilterNCSG-NR*, include an entry in *interFreq-needForNCSG* and set the NCSG requirement information for that band;

4> else:

5> include an entry for each supported NR band in *interFreq-needForNCSG* and set the corresponding NCSG requirement information;

2> if the UE is configured to provide the measurement gap and NCSG requirement information of E‑UTRA target bands:

3> include the *NeedForGapNCSG-InfoEUTRA* and set the contents as follows:

4> if *requestedTargetBandFilterNCSG-EUTRA* is configured:

5> for each supported E-UTRA band included in *requestedTargetBandFilterNCSG-EUTRA*, include an entry in *needForNCSG-EUTRA* and set the NCSG requirement information for that band;

4> else:

5> include an entry for each supported E-UTRA band in *needForNCSG-EUTRA* and set the corresponding NCSG requirement information;

1> submit the *RRCResumeComplete* message to lower layers for transmission;

1> the procedure ends.

NOTE 2: Network only configures at most one of *reportUplinkTxDirectCurrent, reportUplinkTxDirectCurrentTwoCarrier* or *reportUplinkTxDirectCurrentMoreCarrier* in one RRC message*.*

*Next Change (New)*

#### 5.3.13.x RRC connection resume for multicast reception

In RRC\_INACTIVE state, if configured with MBS multicast reception in RRC\_INACTIVE, the UE shall:

1> if the RRC connection resume procedure is triggered for multicast reception at reception of *SIB1*, as specified in 5.2.2.4.2; or

1> if the PTM configuration is not available in the cell after cell selection or reselection for a multicast session that the UE has joined for which the UE is not indicated to stop monitoring the G-RNTI; or

1> if *mbs-NeighbourCellList* acquired in the previous cell indicates that a multicast session that the UE has joined for which the UE is not indicated to stop monitoring the G-RNTI is not provided for RRC\_INACTIVE in the current serving cell; or

1> if the measured RSRP or RSRQ for serving cell as specified in TS 38.304 [20] is below the threshold indicated by *thresholdIndex* for a multicast session that the UE has joined:

2> initiate RRC connection resume procedure in 5.3.13.2 with *resumeCause* set to *mt-Access*.

*Next Change*

#### 5.3.14.4 T302, T390 expiry or stop (Barring alleviation)

The UE shall:

1> if timer T302 expires or is stopped:

2> for each Access Category for which T390 is not running:

3> consider the barring for this Access Category to be alleviated:

1> else if timer T390 corresponding to an Access Category other than '2' expires or is stopped, and if timer T302 is not running:

2> consider the barring for this Access Category to be alleviated;

1> else if timer T390 corresponding to the Access Category '2' expires or is stopped:

2> consider the barring for this Access Category to be alleviated;

1> when barring for an Access Category is considered being alleviated:

2> if the Access Category was informed to upper layers as barred:

3> inform upper layers about barring alleviation for the Access Category.

2> else if the Access Category is Access Category ‘0’:

3> perform actions specified in 5.3.13.x;2> if barring is alleviated for Access Category '8'; or

2> if barring is alleviated for Access Category '2':

3> perform actions specified in 5.3.13.8;

*Next Change*

## 5.9 MBS Broadcast

### 5.9.4 MBS Interest Indication

#### 5.9.4.1 General



Figure 5.9.4.1-1: MBS Interest Indication

The purpose of this procedure is to inform the network that the UE in RRC\_CONNECTED is receiving or is interested to receive MBS broadcast service(s) and to inform the network about the priority of MBS broadcast versus unicast and multicast MRB reception. MBS Interest Indication can only be sent after AS security activation.

#### 5.9.4.2 Initiation

An MBS capable UE in RRC\_CONNECTED may initiate the procedure in several cases including upon successful connection establishment/resume, upon entering or leaving the broadcast service area, upon MBS broadcast session start or stop, upon change of interest, upon change of priority between MBS broadcast reception and unicast/multicast reception, upon change to a PCell providing *SIB21* (i.e. where the *SIB1* scheduling information contains *SIB21*), upon receiving *SIB20* of an SCell via dedicated signalling, upon handover, upon RRC connection re-establishment, upon change to a PCell providing *nonServingCellMII* in *SIB1*, upon starting or stopping reception of MBS broadcast service on a non-serving cell, upon change of CFR information or subcarrier spacing for MBS broadcast reception on a non-serving cell. If the UE does not have the CFR information and subcarrier spacing for MBS broadcast reception on a non-serving cell at the time it sends the MBS Interest Indication, the UE sends an MBS Interest Indication after it has acquired those information from the non-serving cell.

Upon initiating the procedure, the UE shall:

1> if *SIB21* is provided by the PCell; or

1> if *nonServingCellMII* is provided in *SIB1* by the PCell:

2> ensure having a valid version of *SIB21* for the PCell, if present;

2> if the UE did not transmit MBS Interest Indication since last entering RRC\_CONNECTED state; or

2> if since the last time the UE transmitted an MBS Interest Indication, the UE connected to a PCell neither providing *SIB21* nor including *nonServingCellMII* in *SIB1*:

3> if the set of MBS broadcast frequencies of interest, determined in accordance with 5.9.4.3, is not empty:

4> set the contents of MBS Interest Indication according to 5.9.4.5 and initiate transmission of the *MBSInterestIndication* message;

2> else:

3> if the set of MBS broadcast frequencies of interest, determined in accordance with 5.9.4.3, is different from *mbs-FreqList* included in the last transmission of the MBS Interest Indication; or

3> if the set of MBS broadcast frequencies of interest for MBS broadcast reception on non-serving cell, determined in accordance with 5.9.4.3, is different from the list of MBS broadcast frequencies of interest for MBS broadcast reception on non-serving cell included in the last transmission of the MBS Interest Indication; or

3> if any of the subcarrier spacing and the CFR information for MBS broadcast reception on non-serving cell has changed since the last transmission of the MBS Interest Indication; or

3> if the subcarrier spacing and the CFR information for MBS broadcast reception on non-serving cell have been acquired from the non-serving cell which were not reported in the previous MBS Interest Indication; or

3> if the prioritisation of reception of all indicated MBS broadcast frequencies compared to reception of any of the established unicast bearers and multicast MRBs has changed since the last transmission of the MBS Interest Indication:

4> set the contents of MBS Interest Indication according to 5.9.4.5 and initiate transmission of the *MBSInterestIndication* message;

NOTE: The UE may send MBS Interest Indication even when it is able to receive the MBS services it is interested in, i.e. to avoid that the network allocates a configuration inhibiting MBS broadcast reception.

3> else if *SIB20* is provided for the PCell or for the SCell:

4> if since the last time the UE transmitted the MBS Interest Indication, the UE connected to a PCell not providing *SIB20* and the UE was not provided with *SIB20* for an SCell; or

4> if the set of MBS broadcast services of interest determined in accordance with 5.9.4.4 is different from *mbs-ServiceList* included in the last transmission of the MBS Interest Indication:

5> set the contents of MBS Interest Indication according to 5.9.4.5 and initiate the transmission of *MBSInterestIndication* message.

*Next Change*

#### 5.9.4.3 MBS frequencies of interest determination

The UE shall:

1> consider a frequency to be part of the MBS frequencies of interest if the following conditions are met:

2> at least one MBS session the UE is receiving or interested to receive via a broadcast MRB is ongoing or about to start; and

NOTE 1: The UE may determine whether the session is ongoing from the start and stop time indicated in the User Service Description (USD), see TS 38.300 [2] or TS 23.247 [67].

2> for at least one of these MBS sessions, *SIB21* acquired from the PCell or a non-serving cell includes mapping between the concerned frequency and one or more MBS FSAIs indicated in the USD for this session, or for at least one of these MBS sessions, the concerned frequency is not included in *SIB21* but is indicated in the USD for this session; and

NOTE 2: The UE considers a frequency to be part of the MBS frequencies of interest even though NG-RAN may (temporarily) not employ a broadcast MRB for the concerned session, i.e., the UE does not verify if the session is indicated on MCCH.

2> the *supportedBandCombinationList* the UE included in *UE-NR-Capability* contains at least one band combination including the concerned MBS frequency.

NOTE 3: When evaluating which frequencies the UE is capable of receiving, the UE does not take into account whether they are currently configured as serving frequencies.

*Next Change*

#### 5.9.4.5 Setting of the contents of MBS Interest Indication

The UE shall set the contents of the MBS Interest Indication as follows:

1> if the UE has a valid version of *SIB21* for the PCell; and

1> if the set of MBS frequencies of interest, determined in accordance with 5.9.4.3, is not empty:

2> include *mbs-FreqList* and set it to include the MBS frequencies of interest sorted by decreasing order of interest, using the *absoluteFrequencySSB* for serving frequency, if applicable, and the *ARFCN-ValueNR*(s) as included in *SIB21* or in USD (for neighbouring frequencies);

2> include *mbs-Priority* if the UE prioritises reception of all indicated MBS frequencies above reception of any of the unicast bearers and multicast MRBs;

NOTE 1: If the UE prioritises MBS broadcast reception and unicast/multicast data cannot be supported because of congestion on the MBS carrier(s), NG-RAN may for example initiate release of unicast bearers/multicast MRBs.

2> if *SIB20* is provided for the PCell or for the SCell:

3> include *mbs-ServiceList* and set it to indicate the set of MBS services of interest sorted by decreasing order of interest determined in accordance with 5.9.4.4.

NOTE 2: The *mbs-ServiceList* is not required to be used by the NG-RAN to determine the frequency on which to enable MBS broadcast reception for the UE.

1> if *nonServingCellMII* is included in *SIB1* for the PCell; and

1> if the set of MBS frequencies for MBS broadcast reception on non-serving cell, determined in accordance with 5.9.4.3, is not empty:

2> include *freqInfoMBS*;

2> if the UE has acquired *cfr-InfoMBS* and *subcarrierSpacing* for MBS broadcast reception on the non-serving cell:

3> include *cfr-InfoMBS* and *subcarrierSpacing*;

*Next Change (New)*

## 5.x MBS multicast reception in RRC\_INACTIVE

### 5.x.1 Introduction

#### 5.x.1.1 General

UE configured to receive MBS multicast service(s) in RRC\_INACTIVE that the UE has joined applies MBS multicast procedures described in this clause.

MBS multicast configuration information is provided in *RRCRelease* and on multicast MCCH logical channel.

When there is temporarily no data for an active multicast session or when the multicast session is deactivated, the network notifies the UE to stop monitoring the corresponding G-RNTI via MBS multicast configuration information. If the UE is notified to stop monitoring the G-RNTI(s) for all the joined multicast sessions, it stops monitoring the Multicast MCCH-RNTI. PDCCH monitoring occasion(s) for the multicast MCCH transmission are determined according to the common search space indicated by *searchspaceMulticastMCCH*. If *searchspaceMulticastMCCH* is set to zero, PDCCH monitoring occasions for the multicast MCCH message reception in the multicast MCCH transmission window are the same as PDCCH monitoring occasions for *SIB1* where the mapping between PDCCH monitoring occasions and SSBs is specified in TS 38.213 [13]. If *searchspaceMulticastMCCH* is not set to zero, PDCCH monitoring occasions for the multicast MCCH message are determined based on search space indicated by *searchspaceMulticastMCCH*. PDCCH monitoring occasions for the multicast MCCH message which are not overlapping with UL symbols (determined according to *tdd-UL-DL-ConfigurationCommon*) are sequentially numbered from one in the multicast MCCH transmission window. The [x×N+K]th PDCCH monitoring occasion for the multicast MCCH message in the multicast MCCH transmission window corresponds to the Kth transmitted SSB, where x = 0, 1, ...X-1, K = 1, 2, …N, N is the number of actual transmitted SSBs determined according to *ssb-PositionsInBurst* in *SIB1* and X is equal to CEIL(number of PDCCH monitoring occasions in multicast MCCH transmission window/N). The actual transmitted SSBs are sequentially numbered from one in ascending order of their SSB indexes. The UE assumes that, in the multicast MCCH transmission window, PDCCH for a multicast MCCH message is transmitted in at least one PDCCH monitoring occasion corresponding to each transmitted SSB and thus the selection of SSB for the reception multicast MCCH messages is up to UE implementation.

#### 5.x.1.3 Multicast MCCH information validity and notification of changes

Change of multicast MCCH information only occurs at specific radio frames, i.e. the concept of a modification period is used. Within a modification period, the same multicast MCCH information may be transmitted a number of times, as defined by its scheduling (which is based on a repetition period).

When the network changes (some of) the multicast MCCH information, it notifies the UEs about the change starting from the beginning of the multicast MCCH modification period via PDCCH which schedules the multicast MCCH in every repetition in that modification period.

Upon receiving a change notification, a UE receiving MBS multicast service(s) in RRC\_INACTIVE acquires the new multicast MCCH information starting from the same slot. The UE applies the previously acquired multicast MCCH information until the UE acquires the new multicast MCCH information.

### 5.x.2 Multicast MCCH information acquisition

#### 5.x.2.1 General



Figure 5.x.2.1-1: Multicast MCCH information acquisition

#### The UE applies the multicast MCCH information acquisition procedure to acquire the MBS multicast configuration information from the network. The procedure applies to UEs configured to receive MBS multicast services in RRC\_INACTIVE.5.x.2.2 Initiation

If configured to receive MBS multicast services in RRC\_INACTIVE, a UE applies the multicast MCCH information acquisition procedure for PTM configuration update and upon reselection to a new cell providing *SIBx*. A UE that is receiving MBS multicast data in RRC\_INACTIVE shall apply the multicast MCCH information acquisition procedure upon receiving a notification that the multicast MCCH information has changed.

NOTE 1: It is up to UE implementation how to address a possibility of the UE missing a multicast MCCH change notification.

Unless explicitly stated otherwise in the procedural specification, the multicast MCCH information acquisition procedure overwrites any stored multicast MCCH information, i.e. delta configuration is not applicable for multicast MCCH information and the UE discontinues using a field if it is absent in multicast MCCH information.

#### 5.x.2.3 Multicast MCCH information acquisition by the UE

A UE configured to receive an MBS multicast service in RRC\_INACTIVE shall:

1> if the procedure is triggered by a multicast MCCH information change notification:

2> start acquiring the *MBSMulticastConfiguration* message on multicast MCCH in the concerned cell from the slot in which the change notification was received;

1> if the UE moves to a different cell providing *SIBx;* or

1> if the UE receives *RRCRelease* configuring the UE to receive MBS multicast in RRC\_INACTIVE which doesn’t include PTM configuration for at least one multicast session for which the UE is not indicated to stop monitoring the G-RNTI:

2> acquire the *MBSMulticastConfiguration* message on multicast MCCH in the concerned cell at the next repetition period.

#### 5.x.2.4 Actions upon reception of the *MBSMulticastConfiguration* message

No UE requirements related to the contents of the *MBSMulticastConfiguration* message apply other than those specified elsewhere, e.g., within the corresponding field descriptions.

### 5.x.3 MRB configuration

5.x.3.1 General

The multicast MRB configuration procedure is used by the UE in RRC\_INACTIVE state to configure PDCP, RLC, MAC entities and the physical layer upon PTM configuration update and moving to a cell providing *SIBx*. The UE may perform multicast MRB modification or release/establishment when PTM configuration is updated via MCCH or when it moves to a cell where the PDCP COUNT of the corresponding multicast MRB is not synchronized within the RNA. The UE may perform multicast MRB modification when it moves to a cell where the PDCP COUNT of the corresponding multicast MRB is synchronized within the RNA. The UE resets MAC upon cell-reselection.

NOTE: How to perform modification of a multicast MRB which is already configured in the UE is left to UE implementation.

Upon moving to a cell where the PDCP COUNT of a multicast MRB is not synchronized, an indication is sent to the lower layer to inform the PDCP COUNT non-synchronization of the corresponding multicast MRB. Upon transition from RRC\_CONNECTED to RRC\_INACTIVE in the same cell, the UE can continue using the multicast MRBs used in RRC\_CONNECTED.

5.x.3.2 Multicast MRB establishment

Upon establishment of a multicast MRB, the UE shall:

1> establish a PDCP entity and an RLC entity i n accordance with *MRB-InfoBroadcast* for this multicast MRB included in the *MBSMulticastConfiguration* message and the configuration specified in 9.1.1.7;

1> configure the MAC layer in accordance with the *mtch-SchedulingInfo* (if included);

1> configure the physical layer in accordance with the *mbs-SessionInfoList*, *searchSpaceMulticastMTCH,* and *pdsch-ConfigMTCH*, applicable for the multicast MRB;

1> if an SDAP entity with the received *mbs-SessionId* does not exist:

2> establish an SDAP entity as specified in TS 37.324 [24] clause 5.1.1;

2> indicate the establishment of the user plane resources for the *mbs-SessionId* to upper layers;

1> receive DL-SCH on the cell where the *MBSMulticastConfiguration* message was received for the established multicast MRB using *g-RNTI* and *mtch-SchedulingInfo* (if included) in this message for this MBS multicast service.

5.x.3.3 Multicast MRB release

Upon release of a multicast MRB, the UE shall:

1> release the PDCP entity, RLC entity as well as the related MAC and physical layer configuration;

1> if the SDAP entity associated with the corresponding *mbs-SessionId* has no associated MRB:

2> release the SDAP entity, as specified in TS 37.324 [24] clause 5.1.2;

2> indicate the release of the user plane resources for the *mbs-SessionId* to upper layers.

*Next Change*

## 6.2 RRC messages

### 6.2.2 Message definitions

#### *– MBSInterestIndication*

The *MBSInterestIndication* message is used to inform network that the UE is receiving/ interested to receive or no longer receiving/ interested to receive MBS broadcast service(s) via a broadcast MRB or that the information for MBS broadcast reception on the non-serving cell has changed.

Signalling radio bearer: SRB1

RLC-SAP: AM

Logical channel: DCCH

Direction: UE to Network

***MBSInterestIndication message***

-- ASN1START

-- TAG-MBSINTERESTINDICATION-START

MBSInterestIndication-r17 ::= SEQUENCE {

criticalExtensions CHOICE {

mbsInterestIndication-r17 MBSInterestIndication-r17-IEs,

criticalExtensionsFuture SEQUENCE {}

}

}

MBSInterestIndication-r17-IEs ::= SEQUENCE {

mbs-FreqList-r17 CarrierFreqListMBS-r17 OPTIONAL,

mbs-Priority-r17 ENUMERATED {true} OPTIONAL,

mbs-ServiceList-r17 MBS-ServiceList-r17 OPTIONAL,

lateNonCriticalExtension OCTET STRING OPTIONAL,

nonCriticalExtension MBSInterestIndication-v18xy OPTIONAL

}

MBSInterestIndication-v18xy ::= SEQUENCE {

mbs-NonServingInfoList-r18 MBS-NonServingInfoList-r18 OPTIONAL,

lateNonCriticalExtension OCTET STRING OPTIONAL,

nonCriticalExtension SEQUENCE {} OPTIONAL

}

-- TAG-MBSINTERESTINDICATION-STOP

-- ASN1STOP

| ***MBSInterestIndication* field descriptions** |
| --- |
| ***mbs-FreqList***  List of MBS frequencies on which the UE is receiving or interested to receive MBS broadcast service via a broadcast MRB. |
| ***mbs-Priority***  Indicates whether the UE prioritises MBS broadcast reception above unicast and MBS multicast reception. The field is present (i.e. value *true*), if the UE prioritises reception of broadcast services, on frequencies indicated in *mbs-FreqLis*t, above a reception of any of the unicast bearers and multicast MRBs. Otherwise the field is absent. |
| ***mbs-ServiceList***  List of MBS broadcast services which the UE is receiving or interested to receive. |
| ***mbs-NonServingInfoList***  Indicates information for MBS broadcast reception on the non-serving cell. | |

Next Change

#### *– MBSMulticastConfiguration*

The *MBSMulticastConfiguration* message contains the control information applicable for MBS multicast services transmitted via multicast MRBs for RRC\_INACTIVE UEs.

Signalling radio bearer: N/A

RLC-SAP: UM

Logical channel: multicast MCCH

Direction: Network to UE

***MBSMulticastConfiguration message***

-- ASN1START

-- TAG-MBSMULTICASTCONFIGURATION-START

MBSMulticastConfiguration-r18 ::= SEQUENCE {

criticalExtensions CHOICE {

mbsMulticastConfiguration-r18 MBSMulticastConfiguration-r18-IEs,

criticalExtensionsFuture SEQUENCE {}

}

}

MBSMulticastConfiguration-r18-IEs ::= SEQUENCE {

mbs-SessionInfoList-r18 MBS-SessionInfoListMulticast-r18 OPTIONAL, -- Need R

mbs-NeighbourCellList-r18 MBS-NeighbourCellList-r17 OPTIONAL, -- Need S

drx-ConfigPTM-List-r18 SEQUENCE (SIZE (1..maxNrofDRX-ConfigPTM-r17)) OF DRX-ConfigPTM-r17 OPTIONAL, -- Need R

pdsch-ConfigMTCH-r18 PDSCH-ConfigBroadcast-r17 OPTIONAL, -- Need S

mtch-SSB-MappingWindowList-r18 MTCH-SSB-MappingWindowList-r17 OPTIONAL, -- Need R

thresholdMBS-List-r18 SEQUENCE (SIZE (1..maxNrofThresholdMBS-r18)) OF ThresholdMBS-r18 OPTIONAL, -- Need R

lateNonCriticalExtension OCTET STRING OPTIONAL,

nonCriticalExtension SEQUENCE {} OPTIONAL

}

ThresholdMBS-r18 ::= CHOICE {

rsrp-r18 RSRP-Range,

rsrq-r18 RSRQ-Range

}

-- TAG-MBSMULTICASTCONFIGURATION-STOP

-- ASN1STOP

| ***MBSMulticastConfiguration* field descriptions** |
| --- |
| ***mbs-NeighbourCellList***  List of neighbour cells providing one or more MBS multicast services for RRC\_INACTIVE that are provided by the current cell. This field is used by the UE together with *mtch-NeighbourCell* field signalled for each MBS session in the corresponding *MBS-SessionInfo*. When an empty *mbs-NeighbourCellList* list is signalled, the UE shall assume that MBS multicast services signalled in *mbs-SessionInfoList* in the *MBSMulticastConfiguration* message are not provided in any neighbour cell. When a non-empty *mbs-NeighbourCellList* is signalled, the current serving cell does not provide information about MBS multicast services of a neighbour cell that is not included in *mbs-NeighbourCellList*, i.e., the UE cannot determine the presence or absence of an MBS multicast service of a neighbour cell that is absent. When the field *mbs-NeighbourCellList* is absent, the current serving cell does not provide information about MBS multicast services in the neighbouring cells, i.e. the UE cannot determine the presence or absence of an MBS multicast service in neighbouring cells based on the absence of this field. |
| ***mbs-SessionInfoList***  Provides the configuration of each MBS session provided by MBS multicast in the current cell. |
| ***pdsch-ConfigMTCH***  Provides parameters for acquiring the PDSCH for MTCH. When this field is absent, the UE shall use parameters in *pdsch-ConfigMCCH* in SIBx to acquire the PDSCH for MTCH. |
| ***thresholdMBS-List***  List of reception quality thresholds for RRC connection resume for a UE receiving multicast in RRC\_INACTIVE. |

Next Change

– *Paging*

The *Paging* message is used for the notification of one or more UEs.

Signalling radio bearer: N/A

RLC-SAP: TM

Logical channel: PCCH

Direction: Network to UE

***Paging* message**

-- ASN1START

-- TAG-PAGING-START

Paging ::= SEQUENCE {

pagingRecordList PagingRecordList OPTIONAL, -- Need N

lateNonCriticalExtension OCTET STRING OPTIONAL,

nonCriticalExtension Paging-v1700-IEs OPTIONAL

}

Paging-v1700-IEs ::= SEQUENCE {

pagingRecordList-v1700 PagingRecordList-v1700 OPTIONAL, -- Need N

pagingGroupList-r17 PagingGroupList-r17 OPTIONAL, -- Need N

nonCriticalExtension Paging-v18xy-IEs OPTIONAL

}

Paging-v18xy-IEs ::= SEQUENCE {

pagingGroupList-v18xy PagingGroupList-v18xy OPTIONAL, -- Need N

nonCriticalExtension SEQUENCE {} OPTIONAL

}

PagingRecordList ::= SEQUENCE (SIZE(1..maxNrofPageRec)) OF PagingRecord

PagingRecordList-v1700 ::= SEQUENCE (SIZE(1..maxNrofPageRec)) OF PagingRecord-v1700

PagingGroupList-r17 ::= SEQUENCE (SIZE(1..maxNrofPageGroup-r17)) OF TMGI-r17

PagingGroupList-v18xy ::= SEQUENCE (SIZE(1..maxNrofPageGroup-r17)) OF GroupPaging-r18

PagingRecord ::= SEQUENCE {

ue-Identity PagingUE-Identity,

accessType ENUMERATED {non3GPP} OPTIONAL, -- Need N

...

}

PagingRecord-v1700 ::= SEQUENCE {

pagingCause-r17 ENUMERATED {voice} OPTIONAL -- Need N

}

PagingUE-Identity ::= CHOICE {

ng-5G-S-TMSI NG-5G-S-TMSI,

fullI-RNTI I-RNTI-Value,

...

}

GroupPaging-r18 ::= SEQUENCE {

inactiveReceptionAllowed-r18 ENUMERATED {true} OPTIONAL -- Need N

}

-- TAG-PAGING-STOP

-- ASN1STOP

|  |
| --- |
| ***PagingRecord* field descriptions** |
| ***accessType***  Indicates whether the *Paging* message is originated due to the PDU sessions from the non-3GPP access. |
| ***pagingRecordList***  If the network includes pagingRecordList-v1700, it includes the same number of entries, and listed in the same order, as in pagingRecordList (i.e. without suffix). |
| ***pagingCause***  Indicates whether the Paging message is originated due to IMS voice. If this field is present, it implies that the corresponding paging entry is for IMS voice. If upper layers indicate the support of paging cause and if this field is not present but pagingRecordList-v1700 is present, it implies that the corresponding paging entry is for a service other than IMS voice. Otherwise, paging cause is undetermined. |
| ***pagingGroupList***  If the network includes *pagingGroupList-v18xy*, it includes the same number of elements, and listed in the same order, as in *pagingGroupList-r17*. The first element corresponds to the first TMGI in *pagingGroupList-r17*. The second element corresponds to the second TMGI in *pagingGroupList-r17*, and so on. | |
| ***inactiveReceptionAllowed***  Indicates whether the UE with a valid PTM configuration for a *TMGI* in the *PagingGroupList* stays in RRC\_INACTIVE to receive the corresponding MBS multicast session. | |

Next Change

– *RRCRelease*

The *RRCRelease* message is used to command the release of an RRC connection or the suspension of the RRC connection.

Signalling radio bearer: SRB1

RLC-SAP: AM

Logical channel: DCCH

Direction: Network to UE

***RRCRelease* message**

-- ASN1START

-- TAG-RRCRELEASE-START

RRCRelease ::= SEQUENCE {

rrc-TransactionIdentifier RRC-TransactionIdentifier,

criticalExtensions CHOICE {

rrcRelease RRCRelease-IEs,

criticalExtensionsFuture SEQUENCE {}

}

}

RRCRelease-IEs ::= SEQUENCE {

redirectedCarrierInfo RedirectedCarrierInfo OPTIONAL, -- Need N

cellReselectionPriorities CellReselectionPriorities OPTIONAL, -- Need R

suspendConfig SuspendConfig OPTIONAL, -- Need R

deprioritisationReq SEQUENCE {

deprioritisationType ENUMERATED {frequency, nr},

deprioritisationTimer ENUMERATED {min5, min10, min15, min30}

} OPTIONAL, -- Need N

lateNonCriticalExtension OCTET STRING OPTIONAL,

nonCriticalExtension RRCRelease-v1540-IEs OPTIONAL

}

RRCRelease-v1540-IEs ::= SEQUENCE {

waitTime RejectWaitTime OPTIONAL, -- Need N

nonCriticalExtension RRCRelease-v1610-IEs OPTIONAL

}

RRCRelease-v1610-IEs ::= SEQUENCE {

voiceFallbackIndication-r16 ENUMERATED {true} OPTIONAL, -- Need N

measIdleConfig-r16 SetupRelease {MeasIdleConfigDedicated-r16} OPTIONAL, -- Need M

nonCriticalExtension RRCRelease-v1650-IEs OPTIONAL

}

RRCRelease-v1650-IEs ::= SEQUENCE {

mpsPriorityIndication-r16 ENUMERATED {true} OPTIONAL, -- Cond Redirection2

nonCriticalExtension RRCRelease-v1710-IEs OPTIONAL

}

RRCRelease-v1710-IEs ::= SEQUENCE {

noLastCellUpdate-r17 ENUMERATED {true} OPTIONAL, -- Need S

nonCriticalExtension SEQUENCE {} OPTIONAL

}

RedirectedCarrierInfo ::= CHOICE {

nr CarrierInfoNR,

eutra RedirectedCarrierInfo-EUTRA,

...

}

RedirectedCarrierInfo-EUTRA ::= SEQUENCE {

eutraFrequency ARFCN-ValueEUTRA,

cnType ENUMERATED {epc,fiveGC} OPTIONAL -- Need N

}

CarrierInfoNR ::= SEQUENCE {

carrierFreq ARFCN-ValueNR,

ssbSubcarrierSpacing SubcarrierSpacing,

smtc SSB-MTC OPTIONAL, -- Need S

...

}

SuspendConfig ::= SEQUENCE {

fullI-RNTI I-RNTI-Value,

shortI-RNTI ShortI-RNTI-Value,

ran-PagingCycle PagingCycle,

ran-NotificationAreaInfo RAN-NotificationAreaInfo OPTIONAL, -- Need M

t380 PeriodicRNAU-TimerValue OPTIONAL, -- Need R

nextHopChainingCount NextHopChainingCount,

...,

[[

sl-UEIdentityRemote-r17 RNTI-Value OPTIONAL, -- Cond L2RemoteUE

sdt-Config-r17 SetupRelease { SDT-Config-r17 } OPTIONAL, -- Need M

srs-PosRRC-Inactive-r17 SetupRelease { SRS-PosRRC-Inactive-r17 } OPTIONAL, -- Need M

ran-ExtendedPagingCycle-r17 ExtendedPagingCycle-r17 OPTIONAL -- Cond RANPaging

]],

[[

ncd-SSB-RedCapInitialBWP-SDT-r17 SetupRelease {NonCellDefiningSSB-r17} OPTIONAL -- Need M

]],

[[

multicastConfigInactive-r18 SetupRelease { MulticastConfigInactive-r18 } OPTIONAL -- Need M

]]

}

PeriodicRNAU-TimerValue ::= ENUMERATED { min5, min10, min20, min30, min60, min120, min360, min720}

CellReselectionPriorities ::= SEQUENCE {

freqPriorityListEUTRA FreqPriorityListEUTRA OPTIONAL, -- Need M

freqPriorityListNR FreqPriorityListNR OPTIONAL, -- Need M

t320 ENUMERATED {min5, min10, min20, min30, min60, min120, min180, spare1} OPTIONAL, -- Need R

...,

[[

freqPriorityListDedicatedSlicing-r17 FreqPriorityListDedicatedSlicing-r17 OPTIONAL -- Need M

]]

}

PagingCycle ::= ENUMERATED {rf32, rf64, rf128, rf256}

ExtendedPagingCycle-r17 ::= ENUMERATED {rf256, rf512, rf1024, spare1}

FreqPriorityListEUTRA ::= SEQUENCE (SIZE (1..maxFreq)) OF FreqPriorityEUTRA

FreqPriorityListNR ::= SEQUENCE (SIZE (1..maxFreq)) OF FreqPriorityNR

FreqPriorityEUTRA ::= SEQUENCE {

carrierFreq ARFCN-ValueEUTRA,

cellReselectionPriority CellReselectionPriority,

cellReselectionSubPriority CellReselectionSubPriority OPTIONAL -- Need R

}

FreqPriorityNR ::= SEQUENCE {

carrierFreq ARFCN-ValueNR,

cellReselectionPriority CellReselectionPriority,

cellReselectionSubPriority CellReselectionSubPriority OPTIONAL -- Need R

}

RAN-NotificationAreaInfo ::= CHOICE {

cellList PLMN-RAN-AreaCellList,

ran-AreaConfigList PLMN-RAN-AreaConfigList,

...

}

PLMN-RAN-AreaCellList ::= SEQUENCE (SIZE (1.. maxPLMNIdentities)) OF PLMN-RAN-AreaCell

PLMN-RAN-AreaCell ::= SEQUENCE {

plmn-Identity PLMN-Identity OPTIONAL, -- Need S

ran-AreaCells SEQUENCE (SIZE (1..32)) OF CellIdentity

}

PLMN-RAN-AreaConfigList ::= SEQUENCE (SIZE (1..maxPLMNIdentities)) OF PLMN-RAN-AreaConfig

PLMN-RAN-AreaConfig ::= SEQUENCE {

plmn-Identity PLMN-Identity OPTIONAL, -- Need S

ran-Area SEQUENCE (SIZE (1..16)) OF RAN-AreaConfig

}

RAN-AreaConfig ::= SEQUENCE {

trackingAreaCode TrackingAreaCode,

ran-AreaCodeList SEQUENCE (SIZE (1..32)) OF RAN-AreaCode OPTIONAL -- Need R

}

SDT-Config-r17 ::= SEQUENCE {

sdt-DRB-List-r17 SEQUENCE (SIZE (0..maxDRB)) OF DRB-Identity OPTIONAL, -- Need M

sdt-SRB2-Indication-r17 ENUMERATED {allowed} OPTIONAL, -- Need R

sdt-MAC-PHY-CG-Config-r17 SetupRelease {SDT-CG-Config-r17} OPTIONAL, -- Need M

sdt-DRB-ContinueROHC-r17 ENUMERATED { cell, rna } OPTIONAL -- Need S

}

SDT-CG-Config-r17 ::= OCTET STRING (CONTAINING SDT-MAC-PHY-CG-Config-r17)

SDT-MAC-PHY-CG-Config-r17 ::= SEQUENCE {

-- CG-SDT specific configuration

cg-SDT-ConfigLCH-RestrictionToAddModList-r17 SEQUENCE (SIZE(1..maxLC-ID)) OF CG-SDT-ConfigLCH-Restriction-r17 OPTIONAL, -- Need N

cg-SDT-ConfigLCH-RestrictionToReleaseList-r17 SEQUENCE (SIZE(1..maxLC-ID)) OF LogicalChannelIdentity OPTIONAL, -- Need N

cg-SDT-ConfigInitialBWP-NUL-r17 SetupRelease {BWP-UplinkDedicatedSDT-r17} OPTIONAL, -- Need M

cg-SDT-ConfigInitialBWP-SUL-r17 SetupRelease {BWP-UplinkDedicatedSDT-r17} OPTIONAL, -- Need M

cg-SDT-ConfigInitialBWP-DL-r17 BWP-DownlinkDedicatedSDT-r17 OPTIONAL, -- Need M

cg-SDT-TimeAlignmentTimer-r17 TimeAlignmentTimer OPTIONAL, -- Need M

cg-SDT-RSRP-ThresholdSSB-r17 RSRP-Range OPTIONAL, -- Need M

cg-SDT-TA-ValidationConfig-r17 SetupRelease { CG-SDT-TA-ValidationConfig-r17 } OPTIONAL, -- Need M

cg-SDT-CS-RNTI-r17 RNTI-Value OPTIONAL, -- Need M

...

}

CG-SDT-TA-ValidationConfig-r17 ::= SEQUENCE {

cg-SDT-RSRP-ChangeThreshold-r17 ENUMERATED { dB2, dB4, dB6, dB8, dB10, dB14, dB18, dB22,

dB26, dB30, dB34, spare5, spare4, spare3, spare2, spare1}

}

BWP-DownlinkDedicatedSDT-r17 ::= SEQUENCE {

pdcch-Config-r17 SetupRelease { PDCCH-Config } OPTIONAL, -- Need M

pdsch-Config-r17 SetupRelease { PDSCH-Config } OPTIONAL, -- Need M

...

}

BWP-UplinkDedicatedSDT-r17 ::= SEQUENCE {

pusch-Config-r17 SetupRelease { PUSCH-Config } OPTIONAL, -- Need M

configuredGrantConfigToAddModList-r17 ConfiguredGrantConfigToAddModList-r16 OPTIONAL, -- Need N

configuredGrantConfigToReleaseList-r17 ConfiguredGrantConfigToReleaseList-r16 OPTIONAL, -- Need N

...

}

CG-SDT-ConfigLCH-Restriction-r17 ::= SEQUENCE {

logicalChannelIdentity-r17 LogicalChannelIdentity,

configuredGrantType1Allowed-r17 ENUMERATED {true} OPTIONAL, -- Need R

allowedCG-List-r17 SEQUENCE (SIZE (0.. maxNrofConfiguredGrantConfigMAC-1-r16)) OF ConfiguredGrantConfigIndexMAC-r16

OPTIONAL -- Need R

}

SRS-PosRRC-Inactive-r17 ::= OCTET STRING (CONTAINING SRS-PosRRC-InactiveConfig-r17)

SRS-PosRRC-InactiveConfig-r17 ::= SEQUENCE {

srs-PosConfigNUL-r17 SRS-PosConfig-r17 OPTIONAL, -- Need R

srs-PosConfigSUL-r17 SRS-PosConfig-r17 OPTIONAL, -- Need R

bwp-NUL-r17 BWP OPTIONAL, -- Need S

bwp-SUL-r17 BWP OPTIONAL, -- Need S

inactivePosSRS-TimeAlignmentTimer-r17 TimeAlignmentTimer OPTIONAL, -- Need M

inactivePosSRS-RSRP-ChangeThreshold-r17 RSRP-ChangeThreshold-r17 OPTIONAL -- Need M

}

RSRP-ChangeThreshold-r17 ::= ENUMERATED {dB4, dB6, dB8, dB10, dB14, dB18, dB22, dB26, dB30, dB34, spare6, spare5, spare4, spare3, spare2, spare1}

SRS-PosConfig-r17 ::= SEQUENCE {

srs-PosResourceSetToReleaseList-r17 SEQUENCE (SIZE(1..maxNrofSRS-PosResourceSets-r16)) OF SRS-PosResourceSetId-r16 OPTIONAL,-- Need N

srs-PosResourceSetToAddModList-r17 SEQUENCE (SIZE(1..maxNrofSRS-PosResourceSets-r16)) OF SRS-PosResourceSet-r16 OPTIONAL,-- Need N

srs-PosResourceToReleaseList-r17 SEQUENCE (SIZE(1..maxNrofSRS-PosResources-r16)) OF SRS-PosResourceId-r16 OPTIONAL,-- Need N

srs-PosResourceToAddModList-r17 SEQUENCE (SIZE(1..maxNrofSRS-PosResources-r16)) OF SRS-PosResource-r16 OPTIONAL -- Need N

}

MulticastConfigInactive-r18::= SEQUENCE {

inactivePTM-Config-r18 OCTET STRING (CONTAINING MBSMulticastConfiguration) OPTIONAL, -- Need N

inactiveMCCH-Config-r18 OCTET STRING (CONTAINING SystemInformation) OPTIONAL -- Need N

}

-- TAG-RRCRELEASE-STOP

-- ASN1STOP

|  |
| --- |
| ***RRCRelease-IEs* field descriptions** |
| ***cellReselectionPriorities***  Dedicated priorities to be used for cell reselection as specified in TS 38.304 [20]*.* The maximum number of NR carrier frequencies that the network can configure through *FreqPriorityListNR* and *FreqPriorityListDedicatedSlicing* together is eight. If the same frequency is configured in both *FreqPriorityListNR* and *FreqPriorityListDedicatedSlicing*, the frequency is only counted once. |
| ***cnType***  Indicate that the UE is redirected to EPC or 5GC. |
| ***deprioritisationReq***  Indicates whether the current frequency or RAT is to be de-prioritised. |
| ***deprioritisationTimer***  Indicates the period for which either the current carrier frequency or NR is deprioritised. Value *minN* corresponds to N minutes. |
| ***measIdleConfig***  Indicates measurement configuration to be stored and used by the UE while in RRC\_IDLE or RRC\_INACTIVE. |
| ***mpsPriorityIndication***  Indicates the UE can set the establishment cause to to *mps-PriorityAccess* for a new connection following a redirect to NR or set the resume cause to *mps-PriorityAccess* for a resume following a redirect to NR. If the target RAT is E-UTRA, see TS 36.331 [10]. The gNB sets the indication only for UEs authorized to receive MPS treatment as indicated by ARP and/or QoS characteristics at the gNB, and it is applicable only for this instance of release with redirection to carrier/RAT included in the *redirectedCarrierInfo* field in the *RRCRelease* message. |
| ***multicastConfigInactive***  Indicates the multicast service(s) that can be received in RRC\_INACTIVE in the current serving cell and optionally the corresponding configuration. The presence of this field indicates the UE is configured to receive MBS multicast in RRC\_INACTIVE. |
| ***noLastCellUpdate***  Presence of the field indicates that the last used cell for PEI shall not be updated. When the field is absent, the PEI-capable UE shall update its last used cell with the current cell. The UE shall not update its last used cell with the current cell if the AS security is not activated. |
| ***srs-PosRRC-InactiveConfig***  SRS for positioning configuration during RRC\_INACTIVE state. |
| ***suspendConfig***  Indicates configuration for the RRC\_INACTIVE state. The network does not configure *suspendConfig* when the network redirect the UE to an inter-RAT carrier frequency or if the UE is configured with a DAPS bearer. |
| ***redirectedCarrierInfo***  Indicates a carrier frequency (downlink for FDD) and is used to redirect the UE to an NR or an inter-RAT carrier frequency, by means of cell selection at transition to RRC\_IDLE or RRC\_INACTIVE as specified in TS 38.304 [20]. Based on UE capability, the network may include *redirectedCarrierInfo* in *RRCRelease* message with *suspendConfig* if this message is sent in response to an *RRCResumeRequest* or an *RRCResumeRequest1* which is triggered by the NAS layer (see 5.3.1.4 in TS 24.501 [23]). |
| ***voiceFallbackIndication***  Indicates the RRC release is triggered by EPS fallback for IMS voice as specified in TS 23.502 [43]. |

|  |
| --- |
| ***CarrierInfoNR* field descriptions** |
| ***carrierFreq***  Indicates the redirected NR frequency. |
| ***ssbSubcarrierSpacing***  Subcarrier spacing of SSB in the redirected SSB frequency.  Only the following values are applicable depending on the used frequency:  FR1: 15 or 30 kHz  FR2-1: 120 or 240 kHz  FR2-2: 120, 480, or 960 kHz |
| ***smtc***  The SSB periodicity/offset/duration configuration for the redirected SSB frequency. It is based on timing reference of PCell. If the field is absent, the UE uses the SMTC configured in the measObjectNR having the same SSB frequency and subcarrier spacing. |

|  |
| --- |
| ***RAN-NotificationAreaInfo* field descriptions** |
| ***cellList***  A list of cells configured as RAN area. |
| ***ran-AreaConfigList***  A list of RAN area codes or RA code(s) as RAN area. |

|  |
| --- |
| ***PLMN-RAN-AreaConfig* field descriptions** |
| ***plmn-Identity***  PLMN Identity to which the cells in *ran-Area* belong. If the field is absent the UE not in SNPN access mode uses the ID of the registered PLMN. This field is not included for UE in SNPN access mode (for UE in SNPN access mode the *ran-Area* always belongs to the registered SNPN). |
| ***ran-AreaCodeList***  The total number of RAN-AreaCodes of all PLMNs does not exceed 32. |
| ***ran-Area***  Indicates whether TA code(s) or RAN area code(s) are used for the RAN notification area. The network uses only TA code(s) or both TA code(s) and RAN area code(s) to configure a UE. The total number of TACs across all PLMNs does not exceed 16. |

|  |
| --- |
| ***PLMN-RAN-AreaCell* field descriptions** |
| ***plmn-Identity***  PLMN Identity to which the cells in *ran-AreaCells* belong. If the field is absent the UE not in SNPN access mode uses the ID of the registered PLMN. This field is not included for UE in SNPN access mode (for UE in SNPN access mode the *ran-AreaCells* always belongs to the registered SNPN). |
| ***ran-AreaCells***  The total number of cells of all PLMNs does not exceed 32. |

|  |
| --- |
| ***SDT-Config* field descriptions** |
| ***sdt-DRB-ContinueROHC***  Indicates whether the PDCP entity of the radio bearers configured for SDT continues or resets the ROHC header compression protocol during PDCP re-establishment during SDT procedure, as specified in TS 38.323 [5]. Value *cell* indicates that ROHC header compression continues when the UE resumes for SDT in the same cell as the PCell when the RRCRelease message was received. Value *rna* indicates that ROHC header compression continues when the UE resumes for SDT in a cell belonging to the same RNA as the PCell where the RRCRelease message was received. If the field is absent, the UE releases any stored value for this field and the PDCP entity of the radio bearers configured for SDT always resets the ROHC header compression protocol during PDCP re-establishment when SDT procedure is initiated, as specified in TS 38.323 [5]. |
| ***sdt-DRB-List***  Indicates the ID(s) of the DRB(s) that are configured for SDT. If size of the sequence is zero, then the UE assumes that none of the DRBs are configured for SDT. The network only configures MN terminated MCG bearers for SDT. |
| ***sdt-SRB2-Indication***  Indiates whether SRB2 is configured for SDT or not. |

|  |
| --- |
| ***SDT-MAC-PHY-CG-Config* field descriptions** |
| ***cg-SDT-ConfigInitialBWP-DL***  Downlink BWP configuration for CG-SDT. If a UE is a RedCap UE and if the *initialDownlinkBWP-RedCap* is configured in *downlinkConfigCommon* in *SIB1*, this field is configured for *initialDownlinkBWP-RedCap*, otherwise it is configured for *initialDownlinkBWP*. |
| ***cg-SDT-ConfigInitialBWP-NUL***  UL BWP configuration for CG-SDT on NUL carrier. If a UE is a RedCap UE and if the *initialUplinkBWP-RedCap* is configured in *uplinkConfigCommon* in *SIB1*, this field is configured for *initialUplinkBWP-RedCap*, otherwise it is configured for *initialUplinkBWP* for NUL. |
| ***cg-SDT-ConfigInitialBWP-SUL***  UL BWP configuration for CG-SDT on SUL carrier configured for the *initialUplinkBWP* for SUL. |
| ***cg-SDT-CS-RNTI***  The CS-RNTI value for CG-SDT as specified in TS 38.321 [3]. |
| ***cg-SDT-RSRP-ThresholdSSB***  An RSRP threshold configured for SSB selection for CG-SDT as specified in TS 38.321 [3]. |
| ***cg-SDT-TA-ValidationConfig***  Configuration for the RSRP based TA validation. If this field is not configured, then the UE does not perform RSRP based TA validation. |
| ***cg-SDT-timeAlignmentTimer***  TAT value for CG-SDT as specified in TS 38.321 [3]. The network always configures this field when *sdt-MAC-PHY-CG-Config* is configured. |

|  |
| --- |
| ***CG-SDT-ConfigLCH-Restriction* field descriptions** |
| ***allowedCG-List***  This restriction applies only when the UL grant is a configured grant for CG-SDT. If present, UL MAC SDUs from this logical channel can only be mapped to the indicated CG-SDT configured grant configuration. If the size of the sequence is zero, then UL MAC SDUs from this logical channel cannot be mapped to any CG-SDT configured grant configurations. If the field is not present, UL MAC SDUs from this logical channel can be mapped to any CG-SDT configured grant configurations. If the field *configuredGrantType1Allowed* is present, only those CG-SDT configured grant type 1 configurations indicated in this sequence are allowed for use by this logical channel; otherwise, this sequence shall not include any CG-SDT configured grant type 1 configuration. Corresponds to "*allowedCG*-*List*" as specified in TS 38.321 [3]. |
| ***configuredGrantType1Allowed***  If present, or if the capability *lcp-Restriction* as specified in TS 38.306 [26] is not supported, UL MAC SDUs from this logical channel can be transmitted on a configured grant type 1 for CG-SDT. Otherwise, UL MAC SDUs from this logical channel cannot be transmitted on a configured grant type 1 for CG-SDT. Corresponds to "*configuredGrantType1Allowed*" in TS 38.321 [3]. |
| ***logicalChannelIdentity***  ID used commonly for the MAC logical channel and for the RLC bearer associated with a *servedRadioBearer* configured for SDT. |

|  |
| --- |
| ***CG-SDT-TA-ValidationConfig* field descriptions** |
| ***cg-SDT-RSRP-ChangeThreshold***  The RSRP threshold for TA validation for CG-SDT as specified in TS 38.321 [3]. Value *dB2* corresponds to 2 dB, value *dB4* corresponds to 4 dB and so on. |

|  |
| --- |
| ***SRS-PosRRC-InactiveConfig* field descriptions** |
| ***bwp-NUL***  BWP configuration for SRS for Positioning during the RRC\_INACTIVE state in Normal Uplink Carrier. If the field is absent UE is configured with an SRS for Positioning associated with the initial UL BWP and transmitted, during the RRC\_INACTIVE state, inside the initial UL BWP with the same CP and SCS as configured for initial UL BWP. |
| ***bwp-SUL***  BWP configuration for SRS for Positioning during the RRC\_INACTIVE state in Supplementary Uplink Carrier. If the field is absent UE is configured with an SRS for Positioning associated with the initial UL BWP and transmitted, during the RRC\_INACTIVE state, inside the initial UL BWP with the same CP and SCS as configured for initial UL BWP. |
| ***inactivePosSRS-RSRP-ChangeThreshold***  RSRP threshold for the increase/decrease of RSRP for time alignment validation as specified in TS 38.321 [3]. |
| ***inactivePosSRS-TimeAlignmentTimer***  TAT value for SRS for positioning transmission during RRC\_INACTIVE state as specified in TS 38.321 [3]. The network always configures this field when *srs-PosRRC-Inactive* is configured. |
| ***srs-PosConfigNUL***  SRS for Positioning configuration in RRC\_INACTIVE state in Normal Uplink Carrier. |
| ***srs-PosConfigSUL***  SRS for Positioning configuration in RRC\_INACTIVE state in Supplementary Uplink Carrier. |

|  |
| --- |
| ***SuspendConfig* field descriptions** |
| ***ncd-SSB-RedCapInitialBWP-SDT***  Indicates that the UE uses the RedCap-specific initial DL BWP associated with the NCD-SSB for SDT. The network configures this field if a RedCap UE is configured with SDT in the RedCap-specific initial DL BWP not associated with CD-SSB. If configured, the NCD-SSB indicated by this field can only be used during the SDT procedure for CG-SDT or RA-SDT. |
| ***ran-ExtendedPagingCycle***  The extended DRX (eDRX) cycle for RAN-initiated paging to be applied by the UE. Value *rf256* corresponds to 256 radio frames, value *rf512* corresponds to 512 radio frames and so on. Value of the field indicates an eDRX cycle which is shorter or equal to the IDLE mode eDRX cycle configured for the UE. |
| ***ran-NotificationAreaInfo***  Network ensures that the UE in RRC\_INACTIVE always has a valid *ran-NotificationAreaInfo*. |
| ***ran-PagingCycle***  Refers to the UE specific cycle for RAN-initiated paging. Value *rf32* corresponds to 32 radio frames, value *rf64* corresponds to 64 radio frames and so on. |
| ***sl-UEIdentityRemote***  Indicates the C-RNTI to the L2 U2N Remote UE. |
| ***t380***  Refers to the timer that triggers the periodic RNAU procedure in UE. Value *min5* corresponds to 5 minutes, value *min10* corresponds to 10 minutes and so on. |

|  |
| --- |
| ***multicastConfigInactive* field descriptions** |
| ***inactivePTM-Config***  Indicates PTM configuration for MBS multicast reception in RRC\_INACTIVE in the serving cell. |
| ***inactiveMCCH-Config***  Indicates MCCH configuration for MBS multicast reception in RRC\_INACTIVE in the serving cell. Only *SIBx* is allowed to be included. |

|  |  |
| --- | --- |
| **Conditional Presence** | **Explanation** |
| *L2RemoteUE* | The field is mandatory present for L2 U2N Remote UE's RNAU; otherwise it is absent. |
| *RANPaging* | This field is optionally present, Need R, if the UE is configured with IDLE eDRX, see TS 24.501 [23]; otherwise the field is not present. |
| *Redirection2* | The field is optionally present, Need R, if *redirectedCarrierInfo* is included; otherwise the field is not present. |

Next Change

– *SIB1*

*SIB1* contains information relevant when evaluating if a UE is allowed to access a cell and defines the scheduling of other system information.It also contains radio resource configuration information that is common for all UEs and barring information applied to the unified access control.

Signalling radio bearer: N/A

RLC-SAP: TM

Logical channels: BCCH

Direction: Network to UE

***SIB1* message**

-- ASN1START

-- TAG-SIB1-START

SIB1 ::= SEQUENCE {

cellSelectionInfo SEQUENCE {

q-RxLevMin Q-RxLevMin,

q-RxLevMinOffset INTEGER (1..8) OPTIONAL, -- Need S

q-RxLevMinSUL Q-RxLevMin OPTIONAL, -- Need R

q-QualMin Q-QualMin OPTIONAL, -- Need S

q-QualMinOffset INTEGER (1..8) OPTIONAL -- Need S

} OPTIONAL, -- Cond Standalone

cellAccessRelatedInfo CellAccessRelatedInfo,

connEstFailureControl ConnEstFailureControl OPTIONAL, -- Need R

si-SchedulingInfo SI-SchedulingInfo OPTIONAL, -- Need R

servingCellConfigCommon ServingCellConfigCommonSIB OPTIONAL, -- Need R

ims-EmergencySupport ENUMERATED {true} OPTIONAL, -- Need R

eCallOverIMS-Support ENUMERATED {true} OPTIONAL, -- Need R

ue-TimersAndConstants UE-TimersAndConstants OPTIONAL, -- Need R

uac-BarringInfo SEQUENCE {

uac-BarringForCommon UAC-BarringPerCatList OPTIONAL, -- Need S

uac-BarringPerPLMN-List UAC-BarringPerPLMN-List OPTIONAL, -- Need S

uac-BarringInfoSetList UAC-BarringInfoSetList,

uac-AccessCategory1-SelectionAssistanceInfo CHOICE {

plmnCommon UAC-AccessCategory1-SelectionAssistanceInfo,

individualPLMNList SEQUENCE (SIZE (2..maxPLMN)) OF UAC-AccessCategory1-SelectionAssistanceInfo

} OPTIONAL -- Need S

} OPTIONAL, -- Need R

useFullResumeID ENUMERATED {true} OPTIONAL, -- Need R

lateNonCriticalExtension OCTET STRING OPTIONAL,

nonCriticalExtension SIB1-v1610-IEs OPTIONAL

}

SIB1-v1610-IEs ::= SEQUENCE {

idleModeMeasurementsEUTRA-r16 ENUMERATED{true} OPTIONAL, -- Need R

idleModeMeasurementsNR-r16 ENUMERATED{true} OPTIONAL, -- Need R

posSI-SchedulingInfo-r16 PosSI-SchedulingInfo-r16 OPTIONAL, -- Need R

nonCriticalExtension SIB1-v1630-IEs OPTIONAL

}

SIB1-v1630-IEs ::= SEQUENCE {

uac-BarringInfo-v1630 SEQUENCE {

uac-AC1-SelectAssistInfo-r16 SEQUENCE (SIZE (2..maxPLMN)) OF UAC-AC1-SelectAssistInfo-r16

} OPTIONAL, -- Need R

nonCriticalExtension SIB1-v1700-IEs OPTIONAL

}

SIB1-v1700-IEs ::= SEQUENCE {

hsdn-Cell-r17 ENUMERATED {true} OPTIONAL, -- Need R

uac-BarringInfo-v1700 SEQUENCE {

uac-BarringInfoSetList-v1700 UAC-BarringInfoSetList-v1700

} OPTIONAL, -- Cond MINT

sdt-ConfigCommon-r17 SDT-ConfigCommonSIB-r17 OPTIONAL, -- Need R

redCap-ConfigCommon-r17 RedCap-ConfigCommonSIB-r17 OPTIONAL, -- Need R

featurePriorities-r17 SEQUENCE {

redCapPriority-r17 FeaturePriority-r17 OPTIONAL, -- Need R

slicingPriority-r17 FeaturePriority-r17 OPTIONAL, -- Need R

msg3-Repetitions-Priority-r17 FeaturePriority-r17 OPTIONAL, -- Need R

sdt-Priority-r17 FeaturePriority-r17 OPTIONAL -- Need R

} OPTIONAL, -- Need R

si-SchedulingInfo-v1700 SI-SchedulingInfo-v1700 OPTIONAL, -- Need R

hyperSFN-r17 BIT STRING (SIZE (10)) OPTIONAL, -- Need R

eDRX-AllowedIdle-r17 ENUMERATED {true} OPTIONAL, -- Need R

eDRX-AllowedInactive-r17 ENUMERATED {true} OPTIONAL, -- Cond EDRX-RC

intraFreqReselectionRedCap-r17 ENUMERATED {allowed, notAllowed} OPTIONAL, -- Need S

cellBarredNTN-r17 ENUMERATED {barred, notBarred} OPTIONAL, -- Need S

nonCriticalExtension SIB1-v1740-IEs OPTIONAL

}

SIB1-v1740-IEs ::= SEQUENCE {

si-SchedulingInfo-v1740 SI-SchedulingInfo-v1740 OPTIONAL, -- Need R

nonCriticalExtension SIB1-v18xy-IEs OPTIONAL

}

SIB1-v18xy-IEs ::= SEQUENCE {

nonServingCellMII-r18 ENUMERATED {true} OPTIONAL, -- Need R

nonCriticalExtension SEQUENCE {} OPTIONAL

}

UAC-AccessCategory1-SelectionAssistanceInfo ::= ENUMERATED {a, b, c}

UAC-AC1-SelectAssistInfo-r16 ::= ENUMERATED {a, b, c, notConfigured}

SDT-ConfigCommonSIB-r17 ::= SEQUENCE {

sdt-RSRP-Threshold-r17 RSRP-Range OPTIONAL, -- Need R

sdt-LogicalChannelSR-DelayTimer-r17 ENUMERATED { sf20, sf40, sf64, sf128, sf512, sf1024, sf2560, spare1} OPTIONAL, -- Need R

sdt-DataVolumeThreshold-r17 ENUMERATED {byte32, byte100, byte200, byte400, byte600, byte800, byte1000, byte2000, byte4000,

byte8000, byte9000, byte10000, byte12000, byte24000, byte48000, byte96000},

t319a-r17 ENUMERATED { ms100, ms200, ms300, ms400, ms600, ms1000, ms2000,

ms3000, ms4000, spare7, spare6, spare5, spare4, spare3, spare2, spare1}

}

RedCap-ConfigCommonSIB-r17 ::= SEQUENCE {

halfDuplexRedCapAllowed-r17 ENUMERATED {true} OPTIONAL, -- Need R

cellBarredRedCap-r17 SEQUENCE {

cellBarredRedCap1Rx-r17 ENUMERATED {barred, notBarred},

cellBarredRedCap2Rx-r17 ENUMERATED {barred, notBarred}

} OPTIONAL, -- Need R

...

}

FeaturePriority-r17 ::= INTEGER (0..7)

-- TAG-SIB1-STOP

-- ASN1STOP

|  |
| --- |
| ***SIB1* field descriptions** |
| ***cellBarredNTN***  Value *barred* means that the cell is barred for connectivity to NTN, as defined in TS 38.304 [20]. Value *notBarred* means that the cell is allowed for connectivity to NTN. If not present, the UE considers the cell is not allowed for connectivity to NTN, as defined in TS 38.304 [20]. This field is only applicable to NTN-capable UEs. |
| ***cellBarredRedCap1Rx***  Value *barred* means that the cell is barred for a RedCap UE with 1 Rx branch, as defined in TS 38.304 [20]. This field is ignored by non-RedCap UEs. |
| ***cellBarredRedCap2Rx***  Value *barred* means that the cell is barred for a RedCap UE with 2 Rx branches, as defined in TS 38.304 [20]. This field is ignored by non-RedCap UEs. |
| ***cellSelectionInfo***  Parameters for cell selection related to the serving cell. |
| ***eCallOverIMS-Support***  Indicates whether the cell supports eCall over IMS services as defined in TS 23.501 [32]. If absent, eCall over IMS is not supported by the network in the cell. |
| ***eDRX-AllowedIdle***  The presence of this field indicates that extended DRX for CN paging is allowed in the cell for UEs in RRC\_IDLE or RRC\_INACTIVE. The UE shall stop using extended DRX for CN paging in RRC\_IDLE or RRC\_INACTIVE if *eDRX-AllowedIdle* is not present. |
| ***eDRX-AllowedInactive***  The presence of this field indicates that extended DRX for RAN paging is allowed in the cell for UEs in RRC\_INACTIVE. The UE shall stop using extended DRX for RAN paging in RRC\_INACTIVE if *eDRX-AllowedInactive* is not present. |
| ***featurePriorities***  Indicates priorities for features, such as RedCap, Slicing, SDT and MSG3-Repetitions for Coverage Enhancements. These priorities are used to determine which *FeatureCombinationPreambles* the UE shall use when a feature maps to more than one *FeatureCombinationPreambles*, as specified in TS 38.321 [3]. A lower value means a higher priority. The network does not signal the same priority for more than one feature. The network signals a priority for all feature that map to at least one *FeatureCombinationPreambles*. |
| ***halfDuplexRedCap-Allowed***  The presence of this field indicates that the cell supports half-duplex FDD RedCap UEs. |
| ***hsdn-Cell***  This field indicates this is a HSDN cell as specified in TS 38.304 [20]. |
| ***hyperSFN***  Indicates hyper SFN which increments by one when the SFN wraps around. This field is excluded when determining changes in system information, i.e. changes of hyper SFN should not result in system information change notifications. |
| ***idleModeMeasurementsEUTRA***  This field indicates that a UE that is configured for EUTRA idle/inactive measurements shall perform the measurements while camping in this cell and report availability of these measurements when establishing or resuming a connection in this cell. If absent, a UE is not required to perform EUTRA idle/inactive measurements. |
| ***idleModeMeasurementsNR***  This field indicates that a UE that is configured for NR idle/inactive measurements shall perform the measurements while camping in this cell and report availability of these measurements when establishing or resuming a connection in this cell. If absent, a UE is not required to perform NR idle/inactive measurements. |
| ***ims-EmergencySupport***  Indicates whether the cell supports IMS emergency bearer services for UEs in limited service mode. If absent, IMS emergency call is not supported by the network in the cell for UEs in limited service mode. |
| ***intraFreqReselectionRedCap***  Controls cell selection/reselection to intra-frequency cells for RedCap UEs when this cell is barred, or treated as barred by the RedCap UE, as specified in TS 38.304 [20]. If not present, a RedCap UE treats the cell as barred, i.e.,the UE considers that the cell does not support RedCap. |
| ***nonServingCellMII***  Indicates whether the *MBSInterestIndication* message for MBS broadcast reception on a non-serving cell is allowed to be transmitted to the serving gNB. | |
| ***q-QualMin***  Parameter "Qqualmin" in TS 38.304 [20], applicable for serving cell. If the field is absent, the UE applies the (default) value of negative infinity for Qqualmin. |
| ***q-QualMinOffset***  Parameter "Qqualminoffset" in TS 38.304 [20]. Actual value Qqualminoffset = field value [dB]. If the field is absent, the UE applies the (default) value of 0 dB for Qqualminoffset.Affects the minimum required quality level in the cell. |
| ***q-RxLevMin***  Parameter "Qrxlevmin" in TS 38.304 [20], applicable for serving cell. |
| ***q-RxLevMinOffset***  Parameter "Qrxlevminoffset" in TS 38.304 [20]. Actual value Qrxlevminoffset = field value \* 2 [dB]. If absent, the UE applies the (default) value of 0 dB for Qrxlevminoffset*.* Affects the minimum required Rx level in the cell. |
| ***q-RxLevMinSUL***  Parameter "Qrxlevmin" in TS 38.304 [20], applicable for serving cell. |
| ***sdt-RSRP-Threshold***  RSRP threshold used to determine whether SDT procedure can be initiated, as specified in TS 38.321 [3]. |
| ***sdt-DataVolumeThreshold***  Data volume threshold used to determine whether SDT can be initiated, as specified in TS 38.321 [3]. Value *byte32* corresponds to 32 bytes, value *byte100* corresponds to 100 bytes, and so on. |
| ***sdt-LogicalChannelSR-DelayTimer***  The value of *logicalChannelSR-DelayTimer* applied during SDT for logical channels configured with SDT, as specified in TS 38.321 [3]. Value in number of subframes. Value *sf20* corresponds to 20 subframes, *sf40* corresponds to 40 subframes, and so on. If this field is not configured, then logicalChannelSR-DelayTimer is not applied for SDT logical channels. |
| ***servingCellConfigCommon***  Configuration of the serving cell. |
| ***t319a***  Initial value of the timer T319a used for detection of SDT failure. Value *ms100* corresponds to 100 milliseconds, value *ms200* corresponds to 200 milliseconds and so on. |
| ***uac-AccessCategory1-SelectionAssistanceInfo***  Information used to determine whether Access Category 1 applies to the UE, as defined in TS 22.261 [25]. If *plmnCommon* is chosen, the *UAC-AccessCategory1-SelectionAssistanceInfo* is applicable to all the PLMNs and SNPNs in *plmn-IdentityInfoList* and *npn-IdentityInfoList*. If *individualPLMNList* is chosen, the 1st entry in the list corresponds to the first network within all of the PLMNs and SNPNs across the *plmn-IdentityList* and the *npn-IdentityInfoList*, the 2nd entry in the list corresponds to the second network within all of the PLMNs and SNPNs across the *plmn-IdentityList* and the *npn-IdentityInfoList* and so on. If *uac-AC1-SelectAssistInfo-r16* is present, the UE shall ignore the *uac-AccessCategory1-SelectionAssistanceInfo*. |
| ***uac-AC1-SelectAssistInfo***  Information used to determine whether Access Category 1 applies to the UE, as defined in TS 22.261 [25]. The 1st entry in the list corresponds to the first network within all of the PLMNs and SNPNs across the *plmn-IdentityList* and *npn-IdentityInfoList*, the 2nd entry in the list corresponds to the second network within all of the PLMNs and SNPNs across the *plmn-IdentityList* and the *npn-IdentityInfoList* and so on. Value *notConfigured* indicates that Access Category1 is not configured for the corresponding PLMN/SNPN. |
| ***uac-BarringForCommon***  Common access control parameters for each access category. Common values are used for all PLMNs/SNPNs, unless overwritten by the PLMN/SNPN specific configuration provided in *uac-BarringPerPLMN-List*. The parameters are specified by providing an index to the set of configurations (*uac-BarringInfoSetList*). UE behaviour upon absence of this field is specified in clause 5.3.14.2. |
| ***ue-TimersAndConstants***  Timer and constant values to be used by the UE. The cell operating as PCell always provides this field. |
| ***useFullResumeID***  Indicates which resume identifier and Resume request message should be used. UE uses *fullI-RNTI* and *RRCResumeRequest1* if the field is present, or *shortI-RNTI* and *RRCResumeRequest* if the field is absent. |

|  |  |
| --- | --- |
| **Conditional Presence** | **Explanation** |
| *EDRX-RC* | The field is optionally present, Need R, in a cell that enables *eDRX-AllowedIdle*, otherwise it is absent. |
| *MINT* | The field is optionally present, Need R, in a cell that provides a configuration for disaster roaming, otherwise it is absent, Need R. |
| *Standalone* | The field is mandatory present in a cell that supports standalone operation, otherwise it is absent. |

Next Change (new)

– *SystemInformation*

The *SystemInformation* message is used to convey one or more System Information Blocks or Positioning System Information Blocks. All the SIBs or posSIBs included are transmitted with the same periodicity.

Signalling radio bearer: N/A

RLC-SAP: TM

Logical channels: BCCH

Direction: Network to UE

***SystemInformation message***

-- ASN1START

-- TAG-SYSTEMINFORMATION-START

SystemInformation ::= SEQUENCE {

criticalExtensions CHOICE {

systemInformation SystemInformation-IEs,

criticalExtensionsFuture-r16 CHOICE {

posSystemInformation-r16 PosSystemInformation-r16-IEs,

criticalExtensionsFuture SEQUENCE {}

}

}

}

SystemInformation-IEs ::= SEQUENCE {

sib-TypeAndInfo SEQUENCE (SIZE (1..maxSIB)) OF CHOICE {

sib2 SIB2,

sib3 SIB3,

sib4 SIB4,

sib5 SIB5,

sib6 SIB6,

sib7 SIB7,

sib8 SIB8,

sib9 SIB9,

...,

sib10-v1610 SIB10-r16,

sib11-v1610 SIB11-r16,

sib12-v1610 SIB12-r16,

sib13-v1610 SIB13-r16,

sib14-v1610 SIB14-r16,

sib15-v1700 SIB15-r17,

sib16-v1700 SIB16-r17,

sib17-v1700 SIB17-r17,

sib18-v1700 SIB18-r17,

sib19-v1700 SIB19-r17,

sib20-v1700 SIB20-r17,

sib21-v1700 SIB21-r17,

sibx-v1800 SIBx-r18

},

lateNonCriticalExtension OCTET STRING OPTIONAL,

nonCriticalExtension SEQUENCE {} OPTIONAL

}

-- TAG-SYSTEMINFORMATION-STOP

-- ASN1STOP

Next Change (new)

### 6.3.1 System information blocks

– *SIBx*

*SIBx* contains the information required to acquire the multicast MCCH/MTCH configuration for MBS multicast reception in RRC\_INACTIVE.

***SIBx* information element**

-- ASN1START

-- TAG-SIBx-START

SIBx-r18 ::= SEQUENCE {

multicastMCCH-Config-r18 MCCH-Config-r17,

cfr-ConfigMCCH-MTCH-r18 CFR-ConfigMCCH-MTCH-r17 OPTIONAL, -- Need S

lateNonCriticalExtension OCTET STRING OPTIONAL,

...

}

-- TAG-SIBx-STOP

-- ASN1STOP

| ***SIBx* field descriptions** |
| --- |
| ***cfr-ConfigMCCH-MTCH***  Common frequency resource used for multicast MCCH and multicast MTCH reception. If the field is absent, the CFR for multicast has the same location and size as CORESET#0 and PDSCH configuration of MCCH is the same as PDSCH configuration provided in *initialDownlinkBWP* in *SIB1*. |
| ***multicastMCCH-Config***  Indicates MCCH configuration for MBS multicast reception in RRC\_INACTIVE. |

Next Change

### 6.3.2 Radio resource control information elements

– *PDCCH-ConfigCommon*

The IE *PDCCH-ConfigCommon* is used to configure cell specific PDCCH parameters provided in SIB as well as in dedicated signalling.

***PDCCH-ConfigCommon* information element**

-- ASN1START

-- TAG-PDCCH-CONFIGCOMMON-START

PDCCH-ConfigCommon ::= SEQUENCE {

controlResourceSetZero ControlResourceSetZero OPTIONAL, -- Cond InitialBWP-Only

commonControlResourceSet ControlResourceSet OPTIONAL, -- Need R

searchSpaceZero SearchSpaceZero OPTIONAL, -- Cond InitialBWP-Only

commonSearchSpaceList SEQUENCE (SIZE(1..4)) OF SearchSpace OPTIONAL, -- Need R

searchSpaceSIB1 SearchSpaceId OPTIONAL, -- Need S

searchSpaceOtherSystemInformation SearchSpaceId OPTIONAL, -- Need S

pagingSearchSpace SearchSpaceId OPTIONAL, -- Need S

ra-SearchSpace SearchSpaceId OPTIONAL, -- Need S

...,

[[

firstPDCCH-MonitoringOccasionOfPO CHOICE {

sCS15KHZoneT SEQUENCE (SIZE (1..maxPO-perPF)) OF INTEGER (0..139),

sCS30KHZoneT-SCS15KHZhalfT SEQUENCE (SIZE (1..maxPO-perPF)) OF INTEGER (0..279),

sCS60KHZoneT-SCS30KHZhalfT-SCS15KHZquarterT SEQUENCE (SIZE (1..maxPO-perPF)) OF INTEGER (0..559),

sCS120KHZoneT-SCS60KHZhalfT-SCS30KHZquarterT-SCS15KHZoneEighthT SEQUENCE (SIZE (1..maxPO-perPF)) OF INTEGER (0..1119),

sCS120KHZhalfT-SCS60KHZquarterT-SCS30KHZoneEighthT-SCS15KHZoneSixteenthT SEQUENCE (SIZE (1..maxPO-perPF)) OF INTEGER (0..2239),

sCS120KHZquarterT-SCS60KHZoneEighthT-SCS30KHZoneSixteenthT SEQUENCE (SIZE (1..maxPO-perPF)) OF INTEGER (0..4479),

sCS120KHZoneEighthT-SCS60KHZoneSixteenthT SEQUENCE (SIZE (1..maxPO-perPF)) OF INTEGER (0..8959),

sCS120KHZoneSixteenthT SEQUENCE (SIZE (1..maxPO-perPF)) OF INTEGER (0..17919)

} OPTIONAL -- Cond OtherBWP

]],

[[

commonSearchSpaceListExt-r16 SEQUENCE (SIZE(1..4)) OF SearchSpaceExt-r16 OPTIONAL -- Need R

]],

[[

sdt-SearchSpace-r17 CHOICE {

newSearchSpace SearchSpace,

existingSearchSpace SearchSpaceId

} OPTIONAL, -- Need R

searchSpaceMCCH-r17 SearchSpaceId OPTIONAL, -- Need R

searchSpaceMTCH-r17 SearchSpaceId OPTIONAL, -- Need S

commonSearchSpaceListExt2-r17 SEQUENCE (SIZE(1..4)) OF SearchSpaceExt-v1700 OPTIONAL, -- Need R

firstPDCCH-MonitoringOccasionOfPO-v1710 CHOICE {

sCS480KHZoneEighthT SEQUENCE (SIZE (1..maxPO-perPF)) OF INTEGER (0..35839),

sCS480KHZoneSixteenthT SEQUENCE (SIZE (1..maxPO-perPF)) OF INTEGER (0..71679)

} OPTIONAL, -- Need R

pei-ConfigBWP-r17 SEQUENCE {

pei-SearchSpace-r17 SearchSpaceId,

firstPDCCH-MonitoringOccasionOfPEI-O-r17 CHOICE {

sCS15KHZoneT SEQUENCE (SIZE (1..maxPEI-perPF-r17)) OF INTEGER (0..139),

sCS30KHZoneT-SCS15KHZhalfT SEQUENCE (SIZE (1..maxPEI-perPF-r17)) OF INTEGER (0..279),

sCS60KHZoneT-SCS30KHZhalfT-SCS15KHZquarterT SEQUENCE (SIZE (1..maxPEI-perPF-r17)) OF INTEGER (0..559),

sCS120KHZoneT-SCS60KHZhalfT-SCS30KHZquarterT-SCS15KHZoneEighthT SEQUENCE (SIZE (1..maxPEI-perPF-r17)) OF INTEGER (0..1119),

sCS120KHZhalfT-SCS60KHZquarterT-SCS30KHZoneEighthT-SCS15KHZoneSixteenthT SEQUENCE (SIZE (1..maxPEI-perPF-r17)) OF INTEGER (0..2239),

sCS480KHZoneT-SCS120KHZquarterT-SCS60KHZoneEighthT-SCS30KHZoneSixteenthT SEQUENCE (SIZE (1..maxPEI-perPF-r17)) OF INTEGER (0..4479),

sCS480KHZhalfT-SCS120KHZoneEighthT-SCS60KHZoneSixteenthT SEQUENCE (SIZE (1..maxPEI-perPF-r17)) OF INTEGER (0..8959),

sCS480KHZquarterT-SCS120KHZoneSixteenthT SEQUENCE (SIZE (1..maxPEI-perPF-r17)) OF INTEGER (0..17919),

sCS480KHZoneEighthT SEQUENCE (SIZE (1..maxPEI-perPF-r17)) OF INTEGER (0..35839),

sCS480KHZoneSixteenthT SEQUENCE (SIZE (1..maxPEI-perPF-r17)) OF INTEGER (0..71679)

}

} OPTIONAL -- Cond InitialBWP-Paging

]],

[[

followUnifiedTCI-State-v1720 ENUMERATED {enabled} OPTIONAL -- Need R

]],

[[

searchSpaceMulticastMCCH-r18 SearchSpaceId OPTIONAL, -- Need R

searchSpaceMulticastMTCH-r18 SearchSpaceId OPTIONAL -- Need S

]]

}

-- TAG-PDCCH-CONFIGCOMMON-STOP

-- ASN1STOP

|  |
| --- |
| ***PDCCH-ConfigCommon* field descriptions** |
| ***commonControlResourceSet***  An additional common control resource set which may be configured and used for any common or UE-specific search space. If the network configures this field, it uses a *ControlResourceSetId* other than 0 for this *ControlResourceSet*. The network configures the *commonControlResourceSet* in *SIB1* so that it is contained in the bandwidth of CORESET#0. If the RedCap-specific initial downlink BWP does not contain the entire CORESET#0, the network configures the *commonControlResourceSet* in the RedCap-specific initial downlink BWP in *SIB1* for RedCap such that it does not have to be contained in the bandwidth of CORESET#0. |
| ***commonSearchSpaceList, commonSearchSpaceListExt,*** ***commonSearchSpaceListExt2***  A list of additional common search spaces. If the network configures this field, it uses the *SearchSpaceId*s other than 0. If the field is included, it replaces any previous list, i.e. all the entries of the list are replaced and each of the *SearchSpace* entries is considered to be newly created and the conditions and Need codes for setup of the entry apply. If the network includes *commonSearchSpaceListExt/commonSearchSpaceListExt2*, it includes the same number of entries, and listed in the same order, as in *commonSearchSpaceList*. |
| ***controlResourceSetZero***  Parameters of the common CORESET#0 which can be used in any common or UE-specific search spaces. The values are interpreted like the corresponding bits in *MIB* *pdcch-ConfigSIB1*. Even though this field is only configured in the initial BWP (BWP#0) *controlResourceSetZero* can be used in search spaces configured in other DL BWP(s) than the initial DL BWP if the conditions defined in TS 38.213 [13], clause 10 are satisfied. |
| ***firstPDCCH-MonitoringOccasionOfPEI-O***  Offset, in number of symbols, from the start of the reference frame for PEI-O to the start of the first PDCCH monitoring occasion of PEI-O on this BWP, see TS 38.213 [13], clause 10.4A. For the case *po-NumPerPEI* is smaller than Ns, UE applies the (floor(i\_s/po-NumPerPEI)+1)-th value out of (N\_s/po-NumPerPEI) configured values in *firstPDCCH-MonitoringOccasionOfPEI-O* for the symbol-level offset. When *po-NumPerPEI* is one or multiple of Ns, UE applies the first configured value in *firstPDCCH-MonitoringOccasionOfPEI-O* for the symbol-level offset. |
| ***firstPDCCH-MonitoringOccasionOfPO***  Indicates the first PDCCH monitoring occasion of each PO of the PF on this BWP, see TS 38.304 [20]. The field *sCS120KHZquarterT-SCS60KHZoneEighthT-SCS30KHZoneSixteenthT*, *sCS120KHZoneEighthT-SCS60KHZoneSixteenthT* and *sCS120KHZoneSixteenthT* can be applied for SCS 480kHz, corresponding to *sCS480KHZoneT-SCS120KHZquarterT-SCS60KHZoneEighthT-SCS30KHZoneSixteenthT*, *sCS480KHZhalfT-SCS120KHZoneEighthT-SCS60KHZoneSixteenthT* and *sCS480KHZquarterT-SCS120KHZoneSixteenthT* in IE *DownlinkConfigCommonSIB* respectively. |
| ***followUnifiedTCI-State***  When set to enabled, for PDCCH reception in CORESET #0, the UE applies the "indicated" DL only TCI or joint TCI as specified in TS 38.214 [19], clause 5.1.5. |
| ***pagingSearchSpace***  ID of the search space for paging (see TS 38.213 [13], clause 10.1). If the field is absent, the UE does not receive paging in this BWP (see TS 38.213 [13], clause 10). This field is absent for the RedCap-specific initial downlink BWP, if it does not include CD-SSB and the entire CORESET#0. In that case, a RedCap UE in RRC\_IDLE or RRC\_INACTIVE while SDT procedure is not ongoing, shall monitor paging in the initial DL BWP that includes CORESET#0. |
| ***pei-ConfigBWP***  Provides the configuration for PEI reception in this BWP. If the field is absent, the UE does not receive PEI in this BWP. |
| ***pei-SearchSpace***  ID of dedicated search space for PEI. It can be configured to one of up to 4 common SS sets configured by *commonSearchSpaceList* with *SearchSpaceId* > 0. The CCE aggregation levels and maximum number of PDCCH candidates per CCE aggregation level follows Table 10.1-1 of TS38.213 [13]. *SearchSpaceId* = 0 can be configured for the case of SS/PBCH block and CORESET multiplexing pattern 2 or 3. |
| ***ra-SearchSpace***  ID of the Search space for random access procedure (see TS 38.213 [13], clause 10.1). If the field is absent, the UE does not receive RAR in this BWP. This field is mandatory present in the DL BWP(s) if the conditions described in TS 38.321 [3], clause 5.15 are met. |
| ***sdt-SearchSpace***  Common search space for CG-SDT and RA-SDT (see TS 38.213 [13]). If an *existingSearchSpace* is used, the network only signals the search space ID of the *ra-SearchSpace*. |
| ***searchSpaceMCCH***  ID of the search space for MCCH. If the field is absent, the UE does not receive MCCH in this BWP (see TS 38.213 [13], clause 10). This field is absent for the RedCap-specific initial downlink BWP, if it does not include CD-SSB and the entire CORESET#0. |
| ***searchSpaceMTCH***  ID of the search space for MTCH of MBS broadcast. If the field is absent, the UE applies *searchSpaceMCCH* also for MTCH, (see TS 38.213 [13], clause 10). This field is absent for the RedCap-specific initial downlink BWP, if it does not include CD-SSB and the entire CORESET#0. |
| ***searchSpaceMulticastMCCH***  ID of the search space for multicast MCCH. If the field is absent, the UE does not receive multicast MCCH in this BWP (see TS 38.213 [13], clause 10). This field is absent for the RedCap-specific initial downlink BWP, if it does not include CD-SSB and the entire CORESET#0. |
| ***searchSpaceMulticastMTCH***  ID of the search space for multicast MTCH. If the field is absent, the UE applies *searchSpaceMulticastMCCH* also for multicast MTCH, (see TS 38.213 [13], clause 10). This field is absent for the RedCap-specific initial downlink BWP, if it does not include CD-SSB and the entire CORESET#0. |
| ***searchSpaceOtherSystemInformation***  ID of the Search space for other system information, i.e., *SIB2* and beyond (see TS 38.213 [13], clause 10.1). If the field is absent, the UE does not receive other system information in this BWP. This field is absent for the RedCap-specific initial DL BWP, if it does not include CD-SSB and the entire CORESET#0. In that case, a RedCap UE in RRC\_IDLE or RRC\_INACTIVE shall monitor PDCCH to receive other system information using *searchSpaceOtherSystemInformation* in the initial DL BWP that includes CD-SSB and the entire CORESET#0. |
| ***searchSpaceSIB1***  ID of the search space for *SIB1* message. In the initial DL BWP of the UE′s PCell, the network sets this field to 0. If the field is absent, the UE does not receive *SIB1* in this BWP. (see TS 38.213 [13], clause 10). This field is absent for the RedCap-specific initial DL BWP, if it does not include CD-SSB and the entire CORESET#0. In that case, a RedCap UE in RRC\_IDLE or RRC\_INACTIVE shall monitor PDCCH to receive SIB1 using *searchSpaceSIB1* in the initial DL BWP that includes CD-SSB and the entire CORESET#0. |
| ***searchSpaceZero***  Parameters of the common SearchSpace#0. The values are interpreted like the corresponding bits in *MIB* *pdcch-ConfigSIB1*. Even though this field is only configured in the initial BWP (BWP#0), *searchSpaceZero* can be used in search spaces configured in other DL BWP(s) than the initial DL BWP if the conditions described in TS 38.213 [13], clause 10, are satisfied. |

|  |  |
| --- | --- |
| **Conditional Presence** | **Explanation** |
| *InitialBWP-Only* | If *SIB1* is broadcast the field is mandatory present in the *PDCCH-ConfigCommon* of the initial BWP (BWP#0) in *ServingCellConfigCommon* except it is the RedCap-specific initial BWP not including CD-SSB and the entire CORESET#0; it is absent in other BWPs and when sent in system information. If SIB1 is not broadcast and there is an SSB associated to the cell, the field is optionally present, Need M, in the *PDCCH-ConfigCommon* of the initial BWP (BWP#0) in *ServingCellConfigCommon* (still with the same setting for all UEs). In other cases, the field is absent. |
| *OtherBWP* | This field is optionally present, Need R, if this BWP is not the *initialDownlinkBWP* and *pagingSearchSpace* is configured in this BWP. Otherwise this field is absent. |
| *InitialBWP-Paging* | This field is optionally present, Need R, if this BWP is the *initialDownlinkBWP* or *initialDownlinkBWP-RedCap* including CD-SSB and the entire CORESET#0, and *pei-Config* is configured in *DownlinkConfigCommonSIB*. Otherwise, this field is absent. |

– *SI-SchedulingInfo*

The IE *SI-SchedulingInfo* contains information needed for acquisition of SI messages.

***SI-SchedulingInfo* information element**

-- ASN1START

-- TAG-SI-SCHEDULINGINFO-START

SI-SchedulingInfo ::= SEQUENCE {

schedulingInfoList SEQUENCE (SIZE (1..maxSI-Message)) OF SchedulingInfo,

si-WindowLength ENUMERATED {s5, s10, s20, s40, s80, s160, s320, s640, s1280, s2560-v1710, s5120-v1710 },

si-RequestConfig SI-RequestConfig OPTIONAL, -- Cond MSG-1

si-RequestConfigSUL SI-RequestConfig OPTIONAL, -- Cond SUL-MSG-1

systemInformationAreaID BIT STRING (SIZE (24)) OPTIONAL, -- Need R

...

}

SchedulingInfo ::= SEQUENCE {

si-BroadcastStatus ENUMERATED {broadcasting, notBroadcasting},

si-Periodicity ENUMERATED {rf8, rf16, rf32, rf64, rf128, rf256, rf512},

sib-MappingInfo SIB-Mapping

}

SI-SchedulingInfo-v1700 ::= SEQUENCE {

schedulingInfoList2-r17 SEQUENCE (SIZE (1..maxSI-Message)) OF SchedulingInfo2-r17,

dummy SI-RequestConfig OPTIONAL

}

SI-SchedulingInfo-v1740 ::= SEQUENCE {

si-RequestConfigRedCap-r17 SI-RequestConfig OPTIONAL -- Cond REDCAP-MSG-1

}

SchedulingInfo2-r17 ::= SEQUENCE {

si-BroadcastStatus-r17 ENUMERATED {broadcasting, notBroadcasting},

si-WindowPosition-r17 INTEGER (1..256),

si-Periodicity-r17 ENUMERATED {rf8, rf16, rf32, rf64, rf128, rf256, rf512},

sib-MappingInfo-r17 SIB-Mapping-v1700

}

SIB-Mapping ::= SEQUENCE (SIZE (1..maxSIB)) OF SIB-TypeInfo

SIB-Mapping-v1700 ::= SEQUENCE (SIZE (1..maxSIB)) OF SIB-TypeInfo-v1700

SIB-TypeInfo ::= SEQUENCE {

type ENUMERATED {sibType2, sibType3, sibType4, sibType5, sibType6, sibType7, sibType8, sibType9,

sibType10-v1610, sibType11-v1610, sibType12-v1610, sibType13-v1610,

sibType14-v1610, spare3, spare2, spare1,... },

valueTag INTEGER (0..31) OPTIONAL, -- Cond SIB-TYPE

areaScope ENUMERATED {true} OPTIONAL -- Need S

}

SIB-TypeInfo-v1700 ::= SEQUENCE {

sibType-r17 CHOICE {

type1-r17 ENUMERATED {sibType15, sibType16, sibType17, sibType18, sibType19, sibType20, sibType21,

sibTypeX, spare8, spare7, spare6, spare5, spare4, spare3, spare2, spare1,...},

type2-r17 SEQUENCE {

posSibType-r17 ENUMERATED {posSibType1-9, posSibType1-10, posSibType2-24, posSibType2-25,

posSibType6-4, posSibType6-5, posSibType6-6, spare9, spare8, spare7, spare6,

spare5, spare4, spare3, spare2, spare1,...},

encrypted-r17 ENUMERATED { true } OPTIONAL, -- Need R

gnss-id-r17 GNSS-ID-r16 OPTIONAL, -- Need R

sbas-id-r17 SBAS-ID-r16 OPTIONAL -- Need R

}

},

valueTag-r17 INTEGER (0..31) OPTIONAL, -- Cond NonPosSIB

areaScope-r17 ENUMERATED {true} OPTIONAL -- Need S

}

-- TAG-SI-SCHEDULINGINFO-STOP

-- ASN1STOP

|  |
| --- |
| ***SchedulingInfo* field descriptions** |
| ***areaScope***  Indicates that a SIB is area specific. If the field is absent, the SIB is cell specific. |
| ***si-BroadcastStatus***  Indicates if the SI message is being broadcasted or not. Change of *si-BroadcastStat*us should not result in system information change notifications in Short Message transmitted with P-RNTI over DCI (see clause 6.5). The value of the indication is valid until the end of the BCCH modification period when set to *broadcasting.* When *SIB19* is scheduled, the *si-BroadcastStatus* for the mapped *SIB19* is set to *broadcasting*.  If *si-SchedulingInfo-v1700* is present, the network ensures that the total number of SI messages with *si-BroadcastStatus* set to *notBroadcasting* in the list of concatenated SI messages configured by *schedulingInfoList* in *si-SchedulingInfo* and SI messages containing type1 SIB configured by *schedulingInfoList2* in *si-SchedulingInfo-v1700* does not exceed the limit of *maxSI-Message* when *si-RequestConfig*, *si-RequestConfigRedCap* or *si-RequestConfigSUL* is configured. |
| ***si-Periodicity***  Periodicity of the SI-message in radio frames. Value *rf8* corresponds to 8 radio frames, value *rf16* corresponds to 16 radio frames, and so on. |

|  |
| --- |
| ***SI-SchedulingInfo* field descriptions** |
| ***dummy***  This field is not used in this specification. If received, it is ignored by the UE. |
| ***si-RequestConfig***  Configuration of Msg1 resources that the UE uses for requesting SI-messages for which *si-BroadcastStatus* is set to *notBroadcasting*. |
| ***si-RequestConfigRedCap***  Configuration of Msg1 resources for *initialUplinkBWP-RedCap*that the RedCap UE uses for requesting SI-messages for which *si-BroadcastStatus* is set to *notBroadcasting*. |
| ***si-RequestConfigSUL***  Configuration of Msg1 resources that the UE uses for requesting SI-messages for which *si-BroadcastStatus* is set to *notBroadcasting*. |
| ***si-WindowLength***  The length of the SI scheduling window. Value *s5* corresponds to 5 slots, value *s10* corresponds to 10 slots and so on. The network always configures *si-WindowLength* to be shorter than or equal to the *si-Periodicity*. The values *s2560-v1710* and *s5120-v1710* are only applicable for SCS 480 kHz. |
| ***systemInformationAreaID***  Indicates the system information area that the cell belongs to, if any. Any SIB with *areaScope* within the SI is considered to belong to this *systemInformationAreaID*. The systemInformationAreaID is unique within a PLMN/SNPN. |

|  |
| --- |
| ***SchedulingInfo2* field descriptions** |
| ***encrypted***  The presence of this field indicates that the pos-sib-type is encrypted as specified in TS 37.355 [49]. |
| ***gnss-id***  The presence of this field indicates that the positioning SIB type is for a specific GNSS. Indicates a specific GNSS (see also TS 37.355 [49]) |
| ***posSibType***  The posSIBs as defined in TS 37.355 [49] mapped to SI for scheduling using*schedulingInfoList2*. |
| ***sbas-id***  The presence of this field indicates that the positioning SIB type is for a specific SBAS. Indicates a specific SBAS (see also TS 37.355 [49]). |
| ***si-WindowPosition***  This field indicates the SI window position of the associated SI-message. The network provides *si-WindowPosition* in an ascending order, i.e. *si-WindowPosition* in the subsequent entry in *schedulingInfoList2* has always value higher than in the previous entry of *schedulingInfoList2*. The network configures this field in a way that ensures that SI messages scheduled by *schedulingInfoList* and/or *posSchedulingInfoList* do not overlap with SI messages scheduled by *schedulingInfoList2*. |
| ***sib-MappingInfo***  Indicates which SIBs or posSIBs are contained in the SI message. |
| ***sibType***  The type of SIB(s) mapped to SI for scheduling using*schedulingInfoList2*. Value *type1* indicates SIBs and value *type2* indicates posSIBs. |

| **Conditional presence** | **Explanation** |
| --- | --- |
| *MSG-1* | The field is optionally present, Need R, if *si-BroadcastStatus* is set to *notBroadcasting* for any SI-message included in *schedulingInfoList* oranySI-message containing type1 SIB included in *schedulingInfoList2*. It is absent otherwise. |
| *SIB-TYPE* | The field is mandatory present if the SIB type is different from *SIB6*, *SIB7* or *SIB8*. For *SIB6*, *SIB7* and *SIB8* it is absent. |
| *NonPosSIB* | The field is mandatory present if the SIB type is *type1*. For *type2* it is absent. |
| *SUL-MSG-1* | The field is optionally present, Need R, if *supplementaryUplink* is configured in *ServingCellConfigCommonSIB* and if *si-BroadcastStatus* is set to *notBroadcasting* for any SI-message included in *schedulingInfoList* oranySI-message containing type1 SIB included in *schedulingInfoList2*. It is absent otherwise. |
| *REDCAP-MSG-1* | The field is optionally present, Need R, if *initialUplinkBWP-RedCap* is configured in *UplinkConfigCommonSIB* and if *si-BroadcastStatus* is set to *notBroadcasting* for any SI-message included in *schedulingInfoList* oranySI-message containing type1 SIB included in *schedulingInfoList2*. It is absent otherwise. |

*Next Change*

### 6.3.6 MBS information elements

– *MBS-NonServingInfoList*

The IE *MBS-NonServingInfoList* is used to inform network of the frequencies, CFR information and subcarrier spacing for MBS broadcast reception on the non-serving cell.

***MBS-NonServingInfoList* information element**

-- ASN1START

-- TAG-MBSNONSERVINGINFOLIST-START

MBS-NonServingInfoList-r18 ::= SEQUENCE (SIZE (1..maxFreqMBS-r17)) OF NonServingInfo-r18

NonServingInfo-r18 ::= SEQUENCE {

freqInfoMBS-r18 FreqInfoMBS-r18 OPTIONAL,

cfr-InfoMBS-r18 CHOICE {

cfr-Bandwidth-r18 INTEGER (1..maxNrofPhysicalResourceBlocks),

cfr-LocationAndBW-r18 CFR-LocationAndBW-r18

} OPTIONAL,

subcarrierSpacing-r18 SubcarrierSpacing OPTIONAL

}

FreqInfoMBS-r18 ::= SEQUENCE {

carrierFreqMBS-r18 ARFCN-ValueNR,

freqBandIndicatorMBS-r18 FreqBandIndicatorNR

}

CFR-LocationAndBW-r18 ::= SEQUENCE {

locationAndBandwidthMBS-r18 INTEGER (0..37949) OPTIONAL,

absoluteFrequencyPointA-MBS-r18 ARFCN-ValueNR OPTIONAL,

offsetToCarrierMBS-r18 INTEGER (0..2199) OPTIONAL

}

-- TAG-MBSNONSERVINGINFOLIST-STOP

-- ASN1STOP

| ***MBS-NonServingInfoList* field descriptions** |
| --- |
| ***freqInfoMBS***  Indicates MBS frequency of interest and the frequency band of the non-serving cell for MBS broadcast reception acquired from the *SIB21* or the USD as specified in clause 5.9.4.3. |
| ***cfr-infoMBS***  Indicates the CFR information of the non-serving cell for MBS broadcast reception. |
| ***cfr-BandwidthMBS***  Indicates the CFR bandwidth of the non-serving cell for MBS broadcast reception. |
| ***cfr-LocationAndBW***  Indicates the CFR location and bandwidth of the non-serving cell for MBS broadcast reception. |
| ***subcarrierSpacing***  Indicates the subcarrier spacing of the CORESET#0 of the non-serving cell for MBS broadcast reception. |

| ***CFR-LocationAndBW* field descriptions** |
| --- |
| ***locationAndBandwidthMBS***  Indicates the starting PRB and the number of PRBs of CFR used for MBS broadcast reception from non-serving cell. The value of the field shall be interpreted as resource indicator value (RIV) as defined TS 38.214 [19] with assumptions as described in TS 38.213 [13]. The first PRB is a PRB determined by *subcarrierSpacing,* *offsetToCarrierMBS* and *absoluteFrequencyPointA-MBS* of the non-serving cell. |
| ***absoluteFrequencyPointA-MBS*** Indicates the absolute frequency position of the reference resource block (Common RB 0) of the non-serving cell for MBS broadcast reception. Its lowest subcarrier is also known as Point A (see TS 38.211 [16], clause 4.4.4.2). |
| ***offsetToCarrierMBS***  Indicates the offset in frequency domain between Point A (lowest subcarrier of common RB 0) and the lowest usable subcarrier on this carrier in number of PRBs (using the *subcarrierSpacing* indicated for the non-serving cell). |

Next Change

– *DRX-ConfigPTM*

The IE *DRX-Config-PTM* is used to configure DRX related parameters for PTM transmission as specified in TS 38.321 [3].

***DRX-Config-PTM* information element**

-- ASN1START

-- TAG-DRX-CONFIGPTM-START

DRX-ConfigPTM-r17 ::= SEQUENCE {

drx-onDurationTimerPTM-r17 CHOICE {

subMilliSeconds INTEGER (1..31),

milliSeconds ENUMERATED {

ms1, ms2, ms3, ms4, ms5, ms6, ms8, ms10, ms20, ms30, ms40, ms50, ms60,

ms80, ms100, ms200, ms300, ms400, ms500, ms600, ms800, ms1000, ms1200,

ms1600, spare8, spare7, spare6, spare5, spare4, spare3, spare2, spare1

}

},

drx-InactivityTimerPTM-r17 ENUMERATED {

ms0, ms1, ms2, ms3, ms4, ms5, ms6, ms8, ms10, ms20, ms30, ms40, ms50, ms60, ms80,

ms100, ms200, ms300, ms500, ms750, ms1280, ms1920, ms2560, spare9, spare8,

spare7, spare6, spare5, spare4, spare3, spare2, spare1

},

drx-HARQ-RTT-TimerDL-PTM-r17 INTEGER (0..56) OPTIONAL, -- Cond HARQFeedback

drx-RetransmissionTimerDL-PTM-r17 ENUMERATED {

sl0, sl1, sl2, sl4, sl6, sl8, sl16, sl24, sl33, sl40, sl64, sl80, sl96, sl112, sl128,

sl160, sl320, spare15, spare14, spare13, spare12, spare11, spare10, spare9,

spare8, spare7, spare6, spare5, spare4, spare3, spare2, spare1

} OPTIONAL, -- Cond HARQFeedback

drx-LongCycleStartOffsetPTM-r17 CHOICE {

ms10 INTEGER(0..9),

ms20 INTEGER(0..19),

ms32 INTEGER(0..31),

ms40 INTEGER(0..39),

ms60 INTEGER(0..59),

ms64 INTEGER(0..63),

ms70 INTEGER(0..69),

ms80 INTEGER(0..79),

ms128 INTEGER(0..127),

ms160 INTEGER(0..159),

ms256 INTEGER(0..255),

ms320 INTEGER(0..319),

ms512 INTEGER(0..511),

ms640 INTEGER(0..639),

ms1024 INTEGER(0..1023),

ms1280 INTEGER(0..1279),

ms2048 INTEGER(0..2047),

ms2560 INTEGER(0..2559),

ms5120 INTEGER(0..5119),

ms10240 INTEGER(0..10239)

},

drx-SlotOffsetPTM-r17 INTEGER (0..31)

}

-- TAG-DRX-CONFIGPTM-STOP

-- ASN1STOP

|  |
| --- |
| ***DRX-Config-PTM* field descriptions** |
| ***drx-HARQ-RTT-Timer-DL-PTM***  Value in number of symbols of the CFR where the transport block was received. |
| ***drx-InactivityTimerPTM***  Value in multiple integers of 1 ms. *ms0* corresponds to 0, *ms1* corresponds to 1 ms, *ms2* corresponds to 2 ms, and so on. |
| ***drx-LongCycleStartOffsetPTM***  *drx-LongCycle-PTM* in ms and *drx-StartOffset-PTM* in multiples of 1 ms. |
| ***drx-onDurationTimerPTM***  Value in multiples of 1/32 ms (subMilliSeconds) or in ms (milliSecond). For the latter, value *ms1* corresponds to 1 ms, value *ms2* corresponds to 2 ms, and so on. |
| ***drx-RetransmissionTimer-DL-PTM***  Value in number of slot lengths of the CFR where the transport block was received. value *sl0* corresponds to 0 slots, *sl1* corresponds to 1 slot, *sl2* corresponds to 2 slots, and so on. |
| ***drx-SlotOffsetPTM***  Value in 1/32 ms. Value 0 corresponds to 0 ms, value 1 corresponds to 1/32 ms, value 2 corresponds to 2/32 ms, and so on. |

|  |  |
| --- | --- |
| **Conditional Presence** | **Explanation** |
| *HARQFeedback* | The field is mandatory present if HARQ feedback is enabled for a G-RNTI/G-CS-RNTI associated with this DRX configuration. The field is optionally present if the IE *DRX-ConfigPTM* is included in *MBSMulticastConfiguration*, need R. It is absent otherwise. |

Next Change

– *MBS-SessionInfoListMulticast*

The IE *MBS-SessionInfoListMulticast* provides a list of MBS multicast sessions transmitted via multicast MRB for RRC\_INACTIVE UEs and, for each MBS multicast session, the associated G-RNTI and scheduling information.

***MBS-SessionInfoListMulticast* information element**

-- ASN1START

-- TAG-MBS-SESSIONINFOLISTMULTICAST-START

MBS-SessionInfoListMulticast-r18 ::= SEQUENCE (SIZE (1..maxNrofMBS-Session-r17)) OF MBS-SessionInfoMulticast-r18

MBS-SessionInfoMulticast-r18 ::= SEQUENCE {

mbs-SessionId-r18 TMGI-r17,

g-RNTI-r18 RNTI-Value OPTIONAL, -- Need R

mrb-ListMulticast-r18 MRB-ListMulticast-r18 OPTIONAL, -- Need R

mtch-SchedulingInfo-r18 DRX-ConfigPTM-Index-r17 OPTIONAL, -- Need S

mtch-NeighbourCell-r18 BIT STRING (SIZE(maxNeighCellMBS-r17)) OPTIONAL, -- Need S

pdsch-ConfigIndex-r18 PDSCH-ConfigIndex-r17 OPTIONAL, -- Need S

mtch-SSB-MappingWindowIndex-r18 MTCH-SSB-MappingWindowIndex-r17 OPTIONAL, -- Cond MTCH-Mapping

thresholdIndex-r18 INTEGER (0..maxNrofThresholdMBS-r18) OPTIONAL, -- Need R

pdcp-SYNC-Indicator-r18 ENUMERATED {true} OPTIONAL, -- Cond RRCRelease

stopMonitoringRNTI-r18 ENUMERATED {true} OPTIONAL -- Need R

}

MRB-ListMulticast-r18 ::= SEQUENCE (SIZE (1.. maxMRB-r17)) OF MRB-InfoMulticast-r18

MRB-InfoMulticast-r18 ::= SEQUENCE {

pdcp-Config-r18 MRB-PDCP-ConfigMulticast-r18,

rlc-Config-r18 MRB-RLC-ConfigMulticast-r18,

...

}

MRB-PDCP-ConfigMulticast-r18 ::= SEQUENCE {

pdcp-SN-SizeDL-r18 ENUMERATED {len12bits, len18bits},

headerCompression-r18 CHOICE {

notUsed NULL,

rohc SEQUENCE {

maxCID-r18 INTEGER (1..16) DEFAULT 15,

profiles-r18 SEQUENCE {

profile0x0000-r18 BOOLEAN,

profile0x0001-r18 BOOLEAN,

profile0x0002-r18 BOOLEAN

}

}

},

t-Reordering-r17 ENUMERATED {ms1, ms10, ms40, ms160, ms500, ms1000, ms1250, ms2750} OPTIONAL -- Need R

}

MRB-RLC-ConfigMulticast-r18 ::= SEQUENCE {

logicalChannelIdentity-r18 CHOICE {

logicalChannelIdentitymulticast-r18 LogicalChannelIdentity,

logicalChannelIdentityExt-r18 LogicalChannelIdentityExt-r17

},

sn-FieldLength-r18 ENUMERATED {size6, size12},

t-Reassembly-r18 T-Reassembly OPTIONAL -- Need R

}

-- TAG-MBS-SESSIONINFOLISTMULTICAST-STOP

-- ASN1STOP

|  |
| --- |
| ***MBS-SessionInfoListMulticast* field descriptions** |
| ***g-RNTI***  G-RNTI used to scramble the scheduling and transmission of multicast MTCH. |
| ***mbs-SessionId***  Indicates an identifier of the MBS session to be received by the UE in RRC\_INACTIVE. |
| ***mrb-listMulticast***  A list of multicast MRBs to which the associated MBS multicast session is mapped to. |
| ***mtch-neighbourCell***  Indicates neighbour cells which provide this service on MTCH for RRC\_INACTIVE. The first bit is set to 1 if the service is provided on MTCH in the first cell in *mbs-NeighbourCellList*, otherwise it is set to 0. The second bit is set to 1 if the service is provided on MTCH in the second cell in *mbs-NeighbourCellList*, and so on. If the service is not available in any neighbouring cell and *mbs-NeighbourCellList* is signalled, the network sets all bits in this field to 0. The field is absent when *mbs-NeighbourCellList* is absent or an empty *mbs-NeighbourCellList* is signalled. If this field is absent when *mbs-NeighbourCellList* is absent or a non-empty *mbs-NeighbourCellList* is signalled, the related service may or may not be available in any neighbouring cell, i.e. the UE cannot determine the presence or absence of an MBS service in neighbouring cells based on the absence of this field. If this field is absent and an empty *mbs-NeighbourCellList* is signalled, then the UE shall assume that MBS multicast services signalled in *mbs-SessionInfoListMulticast* in the *MBSMulticastConfiguration* message are not provided in any neighbour cell. |
| ***mtch-schedulingInfo***  Indicates the index of DRX configuration entry in *drx-ConfigPTM-List* that is used for scheduling the MTCH. The value 0 corresponds to the first entry in *drx-ConfigPTM-List*, the value 1 corresponds to the second entry in *drx-ConfigPTM-List* and so on. In case *mtch-schedulingInfo* is absent for a G-RNTI (i.e. no PTM DRX), the UE shall monitor for PDCCH scrambled with G-RNTI in any slot according to the search space configured for MTCH. |
| ***mtch-SSB-MappingWindowIndex***  Indicates the index of *MTCH-SSB-MappingWindowCycleOffset* configuration entry in *MTCH-SSB-MappingWindowList*. The value 0 corresponds to the first entry in *MTCH-SSB-MappingWindowList*, the value 1 corresponds to the second entry in *MTCH-SSB-MappingWindowList* and so on. This field is set to the same value for all MBS sessions mapped to the same G-RNTI. |
| ***pdcp-SN-SizeDL***  Indicates PDCP sequence number size of 12 or 18 bits, as specified in TS 38.323 [5]. |
| ***pdschConfigIndex***  Indicates the index of PDSCH configuration entry in *pdschConfigList* for MTCH. Value 0 corresponds to the first entry in *pdschConfigList*, the value 1 corresponds to the second entry in *pdschConfigList* and so on. When the field is absent the UE applies the first entry in *pdschConfigList* for MTCH. |
| ***thresholdIndex***  Indicates the index of *thresholdMBS* entry in *thresholdMBS-List* that is used for RRC connection resume for a UE receiving the corresponding multicast session in RRC\_INACTIVE. Value 0 corresponds to the first entry in *thresholdMBS-List*, the value 1 corresponds to the second entry in *thresholdMBS-List* and so on. |
| ***pdcp-SYNC-indicator***  Indicates the PDCP COUNT of the corresponding multicast session is synchronized in the RNA, i.e. the cells in the RNA follow a common QoS flow to MRB mapping rule and at the same time PDCP COUNT is set according to the MBS QoS Flow SN. |
| ***sn-FieldLength***  Indicates RLC SN field size of 6 or12 bits, as specified in TS 38.322 [4]. |
| ***stopMonitoringRNTI***  Indicates the UE to stop monitoring the G-RNTI for the corresponding multicast session. |
| ***t-Reassembly***  Timer for reassembly in TS 38.322 [4], in milliseconds. Value ms0 means 0 ms, value ms5 means 5 ms and so on. |
| ***t-Reordering***  Value in ms of *t-Reordering* specified in TS 38.323 [5]. Value ms1 corresponds to 1 ms, value ms10 corresponds to 10 ms, and so on. |

|  |  |
| --- | --- |
| **Conditional Presence** | **Explanation** |
| *MTCH-Mapping* | The field is mandatory present if the number of actual transmitted SSBs determined according to *ssb-PositionsInBurst* in SIB1 is more than 1, and *searchspaceMulticastMTCH* is not set to zero (including the case where *searchSpaceMulticastMTCH* is absent and *searchSpaceMulticastMCCH* is not set to zero). Otherwise, it is absent, Need R. |
| *RRCRelease* | The field is optionally present if *MBS-SessionInfoListMulticast* is included in *RRCRelease* message. Otherwise, it is absent. |

Next Change

6.4 RRC multiplicity and type constraint values

– Multiplicity and type constraint definitions

-- ASN1START

-- TAG-MULTIPLICITY-AND-TYPE-CONSTRAINT-DEFINITIONS-START

maxAdditionalRACH-r17 INTEGER ::= 256 -- Maximum number of additional RACH configurations.

maxAI-DCI-PayloadSize-r16 INTEGER ::= 128 --Maximum size of the DCI payload scrambled with ai-RNTI

maxAI-DCI-PayloadSize-1-r16 INTEGER ::= 127 --Maximum size of the DCI payload scrambled with ai-RNTI minus 1

maxBandComb INTEGER ::= 65536 -- Maximum number of DL band combinations

maxBandsUTRA-FDD-r16 INTEGER ::= 64 -- Maximum number of bands listed in UTRA-FDD UE caps

maxBH-RLC-ChannelID-r16 INTEGER ::= 65536 -- Maximum value of BH RLC Channel ID

maxBT-IdReport-r16 INTEGER ::= 32 -- Maximum number of Bluetooth IDs to report

maxBT-Name-r16 INTEGER ::= 4 -- Maximum number of Bluetooth name

maxCAG-Cell-r16 INTEGER ::= 16 -- Maximum number of NR CAG cell ranges in SIB3, SIB4

maxTwoPUCCH-Grp-ConfigList-r16 INTEGER ::= 32 -- Maximum number of supported configuration(s) of {primary PUCCH group

-- config, secondary PUCCH group config}

maxTwoPUCCH-Grp-ConfigList-r17 INTEGER ::= 16 -- Maximum number of supported configuration(s) of {primary PUCCH group

-- config, secondary PUCCH group config} for PUCCH cell switching

maxCBR-Config-r16 INTEGER ::= 8 -- Maximum number of CBR range configurations for sidelink communication

-- congestion control

maxCBR-Config-1-r16 INTEGER ::= 7 -- Maximum number of CBR range configurations for sidelink communication

-- congestion control minus 1

maxCBR-Level-r16 INTEGER ::= 16 -- Maximum number of CBR levels

maxCBR-Level-1-r16 INTEGER ::= 15 -- Maximum number of CBR levels minus 1

maxCellExcluded INTEGER ::= 16 -- Maximum number of NR exclude-listed cell ranges in SIB3, SIB4

maxCellGroupings-r16 INTEGER ::= 32 -- Maximum number of cell groupings for NR-DC

maxCellHistory-r16 INTEGER ::= 16 -- Maximum number of visited PCells reported

maxPSCellHistory-r17 INTEGER ::= 16 -- Maximum number of visited PSCells across all reported PCells

maxCellInter INTEGER ::= 16 -- Maximum number of inter-Freq cells listed in SIB4

maxCellIntra INTEGER ::= 16 -- Maximum number of intra-Freq cells listed in SIB3

maxCellMeasEUTRA INTEGER ::= 32 -- Maximum number of cells in E-UTRAN

maxCellMeasIdle-r16 INTEGER ::= 8 -- Maximum number of cells per carrier for idle/inactive measurements

maxCellMeasUTRA-FDD-r16 INTEGER ::= 32 -- Maximum number of cells in FDD UTRAN

maxCellNTN-r17 INTEGER ::= 4 -- Maximum number of NTN neighbour cells for which assistance information is

-- provided

maxCarrierTypePairList-r16 INTEGER ::= 16 -- Maximum number of supported carrier type pair of (carrier type on which

-- CSI measurement is performed, carrier type on which CSI reporting is

-- performed) for CSI reporting cross PUCCH group

maxCellAllowed INTEGER ::= 16 -- Maximum number of NR allow-listed cell ranges in SIB3, SIB4

maxEARFCN INTEGER ::= 262143 -- Maximum value of E-UTRA carrier frequency

maxEUTRA-CellExcluded INTEGER ::= 16 -- Maximum number of E-UTRA exclude-listed physical cell identity ranges

-- in SIB5

maxEUTRA-NS-Pmax INTEGER ::= 8 -- Maximum number of NS and P-Max values per band

maxFeatureCombPreamblesPerRACHResource-r17 INTEGER ::= 256 -- Maximum number of feature combination preambles.

maxLogMeasReport-r16 INTEGER ::= 520 -- Maximum number of entries for logged measurements

maxMultiBands INTEGER ::= 8 -- Maximum number of additional frequency bands that a cell belongs to

maxNARFCN INTEGER ::= 3279165 -- Maximum value of NR carrier frequency

maxNR-NS-Pmax INTEGER ::= 8 -- Maximum number of NS and P-Max values per band

maxFreqIdle-r16 INTEGER ::= 8 -- Maximum number of carrier frequencies for idle/inactive measurements

maxNrofServingCells INTEGER ::= 32 -- Max number of serving cells (SpCells + SCells)

maxNrofServingCells-1 INTEGER ::= 31 -- Max number of serving cells (SpCells + SCells) minus 1

maxNrofAggregatedCellsPerCellGroup INTEGER ::= 16

maxNrofAggregatedCellsPerCellGroupMinus4-r16 INTEGER ::= 12

maxNrofDUCells-r16 INTEGER ::= 512 -- Max number of cells configured on the collocated IAB-DU

maxNrofAppLayerMeas-r17 INTEGER ::= 16 -- Max number of simultaneous application layer measurements

maxNrofAppLayerMeas-1-r17 INTEGER ::= 15 -- Max number of simultaneous application layer measurements minus 1

maxNrofAvailabilityCombinationsPerSet-r16 INTEGER ::= 512 -- Max number of AvailabilityCombinationId used in the DCI format 2\_5

maxNrofAvailabilityCombinationsPerSet-1-r16 INTEGER ::= 511 -- Max number of AvailabilityCombinationId used in the DCI format 2\_5 minus 1

maxNrofIABResourceConfig-r17 INTEGER ::= 65536 -- Max number of IAB-ResourceConfigID used in MAC CE

maxNrofIABResourceConfig-1-r17 INTEGER ::= 65535 -- Max number of IAB-ResourceConfigID used in MAC CE minus 1

maxNrofSCellActRS-r17 INTEGER ::= 255 -- Max number of RS configurations per SCell for SCell activation

maxNrofSCells INTEGER ::= 31 -- Max number of secondary serving cells per cell group

maxNrofCellMeas INTEGER ::= 32 -- Maximum number of entries in each of the cell lists in a measurement object

maxNrofCRS-IM-InterfCell-r17 INTEGER ::= 8 -- Maximum number of LTE interference cells for CRS-IM per UE

maxNrofRelayMeas-r17 INTEGER ::= 32 -- Maximum number of L2 U2N Relay UEs to measure for each measurement object

-- on sidelink frequency

maxNrofCG-SL-r16 INTEGER ::= 8 -- Max number of sidelink configured grant

maxNrofCG-SL-1-r16 INTEGER ::= 7 -- Max number of sidelink configured grant minus 1

maxSL-GC-BC-DRX-QoS-r17 INTEGER ::= 16 -- Max number of sidelink DRX configurations for NR

-- sidelink groupcast/broadcast communication

maxNrofSL-RxInfoSet-r17 INTEGER ::= 4 -- Max number of sidelink DRX configuration sets in sidelink DRX assistant

-- information

maxNrofSS-BlocksToAverage INTEGER ::= 16 -- Max number for the (max) number of SS blocks to average to determine cell measurement

maxNrofCondCells-r16 INTEGER ::= 8 -- Max number of conditional candidate SpCells

maxNrofCondCells-1-r17 INTEGER ::= 7 -- Max number of conditional candidate SpCells minus 1

maxNrofCSI-RS-ResourcesToAverage INTEGER ::= 16 -- Max number for the (max) number of CSI-RS to average to determine cell measurement

maxNrofDL-Allocations INTEGER ::= 16 -- Maximum number of PDSCH time domain resource allocations

maxNrofDL-AllocationsExt-r17 INTEGER ::= 64 -- Maximum number of PDSCH time domain resource allocations for multi-PDSCH

-- scheduling

maxNrofPDU-Sessions-r17 INTEGER ::= 256 -- Maximum number of PDU Sessions

maxNrofSR-ConfigPerCellGroup INTEGER ::= 8 -- Maximum number of SR configurations per cell group

maxLCG-ID INTEGER ::= 7 -- Maximum value of LCG ID

maxLCG-ID-IAB-r17 INTEGER ::= 255 -- Maximum value of LCG ID for IAB-MT

maxLC-ID INTEGER ::= 32 -- Maximum value of Logical Channel ID

maxLC-ID-Iab-r16 INTEGER ::= 65855 -- Maximum value of BH Logical Channel ID extension

maxLTE-CRS-Patterns-r16 INTEGER ::= 3 -- Maximum number of additional LTE CRS rate matching patterns

maxNrofTAGs INTEGER ::= 4 -- Maximum number of Timing Advance Groups

maxNrofTAGs-1 INTEGER ::= 3 -- Maximum number of Timing Advance Groups minus 1

maxNrofBWPs INTEGER ::= 4 -- Maximum number of BWPs per serving cell

maxNrofCombIDC INTEGER ::= 128 -- Maximum number of reported MR-DC combinations for IDC

maxNrofSymbols-1 INTEGER ::= 13 -- Maximum index identifying a symbol within a slot (14 symbols, indexed from 0..13)

maxNrofSlots INTEGER ::= 320 -- Maximum number of slots in a 10 ms period

maxNrofSlots-1 INTEGER ::= 319 -- Maximum number of slots in a 10 ms period minus 1

maxNrofPhysicalResourceBlocks INTEGER ::= 275 -- Maximum number of PRBs

maxNrofPhysicalResourceBlocks-1 INTEGER ::= 274 -- Maximum number of PRBs minus 1

maxNrofPhysicalResourceBlocksPlus1 INTEGER ::= 276 -- Maximum number of PRBs plus 1

maxNrofControlResourceSets INTEGER ::= 12 -- Max number of CoReSets configurable on a serving cell

maxNrofControlResourceSets-1 INTEGER ::= 11 -- Max number of CoReSets configurable on a serving cell minus 1

maxNrofControlResourceSets-1-r16 INTEGER ::= 15 -- Max number of CoReSets configurable on a serving cell extended in minus 1

maxNrofCoresetPools-r16 INTEGER ::= 2 -- Maximum number of CORESET pools

maxCoReSetDuration INTEGER ::= 3 -- Max number of OFDM symbols in a control resource set

maxNrofSearchSpaces-1 INTEGER ::= 39 -- Max number of Search Spaces minus 1

maxNrofSearchSpacesLinks-1-r17 INTEGER ::= 39 -- Max number of Search Space links minus 1

maxNrofBFDResourcePerSet-r17 INTEGER ::= 64 -- Max number of reference signal in one BFD set

maxSFI-DCI-PayloadSize INTEGER ::= 128 -- Max number payload of a DCI scrambled with SFI-RNTI

maxSFI-DCI-PayloadSize-1 INTEGER ::= 127 -- Max number payload of a DCI scrambled with SFI-RNTI minus 1

maxIAB-IP-Address-r16 INTEGER ::= 32 -- Max number of assigned IP addresses

maxINT-DCI-PayloadSize INTEGER ::= 126 -- Max number payload of a DCI scrambled with INT-RNTI

maxINT-DCI-PayloadSize-1 INTEGER ::= 125 -- Max number payload of a DCI scrambled with INT-RNTI minus 1

maxNrofRateMatchPatterns INTEGER ::= 4 -- Max number of rate matching patterns that may be configured

maxNrofRateMatchPatterns-1 INTEGER ::= 3 -- Max number of rate matching patterns that may be configured minus 1

maxNrofRateMatchPatternsPerGroup INTEGER ::= 8 -- Max number of rate matching patterns that may be configured in one group

maxNrofCSI-ReportConfigurations INTEGER ::= 48 -- Maximum number of report configurations

maxNrofCSI-ReportConfigurations-1 INTEGER ::= 47 -- Maximum number of report configurations minus 1

maxNrofCSI-ResourceConfigurations INTEGER ::= 112 -- Maximum number of resource configurations

maxNrofCSI-ResourceConfigurations-1 INTEGER ::= 111 -- Maximum number of resource configurations minus 1

maxNrofAP-CSI-RS-ResourcesPerSet INTEGER ::= 16

maxNrOfCSI-AperiodicTriggers INTEGER ::= 128 -- Maximum number of triggers for aperiodic CSI reporting

maxNrofReportConfigPerAperiodicTrigger INTEGER ::= 16 -- Maximum number of report configurations per trigger state for aperiodic reporting

maxNrofNZP-CSI-RS-Resources INTEGER ::= 192 -- Maximum number of Non-Zero-Power (NZP) CSI-RS resources

maxNrofNZP-CSI-RS-Resources-1 INTEGER ::= 191 -- Maximum number of Non-Zero-Power (NZP) CSI-RS resources minus 1

maxNrofNZP-CSI-RS-ResourcesPerSet INTEGER ::= 64 -- Maximum number of NZP CSI-RS resources per resource set

maxNrofNZP-CSI-RS-ResourceSets INTEGER ::= 64 -- Maximum number of NZP CSI-RS resource sets per cell

maxNrofNZP-CSI-RS-ResourceSets-1 INTEGER ::= 63 -- Maximum number of NZP CSI-RS resource sets per cell minus 1

maxNrofNZP-CSI-RS-ResourceSetsPerConfig INTEGER ::= 16 -- Maximum number of resource sets per resource configuration

maxNrofNZP-CSI-RS-ResourcesPerConfig INTEGER ::= 128 -- Maximum number of resources per resource configuration

maxNrofZP-CSI-RS-Resources INTEGER ::= 32 -- Maximum number of Zero-Power (ZP) CSI-RS resources

maxNrofZP-CSI-RS-Resources-1 INTEGER ::= 31 -- Maximum number of Zero-Power (ZP) CSI-RS resources minus 1

maxNrofZP-CSI-RS-ResourceSets-1 INTEGER ::= 15

maxNrofZP-CSI-RS-ResourcesPerSet INTEGER ::= 16

maxNrofZP-CSI-RS-ResourceSets INTEGER ::= 16

maxNrofCSI-IM-Resources INTEGER ::= 32 -- Maximum number of CSI-IM resources

maxNrofCSI-IM-Resources-1 INTEGER ::= 31 -- Maximum number of CSI-IM resources minus 1

maxNrofCSI-IM-ResourcesPerSet INTEGER ::= 8 -- Maximum number of CSI-IM resources per set

maxNrofCSI-IM-ResourceSets INTEGER ::= 64 -- Maximum number of NZP CSI-IM resource sets per cell

maxNrofCSI-IM-ResourceSets-1 INTEGER ::= 63 -- Maximum number of NZP CSI-IM resource sets per cell minus 1

maxNrofCSI-IM-ResourceSetsPerConfig INTEGER ::= 16 -- Maximum number of CSI IM resource sets per resource configuration

maxNrofCSI-SSB-ResourcePerSet INTEGER ::= 64 -- Maximum number of SSB resources in a resource set

maxNrofCSI-SSB-ResourceSets INTEGER ::= 64 -- Maximum number of CSI SSB resource sets per cell

maxNrofCSI-SSB-ResourceSets-1 INTEGER ::= 63 -- Maximum number of CSI SSB resource sets per cell minus 1

maxNrofCSI-SSB-ResourceSetsPerConfig INTEGER ::= 1 -- Maximum number of CSI SSB resource sets per resource configuration

maxNrofCSI-SSB-ResourceSetsPerConfigExt INTEGER ::= 2 -- Maximum number of CSI SSB resource sets per resource configuration

-- extended

maxNrofFailureDetectionResources INTEGER ::= 10 -- Maximum number of failure detection resources

maxNrofFailureDetectionResources-1 INTEGER ::= 9 -- Maximum number of failure detection resources minus 1

maxNrofFailureDetectionResources-1-r17 INTEGER ::= 63 -- Maximum number of the enhanced failure detection resources minus 1

maxNrofFreqSL-r16 INTEGER ::= 8 -- Maximum number of carrier frequency for NR sidelink communication

maxNrofSL-BWPs-r16 INTEGER ::= 4 -- Maximum number of BWP for NR sidelink communication

maxFreqSL-EUTRA-r16 INTEGER ::= 8 -- Maximum number of EUTRA anchor carrier frequency for NR sidelink communication

maxNrofSL-MeasId-r16 INTEGER ::= 64 -- Maximum number of sidelink measurement identity (RSRP) per destination

maxNrofSL-ObjectId-r16 INTEGER ::= 64 -- Maximum number of sidelink measurement objects (RSRP) per destination

maxNrofSL-ReportConfigId-r16 INTEGER ::= 64 -- Maximum number of sidelink measurement reporting configuration(RSRP) per destination

maxNrofSL-PoolToMeasureNR-r16 INTEGER ::= 8 -- Maximum number of resource pool for NR sidelink measurement to measure for

-- each measurement object (for CBR)

maxFreqSL-NR-r16 INTEGER ::= 8 -- Maximum number of NR anchor carrier frequency for NR sidelink communication

maxNrofSL-QFIs-r16 INTEGER ::= 2048 -- Maximum number of QoS flow for NR sidelink communication per UE

maxNrofSL-QFIsPerDest-r16 INTEGER ::= 64 -- Maximum number of QoS flow per destination for NR sidelink communication

maxNrofObjectId INTEGER ::= 64 -- Maximum number of measurement objects

maxNrofPageRec INTEGER ::= 32 -- Maximum number of page records

maxNrofPCI-Ranges INTEGER ::= 8 -- Maximum number of PCI ranges

maxPLMN INTEGER ::= 12 -- Maximum number of PLMNs broadcast and reported by UE at establishment

maxTAC-r17 INTEGER ::= 12 -- Maximum number of Tracking Area Codes to which a cell belongs to

maxNrofCSI-RS-ResourcesRRM INTEGER ::= 96 -- Maximum number of CSI-RS resources per cell for an RRM measurement object

maxNrofCSI-RS-ResourcesRRM-1 INTEGER ::= 95 -- Maximum number of CSI-RS resources per cell for an RRM measurement object

-- minus 1.

maxNrofMeasId INTEGER ::= 64 -- Maximum number of configured measurements

maxNrofQuantityConfig INTEGER ::= 2 -- Maximum number of quantity configurations

maxNrofCSI-RS-CellsRRM INTEGER ::= 96 -- Maximum number of cells with CSI-RS resources for an RRM measurement object

maxNrofSL-Dest-r16 INTEGER ::= 32 -- Maximum number of destination for NR sidelink communication and discovery

maxNrofSL-Dest-1-r16 INTEGER ::= 31 -- Highest index of destination for NR sidelink communication and discovery

maxNrofSLRB-r16 INTEGER ::= 512 -- Maximum number of radio bearer for NR sidelink communication per UE

maxSL-LCID-r16 INTEGER ::= 512 -- Maximum number of RLC bearer for NR sidelink communication per UE

maxSL-SyncConfig-r16 INTEGER ::= 16 -- Maximum number of sidelink Sync configurations

maxNrofRXPool-r16 INTEGER ::= 16 -- Maximum number of Rx resource pool for NR sidelink communication and

-- discovery

maxNrofTXPool-r16 INTEGER ::= 8 -- Maximum number of Tx resource pool for NR sidelink communication and

-- discovery

maxNrofPoolID-r16 INTEGER ::= 16 -- Maximum index of resource pool for NR sidelink communication and

-- discovery

maxNrofSRS-PathlossReferenceRS-r16 INTEGER ::= 64 -- Maximum number of RSs used as pathloss reference for SRS power control.

maxNrofSRS-PathlossReferenceRS-1-r16 INTEGER ::= 63 -- Maximum number of RSs used as pathloss reference for SRS power control

-- minus 1.

maxNrofSRS-ResourceSets INTEGER ::= 16 -- Maximum number of SRS resource sets in a BWP.

maxNrofSRS-ResourceSets-1 INTEGER ::= 15 -- Maximum number of SRS resource sets in a BWP minus 1.

maxNrofSRS-PosResourceSets-r16 INTEGER ::= 16 -- Maximum number of SRS Positioning resource sets in a BWP.

maxNrofSRS-PosResourceSets-1-r16 INTEGER ::= 15 -- Maximum number of SRS Positioning resource sets in a BWP minus 1.

maxNrofSRS-Resources INTEGER ::= 64 -- Maximum number of SRS resources.

maxNrofSRS-Resources-1 INTEGER ::= 63 -- Maximum number of SRS resources minus 1.

maxNrofSRS-PosResources-r16 INTEGER ::= 64 -- Maximum number of SRS Positioning resources.

maxNrofSRS-PosResources-1-r16 INTEGER ::= 63 -- Maximum number of SRS Positioning resources minus 1.

maxNrofSRS-ResourcesPerSet INTEGER ::= 16 -- Maximum number of SRS resources in an SRS resource set

maxNrofSRS-TriggerStates-1 INTEGER ::= 3 -- Maximum number of SRS trigger states minus 1, i.e., the largest code point.

maxNrofSRS-TriggerStates-2 INTEGER ::= 2 -- Maximum number of SRS trigger states minus 2.

maxRAT-CapabilityContainers INTEGER ::= 8 -- Maximum number of interworking RAT containers (incl NR and MRDC)

maxSimultaneousBands INTEGER ::= 32 -- Maximum number of simultaneously aggregated bands

maxULTxSwitchingBandPairs INTEGER ::= 32 -- Maximum number of band pairs supporting dynamic UL Tx switching in a band

-- combination.

maxNrofSlotFormatCombinationsPerSet INTEGER ::= 512 -- Maximum number of Slot Format Combinations in a SF-Set.

maxNrofSlotFormatCombinationsPerSet-1 INTEGER ::= 511 -- Maximum number of Slot Format Combinations in a SF-Set minus 1.

maxNrofTrafficPattern-r16 INTEGER ::= 8 -- Maximum number of Traffic Pattern for NR sidelink communication.

maxNrofPUCCH-Resources INTEGER ::= 128

maxNrofPUCCH-Resources-1 INTEGER ::= 127

maxNrofPUCCH-ResourceSets INTEGER ::= 4 -- Maximum number of PUCCH Resource Sets

maxNrofPUCCH-ResourceSets-1 INTEGER ::= 3 -- Maximum number of PUCCH Resource Sets minus 1.

maxNrofPUCCH-ResourcesPerSet INTEGER ::= 32 -- Maximum number of PUCCH Resources per PUCCH-ResourceSet

maxNrofPUCCH-P0-PerSet INTEGER ::= 8 -- Maximum number of P0-pucch present in a p0-pucch set

maxNrofPUCCH-PathlossReferenceRSs INTEGER ::= 4 -- Maximum number of RSs used as pathloss reference for PUCCH power control.

maxNrofPUCCH-PathlossReferenceRSs-1 INTEGER ::= 3 -- Maximum number of RSs used as pathloss reference for PUCCH power control

-- minus 1.

maxNrofPUCCH-PathlossReferenceRSs-r16 INTEGER ::= 64 -- Maximum number of RSs used as pathloss reference for PUCCH power control

-- extended.

maxNrofPUCCH-PathlossReferenceRSs-1-r16 INTEGER ::= 63 -- Maximum number of RSs used as pathloss reference for PUCCH power control

-- minus 1 extended.

maxNrofPUCCH-PathlossReferenceRSs-1-r17 INTEGER ::= 7 -- Maximum number of RSs used as pathloss reference for PUCCH power control

-- minus 1.

maxNrofPUCCH-PathlossReferenceRSsDiff-r16 INTEGER ::= 60 -- Difference between the extended maximum and the non-extended maximum

maxNrofPUCCH-ResourceGroups-r16 INTEGER ::= 4 -- Maximum number of PUCCH resources groups.

maxNrofPUCCH-ResourcesPerGroup-r16 INTEGER ::= 128 -- Maximum number of PUCCH resources in a PUCCH group.

maxNrofPowerControlSetInfos-r17 INTEGER ::= 8 -- Maximum number of PUCCH power control set infos

maxNrofMultiplePUSCHs-r16 INTEGER ::= 8 -- Maximum number of multiple PUSCHs in PUSCH TDRA list

maxNrofP0-PUSCH-AlphaSets INTEGER ::= 30 -- Maximum number of P0-pusch-alpha-sets (see TS 38.213 [13], clause 7.1)

maxNrofP0-PUSCH-AlphaSets-1 INTEGER ::= 29 -- Maximum number of P0-pusch-alpha-sets minus 1 (see TS 38.213 [13], clause 7.1)

maxNrofPUSCH-PathlossReferenceRSs INTEGER ::= 4 -- Maximum number of RSs used as pathloss reference for PUSCH power control.

maxNrofPUSCH-PathlossReferenceRSs-1 INTEGER ::= 3 -- Maximum number of RSs used as pathloss reference for PUSCH power control

-- minus 1.

maxNrofPUSCH-PathlossReferenceRSs-r16 INTEGER ::= 64 -- Maximum number of RSs used as pathloss reference for PUSCH power control

-- extended

maxNrofPUSCH-PathlossReferenceRSs-1-r16 INTEGER ::= 63 -- Maximum number of RSs used as pathloss reference for PUSCH power control

-- extended minus 1

maxNrofPUSCH-PathlossReferenceRSsDiff-r16 INTEGER ::= 60 -- Difference between maxNrofPUSCH-PathlossReferenceRSs-r16 and

-- maxNrofPUSCH-PathlossReferenceRSs

maxNrofPathlossReferenceRSs-r17 INTEGER ::= 64 -- Maximum number of RSs used as pathloss reference for PUSCH, PUCCH, SRS

-- power control for unified TCI state operation

maxNrofPathlossReferenceRSs-1-r17 INTEGER ::= 63 -- Maximum number of RSs used as pathloss reference for PUSCH, PUCCH, SRS

-- power control for unified TCI state operation minus 1

maxNrofNAICS-Entries INTEGER ::= 8 -- Maximum number of supported NAICS capability set

maxBands INTEGER ::= 1024 -- Maximum number of supported bands in UE capability.

maxBandsMRDC INTEGER ::= 1280

maxBandsEUTRA INTEGER ::= 256

maxCellReport INTEGER ::= 8

maxDRB INTEGER ::= 29 -- Maximum number of DRBs (that can be added in DRB-ToAddModList).

maxFreq INTEGER ::= 8 -- Max number of frequencies.

maxFreqLayers INTEGER ::= 4 -- Max number of frequency layers.

maxFreqPlus1 INTEGER ::= 9 -- Max number of frequencies for Slicing.

maxFreqIDC-r16 INTEGER ::= 128 -- Max number of frequencies for IDC indication.

maxCombIDC-r16 INTEGER ::= 128 -- Max number of reported UL CA for IDC indication.

maxFreqIDC-MRDC INTEGER ::= 32 -- Maximum number of candidate NR frequencies for MR-DC IDC indication

maxNrofCandidateBeams INTEGER ::= 16 -- Max number of PRACH-ResourceDedicatedBFR in BFR config.

maxNrofCandidateBeams-r16 INTEGER ::= 64 -- Max number of candidate beam resources in BFR config.

maxNrofCandidateBeamsExt-r16 INTEGER ::= 48 -- Max number of PRACH-ResourceDedicatedBFR in the CandidateBeamRSListExt

maxNrofPCIsPerSMTC INTEGER ::= 64 -- Maximum number of PCIs per SMTC.

maxNrofQFIs INTEGER ::= 64

maxNrofResourceAvailabilityPerCombination-r16 INTEGER ::= 256

maxNrOfSemiPersistentPUSCH-Triggers INTEGER ::= 64 -- Maximum number of triggers for semi persistent reporting on PUSCH

maxNrofSR-Resources INTEGER ::= 8 -- Maximum number of SR resources per BWP in a cell.

maxNrofSlotFormatsPerCombination INTEGER ::= 256

maxNrofSpatialRelationInfos INTEGER ::= 8

maxNrofSpatialRelationInfos-plus-1 INTEGER ::= 9

maxNrofSpatialRelationInfos-r16 INTEGER ::= 64

maxNrofSpatialRelationInfosDiff-r16 INTEGER ::= 56 -- Difference between maxNrofSpatialRelationInfos-r16 and maxNrofSpatialRelationInfos

maxNrofIndexesToReport INTEGER ::= 32

maxNrofIndexesToReport2 INTEGER ::= 64

maxNrofSSBs-r16 INTEGER ::= 64 -- Maximum number of SSB resources in a resource set.

maxNrofSSBs-1 INTEGER ::= 63 -- Maximum number of SSB resources in a resource set minus 1.

maxNrofS-NSSAI INTEGER ::= 8 -- Maximum number of S-NSSAI.

maxNrofTCI-StatesPDCCH INTEGER ::= 64

maxNrofTCI-States INTEGER ::= 128 -- Maximum number of TCI states.

maxNrofTCI-States-1 INTEGER ::= 127 -- Maximum number of TCI states minus 1.

maxUL-TCI-r17 INTEGER ::= 64 -- Maximum number of TCI states.

maxUL-TCI-1-r17 INTEGER ::= 63 -- Maximum number of TCI states minus 1.

maxNrofAdditionalPCI-r17 INTEGER ::= 7 -- Maximum number of additional PCI

maxMPE-Resources-r17 INTEGER ::= 64 -- Maximum number of pooled MPE resources

maxNrofUL-Allocations INTEGER ::= 16 -- Maximum number of PUSCH time domain resource allocations.

maxQFI INTEGER ::= 63

maxRA-CSIRS-Resources INTEGER ::= 96

maxRA-OccasionsPerCSIRS INTEGER ::= 64 -- Maximum number of RA occasions for one CSI-RS

maxRA-Occasions-1 INTEGER ::= 511 -- Maximum number of RA occasions in the system

maxRA-SSB-Resources INTEGER ::= 64

maxSCSs INTEGER ::= 5

maxSecondaryCellGroups INTEGER ::= 3

maxNrofServingCellsEUTRA INTEGER ::= 32

maxMBSFN-Allocations INTEGER ::= 8

maxNrofMultiBands INTEGER ::= 8

maxCellSFTD INTEGER ::= 3 -- Maximum number of cells for SFTD reporting

maxReportConfigId INTEGER ::= 64

maxNrofCodebooks INTEGER ::= 16 -- Maximum number of codebooks supported by the UE

maxNrofCSI-RS-ResourcesExt-r16 INTEGER ::= 16 -- Maximum number of codebook resources supported by the UE for eType2/Codebook combo

maxNrofCSI-RS-ResourcesExt-r17 INTEGER ::= 8 -- Maximum number of codebook resources for fetype2R1 and fetype2R2

maxNrofCSI-RS-Resources INTEGER ::= 7 -- Maximum number of codebook resources supported by the UE

maxNrofCSI-RS-ResourcesAlt-r16 INTEGER ::= 512 -- Maximum number of alternative codebook resources supported by the UE

maxNrofCSI-RS-ResourcesAlt-1-r16 INTEGER ::= 511 -- Maximum number of alternative codebook resources supported by the UE minus 1

maxNrofSRI-PUSCH-Mappings INTEGER ::= 16

maxNrofSRI-PUSCH-Mappings-1 INTEGER ::= 15

maxSIB INTEGER::= 32 -- Maximum number of SIBs

maxSI-Message INTEGER::= 32 -- Maximum number of SI messages

maxSIB-MessagePlus1-r17 INTEGER::= 33 -- Maximum number of SIB messages plus 1

maxPO-perPF INTEGER ::= 4 -- Maximum number of paging occasion per paging frame

maxPEI-perPF-r17 INTEGER ::= 4 -- Maximum number of PEI occasion per paging frame

maxAccessCat-1 INTEGER ::= 63 -- Maximum number of Access Categories minus 1

maxBarringInfoSet INTEGER ::= 8 -- Maximum number of access control parameter sets

maxCellEUTRA INTEGER ::= 8 -- Maximum number of E-UTRA cells in SIB list

maxEUTRA-Carrier INTEGER ::= 8 -- Maximum number of E-UTRA carriers in SIB list

maxPLMNIdentities INTEGER ::= 8 -- Maximum number of PLMN identities in RAN area configurations

maxDownlinkFeatureSets INTEGER ::= 1024 -- (for NR DL) Total number of FeatureSets (size of the pool)

maxUplinkFeatureSets INTEGER ::= 1024 -- (for NR UL) Total number of FeatureSets (size of the pool)

maxEUTRA-DL-FeatureSets INTEGER ::= 256 -- (for E-UTRA) Total number of FeatureSets (size of the pool)

maxEUTRA-UL-FeatureSets INTEGER ::= 256 -- (for E-UTRA) Total number of FeatureSets (size of the pool)

maxFeatureSetsPerBand INTEGER ::= 128 -- (for NR) The number of feature sets associated with one band.

maxPerCC-FeatureSets INTEGER ::= 1024 -- (for NR) Total number of CC-specific FeatureSets (size of the pool)

maxFeatureSetCombinations INTEGER ::= 1024 -- (for MR-DC/NR)Total number of Feature set combinations (size of the pool)

maxInterRAT-RSTD-Freq INTEGER ::= 3

maxGIN-r17 INTEGER ::= 24 -- Maximum number of broadcast GINs

maxHRNN-Len-r16 INTEGER ::= 48 -- Maximum length of HRNNs

maxNPN-r16 INTEGER ::= 12 -- Maximum number of NPNs broadcast and reported by UE at establishment

maxNrOfMinSchedulingOffsetValues-r16 INTEGER ::= 2 -- Maximum number of min. scheduling offset (K0/K2) configurations

maxK0-SchedulingOffset-r16 INTEGER ::= 16 -- Maximum number of slots configured as min. scheduling offset (K0)

maxK2-SchedulingOffset-r16 INTEGER ::= 16 -- Maximum number of slots configured as min. scheduling offset (K2)

maxK0-SchedulingOffset-r17 INTEGER ::= 64 -- Maximum number of slots configured as min. scheduling offset (K0)

maxK2-SchedulingOffset-r17 INTEGER ::= 64 -- Maximum number of slots configured as min. scheduling offset (K2)

maxDCI-2-6-Size-r16 INTEGER ::= 140 -- Maximum size of DCI format 2-6

maxDCI-2-7-Size-r17 INTEGER ::= 43 -- Maximum size of DCI format 2-7

maxDCI-2-6-Size-1-r16 INTEGER ::= 139 -- Maximum DCI format 2-6 size minus 1

maxNrofUL-Allocations-r16 INTEGER ::= 64 -- Maximum number of PUSCH time domain resource allocations

maxNrofP0-PUSCH-Set-r16 INTEGER ::= 2 -- Maximum number of P0 PUSCH set(s)

maxOnDemandSIB-r16 INTEGER ::= 8 -- Maximum number of SIB(s) that can be requested on-demand

maxOnDemandPosSIB-r16 INTEGER ::= 32 -- Maximum number of posSIB(s) that can be requested on-demand

maxCI-DCI-PayloadSize-r16 INTEGER ::= 126 -- Maximum number of the DCI size for CI

maxCI-DCI-PayloadSize-1-r16 INTEGER ::= 125 -- Maximum number of the DCI size for CI minus 1

maxUu-RelayRLC-ChannelID-r17 INTEGER ::= 32 -- Maximum value of Uu Relay RLC channel ID

maxWLAN-Id-Report-r16 INTEGER ::= 32 -- Maximum number of WLAN IDs to report

maxWLAN-Name-r16 INTEGER ::= 4 -- Maximum number of WLAN name

maxRAReport-r16 INTEGER ::= 8 -- Maximum number of RA procedures information to be included in the RA report

maxTxConfig-r16 INTEGER ::= 64 -- Maximum number of sidelink transmission parameters configurations

maxTxConfig-1-r16 INTEGER ::= 63 -- Maximum number of sidelink transmission parameters configurations minus 1

maxPSSCH-TxConfig-r16 INTEGER ::= 16 -- Maximum number of PSSCH TX configurations

maxNrofCLI-RSSI-Resources-r16 INTEGER ::= 64 -- Maximum number of CLI-RSSI resources for UE

maxNrofCLI-RSSI-Resources-1-r16 INTEGER ::= 63 -- Maximum number of CLI-RSSI resources for UE minus 1

maxNrofCLI-SRS-Resources-r16 INTEGER ::= 32 -- Maximum number of SRS resources for CLI measurement for UE

maxCLI-Report-r16 INTEGER ::= 8

maxNrofCC-Group-r17 INTEGER ::= 16 -- Maximum number of CC groups for DC location report

maxNrofConfiguredGrantConfig-r16 INTEGER ::= 12 -- Maximum number of configured grant configurations per BWP

maxNrofConfiguredGrantConfig-1-r16 INTEGER ::= 11 -- Maximum number of configured grant configurations per BWP minus 1

maxNrofCG-Type2DeactivationState INTEGER ::= 16 -- Maximum number of deactivation state for type 2 configured grants per BWP

maxNrofConfiguredGrantConfigMAC-1-r16 INTEGER ::= 31 -- Maximum number of configured grant configurations per MAC entity minus 1

maxNrofSPS-Config-r16 INTEGER ::= 8 -- Maximum number of SPS configurations per BWP

maxNrofSPS-Config-1-r16 INTEGER ::= 7 -- Maximum number of SPS configurations per BWP minus 1

maxNrofSPS-DeactivationState INTEGER ::= 16 -- Maximum number of deactivation state for SPS per BWP

maxNrofPPW-Config-r17 INTEGER ::= 4 -- Maximum number of Preconfigured PRS processing windows per DL BWP

maxNrofPPW-ID-1-r17 INTEGER ::= 15 -- Maximum number of Preconfigured PRS processing windows minus 1

maxNrOfTxTEGReport-r17 INTEGER ::= 256 -- Maximum number of UE Tx Timing Error Group Report

maxNrOfTxTEG-ID-1-r17 INTEGER ::= 7 -- Maximum number of UE Tx Timing Error Group ID minus 1

maxNrofPagingSubgroups-r17 INTEGER ::= 8 -- Maximum number of paging subgroups per paging occasion

maxNrofPUCCH-ResourceGroups-1-r16 INTEGER ::= 3

maxNrofReqComDC-Location-r17 INTEGER ::= 128 -- Maximum number of requested carriers/BWPs combinations for DC location

-- report

maxNrofServingCellsTCI-r16 INTEGER ::= 32 -- Maximum number of serving cells in simultaneousTCI-UpdateList

maxNrofTxDC-TwoCarrier-r16 INTEGER ::= 64 -- Maximum number of UL Tx DC locations reported by the UE for 2CC uplink CA

maxNrofRB-SetGroups-r17 INTEGER ::= 8 -- Maximum number of RB set groups

maxNrofRB-Sets-r17 INTEGER ::= 8 -- Maximum number of RB sets

maxNrofEnhType3HARQ-ACK-r17 INTEGER ::= 8 -- Maximum number of enhanced type 3 HARQ-ACK codebook

maxNrofEnhType3HARQ-ACK-1-r17 INTEGER ::= 7 -- Maximum number of enhanced type 3 HARQ-ACK codebook minus 1

maxNrofPRS-ResourcesPerSet-r17 INTEGER ::= 64 -- Maximum number of PRS resources for one set

maxNrofPRS-ResourcesPerSet-1-r17 INTEGER ::= 63 -- Maximum number of PRS resources for one set minus 1

maxNrofPRS-ResourceOffsetValue-1-r17 INTEGER ::= 511

maxNrofGapId-r17 INTEGER ::= 8 -- Maximum number of measurement gap ID is FFS

maxNrofPreConfigPosGapId-r17 INTEGER ::= 16 -- Maximum number of preconfigured positioning measurement gap

maxNrOfGapPri-r17 INTEGER ::= 16 -- Maximum number of gap priority level

maxCEFReport-r17 INTEGER ::= 4 -- Maximum number of CEF reports by the UE

maxNrofMultiplePDSCHs-r17 INTEGER ::= 8 -- Maximum number of PDSCHs in PDSCH TDRA list

maxSliceInfo-r17 INTEGER ::= 8 -- Maximum number of NSAGs

maxCellSlice-r17 INTEGER ::= 16 -- Maximum number of cells supporting the NSAG

maxNrofTRS-ResourceSets-r17 INTEGER ::= 64 -- Maximum number of TRS resource sets

maxNrofSearchSpaceGroups-1-r17 INTEGER ::= 2 -- Maximum number of search space groups minus 1

maxNrofRemoteUE-r17 INTEGER ::= 32 -- Maximum number of connected L2 U2N Remote UEs

maxDCI-4-2-Size-r17 INTEGER ::= 140 -- Maximum size of DCI format 4-2

maxFreqMBS-r17 INTEGER ::= 16 -- Maximum number of MBS frequencies reported in MBSInterestIndication

maxNrofDRX-ConfigPTM-r17 INTEGER ::= 64 -- Max number of DRX configuration for PTM provided in MBS broadcast in a

-- cell

maxNrofDRX-ConfigPTM-1-r17 INTEGER ::= 63 -- Max number of DRX configuration for PTM provided in MBS broadcast in a

-- cell minus 1

maxNrofMBS-ServiceListPerUE-r17 INTEGER ::= 16 -- Maximum number of services which the UE can include in the MBS interest

-- indication

maxNrofMBS-Session-r17 INTEGER ::= 1024 -- Maximum number of MBS sessions provided in MBS broadcast in a cell

maxNrofMTCH-SSB-MappingWindow-r17 INTEGER ::= 16 -- Maximum number of MTCH to SSB beam mapping pattern

maxNrofMTCH-SSB-MappingWindow-1-r17 INTEGER ::= 15 -- Maximum number of MTCH to SSB beam mapping pattern minus 1

maxNrofMRB-Broadcast-r17 INTEGER ::= 4 -- Maximum number of broadcast MRBs configured for one MBS broadcast service

maxNrofPageGroup-r17 INTEGER ::= 32 -- Maximum number of paging groups in a paging message

maxNrofPDSCH-ConfigPTM-r17 INTEGER ::= 16 -- Maximum number of PDSCH configuration groups for PTM

maxNrofPDSCH-ConfigPTM-1-r17 INTEGER ::= 15 -- Maximum number of PDSCH configuration groups for PTM minus 1

maxG-RNTI-r17 INTEGER ::= 16 -- Maximum number of G-RNTI that can be configured for a UE.

maxG-RNTI-1-r17 INTEGER ::= 15 -- Maximum number of G-RNTI that can be configured for a UE minus 1.

maxG-CS-RNTI-r17 INTEGER ::= 8 -- Maximum number of G-CS-RNTI that can be configured for a UE.

maxG-CS-RNTI-1-r17 INTEGER ::= 7 -- Maximum number of G-CS-RNTI that can be configured for a UE minus 1.

maxMRB-r17 INTEGER ::= 32 -- Maximum number of multicast MRBs (that can be added in MRB-ToAddModLIst)

maxFSAI-MBS-r17 INTEGER ::= 64 -- Maximum number of MBS frequency selection area identities

maxNeighCellMBS-r17 INTEGER ::= 8 -- Maximum number of MBS broadcast neighbour cells

maxNrofPdcch-BlindDetectionMixed-1-r16 INTEGER ::= 7 -- Maximum number of combinations of mixed Rel-16 and Rel-15 PDCCH

-- monitoring capabilities minus 1

maxNrofPdcch-BlindDetection-r17 INTEGER ::= 16 -- Maximum number of combinations of PDCCH blind detection monitoring

-- capabilities

maxNrofThresholdMBS-r18 INTEGER ::= 8 -- Max number of thresholds of MBS sessions for RRC connection resume for a UE

-- receiving multicast in RRC\_INACTIVE

-- TAG-MULTIPLICITY-AND-TYPE-CONSTRAINT-DEFINITIONS-STOP

-- ASN1STOP

End of Change

Annex - collection of RAN2 agreements on enhancements of MBS WI

RAN2#119 agreements

* In Rel-18, multicast reception for UEs in INACTIVE supports at least the following scenarios, with the assumption that the UE already has a valid PTM configuration:

- Scenario 1: a UE has been receiving multicast in CONNECTED, and it enters INACTIVE and continues the multicast reception.

- Scenario 2: a UE has joined a multicast session and has been directed to INACTIVE, the UE starts to receive the multicast session

**FFS for state changes, e.g. due to service being not provided in INACTIVE anymore etc.**

* It is up to gNB to decide whether a multicast session may be received by UE(s) in INACTIVE. FFS what information gNB may be provided to form such decision (related to SA2 discussion).
* It is supported that gNB transmit one multicast session to both UEs in CONNECTED and INACTIVE in the same cell. FFS how the gNB configures this.
* It is assumed the network can choose which UEs receive in RRC INACTIVE and which in RRC Connected and can move UEs between the states for Multicast service reception.
* The following is taken as baseline: we assume the same PDCCH/PDSCH resources (e.g. resources used for MTCH) can be used for all UEs (including UEs in CONNECTED and/or INACTIVE states) for receiving the same multicast session. Different configuration/resources are not precluded as well. FFS what exactly can be common and what not (e.g. HARQ, SPS etc.) and what is needed in addition (to legacy PTM config).
* For PTM configuration delivery, RAN2 further investigates the following solutions:

Option 1: Dedicated signalling

Option 2: Solution based on SIB+MCCH

We do not preclude some “mix” of the options

* HARQ feedback and PTP are not supported for multicast reception in RRC\_INACTIVE.
* Multicast service continuity after cell reselection in RRC\_INACTIVE state (i.e. without resuming RRC connection) will be supported (if the configuration of the new cell is available for the UE). FFS whether there are cases where the UE needs to resume the connection. FFS RAN3 impacts due to inter-gNB mobility.
* Upon cell reselection to neighbour cells during active multicast session, if the configuration of the session is not available for the new cell for UEs in INACTIVE, then the UE is required to resume RRC connection to get the Multicast MRB configuration.
* RAN2 focuses on solutions taking multi-Rx UEs (i.e. no specific enhancements for 1Rx UEs).

RAN2#119 bis agreements

* RAN2 Answer to Q1-a) If there are significant differences in the quality and reliability of the reception of MBS data between UEs in RRC Connected state and UEs in RRC Inactive state:

The quality and reliability of the reception of MBS data between UEs in RRC\_CONNECTED state and UEs in RRC\_INACTIVE state may or may not be different, as HARQ feedback and PTP transmission are not supported and seamless/lossless mobility is not required for multicast reception in RRC\_INACTIVE.

* Revised LS to be provided for final (editorial) review
* Final LS to be provided in R2-2210882
* The following general description is taken as baseline for PTM configuration delivery Option 1:

(1-a) PTM configuration(s) (i.e., configurations used for multicast reception in RRC\_INACTIVE) of one or more multicast sessions for at least one cell are provided via dedicated RRC signaling to a UE.

(1-b) The RRC message for this includes RRCReconfiguration and/or RRCRelease and/or RRCResume (details FFS)

(1-c) UE stores the received configurations while it is in RRC\_INACTIVE, and if there is a need to update some or all the configurations, the UE is notified of such changes and may trigger RRC connection resume to obtain the updated configurations. In case of mobility in RRC\_INACTIVE, the UE triggers RRC connection resume if the configuration of the session is not available for the new cell.

* The following general description is taken as baseline for PTM configuration delivery Option 2:

(2-a) PTM configurations (i.e., configurations used for multicast reception in RRC\_INACTIVE) are provided via an MCCH-like channel (same or different as used for MBS broadcast), and information regarding MCCH scheduling is provided via SIB, FFS dedicated signalling

(2-b) UE can receive such configurations when it is in RRC\_INACTIVE, FFS whether it is allowed/needed to also receive when UE is in RRC\_CONNECTED

(2-c) If there is a need to update some or all the received configurations, UE does not need to resume RRC connection but is notified of such changes (e.g. via MCCH DCI) and obtains the updated configurations via MCCH.

* Dedicated RRC signalling (i.e. RRC release message with suspendConfig) is used for switching a multicast receiving UE from RRC\_CONNECTED to RRC\_INACTIVE and continue multicast reception (details FFS).
* For both option 1 and option 2, as a baseline, group paging can be used to switch UEs receiving multicast from RRC\_INACTIVE to RRC\_CONNECTED, and UEs continue the multicast reception in CONNECTED. FFS if there is any potential issue if Rel-17 group paging is reused. FFS if there are other cases when UE triggers resume. FFS if MCCH can also be used in case of option 2.
* FFS whether to introduce PTM configuration applicable area, i.e., the mechanism that the PTM configurations, once acquired by a UE, may apply to a certain area (i.e., a set of cells instead of a single cell).
* Rel-18 UE in INACTIVE can be informed when the session is activated (Details FFS).
* As a baseline, group paging can be used to inform Rel-18 UE(s) about the session activation (Details FFS, e.g., UE behavior when receiving such group notification).
* If a UE is in RRC\_INACTIVE and is configured to receive a multicast session in RRC\_INACTIVE, the UE may be notified when the multicast session is deactivated. FFS how (e.g., informed via group paging, MCCH, or other ways).
* Rel-17 mechanism (NAS-based indication) is applicable for multicast session release. FFS if any enhancement is needed.
* FFS how UE determines whether it can receive the multicast session in RRC\_INACTIVE or not when the session is activated, taking into account the following solutions (can further update the descriptions if needed, and several solutions may be needed, some solutions may apply only for certain configuration options)

1. When the multicast session is activated, UE can receive the multicast session in RRC\_INACTIVE if the PTM configuration used in RRC\_INACTIVE for the session is available to the UE and the UE has joined the session already (e.g., configuration provided to UE via dedicated RRC signaling or via MCCH), otherwise it goes back to RRC\_CONNECTED to receive the multicast session.

2. When the multicast session is activated, UE is indicated by group paging whether it can receive the multicast session in RRC\_INACTIVE or not (detailed signaling FFS).

3. UE is configured "whether it can receive the multicast session in RRC\_INACTIVE" by dedicated signaling before UE is released. When the multicast session is activated, UE stays in RRC\_INACTIVE or resumes RRC connection accordingly (detailed signaling FFS).

* If option 1 is supported for PTM configuration

As a baseline, group paging may be used to inform the UE when network changes the PTM configurations, and UE upon reception triggers RRC connection resume procedure to obtain the updated configurations (details of group paging can be FFS).

FFS whether and how to solve the issue in signalling/system load when a large number of UEs in the cell need PTM configuration update.

* FFS if there is an issue that a UE can obtain all the PTM configurations for a multicast service via Option 2 without/before joining the multicast session on the condition that security is enabled by service layer. And if yes FFS how to solve the issue (e.g., dedicated configuration + MCCH).
* For shared processing we adopt the following as a baseline:

1) new IE is added in system information to control whether MBSInterestIndication for shared processing can be sent or not;

2) MBSInterestIndication message content and related procedure is updated for shared processing.

* New IE to control whether MBSInterestIndication for shared processing can be sent or not is added to SIB1.
* In MBSInterestIndication, for a broadcast service that the UE is receiving or is interested to receive, at least the following information can be signalled: broadcast frequency, subcarrier spacing, and bandwidth. FFS details/exact parameters and other information. FFS in which scenarios the UE reports this information (e.g. intra-PLMN case, inter-PLMN case)
* FFS whether UE capability is needed to enable shared processing.

RAN2#120 agreements

* We will have a mixed approach and we start with the following:
  + 1. When NW configures UE to continue the multicast reception in INACTIVE state, NW provides the PTM configuration for the activated multicast session via the RRC dedicated signalling, at least for the serving cell (FFS other cases).
    2. **MCCH is used in case there is a need to indicate a PTM configuration in case there is a need for change in PTM config or during mobility beyond serving cell / gNB. FFS session status change and other indications.**
    3. **We assume that the UE can only receive multicast service after it joined the session.**
    4. **FFS whether MCCH configuration is initially provided to the UE via dedicated signalling.**

RAN2#121 agreements

* UE shall join in the multicast session before receiving multicast in RRC INACTIVE.
* If network finds it useful, the PTM configuration for the (single) serving cell can be configured to UE before the session activation, and UE stores the configuration. When session is activated, UE can receive multicast in INACTIVE state by applying the configuration without going back to RRC\_CONNECTED, if not updated by MCCH after being configured.
* When network configures UE to receive multicast in INACTIVE state, RRCRelease message with suspendconfig can be used to deliver the PTM configuration. Other dedicated RRC messages will not be used to provide PTM configuration for MBS multicast for INACTIVE.
* We introduce a new MCCH logical channel for multicast in INACTIVE (different from broadcast MCCH)
* Multicast MCCH configuration is provided via new SIB.
* Optionally, Multicast MCCH configuration for the serving cell can also be provided in dedicated signalling. Understanding is we are not optimizing mobility case because of this.
* Serving cell will not provide the PTM configuration of neighbour cells from other gNBs.
* FFS whether the network can provide PTM configuration for intra-gNB cells.
* Indicate the capability of receiving MBS broadcast from a non-serving cell. FFS whether the granularity is at FeatureSetDownlink or FeatureSetDownlinkPerCC level.
* FFS Whether to include additional information in MII can be controlled by the network. Should consider whether this would be two-step procedure or one-step procedure (e.g. having more info in SIB1)

RAN2#121bis agreements

* Similar to Rel-17 broadcast reception procedure, UE acquires new SIB and multicast MCCH to get PTM configuration after cell reselection.
* When a UE reselects to a cell for which PTM configuration is not available in multicast MCCH, the UE initiates RRC resumption procedure for an active multicast session it is interested to receive or continue receiving.
* UE may trigger RRC connection resumption if the reception quality of the multicast data is below a configured threshold, FFS how to specify the threshold/reception quality.
* Frequency prioritization may be provided to the UE for cell reselection for multicast reception in RRC\_INACTIVE, detailed mechanism on how to identify the frequency info (e.g., SAI, USD, or frequency info directly provided by network) is FFS.
* No need to define a mechanism other than the frequency prioritization, i.e., per cell based prioritization in cell re-selection, to help UE choose the right cell to camp on.
* The neighbor cell list mechanism for multicast reception in RRC\_INACTIVE may be configured e.g. it can be used by UE to resume RRC connection if service is not available in the re-selected cell by NCL, without reading MCCH in the re-selected cell, in some aspects similar to Rel-17 NCL mechanism in MBS broadcast.
* A "special UE" identified by MBS assistance information from 5GC can be released to RRC\_INACTIVE (e.g., when the session is deactivated). FFS how can network enable such UE to resume to RRC\_CONNECTED upon session activation
* Rel-18 UE can stay in RRC\_INACTIVE and start monitoring corresponding G-RNTI upon an enhanced group paging (e.g., upon session activation or data transmission resumed). Details FFS.
* For one UE already in RRC\_INACTIVE, it can stay in RRC\_INACTIVE and stop monitoring corresponding G-RNTI upon events like session deactivation/temporary no data.
* FFS which option to take: enhanced group paging or enhanced MCCH, to enable Rel-18 UE to stay in RRC\_INACTIVE and stop monitoring corresponding G-RNTI upon events like session deactivation/temporary no data.
* No additional enhancement (with regard to enhancements made for ‘deactivation/temp no data’) is needed specifically for enabling UE to stay in RRC\_INACTIVE and stop monitoring corresponding G-RNTI upon session release.
* Legacy group paging (i.e., Rel-17 group paging) can be used to resume UE to RRC\_CONNECTED state.
* Upon events like session activation/data transmission resumed, if PTM configuration is not available to UE, UE initiates RRC connection resumption.
* UE-specific paging (i.e. PagingRecordList) can be used to move specific MBS multicast UE(s) to RRC\_CONNECTED (i.e. legacy UE behavior).
* When both enhanced group paging and unicast paging are received by the UE (and targeted for this UE), the UE follows unicast Paging and goes to RRC CONNECTED.
* From the location&bandwidth and SCS configuration perspective,follow R17 MBS broadcast CFR principle (i.e. case A,C,E) to provide multicast CFR configuration in RRC\_INACTIVE.
* Multicast CFR in RRC\_INACTIVE and broadcast CFR can be configured differently. FFS whether we need to restrict that one CFR is completely contained within the other in this case (we should understand what the issue is otherwise).
* Case B and case D are not supported for multicast CFR in RRC\_INACTIVE;
* Whether multicast CFR in RRC\_CONNECTED and in RRC\_INACTIVE are different is up to NW implementation. FFS whether this causes some issues which need to be addressed.
* HARQ feedback related information in the DCI is not needed or can be ignored for multicast transmission to RRC\_INACTIVE UE. (
* The HARQ operation for multicast reception in RRC\_INACTIVE is same as the operation without HARQ feedback in RRC\_CONNECTED state.
* The multicast transmission RRC\_INACTIVE is performed via beam sweeping based on SSB index like broadcast MBS (i.e. beam information is not need in DCI.
* For MTCH, RAN2 assumes to reuse the same DCI format of R17 multicast (i.e. DCI format 4-1/4-2) for dynamic scheduling of multicast in RRC INACTIVE. RAN2 assumes for MCCH scheduling, DCI format 4-0 is used. We will ask RAN1 to confirm whether it is feasible and whether both 4-1 and 4-2 are needed.
* We will also indicate other relevant agreements to RAN1 (e.g. on beam sweeping etc.)
* On support of multicast SPS in RRC\_INACTIVE, postpone RAN2 discussion to next meeting.
* On DRX operation for multicast in RRC\_INACTIVE, take the multicast DRX as baseline. FFS handling on PTM related HARQ RTT Timer and DRX Retransmission Timer.
* The common LCID space is used for multicast MRB and unicast DRB regardless of UE RRC state (i.e. no change on the LCID table for MTCH).
* Postpone the UP discussion on L2 operation during RRC state transition until the signaling design of PTM configuration in RRCRelease message is concluded.
* Postpone the discussion on L2 operation during mobility to next RAN2 meeting.
* Including the following two issues in LS to RAN1:
  + - Issue 1: RAN1 to confirm RAN2 understanding that PDSCH aggregation is supported for multicast MTCH in RRC\_INACTIVE (as that is supported in Rel-17 multicast MTCH in RRC\_CONNECTED as well as broadcast MTCH).
    - Issue 2: RAN1 to check the feasibility of following Rel-17 CSS design for multicast MTCH and MCCH: 1) reusing the same CSS for multicast MTCH in RRC\_INACTIVE (same as multicast MTCH in RRC\_CONNECTED); 2) separate CSS for MCCH and MTCH.
* UE in RRC CONNECTED state is not required to read multicast MCCH to be able to receive multicast MBS service i.e. the UE receives the PTM configuration via dedicated signalling. This can be revisited if issues with service continuity are identified.
* Change the working agreement to the agreement below:

Agreement: The same CFR is used for multicast MCCH and MTCH. It can be revisited if there is any issue found, e.g. for RedCap UEs.

RAN2#122 agreements

* The multicast MCCH configuration takes the broadcast MCCH configuration structure (i.e., mcch-Config-r17) as baseline.
* To notify the multicast MCCH change, change notification mechanism for Rel-17 broadcast MCCH is the baseline.
* Working assumption (to be confirmed by RAN1 via pending reply LS): One bit in the MCCH DCI is used to notify the change of the multicast MCCH. We reuse the bit used for MCCH change indication from Rel-17 MBS broadcast. This does not cover session deactivation which is FFS.
* It is not supported to provide the PTM configuration of intra-gNB neighbour cells in the dedicated signalling.
* For PTM configuration structure on the multicast MCCH, Rel-17 broadcast PTM configuration structure is taken as baseline.
* As a baseline, The PTM configuration in the RRCRelease message with suspendconfig has the same structure as the PTM configuration in multicast MCCH.
* FFS how existing MRBs are handled.
* Introduce a new indication per tmgi in the group paging which informs Rel-18 UEs having a valid PTM configuration to receive the multicast in RRC\_INACTIVE.
* MCCH is used for notifying MC session deactivation for multicast reception in RRC\_INACTIVE to enable Rel-18 UE to stay in RRC\_INACTIVE and stop monitoring corresponding G-RNTI.
* This is assumed to have no/minor impact on RAN1/PHY
* The granularity for capability of receiving MBS broadcast from a non-serving cell is at FeatureSetDownlinkPerCC level. This capability does not imply simultaneous reception on multiple CCs.
* No additional signalling is introduced to control information to be reported by the UE (on top of what we have already agreed).
* When sending MII, UE reports the whole information (i.e. at least frequency, bandwidth, SCS) when indicated by SIB1 of its unicast serving cell. FFS whether there are cases where this information is not available at the UE and what happens then.
* FFS if any special handling is needed when the non-serving cell updates the configuration (which is relevant for MII)
* No additional information is added to MII on top of what has been already agreed.

RAN2#123 agreements

* For a UE receiving multicast in RRC\_INACTIVE, the UE resumes the RRC connection when the measured RSRP or RSRQ based on the existing measurement requirements (whichever is configured by the NW) of the serving cell becomes lower than the threshold configured by network. FFS whether/how we need to address ping-pong issue
* The threshold can be configured in PTM configuration per MBS session via RRCRelease or multicast MCCH message.
* Unless issues are identified with using one of existing resume causes, no new resume causes are introduced for UEs receiving MC in INACTIVE when they resume due to bad quality or lack of SIBx/PTM configuration
* Dedicated frequencies in RRCRelease can be used by the NW, as legacy
* FFS whether we need something more, e.g. frequency priorities in MCCH or a solution based on FSAI
* NW indicates which multicast service can be received in INACTIVE in suspendConfig of RRC Release. FFS how exactly this is indicated
* Unless blocking issues are identified, UE behaviour is not to suspend corresponding multicast MRBs and to keep using them in INACTIVE
* For “non-synchronised“ cell (in terms of PDCP COUNT), upon cell reselection, UE sets the initial PDCP count of the MRB for the multicast reception in RRC\_INACTIVE state based on the same mechanism as R17 MBS broadcast.
* One cell can indicate "synchronized", if by implementation, it follows a common QoS flow to MRB mapping rule and at the same time PDCP COUNT is set according to the MBS QoS Flow SN.
* FFS how the UE is indicated about cells being synchronized (i.e. what information the NW needs to provide to the UE)
* Solutions which require COUNT broadcasting via MCCH are not considered
* SPS is not supported for multicast reception in RRC\_INACTIVE.
* RAN2 enables RRC\_INACTIVE UE receiving multicast to also receive possible PTM retransmissions initiated by UEs receiving multicast in RRC\_CONNECTED.
* Allow configuration of drx-HARQ-RTT-TimerDL-PTM and drx-RetransmissionTimerDL-PTM for INACTIVE UEs (38.331).
* UE receiving MBS multicast in RRC\_INACTIVE should start drx-HARQ-RTT-TimerDL-PTM and drx-RetransmissionTimerDL-PTM when reception of the transport block has not been successful. FFS the details, e.g. when the timers are started exactly.
* This is optional UE capability
* As per the previous agreement, if the UE is able to get the additional information (i.e. its current configuration does not prevent it from doing so), the UE shall do this (if capable and configured by the network)
* In case additional information (SCS, bandwidth) is not available at the time of sending the MII to the unicast serving cell (e.g. the UE is not able to read SIB1 from the non-serving cell), the UE reports whatever is available information at that time (i.e. at least the frequency, and optionally SCS and/or BW as available).
* UE reports updated MII after acquiring additional information from the non-serving cell (if previously it reported only frequency) or if the information in the non-serving cell changes.
* The SCS in the MII is set to the SCS of the CORESET#0 for the MBS broadcast cell.
* Combination of FreqBandIndicatorNR and ARFCN-ValueNR is used to signal the frequency information in the MII for shared processing.
* At least CFR bandwidth is reported by the UE in MII. FFS whether “location” needs to be also reported and how exactly this is captured in RRC (i.e. which IE is used).

RAN2#123bis agreements

* For multicast in INACTIVE, the capability for PTM retransmission reception with HARQ disabled (i.e. starting drx-HARQ-RTT-TimerDL-PTM and drx-RetransmissionTimerDL-PTM) is signalled per UE, no FDD-TDD DIFF, and no FR1-FR2 DIFF.
* RAN2 assumes to support FDMed between multicast MCCH and PBCH in a slot (check with RAN1).
* Introduce an explicit indication in the multicast MCCH/RRCRelease(i.e., in the IE MBSMulticastConfiguration) for the UE to stop G-RNTI monitoring. It is used for notification triggered by the multicast session deactivation or the temporary no data.
* UE in RRC\_INACTIVE does not need to monitor multicast MCCH DCI in the current cell until next group paging is received if UE is notified “the stop of G-RNTI monitoring” for all the joined multicast sessions, including the following cases,
  + - Case 1: UE is receiving multicast in RRC\_INACTIVE and then is notified about the session deactivation via MCCH.
    - Case 2: UE transits from RRC\_CONNECTED to RRC\_INACTIVE, and “the stop of G-RNTI monitoring” is indicated in RRCRelease message.
* If UE receives PTM configuration of multicast session(s) in RRCRelease and “the stop of G-RNTI monitoring” is indicated for the corresponding session(s) and then UE selects the same cell as on which it received RRCRelease, UE starts to monitor MCCH DCI upon receiving group paging that indicates to allow the multicast reception in RRC\_INACTIVE.
* If “the stop of G-RNTI monitoring” for a session is indicated in RRCRelease message and the PTM configuration of the corresponding multicast session is not included in same message , UE reads multicast MCCH(if present) upon receiving group paging that indicates to allow the multicast reception in RRC\_INACTIVE.
* If the whole Rel-18 multicast related configuration is absent in RRC Release, UE behaves the same as Rel-17 MBS UE.
* If the session is active and UE receives PTM configuration in RRCRelease message and then UE selects the same cell as it received RRCRelease, UE does not perform Multicast MCCH information acquisition immediately but starts to monitor MCCH DCI for possible change notification after transiting to INACTIVE.
* FFS UE in RRC\_INACTIVE reads MCCH(if present) on the reselected cell after cell reselection to acquire the PTM configuration session if UE received“the stop of G-RNTI monitoring” indication for the session.
* FFS If UE receives PTM configuration of multicast session(s) in RRCRelease and “the stop of G-RNTI monitoring” is indicated for the corresponding session(s) and then UE selects the same cell as on which it received RRCRelease, UE acquires the PTM configuration from MCCH (if present) upon receiving group paging that indicates to allow the multicast reception in RRC\_INACTIVE. FFS if the UE uses the configuration from RRCRelease until having read the one from MCCH
* FFS whether there can be case where MCCH is not present
* If UE in RRC\_INACTIVE received “the stop of G-RNTI monitoring” indication for the session in the source cell, the UE reads MCCH(if present) in the reselected cell after cell reselection.
* If UE receives PTM configuration of multicast session(s) in RRCRelease and “the stop of G-RNTI monitoring” is indicated for all of the the corresponding session(s) and if UE selects the same cell as on which it received RRCRelease, UE acquires the PTM configuration from MCCH (if present) upon receiving group paging that indicates to allow the multicast reception in RRC\_INACTIVE.
* UE can use the PTM configuration from RRCRelease until having read the one from MCCH.
* Multicast MCCH can be optionally present for a cell providing multicast reception in RRC\_INACTIVE. We do not optimize for this in RAN2, e.g. we are targeting a single cell scenario without mobility and without PTM configuration update for optional MCCH.
* The RSRP/RSRQ measurement as specified in TS 38.304 are reused (i.e. no new measurements and measurement requirements).
* No TTT is introduced
* All MRBs corresponding to the same multicast session to be received in RRC\_INACTIVE should be continued.
* MRB ID is not configured in PTM configuration for multicast in INACTIVE. FFS if anything is needed.
* mt-Access is selected for multicast reception when it is applicable to the legacy mt-Access use case (i.e. it is not applicable to access identities 1, 2 and 11-15).
* UE selects '0' as the Access Category when the resumption of the RRC connection is triggered for multicast reception.
* A UE starts the drx-HARQ-RTT-TimerDL-PTM for the corresponding HARQ process in the first symbol after the end of the corresponding multicast transmission.
* Potential agreement: A 1-bit indication on cell PDCP COUNT synchronization for an MBS service is present with the INACTIVE MRB PTM configuration provided in RRCRelease/MCCH. FFS whether the indication is for RNA or another area.
* Offline ZTE to understand whether there are concerns with the above and clarify how it works in detail
* A 1-bit indication on cell PDCP COUNT synchronization for an MBS service is present with the INACTIVE MRB PTM configuration provided in RRCRelease, and cells in the RNA area are synchronized for PDCP COUNT.
* UE initiates the MII reporting for the non-serving cell upon stopping the reception of all the broadcast services that UE were receiving on a non-serving cell (TP in [R2-2309559](file:///D:\3GPP\Extracts\R2-2309559%20Remaining%20Issues%20on%20Shared%20Processing.docx) can be taken as baseline).
* For Rel-18 MII reporting, frequency of interest determination is amended to add a condition that at least one of the MBS sessions is from non-serving cell for the concerned frequency included in SIB21 from the non-serving cell and/or USD (TP in [R2-2310088](file:///D:\3GPP\Extracts\R2-2310088%20Shared%20processing%20for%20broadcast%20and%20unicast%20reception.docx) can be taken as baseline).
* For MII for shared processing, *FreqInfoMBS* in the running CR refers to the frequency information obtained from the USD or the SIB21 (i.e. same understanding as Rel-17).
* For MII for shared processing, signalling will support reporting CFR location & BW (i.e. actual value of *locationAndBandwidthBroadcast-r17* encoded as INTEGER (0..37949)) as well as point A of non-serving cell, i.e. information enough to point to the exact location of CFR, if available at the UE. It is an optional IE in MII.

RAN2#124 agreements

* If not captured already properly, we can clarify in stage-2 specs that the UE can only receive MCCH with multicast configurations after joining multicast session.
* If not captured already properly, in the next revision we will capture in RRC that UE can use PTM configuration from RRC Release until it receives the one from MCCH.
* DRX Command MAC CE is applicable for inactive multicast DRX operation.
* Remove EN1 in section 5.7b of running MAC CR for eMBS.
* Introduce a new fix RNTI value for Multicast MCCH-RNTI.
* We will call the new RNTI: “multicast MCCH-RNTI” (we align also in other specs)
* The same LCID value is used for multicast MCCH and broadcast MCCH.
* Remove the Editor Note 1 in section 5.3.1 of MAC running CR.
* Clarify in MAC specs section 5.8.1a only applies to UEs in RRC CONNECTED.
* In the next revision, draft UE capas CR drafting rules should be applied, as requested by the mega CR rapporteur
* In the next revision, draft UE capas CR drafting rules should be applied, as requested by the mega CR rapporteur
* As a baseline, a UE supporting multicast reception in RRC\_INACTIVE state also supports the following components:
* - 12-bit length of PDCP sequence number;
* - ROHC profiles 0x0000, 0x0001, and 0x0002;
* - 4 ROHC header compression context sessions as the minimum number;
* - UM MRB with 12-bit length of RLC sequence number;
* - UM MRB with 6-bit length of RLC sequence number.
* Offline if anything else needs to be captured for a minimum capability or if any other capabilities are needed (vivo)
* Capabilities maxMRB-Add-r17 and maxNumberG-RNTI-r17 are also applicable to multicast reception in RRC INACTIVE state.
* FFS whether the functionality of RRC connection resumption triggering due to the reception quality below the configured threshold is mandatory/optional capability.
* Support the simultaneous configuration of SDT and MBS multicast reception in RRC\_INACTIVE to one UE, unless serious issues are identified during implementation in the CR.
* MRB cannot be configured as SDT bearer.
* The UE is not required to monitor group Paging during SDT procedure.
* The understanding is NW can send the UE directly to INACTIVE with PTM config for MC in INACTIVE.
* In a “synced” RNA area, the order of MRBs within the same session configuration in the source and target cells’ MCCH messages should be consistent.
* For transition from RRC CONNECTED to RRC INACTIVE, the same LCIDs are used for the same MRBs if UE continues in the same cell from which it received RRCRelease.
* Offline on different cell case and RRC INACTIVE to CONNECTED transition (ZTE)
* MRB continuity is guaranteed only when the UE transits from RRC CONNECTED to RRC INACTIVE in the same cell.
* Understanding is the UE uses the latest available measurement for condition evaluation, no need to capture special cases. Check whether this requires some spec changes, e.g. a NOTE.
* NW should be able to configure eLCID for multicast MRB in RRC\_INACTIVE, similar as in Rel-17.
* The max number of thresholds for resume is set to 8.
* For RRC\_INACTIVE, when Multicast CFR for RRC\_INACTIVE and broadcast CFR are configured differently, if one CFR is not completely contained within the other CFR, then UE is not required to receive both broadcast and multicast simultaneously.
* If multicast CFR for RRC\_INACTIVE is not configured, the default is same as CORESET#0 (check whether/not already captured in the running CR).
* Upon transition to RRC\_INACTIVE from RRC\_CONNECTED, MAC is reset (including flushing of soft buffer for HARQ process used for multicast reception in RRC\_INACTIVE). No spec impact is expected.
* Upon cell reselection, MAC is reset (including flushing of soft buffer for HARQ process used for multicast reception in RRC\_INACTIVE). There may be impact to RRC spec (to indicate the MAC reset).
* Upon transition to RRC\_INACTIVE from RRC\_CONNECTED, MAC is reset (including stopping of drx-HARQ-RTT-TimerDL-PTM and drx-RetransmissionTimerDL-PTM, if running). No spec impact is expected.