**3GPP TSG-RAN2 Meeting #125 *draft R2-2401609***

**Athens, Greece, 26th Feb 2024 - 1st Mar 2024**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **38.331** | **CR** | **draftCR** | **rev** | **-** | **Current version:** | **18.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | UE capability corrections for NR Support for UAV (Uncrewed Aerial Vehicles) |
|  |  |
| ***Source to WG:*** | Qualcomm Incorporated |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | NR\_UAV-Core |  | ***Date:*** | 2024-03-06 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | UE capability corrections for NR UAV WI |
|  |  |
| ***Summary of change:*** |  Following agreements from RAN2#125 are captured (i.e. Editor’s Notes are removed)**Agreements:**1. <<skip>>
2. For both NR and LTE: Introduce optional per UE capability to indicate support of the mechanisms defined for cells broadcasting aerial-specific emission list. For nr-NS-PmaxListAerial-r18, keep it as per-UE optional capability (both LTE and NR) with No FDD/TDD diff and No FR1/FR2 diff. Remove Editor’s Note. Also capture description in TS 38.306.
3. sl-A2X-Service-r18 capability is per UE. This implies that the UE doesn’t support both SL V2X/ProSe and A2X, but can be revisited when there is a need to support both.
 |
|  |  |
| ***Consequences if not approved:*** | NR UAV UE capability specifications remain ambiguous with Editor’s Notes |
|  |  |
| ***Clauses affected:*** | 6.3.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **X** |  |  Other core specifications  | TS 38.331 CR 4563  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This draftCR is merged in capability mega CR 4638 in R2-2401691. |
|  |  |
| ***This CR's revision history:*** |  |

Start of Changes

### 6.3.3 UE capability information elements

<<unchaged text skipped>>

#### – *AerialParameters*

The IE *AerialParameters* is used to convey the capabilities supported by the UE for aerial operation.

*AerialParameters* information element

-- ASN1START

-- TAG-AERIALPARAMETERS-START

AerialParameters-r18 ::= SEQUENCE {

 -- Support of Aerial UE features

 aerialUE-Capability-r18 ENUMERATED {supported} OPTIONAL,

 -- Support of altitude measurement and event H1/H2-triggered reporting

 altitudeMeas-r18 ENUMERATED {supported} OPTIONAL,

 -- Support of altitude based measurement configuration of SSB-ToMeasure

 altitudeBasedSSB-ToMeasure-r18 ENUMERATED {supported} OPTIONAL,

 -- Support of events A3H1, A3H2, A4H1, A4H2, A5H1, A5H2

 eventAxHy-r18 ENUMERATED {supported} OPTIONAL,

 -- Support of flight path reporting

 flightPathReporting-r18 ENUMERATED {supported} OPTIONAL,

 -- Support of flight path availability indication via UAI

 flightPathAvailabilityIndicationUAI-r18 ENUMERATED {supported} OPTIONAL,

 -- Support of numberOfTriggeringCells for eventA3, eventA4, and eventA5, and additionally, if the UE supports eventAxHy-r18,

 -- support of numberOfTriggeringCells for eventA3H1, eventA3H2, eventA4H1, eventA4H2, eventA5H1, and eventA5H2

 multipleCellsMeasExtension-r18 ENUMERATED {supported} OPTIONAL,

 -- Support of handling aerial-specific Ns value(s) and Pmax list broadcasted by the cell

 nr-NS-PmaxListAerial-r18 ENUMERATED {supported} OPTIONAL,

 -- Support of reporting only the measurement report corresponding to the event with the smallest value between the

 -- altitude of the UAV and the altitude threshold for which the altitude-related entering condition e.g. A3H1-2 is satisfied, when

 -- multiple events of the same type (Hx or AxHy) for the same MO (for AxHy) are triggered simultaneously.

 simulMultiTriggerSingleMeasReport-r18 ENUMERATED {supported} OPTIONAL,

 -- Support of A2X service(s) using PC5 Sidelink and dedicated resource pool for A2X service(s)

 sl-A2X-Service-r18 ENUMERATED {brid, daa, bridAndDAA} OPTIONAL,

 ...

}

-- TAG-AERIALPARAMETERS-STOP

-- ASN1STOP

<<unchaged text skipped>>

End of Changes