**3GPP TSG-RAN WG2 Meeting #125 *R2-230xxxx***

**Athens, Greece, February 26th – March 1st, 2024**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.331** | **CR** | **-** | **rev** | **-** | **Current version:** | **18.0.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Updates to UE capabilities for Rel-18 NR NTN Enh. | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Intel Corporation | | | | | | | | | |
| ***Source to TSG:*** | R2 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_NTN\_enh-Core | | | | |  | ***Date:*** | | | 2024-03-07 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Updates to UE capabilities for Rel-18 NR NTN Enh. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | 1. Define a new UE capability for *ntn-VSAT-AntennaType-r18*. 2. Define a new UE capability for *ntn-VSAT-MobilityType-r18*. 3. Define a new UE capability for *eventD2-MeasReportTrigger-r18*. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | NR NTN Enh. WI is not completed. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 6.3.3 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | | **x** |  | Other core specifications | | | | TS/TR 38.306 CR ... | | |
| ***affected:*** | |  | **xx** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  |  | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

1. ***Modified section***

### 6.3.3 UE capability information elements

\*\*\* OMITTED TEXT \*\*\*

#### – *MeasAndMobParameters*

The IE *MeasAndMobParameters* is used to convey UE capabilities related to measurements for radio resource management (RRM), radio link monitoring (RLM) and mobility (e.g. handover).

*MeasAndMobParameters* information element

-- ASN1START

-- TAG-MEASANDMOBPARAMETERS-START

MeasAndMobParameters ::= SEQUENCE {

measAndMobParametersCommon MeasAndMobParametersCommon OPTIONAL,

measAndMobParametersXDD-Diff MeasAndMobParametersXDD-Diff OPTIONAL,

measAndMobParametersFRX-Diff MeasAndMobParametersFRX-Diff OPTIONAL

}

MeasAndMobParameters-v1700 ::= SEQUENCE {

measAndMobParametersFR2-2-r17 MeasAndMobParametersFR2-2-r17 OPTIONAL

}

MeasAndMobParametersCommon ::= SEQUENCE {

supportedGapPattern BIT STRING (SIZE (22)) OPTIONAL,

ssb-RLM ENUMERATED {supported} OPTIONAL,

ssb-AndCSI-RS-RLM ENUMERATED {supported} OPTIONAL,

...,

[[

eventB-MeasAndReport ENUMERATED {supported} OPTIONAL,

handoverFDD-TDD ENUMERATED {supported} OPTIONAL,

eutra-CGI-Reporting ENUMERATED {supported} OPTIONAL,

nr-CGI-Reporting ENUMERATED {supported} OPTIONAL

]],

[[

independentGapConfig ENUMERATED {supported} OPTIONAL,

periodicEUTRA-MeasAndReport ENUMERATED {supported} OPTIONAL,

handoverFR1-FR2 ENUMERATED {supported} OPTIONAL,

maxNumberCSI-RS-RRM-RS-SINR ENUMERATED {n4, n8, n16, n32, n64, n96} OPTIONAL

]],

[[

nr-CGI-Reporting-ENDC ENUMERATED {supported} OPTIONAL

]],

[[

eutra-CGI-Reporting-NEDC ENUMERATED {supported} OPTIONAL,

eutra-CGI-Reporting-NRDC ENUMERATED {supported} OPTIONAL,

nr-CGI-Reporting-NEDC ENUMERATED {supported} OPTIONAL,

nr-CGI-Reporting-NRDC ENUMERATED {supported} OPTIONAL

]],

[[

reportAddNeighMeasForPeriodic-r16 ENUMERATED {supported} OPTIONAL,

condHandoverParametersCommon-r16 SEQUENCE {

condHandoverFDD-TDD-r16 ENUMERATED {supported} OPTIONAL,

condHandoverFR1-FR2-r16 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

nr-NeedForGap-Reporting-r16 ENUMERATED {supported} OPTIONAL,

supportedGapPattern-NRonly-r16 BIT STRING (SIZE (10)) OPTIONAL,

supportedGapPattern-NRonly-NEDC-r16 ENUMERATED {supported} OPTIONAL,

maxNumberCLI-RSSI-r16 ENUMERATED {n8, n16, n32, n64} OPTIONAL,

maxNumberCLI-SRS-RSRP-r16 ENUMERATED {n4, n8, n16, n32} OPTIONAL,

maxNumberPerSlotCLI-SRS-RSRP-r16 ENUMERATED {n2, n4, n8} OPTIONAL,

mfbi-IAB-r16 ENUMERATED {supported} OPTIONAL,

dummy ENUMERATED {supported} OPTIONAL,

nr-CGI-Reporting-NPN-r16 ENUMERATED {supported} OPTIONAL,

idleInactiveEUTRA-MeasReport-r16 ENUMERATED {supported} OPTIONAL,

idleInactive-ValidityArea-r16 ENUMERATED {supported} OPTIONAL,

eutra-AutonomousGaps-r16 ENUMERATED {supported} OPTIONAL,

eutra-AutonomousGaps-NEDC-r16 ENUMERATED {supported} OPTIONAL,

eutra-AutonomousGaps-NRDC-r16 ENUMERATED {supported} OPTIONAL,

pcellT312-r16 ENUMERATED {supported} OPTIONAL,

supportedGapPattern-r16 BIT STRING (SIZE (2)) OPTIONAL

]],

[[

-- R4 19-2 Concurrent measurement gaps

concurrentMeasGap-r17 CHOICE {

concurrentPerUE-OnlyMeasGap-r17 ENUMERATED {supported},

concurrentPerUE-PerFRCombMeasGap-r17 ENUMERATED {supported}

} OPTIONAL,

-- R4 19-1 Network controlled small gap (NCSG)

nr-NeedForGapNCSG-Reporting-r17 ENUMERATED {supported} OPTIONAL,

eutra-NeedForGapNCSG-Reporting-r17 ENUMERATED {supported} OPTIONAL,

-- R4 19-1-1 per FR Network controlled small gap (NCSG)

ncsg-MeasGapPerFR-r17 ENUMERATED {supported} OPTIONAL,

-- R4 19-1-2 Network controlled small gap (NCSG) supported patterns

ncsg-MeasGapPatterns-r17 BIT STRING (SIZE(24)) OPTIONAL,

-- R4 19-1-3 Network controlled small gap (NCSG) supported NR-only patterns

ncsg-MeasGapNR-Patterns-r17 BIT STRING (SIZE(24)) OPTIONAL,

-- R4 19-3-2 pre-configured measurement gap

preconfiguredUE-AutonomousMeasGap-r17 ENUMERATED {supported} OPTIONAL,

-- R4 19-3-1 pre-configured measurement gap

preconfiguredNW-ControlledMeasGap-r17 ENUMERATED {supported} OPTIONAL,

handoverFR1-FR2-2-r17 ENUMERATED {supported} OPTIONAL,

handoverFR2-1-FR2-2-r17 ENUMERATED {supported} OPTIONAL,

-- RAN4 14-1: per-FR MG for PRS measurement

independentGapConfigPRS-r17 ENUMERATED {supported} OPTIONAL,

rrm-RelaxationRRC-ConnectedRedCap-r17 ENUMERATED {supported} OPTIONAL,

-- R4 25-3: Parallel measurements with multiple measurement gaps

parallelMeasurementGap-r17 ENUMERATED {n2} OPTIONAL,

condHandoverWithSCG-NRDC-r17 ENUMERATED {supported} OPTIONAL,

gNB-ID-LengthReporting-r17 ENUMERATED {supported} OPTIONAL,

gNB-ID-LengthReporting-ENDC-r17 ENUMERATED {supported} OPTIONAL,

gNB-ID-LengthReporting-NEDC-r17 ENUMERATED {supported} OPTIONAL,

gNB-ID-LengthReporting-NRDC-r17 ENUMERATED {supported} OPTIONAL,

gNB-ID-LengthReporting-NPN-r17 ENUMERATED {supported} OPTIONAL

]],

[[

-- R4 25-1: Parallel measurements on multiple SMTC-s for a single frequency carrier

parallelSMTC-r17 ENUMERATED {n4} OPTIONAL,

-- R4 19-2-1 Concurrent measurement gaps for EUTRA

concurrentMeasGapEUTRA-r17 ENUMERATED {supported} OPTIONAL,

serviceLinkPropDelayDiffReporting-r17 ENUMERATED {supported} OPTIONAL,

-- R4 19-1-4 Network controlled small gap (NCSG) performing measurement based on flag deriveSSB-IndexFromCellInter

ncsg-SymbolLevelScheduleRestrictionInter-r17 ENUMERATED {supported} OPTIONAL

]],

[[

eventD1-MeasReportTrigger-r17 ENUMERATED {supported} OPTIONAL,

independentGapConfig-maxCC-r17 SEQUENCE {

fr1-Only-r17 INTEGER (1..32) OPTIONAL,

fr2-Only-r17 INTEGER (1..32) OPTIONAL,

fr1-AndFR2-r17 INTEGER (1..32) OPTIONAL

} OPTIONAL

]],

[[

interSatMeas-r17 ENUMERATED {supported} OPTIONAL,

deriveSSB-IndexFromCellInterNon-NCSG-r17 ENUMERATED {supported} OPTIONAL

]],

[[

-- R4 31-1 Enhanced L3 measurement reporting for unknown SCell activation if the valid L3 measurement results are available

l3-MeasUnknownSCellActivation-r18 ENUMERATED {supported} OPTIONAL,

-- R4 31-3 Shorter measurement interval for unknown SCell activation

shortMeasInterval-r18 ENUMERATED {supported} OPTIONAL,

nr-NeedForInterruptionReport-r18 ENUMERATED {supported} OPTIONAL,

measSequenceConfig-r18 ENUMERATED {supported} OPTIONAL,

cellIndividualOffsetPerMeasEvent-r18 ENUMERATED {supported} OPTIONAL,

eventD2-MeasReportTrigger-r18 ENUMERATED {supported} OPTIONAL ]]

}

MeasAndMobParametersXDD-Diff ::= SEQUENCE {

intraAndInterF-MeasAndReport ENUMERATED {supported} OPTIONAL,

eventA-MeasAndReport ENUMERATED {supported} OPTIONAL,

...,

[[

handoverInterF ENUMERATED {supported} OPTIONAL,

handoverLTE-EPC ENUMERATED {supported} OPTIONAL,

handoverLTE-5GC ENUMERATED {supported} OPTIONAL

]],

[[

sftd-MeasNR-Neigh ENUMERATED {supported} OPTIONAL,

sftd-MeasNR-Neigh-DRX ENUMERATED {supported} OPTIONAL

]],

[[

dummy ENUMERATED {supported} OPTIONAL

]]

}

MeasAndMobParametersFRX-Diff ::= SEQUENCE {

ss-SINR-Meas ENUMERATED {supported} OPTIONAL,

csi-RSRP-AndRSRQ-MeasWithSSB ENUMERATED {supported} OPTIONAL,

csi-RSRP-AndRSRQ-MeasWithoutSSB ENUMERATED {supported} OPTIONAL,

csi-SINR-Meas ENUMERATED {supported} OPTIONAL,

csi-RS-RLM ENUMERATED {supported} OPTIONAL,

...,

[[

handoverInterF ENUMERATED {supported} OPTIONAL,

handoverLTE-EPC ENUMERATED {supported} OPTIONAL,

handoverLTE-5GC ENUMERATED {supported} OPTIONAL

]],

[[

maxNumberResource-CSI-RS-RLM ENUMERATED {n2, n4, n6, n8} OPTIONAL

]],

[[

simultaneousRxDataSSB-DiffNumerology ENUMERATED {supported} OPTIONAL

]],

[[

nr-AutonomousGaps-r16 ENUMERATED {supported} OPTIONAL,

nr-AutonomousGaps-ENDC-r16 ENUMERATED {supported} OPTIONAL,

nr-AutonomousGaps-NEDC-r16 ENUMERATED {supported} OPTIONAL,

nr-AutonomousGaps-NRDC-r16 ENUMERATED {supported} OPTIONAL,

dummy ENUMERATED {supported} OPTIONAL,

cli-RSSI-Meas-r16 ENUMERATED {supported} OPTIONAL,

cli-SRS-RSRP-Meas-r16 ENUMERATED {supported} OPTIONAL,

interFrequencyMeas-NoGap-r16 ENUMERATED {supported} OPTIONAL,

simultaneousRxDataSSB-DiffNumerology-Inter-r16 ENUMERATED {supported} OPTIONAL,

idleInactiveNR-MeasReport-r16 ENUMERATED {supported} OPTIONAL,

-- R4 6-2: Support of beam level Early Measurement Reporting

idleInactiveNR-MeasBeamReport-r16 ENUMERATED {supported} OPTIONAL

]],

[[

increasedNumberofCSIRSPerMO-r16 ENUMERATED {supported} OPTIONAL

]]

}

MeasAndMobParametersFR2-2-r17 ::= SEQUENCE {

handoverInterF-r17 ENUMERATED {supported} OPTIONAL,

handoverLTE-EPC-r17 ENUMERATED {supported} OPTIONAL,

handoverLTE-5GC-r17 ENUMERATED {supported} OPTIONAL,

idleInactiveNR-MeasReport-r17 ENUMERATED {supported} OPTIONAL,

...

}

-- TAG-MEASANDMOBPARAMETERS-STOP

-- ASN1STOP

\*\*\* OMITTED TEXT \*\*\*

1. ***Modified section***

#### – *UE-NR-Capability*

The IE *UE-NR-Capability* is used to convey the NR UE Radio Access Capability Parameters, see TS 38.306 [26].

*UE-NR-Capability* information element

-- ASN1START

-- TAG-UE-NR-CAPABILITY-START

UE-NR-Capability ::= SEQUENCE {

accessStratumRelease AccessStratumRelease,

pdcp-Parameters PDCP-Parameters,

rlc-Parameters RLC-Parameters OPTIONAL,

mac-Parameters MAC-Parameters OPTIONAL,

phy-Parameters Phy-Parameters,

rf-Parameters RF-Parameters,

measAndMobParameters MeasAndMobParameters OPTIONAL,

fdd-Add-UE-NR-Capabilities UE-NR-CapabilityAddXDD-Mode OPTIONAL,

tdd-Add-UE-NR-Capabilities UE-NR-CapabilityAddXDD-Mode OPTIONAL,

fr1-Add-UE-NR-Capabilities UE-NR-CapabilityAddFRX-Mode OPTIONAL,

fr2-Add-UE-NR-Capabilities UE-NR-CapabilityAddFRX-Mode OPTIONAL,

featureSets FeatureSets OPTIONAL,

featureSetCombinations SEQUENCE (SIZE (1..maxFeatureSetCombinations)) OF FeatureSetCombination OPTIONAL,

lateNonCriticalExtension OCTET STRING (CONTAINING UE-NR-Capability-v15c0) OPTIONAL,

nonCriticalExtension UE-NR-Capability-v1530 OPTIONAL

}

-- Regular non-critical Rel-15 extensions:

UE-NR-Capability-v1530 ::= SEQUENCE {

fdd-Add-UE-NR-Capabilities-v1530 UE-NR-CapabilityAddXDD-Mode-v1530 OPTIONAL,

tdd-Add-UE-NR-Capabilities-v1530 UE-NR-CapabilityAddXDD-Mode-v1530 OPTIONAL,

dummy ENUMERATED {supported} OPTIONAL,

interRAT-Parameters InterRAT-Parameters OPTIONAL,

inactiveState ENUMERATED {supported} OPTIONAL,

delayBudgetReporting ENUMERATED {supported} OPTIONAL,

nonCriticalExtension UE-NR-Capability-v1540 OPTIONAL

}

UE-NR-Capability-v1540 ::= SEQUENCE {

sdap-Parameters SDAP-Parameters OPTIONAL,

overheatingInd ENUMERATED {supported} OPTIONAL,

ims-Parameters IMS-Parameters OPTIONAL,

fr1-Add-UE-NR-Capabilities-v1540 UE-NR-CapabilityAddFRX-Mode-v1540 OPTIONAL,

fr2-Add-UE-NR-Capabilities-v1540 UE-NR-CapabilityAddFRX-Mode-v1540 OPTIONAL,

fr1-fr2-Add-UE-NR-Capabilities UE-NR-CapabilityAddFRX-Mode OPTIONAL,

nonCriticalExtension UE-NR-Capability-v1550 OPTIONAL

}

UE-NR-Capability-v1550 ::= SEQUENCE {

reducedCP-Latency ENUMERATED {supported} OPTIONAL,

nonCriticalExtension UE-NR-Capability-v1560 OPTIONAL

}

UE-NR-Capability-v1560 ::= SEQUENCE {

nrdc-Parameters NRDC-Parameters OPTIONAL,

receivedFilters OCTET STRING (CONTAINING UECapabilityEnquiry-v1560-IEs) OPTIONAL,

nonCriticalExtension UE-NR-Capability-v1570 OPTIONAL

}

UE-NR-Capability-v1570 ::= SEQUENCE {

nrdc-Parameters-v1570 NRDC-Parameters-v1570 OPTIONAL,

nonCriticalExtension UE-NR-Capability-v1610 OPTIONAL

}

-- Late non-critical Rel-15 extensions:

UE-NR-Capability-v15c0 ::= SEQUENCE {

nrdc-Parameters-v15c0 NRDC-Parameters-v15c0 OPTIONAL,

partialFR2-FallbackRX-Req ENUMERATED {true} OPTIONAL,

nonCriticalExtension UE-NR-Capability-v15g0 OPTIONAL

}

UE-NR-Capability-v15g0 ::= SEQUENCE {

rf-Parameters-v15g0 RF-Parameters-v15g0 OPTIONAL,

nonCriticalExtension UE-NR-Capability-v15j0 OPTIONAL

}

UE-NR-Capability-v15j0 ::= SEQUENCE {

-- Following field is only for REL-15 late non-critical extensions

lateNonCriticalExtension OCTET STRING OPTIONAL,

nonCriticalExtension UE-NR-Capability-v16a0 OPTIONAL

}

-- Regular non-critical Rel-16 extensions:

UE-NR-Capability-v1610 ::= SEQUENCE {

inDeviceCoexInd-r16 ENUMERATED {supported} OPTIONAL,

dl-DedicatedMessageSegmentation-r16 ENUMERATED {supported} OPTIONAL,

nrdc-Parameters-v1610 NRDC-Parameters-v1610 OPTIONAL,

powSav-Parameters-r16 PowSav-Parameters-r16 OPTIONAL,

fr1-Add-UE-NR-Capabilities-v1610 UE-NR-CapabilityAddFRX-Mode-v1610 OPTIONAL,

fr2-Add-UE-NR-Capabilities-v1610 UE-NR-CapabilityAddFRX-Mode-v1610 OPTIONAL,

bh-RLF-Indication-r16 ENUMERATED {supported} OPTIONAL,

directSN-AdditionFirstRRC-IAB-r16 ENUMERATED {supported} OPTIONAL,

bap-Parameters-r16 BAP-Parameters-r16 OPTIONAL,

referenceTimeProvision-r16 ENUMERATED {supported} OPTIONAL,

sidelinkParameters-r16 SidelinkParameters-r16 OPTIONAL,

highSpeedParameters-r16 HighSpeedParameters-r16 OPTIONAL,

mac-Parameters-v1610 MAC-Parameters-v1610 OPTIONAL,

mcgRLF-RecoveryViaSCG-r16 ENUMERATED {supported} OPTIONAL,

resumeWithStoredMCG-SCells-r16 ENUMERATED {supported} OPTIONAL,

resumeWithStoredSCG-r16 ENUMERATED {supported} OPTIONAL,

resumeWithSCG-Config-r16 ENUMERATED {supported} OPTIONAL,

ue-BasedPerfMeas-Parameters-r16 UE-BasedPerfMeas-Parameters-r16 OPTIONAL,

son-Parameters-r16 SON-Parameters-r16 OPTIONAL,

onDemandSIB-Connected-r16 ENUMERATED {supported} OPTIONAL,

nonCriticalExtension UE-NR-Capability-v1640 OPTIONAL

}

UE-NR-Capability-v1640 ::= SEQUENCE {

redirectAtResumeByNAS-r16 ENUMERATED {supported} OPTIONAL,

phy-ParametersSharedSpectrumChAccess-r16 Phy-ParametersSharedSpectrumChAccess-r16 OPTIONAL,

nonCriticalExtension UE-NR-Capability-v1650 OPTIONAL

}

UE-NR-Capability-v1650 ::= SEQUENCE {

mpsPriorityIndication-r16 ENUMERATED {supported} OPTIONAL,

highSpeedParameters-v1650 HighSpeedParameters-v1650 OPTIONAL,

nonCriticalExtension UE-NR-Capability-v1690 OPTIONAL

}

UE-NR-Capability-v1690 ::= SEQUENCE {

ul-RRC-Segmentation-r16 ENUMERATED {supported} OPTIONAL,

nonCriticalExtension UE-NR-Capability-v1700 OPTIONAL

}

-- Late non-critical extensions from Rel-16 onwards:

UE-NR-Capability-v16a0 ::= SEQUENCE {

phy-Parameters-v16a0 Phy-Parameters-v16a0 OPTIONAL,

rf-Parameters-v16a0 RF-Parameters-v16a0 OPTIONAL,

nonCriticalExtension UE-NR-Capability-v16c0 OPTIONAL

}

UE-NR-Capability-v16c0 ::= SEQUENCE {

rf-Parameters-v16c0 RF-Parameters-v16c0 OPTIONAL,

nonCriticalExtension UE-NR-Capability-v16d0 OPTIONAL

}

UE-NR-Capability-v16d0 ::= SEQUENCE {

featureSets-v16d0 FeatureSets-v16d0 OPTIONAL,

nonCriticalExtension SEQUENCE {} OPTIONAL

}

-- Regular non-critical Rel-17 extensions:

UE-NR-Capability-v1700 ::= SEQUENCE {

inactiveStatePO-Determination-r17 ENUMERATED {supported} OPTIONAL,

highSpeedParameters-v1700 HighSpeedParameters-v1700 OPTIONAL,

powSav-Parameters-v1700 PowSav-Parameters-v1700 OPTIONAL,

mac-Parameters-v1700 MAC-Parameters-v1700 OPTIONAL,

ims-Parameters-v1700 IMS-Parameters-v1700 OPTIONAL,

measAndMobParameters-v1700 MeasAndMobParameters-v1700,

appLayerMeasParameters-r17 AppLayerMeasParameters-r17 OPTIONAL,

redCapParameters-r17 RedCapParameters-r17 OPTIONAL,

ra-SDT-r17 ENUMERATED {supported} OPTIONAL,

srb-SDT-r17 ENUMERATED {supported} OPTIONAL,

gNB-SideRTT-BasedPDC-r17 ENUMERATED {supported} OPTIONAL,

bh-RLF-DetectionRecovery-Indication-r17 ENUMERATED {supported} OPTIONAL,

nrdc-Parameters-v1700 NRDC-Parameters-v1700 OPTIONAL,

bap-Parameters-v1700 BAP-Parameters-v1700 OPTIONAL,

musim-GapPreference-r17 ENUMERATED {supported} OPTIONAL,

musimLeaveConnected-r17 ENUMERATED {supported} OPTIONAL,

mbs-Parameters-r17 MBS-Parameters-r17,

nonTerrestrialNetwork-r17 ENUMERATED {supported} OPTIONAL,

ntn-ScenarioSupport-r17 ENUMERATED {gso, ngso} OPTIONAL,

sliceInfoforCellReselection-r17 ENUMERATED {supported} OPTIONAL,

ue-RadioPagingInfo-r17 UE-RadioPagingInfo-r17 OPTIONAL,

-- R4 17-2 UL gap pattern for Tx power management

ul-GapFR2-Pattern-r17 BIT STRING (SIZE (4)) OPTIONAL,

ntn-Parameters-r17 NTN-Parameters-r17 OPTIONAL,

nonCriticalExtension UE-NR-Capability-v1740 OPTIONAL

}

UE-NR-Capability-v1740 ::= SEQUENCE {

redCapParameters-v1740 RedCapParameters-v1740,

nonCriticalExtension UE-NR-Capability-v1750 OPTIONAL

}

UE-NR-Capability-v1750 ::= SEQUENCE {

crossCarrierSchedulingConfigurationRelease-r17 ENUMERATED {supported} OPTIONAL,

nonCriticalExtension UE-NR-Capability-v1800 OPTIONAL

}

-- Regular non-critical Rel-18 extensions:

UE-NR-Capability-v1800 ::= SEQUENCE {

airToGroundNetwork-r18 ENUMERATED {supported} OPTIONAL,

eRedCapParameters-r18 ERedCapParameters-r18 OPTIONAL,

ncr-Parameters-r18 NCR-Parameters-r18 OPTIONAL,

softSatelliteSwitchResyncNTN-r18 ENUMERATED {supported} OPTIONAL,

hardSatelliteSwitchResyncNTN-r18 ENUMERATED {supported} OPTIONAL,

mt-SDT-r18 ENUMERATED {supported} OPTIONAL,

mt-SDT-NTN-r18 ENUMERATED {supported} OPTIONAL,

inDeviceCoexIndAutonomousDenial-r18 ENUMERATED {supported} OPTIONAL,

inDeviceCoexIndFDM-r18 ENUMERATED {supported} OPTIONAL,

inDeviceCoexIndTDM-r18 ENUMERATED {supported} OPTIONAL,

musim-GapPriorityPreference-r18 ENUMERATED {supported} OPTIONAL,

musim-CapabilityRestriction-r18 ENUMERATED {supported} OPTIONAL,

multiRx-FR2-Preference-r18 ENUMERATED {supported} OPTIONAL,

ra-InsteadCG-SDT-r18 ENUMERATED {supported} OPTIONAL,

resumeAfterSDT-Release-r18 ENUMERATED {supported} OPTIONAL,

additionalBSR-Table-r18 ENUMERATED {supported} OPTIONAL,

delayStatusReport-r18 ENUMERATED {supported} OPTIONAL,

disableCG-RetransmissionMonitoring-r18 ENUMERATED {supported} OPTIONAL,

enhancedDRX-r18 ENUMERATED {supported} OPTIONAL,

pdu-SetDiscard-r18 ENUMERATED {supported} OPTIONAL,

psi-BasedDiscard-r18 ENUMERATED {supported} OPTIONAL,

ul-TrafficInfo-r18 ENUMERATED {supported} OPTIONAL,

aerialParameters-r18 AerialParameters-r18 OPTIONAL,

ntn-VSAT-AntennaType-r18 ENUMERATED {electronicSteering, mechanicalSteering} OPTIONAL,

ntn-VSAT-MobilityType-r18 ENUMERATED {fixed, mobile} OPTIONAL,

nonCriticalExtension SEQUENCE{} OPTIONAL

}

UE-NR-CapabilityAddXDD-Mode ::= SEQUENCE {

phy-ParametersXDD-Diff Phy-ParametersXDD-Diff OPTIONAL,

mac-ParametersXDD-Diff MAC-ParametersXDD-Diff OPTIONAL,

measAndMobParametersXDD-Diff MeasAndMobParametersXDD-Diff OPTIONAL

}

UE-NR-CapabilityAddXDD-Mode-v1530 ::= SEQUENCE {

eutra-ParametersXDD-Diff EUTRA-ParametersXDD-Diff

}

UE-NR-CapabilityAddFRX-Mode ::= SEQUENCE {

phy-ParametersFRX-Diff Phy-ParametersFRX-Diff OPTIONAL,

measAndMobParametersFRX-Diff MeasAndMobParametersFRX-Diff OPTIONAL

}

UE-NR-CapabilityAddFRX-Mode-v1540 ::= SEQUENCE {

ims-ParametersFRX-Diff IMS-ParametersFRX-Diff OPTIONAL

}

UE-NR-CapabilityAddFRX-Mode-v1610 ::= SEQUENCE {

powSav-ParametersFRX-Diff-r16 PowSav-ParametersFRX-Diff-r16 OPTIONAL,

mac-ParametersFRX-Diff-r16 MAC-ParametersFRX-Diff-r16 OPTIONAL

}

BAP-Parameters-r16 ::= SEQUENCE {

flowControlBH-RLC-ChannelBased-r16 ENUMERATED {supported} OPTIONAL,

flowControlRouting-ID-Based-r16 ENUMERATED {supported} OPTIONAL

}

BAP-Parameters-v1700 ::= SEQUENCE {

bapHeaderRewriting-Rerouting-r17 ENUMERATED {supported} OPTIONAL,

bapHeaderRewriting-Routing-r17 ENUMERATED {supported} OPTIONAL

}

MBS-Parameters-r17 ::= SEQUENCE {

maxMRB-Add-r17 INTEGER (1..16) OPTIONAL

}

-- TAG-UE-NR-CAPABILITY-STOP

-- ASN1STOP

|  |
| --- |
| *UE-NR-Capability* field descriptions |
| ***featureSetCombinations***  A list of *FeatureSetCombination:s* for *supportedBandCombinationList* in *UE-NR-Capability*. The *FeatureSetDownlink:s* and *FeatureSetUplink:s* referred to from these *FeatureSetCombination:s* are defined in the *featureSets* list in *UE-NR-Capability*. |

|  |
| --- |
| *UE-NR-Capability-v1540 field descriptions* |
| ***fr1-fr2-Add-UE-NR-Capabilities***  This instance of *UE-NR-CapabilityAddFRX-Mode* does not include any other fields than *csi-RS-IM-ReceptionForFeedback*/ *csi-RS-ProcFrameworkForSRS*/ *csi-ReportFramework*. |

\*\*\* OMITTED TEXT \*\*\*

***End of the modified section***