**3GPP TSG-RAN WG2 Meeting #125 *R2-230xxxx***

**Athens, Greece, February 26th – March 1st, 2024**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** |  | **Current version:** | **18.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Updates to UE capabilities for Rel-18 NR NTN Enh. |
|  |  |
| ***Source to WG:*** | Intel Corporation |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | NR\_NTN\_enh-Core |  | ***Date:*** | 2024-03-07 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | Updates to UE capabilities for Rel-18 NR NTN Enh. |
|  |  |
| ***Summary of change:*** | 1. Define a new UE capability for *ntn-VSAT-AntennaType-r18*.
2. Define a new UE capability for *ntn-VSAT-MobilityType-r18*.
3. Define a new UE capability for *eventD2-MeasReportTrigger-r18*.
 |
|  |  |
| ***Consequences if not approved:*** | NR NTN Enh. WI is not completed. |
|  |  |
| ***Clauses affected:*** | 6.3.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **x** |  |  Other core specifications  | TS/TR 38.306 CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

1. ***Modified section***

### 6.3.3 UE capability information elements

\*\*\* OMITTED TEXT \*\*\*

#### – *MeasAndMobParameters*

The IE *MeasAndMobParameters* is used to convey UE capabilities related to measurements for radio resource management (RRM), radio link monitoring (RLM) and mobility (e.g. handover).

*MeasAndMobParameters* information element

-- ASN1START

-- TAG-MEASANDMOBPARAMETERS-START

MeasAndMobParameters ::= SEQUENCE {

 measAndMobParametersCommon MeasAndMobParametersCommon OPTIONAL,

 measAndMobParametersXDD-Diff MeasAndMobParametersXDD-Diff OPTIONAL,

 measAndMobParametersFRX-Diff MeasAndMobParametersFRX-Diff OPTIONAL

}

MeasAndMobParameters-v1700 ::= SEQUENCE {

 measAndMobParametersFR2-2-r17 MeasAndMobParametersFR2-2-r17 OPTIONAL

}

MeasAndMobParametersCommon ::= SEQUENCE {

 supportedGapPattern BIT STRING (SIZE (22)) OPTIONAL,

 ssb-RLM ENUMERATED {supported} OPTIONAL,

 ssb-AndCSI-RS-RLM ENUMERATED {supported} OPTIONAL,

 ...,

 [[

 eventB-MeasAndReport ENUMERATED {supported} OPTIONAL,

 handoverFDD-TDD ENUMERATED {supported} OPTIONAL,

 eutra-CGI-Reporting ENUMERATED {supported} OPTIONAL,

 nr-CGI-Reporting ENUMERATED {supported} OPTIONAL

 ]],

 [[

 independentGapConfig ENUMERATED {supported} OPTIONAL,

 periodicEUTRA-MeasAndReport ENUMERATED {supported} OPTIONAL,

 handoverFR1-FR2 ENUMERATED {supported} OPTIONAL,

 maxNumberCSI-RS-RRM-RS-SINR ENUMERATED {n4, n8, n16, n32, n64, n96} OPTIONAL

 ]],

 [[

 nr-CGI-Reporting-ENDC ENUMERATED {supported} OPTIONAL

 ]],

 [[

 eutra-CGI-Reporting-NEDC ENUMERATED {supported} OPTIONAL,

 eutra-CGI-Reporting-NRDC ENUMERATED {supported} OPTIONAL,

 nr-CGI-Reporting-NEDC ENUMERATED {supported} OPTIONAL,

 nr-CGI-Reporting-NRDC ENUMERATED {supported} OPTIONAL

 ]],

 [[

 reportAddNeighMeasForPeriodic-r16 ENUMERATED {supported} OPTIONAL,

 condHandoverParametersCommon-r16 SEQUENCE {

 condHandoverFDD-TDD-r16 ENUMERATED {supported} OPTIONAL,

 condHandoverFR1-FR2-r16 ENUMERATED {supported} OPTIONAL

 } OPTIONAL,

 nr-NeedForGap-Reporting-r16 ENUMERATED {supported} OPTIONAL,

 supportedGapPattern-NRonly-r16 BIT STRING (SIZE (10)) OPTIONAL,

 supportedGapPattern-NRonly-NEDC-r16 ENUMERATED {supported} OPTIONAL,

 maxNumberCLI-RSSI-r16 ENUMERATED {n8, n16, n32, n64} OPTIONAL,

 maxNumberCLI-SRS-RSRP-r16 ENUMERATED {n4, n8, n16, n32} OPTIONAL,

 maxNumberPerSlotCLI-SRS-RSRP-r16 ENUMERATED {n2, n4, n8} OPTIONAL,

 mfbi-IAB-r16 ENUMERATED {supported} OPTIONAL,

 dummy ENUMERATED {supported} OPTIONAL,

 nr-CGI-Reporting-NPN-r16 ENUMERATED {supported} OPTIONAL,

 idleInactiveEUTRA-MeasReport-r16 ENUMERATED {supported} OPTIONAL,

 idleInactive-ValidityArea-r16 ENUMERATED {supported} OPTIONAL,

 eutra-AutonomousGaps-r16 ENUMERATED {supported} OPTIONAL,

 eutra-AutonomousGaps-NEDC-r16 ENUMERATED {supported} OPTIONAL,

 eutra-AutonomousGaps-NRDC-r16 ENUMERATED {supported} OPTIONAL,

 pcellT312-r16 ENUMERATED {supported} OPTIONAL,

 supportedGapPattern-r16 BIT STRING (SIZE (2)) OPTIONAL

 ]],

 [[

 -- R4 19-2 Concurrent measurement gaps

 concurrentMeasGap-r17 CHOICE {

 concurrentPerUE-OnlyMeasGap-r17 ENUMERATED {supported},

 concurrentPerUE-PerFRCombMeasGap-r17 ENUMERATED {supported}

 } OPTIONAL,

 -- R4 19-1 Network controlled small gap (NCSG)

 nr-NeedForGapNCSG-Reporting-r17 ENUMERATED {supported} OPTIONAL,

 eutra-NeedForGapNCSG-Reporting-r17 ENUMERATED {supported} OPTIONAL,

 -- R4 19-1-1 per FR Network controlled small gap (NCSG)

 ncsg-MeasGapPerFR-r17 ENUMERATED {supported} OPTIONAL,

 -- R4 19-1-2 Network controlled small gap (NCSG) supported patterns

 ncsg-MeasGapPatterns-r17 BIT STRING (SIZE(24)) OPTIONAL,

 -- R4 19-1-3 Network controlled small gap (NCSG) supported NR-only patterns

 ncsg-MeasGapNR-Patterns-r17 BIT STRING (SIZE(24)) OPTIONAL,

 -- R4 19-3-2 pre-configured measurement gap

 preconfiguredUE-AutonomousMeasGap-r17 ENUMERATED {supported} OPTIONAL,

 -- R4 19-3-1 pre-configured measurement gap

 preconfiguredNW-ControlledMeasGap-r17 ENUMERATED {supported} OPTIONAL,

 handoverFR1-FR2-2-r17 ENUMERATED {supported} OPTIONAL,

 handoverFR2-1-FR2-2-r17 ENUMERATED {supported} OPTIONAL,

 -- RAN4 14-1: per-FR MG for PRS measurement

 independentGapConfigPRS-r17 ENUMERATED {supported} OPTIONAL,

 rrm-RelaxationRRC-ConnectedRedCap-r17 ENUMERATED {supported} OPTIONAL,

 -- R4 25-3: Parallel measurements with multiple measurement gaps

 parallelMeasurementGap-r17 ENUMERATED {n2} OPTIONAL,

 condHandoverWithSCG-NRDC-r17 ENUMERATED {supported} OPTIONAL,

 gNB-ID-LengthReporting-r17 ENUMERATED {supported} OPTIONAL,

 gNB-ID-LengthReporting-ENDC-r17 ENUMERATED {supported} OPTIONAL,

 gNB-ID-LengthReporting-NEDC-r17 ENUMERATED {supported} OPTIONAL,

 gNB-ID-LengthReporting-NRDC-r17 ENUMERATED {supported} OPTIONAL,

 gNB-ID-LengthReporting-NPN-r17 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 -- R4 25-1: Parallel measurements on multiple SMTC-s for a single frequency carrier

 parallelSMTC-r17 ENUMERATED {n4} OPTIONAL,

 -- R4 19-2-1 Concurrent measurement gaps for EUTRA

 concurrentMeasGapEUTRA-r17 ENUMERATED {supported} OPTIONAL,

 serviceLinkPropDelayDiffReporting-r17 ENUMERATED {supported} OPTIONAL,

 -- R4 19-1-4 Network controlled small gap (NCSG) performing measurement based on flag deriveSSB-IndexFromCellInter

 ncsg-SymbolLevelScheduleRestrictionInter-r17 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 eventD1-MeasReportTrigger-r17 ENUMERATED {supported} OPTIONAL,

 independentGapConfig-maxCC-r17 SEQUENCE {

 fr1-Only-r17 INTEGER (1..32) OPTIONAL,

 fr2-Only-r17 INTEGER (1..32) OPTIONAL,

 fr1-AndFR2-r17 INTEGER (1..32) OPTIONAL

 } OPTIONAL

 ]],

 [[

 interSatMeas-r17 ENUMERATED {supported} OPTIONAL,

 deriveSSB-IndexFromCellInterNon-NCSG-r17 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 -- R4 31-1 Enhanced L3 measurement reporting for unknown SCell activation if the valid L3 measurement results are available

 l3-MeasUnknownSCellActivation-r18 ENUMERATED {supported} OPTIONAL,

 -- R4 31-3 Shorter measurement interval for unknown SCell activation

 shortMeasInterval-r18 ENUMERATED {supported} OPTIONAL,

 nr-NeedForInterruptionReport-r18 ENUMERATED {supported} OPTIONAL,

 measSequenceConfig-r18 ENUMERATED {supported} OPTIONAL,

 cellIndividualOffsetPerMeasEvent-r18 ENUMERATED {supported} OPTIONAL,

 eventD2-MeasReportTrigger-r18 ENUMERATED {supported} OPTIONAL

 ]]

}

MeasAndMobParametersXDD-Diff ::= SEQUENCE {

 intraAndInterF-MeasAndReport ENUMERATED {supported} OPTIONAL,

 eventA-MeasAndReport ENUMERATED {supported} OPTIONAL,

 ...,

 [[

 handoverInterF ENUMERATED {supported} OPTIONAL,

 handoverLTE-EPC ENUMERATED {supported} OPTIONAL,

 handoverLTE-5GC ENUMERATED {supported} OPTIONAL

 ]],

 [[

 sftd-MeasNR-Neigh ENUMERATED {supported} OPTIONAL,

 sftd-MeasNR-Neigh-DRX ENUMERATED {supported} OPTIONAL

 ]],

 [[

 dummy ENUMERATED {supported} OPTIONAL

 ]]

}

MeasAndMobParametersFRX-Diff ::= SEQUENCE {

 ss-SINR-Meas ENUMERATED {supported} OPTIONAL,

 csi-RSRP-AndRSRQ-MeasWithSSB ENUMERATED {supported} OPTIONAL,

 csi-RSRP-AndRSRQ-MeasWithoutSSB ENUMERATED {supported} OPTIONAL,

 csi-SINR-Meas ENUMERATED {supported} OPTIONAL,

 csi-RS-RLM ENUMERATED {supported} OPTIONAL,

 ...,

 [[

 handoverInterF ENUMERATED {supported} OPTIONAL,

 handoverLTE-EPC ENUMERATED {supported} OPTIONAL,

 handoverLTE-5GC ENUMERATED {supported} OPTIONAL

 ]],

 [[

 maxNumberResource-CSI-RS-RLM ENUMERATED {n2, n4, n6, n8} OPTIONAL

 ]],

 [[

 simultaneousRxDataSSB-DiffNumerology ENUMERATED {supported} OPTIONAL

 ]],

 [[

 nr-AutonomousGaps-r16 ENUMERATED {supported} OPTIONAL,

 nr-AutonomousGaps-ENDC-r16 ENUMERATED {supported} OPTIONAL,

 nr-AutonomousGaps-NEDC-r16 ENUMERATED {supported} OPTIONAL,

 nr-AutonomousGaps-NRDC-r16 ENUMERATED {supported} OPTIONAL,

 dummy ENUMERATED {supported} OPTIONAL,

 cli-RSSI-Meas-r16 ENUMERATED {supported} OPTIONAL,

 cli-SRS-RSRP-Meas-r16 ENUMERATED {supported} OPTIONAL,

 interFrequencyMeas-NoGap-r16 ENUMERATED {supported} OPTIONAL,

 simultaneousRxDataSSB-DiffNumerology-Inter-r16 ENUMERATED {supported} OPTIONAL,

 idleInactiveNR-MeasReport-r16 ENUMERATED {supported} OPTIONAL,

 -- R4 6-2: Support of beam level Early Measurement Reporting

 idleInactiveNR-MeasBeamReport-r16 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 increasedNumberofCSIRSPerMO-r16 ENUMERATED {supported} OPTIONAL

 ]]

}

MeasAndMobParametersFR2-2-r17 ::= SEQUENCE {

 handoverInterF-r17 ENUMERATED {supported} OPTIONAL,

 handoverLTE-EPC-r17 ENUMERATED {supported} OPTIONAL,

 handoverLTE-5GC-r17 ENUMERATED {supported} OPTIONAL,

 idleInactiveNR-MeasReport-r17 ENUMERATED {supported} OPTIONAL,

...

}

-- TAG-MEASANDMOBPARAMETERS-STOP

-- ASN1STOP

\*\*\* OMITTED TEXT \*\*\*

1. ***Modified section***

#### – *UE-NR-Capability*

The IE *UE-NR-Capability* is used to convey the NR UE Radio Access Capability Parameters, see TS 38.306 [26].

*UE-NR-Capability* information element

-- ASN1START

-- TAG-UE-NR-CAPABILITY-START

UE-NR-Capability ::= SEQUENCE {

 accessStratumRelease AccessStratumRelease,

 pdcp-Parameters PDCP-Parameters,

 rlc-Parameters RLC-Parameters OPTIONAL,

 mac-Parameters MAC-Parameters OPTIONAL,

 phy-Parameters Phy-Parameters,

 rf-Parameters RF-Parameters,

 measAndMobParameters MeasAndMobParameters OPTIONAL,

 fdd-Add-UE-NR-Capabilities UE-NR-CapabilityAddXDD-Mode OPTIONAL,

 tdd-Add-UE-NR-Capabilities UE-NR-CapabilityAddXDD-Mode OPTIONAL,

 fr1-Add-UE-NR-Capabilities UE-NR-CapabilityAddFRX-Mode OPTIONAL,

 fr2-Add-UE-NR-Capabilities UE-NR-CapabilityAddFRX-Mode OPTIONAL,

 featureSets FeatureSets OPTIONAL,

 featureSetCombinations SEQUENCE (SIZE (1..maxFeatureSetCombinations)) OF FeatureSetCombination OPTIONAL,

 lateNonCriticalExtension OCTET STRING (CONTAINING UE-NR-Capability-v15c0) OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1530 OPTIONAL

}

-- Regular non-critical Rel-15 extensions:

UE-NR-Capability-v1530 ::= SEQUENCE {

 fdd-Add-UE-NR-Capabilities-v1530 UE-NR-CapabilityAddXDD-Mode-v1530 OPTIONAL,

 tdd-Add-UE-NR-Capabilities-v1530 UE-NR-CapabilityAddXDD-Mode-v1530 OPTIONAL,

 dummy ENUMERATED {supported} OPTIONAL,

 interRAT-Parameters InterRAT-Parameters OPTIONAL,

 inactiveState ENUMERATED {supported} OPTIONAL,

 delayBudgetReporting ENUMERATED {supported} OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1540 OPTIONAL

}

UE-NR-Capability-v1540 ::= SEQUENCE {

 sdap-Parameters SDAP-Parameters OPTIONAL,

 overheatingInd ENUMERATED {supported} OPTIONAL,

 ims-Parameters IMS-Parameters OPTIONAL,

 fr1-Add-UE-NR-Capabilities-v1540 UE-NR-CapabilityAddFRX-Mode-v1540 OPTIONAL,

 fr2-Add-UE-NR-Capabilities-v1540 UE-NR-CapabilityAddFRX-Mode-v1540 OPTIONAL,

 fr1-fr2-Add-UE-NR-Capabilities UE-NR-CapabilityAddFRX-Mode OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1550 OPTIONAL

}

UE-NR-Capability-v1550 ::= SEQUENCE {

 reducedCP-Latency ENUMERATED {supported} OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1560 OPTIONAL

}

UE-NR-Capability-v1560 ::= SEQUENCE {

 nrdc-Parameters NRDC-Parameters OPTIONAL,

 receivedFilters OCTET STRING (CONTAINING UECapabilityEnquiry-v1560-IEs) OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1570 OPTIONAL

}

UE-NR-Capability-v1570 ::= SEQUENCE {

 nrdc-Parameters-v1570 NRDC-Parameters-v1570 OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1610 OPTIONAL

}

-- Late non-critical Rel-15 extensions:

UE-NR-Capability-v15c0 ::= SEQUENCE {

 nrdc-Parameters-v15c0 NRDC-Parameters-v15c0 OPTIONAL,

 partialFR2-FallbackRX-Req ENUMERATED {true} OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v15g0 OPTIONAL

}

UE-NR-Capability-v15g0 ::= SEQUENCE {

 rf-Parameters-v15g0 RF-Parameters-v15g0 OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v15j0 OPTIONAL

}

UE-NR-Capability-v15j0 ::= SEQUENCE {

 -- Following field is only for REL-15 late non-critical extensions

 lateNonCriticalExtension OCTET STRING OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v16a0 OPTIONAL

}

-- Regular non-critical Rel-16 extensions:

UE-NR-Capability-v1610 ::= SEQUENCE {

 inDeviceCoexInd-r16 ENUMERATED {supported} OPTIONAL,

 dl-DedicatedMessageSegmentation-r16 ENUMERATED {supported} OPTIONAL,

 nrdc-Parameters-v1610 NRDC-Parameters-v1610 OPTIONAL,

 powSav-Parameters-r16 PowSav-Parameters-r16 OPTIONAL,

 fr1-Add-UE-NR-Capabilities-v1610 UE-NR-CapabilityAddFRX-Mode-v1610 OPTIONAL,

 fr2-Add-UE-NR-Capabilities-v1610 UE-NR-CapabilityAddFRX-Mode-v1610 OPTIONAL,

 bh-RLF-Indication-r16 ENUMERATED {supported} OPTIONAL,

 directSN-AdditionFirstRRC-IAB-r16 ENUMERATED {supported} OPTIONAL,

 bap-Parameters-r16 BAP-Parameters-r16 OPTIONAL,

 referenceTimeProvision-r16 ENUMERATED {supported} OPTIONAL,

 sidelinkParameters-r16 SidelinkParameters-r16 OPTIONAL,

 highSpeedParameters-r16 HighSpeedParameters-r16 OPTIONAL,

 mac-Parameters-v1610 MAC-Parameters-v1610 OPTIONAL,

 mcgRLF-RecoveryViaSCG-r16 ENUMERATED {supported} OPTIONAL,

 resumeWithStoredMCG-SCells-r16 ENUMERATED {supported} OPTIONAL,

 resumeWithStoredSCG-r16 ENUMERATED {supported} OPTIONAL,

 resumeWithSCG-Config-r16 ENUMERATED {supported} OPTIONAL,

 ue-BasedPerfMeas-Parameters-r16 UE-BasedPerfMeas-Parameters-r16 OPTIONAL,

 son-Parameters-r16 SON-Parameters-r16 OPTIONAL,

 onDemandSIB-Connected-r16 ENUMERATED {supported} OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1640 OPTIONAL

}

UE-NR-Capability-v1640 ::= SEQUENCE {

 redirectAtResumeByNAS-r16 ENUMERATED {supported} OPTIONAL,

 phy-ParametersSharedSpectrumChAccess-r16 Phy-ParametersSharedSpectrumChAccess-r16 OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1650 OPTIONAL

}

UE-NR-Capability-v1650 ::= SEQUENCE {

 mpsPriorityIndication-r16 ENUMERATED {supported} OPTIONAL,

 highSpeedParameters-v1650 HighSpeedParameters-v1650 OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1690 OPTIONAL

}

UE-NR-Capability-v1690 ::= SEQUENCE {

 ul-RRC-Segmentation-r16 ENUMERATED {supported} OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1700 OPTIONAL

}

-- Late non-critical extensions from Rel-16 onwards:

UE-NR-Capability-v16a0 ::= SEQUENCE {

 phy-Parameters-v16a0 Phy-Parameters-v16a0 OPTIONAL,

 rf-Parameters-v16a0 RF-Parameters-v16a0 OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v16c0 OPTIONAL

}

UE-NR-Capability-v16c0 ::= SEQUENCE {

 rf-Parameters-v16c0 RF-Parameters-v16c0 OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v16d0 OPTIONAL

}

UE-NR-Capability-v16d0 ::= SEQUENCE {

 featureSets-v16d0 FeatureSets-v16d0 OPTIONAL,

 nonCriticalExtension SEQUENCE {} OPTIONAL

}

-- Regular non-critical Rel-17 extensions:

UE-NR-Capability-v1700 ::= SEQUENCE {

 inactiveStatePO-Determination-r17 ENUMERATED {supported} OPTIONAL,

 highSpeedParameters-v1700 HighSpeedParameters-v1700 OPTIONAL,

 powSav-Parameters-v1700 PowSav-Parameters-v1700 OPTIONAL,

 mac-Parameters-v1700 MAC-Parameters-v1700 OPTIONAL,

 ims-Parameters-v1700 IMS-Parameters-v1700 OPTIONAL,

 measAndMobParameters-v1700 MeasAndMobParameters-v1700,

 appLayerMeasParameters-r17 AppLayerMeasParameters-r17 OPTIONAL,

 redCapParameters-r17 RedCapParameters-r17 OPTIONAL,

 ra-SDT-r17 ENUMERATED {supported} OPTIONAL,

 srb-SDT-r17 ENUMERATED {supported} OPTIONAL,

 gNB-SideRTT-BasedPDC-r17 ENUMERATED {supported} OPTIONAL,

 bh-RLF-DetectionRecovery-Indication-r17 ENUMERATED {supported} OPTIONAL,

 nrdc-Parameters-v1700 NRDC-Parameters-v1700 OPTIONAL,

 bap-Parameters-v1700 BAP-Parameters-v1700 OPTIONAL,

 musim-GapPreference-r17 ENUMERATED {supported} OPTIONAL,

 musimLeaveConnected-r17 ENUMERATED {supported} OPTIONAL,

 mbs-Parameters-r17 MBS-Parameters-r17,

 nonTerrestrialNetwork-r17 ENUMERATED {supported} OPTIONAL,

 ntn-ScenarioSupport-r17 ENUMERATED {gso, ngso} OPTIONAL,

 sliceInfoforCellReselection-r17 ENUMERATED {supported} OPTIONAL,

 ue-RadioPagingInfo-r17 UE-RadioPagingInfo-r17 OPTIONAL,

 -- R4 17-2 UL gap pattern for Tx power management

 ul-GapFR2-Pattern-r17 BIT STRING (SIZE (4)) OPTIONAL,

 ntn-Parameters-r17 NTN-Parameters-r17 OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1740 OPTIONAL

}

UE-NR-Capability-v1740 ::= SEQUENCE {

 redCapParameters-v1740 RedCapParameters-v1740,

 nonCriticalExtension UE-NR-Capability-v1750 OPTIONAL

}

UE-NR-Capability-v1750 ::= SEQUENCE {

 crossCarrierSchedulingConfigurationRelease-r17 ENUMERATED {supported} OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1800 OPTIONAL

}

-- Regular non-critical Rel-18 extensions:

UE-NR-Capability-v1800 ::= SEQUENCE {

 airToGroundNetwork-r18 ENUMERATED {supported} OPTIONAL,

 eRedCapParameters-r18 ERedCapParameters-r18 OPTIONAL,

 ncr-Parameters-r18 NCR-Parameters-r18 OPTIONAL,

 softSatelliteSwitchResyncNTN-r18 ENUMERATED {supported} OPTIONAL,

 hardSatelliteSwitchResyncNTN-r18 ENUMERATED {supported} OPTIONAL,

 mt-SDT-r18 ENUMERATED {supported} OPTIONAL,

 mt-SDT-NTN-r18 ENUMERATED {supported} OPTIONAL,

 inDeviceCoexIndAutonomousDenial-r18 ENUMERATED {supported} OPTIONAL,

 inDeviceCoexIndFDM-r18 ENUMERATED {supported} OPTIONAL,

 inDeviceCoexIndTDM-r18 ENUMERATED {supported} OPTIONAL,

 musim-GapPriorityPreference-r18 ENUMERATED {supported} OPTIONAL,

 musim-CapabilityRestriction-r18 ENUMERATED {supported} OPTIONAL,

 multiRx-FR2-Preference-r18 ENUMERATED {supported} OPTIONAL,

 ra-InsteadCG-SDT-r18 ENUMERATED {supported} OPTIONAL,

 resumeAfterSDT-Release-r18 ENUMERATED {supported} OPTIONAL,

 additionalBSR-Table-r18 ENUMERATED {supported} OPTIONAL,

 delayStatusReport-r18 ENUMERATED {supported} OPTIONAL,

 disableCG-RetransmissionMonitoring-r18 ENUMERATED {supported} OPTIONAL,

 enhancedDRX-r18 ENUMERATED {supported} OPTIONAL,

 pdu-SetDiscard-r18 ENUMERATED {supported} OPTIONAL,

 psi-BasedDiscard-r18 ENUMERATED {supported} OPTIONAL,

 ul-TrafficInfo-r18 ENUMERATED {supported} OPTIONAL,

 aerialParameters-r18 AerialParameters-r18 OPTIONAL,

 ntn-VSAT-AntennaType-r18 ENUMERATED {electronic, mechanical} OPTIONAL,

 ntn-VSAT-MobilityType-r18 ENUMERATED {fixed, mobile} OPTIONAL,

 nonCriticalExtension SEQUENCE{} OPTIONAL

}

UE-NR-CapabilityAddXDD-Mode ::= SEQUENCE {

 phy-ParametersXDD-Diff Phy-ParametersXDD-Diff OPTIONAL,

 mac-ParametersXDD-Diff MAC-ParametersXDD-Diff OPTIONAL,

 measAndMobParametersXDD-Diff MeasAndMobParametersXDD-Diff OPTIONAL

}

UE-NR-CapabilityAddXDD-Mode-v1530 ::= SEQUENCE {

 eutra-ParametersXDD-Diff EUTRA-ParametersXDD-Diff

}

UE-NR-CapabilityAddFRX-Mode ::= SEQUENCE {

 phy-ParametersFRX-Diff Phy-ParametersFRX-Diff OPTIONAL,

 measAndMobParametersFRX-Diff MeasAndMobParametersFRX-Diff OPTIONAL

}

UE-NR-CapabilityAddFRX-Mode-v1540 ::= SEQUENCE {

 ims-ParametersFRX-Diff IMS-ParametersFRX-Diff OPTIONAL

}

UE-NR-CapabilityAddFRX-Mode-v1610 ::= SEQUENCE {

 powSav-ParametersFRX-Diff-r16 PowSav-ParametersFRX-Diff-r16 OPTIONAL,

 mac-ParametersFRX-Diff-r16 MAC-ParametersFRX-Diff-r16 OPTIONAL

}

BAP-Parameters-r16 ::= SEQUENCE {

 flowControlBH-RLC-ChannelBased-r16 ENUMERATED {supported} OPTIONAL,

 flowControlRouting-ID-Based-r16 ENUMERATED {supported} OPTIONAL

}

BAP-Parameters-v1700 ::= SEQUENCE {

 bapHeaderRewriting-Rerouting-r17 ENUMERATED {supported} OPTIONAL,

 bapHeaderRewriting-Routing-r17 ENUMERATED {supported} OPTIONAL

}

MBS-Parameters-r17 ::= SEQUENCE {

 maxMRB-Add-r17 INTEGER (1..16) OPTIONAL

}

-- TAG-UE-NR-CAPABILITY-STOP

-- ASN1STOP

|  |
| --- |
| *UE-NR-Capability* field descriptions |
| ***featureSetCombinations***A list of *FeatureSetCombination:s* for *supportedBandCombinationList* in *UE-NR-Capability*. The *FeatureSetDownlink:s* and *FeatureSetUplink:s* referred to from these *FeatureSetCombination:s* are defined in the *featureSets* list in *UE-NR-Capability*. |

|  |
| --- |
| *UE-NR-Capability-v1540 field descriptions* |
| ***fr1-fr2-Add-UE-NR-Capabilities***This instance of *UE-NR-CapabilityAddFRX-Mode* does not include any other fields than *csi-RS-IM-ReceptionForFeedback*/ *csi-RS-ProcFrameworkForSRS*/ *csi-ReportFramework*. |

\*\*\* OMITTED TEXT \*\*\*

***End of the modified section***