|  |  |  |
| --- | --- | --- |
| **Company** | **Clause Number and Related specification** | **Comment** |
| Xiaomi | 5.8.9.1a.4Do we need to reflect the condition for RRC\_IDLE/INACTIVE when duplication is configured and for all RRC states when duplication is not configured？ |  |
| Huawei, HiSilicon | The agreed changes based on P2, P3 in R2-2402227 are added in the section for PC5-S message:1> if transmission of PC5-S message for a specific destination is requested by upper layers for sidelink SRB:Should be added instead in the section for PC5-RRC message (?):1> if a PC5-RRC connection establishment for a specific destination is indicated by upper layers: |  |
|  |  |  |
|  |  |  |