**3GPP TSG RAN WG2 #126 *R2-24xxxxx***

**Fukuoka, Japan, 20 - 24 May, 2024**

**Source:** Huawei, HiSilicon

**Title:** Report of [Post126][305][IoT-NTN Enh] 36.331 CR (Huawei)

**Agenda Item:** 7.6.1

**Document for:** Discussion and decision

# Introduction

This document captures the outcome of the following email discussion:

* [Post126][305][IoT-NTN Enh] 36.331 CR (Huawei)

 Scope: update the RRC CR with meeting agreements

 Intended outcome: Agreed CR

 Deadline for agreed CR (in R2-2405758): short

# Discussion

The issue to be discussed in this document is the T390 stop condition for GNSS position fix during C-DRX inactive time:

|  |
| --- |
| Proposal 4: T390 is stopped after successful GNSS position fix during C-DRX inactive time. - Google could be fine but thinks we should have a single criterion for stopping T390. - QC agrees and thinks we can remove “during C-DRX inactive time”- Oppo is fine with p4 and thinks this is a special case to be treated separately. Nokia agree* Agreed (can further discuss how to capture this in the CR review)

Proposal 5: Discuss in CR review phase how to capture T390 stopping condition for the following cases: - Network-triggered GNSS position fix- Autonomous GNSS position fix- GNSS position fix during C-DRX inactive time- ZTE thinks the first 2 points have already been covered and we just need to focus on the last point. Apple agrees* In the CR review we focus on how to capture T390 stopping condition for GNSS position fix during C-DRX inactive time
 |

The agreed proposal during the meeting is “T390 is stopped after successful GNSS position fix during C-DRX inactive time”, however, in the current spec, for network triggered GNSS measurement, T390 is stopped once GNSS measurement MAC CE is received (instead of after successful completion of GNSS position fix):

|  |  |  |  |
| --- | --- | --- | --- |
| T390NOTE1 | Upon GNSS validity duration expiry if *ul-TransmissionExtensionEnabled* is configured. | Upon leaving RRC\_CONNECTED, or upon reception of network triggered GNSS measurement, or upon initiating the connection re-establishment procedure. | Perform the actions as specified in 5.3.3.21. |

There are several options for implementing the T390 stop condition for GNSS position fix during C-DRX inactive time:

* **Option 1** (as in the agreed proposal): T390 is stopped after successful GNSS position fix during C-DRX inactive time;
* **Option 2** (“aligned” with NW triggered GNSS): T390 is stopped upon initiating GNSS position fix during C-DRX inactive time:
	+ **Option 2-1**: separate condition with NW triggered GNSS
	+ **Option 2-2**: common criterion for NW triggered GNSS and C-DRX based GNSS
* **Other options**, e.g. T390 is stopped after sending GNSS Validity Duration Report MAC CE (so that UE and NW can have an aligned understanding of T390 status), but this may introduce further RRC-MAC interaction

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| ***TP for Option 1***# Clause 5.5.9:NOTE: UE can also autonomously start GNSS measurements during available idle periods in RRC\_CONNECTED to keep GNSS valid and stop T390 upon indication that a new GNSS position becomes valid, and the exact time of starting GNSS measurements during available idle periods is left to UE implementation.# Clause 7.3.1:

|  |  |  |  |
| --- | --- | --- | --- |
| T390NOTE1 | Upon GNSS validity duration expiry if *ul-TransmissionExtensionEnabled* is configured. | Upon leaving RRC\_CONNECTED, or upon reception of network triggered GNSS measurement, or upon indication that a new GNSS position becomes valid during available idle periods in RRC\_CONNECTED, or upon initiating the connection re-establishment procedure. | Perform the actions as specified in 5.3.3.21. |

 |
| ***TP for Option 2-1***# Clause 5.5.9:NOTE: UE can also autonomously start GNSS measurements during available idle periods in RRC\_CONNECTED to keep GNSS valid and stop T390 upon starting GNSS measurement, and the exact time of starting GNSS measurements during available idle periods is left to UE implementation.# Clause 7.3.1:

|  |  |  |  |
| --- | --- | --- | --- |
| T390NOTE1 | Upon GNSS validity duration expiry if *ul-TransmissionExtensionEnabled* is configured. | Upon leaving RRC\_CONNECTED, or upon reception of network triggered GNSS measurement, or upon initiating GNSS measurement during available idle periods in RRC\_CONNECTED, or upon initiating the connection re-establishment procedure. | Perform the actions as specified in 5.3.3.21. |

 |
| ***TP for Option 2-2***# Clause 5.5.9:The UE shall:1> if an indication to perform GNSS measurement is received from lower layers:2> perform GNSS measurement using the measurement gap with a gap length indicated by lower layers, as specified in TS 36.213 [23];1> if *gnss-AutonomousEnabled* is configured:2> perform GNSS measurement using an autonomous gap starting from T390 expiry if *ul-TransmissionExtensionEnabled* is configured, otherwise starting from GNSS validity duration expiry, with a gap length indicated by lower layers or equal to the latest reported time duration required for the UE to acquire a GNSS position if not indicated by lower layers;NOTE: UE can also autonomously start GNSS measurements during available idle periods in RRC\_CONNECTED to keep GNSS valid, and the exact time of starting GNSS measurements during available idle periods is left to UE implementation.1> upon starting GNSS measurement:2> stop timer T318, if running;2> stop timer T390, if running;# Clause 7.3.1:

|  |  |  |  |
| --- | --- | --- | --- |
| T390NOTE1 | Upon GNSS validity duration expiry if *ul-TransmissionExtensionEnabled* is configured. | Upon leaving RRC\_CONNECTED, or upon performing GNSS measurement. | Perform the actions as specified in 5.3.3.21. |

 |

**Q1: Please indicate your preferred option:**

* **Option 1** (as in the agreed proposal): T390 is stopped after successful GNSS position fix during C-DRX inactive time;
* **Option 2** (“aligned” with NW triggered GNSS): T390 is stopped upon initiating GNSS position fix during C-DRX inactive time:
	+ **Option 2-1**: separate condition with NW triggered GNSS
	+ **Option 2-2**: common criterion for NW triggered GNSS and C-DRX based GNSS
* **Other options**, e.g. T390 is stopped after sending GNSS Validity Duration Report MAC CE etc.

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Conclusion

To be completed

1. Contact Information

To make it easier to find the contact delegate for potential follow-up questions, delegates are encouraged to provide their contact information in the following table:

|  |  |  |
| --- | --- | --- |
| **Company** | **Name** | **Email** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |