**3GPP TSG-RAN WG2 Meeting #129 R2-250xxxx**

**Orlando, USA, Oct 18th – 22nd, 2024**

Agenda item:

Source: Apple (moderator)

Title: Email discussion summary for  [Post128][018][AI Mob] generalization (Apple)

Document for: Discussion and Decision

# 1 Introduction

This is the draft document (and the future email discussion summary) for the following email discussion.

* [Post128][018][AI Mob] generalization (Apple)

 Intended outcome: Discuss parameters for different cell configuration and attempt to prioritize 1 parameters and not more than 2 values per parameter. Can do 2 max values if really reneed. for

 Deadline: 3 weeks (i.e. December 13)

For your convenience, below you can find the relevant agreements on model generalization from RAN2#128.

|  |
| --- |
| **Agreements on generalization** 1. Reuse the evaluation methodology in TR38.843 for generalization study, i.e., the generalization performance is evaluated with the following cases,
* *Baseline:* The AI/ML model is trained using the dataset with Configuration #B and tested using the dataset with Configuration #B.
* *Generalization Case #1 (GC#1):* The AI/ML model is trained using the dataset with Configuration #A but tested using the dataset with Configuration #B.
* *Generalization Case #2 (GC#2):* The AI/ML model is trained using mixed datasets with both configurations and tested using the dataset with Configuration #B.

2 Companies can choose which case they compare with and should report it with simulation results. 3 Generalization issues on RRM measurement prediction are prioritized. 4 Start the study with generalization issue with RRM measurement prediction in temporal domain. Companies can chose to study frequency domain prediction cases and report what they have simulated. 5 Study generalization over UE speeds 6 The simulation assumption of FR1 temporal domain case B is reused for generalization study with 3 UE speeds i.e. 30Km/h, 60Km/h and 90Km/h. FFS on combinations 7 The simulation assumption of FR2 temporal domain case A is reused for generalization study with 3 UE speeds i.e. 60Km/h, 90Km/h and 120Km/h. FFS on combinations |

**Further agreements on generalization**

1. Companies that would like to study inter-frequency generalization can start with input 2GHz and output 4GHz, and 4GHz to 2GHz. FFS if we introduce a third frequency.
2. Study model generalization across different cell configurations (e.g. ISD, gNB height, power, beam pattern, etc). FFS which parameters we prioritize.

# 2 Discussion

The following is hopefully a complete list of all the proposals relevant to the present discussion made in contributions submitted to RAN2#128:

* R2-2409652
	+ Proposal 3: Study AI/ML generalization from cell perspective for intra-frequency RRM measurement prediction, i.e., whether the model trained based on one cell’s data can also be applied to another cell’s intra-frequency RRM measurement prediction.
* R2-2409668
	+ Proposal 1: The following factors are considered in the generalization study for RRM prediction:
		- Scenarios, including deployment scenarios (e.g., UMa, UMi), ISD (e.g., 500m, 200m), UE speed (e.g., 30/90 km/h for goal 1 and 60/120 km/h for goal 2), gNB height (e.g., 25m, 10m), and UE height (e.g., 1m, 1.5m).
		- Configurations (parameters and settings), including gNB settings (e.g., DL Tx beam codebook), UE parameters (e.g., Rx beam number), set B of beam (pairs) for spatial domain prediction, and sample period/measurement period.
* R2-2409829
	+ Proposal 5: RAN2 to study generalization issue on RRM measurement prediction in frequency domain with different frequency combinations.
	+ Proposal 6: RAN2 to verify the impact of including source/target frequency information as input of AI/ML to study generalization issue on RRM measurement prediction in frequency domain with different frequency combinations
* R2-2409869
	+ Proposal 14: RAN2 use the definition of model generalization:
		- Model generalization, i.e., using one model that is generalizable to different scenarios/configurations/areas.
	+ Proposal 16: RAN2 consider to study the impact of setting(scenarios/configurations/areas) on model generalization, including UE speed, beam pattern, and the collection area of data.
	+ Proposal 18: To evaluate the impact of data collection area, considering following options:
		- Model trained with dataset of one certain cell, apply inference on certain cell (one model for one cell).
		- Model trained with dataset of cluster(all cells), apply inference on any one cell of the cluster (one model for cluster);
		- Model trained with dataset of one cell, apply inference on any other of cells within the cluster (one model for cluster);
* R2-2409972
	+ Proposal 7: model generalization refers to generalization across cells with potentially different configuration. It is evaluated in a limited number of scenarios of high priority for RRM measurement prediction.
	+ Proposal 9: to use field data for mode generalization study; to discuss simulation assumptions to generate an environment with multiple different cell configurations (for model generalization study).
* R2-2410023
	+ Proposal 3
		- Study the generalization aspects according to the prediction domain of the use cases.
			* For Case 2 and 4 (temporal domain), the aspects are
				+ UE speed,
				+ Temporal domain configurations (measurement period, observation window length, prediction window length).
			* For Case 3 (frequency domain), the aspect is
				+ The carrier frequencies and frequency gap between the two bands.
			* For Case 6 (spatial domain), the aspects are
				+ TXRU mapping, tilt angle, and SSB/CSI-RS beam number and pattern.
* R2-2410263
	+ Proposal 3 For generalization purposes, the following parameters can be prioritized in the study:
		- UE speed: the AI/ML model is trained using a certain UE speed and the AI/ML model performs inference for a UE with a different speed, including stationary UEs.
		- Frequency: The AI/ML model is trained using a certain frequency, but the inference is done using another frequency.
		- Cell size: the AI/ML model is trained for small cells, but the inference is done for large cells.
	+ Proposal 8 For generalization evaluation over cell size:
		- Training dataset is small cells, and inference dataset is large cells.
		- Training dataset is large cells and inference dataset is small cells.
* R2-241054
	+ Proposal 4: To verify how well the AIML model can be generalized, RAN2 should check the following (a prioritization discussion is expected):
		- how well the model trained in one frequency (e.g. 2GHz) performs in another one (e.g. 4GHz)
		- how well the model trained in a certain deployment scenario performs on another one, e.g. UMa, UMi deployments, different ISDs
		- how well a model trained in a certain cell configuration perform in another one, e.g. gNB/UE antenna heights, different UE/gNB port settings, different number of beams etc.
		- how well the same model works for different prediction window lengths
* R2-2410800
	+ Proposal 3: For generalization performance verification, consider the following scenario/configuration:
		- Scenarios:
			* Various deployment scenarios, e.g., UMa, UMi and others; e.g., 200m ISD or 500m ISD and others; e.g., same deployment, different cells with different configuration/assumption; e.g., gNB height and UE height;
			* Various UE mobility, e.g., 30km/h, 60km/h, 90km/h, and 120km/h.
		- Configurations (parameters and settings):
			* Various UE parameters, e.g., number of UE Rx beams, UE antenna configuration, measurement period, L3 filtering parameter, system bandwidth
			* Various gNB settings, e.g., the number of BS Tx beams, BS Antenna configuration.
* R2-2410345
	+ Proposal 2: For intra-frequency temporal prediction, the following aspects can be considered to verify the generalization performance of an AI/ML model over various configurations:
		- UE speed (e.g. 30km/h, 60km/h, 90km/h, etc.)
		- the number of TX/RX (e.g. 1/1,1/2,1/4 for FR1, 8/4,16/4,32/4 for FR2)
		- MRRT for FR1 (e.g. 50%, 80%)
		- OW/PW (e.g. 5/1, 4/1, 1/1, 1/2, etc.)

Based on the proposals listed above, it appears that the following would be a fair summary of all the cell configuration parameters proposed for the generalization study (with comments from the moderator):

1. deployment scenarios/channel model
* Moderator’s comments:
	+ Only UMa and UMi have been agreed so far
	+ Furthermore, UMa was agreed for FR1 and UMi for FR2
1. ISD
* Moderator’s comments:
	+ Only 500m and 200m have been agreed so far
	+ Furthermore, 500m was agreed for FR1 and 200m for FR2
1. BS antenna height (e.g., 25m, 10m)
* Moderator’s comments:
	+ Only 10m and 25m have been agreed so far
	+ Furthermore, 25m has been agreed for FR1 and 10m for FR2
1. BS antenna configuration
* Moderator’s comments:
	+ In currently agreed spreadsheets, the following is used for FR1
		- 32 ports: (8,8,2,1,1,2,8), (dH,dV) = (0.5, 0.8)λ
		- 16 ports: (8,4,2,1,1,2,4), (dH,dV) = (0.5, 0.8)λ
	+ In currently agreed spreadsheets, the following is used for FR2
		- Antenna setup and port layouts at gNB: (4, 8, 2, 1, 1, 1, 1), (dV, dH) = (0.5, 0.5) λ
1. BS antenna radiation pattern
* Moderator’s comments:
	+ In currently agreed spreadsheets, the following is used for FR1
		- 3-sector antenna radiation pattern, 8 dBi
	+ In currently agreed spreadsheets, the following is used for FR2
		- TR 38.802 Table A.2.1-6
1. BS antenna tilt
* Moderator’s comments:
	+ No explicit agreements in RAN2
1. Number of Tx beams
* Moderator’s comments:
	+ 1,2 and 4 have been agreed for FR1
	+ 8, 16, and 32 have been agreed for FR2
1. BS Tx power
* Moderator’s comments:
	+ This is my interpretation of the proposal to generalize across “small vs large cells”
	+ In currently agreed spreadsheets 44 dBm is used for FR1 and 40 dBm for FR2
1. Usage of field data:
* Moderator’s comments:
	+ This is not strictly speaking a network configuration parameter, but it sort of incorporates all of them

### Question 1

**Question 1: which of the parameters listed above you prefer to use for the generalization across different cell configurations study? Please try to limit your response to the lowest number of parameters you can accept. Please consider providing additional technical details for your favourite parameters in the comments column, if needed.**

|  |  |  |
| --- | --- | --- |
| Company | Preferred parameters | Comments |
| Ericsson | a), b), c) and h) all together | We believe for a realistic evaluation of the generalization across “small vs large cell”, the parameters a), b), c), h) should be jointly considered. That is, in a real scenario, a change of one parameter implies changes of the other parameters. In this respect we propose the following configurations.* Only one frequency is used, e.g.: FR1
* Parameter values used for small cell
	+ a) deployment scenarios: UMi
	+ b) ISD = 200m
	+ c) BS antenna height = 10m
	+ h) BS Tx power = 40dBm
* Parameter values used for large cell
	+ a) deployment scenarios: UMa
	+ b) ISD = 500m
	+ c) BS antenna height = 25m
	+ h) BS Tx power = 44dBm

The “small vs large cell” generalization is done by training the model using the parameters with values for small cell, and inference on the data collected in the network with cells the parameters associated to the large cell (or vice versa). |
| Nokia | See comments | In our view, the order of importance would be: a) deployment scenarios/channel model, including changing the LOS/NLOS and shadow fading random seeds and UE trajectoriesb) ISD and c) BS antenna height h) BS Tx powerg) Number of Tx beamsThen d) e) f).  |
| Huawei | b), c), d), h), all together | We agree with the approach proposed by Ericsson, i.e. to evaluate the model in two different cell configurations, combining several different parameter settings. But in our view, it is better to focus on the UMa deployment with different cell sizes/settings, because such cells are more likely co-exist and being deployed next to each other on a certain area. Also, this would limit the workload a bit as, so far, we considered UMa only. Hence, we propose the following scenarios, starting from Ericsson’s proposal:* Frequency – FR1
* Parameter values used for Parameter-Set A
	+ b) ISD = 200m
	+ c) BS antenna height = 10m
	+ d) BS antenna configuration 16 ports: (8,4,2,1,1,2,4), (dH,dV) = (0.5, 0.8)λ
	+ h) BS Tx power = 40dBm
* Parameter values used for Parameter-Set B
	+ b) ISD = 500m
	+ c) BS antenna height = 25m
	+ d) BS antenna configuration 32 ports: (8,8,2,1,1,2,8), (dH,dV) = (0.5, 0.8)λ
	+ h) BS Tx power = 44dBm
 |
| NTT DOCOMO | g, a, b, c | We have a similar view to Ericsson’s. These parameters are mutually impacted in practical deployments. Therefore, it is not necessary to study them separately. Several combinations can be considered, e.g., considering the following two combinations for FR2, Config. 1: (g = 32, a = UMi, b = 200m, c = 10m)Config. 2: (g = 16, a = UMa, b = 500m, c = 25m)For FR1, different *g) Number of Tx beams* can be further considered based on the two sets of parameters suggested by Ericsson. |
| vivo | Combination of a), b), c) and h) for both FR1 and FR2 as 1st priority and d) or g) as 2nd priority. | To relieve the workload of simulation, we agree with Ericsson on combining multiple parameters for generalization simulation as a starting point. However, as the generalization study on FR1 is for temporal domain case B and the study on FR2 is for temporal domain case A, we think both FR1 and FR2 should be considered. If one single FR is to be selected, we think FR2 should be prioritized to optimize mobility performance.Based on 38.901, UMa and UMi are two typical high-level descriptions of deployment scenarios, which will reflect multiple typical evaluation parameters as follows. For instance, ISD is 200m for UMi and 500m for UMa; BS antenna height is 10m for UMi and 25m for UMa.Table 7.2-1: Evaluation parameters for UMi-street canyon and UMa scenarios

|  |  |  |
| --- | --- | --- |
| Parameters | UMi - street canyon | UMa |
| Cell layout | Hexagonal grid, 19 micro sites, 3 sectors per site (ISD = 200m) | Hexagonal grid, 19 macro sites, 3 sectors per site (ISD = 500m) |
| BS antenna height  | 10m | 25m |
| UT location | Outdoor/indoor | Outdoor and indoor | Outdoor and indoor |
| LOS/NLOS | LOS and NLOS | LOS and NLOS |
| Height  | Same as 3D-UMi in TR36.873 | Same as 3D-UMa in TR36.873 |
| Indoor UT ratio | 80% | 80% |
| UT mobility (horizontal plane only) | 3km/h | 3km/h |
| Min. BS - UT distance (2D) | 10m | 35m |
| UT distribution (horizontal) | Uniform | Uniform |

Therefore, no need to consider the ISD and antenna height individually. Besides, based on the generalization simulation results of beam management in 38.843, with ISD 200m/ISD 500m, for generalization Case 2 compared to Case 1, evaluation results from 3 sources show about 1%~2% degradation.To study the comprehensive generalization ability of the model in different scenarios for different goals, two sets of parameters in these two scenarios for FR1 and FR2 can be considered. The parameters proposed by Ericsson can be the baseline:* ~~Only one frequency is used, e.g.: FR1~~
* Parameter values set 1
	+ a) deployment scenarios: UMi
	+ b) ISD = 200m
	+ c) BS antenna height = 10m
	+ h) BS Tx power = 40dBm
* Parameter values set 2
	+ a) deployment scenarios: UMa
	+ b) ISD = 500m
	+ c) BS antenna height = 25m
	+ h) BS Tx power = 44dBm

As to the impact of gNB antenna configuration, i.e., d), proposed by Huawei, we think it should be studied individually since gNB antenna configuration can be different for the same deployment scenario in different areas. Due to limited time, it can be optional and with 2nd priority. For FR2, as only one antenna setup and port layouts were agreed, the number of Tx beams, i.e., parameter g), can be considered for generalization simulation.  |

### Question 2

**Question 2: any additional parameters not listed above we should consider? If you chose to suggest an additional parameter, please provide a technical justification.**

|  |  |  |
| --- | --- | --- |
| Company | Additional parameters | Comments |
| Nokia | Control of random seeds:spatial channel model, UE trajectory, etc | We have some doubts on the categorization of the above configurations into “cell parameters”. First, the generalization aspects being considered are about simulation studies, so we need to understand which part may affect the DL radio measurements for all the use cases (mainly RRM prediction). All the above listed parameters can affect path-loss, propagation. However, the discussion on control of random seeds for channel model, UE trajectory seems to be missing. We think this is also important for generalization aspects. |
|  |  |  |

# 3 Proposals

[TBD]

# 5 References

[1] R2-2409652 Discussion on generalization for RRM prediction CATT, Turkcell

[2] R2-2409668 Discussion on generalization study for RRM prediction vivo

[3] R2-2409829 Discussion on Generalization Issues for AI/ML Mobility Samsung

[4] R2-2409869 Simulation Assumptions of SLS, measurement event prediction, RLF prediction and generalzatiion study MediaTek Inc.

[5] R2-2409972 Model generalization, RLF evaluation assumptions, etc. Apple

[6] R2-2410023 Discussions on evaluation methodology of AI/ML for mobility NTT DOCOMO, INC.

[7] R2-2410263 Discussion on generalization aspects Ericsson

[8] R2-2410540 Discussion on simulation assumptions and generalization Huawei, HiSilicon

[9] R2-2410800 Discussion on generalization aspects and simulation assumption ZTE Corporation

[10] R2-2410345 Discussion on other aspects of simulation assumption CMCC