**3GPP TSG-RAN WG2 Meeting #129**  **R2-2500xxx**

**Athens, Greece, Feb. 17th – 21st, 2025**

Agenda Item: 8.6.2

Source: CATT

**Title:** Report of [POST129][111][MOB] (CATT)

**Document for:** Discussion and Decision

# Introduction

This document is the report of the following email discussion.

* **[POST129][111][MOB] (CATT)**

**Scope:** Discuss UE capability open issues in R2-2500224.

**Intended outcome:** Discussion summary.

**Deadline: Long email discussion**

|  |  |
| --- | --- |
| **Company** | **Name (Email)** |
| MediaTek | Xiaonan.zhang@mediatek.com |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# UE capability open issues

In paper R2-2500224, there are some initial considerations on the high-layer specific UE capabilities for inter-CU LTM and CLTM.

***Note: The email discussion will be performed directly based on the proposals from R2-2500224.***

## Inter-CU LTM

To support intra-CU LTM in R18, the capabilities indicating whether a UE can support intra-frequency MCG/SCG LTM have been defined on a per-band basis, namely ltm-MCG - IntraFreq-r18 and ltm-SCG-IntraFreq-r18. Meanwhile, the capability specifying whether a UE can support inter-frequency MCG/SCG LTM, denoted as ltm-InterFreq-r18, has been defined on a per-UE basis. Since the main difference between inter-CU LTM and intra-CU LTM lies in the L2 behavior, these capabilities can be reused for inter-CU LTM scenarios.

Similarly, the capabilities related to beam indication with TCI/L1 measurement/UE fast processing/RACH-Less/TA acquisition/LTM for MCG with or without of NR-DC, can also be reused for inter - CU LTM. The detailed capabilities are presented in Annex A.

**Proposal 1: The following R18 intra-CU LTM related capabilities are reused for inter-CU LTM, separate capabilities are not needed.**

* **Intra-frequency LTM/inter-frequency LTM**
* **beam indication with TCI/L1 measurement**
* **UE fast processing**
* **RACH-Less**
* **TA acquisition**
* **LTM for MCG with or without of NR-DC**

### Question 1

**Do you think P1 is agreeable?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes or No** | **Comments if any** |
| MediaTek | Yes | It seems Annex A includes almost all R18 LTM capabilities. Could rapporteur clarify which capability is NOT included in Annex A and need further modification in R19 inter-CU LTM for simplicity?  Besides, for the capabilities in Annex A,   1. The ltm-Recovery-r18 may need further discussion, as we are unsure the fast recovery procedure for R19 inter-CU LTM. 2. The ltm-ReferenceConfig-r18 may need further discussion, if the reference configuration for inter-CU differs much than intra-CU (not sure about this one)   The following capabilities are not included in Annex A, but we think they should be (can be reused):  L1 MR related:   * currentSpCellInclL1-Report-r18 (per BC) * supportedMaxCellsWithoutGapsL1-Meas-r18 (per BC) * supportedMaxSSB-WithinSlotL1-Meas-r18 (per BC) * supportedMaxSSB-L1-Meas-r18 (per BC)   Early TA related:   * pdcch-RACH-AffectedBandsList-r18 (per FS) * pdcch-RACH-PrepTimeList-r18 (per FS) * pdcch-RACH-SwitchingTimeList-r18 (per FS) |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

As a new functionality, UE capability is to be defined for “inter-CU LTM”. Given the distinct UE behaviors in inter-CU SCG LTM and inter-CU MCG LTM, it is advisable to have separate capabilities for inter-CU MCG LTM and inter-CU SCG LTM. Moreover, these capabilities ought to be configured on a per - UE basis.

**Proposal 2: Define per-UE capabilities for inter-CU MCG LTM and inter-CU SCG LTM e.g. ltm-interCU-MCG-r19 and ltm-interCU-SCG-r19. UE supports these capabilities should also support ltm-MCG-IntraFreq-r18 or ltm-SCG-IntraFreq-r18 respectively.**

### Question 2

**Do you think P2 is agreeable?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes or No** | **Comments if any** |
| MediaTek | Yes |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## Conditional LTM

As only the conditional intra-CU LTM in non-DC is supported, hence only this case is taken into consideration in the following discussion.

In R16 CHO, the capability of condHandover-r16 is defined on a per band basis, the same way can be reused for conditional LTM.

**Proposal 3: Define a per-band capability for conditional LTM e.g. cltm-IntraCU-MCG-r19.It indicates whether the UE supports intra-CU MCG LTM on the band where the UE is in non-DC. This includes supports execution condition, subsequent LTM. UE supports this capability should support ltm-MCG-IntraFreq-r18 on the same band.**

### Question 3

**Do you think P3 is agreeable?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes or No** | **Comments if any** |
| MediaTek | Yes | “Conditional” is missing in P3:  “It indicates whether the UE supports intra-CU MCG Conditional LTM on the band where the UE is in non-DC” |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

It was agreed that both L3 based execution condition and L1 based execution condition are supported for C-LTM. And only one triggering event is associated with L1 execution condition, but one or two triggering events can be associated with L3 execution condition as CHO.

1. The triggering condition of conditional LTM can be based on L3 measurement.
2. CondEventA3 and CondEventA5 conditions can be baseline for the conditional LTM execution.
3. The L1 execution condition of a candidate cell is associated to only one triggering event.
4. For L3 execution condition, it may consist of one or two triggering condition(s). If there are two triggering conditions associated with the same candidate cell, the UE shall consider the execution condition is fulfilled only when both triggering conditions are met. Only single RS type is supported and at most two different trigger quantities can be configured simultaneously for the evaluation of execution condition of a single candidate cell.

Hence separate capability can be defined for L1 and L3 execution condition. UE supports CLTM should support at least one of the two capabilities. In R16 CHO, the capability of condHandoverTwoTriggerEvents-r16 is defined per band, the same way can be reused for these related execution condition capabilities for conditional LTM. i.e. define these capabilities to be per band capability.

**Proposal 4: Define a per-band capability for L1 execution condition, e.g.** **cltm-ExecutionConditionL1-r19 is defined to indicate whether the UE supports L1 execution condition for conditional LTM. The UE supports this capability should support cltm-IntraCU-MCG-r19 on the same band.**

### Question 4

**Do you think P4 is agreeable?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes or No** | **Comments if any** |
| MediaTek | Yes |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Proposal 5: Define a per-band capability for L3 execution condition, e.g.** **cltm-ExecutionConditionL3-r19 is defined to indicate whether the UE supports L3 execution condition for conditional LTM and whether the UE supports 2 trigger events for same execution condition. UE supports this capability should support cltm-IntraCU-MCG-r19 on the same band.**

### Question 5

**Do you think P5 is agreeable?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes or No** | **Comments if any** |
| MediaTek | Yes |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Proposal 6: A UE that supports conditional LTM (i.e., cltm-IntraCU-MCG-r19) should indicate the support for at least one of cltm-ExecutionConditionL3-r19 or cltm-ExecutionConditionL1-r19.**

### Question 6

**Do you think P6 is agreeable?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes or No** | **Comments if any** |
| MediaTek | Yes |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

It has agreed CG based RACH-Less LTM is supported for C-LTM, the capability of ltm-RACH-LessCG-r18 can be reused for C-LTM. If the UE indicates support of cltm-IntraCU-MCG-r19 and ltm-RACH-LessCG-r18, it indicates that the UE supports RACH-less conditional LTM with configured grant.

**Proposal 7: When a UE indicates support for both conditional LTM (i.e., cltm-IntraCU-MCG-r19) and ltm-RACH-LessCG-r18, it implies that the UE has the capacity to support RACH-less conditional LTM with a configured grant.**

### Question 7

**Do you think P7 is agreeable?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes or No** | **Comments if any** |
| MediaTek | Yes, but | In the description of ltm-RACH-LessCG-r18, it is mentioned UE should also support at least one band of either ta-IndicationCellSwitch-r18 or ue-TA-Measurement-r18.  But as discussed in Q9, ta-IndicationCellSwitch-r18 will not be used for R19 CLTM and a new capability is introduced. Does it introduce compatibility issue if we reuse ltm-RACH-LessCG-r18 for R19 CLTM? |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Conditional LTM supports UE based early TA acquisition and PDCCH order based TA acquisition. Due to there is no difference between the UE behaviors of UE based TA measurement for LTM and conditional LTM, hence the capability of ue-TA-Measurement-r18 could be reused for CLTM and LTM.

**Proposal 8a: Reuse the R18 capability (i.e., ue-TA-Measurement-r18) to indicate whether UE supports UE-based TA measurement for C-LTM. There is no need to define a separate capability for this purpose.**

### Question 8a

**Do you think P8a is agreeable?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes or No** | **Comments if any** |
| MediaTek | Yes |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

However, in the case of PDCCH order-based TA acquisition, it mandates that the UE acquires the TA (Timing Advance) value prior to CLTM execution. Moreover, for CLTM, the UE must maintain this TA value using a new timer. This process differs from the R18 PDCCH-ordered TA acquisition mechanism.

In R18 LTM, the UE capability rach-EarlyTA-Measurement-r18 is defined for PDCCH ordered TA acquisition.

| ***rach-EarlyTA-Measurement-r18***  Indicates the maximum number of candidate cells for TA acquisition based on PDCCH ordered CFRA procedure before receiving cell switch command MAC-CE. Power ramping for PRACH retransmission based on PDCCH order indication. UE also supports dropping the serving cell UL to handle the overlap between UL transmission on serving cell(s) and PRACH on candidate cell(s).  A UE supporting this feature shall also indicate support of *ta-IndicationCellSwitch-r18* and at least one of *ltm-MCG-IntraFreq-r18* or *ltm-SCG-IntraFreq-r18*. | Band | No | N/A | N/A |
| --- | --- | --- | --- | --- |

Whether new capability is needed for PDCCH order TA acquisition in CLTM should be discussed.

**Proposal 8b: RAN2 discuss whether rach-EarlyTA-Measurement-r18 could be reused for PDCCH order TA acquisition in CLTM.**

### Question 8b

**Do you think rach-EarlyTA-Measurement-r18 could be reused for PDCCH order TA acquisition in CLTM?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes or No** | **Comments if any** |
| MediaTek | No | We believe a new capability(s) is needed due to the introduction of the TA timer maintenance of candidate cells. This capability is abandoned as the new capability is introduced. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

RAN2 has reached an agreement that the network can convey the timing advance (TA) information of the candidate cell to the UE through a new MAC CE. In light of this, a new capability needs to be defined for TA indication in the context of CLTM.

**Proposal 9: Define a per-band capability, such as “cltm-TA-Indication-r19”. This capability serves to indicate whether the UE can support TA indication within the early TA MAC CE for conditional LTM.**

### Question 9

**Do you think P9 is agreeable?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes or No** | **Comments if any** |
| MediaTek | Yes |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

There was also an agreement to reuse the Candidate Cell TCI States Activation/Deactivation MAC CE for the early activation or deactivation of the CLTM candidate cell. The capabilities defined for R18 LTM, namely “ltm-MAC-CE-JointTCI-r18” and “ltm-MAC-CE-SeparateTCI-r18”, can be reused. As such, there is no necessity to define a new capability for CLTM in this regard.

**Proposal 10: Reuse the R18 capability (i.e., ltm-MAC-CE-JointTCI-r18 and ltm-MAC-CE-SeparateTCI-r18) to indicate whether the UE supports MAC-CE activated joint/separate LTM TCI states for CLTM.**

### Question 10

**Do you think P10 is agreeable?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes or No** | **Comments if any** |
| MediaTek | Yes |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## Other UE capability open issues

This section is to collect other UE capability open issues identified by companies.

### Question 11

**Do you identify other UE capability open issues?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes or No** | **Comments if any** |
| MediaTek |  | We assume the following Annex A is only for inter-CU LTM. In the case of CLTM, do we need a question similar to Question 1 to discuss which R18 LTM capabilities can be reused? |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Conclusion

# Reference

1. 3GPP TS 38.306, " NR;User Equipment (UE) radio access capabilities"

# Annex A

| ***ltm-BeamIndicationJointTCI-r18***  Indicates whether the UE supports unified TCI with joint DL/UL LTM TCI-state indication for LTM procedure, indicating and activating a single joint LTM TCI state in a cell switch command.  This capability comprises the following parameters:  - *maxNumberJointTCI-PerCell-r18* indicates the maximum number of configured joint LTM TCI state(s) per candidate cell  - *qcl-Resource-r18* indicates of the supported QCL source RS in the LTM TCI-state- configuration.  - *maxNumberJointTCI-AcrossCells-r18* indicates index *N* of the maximum number of configured joint DL LTM TCI state(s) across candidate cells. The maximum number of configured joint LTM TCI state(s) across candidate cells is *N*\*8, where *N*={1..128}.  - *maxNumberCells-r18* indicates the maximum number of configured cells for joint LTM TCI state(s).  A UE supporting this feature shall also indicate support of *unifiedJointTCI-r17* and at least one of *ltm-MCG-IntraFreq-r18* or *ltm-SCG-IntraFreq-r18*. |
| --- |
| ***ltm-BeamIndicationSeparateTCI-r18***  Indicates whether the UE supports unified TCI with separate DL/UL TCI-state indication for LTM procedure and indicating/activating a pair of UL/DL TCI-state in a cell switch command.  This capability comprises the following parameters:  - *maxNumberDL-TCI-PerCell-r18* indicates the maximum number of configured DL TCI state(s) per candidate cell.  - *maxNumberUL-TCI-PerCell-r18* indicates the maximum number of configured UL TCI state(s) per candidate cell.  - *qcl-Resource-r18* indicates the supported QCL source RS in the LTM TCI-state configuration.  - *maxNumberDL-TCI-AcrossCells-r18* indicates value *N* of the maximum number of configured separate DL LTM TCI state(s) across candidate cells. The maximum number of configured separate DL LTM TCI state(s) across candidate cells is *N*\*8, where *N*={1..128}.  - *maxNumberUL-TCI-AcrossCells-r18* indicates value *N* of the maximum number of configured separate UL LTM TCI state(s) across candidate cells. The maximum number of configured separate UL LTM TCI state(s) across candidate cells is *N*\*8, where *N*={1..64}.  - *maxNumberCells-r18*indicates the maximum number of configured cells for separate DL/UL LTM TCI states  A UE supporting this feature shall also indicate support of *unifiedSeparateTCI-r17* and at least one of *ltm-MCG-IntraFreq-r18* or *ltm-SCG-IntraFreq-r18*. |
| ***ltm-FastProcessingConfig-r18***  Indicates whether the UE supports fast processing of LTM candidate cell RRC configuration. This capability signalling comprises the following parameters:  - *maxNumberStoredConfigCells-r18* indicates the maximum number of serving cell(s) and candidate cell(s), including serving SpCell(s), serving SCell(s) in MCG and SCG, SpCell in LTM candidate configurations and Scell(s) in LTM candidate configurations for MCG and SCG, that UE can store the configurations.  - *maxNumberConfigs-r18* represents the maximum number of LTM candidate configuration for which the UE can perform early ASN.1 decoding and validity check, as described in TS 38.133 [5].  A UE supporting this capability shall also indicate support of *ltm-MAC-CE-JointTCI-r18* or *ltm-MAC-CE-SeparateTCI-r18*. UE shall set the capability values for *maxNumberStoredConfigCells-r18* and *maxNumberConfigs-r18* consistently for all bands. These capability values represent the maximum number across all the supported bands.  NOTE: The conditions for fast processing of an LTM candidate cell RRC configuration is defined in clause 6.3 in TS 38.133 [5]. |
| ***ltm-MAC-CE-JointTCI-r18***  Indicates whether the UE supports MAC-CE activated joint LTM TCI states.  This capability comprises the following parameters:  - *qcl-Resource-r18* indicates the supported QCL source RS for MAC-CE activated DL/UL LTM TCI states configuration.  - *maxNumberJointTCI-PerCell-r18* indicates the maximum number of MAC-CE activated joint LTM TCI states per candidate cell.  - *maxNumberJointTCI-AcrossCells-r18* indicates the maximum number of MAC-CE activated joint LTM TCI states across candidate cells and serving cell TCI states across serving cells in the band.  A UE supporting this feature shall also indicate support of *ltm-BeamIndicationJointTCI-r18*.  NOTE: The maximum number of MAC-CE activated joint TCI states across all servings cells is limited by of *unifiedJointTCI-r17.* |
| ***ltm-MAC-CE-SeparateTCI-r18***  Indicates whether the UE supports MAC-CE activated DL/UL LTM TCI states.  This capability comprises the following parameters:  - *qcl-Resource-r18* indicates the supported QCL source RS for MAC-CE activated DL/UL LTM TCI states configuration.  - *maxNumberDL-TCI-PerCell-r18* indicates the maximum number of MAC-CE activated DL TCI states per candidate cell.  - *maxNumberUL-TCI-PerCell-r18* indicates the maximum number of MAC-CE activated UL TCI states per candidate cell.  - *maxNumberDL-TCI-AcrossCells-r18* indicates the maximum number of MAC-CE activated LTM DL TCI states across all candidate cells and serving cell DL TCI states across all serving cells.  - *maxNumberUL-TCI-AcrossCells-r18* indicates the maximum number of MAC-CE activated UL TCI states across all candidate cells and serving cell UL TCI states across all serving cells in the band.  A UE supporting this feature shall also indicate support of *ltm-BeamIndicationSeparateTCI-r18*.  The maximum number of MAC-CE activated DL/UL TCI states across all servings cells is limited by *unifiedSeparateTCI-r17.* |
| ***ltm-MCG-IntraFreq-r18***  Indicates whether the UE supports intra-frequency LTM for MCG with RACH as defined in TS 38.331 [9] and TS 38.321 [8] without NR-DC configured. UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively.  UE supporting this feature shall also indicate support for *ltm-BeamIndicationJointTCI-r18* or *ltm-BeamIndicationSeparateTCI-r18*. |
| ***ltm-SCG-IntraFreq-r18***  Indicates whether the UE supports intra-frequency LTM for SCG with RACH as defined in TS 38.331 [9] and TS 38.321 [8]. UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively.  UE supporting this feature shall also indicate support for *ltm-BeamIndicationJointTCI-r18* or *ltm-BeamIndicationSeparateTCI-r18*. |
| ***rach-EarlyTA-Measurement-r18***  Indicates the maximum number of candidate cells for TA acquisition based on PDCCH ordered CFRA procedure before receiving cell switch command MAC-CE. Power ramping for PRACH retransmission based on PDCCH order indication. UE also supports dropping the serving cell UL to handle the overlap between UL transmission on serving cell(s) and PRACH on candidate cell(s).  A UE supporting this feature shall also indicate support of *ta-IndicationCellSwitch-r18* and at least one of *ltm-MCG-IntraFreq-r18* or *ltm-SCG-IntraFreq-r18*. |
| ***ta-IndicationCellSwitch-r18***  Indicates whether the UE supports TA indication in cell switch command.  A UE supporting this feature shall also indicate support of at least one of *ltm-MCG-IntraFreq-r18* or *ltm-SCG-IntraFreq-r18*. |
| ***ue-TA-Measurement-r18***  Indicates whether the UE supports UE-based TA measurement by indicating the maximum number of candidate cells that the UE maintains the TA for.  A UE supporting this feature shall also indicate the support of at least one of *ltm-MCG-IntraFreq-r18* or *ltm-SCG-IntraFreq-r18*. |
| ***interFreqL1-MeasConfig-r18***  Indicates whether UE supports inter-frequency L1-RSRP measurement and reporting based on SSB(s) of candidate cell(s), regardless whether the candidate cell(s) are inside or outside of the BC (unless the UE also indicates support of *ltm-interFreqL1-OnlyInBC-r18*).  This capability signalling comprises of the following parameters:  - *supportedMaxIntraInterFreqCellsConfig-r18* indicates the maximum number of RRC configured candidate cells for intra- and inter-frequency L1-RSRP measurement;  - *supportedMaxIntraInterFreqCellsPerReport-r18* indicates maximum number of candidate cells in one report where a SSBRI-RSRP pair is used for each beam report for intra- and inter-frequency L1-RSRP measurement;  - *supportedMaxIntraInterFreqBeamsPerCellReports-r18* indicates maximum number of candidate beams per candidate cell in one report where a SSBRI-RSRP pair is used for each beam report for intra- and inter-frequency L1-RSRP measurement;  - *supportedMaxIntraInterFreqBeamsReports-r18* indicates maximum number of candidate cells beams in total across all cells in one report where a SSBRI-RSRP pair is used for each beam report for intra- and inter-frequency L1-RSRP measurement;  UE supporting this feature shall also indicate support of *intraFreqL1-MeasConfig-r18*. |
| ***interFreqSSB-L1-MeasWithoutGaps-r18***  Indicates whether UE supports SSB based inter-frequency L1-RSRP measurements on SSBs within active DL BWP without measurement gaps (without interruption on serving cell(s)) for LTM.  UE supporting this feature shall also indicate support of *interFreqL1-MeasConfig-r18.* |
| ***intraFreqL1-MeasConfig-r18***  Indicates whether UE supports intra-frequency L1-RSRP measurement and reporting based on SSB(s) of candidate cell(s).  This capability signalling comprises of the following parameters:  - *supportedMaxIntraFreqCellsConfig-r18* indicates the maximum number of RRC configured candidate cells for intra-frequency L1-RSRP measurement;  - *supportedMaxIntraFreqCellsPerReport-r18* indicates the maximum number of candidate cells in one report where a SSBRI-RSRP pair is used for each beam report for intra-frequency L1-RSRP measurement;  - *supportedMaxReportBeamsPerReportedCell-r18* indicates the maximum number of candidate beams per candidate cell in one report where a SSBRI-RSRP pair is used for each beam report for intra-frequency L1-RSRP measurement;  - *supportedMaxReportBeamsReports-r18* indicates the maximum number of candidate beams in total across all cells in one report where a SSBRI-RSRP pair is used for each beam report for intra-frequency L1-RSRP measurement;  - *supportedMaxAperiodic-LTM-CSI-ReportConfig-r18* indicates maximum number of aperiodic *LTM-CSI-ReportConfig*;  - *supportedMaxPeriodic-LTM-CSI-ReportConfig-r18* indicates maximum number of periodic *LTM-CSI-ReportConfig*;  - *supportedMaxSemiPersistent-LTM-CSI-ReportConfig-r18* indicates maximum number of semi-persistant *LTM-CSI-ReportConfig*;  UE supporting this feature shall also indicate support of *periodicBeamReport* or *aperiodicBeamReport* or *sp-BeamReportPUCCH* or *sp-BeamReportPUSCH.* |
| ***maxFreqLayersL1-Meas-r18***  Indicates the number of frequency layers for L1-RSRP measurement.  This capability signalling comprises of the following parameters:  - *supportedMaxIntraInterFreqLayersWithoutGaps-r18* indicates the maximum number of frequency layers UE can measure for intra- and inter-frequency without measurement gaps L1-RSRP measurement.  A UE indicating support for this component shall also indicate support for *intraFreqL1-MeasConfig-r18* and/or *interFreqSSB-L1-MeasWithoutGaps-r18.*  - *supportedMaxInterFreqLayersWithGaps-r18* indicates the maximum number of frequency layers UE can measure for inter-frequency L1-RSRP measurement with measurement gaps. A UE indicating support for this component shall also indicate support for *ltm-InterFreqMeasGap-r18*. |
| ***maxNeighCellsPerFreqLayerL1-Meas-r18***  Indicates the number of neighbouring cells per frequency layer for L1-RSRP measurement.  This capability signalling comprises of the following parameters:  - *supportedMaxNeighCellsPerFreqLayersWithoutGaps-r18* indicates the max number of neighbour cells UE can measure for L1-RSRP per frequency layer for intra-frequency or inter-frequency without measurement gaps.  A UE indicating support for this component shall also indicate support for *intraFreqL1-MeasConfig-r18* or *interFreqSSB-L1-MeasWithoutGaps-r18.*  - *supportedMaxNeighCellsPerFreqLayersWithGaps-r18* indicates the max number of neighbour cells UE can measure for L1-RSRP per frequency layer for inter-frequency with measurement gaps. A UE indicating support for this component shall also indicate support for *ltm-InterFreqMeasGap-r18.* |
| ***maxSSB-PerFreqLayerL1-Meas-r18***  Indicates the maximum number of SSB resources for L1-RSRP measurement per frequency layer UE can measure.  This capability signalling comprises of the following parameters:  - *supportedMaxSSB-PerFreqLayersWithoutGaps-r18* indicates the max number of SSB resources UE can measure for L1-RSRP per frequency layer for intra-frequency or inter-frequency without measurement gaps.  A UE indicating support for this component shall also indicate support for *intraFreqL1-MeasConfig-r18* or *interFreqSSB-L1-MeasWithoutGaps-r18.*  - *supportedMaxSSB-PerFreqLayersWithGaps-r18* indicates the max number of SSB resources UE can measure for L1-RSRP per frequency layer for inter-frequency with measurement gaps. A UE indicating support for this component shall also indicate support for *ltm-InterFreqMeasGap-r18*. |
| ***multiCellL1-measRTD-greaterThan-CP-r18***  Indicates the capability of simultaneous L1-RSRP measurements for more than one cell when the max RTD among the cells on the same frequency layer or in the same active BWP is larger than CP length of the cell on the frequency layer or in the same active BWP.  A UE supporting this feature shall also indicate support of either *intraFreqL1-MeasConfig-r18, interFreqSSB-L1-MeasWithoutGaps-r18* or *ltm-InterFreqMeasGap-r18.* |
| ***ltm-FastUE-Processing-r18***  Indicates the reduced TLTM\_processing delay of the UE during cell switch.  The capability signalling includes the following parameters:  - *fr1-r18* indicates the reduced TLTM\_processing for cell switch from FR1 to FR1.  - *fr2-r18* indicates the reduced TLTM\_processing for cell switch from FR2 to FR2.  - *fr1-AndFR2-r18* indicates the reduced TLTM\_processing for cell switch from FR1/FR2 to FR2/FR1. |
| ***ltm-InterFreq-r18***  Indicates UE supports inter-frequency MCG LTM on all the bands where the UE indicates support of *ltm-MCG-IntraFreq-r18* or inter-frequency SCG LTM on all the bands where the UE indicates support of *ltm-SCG-IntraFreq-r18* respectively.  A UE supporting this feature shall also indicate support of *ltm-MCG-IntraFreq-r18* or *ltm-SCG-IntraFreq-r18.* |
| ***ltm-interFreqL1-OnlyInBC-r18***  When included, for each BC in which the UE indicates support of *interFreqL1-MeasConfig-r18*, the UE only supports inter-frequency L1-RSRP measurement and reporting based on SSB(s) of LTM candidate cell(s) that are inside the BC. When not included, the description in *interFreqL1-MeasConfig-r18* is applicable.  A UE supporting this feature shall also indicate support of *interFreqL1-MeasConfig-r18*. |
| ***ltm-InterFreqMeasGap-r18***  Indicates whether the UE supports SSB based inter-frequency L1-RSRP measurements with measurement gaps for LTM.  A UE supporting this feature shall also indicate support of *interFreqL1-MeasConfig-r18*. | |
| ***ltm-MCG-NRDC-r18***  Indicates whether the UE supports LTM for MCG with RACH with NR-DC configured as defined in TS 38.331 [9] and TS 38.321 [8]. UE indicating support for this feature shall also indicate support of *ltm-MCG-IntraFreq-r18.* | |
| ***ltm-MCG-NRDC-Release-r18***  Indicates whether the UE supports LTM for MCG with the release of NR-DC configuration as part of LTM execution when LTM cell switch command MAC CE is received. UE indicating support for this feature shall also indicate support of *ltm-MCG-IntraFreq-r18.* | |
| ***ltm-RACH-LessCG-r18***  Indicates whether the UE supports RACH-less LTM with configured grant for MCG LTM if the UE indicates support of *ltm-MCG-IntraFreq-r18* or for SCG LTM if the UE indicates support of *ltm-SCG-IntraFreq-r18* respectively.  UE indicating support for this feature shall also indicate support of either *ltm-BeamIndicationJointTCI-r18* or *ltm-BeamIndicationSeparateTCI-r18* for at least one band and either *ta-IndicationCellSwitch-r18* or *ue-TA-Measurement-r18*. | |
| ***ltm-RACH-LessDG-r18***  Indicates whether the UE supports RACH-Less LTM with dynamic grant, for MCG LTM if the UE indicates support of *ltm-MCG-IntraFreq-r18* or for SCG LTM if the UE indicates support of *ltm-SCG-IntraFreq-r18* respectively.  UE indicating support for this feature shall also indicate support of either *ltm-BeamIndicationJointTCI-r18* or *ltm-BeamIndicationSeparateTCI-r18* for at least one band and TA indication in *ta-IndicationCellSwitch-r18* or *ue-TA-Measurement-r18*. | |
| ***ltm-Recovery-r18***  Indicates whether the UE supports recovery procedure for MCG LTM execution when the selected cell in RRC re-establishment procedure is a LTM candidate as specified in TS 38.331 [9].  UE indicating support for this feature shall also indicate support of *ltm-MCG-IntraFreq-r18* for at least one band. | |
| ***ltm-ReferenceConfig-r18***  Indicates whether UE supports a reference configuration for LTM.  UE indicating support for this feature shall also indicate support of either *ltm-MCG-IntraFreq-r18* or *ltm-SCG-IntraFreq-r18* for at least one band. | |

# Annex B

UE feature list for Rel-19 mobility enhancement Ph4 based on above proposals.

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Features** | **Index** | **Feature group** | **Components** | **Prerequisite feature groups** | **Field name in TS 38.331 [2]** | **Parent IE in TS 38.331 [2]** | **Need of FDD/TDD differentiation** | **Need of FR1/FR2 differentiation** | **Note** | **Mandatory/Optional** |
| x. Mob\_enh\_Ph4 | x-1 | Inter-CU LTM | Indicates UE supports inter-CU MCG LTM on all the bands where the UE indicates support of *ltm-MCG-IntraFreq-r18* | support of intra-CU LTM as specified in TS 38.331 [2]. | *ltm-interCU-MCG-r19* | *measAndMobParametersCommon* | No | No | A UE supporting this feature shall also indicate support of *ltm-MCG-IntraFreq-r18* | Optional with capability signalling |
| x-2 | Inter-CU LTM | Indicates UE supports SN initiated inter-CU SCG LTM on all the bands where the UE indicates support of *ltm-SCG-IntraFreq-r18*. | support of Intra-CU LTM as specified in TS 38.331 [2]. | *ltm-interCU-SCG-r19* | *MeasAndMobParametersMRDC-Common-v1900* | No | No | A UE supporting this feature shall also indicate support of *ltm-SCG-IntraFreq-r18* | Optional with capability signalling |
| x-3 | Conditional LTM | Indicates whether the UE supports conditional intra-CU MCG LTM when the UE is in non-DC. Including execution condition, subsequent LTM. If the UE indicates support of ltm-RACH-LessCG-r18, it indicates the UE supporting RACH-less conditional LTM with configured grant. UE supporting this feature shall also indicate support of at least one of *cltm-ExecutionConditionL1-r19* or *cltm-ExecutionConditionL3-r19.* | support of Intra-CU LTM as specified in TS 38.331 [2]. | *cltm-IntraCU-MCG-r19* | BandNR | No | No | A UE supporting this feature shall also indicate support of *ltm-MCG-IntraFreq-r18* | Optional with capability signalling |
| x-4 | Conditional LTM | Indicates whether the UE supports L1 measurement based execution condition for conditional MCG LTM. | Support *cltm-IntraCU-MCG-r19* | *cltm-ExecutionConditionL1-r19* | BandNR | No | No | A UE supporting this feature shall also indicate support of *tm-CondIntraCU-MCG-r19.* | Optional with capability signalling |
| x-5 | Conditional LTM | Indicates whether the UE supports L3 measurement based execution condition for conditional MCG LTM and whether the UE supports 2 trigger events for same execution condition. | Support *cltm-IntraCU-MCG-r19* | *cltm-ExecutionConditionL3-r19* | BandNR | No | No | A UE supporting this feature shall also indicate support of *tm-CondIntraCU-MCG-r19.* | Optional with capability signalling |
| x-6 | Conditional LTM | Indicates whether the UE supports TA indication and maintain before conditional LTM execution.A UE supporting this feature shall also indicate support of ltm-CondIntraCU-MCG-r19. | Support *cltm-IntraCU-MCG-r19* | *cltm-TA-Indication-r19* | BandNR | No | No | A UE supporting this feature shall also indicate support of *tm-CondIntraCU-MCG-r19.* | Optional with capability signalling |