3GPP TSG RAN WG2#129 R2-250xxxx

Athens, Greece, 17th – 21st February, 2025

**Title: LS on number of beam measurements in the measurement report MAC CE**

**Response to: -**

**Release: Rel-19**

**Work Item: NR\_Mob\_Ph4-Core**

**Source: Huawei, HiSilicon [To be RAN2]**

**To: RAN1**

**Cc:**

**Contact person: Yinghao Guo**

**yinghaoguo@huawei.com**

**Send any reply LS to: 3GPP Liaisons Coordinator,** [**mailto:3GPPLiaison@etsi.org**](mailto:3GPPLiaison@etsi.org)

**Attachments:**

# 1 Overall description

In the previous RAN2 meetings, RAN2 has agreed that the event-triggered measurement report shall be transmitted via MAC CE. The MAC CE shall include the beam-level measurement results corresponding to the event-triggered report configuration in *LTM-CSI-ReportConfig* in the RRC spec.

Regarding the format of the MAC CE, we would like to ask the following question:

* What should be the maximum number of beam-level measurement results that can be included in the MAC CE?

# 2 Actions

**To RAN1**

**ACTION:** RAN2 respectfully asks RAN1 to provide answer to the above question.

# 3 Dates of next TSG RAN WG2 meetings

RAN2#129bis 2025-04-07 – 2025-04-11 Wuhan, China

RAN2#130 2025-05-19 – 2025-05-23 Malta