**3GPP TSG-RAN WG2 Meeting #129bis R2-250xxxx**

**Wuhan, China, 17th – 21st April 2025**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | **38.331** | **CR** | **DraftCR** | **rev** | **-** | **Current version:** | **18.4.0** |  |
|  |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Running RRC CR for LP-WUS  |
|  |  |
| ***Source to WG:*** | vivo (Rapporteur) |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | NR\_LPWUS-Core |  | ***Date:*** | 2025-04-07 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-19 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | To capture the agreements for LP-WUS into RRC specification.This is a draft of the running RRC CR for LP-WUS. To be updated based on the progress in RAN1, RAN2, RAN3, RAN4. |
|  |  |
| ***Summary of change:*** | Introduction of LP-WUS.This CR captures the RRC aspects of LP-WUS and it is based on RAN2 and RAN1 agreements made so far, which could be found in Annex at the end of this document. |
|  |  |
| ***Consequences if not approved:*** | LP-WUS is not supported in RRC specification TS 38.331. |
|  |  |
| ***Clauses affected:*** | TBD |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **X** |  |  Other core specifications  | TS/TR 38.321 CR TBDTS/TR 38.306 CR TBDTS/TR 38.304 CR TBDTS/TR 38.300 CR TBDTS/TR 37.340 CR TBD |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR should be lifted to the latest version of the specification. |
|  |  |
| ***This CR's revision history:*** | This is the initial version of running CR for 38.331 for LP-WUS. |

Start of change

# 3 Definitions, symbols and abbreviations

## 3.1 Definitions

For the purposes of the present document, the terms and definitions given in TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in TR 21.905 [1].

**2Rx XR UE:** Two antenna port XR UE as specified in TS 38.101-1 [15].

**A2X communication:** A communication to support A2X services leveraging PC5 reference points, as defined in TS 23.256 [76]. A2X services are realized by various types of A2X applications, e.g., BRID or DAA.

**Additional sidelink RLC bearer:** If the sidelink PDCP entity is associated with two sidelink RLC entities, the additional sidelink RLC bearer is the RLC bearer configured by *sl-RLC-BearerToAddModListSizeExt* in *sl-ConfigDedicatedNR*, or *sl-RLC-BearerConfigListSizeExt* in *SIB12* or in *SidelinkPreconfigNR*.

**Aerial UE:** UE performingAerial UE communication, as defined in TS 38.300 [2], clause 16.18 and TS 23.256 [76].

**AM MRB:** An MRB associated with at least an AM RLC bearer for PTP transmission.

**BH RLC channel:** An RLC channel between two nodes, which is used to transport backhaul packets.

**Broadcast MRB:** A radio bearer configured for MBS broadcast delivery.

**CEIL:** Mathematical function used to 'round up' i.e. to the nearest integer having a higher or equal value.

**DAPS bearer:** a bearer whose radio protocols are located in both the source gNB and the target gNB during DAPS handover to use both source gNB and target gNB resources.

**Data Burst:** A set of multiple PDUs generated and sent by the application in a short period of time, as defined in TS 23.501 [32].

**Dedicated signalling:** Signalling sent on DCCH logical channel between the network and a single UE.

**Dormant BWP:** The dormant BWP is one of downlink BWPs configured by the network via dedicated RRC signalling. In the dormant BWP, the UE stops monitoring PDCCH on/for the SCell, but continues performing CSI measurements, Automatic Gain Control (AGC) and beam management, if configured. For each serving cell other than the SpCell or PUCCH SCell, the network may configure one BWP as a dormant BWP.

**Earth-fixed cell:** An NTN cell fixed with respect to a certain geographic area on Earth. It can be provisioned by beam(s) continuously covering the same geographical area (e.g., the case of GSO satellites).

**Earth-moving cell:** An NTN cell moving on the ground. It can be provisioned by beam(s) whose coverage area slides over the Earth's surface (e.g., the case of NGSO satellites generating fixed or non-steerable beams).

**eRedCap UE:** A UE with enhanced reduced capabilities as specified in clause 4.2.22.1 in TS 38.306 [26].

**Field:** The individual contents of an information element are referred to as fields.

**FLOOR:** Mathematical function used to 'round down' i.e. to the nearest integer having a lower or equal value.

**Frequency Selection Area ID:** An identity used for broadcast MBS session to guide the frequency selection of the UE as defined in TS 23.247 [67].

**Global cell identity:** An identity to uniquely identifying an NR cell. It is consisted of *cellIdentity* and *plmn-Identity* of the first *PLMN-Identity* in *plmn-IdentityList* in SIB1.

**Information element:** A structural element containing single or multiple fields is referred as information element.

**Candidate configuration:** A configuration part of an *RRCReconfiguration* message associated with a candidate cell, e.g., for LTM or subsequent CPAC. A candidate configuration can be a complete candidate configuration or a delta configuration relatively to a reference configuration.

**Reference configuration:** A configuration provided by the network to the UE that is common, within the same cell group, to a group of configured non-complete candidate configurations.

**MBS Radio Bearer:** A radio bearer that is configured for MBS delivery.

**Mobile IAB-MT**: mobile IAB-node function that terminates the Uu interface to the parent node using the procedures and behaviours specified for UEs unless stated otherwise. The mobile IAB-MT uses the same procedures and behaviours specified for the IAB-MT, unless explicitly stated otherwise.

**Mobile IAB-node**: RAN node that supports NR access links to UEs and an NR backhaul link to a parent node, and that can conduct physical mobility across the RAN area. The mobile IAB-node function used in 38-series of 3GPP Specifications corresponds to the MBSR function defined in TS 23.501 [32]. The mobile IAB-node uses the same procedures and behaviours specified for the IAB-node, unless explicitly stated otherwise.

**Multicast/Broadcast Service:** A point-to-multipoint service as defined in TS 23.247 [67].

**Multicast MRB:** A radio bearer configured for MBS multicast delivery.

**MUSIM gap:** Period that the UE may use to perform MUSIM operations.

**Multi-path:** Mode of operation of a UE in RRC\_CONNECTED configured with one direct path on which the UE connects to gNB using NR Uu, and one indirect path on which the UE connects to the same gNB via another UE using PC5 unicast link or Non-3GPP Connection.

**MP remote UE:** A UE configured with Multi-path. When the connectivity of indirect path is PC5 unicast link, the MP remote UE is acting as a L2 U2N Remote UE. When the connectivity of indirect path is Non-3GPP Connection, the MP remote UE is acting as a N3C remote UE.

**MP relay UE:** A UE that provides connectivity of indirect path to a MP remote UE. When the connectivity is PC5 unicast link, the MP relay UE is acting as a L2 U2N Relay UE. When the connectivity is Non-3GPP Connection, the MP relay UE is acting as a N3C relay UE.

**NCSG:** Network controlled small gap as defined in TS 38.133 [14].

**NPN-only Cell**: A cell that is only available for normal service for NPNs' subscriber. An NPN-capable UE determines that a cell is NPN-only Cell by detecting that the *cellReservedForOtherUse* IE is set to true while the *npn-IdentityInfoList* IE is present in *CellAccessRelatedInfo*.

**N3C indirect path:** In Multi-path, the indirect path using Non-3GPP Connection between remote UE and relay UE.

**NR sidelink communication**: AS functionality enabling at least V2X Communication as defined in TS 23.287 [55] and/or A2X Communication as defined in TS 23.256 [76] and/or ProSe Communication (including ProSe UE-to-Network Relay, non-Relay communication, and ProSe UE-to-UE Relay Communication including UE-to-UE Relay communication with integrated discovery) as defined in TS 23.304 [65] between two or more nearby UEs, using NR technology but not traversing any network node.

**NR sidelink discovery**: AS functionality enabling ProSe non-Relay Discovery, ProSe UE-to-Network Relay discovery and ProSe UE-to-UE Relay discovery for Proximity based Services as defined in TS 23.304 [65] between two or more nearby UEs, using NR technology but not traversing any network node.

**NR sidelink positioning:** AS functionality which determines geographical or relative location and possibly velocity of a target UE or ranging via PC5 interface using SL-PRS transmission and reception as defined in TS 38.305 [73] and TS 38.355 [77].

**PNI-NPN identity:** an identifier of a PNI-NPN comprising of a PLMN ID and a CAG-ID combination.

**Primary Cell**: The MCG cell, operating on the primary frequency, in which the UE either performs the initial connection establishment procedure or initiates the connection re-establishment procedure.

**PC5 Relay RLC channel**: An RLC channel between L2 U2N Remote UE and L2 U2N Relay UE, or between L2 U2U Remote UE and L2 U2U Relay UE, which is used to transport packets over PC5 for L2 UE-to-Network relay or L2 UE-to-UE relay.

**PDU Set**: one or more PDUs carrying the payload of one unit of information generated at the application level (e.g. frame(s) or video slice(s) for XR Services), as defined in TS 23.501 [32].

**Primary SCG Cell**: For dual connectivity operation, the SCG cell in which the UE performs random access when performing the Reconfiguration with Sync procedure.

**Primary Timing Advance Group**: Timing Advance Group containing the SpCell.

**PUCCH SCell:** An SCell configured with PUCCH by *PUCCH-Config*.

**PUSCH-Less SCell:** An SCell configured without PUSCH.

**Quasi-Earth-fixed cell**: An NTN cell fixed with respect to a certain geographic area on Earth during a certain time duration. It can be provisioned by beam(s) covering one geographic area for a limited period and a different geographic area during another period (e.g., the case of NGSO satellites generating steerable beams).

**RedCap UE:** A UE with reduced capabilities as specified in clause 4.2.21.1 in TS 38.306 [26].

**RLC bearer configuration:** The lower layer part of the radio bearer configuration comprising the RLC and logical channel configurations.

**Secondary Cell**: For a UE configured with CA, a cell providing additional radio resources on top of Special Cell.

**Secondary Cell Group**: For a UE configured with dual connectivity, the subset of serving cells comprising of the PSCell and zero or more secondary cells.

**Serving Cell**: For a UE in RRC\_CONNECTED not configured with CA/DC there is only one serving cell comprising of the primary cell. For a UE in RRC\_CONNECTED configured with CA/ DC the term 'serving cells' is used to denote the set of cells comprising of the Special Cell(s) and all secondary cells.

**Small Data Transmission**: A procedure used for transmission of data and/or signalling over allowed radio bearers in RRC\_INACTIVE state (i.e. without the UE transitioning to RRC\_CONNECTED state). The SDT procedure is considered to be ongoing once the conditions for initating SDT as specified in clause 5.3.13.1b are fulfilled until the SDT procedure is completed either successfully or unsuccessfully as specified in clause 18.0 in TS 38.300 [2].

**SNPN identity:** an identifier of an SNPN comprising of a PLMN ID and an NID combination.

**SL indirect path:** In Multi-path, the indirect path using PC5 unicast link between remote UE and relay UE.

**Special Cell:** For Dual Connectivity operation the term Special Cell refers to the PCell of the MCG or the PSCell of the SCG, otherwise the term Special Cell refers to the PCell.

**Split DRB:** In MR-DC, a DRB that supports transmission via MCG and SCG, as well as duplication of PDCP PDUs as defined in TS 37.340 [41]; or in MP, a DRB that supports transmission via direct path and indirect path, as well as duplication of PDCP PDUs.

**Split SRB**: In MR-DC, an SRB that supports transmission via MCG and SCG as well as duplication of RRC PDUs as defined in TS 37.340 [41]; or in MP, a SRB that supports transmission via direct path and indirect path, as well as duplication of PDCP PDUs.

**SSB Frequency**: Frequency referring to the position of resource element RE=#0 (subcarrier #0) of resource block RB#10 of the SS block.

**U2N Relay UE**: A UE that provides functionality to support connectivity to the network for U2N Remote UE(s).

**U2N Remote UE**: A UE that communicates with the network via a U2N Relay UE.

**U2U Relay UE:** A UE that provides functionality to support connectivity between two U2U Remote UEs.

**U2U Remote UE:** A UE that communicates with other UEs via a U2U Relay UE.

**Uu Relay RLC channel**: An RLC channel between L2 U2N Relay UE and gNB, which is used to transport packets over Uu for L2 UE-to-Network relay or for indirect path in case of MP**.**

**UE Inactive AS Context**: UE Inactive AS Context is stored when the connection is suspended and restored when the connection is resumed. It includes information as defined in clause 5.3.8.3.

**V2X sidelink communication**: AS functionality enabling V2X Communication as defined in TS 23.285 [56], between nearby UEs, using E-UTRA technology but not traversing any network node.

## 3.2 Abbreviations

For the purposes of the present document, the abbreviations given in TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in TR 21.905 [1].

5GC 5G Core Network

A2X Aircraft-to-Everything

ACK Acknowledgement

AM Acknowledged Mode

ARQ Automatic Repeat Request

AS Access Stratum

ASN.1 Abstract Syntax Notation One

ATG Air to Ground

BAP Backhaul Adaptation Protocol

BCD Binary Coded Decimal

BFD Beam Failure Detection

BH Backhaul

BLER Block Error Rate

BRID Broadcast Remote Identification

BSR Buffer Status Report

BWP Bandwidth Part

CA Carrier Aggregation

CAG Closed Access Group

CAG-ID Closed Access Group Identifier

CAPC Channel Access Priority Class

CBR Channel Busy Ratio

CCCH Common Control Channel

CFR Common Frequency Resources

CG Cell Group

CHO Conditional Handover

CLI Cross Link Interference

CMAS Commercial Mobile Alert Service

CP Control Plane

CPA Conditional PSCell Addition

CPAC Conditional PSCell Addition or Change

CPC Conditional PSCell Change

C-RNTI Cell RNTI

CSI Channel State Information

DAA Detect And Avoid

DAPS Dual Active Protocol Stack

DC Dual Connectivity

DCCH Dedicated Control Channel

DCI Downlink Control Information

DCP DCI with CRC scrambled by PS-RNTI

DFN Direct Frame Number

DL Downlink

DL-PRS Downlink Positioning Reference Signal

DL-SCH Downlink Shared Channel

DM-RS Demodulation Reference Signal

DRB (user) Data Radio Bearer

DRX Discontinuous Reception

DSR Delay Status Report

DTCH Dedicated Traffic Channel

DTX Discontinuous Transmission

ECEF Earth-Centered, Earth-Fixed

ECI Earth-Centered Inertial

EN-DC E-UTRA NR Dual Connectivity with E-UTRA connected to EPC

EPC Evolved Packet Core

EPS Evolved Packet System

ETWS Earthquake and Tsunami Warning System

E-UTRA Evolved Universal Terrestrial Radio Access

E-UTRA/5GC E-UTRA connected to 5GC

E-UTRA/EPC E-UTRA connected to EPC

E-UTRAN Evolved Universal Terrestrial Radio Access Network

FDD Frequency Division Duplex

FFS For Further Study

G-CS-RNTI Group Configured Scheduling RNTI

GERAN GSM/EDGE Radio Access Network

GIN Group ID for Network selection

GNSS Global Navigation Satellite System

G-RNTI Group RNTI

GSM Global System for Mobile Communications

GSO Geosynchronous Orbit

HARQ Hybrid Automatic Repeat Request

HRNN Human Readable Network Name

HSDN High Speed Dedicated Network

H-SFN Hyper SFN

HST High Speed Train

IAB Integrated Access and Backhaul

IAB-DU IAB-node DU

IAB-MT IAB Mobile Termination

IDC In-Device Coexistence

IE Information element

IMSI International Mobile Subscriber Identity

kB Kilobyte (1000 bytes)

L1 Layer 1

L2 Layer 2

L3 Layer 3

LBT Listen Before Talk

LEO Low Earth Orbit

LP-WUR Low Power Wake-up Radio

LP-WUS Low Power Wake-up Signaling

LP-SS Low Power Synchronization Signaling

Editor’s NOTE: The terminology for LP-WUS/LP-SS will be further updated to align with other specifications (e.g. 38.306/38.211/38.213/214).

LTM L1/L2 Triggered Mobility

MAC Medium Access Control

MBS Multicast/Broadcast Service

MBS FSAI MBS Frequency Selection Area Identity

MCCH MBS Control Channel

MCG Master Cell Group

MDT Minimization of Drive Tests

MIB Master Information Block

MO-SDT Mobile Originated SDT

MPE Maximum Permissible Exposure

MP Multi-path

MRB MBS Radio Bearer

MR-DC Multi-Radio Dual Connectivity

MTCH MBS Traffic Channel

MT-SDT Mobile Terminated SDT

MTSI Multimedia Telephony Service for IMS

MUSIM Multi-Universal Subscriber Identity Module

N3C Non-3GPP Connection

N/A Not Applicable

NCR Network-Controlled Repeater

NCR-Fwd NCR Forwarding

NCR-MT NCR Mobile Termination

NE-DC NR E-UTRA Dual Connectivity

NES Network Energy Savings

(NG)EN-DC E-UTRA NR Dual Connectivity (covering E-UTRA connected to EPC or 5GC)

NGEN-DC E-UTRA NR Dual Connectivity with E-UTRA connected to 5GC

NID Network Identifier

NPN Non-Public Network

NR-DC NR-NR Dual Connectivity

NR/5GC NR connected to 5GC

NSAG Network Slice AS Group

NTN Non-Terrestrial Network

PCell Primary Cell

PDCP Packet Data Convergence Protocol

PDU Protocol Data Unit

PEI Paging Early Indication

PEI-O Paging Early Indication-Occasion

PLMN Public Land Mobile Network

PNI-NPN Public Network Integrated Non-Public Network

posSIB Positioning SIB

PPW PRS Processing Window

PRS Positioning Reference Signal

PSCell Primary SCG Cell

PSI PDU Set Importance

PTM Point to Multipoint

PTP Point to Point

PWS Public Warning System

QoE Quality of Experience

QoS Quality of Service

RAN Radio Access Network

RAT Radio Access Technology

RLC Radio Link Control

RLM Radio Link Monitoring

RMTC RSSI Measurement Timing Configuration

RNA RAN-based Notification Area

RNTI Radio Network Temporary Identifier

ROHC Robust Header Compression

RPLMN Registered Public Land Mobile Network

RRC Radio Resource Control

RS Reference Signal

SBAS Satellite Based Augmentation System

SCell Secondary Cell

SCG Secondary Cell Group

SCS Subcarrier Spacing

SD-RSRP Sidelink Discovery RSRP

SDT Small Data Transmission

SFN Single Frequency Network

SFN System Frame Number

SFTD SFN and Frame Timing Difference

SI System Information

SIB System Information Block

SL Sidelink

SL-PRS Sidelink Positioning Reference Signal

SLSS Sidelink Synchronisation Signal

SNPN Stand-alone Non-Public Network

SpCell Special Cell

SRAP Sidelink Relay Adaptation Protocol

SRB Signalling Radio Bearer

SRS Sounding Reference Signal

SSB Synchronization Signal Block

TAG Timing Advance Group

TDCP Time Domain Channel Property

TDD Time Division Duplex

TEG Timing Error Group

TM Transparent Mode

TMGI Temporary Mobile Group Identity

TN Terrestrial Network

TSS Timing Synchronization Status.

U2N UE-to-Network

U2U UE-to-UE

UDC Uplink Data Compression

UE User Equipment

UL Uplink

UM Unacknowledged Mode

UP User Plane

VR Virtual Reality

VSAT Very Small Aperture Terminal

XR eXtended Reality

In the ASN.1, lower case may be used for some (parts) of the above abbreviations e.g. c-RNTI.

Nex change

### 6.3.1 System information blocks

#### – *SIB2*

*SIB2* contains cell re-selection information common for intra-frequency, inter-frequency and/or inter-RAT cell re-selection (i.e. applicable for more than one type of cell re-selection but not necessarily all) as well as intra-frequency cell re-selection information other than neighbouring cell related.

*SIB2* information element

-- ASN1START

-- TAG-SIB2-START

SIB2 ::= SEQUENCE {

 cellReselectionInfoCommon SEQUENCE {

 nrofSS-BlocksToAverage INTEGER (2..maxNrofSS-BlocksToAverage) OPTIONAL, -- Need S

 absThreshSS-BlocksConsolidation ThresholdNR OPTIONAL, -- Need S

 rangeToBestCell RangeToBestCell OPTIONAL, -- Need R

 q-Hyst ENUMERATED {

 dB0, dB1, dB2, dB3, dB4, dB5, dB6, dB8, dB10,

 dB12, dB14, dB16, dB18, dB20, dB22, dB24},

 speedStateReselectionPars SEQUENCE {

 mobilityStateParameters MobilityStateParameters,

 q-HystSF SEQUENCE {

 sf-Medium ENUMERATED {dB-6, dB-4, dB-2, dB0},

 sf-High ENUMERATED {dB-6, dB-4, dB-2, dB0}

 }

 } OPTIONAL, -- Need R

 ...

 },

 cellReselectionServingFreqInfo SEQUENCE {

 s-NonIntraSearchP ReselectionThreshold OPTIONAL, -- Need S

 s-NonIntraSearchQ ReselectionThresholdQ OPTIONAL, -- Need S

 threshServingLowP ReselectionThreshold,

 threshServingLowQ ReselectionThresholdQ OPTIONAL, -- Need R

 cellReselectionPriority CellReselectionPriority,

 cellReselectionSubPriority CellReselectionSubPriority OPTIONAL, -- Need R

 ...

 },

 intraFreqCellReselectionInfo SEQUENCE {

 q-RxLevMin Q-RxLevMin,

 q-RxLevMinSUL Q-RxLevMin OPTIONAL, -- Need R

 q-QualMin Q-QualMin OPTIONAL, -- Need S

 s-IntraSearchP ReselectionThreshold,

 s-IntraSearchQ ReselectionThresholdQ OPTIONAL, -- Need S

 t-ReselectionNR T-Reselection,

 frequencyBandList MultiFrequencyBandListNR-SIB OPTIONAL, -- Need S

 frequencyBandListSUL MultiFrequencyBandListNR-SIB OPTIONAL, -- Need R

 p-Max P-Max OPTIONAL, -- Need S

 smtc SSB-MTC OPTIONAL, -- Need S

 ss-RSSI-Measurement SS-RSSI-Measurement OPTIONAL, -- Need R

 ssb-ToMeasure SSB-ToMeasure OPTIONAL, -- Need S

 deriveSSB-IndexFromCell BOOLEAN,

 ...,

 [[

 t-ReselectionNR-SF SpeedStateScaleFactors OPTIONAL -- Need R

 ]],

 [[

 smtc2-LP-r16 SSB-MTC2-LP-r16 OPTIONAL, -- Need R

 ssb-PositionQCL-Common-r16 SSB-PositionQCL-Relation-r16 OPTIONAL -- Cond SharedSpectrum

 ]],

 [[

 ssb-PositionQCL-Common-r17 SSB-PositionQCL-Relation-r17 OPTIONAL -- Cond SharedSpectrum2

 ]],

 [[

 smtc4list-r17 SSB-MTC4List-r17 OPTIONAL -- Need R

 ]],

 [[

 frequencyBandList-v1760 MultiFrequencyBandListNR-SIB-v1760 OPTIONAL, -- Need R

 frequencyBandListSUL-v1760 MultiFrequencyBandListNR-SIB-v1760 OPTIONAL -- Need R

 ]],

 [[

 frequencyBandListAerial-r18 MultiFrequencyBandListNR-Aerial-SIB-r18 OPTIONAL -- Need S

 ]]

 },

 ...,

 [[

 relaxedMeasurement-r16 SEQUENCE {

 lowMobilityEvaluation-r16 SEQUENCE {

 s-SearchDeltaP-r16 ENUMERATED {

 dB3, dB6, dB9, dB12, dB15,

 spare3, spare2, spare1},

 t-SearchDeltaP-r16 ENUMERATED {

 s5, s10, s20, s30, s60, s120, s180,

 s240, s300, spare7, spare6, spare5,

 spare4, spare3, spare2, spare1}

 } OPTIONAL, -- Need R

 cellEdgeEvaluation-r16 SEQUENCE {

 s-SearchThresholdP-r16 ReselectionThreshold,

 s-SearchThresholdQ-r16 ReselectionThresholdQ OPTIONAL -- Need R

 } OPTIONAL, -- Need R

 combineRelaxedMeasCondition-r16 ENUMERATED {true} OPTIONAL, -- Need R

 highPriorityMeasRelax-r16 ENUMERATED {true} OPTIONAL -- Need R

 } OPTIONAL -- Need R

 ]],

 [[

 cellEquivalentSize-r17 INTEGER(2..16) OPTIONAL, -- Cond HSDN

 relaxedMeasurement-r17 SEQUENCE {

 stationaryMobilityEvaluation-r17 SEQUENCE {

 s-SearchDeltaP-Stationary-r17 ENUMERATED {dB2, dB3, dB6, dB9, dB12, dB15, spare2, spare1},

 t-SearchDeltaP-Stationary-r17 ENUMERATED {s5, s10, s20, s30, s60, s120, s180, s240, s300, spare7, spare6, spare5,

 spare4, spare3, spare2, spare1}

 },

 cellEdgeEvaluationWhileStationary-r17 SEQUENCE {

 s-SearchThresholdP2-r17 ReselectionThreshold,

 s-SearchThresholdQ2-r17 ReselectionThresholdQ OPTIONAL -- Need R

 } OPTIONAL, -- Need R

 combineRelaxedMeasCondition2-r17 ENUMERATED {true} OPTIONAL -- Need R

 } OPTIONAL -- Need R

 ]],

 relaxedMeasurementForSevingCell-r19 SEQUENCE {

 cellEdgeEvaluationOnMR-r19 SEQUENCE {

 s-SearchThresholdP3-r19 ReselectionThreshold,

 s-SearchThresholdQ3-r19 ReselectionThresholdQ OPTIONAL -- Need R

 }

 cellEdgeEvaluationOnLROnLPSS-r19 SEQUENCE {

 s-SearchThresholdPLP-r19 TBD,

 s-SearchThresholdQLP-r19 TBD OPTIONAL -- Need R

 } OPTIONAL, -- Need R

 FFS cellEdgeEvaluationOnLROnSSB-r19 SEQUENCE {

 s-SearchThresholdPx-r19 TBD,

 s-SearchThresholdQx-r19 TBD OPTIONAL -- Need R

 } OPTIONAL -- Need R

 } OPTIONAL, -- Need R

 relaxedMeasurementForNeighboringCell-r19 SEQUENCE {

 cellEdgeEvaluationOnMR-r19 SEQUENCE {

 s-SearchThresholdP4-r19 ReselectionThreshold,

 s-SearchThresholdQ4-r19 ReselectionThresholdQ OPTIONAL -- Need R

 }

 cellEdgeEvaluationOnLROnLPSS-r19 SEQUENCE {

 s-SearchThresholdPLP2-r19 TBD,

 s-SearchThresholdQLP2-r19 TBD OPTIONAL -- Need R

 } OPTIONAL, -- Need R

 FFS cellEdgeEvaluationOnLROnSSB-r19 SEQUENCE {

 s-SearchThresholdPx-r19 TBD,

 s-SearchThresholdQx-r19 TBD OPTIONAL -- Need R

 } OPTIONAL -- Need R

 } OPTIONAL, -- Need R

 offloadMeasurementForServingCell-r19 SEQUENCE {

 cellEdgeEvaluationOnMR-r19 SEQUENCE {

 s-SearchThresholdP5-r19 ReselectionThreshold,

 s-SearchThresholdQ5-r19 ReselectionThresholdQ OPTIONAL -- Need R

 }

 cellEdgeEvaluationOnLROnLPSS-r19 SEQUENCE {

 s-SearchThresholdPLP3-r19 TBD,

 s-SearchThresholdQLP3-r19 TBD OPTIONAL -- Need R

 } OPTIONAL, -- Need R

 FFS cellEdgeEvaluationOnLROnSSB-r19 SEQUENCE {

 s-SearchThresholdPx-r19 TBD,

 s-SearchThresholdQx-r19 TBD OPTIONAL -- Need R

 } OPTIONAL, -- Need R

 cellEdgeEvaluationOnLROnLPSS-Exit-r19 SEQUENCE {

 s-SearchThresholdPLP4-r19 TBD,

 s-SearchThresholdQLP4-r19 TBD OPTIONAL -- Need R

 }

 FFS cellEdgeEvaluationOnLROnSSB-Exit-r19 SEQUENCE {

 s-SearchThresholdPx-r19 TBD,

 s-SearchThresholdQx-r19 TBD OPTIONAL -- Need R

 } OPTIONAL -- Need R

 } OPTIONAL -- Need R

 ]]

}

RangeToBestCell ::= Q-OffsetRange

-- TAG-SIB2-STOP

-- ASN1STOP

Editor’s NOTE: FFS on the value range for LR measurement based threshold for serving cell relaxation/offloading and neighboring cell relaxation.

Editor’s NOTE: FFS on exit condition for serving cell RRM relaxation, e.g., whether a separate exit condition other than ‘not fulfilling the entry condition’ is needed, or whether exit condition include MR and/or LR-based measurements.

Editor’s NOTE: FFS if the entry condition for serving cell RRM measurement relaxation is the same as neighbour cell RRM measurement relaxation.

Editor’s NOTE: FFS (if needed) on enhancements based on R16 criteria (e.g., based on the LR measurements) for neighboring cell measurement relaxation for the case when MR serving cell measurement results are not available.

Editor’s NOTE: FFS on whether separate thresholds of RRM relaxation/offloading can be configured for OFDM-based and OOK-based WUR if a cell supports both types of LRs.

Editor’s NOTE: FFS on the relationship between the thresholds for serving cell relaxation and offloading. FFS on the relationship between the thresholds for serving cell relaxation/offloading and neighboring cell relaxation. FFS on the relationship between the thresholds for serving cell relaxation/offloading, neighboring cell relaxation and *s-IntraSearchP/s-NonIntraSearchP*.

Editor’s NOTE: FFS on the relationship between the thresholds for serving cell relaxation/offloading, neighboring cell relaxation and entry/exit condition of using LP-WUS, [and potential pre-condition between RRM relaxation/offloading criteria and entry/exit condition of using LP-WUS].

Editor’s NOTE: FFS on “low mobility” criteria.

Editor’s NOTE: FFS on whether RRM relaxation is applicable for high priority frequency.

| *SIB2* field descriptions |
| --- |
| ***absThreshSS-BlocksConsolidation***Threshold for consolidation of L1 measurements per RS index. If the field is absent, the UE uses the measurement quantity as specified in TS 38.304 [20]. |
| ***cellEdgeEvaluation***Indicates the criteria for a UE to detect that it is not at cell edge, in order to relax measurement requirements for cell reselection (see TS 38.304 [20], clause 5.2.4.9.2). |
| ***cellEdgeEvaluationOnLROnLPSS***Indicates the criteria for a UE to detect that it is not at cell edge based on the serving cell measurement on OOK based LP-WUR or OFDM based LP-WUS measure on LP-SS, in order to relax serving cell measurement requirements for cell reselection (see TS 38.304 [20], clause xxxx), or to relax neighboring cell measurement requirements for cell reselection (see TS 38.304 [20], clause xxxx), or to offload serving cell measurement to low power receiver. |
| ***FFS cellEdgeEvaluationOnLROnSSB***FFS Indicates the criteria for a UE to detect that it is not at cell edge based on the serving cell measurement on OFDM based LP-WUR measure on SSB, in order to relax serving cell measurement requirements for cell reselection (see TS 38.304 [20], clause xxxx), or to relax neighboring cell measurement requirements for cell reselection (see TS 38.304 [20], clause xxxx), or to offload serving cell measurement to low power receiver. |
| ***cellEdgeEvaluationOnMR***Indicates the criteria for a UE to detect that it is not at cell edge based on the serving cell measurement on main radio, in order to relax serving cell measurement requirements for cell reselection (see TS 38.304 [20], clause xxxx), or to relax neighboring cell measurement requirements for cell reselection (see TS 38.304 [20], clause xxxx), or to offload serving cell measurement to low power receiver. |
| ***cellEdgeEvaluationWhileStationary***Indicates the criteria for a UE to detect that it is not at cell edge while stationary, in order to relax measurement requirements for cell reselection (see TS 38.304 [20], clause 5.2.4.9.4). |
| ***cellEquivalentSize***The number of cell count used for mobility state estimation for this cell as specified in TS 38.304 [20]. |
| ***cellReselectionInfoCommon***Cell re-selection information common for intra-frequency, inter-frequency and/ or inter-RAT cell re-selection. |
| ***cellReselectionServingFreqInfo***Information common for non-intra-frequency cell re-selection i.e. cell re-selection to inter-frequency and inter-RAT cells. |
| ***combineRelaxedMeasCondition***When both *lowMobilityEvaluation* and *cellEdgeEvaluation* criteria are present in SIB2, this parameter configures the UE to fulfil both criteria in order to relax measurement requirements for cell reselection. If the field is absent, the UE is allowed to relax measurement requirements for cell reselection when either or both of the criteria are met. (See TS 38.304 [20], clause 5.2.4.9.0) |
| ***combineRelaxedMeasCondition2***When both *stationaryMobilityEvaluation* and *cellEdgeEvaluationWhileStationary* criteria are present in SIB2, this parameter configures the UE to fulfil both criteria in order to relax measurement requirements for cell reselection. If the field is absent, the UE is allowed to relax measurement requirements for cell reselection when only the stationary criteria is met. (See TS 38.304 [20], clause 5.2.4.9.0) |
| ***deriveSSB-IndexFromCell***This field indicates whether the UE can utilize serving cell timing to derive the index of SS block transmitted by neighbour cell. If this field is set to *true*, the UE assumes SFN and frame boundary alignment across cells on the serving frequency as specified in TS 38.133 [14]. |
| ***frequencyBandList***Indicates the list of frequency bands for which the NR cell reselection parameters apply. The UE behaviour in case the field is absent is described in clause 5.2.2.4.3. |
| ***frequencyBandListAerial***Indicates the list of frequency bands for aerial operation for which the NR cell reselection parameters apply. The UE behaviour in case the field is absent is described in clause 5.2.2.4.3. |
| ***highPriorityMeasRelax***Indicates whether measurements can be relaxed on high priority frequencies. If the field is absent, the UE shall not relax measurements on high priority frequencies beyond "Thigher\_priority\_search" unless both low mobility and not at cell edge criteria are fulfilled (see TS 38.133 [14], clauses 4.2.2.7, 4.2.2.10 and 4.2.2.11). |
| ***intraFreqCellReselectionInfo***Cell re-selection information common for intra-frequency cells. |
| ***lowMobilityEvaluation***Indicates the criteria for a UE to detect low mobility, in order to relax measurement requirements for cell reselection (see TS 38.304 [20], clause 5.2.4.9.1). |
| ***nrofSS-BlocksToAverage***Number of SS blocks to average for cell measurement derivation. If the field is absent the UE uses the measurement quantity as specified in TS 38.304 [20]. |
| ***offloadMeasurementForServingCell***Configuration to allow offloading of serving cell RRM measurement (see TS 38.304 [20], clause xxxx). |
| ***p-Max***Value in dBm applicable for the intra-frequency neighbouring NR cells. If absent the UE applies the maximum power according to TS 38.101-1 [15] in case of an FR1 cell, TS 38.101-2 [39] in case of an FR2 cell or TS 38.101-5 [75] in case of an NTN cell. In this release of the specification, if *p-Max* is present on a carrier frequency in FR2, the UE shall ignore the field and applies the maximum power according to TS 38.101-2 [39] for FR2-1/2 or according to TS 38.101-5 [75] for FR2-NTN. This field is ignored by IAB-MT and NCR-MT. The IAB-MT applies output power and emissions requirements, as specified in TS 38.174 [63]. The NCR-MT applies output power and emissions requirements as specified in TS 38.106 [79]. |
| ***q-Hyst***Parameter "*Qhyst*" in TS 38.304 [20], Value in dB. Value *dB1* corresponds to 1 dB, *dB2* corresponds to 2 dB and so on. |
| ***q-HystSF***Parameter "Speed dependent ScalingFactor for Qhyst" in TS 38.304 [20]. The *sf-Medium* and *sf-High* concern the additional hysteresis to be applied, in Medium and High Mobility state respectively, to Qhyst as defined in TS 38.304 [20]. In dB. Value *dB-6* corresponds to -6dB, *dB-4* corresponds to -4dB and so on. |
| ***q-QualMin***Parameter "Qqualmin" in TS 38.304 [20], applicable for intra-frequency neighbour cells. If the field is absent, the UE applies the (default) value of negative infinity for Qqualmin.  |
| ***q-RxLevMin***Parameter "Qrxlevmin" in TS 38.304 [20], applicable for intra-frequency neighbour cells. |
| ***q-RxLevMinSUL***Parameter "Qrxlevmin" in TS 38.304 [20], applicable for intra-frequency neighbour cells. |
| ***rangeToBestCell***Parameter "rangeToBestCell" in TS 38.304 [20]. The network configures only non-negative (in dB) values. |
| ***relaxedMeasurement***Configuration to allow relaxation of RRM measurement requirements for cell reselection (see TS 38.304 [20], clause 5.2.4.9). In NTN, this field is only applicable for GSO neighbour cells. |
| ***relaxedMeasurementForSevingCell***Configuration to allow relaxation of serving cell RRM measurement requirements for cell reselection (see TS 38.304 [20], clause xxxx). |
| ***relaxedMeasurementForNeighboringCell***Configuration to allow relaxation of neighboring cell RRM measurement requirements for cell reselection (see TS 38.304 [20], clause xxxx). |
| ***s-IntraSearchP***Parameter "SIntraSearchP" in TS 38.304 [20]. |
| ***s-IntraSearchQ***Parameter "SIntraSearchQ" in TS 38.304 [20]. If the field is absent, the UE applies the (default) value of 0 dB for SIntraSearchQ. |
| ***s-NonIntraSearchP***Parameter "SnonIntraSearchP" in TS 38.304 [20]. If this field is absent, the UE applies the (default) value of infinity for SnonIntraSearchP. |
| ***s-NonIntraSearchQ***Parameter "SnonIntraSearchQ" in TS 38.304 [20]. If the field is absent, the UE applies the (default) value of 0 dB for SnonIntraSearchQ. |
| ***s-SearchDeltaP***Parameter "SSearchDeltaP" in TS 38.304 [20]. Value dB3 corresponds to 3 dB, dB6 corresponds to 6 dB and so on. |
| ***s-SearchDeltaP-Stationary***Parameter "SSearchDeltaP-Stationary" in TS 38.304 [20]. Value *dB2* corresponds to 2 dB, *dB3* corresponds to 3 dB and so on. |
| ***s-SearchThresholdP, s-SearchThresholdP2, s-SearchThresholdP3, s-SearchThresholdP4, s-SearchThresholdP5, FFS s-SearchThresholdPX***Parameters "SSearchThresholdP", "SSearchThresholdP2", "SSearchThresholdP3", "SSearchThresholdP4", and "SSearchThresholdP5" in TS 38.304 [20]. The network configures *s-SearchThresholdP* and *s-SearchThresholdP2* to be less than or equal to *s-IntraSearchP* and *s-NonIntraSearchP*. [FFS The network configures *s-SearchThresholdP5* to be larger than or equal to *s-IntraSearchP* and *s-NonIntraSearchP*.] [FFS The network configures *s-SearchThresholdP5* to be larger than or equal to *s-IntraSearchP3* and *s-NonIntraSearchP4*.] [FFS The network configures *s-SearchThresholdP3* to be larger than or equal to *s-NonIntraSearchP4*.] |
| ***s-SearchThresholdPLP, s-SearchThresholdPLP2, s-SearchThresholdPLP3, s-SearchThresholdPLP4***Parameters "SSearchThresholdPLP", SSearchThresholdPLP2", SSearchThresholdPLP3", and "SSearchThresholdPLP4" in TS 38.304 [20]. [FFS The network configures *s-SearchThresholdPLP3* to be larger than or equal to *s-IntraSearchPLP1* and *s-NonIntraSearchPLP2*.] [FFS The network configures *s-SearchThresholdPLP1* to be larger than or equal to *s-NonIntraSearchPLP2*.] |
| ***s-SearchThresholdQ, s-SearchThresholdQ2, s-SearchThresholdQ3, s-SearchThresholdQ4, s-SearchThresholdQ5, FFS s-SearchThresholdQX***Parameters "SSearchThresholdQ", "SSearchThresholdQ2", "SSearchThresholdQ3", "SSearchThresholdQ4", and "SSearchThresholdQ5" in TS 38.304 [20]. The network configures *s-SearchThresholdQ* and *s-SearchThresholdQ2* to be less than or equal to *s-IntraSearchQ* and *s-NonIntraSearchQ*. [FFS The network configures *s-SearchThresholdQ5* to be larger than *s-IntraSearchQ* and *s-NonIntraSearchQ*.] [FFS The network configures *s-SearchThresholdQ5* to be larger than or equal to *s-IntraSearchQ3* and *s-NonIntraSearchQ4*.] [FFS The network configures *s-SearchThresholdQ3* to be larger than or equal to *s-NonIntraSearchQ4*.] |
| ***s-SearchThresholdQLP, s-SearchThresholdQLP2, s-SearchThresholdQLP3, s-SearchThresholdQLP4***Parameters "SSearchThresholdQLP", "SSearchThresholdQLP2", "SSearchThresholdQLP3", and "SSearchThresholdQ4" in TS 38.304 [20]. [FFS The network configures *s-SearchThresholdQLP3* to be larger than or equal to *s-IntraSearchQLP1* and *s-NonIntraSearchQLP2*.] [FFS The network configures *s-SearchThresholdQLP1* to be larger than or equal to *s-NonIntraSearchQLP2*.] |
| ***smtc***Measurement timing configuration for intra-frequency measurement. If this field is absent, the UE assumes that SSB periodicity is 5 ms for the intra-frequnecy cells. If the field is broadcast by an NTN cell, the *offset* (derived from parameter *periodicityAndOffset*) is based on the assumption that the gNB-UE propagation delay difference between the serving cell and neighbour cells equals to 0 ms, and UE can adjust the actual *offset* based on the actual propagation delay difference. |
| ***smtc2-LP***Measurement timing configuration for intra-frequency neighbour cells with a Long Periodicity (LP) indicated by periodicity in *smtc2-LP*. The timing offset and duration are equal to the offset and duration indicated in *smtc* in *intraFreqCellReselectionInfo*. The periodicity in *smtc2-LP* can only be set to a value strictly larger than the periodicity in *smtc* in *intraFreqCellReselectionInfo* (e.g. if *smtc* indicates sf20 the Long Periodicity can only be set to sf40, sf80 or sf160, if *smtc* indicates sf160, *smtc2-LP* cannot be configured). The *pci-List*, if present, includes the physical cell identities of the intra-frequency neighbour cells with Long Periodicity. If *smtc2-LP* is absent, the UE assumes that there are no intra-frequency neighbour cells with a Long Periodicity. |
| ***smtc4list***Measurement timing configuration list for NTN deployments, see clause 5.5.2.10. The offset of each SSB-MTC4 in *smtc4list* is based on the assumption that the gNB-UE propagation delay difference between the serving cell and neighbour cells equals to 0 ms, and UE can adjust the actual *offset* based on the actual propagation delay difference. For a UE that supports less SMTCs than what is included in this list, it is up to the UE to select which SMTCs to consider. |
| ***ssb-PositionQCL-Common***Indicates the QCL relation between SS/PBCH blocks for intra-frequency neighbor cells as specified in TS 38.213 [13], clause 4.1. |
| ***ssb-ToMeasure***The set of SS blocks to be measured within the SMTC measurement duration (see TS 38.215 [9]). When the field is absent the UE measures on all SS-blocks. |
| ***stationaryMobilityEvaluation***Indicates the criteria for a UE to detect stationary mobility, in order to relax measurement requirements for cell reselection (see TS 38.304 [20], clause 5.2.4.9.0). |
| ***t-ReselectionNR***Parameter "TreselectionNR" in TS 38.304 [20]. |
| ***t-ReselectionNR-SF***Parameter "Speed dependent ScalingFactor for TreselectionNR" in TS 38.304 [20]. If the field is absent, the UE behaviour is specified in TS 38.304 [20]. |
| ***threshServingLowP***Parameter "ThreshServing, LowP" in TS 38.304 [20]. |
| ***threshServingLowQ***Parameter "ThreshServing, LowQ" in TS 38.304 [20]. |
| ***t-SearchDeltaP***Parameter "TSearchDeltaP" in TS 38.304 [20]. Value in seconds. Value *s5* means 5 seconds, value *s10* means 10 seconds and so on. |
| ***t-SearchDeltaP-Stationary***Parameter "TSearchDeltaP-Stationary" in TS 38.304 [20]. Value in seconds. Value *s5* means 5 seconds, value *s10* means 10 seconds and so on. |

|  |  |
| --- | --- |
| Conditional Presence | Explanation |
| *HSDN* | The field is optionally present, Need R, if *speedStateReselectionPars* is present; otherwise the field is not present. |
| *SharedSpectrum* | This field is mandatory present if this intra-frequency operates with shared spectrum channel access in FR1. Otherwise, it is absent, Need R. |
| *SharedSpectrum2* | This field is optionally present if this intra-frequency operates with shared spectrum channel access in FR2-2, Need R. Otherwise, it is absent, Need R. |

Next change

#### – *DownlinkConfigCommonSIB*

The IE *DownlinkConfigCommonSIB* provides common downlink parameters of a cell.

*DownlinkConfigCommonSIB* information element

-- ASN1START

-- TAG-DOWNLINKCONFIGCOMMONSIB-START

DownlinkConfigCommonSIB ::= SEQUENCE {

 frequencyInfoDL FrequencyInfoDL-SIB,

 initialDownlinkBWP BWP-DownlinkCommon,

 bcch-Config BCCH-Config,

 pcch-Config PCCH-Config,

 ...,

 [[

 pei-Config-r17 PEI-Config-r17 OPTIONAL, -- Need R

 initialDownlinkBWP-RedCap-r17 BWP-DownlinkCommon OPTIONAL -- Need R

 ]],

 [[

 frequencyInfoDL-v1800 FrequencyInfoDL-SIB-v1800 OPTIONAL -- Need R

 ]],

 [[

 lowPower-Config-r19 LowPower-Config-r19 OPTIONAL -- Need R

 ]]

}

DownlinkConfigCommonSIB-v1760 ::= SEQUENCE {

 frequencyInfoDL-v1760 FrequencyInfoDL-SIB-v1760

}

BCCH-Config ::= SEQUENCE {

 modificationPeriodCoeff ENUMERATED {n2, n4, n8, n16},

 ...

}

PCCH-Config ::= SEQUENCE {

 defaultPagingCycle PagingCycle,

 nAndPagingFrameOffset CHOICE {

 oneT NULL,

 halfT INTEGER (0..1),

 quarterT INTEGER (0..3),

 oneEighthT INTEGER (0..7),

 oneSixteenthT INTEGER (0..15)

 },

 ns ENUMERATED {four, two, one},

 firstPDCCH-MonitoringOccasionOfPO CHOICE {

 sCS15KHZoneT SEQUENCE (SIZE (1..maxPO-perPF)) OF INTEGER (0..139),

 sCS30KHZoneT-SCS15KHZhalfT SEQUENCE (SIZE (1..maxPO-perPF)) OF INTEGER (0..279),

 sCS60KHZoneT-SCS30KHZhalfT-SCS15KHZquarterT SEQUENCE (SIZE (1..maxPO-perPF)) OF INTEGER (0..559),

 sCS120KHZoneT-SCS60KHZhalfT-SCS30KHZquarterT-SCS15KHZoneEighthT SEQUENCE (SIZE (1..maxPO-perPF)) OF INTEGER (0..1119),

 sCS120KHZhalfT-SCS60KHZquarterT-SCS30KHZoneEighthT-SCS15KHZoneSixteenthT SEQUENCE (SIZE (1..maxPO-perPF)) OF INTEGER (0..2239),

 sCS480KHZoneT-SCS120KHZquarterT-SCS60KHZoneEighthT-SCS30KHZoneSixteenthT SEQUENCE (SIZE (1..maxPO-perPF)) OF INTEGER (0..4479),

 sCS480KHZhalfT-SCS120KHZoneEighthT-SCS60KHZoneSixteenthT SEQUENCE (SIZE (1..maxPO-perPF)) OF INTEGER (0..8959),

 sCS480KHZquarterT-SCS120KHZoneSixteenthT SEQUENCE (SIZE (1..maxPO-perPF)) OF INTEGER (0..17919)

 } OPTIONAL, -- Need R

 ...,

 [[

 nrofPDCCH-MonitoringOccasionPerSSB-InPO-r16 INTEGER (2..4) OPTIONAL -- Cond SharedSpectrum2

 ]],

 [[

 ranPagingInIdlePO-r17 ENUMERATED {true} OPTIONAL, -- Need R

 firstPDCCH-MonitoringOccasionOfPO-v1710 CHOICE {

 sCS480KHZoneEighthT SEQUENCE (SIZE (1..maxPO-perPF)) OF INTEGER (0..35839),

 sCS480KHZoneSixteenthT SEQUENCE (SIZE (1..maxPO-perPF)) OF INTEGER (0..71679)

} OPTIONAL -- Need R

 ]]

}

PEI-Config-r17 ::= SEQUENCE {

 po-NumPerPEI-r17 ENUMERATED {po1, po2, po4, po8},

 payloadSizeDCI-2-7-r17 INTEGER (1..maxDCI-2-7-Size-r17),

 pei-FrameOffset-r17 INTEGER (0..16),

 subgroupConfig-r17 SubgroupConfig-r17,

 lastUsedCellOnly-r17 ENUMERATED {true} OPTIONAL, -- Need R

 ...

}

SubgroupConfig-r17 ::= SEQUENCE {

 subgroupsNumPerPO-r17 INTEGER (1.. maxNrofPagingSubgroups-r17),

 subgroupsNumForUEID-r17 INTEGER (1.. maxNrofPagingSubgroups-r17) OPTIONAL, -- Need S

 ...

}

LowPower-Config-r19 ::= SEQUENCE {

 lpwus-MvalueFR1-r19 ENUMERATED {1, 2, 4} OPTIONAL, -- Cond FR1-only

 FFS lpwus-MvalueFR2-r19 TBD OPTIONAL, -- Cond FR2-only

 FFS lpss-MvalueFR1-r19 ENUMERATED {1, 2, 4} OPTIONAL, -- Cond FR1-only

 FFS lpss-MvalueFR2-r19 TBD OPTIONAL, -- Cond FR2-only

 FFS lpwus-Lpss-StartRB-r19 INTEGER (0..263) OPTIONAL, -- Need R

 FFS lpss-BinarySeq-r19 INTEGER (1..[4]) OPTIONAL, -- Cond OOK-only

 FFS lpss-PeriodicityAndOffset CHOICE {

 TBD Periodicity1 TBD OFFSET1,

 TBD Periodicity2 TBD OFFSET2,

 TBD Periodicity3 TBD OFFSET3

 } OPTIONAL, -- Cond OOK-only

 TBD additionalSync-r19 TBD OPTIONAL, -- Need R

 FFS lpwus-OverlaidSeq-r19 TBD OPTIONAL, -- Cond OFDM-only

 FFS lpss-OverlaidSeq-r19 TBD OPTIONAL, -- Cond OOK-only FFS OOK-4

 FFS lpwus-MoNumPerLo-r19 TBD,

 FFS lpwus-PoNumPerLo-r19 TBD ENUMERATED {po1, po2, po4, po8} OPTIONAL, -- Need R

 FFS lpwus-LoOffset-r19 TBD,

 epre-Ratio-LPWUS-LPSS-r19 TBD,

 lp-subgroupConfig-r19 LP-SubgroupConfig-r19,

 entryCondition-r19 EntryCondition-r19,

 exitCondition-r19 ExitCondition-r19,

 ...

}

LP-SubgroupConfig-r19 ::= SEQUENCE {

 lpSubgroupsNumPerPO-r19 INTEGER (1.. maxNrofPagingSubgroupsLP-r19),

 lpSubgroupsNumForUEID-r19 INTEGER (1.. maxNrofPagingSubgroupsLP-r19) OPTIONAL -- Need S

 ...

}

EntryCondition-r19 ::= SEQUENCE {

 enryEvaluationOnMRForLROnLPSS-r19 SEQUENCE {

 thresholdP1-r19 ThresholdP,

 thresholdQ1-r19 ThresholdQ OPTIONAL -- Need R

 } OPTIONAL, -- Cond SupportLROnLPSS

 enryEvaluationOnMRForLROnSSB-r19 SEQUENCE {

 thresholdP2-r19 ThresholdP,

 thresholdQ2-r19 ThresholdQ OPTIONAL -- Need R

 } OPTIONAL, -- Cond SupportLROnSSB

 entryEvaluationOnLROnSSB-r19 SEQUENCE {

 thresholdPLP1-r19 ThresholdPLP,

 thresholdQLP1-r19 ThresholdQLP OPTIONAL -- Need R

 } OPTIONAL, -- Need R

 enryEvaluationOnLROnLPSS-r19 SEQUENCE {

 thresholdP3-r19 ThresholdPLP,

 thresholdQ3-r19 ThresholdQLP OPTIONAL -- Need R

 } OPTIONAL, -- Need R

 ...

}

ExitCondition-r19 ::= SEQUENCE {

 exitEvaluationOnLROnLPSS-r19 SEQUENCE {

 thresholdPLP2-r19 ThresholdPLP,

 thresholdQLP2-r19 ThresholdQLP OPTIONAL -- Need R

 } OPTIONAL, -- Cond SupportLROnLPSS

 exitEvaluationOnLROnSSB-r19 SEQUENCE {

 thresholdP4-r19 ThresholdPLP,

 thresholdQ4-r19 ThresholdQLP OPTIONAL -- Need R

 } OPTIONAL, -- Cond SupportLROnSSB

 ...

}

-- TAG-DOWNLINKCONFIGCOMMONSIB-STOP

-- ASN1STOP

Editor’s NOTE: FFS on whether LP-WUS/LP-SS configuration is provided in SIB1 or new SIB.

Editor’s NOTE: FFS on the values for each RRC parameters. To be updated based on RAN1/RAN2 progress.

Editor’s NOTE: FFS on the detailed RRC parameters. To be updated based on RAN1/RAN2 progress.

Editor’s NOTE: FFS on common or separate configuration for EPRA ratio between LP-WUS/LP-SS and SSB for LP-WUS and LP-SS.

Editor’s NOTE: FFS on whether entry/exit condition is mandatory or optional.

Editor’s NOTE: FFS on the relationship between the thresholds for serving cell relaxation/offloading, neighboring cell relaxation and entry/exit condition of using LP-WUS, [and potential pre-condition between RRM relaxation/offloading criteria and entry/exit condition of using LP-WUS].

|  |
| --- |
| *DownlinkConfigCommonSIB* field descriptions |
| ***bcch-Config***The modification period related configuration. |
| ***frequencyInfoDL-SIB***Basic parameters of a downlink carrier and transmission thereon. |
| ***initialDownlinkBWP***The initial downlink BWP configuration for a PCell. The network configures the *locationAndBandwidth* so that the initial downlink BWP contains the entire CORESET#0 of this serving cell in the frequency domain. The UE applies the *locationAndBandwidth* upon reception of this field (e.g. to determine the frequency position of signals described in relation to this *locationAndBandwidth*) but it keeps CORESET#0 until after reception of *RRCSetup*/*RRCResume/RRCReestablishment*. |
| ***initialDownlinkBWP-RedCap***If present, (e)RedCap UEs use this DL BWP instead of *initialDownlinkBWP*. If the *locationAndBandwidth* of this BWP contains the entire CORESET#0, the UE applies the *locationAndBandwidth* upon reception of this field (e.g. to determine the frequency position of signals described in relation to this *locationAndBandwidth*) but it keeps CORESET#0 until after reception of *RRCSetup*/*RRCResume/RRCReestablishment*. Otherwise, i.e., if the *locationAndBandwidth* of this BWP does not contain the entire CORESET#0, the UE uses this BWP for receiving DL messages during initial access (Msg2, MsgB, Msg4) and after initial access.If absent, (e)RedCap UEs use *initialDownlinkBWP* provided that it does not exceed the (e)RedCap UE maximum bandwidth (see also clause 5.2.2.4.2). |
| ***lastUsedCellOnly***When present, the field indicates that the UE monitors PEI only if the latest received *RRCRelease* without *noLastCellUpdate* is from this cell. A PEI-capable UE stores its last used cell information. |
| ***lowPower-Config***The LP-WUS and LP-SS related configuration. |
| ***lp-subgroupConfig***The LP-WUS subgroup related configuration. |
| ***pcch-Config***The paging related configuration. |
| ***pei-Config***The PEI related configuration. |
| ***subgroupConfig***The paging subgroup related configuration. |

|  |
| --- |
| *BCCH-Config* field descriptions |
| ***modificationPeriodCoeff***Actual modification period, expressed in number of radio frames m = *modificationPeriodCoeff* \* *defaultPagingCycle*, see clause 5.2.2.2.2. *n2* corresponds to value 2, *n4* corresponds to value 4, and so on. |

|  |
| --- |
| *PCCH-Config* field descriptions |
| ***defaultPagingCycle***Default paging cycle, used to derive 'T' in TS 38.304 [20]. Value *rf32* corresponds to 32 radio frames, value *rf64* corresponds to 64 radio frames and so on. |
| ***firstPDCCH-MonitoringOccasionOfPO***Points out the first PDCCH monitoring occasion for paging of each PO of the PF, see TS 38.304 [20]. |
| ***nAndPagingFrameOffset***Used to derive the number of total paging frames in T (corresponding to parameter N in TS 38.304 [20]) and paging frame offset (corresponding to parameter PF\_offset in TS 38.304 [20]). A value of *oneSixteenthT* corresponds to T / 16, a value of oneEighthT corresponds to T / 8, and so on.If *pagingSearchSpace* is set to zero and if SS/PBCH block and CORESET multiplexing pattern is 2 or 3 (as specified in TS 38.213 [13]):- for *ssb-periodicityServingCell* of 5 or 10 ms, N can be set to one of {*oneT, halfT, quarterT, oneEighthT, oneSixteenthT*}- for *ssb-periodicityServingCell* of 20 ms, N can be set to one of {*halfT, quarterT, oneEighthT, oneSixteenthT*}- for *ssb-periodicityServingCell* of 40 ms, N can be set to one of {*quarterT, oneEighthT, oneSixteenthT*}- for *ssb-periodicityServingCell* of 80 ms, N can be set to one of {*oneEighthT, oneSixteenthT*}- for *ssb-periodicityServingCell* of 160 ms, N can be set to *oneSixteenthT*If *pagingSearchSpace* is set to zero and if SS/PBCH block and CORESET multiplexing pattern is 1 (as specified in TS 38.213 [13]), N can be set to one of {*halfT, quarterT, oneEighthT, oneSixteenthT*}If *pagingSearchSpace* is not set to zero, N can be configured to one of {*oneT, halfT, quarterT, oneEighthT, oneSixteenthT*} |
| ***nrofPDCCH-MonitoringOccasionPerSSB-InPO***The number of PDCCH monitoring occasions corresponding to an SSB within a Paging Occasion, see TS 38.304 [20], clause 7.1. |
| ***ns***Number of paging occasions per paging frame. |
| ***ranPagingInIdlePO***Indicates that the network supports to send RAN paging in PO that corresponds to the i\_s as determined by UE in RRC\_IDLE state, see TS38.304 [20]. |

|  |
| --- |
| *PEI-Config* field descriptions |
| ***payloadSizeDCI-2-7***Payload size of PEI DCI, i.e., DCI format 2\_7. The size is no larger than the payload size of paging DCI which has maximum of 41 bits and 43 bits for licensed and unlicensed spectrums, respectively. |
| ***pei-FrameOffset***Offset, in number of frames from the start of a reference frame for PEI-O to the start of a first paging frame of the paging frames associated with the PEI-O, see TS 38.213 [13], clause 10.4A. |
| ***po-NumPerPEI***The number of PO(s) associated with one PEI monitoring occasion. It is a factor of the total PO number in a paging cycle, i.e N x Ns, as specified in TS 38.304 [20]. The maximum number of PF associated with one PEI monitoring occasion is 2. The number of PO mapping to one PEI should be multiple of Ns when *po-NumPerPEI* is larger than Ns. |

|  |
| --- |
| *SubgroupConfig* field descriptions |
| ***subgroupsNumPerPO***Total number of subgroups per Paging Occasion (PO) for UE to read subgroups indication from physical-layer signaling. The field represents the sum of CN-assigned and UEID-based subgroups supported for PEI by the network. When *PEI-Config* is configured, there is always at least one subgroup (UEID-based subgroup or CN-assigned subgroup) configured. |
| ***subgroupsNumForUEID***Number of subgroups per Paging Occasion (PO) for UE to read subgroups indication from physical-layer signaling, for UEID-based subgrouping method for PEI. When present, the fieldis set to an integer smaller than or equal to *subgroupsNumPerPO. subgroupsNumPerPO* equals to *subgroupsNumForUEID* when the network does not configure CN-assigned subgrouping for PEI. When *pei-Config* is configured, the field is absent when the network only configures CN-assigned subgrouping. Both this field and *subgroupsNumPerPO* are equal to 1 when the network does not configure subgrouping. When *pei-Config* is configured, if the field is absent, the UE uses subgrouping according to TS 38.304 [20], clause 7.3.0. |

|  |
| --- |
| *LowPower-Config* field descriptions |
| ***lpwus-MvalueFR1***Indicates the number of OOK symbols in an OFDM symbol for LP-WUS in FR1 (see TS 38.211 [16], clause xxxx). |
| ***lpwus-MvalueFR2***Indicates the number of OOK symbols in an OFDM symbol for LP-WUS in FR2 (see TS 38.211 [16], clause xxxx). |
| ***lpss-MvalueFR1***Indicates the number of OOK symbols in an OFDM symbol for LP-SS in FR1 (see TS 38.211 [16], clause xxxx). |
| ***lpss-MvalueFR2***Indicates the number of OOK symbols in an OFDM symbol for LP-SS in FR2 (see TS 38.211 [16], clause xxxx). |
| ***lpwus-Lpss-StartRB***Indicates the starting RB of LP-WUS and LP-SS (see TS 38.211 [16], clause xxxx).  |
| ***lpwus-BinarySeq-StartRB***Indicates the LP-SS binary sequence index in the cell (see TS 38.211 [16], clause xxxx).  |
| ***lpss-PeriodicityAndOffset***Used to derive the periodicity and offset for LP-SS (see TS 38.211 [16], clause xxxx). |
| ***additionalSync***TBD Indicates the dditional sync signal related information, e.g. enable/disable of additional sync signal (see TS 38.211 [16], clause xxxx). |
| ***lpwus-OverlaidSeq***Indicates the configuration of overlaid OFDM sequence used per OOK symbol for LP-WUS (see TS 38.211 [16], clause xxx). |
| ***lpss-OverlaidSeq***Indicates the configuration of overlaid OFDM sequence used per OOK symbol for LP-SS (see TS 38.211 [16], clause xxx). |
| ***lpwus-MoNumPerLo***Indicates the number of LP-WUS MO(s) per beam within a LO for LP-WUS (see TS 38.213 [13], clause xxx). |
| ***lpwus-PoNumPerLo***Indicates the number of PO(s) associated with one LO for LP-WUS (see TS 38.213 [13], clause xxx). |
| ***lpwus-LoOffset***Indicates the offset value(s) between a LO and a reference PO/PF, which includes at least a frame-level offset, FFS other offsets (slot/symbol level). |

|  |
| --- |
| *LP-SubgroupConfig* field descriptions |
| ***lpSubgroupsNumPerPO***Total number of subgroups per Paging Occasion (PO) for UE to read subgroups indication from LP-WUS signaling. The field represents the sum of CN-assigned and UEID-based subgroups supported for LP-WUS by the network. When lowPower*-Config* is configured, there is always at least one subgroup (UEID-based subgroup or CN-assigned subgroup) configured. |
| ***lpSubgroupsNumForUEID***Number of subgroups per Paging Occasion (PO) for UE to read subgroups indication from LP-WUS signaling, for UEID-based subgrouping method for LP-WUS. When present, the fieldis set to an integer smaller than or equal to *lpSubgroupsNumPerPO. lpSubgroupsNumPerPO* equals to *lpSubgroupsNumForUEID* when the network does not configure CN-assigned subgrouping for LP-WUS. When *lowPower-Config* is configured, the field is absent when the network only configures CN-assigned subgrouping. Both this field and *lpSubgroupsNumPerPO* are equal to 1 when the network does not configure subgrouping. When *lowPower-Config* is configured, if the field is absent, the UE uses subgrouping according to TS 38.304 [20], clause xxx. |

|  |
| --- |
| EntryCondition, ExitConditionfield descriptions |
| ***enryEvaluationOnMRForLROnLPSS***Indicates the threshold(s) for a UE supporting OOK based LP-WUR or OFDM based LP-WUS measure on LP-SS to determine whether the entry condition for using LP-WUS is fulfilled or not based on the serving cell measurement on MR (see TS 38.304 [20], clause xxxx).  |
| ***enryEvaluationOnMRForLROnSSB***Indicates the threshold(s) for a UE supporting OFDM based LP-WUR measure on SSB to determine whether the entry condition for using LP-WUS is fulfilled or not based on the serving cell measurement on MR (see TS 38.304 [20], clause xxxx). |
| ***entryEvaluationOnLROnLPSS***Indicates the threshold(s) for a UE supporting OOK based LP-WUR or OFDM based LP-WUS measure on LP-SS to determine whether the entry condition for using LP-WUS is fulfilled or not based on the serving cell measurement on OOK based LP-WUR (see TS 38.304 [20], clause xxxx). |
| ***entryEvaluationOnLROnSSB***Indicates the threshold(s) for a UE supporting OFDM based LP-WUR measure on SSB to determine whether the entry condition for using LP-WUS is fulfilled or not based on the serving cell measurement on OFDM based LP-WUR (see TS 38.304 [20], clause xxxx). |
| ***exitEvaluationOnLROnLPSS***Indicates the threshold(s) for a UE supporting OOK based LP-WUR or OFDM based LP-WUS measure on LP-SS to determine whether the exit condition for using LP-WUS is fulfilled or not based on the serving cell measurement on OOK based LP-WUR (see TS 38.304 [20], clause xxxx). |
| ***exitEvaluationOnLROnSSB***Indicates the threshold(s) for a UE supporting OFDM based LP-WUR measure on SSB to determine whether the exit condition for using LP-WUS is fulfilled or not based on the serving cell measurement on OFDM based LP-WUR (see TS 38.304 [20], clause xxxx). |
| ***thresholdP1, thresholdP2, thresholdP3, thresholdP4***Parameters "xx", "xx", "xx", and "xxx" in TS 38.304 [20].  |
| ***thresholdQ1, thresholdQ2, thresholdQ3, thresholdQ4*** Parameters "xx", "xx", "xx", and "xxx" in TS 38.304 [20]. |
| ***thresholdPLP1, thresholdPLP2*** Parameters "xx", "xx", and "xxx" in TS 38.304 [20].  |
| ***thresholdQLP1, thresholdQLP2*** Parameters "xx", "xx", and "xxx" in TS 38.304 [20].  |

|  |  |
| --- | --- |
| Conditional Presence | Explanation |
| *SharedSpectrum2* | The field is optional present, Need R, if this cell operates with shared spectrum channel access. Otherwise, it is absent, Need R. |
| *FR1-Only* | This field is mandatory present for an FR1 carrier frequency. It is absent otherwise. |
| *FR2-Only* | This field is mandatory present for an FR2 carrier frequency. It is absent otherwise. |
| *OOK-Only* | This field is mandatory present for OOK-based LP-WUR for LP-WUS operation (see TS 38.211 [16], clause xxx). It is absent otherwise. |
| *OFDM-Only* | This field is mandatory present for OFDM-based LP-WUR for LP-WUS operation (see TS 38.211 [16], clause xxx). It is absent otherwise. |
| *SupportLROnLPSS* | This field is [mandatory present] or [optional present, Need R,] for the cell supporting OOK based LP-WUR or OFDM based LP-WUR measure on LP-SS. It is absent otherwise. |
| *SupportLROnSSB* | This field is [mandatory present] or [optional present, Need R,] for the cell supporting OFDM based LP-WUR measure on SSB. It is absent otherwise. |

Next change

#### – *PhysicalCellGroupConfig*

The IE *PhysicalCellGroupConfig* is used to configure cell-group specific L1 parameters.

*PhysicalCellGroupConfig* information element

-- ASN1START

-- TAG-PHYSICALCELLGROUPCONFIG-START

PhysicalCellGroupConfig ::= SEQUENCE {

 harq-ACK-SpatialBundlingPUCCH ENUMERATED {true} OPTIONAL, -- Need S

 harq-ACK-SpatialBundlingPUSCH ENUMERATED {true} OPTIONAL, -- Need S

 p-NR-FR1 P-Max OPTIONAL, -- Need R

 pdsch-HARQ-ACK-Codebook ENUMERATED {semiStatic, dynamic},

 tpc-SRS-RNTI RNTI-Value OPTIONAL, -- Need R

 tpc-PUCCH-RNTI RNTI-Value OPTIONAL, -- Need R

 tpc-PUSCH-RNTI RNTI-Value OPTIONAL, -- Need R

 sp-CSI-RNTI RNTI-Value OPTIONAL, -- Need R

 cs-RNTI SetupRelease { RNTI-Value } OPTIONAL, -- Need M

 ...,

 [[

 mcs-C-RNTI RNTI-Value OPTIONAL, -- Need R

 p-UE-FR1 P-Max OPTIONAL -- Cond MCG-Only

 ]],

 [[

 xScale ENUMERATED {dB0, dB6, spare2, spare1} OPTIONAL -- Cond SCG-Only

 ]],

 [[

 pdcch-BlindDetection SetupRelease { PDCCH-BlindDetection } OPTIONAL -- Need M

 ]],

 [[

 dcp-Config-r16 SetupRelease { DCP-Config-r16 } OPTIONAL, -- Need M

 harq-ACK-SpatialBundlingPUCCH-secondaryPUCCHgroup-r16 ENUMERATED {enabled, disabled} OPTIONAL, -- Cond twoPUCCHgroup

 harq-ACK-SpatialBundlingPUSCH-secondaryPUCCHgroup-r16 ENUMERATED {enabled, disabled} OPTIONAL, -- Cond twoPUCCHgroup

 pdsch-HARQ-ACK-Codebook-secondaryPUCCHgroup-r16 ENUMERATED {semiStatic, dynamic} OPTIONAL, -- Cond twoPUCCHgroup

 p-NR-FR2-r16 P-Max OPTIONAL, -- Need R

 p-UE-FR2-r16 P-Max OPTIONAL, -- Cond MCG-Only

 nrdc-PCmode-FR1-r16 ENUMERATED {semi-static-mode1, semi-static-mode2, dynamic} OPTIONAL, -- Cond MCG-Only

 nrdc-PCmode-FR2-r16 ENUMERATED {semi-static-mode1, semi-static-mode2, dynamic} OPTIONAL, -- Cond MCG-Only

 pdsch-HARQ-ACK-Codebook-r16 ENUMERATED {enhancedDynamic} OPTIONAL, -- Need R

 nfi-TotalDAI-Included-r16 ENUMERATED {true} OPTIONAL, -- Need R

 ul-TotalDAI-Included-r16 ENUMERATED {true} OPTIONAL, -- Need R

 pdsch-HARQ-ACK-OneShotFeedback-r16 ENUMERATED {true} OPTIONAL, -- Need R

 pdsch-HARQ-ACK-OneShotFeedbackNDI-r16 ENUMERATED {true} OPTIONAL, -- Need R

 pdsch-HARQ-ACK-OneShotFeedbackCBG-r16 ENUMERATED {true} OPTIONAL, -- Need R

 downlinkAssignmentIndexDCI-0-2-r16 ENUMERATED { enabled } OPTIONAL, -- Need S

 downlinkAssignmentIndexDCI-1-2-r16 ENUMERATED {n1, n2, n4} OPTIONAL, -- Need S

 pdsch-HARQ-ACK-CodebookList-r16 SetupRelease {PDSCH-HARQ-ACK-CodebookList-r16} OPTIONAL, -- Need M

 ackNackFeedbackMode-r16 ENUMERATED {joint, separate} OPTIONAL, -- Need R

 pdcch-BlindDetectionCA-CombIndicator-r16 SetupRelease { PDCCH-BlindDetectionCA-CombIndicator-r16 } OPTIONAL, -- Need M

 pdcch-BlindDetection2-r16 SetupRelease { PDCCH-BlindDetection2-r16 } OPTIONAL, -- Need M

 pdcch-BlindDetection3-r16 SetupRelease { PDCCH-BlindDetection3-r16 } OPTIONAL, -- Need M

 bdFactorR-r16 ENUMERATED {n1} OPTIONAL -- Need R

 ]],

 [[

 -- start of enhanced Type3 feedback

 pdsch-HARQ-ACK-EnhType3ToAddModList-r17 SEQUENCE (SIZE(1..maxNrofEnhType3HARQ-ACK-r17)) OF PDSCH-HARQ-ACK-EnhType3-r17

 OPTIONAL, -- Need N

 pdsch-HARQ-ACK-EnhType3ToReleaseList-r17 SEQUENCE (SIZE(1..maxNrofEnhType3HARQ-ACK-r17)) OF PDSCH-HARQ-ACK-EnhType3Index-r17

 OPTIONAL, -- Need N

 pdsch-HARQ-ACK-EnhType3SecondaryToAddModList-r17 SEQUENCE (SIZE(1..maxNrofEnhType3HARQ-ACK-r17)) OF PDSCH-HARQ-ACK-EnhType3-r17

 OPTIONAL, -- Need N

 pdsch-HARQ-ACK-EnhType3SecondaryToReleaseList-r17 SEQUENCE (SIZE(1..maxNrofEnhType3HARQ-ACK-r17)) OF PDSCH-HARQ-ACK-EnhType3Index-r17

 OPTIONAL, -- Need N

 pdsch-HARQ-ACK-EnhType3DCI-FieldSecondaryPUCCHgroup-r17 ENUMERATED {enabled} OPTIONAL, -- Cond twoPUCCHgroup

 pdsch-HARQ-ACK-EnhType3DCI-Field-r17 ENUMERATED {enabled} OPTIONAL, -- Need R

 -- end of enhanced Type3 feedback

 -- start of triggering of HARQ-ACK re-transmission on a PUCCH resource

 pdsch-HARQ-ACK-Retx-r17 ENUMERATED {enabled} OPTIONAL, -- Need R

 pdsch-HARQ-ACK-RetxSecondaryPUCCHgroup-r17 ENUMERATED {enabled} OPTIONAL, -- Cond twoPUCCHgroup

 -- end of triggering of HARQ-ACK re-transmission on a PUCCH resource

 -- start of PUCCH Cell switching

 pucch-sSCell-r17 SCellIndex OPTIONAL, -- Need R

 pucch-sSCellSecondaryPUCCHgroup-r17 SCellIndex OPTIONAL, -- Cond twoPUCCHgroup

 pucch-sSCellDyn-r17 ENUMERATED {enabled} OPTIONAL, -- Need R

 pucch-sSCellDynSecondaryPUCCHgroup-r17 ENUMERATED {enabled} OPTIONAL, -- Cond twoPUCCHgroup

 pucch-sSCellPattern-r17 SEQUENCE (SIZE(1..maxNrofSlots)) OF INTEGER (0..1) OPTIONAL, -- Need R

 pucch-sSCellPatternSecondaryPUCCHgroup-r17 SEQUENCE (SIZE(1..maxNrofSlots)) OF INTEGER (0..1) OPTIONAL, -- Cond twoPUCCHgroup

 -- end of PUCCH Cell switching

 uci-MuxWithDiffPrio-r17 ENUMERATED {enabled} OPTIONAL, -- Need R

 uci-MuxWithDiffPrioSecondaryPUCCHgroup-r17 ENUMERATED {enabled} OPTIONAL, -- Cond twoPUCCHgroup

 simultaneousPUCCH-PUSCH-r17 ENUMERATED {enabled} OPTIONAL, -- Need R

 simultaneousPUCCH-PUSCH-SecondaryPUCCHgroup-r17 ENUMERATED {enabled} OPTIONAL, -- Cond twoPUCCHgroup

 prioLowDG-HighCG-r17 ENUMERATED {enabled} OPTIONAL, -- Need R

 prioHighDG-LowCG-r17 ENUMERATED {enabled} OPTIONAL, -- Need R

 twoQCLTypeDforPDCCHRepetition-r17 ENUMERATED {enabled} OPTIONAL, -- Need R

 multicastConfig-r17 SetupRelease { MulticastConfig-r17 } OPTIONAL, -- Need M

 pdcch-BlindDetectionCA-CombIndicator-r17 SetupRelease { PDCCH-BlindDetectionCA-CombIndicator-r17 } OPTIONAL -- Need M

 ]],

 [[

 simultaneousSR-PUSCH-diffPUCCH-Groups-r17 ENUMERATED {enabled} OPTIONAL -- Cond twoPUCCHgroup

 ]],

 [[

 intraBandNC-PRACH-simulTx-r17 ENUMERATED {enabled} OPTIONAL -- Need R

 ]],

 [[

 pdcch-BlindDetection4-r17 SetupRelease { PDCCH-BlindDetection4-r17 } OPTIONAL -- Need M

 ]],

 [[

 simultaneousPUCCH-PUSCH-SamePriority-r17 ENUMERATED {enabled} OPTIONAL, -- Need R

 simultaneousPUCCH-PUSCH-SamePriority-SecondaryPUCCHgroup-r17 ENUMERATED {enabled} OPTIONAL -- Cond twoPUCCHgroup

 ]],

 [[

 ncr-RNTI-r18 RNTI-Value OPTIONAL, -- Cond NCR

 cellDTRX-DCI-config-r18 SetupRelease { CellDTRX-DCI-config-r18 } OPTIONAL, -- Need M

 twoQCL-TypeD-ForMultiDCI-r18 ENUMERATED {enabled} OPTIONAL, -- Need R

 enableType1HARQ-ACK-MuxForDL-AssignmentAfterUL-Grant-r18 ENUMERATED {enabled} OPTIONAL, -- Need R

 enableType2HARQ-ACK-MuxForDL-AssignmentAfterUL-Grant-r18 ENUMERATED {enabled} OPTIONAL, -- Need R

 enableType3HARQ-ACK-MuxForDL-AssignmentAfterUL-Grant-r18 ENUMERATED {enabled} OPTIONAL, -- Need R

 enableDiffPUCCH-Resource-r18 ENUMERATED {enabled} OPTIONAL, -- Need R

 enableDiffCB-Size-r18 ENUMERATED {enabled} OPTIONAL -- Need R

 ]],

 [[

 lpwus-Config-r19 SetupRelease { LPWUS-Config-r19 } OPTIONAL -- Need M

 ]]

}

PDSCH-HARQ-ACK-EnhType3-r17 ::= SEQUENCE {

 pdsch-HARQ-ACK-EnhType3Index-r17 PDSCH-HARQ-ACK-EnhType3Index-r17,

 applicable-r17 CHOICE {

 perCC SEQUENCE (SIZE (1..maxNrofServingCells)) OF INTEGER (0..1),

 perHARQ SEQUENCE (SIZE (1..maxNrofServingCells)) OF BIT STRING (SIZE (16))

 },

 pdsch-HARQ-ACK-EnhType3NDI-r17 ENUMERATED {true} OPTIONAL, -- Need R

 pdsch-HARQ-ACK-EnhType3CBG-r17 ENUMERATED {true} OPTIONAL, -- Need S

 ...,

 [[

 perHARQ-Ext-r17 SEQUENCE (SIZE (1..maxNrofServingCells)) OF BIT STRING (SIZE (32)) OPTIONAL -- Need R

 ]]

}

PDSCH-HARQ-ACK-EnhType3Index-r17 ::= INTEGER (0..maxNrofEnhType3HARQ-ACK-1-r17)

PDCCH-BlindDetection ::= INTEGER (1..15)

DCP-Config-r16 ::= SEQUENCE {

 ps-RNTI-r16 RNTI-Value,

 ps-Offset-r16 INTEGER (1..120),

 sizeDCI-2-6-r16 INTEGER (1..maxDCI-2-6-Size-r16),

 ps-PositionDCI-2-6-r16 INTEGER (0..maxDCI-2-6-Size-1-r16),

 ps-WakeUp-r16 ENUMERATED {true} OPTIONAL, -- Need S

 ps-TransmitPeriodicL1-RSRP-r16 ENUMERATED {true} OPTIONAL, -- Need S

 ps-TransmitOtherPeriodicCSI-r16 ENUMERATED {true} OPTIONAL -- Need S

}

PDSCH-HARQ-ACK-CodebookList-r16 ::= SEQUENCE (SIZE (1..2)) OF ENUMERATED {semiStatic, dynamic}

PDCCH-BlindDetectionCA-CombIndicator-r16 ::= SEQUENCE {

 pdcch-BlindDetectionCA1-r16 INTEGER (1..15),

 pdcch-BlindDetectionCA2-r16 INTEGER (1..15)

}

PDCCH-BlindDetection2-r16 ::= INTEGER (1..15)

PDCCH-BlindDetection3-r16 ::= INTEGER (1..15)

PDCCH-BlindDetection4-r17 ::= INTEGER (1..15)

MulticastConfig-r17 ::= SEQUENCE {

 pdsch-HARQ-ACK-CodebookListMulticast-r17 SetupRelease { PDSCH-HARQ-ACK-CodebookList-r16} OPTIONAL, -- Need M

 type1CodebookGenerationMode-r17 ENUMERATED { mode1, mode2} OPTIONAL -- Need M

}

PDCCH-BlindDetectionCA-CombIndicator-r17 ::= SEQUENCE {

 pdcch-BlindDetectionCA1-r17 INTEGER (1..15) OPTIONAL, -- Need R

 pdcch-BlindDetectionCA2-r17 INTEGER (1..15) OPTIONAL, -- Need R

 pdcch-BlindDetectionCA3-r17 INTEGER (1..15)

}

CellDTRX-DCI-config-r18 ::= SEQUENCE {

 cellDTRX-RNTI-r18 RNTI-Value,

 sizeDCI-2-9-r18 INTEGER (1..maxDCI-2-9-Size-r18)

}

LPWUS-Config-r19 ::= SEQUENCE {

 lpwus-MvalueFR1-r19 ENUMERATED {1, 2, 4} OPTIONAL, -- Cond FR1-only

 FFS lpwus-MvalueFR2-r19 TBD OPTIONAL, -- Cond FR2-only

---------Method 1-------------

 FFS lpwus-Offset11-r19 TBD [INTEGER (1..120)] OPTIONAL, -- Cond xx

 FFS lpwus-Offset12-r19 TBD [INTEGER (1..120)] OPTIONAL, -- Cond yy

 FFS lpwus-MO11-r19 TBD,

 FFS lpwus-MO12-r19 TBD,

---------Method 2-------------

 FFS lpwus-Offset-r19 TBD [INTEGER (1..120)],

 FFS lpwus-MO-r19 TBD,

 FFS lpwus-StartRB-r19 INTEGER (0..263) OPTIONAL, -- Need R

 FFS lpwus-OverlaidSeq-r19 TBD,

 lpwus-PDCCHMonitoringTimer-r19 TBD OPTIONAL, -- Cond TBD\_Offset12

 lpwus-TransmitOtherPeriodicCSI-r19 ENUMERATED {true} OPTIONAL, -- Need S

 lpwus-TransmitPeriodicL1-RSRP-r19 ENUMERATED {true} OPTIONAL, -- Need S

 FFS lpwus-Codepoint-r19 TBD,

 lpwus-WakeUp11-r19 ENUMERATED {true} OPTIONAL -- Need S

}

-- TAG-PHYSICALCELLGROUPCONFIG-STOP

-- ASN1STOP

Editor’s NOTE: FFS on whether the LP-WUS configuration is per-UE or per-CG.

Editor’s NOTE: FFS on the values for each RRC parameters. To be updated based on RAN1/RAN2 progress.

Editor’s NOTE: FFS on the detailed RRC parameters. To be updated based on RAN1/RAN2 progress.

Editor’s NOTE: FFS on whether each configuration for LP-WUS is optional or mandatory. To be updated based on RAN1/RAN2 progress.

Editor’s NOTE: FFS on whether offset for option 1-1 and option 1-2 are configured separately (i.e. method 1 above) or only one offset is configured for both option 1-1 and option 1-2 (i.e. method 2 above), and introducing another parameter to differentiate the option 1-1 and option 1-2. To be updated based on RAN1/RAN2 progress.

|  |
| --- |
| *PhysicalCellGroupConfig* field descriptions |
| ***ackNackFeedbackMode***Indicates which among the joint and separate ACK/NACK feedback modes to use within a slot as specified in TS 38.213 [13] (clause 9). |
| ***bdFactorR***Parameter for determining and distributing the maximum numbers of BD/CCE for mPDCCH based mPDSCH transmission as specified in TS 38.213 [13] Clause 10.1. |
| ***cs-RNTI***RNTI value for downlink SPS (see *SPS-Config*) and uplink configured grant (see *ConfiguredGrantConfig*). |
| ***downlinkAssignmentIndexDCI-0-2***Indicates if "Downlink assignment index" is present or absent in DCI format 0\_2. If the field "*downlinkAssignmentIndexDCI-0-2*" is absent, then 0 bit for "Downlink assignment index" in DCI format 0\_2. If the field "*downlinkAssignmentIndexDCI-0-2*" is present, then the bitwidth of "Downlink assignment index" in DCI format 0\_2 is defined in the same was as that in DCI format 0\_1 (see TS 38.212 [17], clause 7.3.1 and TS 38.213 [13], clause 9.1). |
| ***downlinkAssignmentIndexDCI-1-2***Configures the number of bits for "Downlink assignment index" in DCI format 1\_2. If the field is absent, then 0 bit is applied for "Downlink assignment index" in DCI format 1\_2. Note that 1 bit and 2 bits are applied if only one serving cell is configured in the DL and *pdsch-HARQ-ACK-Codebook* is set to *dynamic*. 4 bits is applied if more than one serving cell are configured in the DL and *pdsch-HARQ-ACK-Codebook* is set to *dynamic* (see TS 38.212 [17], clause 7.3.1 and TS 38.213 [13], clause 9.1). |
| ***enableDiffCB-Size***This field indicates whether a different codebook size from the size determined based on HARQ-ACK information associated with PDSCH reception(s) scheduled before a UL grant, is determined or not to include HARQ-ACK information associated with PDSCH reception(s) scheduled after a UL grant scheduling a PUSCH transmission with repetitions and the HARQ-ACK information are multiplexed on a repetition of the PUSCH transmission other than a first repetition. If enabled, a different HARQ codebook size might be determined. See clause 9 in TS 38.213 [13]. |
| ***enableDiffPUCCH-Resource***This field indicates whether a different PUCCH resource in time domain in a slot from the PUCCH resource indicated by the last DCI format before a UL grant in the slot, is determined or not to include HARQ-ACK information associated with PDSCH reception(s) scheduled after a UL grant scheduling a PUSCH transmission with repetitions and the HARQ-ACK information are multiplexed on a repetition of the PUSCH transmission other than a first repetition in the same slot. If enabled, a different PUCCH resource in time domain might be determined. See clause 9 in TS 38.213 [13]. |
| ***enableType1HARQ-ACK-MuxForDL-AssignmentAfterUL-Grant***If enabled, UE multiplexes Type-1 HARQ-ACK codebook on a repetition of a PUSCH transmission other than a first repetition, where the HARQ-ACK codebook includes HARQ-ACK information associated with PDSCH reception(s) scheduled after the UL grant scheduling the PUSCH transmission. See clause 9 in TS 38.213 [13]. This feature is not simultaneously enabled with PUCCH cell switching. |
| ***enableType2HARQ-ACK-MuxForDL-AssignmentAfterUL-Grant***If enabled, UE multiplexes Type-2 HARQ-ACK codebook on a repetition of a PUSCH transmission other than a first repetition, where the HARQ-ACK codebook includes HARQ-ACK information associated with PDSCH reception(s) scheduled after the UL grant scheduling the PUSCH transmission. See clause 9 in TS 38.213 [13]. This feature is not simultaneously enabled with PUCCH cell switching. |
| ***enableType3HARQ-ACK-MuxForDL-AssignmentAfterUL-Grant***If enabled, UE multiplexes Type-3 HARQ-ACK codebook on a repetition of a PUSCH transmission other than a first repetition, where the HARQ-ACK codebook includes HARQ-ACK information associated with PDSCH reception(s) scheduled after the UL grant scheduling the PUSCH transmission. See clause 9 in TS 38.213 [13]. This feature is not simultaneously enabled with PUCCH cell switching. |
| ***harq-ACK-SpatialBundlingPUCCH***Enables spatial bundling of HARQ ACKs. It is configured per cell group (i.e. for all the cells within the cell group) for PUCCH reporting of HARQ-ACK. It is only applicable when more than 4 layers are possible to schedule. When the field is absent, the spatial bundling of PUCCH HARQ ACKs for the primary PUCCH group is disabled (see TS 38.213 [13], clause 9.1.2.1). If the field *harq-ACK SpatialBundlingPUCCH-secondaryPUCCHgroup* is present, *harq-ACK-SpatialBundlingPUCCH* is only applied to primary PUCCH group. Network does not configure for a UE both spatial bundling of HARQ ACKs and *codeBlockGroupTransmission* within the same cell group. |
| ***harq-ACK-SpatialBundlingPUCCH-secondaryPUCCHgroup***Indicates whether spatial bundling of PUCCH HARQ ACKs for the secondary PUCCH group is enabled or disabled. The field is only applicable when more than 4 layers are possible to schedule (see TS 38.213 [13], clause 9.1.2.1). When the field is absent, the use of spatial bundling of PUCCH HARQ ACKs for the secondary PUCCH group is indicated by *harq-ACK-SpatialBundlingPUCCH*. See TS 38.213 [13], clause 9.1.2.1. Network does not configure for a UE both spatial bundling of HARQ ACKs and *codeBlockGroupTransmission* within the same cell group. |
| ***harq-ACK-SpatialBundlingPUSCH***Enables spatial bundling of HARQ ACKs. It is configured per cell group (i.e. for all the cells within the cell group) for PUSCH reporting of HARQ-ACK. It is only applicable when more than 4 layers are possible to schedule. When the field is absent, the spatial bundling of PUSCH HARQ ACKs for the primary PUCCH group is disabled (see TS 38.213 [13], clauses 9.1.2.2 and 9.1.3.2). If the field *harq-ACK SpatialBundlingPUSCH-secondaryPUCCHgroup* is present, *harq-ACK-SpatialBundlingPUSCH* is only applied to primary PUCCH group. Network does not configure for a UE both spatial bundling of HARQ ACKs and *codeBlockGroupTransmission* within the same cell group. |
| ***harq-ACK-SpatialBundlingPUSCH-secondaryPUCCHgroup***Indicates whether spatial bundling of PUSCH HARQ ACKs for the secondary PUCCH group is enabled or disabled. The field is only applicable when more than 4 layers are possible to schedule (see TS 38.213 [13], clauses 9.1.2.2 and 9.1.3.2). When the field is absent, the use of spatial bundling of PUSCH HARQ ACKs for the secondary PUCCH group is indicated by *harq-ACK-SpatialBundlingPUSCH*. See TS 38.213 [13], clauses 9.1.2.2 and 9.1.3.2. Network does not configure for a UE both spatial bundling of HARQ ACKs and *codeBlockGroupTransmission* within the same cell group. |
| ***intraBandNC-PRACH-simulTx***Enables parallel PRACH and SRS/PUCCH/PUSCH transmissions across CCs in intra-band non-contiguous CA (see TS 38.213 [13], clause 8.1 and TS 38.214 [19], clause 6.2.1). This field is absent in the IE *CellGroupConfig* when provided as part of *RRCSetup* message. |
| ***lpwus-Config***Configuration for UE to use LP-WUS *[to control the PDCCH monitoring]* as specified in TS 38.321 [3] Clause xxxx. The network will not configure *lpwus-Config* and *dcp-Config* for a UE simultaneously. |
| ***mcs-C-RNTI***RNTI to indicate use of *qam64LowSE* for grant-based transmissions. When the *mcs*-*C-RNTI* is configured, RNTI scrambling of DCI CRC is used to choose the corresponding MCS table. |
| ***ncr-RNTI***RNTI value for NCR-MT, used to scramble the PDCCHs carrying side control information (see TS 38.213 [13], clause 10.1). |
| ***nfi-TotalDAI-Included***Indicates whether the NFI and total DAI fields of the non-scheduled PDSCH group is included in the non-fallback DL grant DCI (see TS 38.212 [17], clause 7.3.1). The network configures this only when enhanced dynamic codebook is configured (*pdsch-HARQ-ACK-Codebook* is set to *enhancedDynamic*). |
| ***nrdc-PCmode-FR1***Indicates the uplink power sharing mode that the UE uses in NR-DC in frequency range 1 (FR1) (see TS 38.213 [13], clause 7.6). |
| ***nrdc-PCmode-FR2***Indicates the uplink power sharing mode that the UE uses in NR-DC in frequency range 2 (FR2) (see TS 38.213 [13], clause 7.6). |
| ***pdcch-BlindDetection, pdcch-BlindDetection2, pdcch-BlindDetection3, pdcch-BlindDetection4***Indicates the reference number of cells for PDCCH blind detection for the CG. Network configures the field for each CG when the UE is in NR DC and sets the value in accordance with the constraints specified in TS 38.213 [13]. The network configures *pdcch-BlindDetection* only if the UE is in NR-DC. The network configures *pdcch-BlindDetection2* only if the UE is in NR-DC with at least one downlink cell using Rel-16 PDCCH monitoring capability. The network configures *pdcch-BlindDetection3* only if the UE is in NR-DC with at least one downlink cell using Rel-15 PDCCH monitoring capability. The network configures *pdcch-BlindDetection4* only if the UE is in NR-DC with at least one downlink cell using Rel-17 PDCCH monitoring capability. |
| ***pdcch-BlindDetectionCA-CombIndicator***Configure one combination of *pdcch-BlindDetectionCA1* (for R15) and *pdcch-BlindDetectionCA2* (for R16) for UE to use for scaling PDCCH monitoring capability if the number of serving cells configured to a UE is larger than the reported capability, and if UE reports more than one combination of *pdcch-BlindDetectionCA1* and *pdcch-BlindDetectionCA2* as UE capability. The combination of *pdcch-BlindDetectionCA1* and *pdcch-BlindDetectionCA2* configured by *pdcch-BlindDetectionCA-CombIndicator* is from the more than one combination of *pdcch-BlindDetectionCA1* and *pdcch-BlindDetectionCA2* reported by UE (see TS 38.213 [13], clause 10).*pdcch-BlindDetectionCA-CombIndicator-r17* is used to configure one combination of *pdcch-BlindDetectionCA1* (for R15), *pdcch-BlindDetectionCA2* (for R16) and *pdcch-BlindDetectionCA3* (for R17) for UE to use for scaling PDCCH monitoring capability if the number of serving cells configured to a UE is larger than the reported capability, and if UE reports more than one combination of *pdcch-BlindDetectionCA1*, *pdcch-BlindDetectionCA2* and *pdcch-BlindDetectionCA3* as UE capability. The combination of *pdcch-BlindDetectionCA1*, *pdcch-BlindDetectionCA2* and *pdcch-BlindDetectionCA3* configured by *pdcch-BlindDetectionCA-CombIndicator-r17* is from the more than one combination of *pdcch-BlindDetectionCA1*, *pdcch-BlindDetectionCA2* and *pdcch-BlindDetectionCA3* reported by UE (see TS 38.213 [13], clause 10).*pdcch-BlindDetectionCA-CombIndicator-r16* and *pdcch-BlindDetectionCA-CombIndicator-r17* are not configured simultaneously. |
| ***p-NR-FR1***The maximum total transmit power to be used by the UE in this NR cell group across all serving cells in frequency range 1 (FR1). The maximum transmit power that the UE may use may be additionally limited by *p-Max* (configured in *FrequencyInfoUL*) and by *p-UE-FR1* (configured total for all serving cells operating on FR1). |
| ***p-NR-FR2***The maximum total transmit power to be used by the UE in this NR cell group across all serving cells in frequency range 2 (FR2). The maximum transmit power that the UE may use may be additionally limited by *p-Max* (configured in *FrequencyInfoUL*) and by *p-UE-FR2* (configured total for all serving cells operating on FR2). This field is only used in NR-DC. A UE does not expect to be configured with this parameter in this release of the specification. |
| ***prioLowDG-HighCG***Enable PHY prioritization for the case where low-priority dynamic grant-PUSCH collides with high-priority configured grant-PUSCH on a BWP of a serving cell (see TS 38.213 [13], clause 9), when the UE has generated transport blocks for both DG-PUSCH and CG-PUSCH as described in TS 38.321 [3]. |
| ***prioHighDG-LowCG***Enable PHY prioritization for the case where high-priority dynamic grant PUSCH collides with low-priority configured grant PUSCH on a BWP of a serving cell (see TS 38.213 [13], clause 9), when the UE has generated transport blocks for both DG-PUSCH and CG-PUSCH as described in TS 38.321 [3]. |
| ***ps-RNTI***RNTI value for scrambling CRC of DCI format 2-6 used for power saving (see TS 38.213 [13], clause 10.1). |
| ***ps-Offset***The start of the search-time of DCI format 2-6 with CRC scrambled by PS-RNTI relative to the start of the *drx-onDurationTimer* of Long DRX (see TS 38.213 [13], clause 10.3). Value in multiples of 0.125ms (milliseconds). 1 corresponds to 0.125 ms, 2corresponds to 0.25 ms, 3 corresponds to 0.375 ms and so on. |
| ***ps-WakeUp***Indicates the UE to wake-up if DCI format 2-6 is not detected outside active time (see TS 38.321 [3], clause 5.7). If the field is absent, the UE does not wake-up if DCI format 2-6 is not detected outside active time. |
| ***ps-PositionDCI-2-6***Starting position of UE wakeup and SCell dormancy indication in DCI format 2-6 (see TS 38.213 [13], clause 10.3). |
| ***ps-TransmitPeriodicL1-RSRP***Indicates the UE to transmit periodic L1-RSRP report(s) when the *drx-onDurationTimer* does not start (see TS 38.321 [3], clause 5.7). If the field is absent, the UE does not transmit periodic L1-RSRP report(s) when the *drx-onDurationTimer* does not start. |
| ***ps-TransmitOtherPeriodicCSI***Indicates the UE to transmit periodic CSI report(s) other than L1-RSRP reports when the *drx-onDurationTimer* does not start (see TS 38.321 [3], clause 5.7). If the field is absent, the UE does not transmit periodic CSI report(s) other than L1-RSRP reports when the *drx-onDurationTimer* does not start. |
| ***p-UE-FR1***The maximum total transmit power to be used by the UE across all serving cells in frequency range 1 (FR1) across all cell groups. The maximum transmit power that the UE may use may be additionally limited by *p-Max* (configured in *FrequencyInfoUL*) and by *p-NR-FR1* (configured for the cell group). |
| ***p-UE-FR2***The maximum total transmit power to be used by the UE across all serving cells in frequency range 2 (FR2) across all cell groups. The maximum transmit power that the UE may use may be additionally limited by *p-Max* (configured in *FrequencyInfoUL*) and by p-NR-FR2 (configured for the cell group). A UE does not expect to be configured with this parameter in this release of the specification. |
| ***pdsch-HARQ-ACK-Codebook***The PDSCH HARQ-ACK codebook is either semi-static or dynamic. This is applicable to both CA and non-CA operation (see TS 38.213 [13], clauses 9.1.2 and 9.1.3). If *pdsch-HARQ-ACK-Codebook-r16* is signalled, UE shall ignore the *pdsch-HARQ-ACK-Codebook* (without suffix). For the HARQ-ACK for sidelink, if *pdsch-HARQ-ACK-Codebook-r16* is signalled, the UE uses *pdsch-HARQ-ACK-Codebook* (without suffix) and ignores *pdsch-HARQ-ACK-Codebook-r16*. If the field *pdsch-HARQ-ACK-Codebook-secondaryPUCCHgroup* is present, *pdsch-HARQ-ACK-Codebook* is applied to primary PUCCH group. Otherwise, this field is applied to the cell group (i.e. for all the cells within the cell group). For the HARQ-ACK for sidelink, if the field *pdsch-HARQ-ACK-Codebook-secondaryPUCCHgroup* is present, *pdsch-HARQ-ACK-Codebook* is applied to primary and secondary PUCCH group and the UE ignores *pdsch-HARQ-ACK-Codebook-secondaryPUCCHgroup*. |
| ***pdsch-HARQ-ACK-CodebookList***A list of configurations for one or two HARQ-ACK codebooks. Each configuration in the list is defined in the same way as *pdsch-HARQ-ACK-Codebook* (see TS 38.212 [17], clause 7.3.1.2.2 and TS 38.213 [13], clauses 7.2.1, 9.1.2, 9.1.3 and 9.2.1). If this field is present, the field *pdsch-HARQ-ACK-Codebook* is ignored. If this field is present, the value of this field is applied for primary PUCCH group and for secondary PUCCH group (if configured). For the HARQ-ACK for sidelink, the UE uses *pdsch-HARQ-ACK-Codebook* and ignores *pdsch-HARQ-ACK-CodebookList* if this field is present. |
| ***pdsch-HARQ-ACK-Codebook-secondaryPUCCHgroup***The PDSCH HARQ-ACK codebook is either semi-static or dynamic. This is applicable to CA operation (see TS 38.213 [13], clauses 9.1.2 and 9.1.3). It is configured for secondary PUCCH group*.* |
| ***pdsch-HARQ-ACK-EnhType3DCI-Field, pdsch-HARQ-ACK-EnhType3DCI-FieldSecondaryPUCCHgroup***Indicates the enhanced Type 3 codebook through a new DCI field to indicate the enhanced Type 3 HARQ-ACK codebook in the primary PUCCH group if the more than one enhanced Type 3 HARQ-ACK codebook is configured for the primary PUCCH group, or in the secondary PUCCH group if the more than one enhanced Type 3 HARQ-ACK code is configured for the secondary PUCCH group, respectively. |
| ***pdsch-HARQ-ACK-EnhType3ToAddModList, pdsch-HARQ-ACK-EnhType3SecondaryToAddModList***Configure the list of enhanced Type 3 HARQ-ACK codebooks for the primary PUCCH group and the secondary PUCCH group, respectively. When configured, DCI format 1\_1 can request the UE to report A/N for one of the configured enhanced Type 3 HARQ-ACK codebooks in the corresponding PUCCH group (see TS 38.213 [13], clause 9.1.4). The network can configure *pdsch-HARQ-ACK-EnhType3SecondaryToAddModList* only if secondary PUCCH group is configured. |
| ***pdsch-HARQ-ACK-OneShotFeedback***When configured, the DCI format 1\_1 can request the UE to report A/N for all HARQ processes and all CCs configured in the PUCCH group (see TS 38.212 [17], clause 7.3.1). |
| ***pdsch-HARQ-ACK-OneShotFeedbackCBG***When configured, the DCI format 1\_1 can request the UE to include CBG level A/N for each CC with CBG level transmission configured. When not configured, the UE will report TB level A/N even if CBG level transmission is configured for a CC.The network configures this only when *pdsch-HARQ-ACK-OneShotFeedback* is configured. |
| ***pdsch-HARQ-ACK-OneShotFeedbackNDI***When configured, the DCI format 1\_1 can request the UE to include NDI for each A/N reported.The network configures this only when *pdsch-HARQ-ACK-OneShotFeedback* is configured. |
| ***pdsch-HARQ-ACK-Retx, pdsch-HARQ-ACK-RetxSecondaryPUCCHgroup***When configured, the DCI format 1\_1 can request the UE to perform a HARQ-ACK re-transmission on a PUCCH resource in the primary PUCCH group and the secondary PUCCH group, respectively (see TS 38.213 [13], clause 9.1.5). |
| ***pucch-sSCell, pucch-sSCellSecondaryPUCCHgroup***indictates the alternative PUCCH cells for PUCCH cell switching in the primary and the secondary PUCCH group, respectively. For the primary PUCCH group, it is configured for cells on top of SpCell. For the secondary PUCCH group, it is configured for cell on top of the PUCCH SCell. |
| ***pucch-sSCellDyn, pucch-sSCellDynsecondaryPUCCHgroup***When configured, PUCCH cell switching based on dynamic indication in DCI format 1\_1 is enabled (see TS 38.213 [13], clause 9.A, clause 9.1.5), respectively for the primary PUCCH group and the secondary PUCCH group. |
| ***pucch-sSCellPattern, pucch-sSCellPatternSecondaryPUCCHgroup***When configured, the UE applies the semi-static PUCCH cell switching (see TS 38.213 [13], clause 9.A) using the time domain pattern of applicable PUCCH cells indicated by this field, respectively for the primary PUCCH group and the secondary PUCCH group. |
| ***simultaneousPUCCH-PUSCH, simultaneousPUCCH-PUSCH-SecondaryPUCCHgroup***Enables simultaneous PUCCH and PUSCH transmissions with different priorities for the primary PUCCH group and the secondary PUCCH group, respectively. |
| ***simultaneousPUCCH-PUSCH-SamePriority, simultaneousPUCCH-PUSCH-SamePriority-SecondaryPUCCHgroup***Enables simultaneous PUCCH and PUSCH transmissions on different cells in different bands with same prioritiy for the primary PUCCH group and the secondary PUCCH group, respectively, as specified in clause 9 of TS 38.213 [13]. |
| ***simultaneousSR-PUSCH-diffPUCCH-Groups***Enables simultaneous SR and PUSCH transmissions in different PUCCH groups (see TS 38.321 [3], clause 5.4.1, clause 5.4.4). |
| ***sizeDCI-2-6***Size of DCI format 2-6 (see TS 38.213 [13], clause 10.3). |
| ***sp-CSI-RNTI***RNTI for Semi-Persistent CSI reporting on PUSCH (see *CSI-ReportConfig*) (see TS 38.214 [19], clause 5.2.1.5.2). Network always configures the UE with a value for this field when at least one *CSI-ReportConfig* with *reportConfigType* set to *semiPersistentOnPUSCH* is configured. |
| ***tpc-PUCCH-RNTI***RNTI used for PUCCH TPC commands on DCI (see TS 38.213 [13], clause 10.1). |
| ***tpc-PUSCH-RNTI***RNTI used for PUSCH TPC commands on DCI (see TS 38.213 [13], clause 10.1). |
| ***tpc-SRS-RNTI***RNTI used for SRS TPC commands on DCI (see TS 38.213 [13], clause 10.1). |
| ***twoQCL-TypeD-ForMultiDCI***Indicates whether a UE is expected to identify and monitor two QCL-TypeD properties for multiple overlapping CORESETs, where the first QCL-TypeD is associated with *coresetPoolIndex* value 0, and the second QCL-TypeD is associated with *coresetPoolIndex* value 1. (See TS 38,213 [13], clause 10). |
| ***twoQCLTypeDforPDCCHRepetition***Indicates whether a UE is expected UE to identify and monitor two QCL-TypeD properties for multiple overlapping CORESETs in the case of PDCCH repetition. |
| ***uci-MuxWithDiffPrio, uci-MuxWithDiffPrio-secondaryPUCCHgroup***When configured, enables multiplexing a high-priority (HP) HARQ-ACK UCI and a low-priority (LP) HARQ-ACK UCI into a PUCCH or PUSCH for the primary PUCCH group and the secondary PUCCH group, respectively. |
| ***ul-TotalDAI-Included***Indicates whether the total DAI fields of the additional PDSCH group is included in the non-fallback UL grant DCI (see TS 38.212 [17], clause 7.3.1). The network configures this only when enhanced dynamic codebook is configured (*pdsch-HARQ-ACK-Codebook* is set to *enhancedDynamic*). |
| ***xScale***The UE is allowed to drop NR only if the power scaling applied to NR results in a difference between scaled and unscaled NR UL of more than *xScale* dB (see TS 38.213 [13]). If the value is not configured for dynamic power sharing, the UE assumes default value of 6 dB. |

|  |
| --- |
| *MulticastConfig* field descriptions |
| ***pdsch-HARQ-ACK-CodebookListMulticast***A list of configurations for one or two HARQ-ACK codebooks for MBS multicast. Each configuration in the list is defined in the same way as *pdsch-HARQ-ACK-Codebook* (see TS 38.212 [17], clause 7.3.1.2.2 and TS 38.213 [13], clauses 7.2.1, 9.1.2, 9.1.3 and 9.2.1). If this field is present, the field *pdsch-HARQ-ACK-Codebook* is ignored. If this field is present, the value of this field is applied for primary PUCCH group and for secondary PUCCH group (if configured). |
| ***type1CodebookGenerationMode***Indicates the mode of Type-1 HARQ-ACK codebook generation, as specified in TS 38.213 [13]. Mode 1 is based on the k1 values that are in the intersection of K1 set for unicast and K1 set for multicast. Mode 2 is based on the k1 values that are in the union of K1 set for unicast and K1 set for multicast. |

|  |
| --- |
| *PDSCH-HARQ-ACK-EnhType3* field descriptions |
| ***pdsch-HARQ-ACK-EnhType3CBG***When configured, the DCI format 1\_1 or DCI format 1\_2 can request the UE to include CBG level A/N for each CC with CBG level transmission configured of the enhanced Type 3 HARQ-ACK codebook. When not configured, the UE will report TB level A/N even if CBG level transmission is configured for a CC. |
| ***pdsch-HARQ-ACK-EnhType3NDI***When configured, the DCI format 1\_1 or DCI format 1\_2 can request the UE to include NDI for each A/N reported of the enhanced Type 3 HARQ-ACK codebook. |
| ***perCC***Configures enhanced Type 3 HARQ-ACK codebook using per CC configuration. |
| ***perHARQ, perHARQ-Ext***Configures enhanced Type 3 HARQ-ACK codebook using per HARQ process and CC configuration. *perHARQ-Ext* is present only when *nrofHARQ-ProcessesForPDSCH-v1700* is present in *pdsch-ServingCellConfig* of at least one serving cell in the PUCCH group. If *perHARQ-Ext* is present, the UE ignores *perHARQ*. |

|  |
| --- |
| *CellDTRX-DCI-config* field descriptions |
| ***cellDTRX-RNTI***The RNTI value for scrambling CRC of DCI format 2\_9 for activating and/or deactivating Cell DTX and/or Cell DRX and/or NES mode for CHO indication. |
| ***sizeDCI-2-9***The size of DCI format 2\_9. |

|  |
| --- |
| *lpwus-config* field descriptions |
| ***lpwus-Codepoint***Indicates the codepoint(s) that UE monitors for LP-WUS (see TS 38.213 [13], clause xxx). |
| ***lpwus-PDCCHMonitoringTimer***Indicates the length of the timer for UE to monitor PDCCH after LP-WUS is detected (see TS 38.321 [3], clause xxx). |
| ***lpwus-MvalueFR1***Indicates the number of OOK symbols in an OFDM symbol for LP-WUS in FR1. |
| ***lpwus-MvalueFR2***Indicates the number of OOK symbols in an OFDM symbol for LP-WUS in FR2. |
| ***lpwus-Offset11***Indicates the start of LP-WUS monitoring relative to the start of the *drx-onDurationTimer* [of Long DRX] (see TS 38.213 [13], clause xxx). [TBD Value in multiples of 0.125ms (milliseconds). 1 corresponds to 0.125 ms, 2corresponds to 0.25 ms, 3 corresponds to 0.375 ms and so on.] The network will not configure *lpwus-Offset11* and *lpwus-Offset12* for a UE simultaneously. |
| ***lpwus-Offset12***Indicates the start of UE PDCCH monitoring after LP-WUS is detected (see TS 38.213 [13], clause xxx). [TBD Value in multiples of 0.125ms (milliseconds). 1 corresponds to 0.125 ms, 2corresponds to 0.25 ms, 3 corresponds to 0.375 ms and so on.] The network will not configure *lpwus-Offset11* and *lpwus-Offset12* for a UE simultaneously. |
| ***lpwus-OverlaidSeq***Indicates the configuration of overlaid OFDM sequence used per OOK symbol for LP-WUS (see TS 38.321 [3], clause xxx). |
| ***lpwus-StartRB***The starting RB of LP-WUS (see TS 38.213 [13], clause xxxx).  |
| ***lpwus-WakeUp11***Indicates the UE to wake-up if LP-WUS is not detected (see TS 38.321 [3], clause xxx). If the field is absent, the UE does not wake-up if LP-WUS is not detected. The network will not configure *lpwus-WakeUp11 and lpwus-Offset12* for a UE simultaneously. |
| ***lpwus-TransmitPeriodicL1-RSRP***Indicates the UE to transmit periodic L1-RSRP report(s) during the time given by the configured *drx-onDurationTimer* if the UE is not indicated to wake-up (see TS 38.321 [3], clause xxx). If the field is absent, the UE does not transmit periodic L1-RSRP report(s) during the time given by the configured *drx-onDurationTimer* if the UE is not indicated to wake-up. |
| ***lpwus-TransmitOtherPeriodicCSI***Indicates the UE to transmit periodic CSI report(s) other than L1-RSRP reports during the time given by the configured *drx-onDurationTimer* if the UE is not indicated to wake-up (see TS 38.321 [3], clause xx). If the field is absent, the UE does not transmit periodic CSI report(s) other than L1-RSRP reports during the time given by the configured *drx-onDurationTimer* if the UE is not indicated to wake-up. |

|  |  |
| --- | --- |
| Conditional Presence | Explanation |
| *MCG-Only* | This field is optionally present, Need R, in the *PhysicalCellGroupConfig* of the MCG. It is absent otherwise.  |
| *NCR* | This field is optionally present, Need M for NCR-MT. It is absent otherwise. |
| *SCG-Only* | This field is optionally present, Need S, in the *PhysicalCellGroupConfig* of the SCG in (NG)EN-DC as defined in TS 38.213 [13]. It is absent otherwise. |
| *twoPUCCHgroup* | This field is optionally present, Need R, if secondary PUCCH group is configured. It is absent otherwise, Need R.  |
| *FR1-Only* | This field is mandatory present for an FR1 carrier frequency. It is absent otherwise and UE releases any configured value. |
| *FR2-Only* | This field is mandatory present for an FR2 carrier frequency. It is absent otherwise and UE releases any configured value. |
| *TBD\_Offset12* | This field is mandatory present if Offset12 is configured. It is absent otherwise and UE releases any configured value. |

Next change

## 6.4 RRC multiplicity and type constraint values

### – Multiplicity and type constraint definitions

-- ASN1START

-- TAG-MULTIPLICITY-AND-TYPE-CONSTRAINT-DEFINITIONS-START

maxAdditionalRACH-r17 INTEGER ::= 256 -- Maximum number of additional RACH configurations.

maxAI-DCI-PayloadSize-r16 INTEGER ::= 128 --Maximum size of the DCI payload scrambled with ai-RNTI

maxAI-DCI-PayloadSize-1-r16 INTEGER ::= 127 --Maximum size of the DCI payload scrambled with ai-RNTI minus 1

maxBandComb INTEGER ::= 65536 -- Maximum number of DL band combinations

maxBandComb-MUSIM-r18 INTEGER ::= 64 -- Maximum number of MUSIM bands and/or band combinations

maxBandsUTRA-FDD-r16 INTEGER ::= 64 -- Maximum number of bands listed in UTRA-FDD UE caps

maxCandidateBandIndex-r18 INTEGER ::= 8 -- Maximum number of band entry index for MUSIM capability

maxBH-RLC-ChannelID-r16 INTEGER ::= 65536 -- Maximum value of BH RLC Channel ID

maxBT-IdReport-r16 INTEGER ::= 32 -- Maximum number of Bluetooth IDs to report

maxBT-Name-r16 INTEGER ::= 4 -- Maximum number of Bluetooth name

maxCAG-Cell-r16 INTEGER ::= 16 -- Maximum number of NR CAG cell ranges in SIB3, SIB4

maxTwoPUCCH-Grp-ConfigList-r16 INTEGER ::= 32 -- Maximum number of supported configuration(s) of {primary PUCCH group

 -- config, secondary PUCCH group config}

maxTwoPUCCH-Grp-ConfigList-r17 INTEGER ::= 16 -- Maximum number of supported configuration(s) of {primary PUCCH group

 -- config, secondary PUCCH group config} for PUCCH cell switching

maxCBR-Config-r16 INTEGER ::= 8 -- Maximum number of CBR range configurations for sidelink communication

 -- congestion control

maxCBR-Config-1-r16 INTEGER ::= 7 -- Maximum number of CBR range configurations for sidelink communication

 -- congestion control minus 1

maxCBR-Level-r16 INTEGER ::= 16 -- Maximum number of CBR levels

maxCBR-Level-1-r16 INTEGER ::= 15 -- Maximum number of CBR levels minus 1

maxCellATG-r18 INTEGER ::= 8 -- Maximum number of ATG neighbour cells for which assistance information is

 -- provided

maxCellExcluded INTEGER ::= 16 -- Maximum number of NR exclude-listed cell ranges in SIB3, SIB4

maxCellGroupings-r16 INTEGER ::= 32 -- Maximum number of cell groupings for NR-DC

maxCellHistory-r16 INTEGER ::= 16 -- Maximum number of visited PCells reported

maxPSCellHistory-r17 INTEGER ::= 16 -- Maximum number of visited PSCells across all reported PCells

maxCellInter INTEGER ::= 16 -- Maximum number of inter-Freq cells listed in SIB4

maxCellIntra INTEGER ::= 16 -- Maximum number of intra-Freq cells listed in SIB3

maxCellMeasEUTRA INTEGER ::= 32 -- Maximum number of cells in E-UTRAN

maxCellMeasIdle-r16 INTEGER ::= 8 -- Maximum number of cells per carrier for idle/inactive measurements

maxCellMeasUTRA-FDD-r16 INTEGER ::= 32 -- Maximum number of cells in FDD UTRAN

maxCellNTN-r17 INTEGER ::= 4 -- Maximum number of NTN neighbour cells for which assistance information is

 -- provided

maxCarrierTypePairList-r16 INTEGER ::= 16 -- Maximum number of supported carrier type pair of (carrier type on which

 -- CSI measurement is performed, carrier type on which CSI reporting is

 -- performed) for CSI reporting cross PUCCH group

maxCellAllowed INTEGER ::= 16 -- Maximum number of NR allow-listed cell ranges in SIB3, SIB4

maxEARFCN INTEGER ::= 262143 -- Maximum value of E-UTRA carrier frequency

maxEUTRA-CellExcluded INTEGER ::= 16 -- Maximum number of E-UTRA exclude-listed physical cell identity ranges

 -- in SIB5

maxEUTRA-NS-Pmax INTEGER ::= 8 -- Maximum number of NS and P-Max values per band

maxFeatureCombPreamblesPerRACHResource-r17 INTEGER ::= 256 -- Maximum number of feature combination preambles.

maxLogMeasReport-r16 INTEGER ::= 520 -- Maximum number of entries for logged measurements

maxMultiBands INTEGER ::= 8 -- Maximum number of additional frequency bands that a cell belongs to

maxNARFCN INTEGER ::= 3279165 -- Maximum value of NR carrier frequency

maxNR-NS-Pmax INTEGER ::= 8 -- Maximum number of NS and P-Max values per band

maxFreqIdle-r16 INTEGER ::= 8 -- Maximum number of carrier frequencies for idle/inactive measurements

maxNrofServingCells INTEGER ::= 32 -- Max number of serving cells (SpCells + SCells)

maxNrofServingCells-1 INTEGER ::= 31 -- Max number of serving cells (SpCells + SCells) minus 1

maxNrofAggregatedCellsPerCellGroup INTEGER ::= 16

maxNrofAggregatedCellsPerCellGroupMinus4-r16 INTEGER ::= 12

maxNrofAperiodicFwdTimeResource-r18 INTEGER ::= 112 -- Max number of aperiodic fowarding time resources for NCR

maxNrofAperiodicFwdTimeResource-1-r18 INTEGER ::= 111 -- Max number of aperiodic fowarding time resources for NCR minus 1

maxNrofDUCells-r16 INTEGER ::= 512 -- Max number of cells configured on the collocated IAB-DU

maxNrofAppLayerMeas-r17 INTEGER ::= 16 -- Max number of simultaneous application layer measurements

maxNrofAppLayerMeas-1-r17 INTEGER ::= 15 -- Max number of simultaneous application layer measurements minus 1

maxNrofAppLayerReports-r18 INTEGER ::= 16 -- Max number of application layer measurement reports with the same

 -- measConfigAppLayerId included in the same

 -- MeasurementReportAppLayerMessage

maxNrofAvailabilityCombinationsPerSet-r16 INTEGER ::= 512 -- Max number of AvailabilityCombinationId used in the DCI format 2\_5

maxNrofAvailabilityCombinationsPerSet-1-r16 INTEGER ::= 511 -- Max number of AvailabilityCombinationId used in the DCI format 2\_5 minus 1

maxNrofIABResourceConfig-r17 INTEGER ::= 65536 -- Max number of IAB-ResourceConfigID used in MAC CE

maxNrofIABResourceConfig-1-r17 INTEGER ::= 65535 -- Max number of IAB-ResourceConfigID used in MAC CE minus 1

maxNrofPeriodicFwdResourceSet-r18 INTEGER ::= 32 -- Max number of periodic fowarding resource sets for NCR

maxNrofPeriodicFwdResourceSet-1-r18 INTEGER ::= 31 -- Max number of periodic fowarding resource sets for NCR minus 1

maxNrofPeriodicFwdResource-r18 INTEGER ::= 1024 -- Max number of periodic fowarding resources for NCR

maxNrofPeriodicFwdResource-1-r18 INTEGER ::= 1023 -- Max number of periodic fowarding resources for NCR minus 1

maxNrofSemiPersistentFwdResourceSet-r18 INTEGER ::= 32 -- Max number of semi-persistent fowarding resource sets for NCR

maxNrofSemiPersistentFwdResourceSet-1-r18 INTEGER ::= 31 -- Max number of semi-persistent fowarding resource sets for NCR minus 1

maxNrofSemiPersistentFwdResource-r18 INTEGER ::= 128 -- Max number of semi-persistent fowarding resources for NCR

maxNrofSemiPersistentFwdResource-1-r18 INTEGER ::= 127 -- Max number of semi-persistent fowarding resources for NCR minus 1

maxNrofSCellActRS-r17 INTEGER ::= 255 -- Max number of RS configurations per SCell for SCell activation

maxNrofSCells INTEGER ::= 31 -- Max number of secondary serving cells per cell group

maxNrofCellMeas INTEGER ::= 32 -- Maximum number of entries in each of the cell lists in a measurement object

maxNrofCRS-IM-InterfCell-r17 INTEGER ::= 8 -- Maximum number of LTE interference cells for CRS-IM per UE

maxNrofRelayMeas-r17 INTEGER ::= 32 -- Maximum number of L2 U2N Relay UEs to measure for each measurement object

 -- on sidelink frequency

maxNrofCG-SL-r16 INTEGER ::= 8 -- Max number of sidelink configured grant

maxNrofCG-SL-1-r16 INTEGER ::= 7 -- Max number of sidelink configured grant minus 1

maxSL-GC-BC-DRX-QoS-r17 INTEGER ::= 16 -- Max number of sidelink DRX configurations for NR

 -- sidelink groupcast/broadcast communication

maxNrofSL-RxInfoSet-r17 INTEGER ::= 4 -- Max number of sidelink DRX configuration sets in sidelink DRX assistant

 -- information

maxNrofSS-BlocksToAverage INTEGER ::= 16 -- Max number for the (max) number of SS blocks to average to determine cell measurement

maxNrofCondCells-r16 INTEGER ::= 8 -- Max number of conditional candidate SpCells

maxNrofCondCells-1-r17 INTEGER ::= 7 -- Max number of conditional candidate SpCells minus 1

maxNrofCSI-RS-ResourcesToAverage INTEGER ::= 16 -- Max number for the (max) number of CSI-RS to average to determine cell measurement

maxNrofDL-Allocations INTEGER ::= 16 -- Maximum number of PDSCH time domain resource allocations

maxNrofDL-AllocationsExt-r17 INTEGER ::= 64 -- Maximum number of PDSCH time domain resource allocations for multi-PDSCH

 -- scheduling

maxNrofDL-Allocations-1-r18 INTEGER ::= 15 -- Maximum number of PDSCH time domain resource allocations minus 1

maxNrofPDU-Sessions-r17 INTEGER ::= 256 -- Maximum number of PDU Sessions

maxNrofSR-ConfigPerCellGroup INTEGER ::= 8 -- Maximum number of SR configurations per cell group

maxNrofLCGs-r18 INTEGER ::= 8 -- Maximum number of LCGs

maxLCG-ID INTEGER ::= 7 -- Maximum value of LCG ID

maxLCG-ID-IAB-r17 INTEGER ::= 255 -- Maximum value of LCG ID for IAB-MT

maxLC-ID INTEGER ::= 32 -- Maximum value of Logical Channel ID

maxLC-ID-Iab-r16 INTEGER ::= 65855 -- Maximum value of BH Logical Channel ID extension

maxLTE-CRS-Patterns-r16 INTEGER ::= 3 -- Maximum number of additional LTE CRS rate matching patterns

maxNrOfLinkedSRS-CarriersInactive-1-r18 INTEGER ::= 2 -- Maximum number of carriers for positioning SRS CA in RRC\_INACTIVE minus 1

maxNrofTAGs INTEGER ::= 4 -- Maximum number of Timing Advance Groups

maxNrofTAGs-1 INTEGER ::= 3 -- Maximum number of Timing Advance Groups minus 1

maxNrofBWPs INTEGER ::= 4 -- Maximum number of BWPs per serving cell

maxNrofCombIDC INTEGER ::= 128 -- Maximum number of reported MR-DC combinations for IDC

maxNrofSymbols-1 INTEGER ::= 13 -- Maximum index identifying a symbol within a slot (14 symbols, indexed from 0..13)

maxNrofSlots INTEGER ::= 320 -- Maximum number of slots in a 10 ms period

maxNrofSlots-1 INTEGER ::= 319 -- Maximum number of slots in a 10 ms period minus 1

maxNrofPhysicalResourceBlocks INTEGER ::= 275 -- Maximum number of PRBs

maxNrofPhysicalResourceBlocks-1 INTEGER ::= 274 -- Maximum number of PRBs minus 1

maxNrofPhysicalResourceBlocksPlus1 INTEGER ::= 276 -- Maximum number of PRBs plus 1

maxNrofControlResourceSets INTEGER ::= 12 -- Max number of CoReSets configurable on a serving cell

maxNrofControlResourceSets-1 INTEGER ::= 11 -- Max number of CoReSets configurable on a serving cell minus 1

maxNrofControlResourceSets-1-r16 INTEGER ::= 15 -- Max number of CoReSets configurable on a serving cell extended in minus 1

maxNrofCoresetPools-r16 INTEGER ::= 2 -- Maximum number of CORESET pools

maxCoReSetDuration INTEGER ::= 3 -- Max number of OFDM symbols in a control resource set

maxNrofSearchSpaces-1 INTEGER ::= 39 -- Max number of Search Spaces minus 1

maxNrofSearchSpacesLinks-1-r17 INTEGER ::= 39 -- Max number of Search Space links minus 1

maxNrofBFDResourcePerSet-r17 INTEGER ::= 64 -- Max number of reference signal in one BFD set

maxSFI-DCI-PayloadSize INTEGER ::= 128 -- Max number payload of a DCI scrambled with SFI-RNTI

maxSFI-DCI-PayloadSize-1 INTEGER ::= 127 -- Max number payload of a DCI scrambled with SFI-RNTI minus 1

maxIAB-IP-Address-r16 INTEGER ::= 32 -- Max number of assigned IP addresses

maxINT-DCI-PayloadSize INTEGER ::= 126 -- Max number payload of a DCI scrambled with INT-RNTI

maxINT-DCI-PayloadSize-1 INTEGER ::= 125 -- Max number payload of a DCI scrambled with INT-RNTI minus 1

maxNrofRateMatchPatterns INTEGER ::= 4 -- Max number of rate matching patterns that may be configured

maxNrofRateMatchPatterns-1 INTEGER ::= 3 -- Max number of rate matching patterns that may be configured minus 1

maxNrofRateMatchPatternsPerGroup INTEGER ::= 8 -- Max number of rate matching patterns that may be configured in one group

maxNrofCSI-ReportConfigurations INTEGER ::= 48 -- Maximum number of report configurations

maxNrofCSI-ReportConfigurations-1 INTEGER ::= 47 -- Maximum number of report configurations minus 1

maxNrofCSI-ResourceConfigurations INTEGER ::= 112 -- Maximum number of resource configurations

maxNrofCSI-ResourceConfigurations-1 INTEGER ::= 111 -- Maximum number of resource configurations minus 1

maxNrofAP-CSI-RS-ResourcesPerSet INTEGER ::= 16

maxNrOfCSI-AperiodicTriggers INTEGER ::= 128 -- Maximum number of triggers for aperiodic CSI reporting

maxNrofReportConfigPerAperiodicTrigger INTEGER ::= 16 -- Maximum number of report configurations per trigger state for aperiodic reporting

maxNrofNZP-CSI-RS-Resources INTEGER ::= 192 -- Maximum number of Non-Zero-Power (NZP) CSI-RS resources

maxNrofNZP-CSI-RS-Resources-1 INTEGER ::= 191 -- Maximum number of Non-Zero-Power (NZP) CSI-RS resources minus 1

maxNrofNZP-CSI-RS-ResourcesPerSet INTEGER ::= 64 -- Maximum number of NZP CSI-RS resources per resource set

maxNrofNZP-CSI-RS-ResourcesPerSet-1-r18 INTEGER ::= 63 -- Maximum number of NZP CSI-RS resources per resource set minus 1

maxNrofNZP-CSI-RS-ResourceSets INTEGER ::= 64 -- Maximum number of NZP CSI-RS resource sets per cell

maxNrofNZP-CSI-RS-ResourceSets-1 INTEGER ::= 63 -- Maximum number of NZP CSI-RS resource sets per cell minus 1

maxNrofNZP-CSI-RS-ResourceSetsPerConfig INTEGER ::= 16 -- Maximum number of resource sets per resource configuration

maxNrofNZP-CSI-RS-ResourcesPerConfig INTEGER ::= 128 -- Maximum number of resources per resource configuration

maxNrofZP-CSI-RS-Resources INTEGER ::= 32 -- Maximum number of Zero-Power (ZP) CSI-RS resources

maxNrofZP-CSI-RS-Resources-1 INTEGER ::= 31 -- Maximum number of Zero-Power (ZP) CSI-RS resources minus 1

maxNrofZP-CSI-RS-ResourceSets-1 INTEGER ::= 15

maxNrofZP-CSI-RS-ResourcesPerSet INTEGER ::= 16

maxNrofZP-CSI-RS-ResourceSets INTEGER ::= 16

maxNrofCSI-IM-Resources INTEGER ::= 32 -- Maximum number of CSI-IM resources

maxNrofCSI-IM-Resources-1 INTEGER ::= 31 -- Maximum number of CSI-IM resources minus 1

maxNrofCSI-IM-ResourcesPerSet INTEGER ::= 8 -- Maximum number of CSI-IM resources per set

maxNrofCSI-IM-ResourceSets INTEGER ::= 64 -- Maximum number of NZP CSI-IM resource sets per cell

maxNrofCSI-IM-ResourceSets-1 INTEGER ::= 63 -- Maximum number of NZP CSI-IM resource sets per cell minus 1

maxNrofCSI-IM-ResourceSetsPerConfig INTEGER ::= 16 -- Maximum number of CSI IM resource sets per resource configuration

maxNrofCSI-SSB-ResourcePerSet INTEGER ::= 64 -- Maximum number of SSB resources in a resource set

maxNrofCSI-SSB-ResourceSets INTEGER ::= 64 -- Maximum number of CSI SSB resource sets per cell

maxNrofCSI-SSB-ResourceSets-1 INTEGER ::= 63 -- Maximum number of CSI SSB resource sets per cell minus 1

maxNrofCSI-SSB-ResourceSetsPerConfig INTEGER ::= 1 -- Maximum number of CSI SSB resource sets per resource configuration

maxNrofCSI-SSB-ResourceSetsPerConfigExt INTEGER ::= 2 -- Maximum number of CSI SSB resource sets per resource configuration

 -- extended

maxNrofFailureDetectionResources INTEGER ::= 10 -- Maximum number of failure detection resources

maxNrofFailureDetectionResources-1 INTEGER ::= 9 -- Maximum number of failure detection resources minus 1

maxNrofFailureDetectionResources-1-r17 INTEGER ::= 63 -- Maximum number of the enhanced failure detection resources minus 1

maxNrofFreqSL-r16 INTEGER ::= 8 -- Maximum number of carrier frequency for NR sidelink communication

maxNrofFreqSL-1-r18 INTEGER ::= 7 -- Maximum number of carrier frequency for NR sidelink communication minus 1

maxNrofSL-BWPs-r16 INTEGER ::= 4 -- Maximum number of BWP for NR sidelink communication

maxNrofSL-CarrierSetConfig-r18 INTEGER ::= 96 -- Maximum number of SCCH carrier set configuration for NR sidelink

 -- communication

maxFreqSL-EUTRA-r16 INTEGER ::= 8 -- Maximum number of EUTRA anchor carrier frequency for NR sidelink

 -- communication

maxNrofSL-MeasId-r16 INTEGER ::= 64 -- Maximum number of sidelink measurement identity (RSRP) per destination

maxNrofSL-ObjectId-r16 INTEGER ::= 64 -- Maximum number of sidelink measurement objects (RSRP) per destination

maxNrofSL-ReportConfigId-r16 INTEGER ::= 64 -- Maximum number of sidelink measurement reporting configuration(RSRP) per destination

maxNrofSL-PoolToMeasureNR-r16 INTEGER ::= 8 -- Maximum number of resource pool for NR sidelink measurement to measure

 -- for each measurement object (for CBR)

maxNrofDedicatedSL-PRS-PoolToMeas-r18 INTEGER ::= 8 -- Maximum number of SL-PRS dedicated resource pool for positioning

 -- measurement to measure for each measurement object (for SL-PRS CBR)

maxFreqSL-NR-r16 INTEGER ::= 8 -- Maximum number of NR anchor carrier frequency for NR sidelink communication

maxNrofSL-QFIs-r16 INTEGER ::= 2048 -- Maximum number of QoS flow for NR sidelink communication per UE

maxNrofSL-QFIsPerDest-r16 INTEGER ::= 64 -- Maximum number of QoS flow per destination for NR sidelink communication

maxNrofObjectId INTEGER ::= 64 -- Maximum number of measurement objects

maxNrofPageRec INTEGER ::= 32 -- Maximum number of page records

maxNrofPCI-Ranges INTEGER ::= 8 -- Maximum number of PCI ranges

maxPLMN INTEGER ::= 12 -- Maximum number of PLMNs broadcast and reported by UE at establishment

maxTAC-r17 INTEGER ::= 12 -- Maximum number of Tracking Area Codes to which a cell belongs to

maxNrofCSI-RS-ResourcesRRM INTEGER ::= 96 -- Maximum number of CSI-RS resources per cell for an RRM measurement object

maxNrofCSI-RS-ResourcesRRM-1 INTEGER ::= 95 -- Maximum number of CSI-RS resources per cell for an RRM measurement object

 -- minus 1.

maxNrofMeasId INTEGER ::= 64 -- Maximum number of configured measurements

maxNrofQuantityConfig INTEGER ::= 2 -- Maximum number of quantity configurations

maxNrofCSI-RS-CellsRRM INTEGER ::= 96 -- Maximum number of cells with CSI-RS resources for an RRM measurement object

maxNrofSL-Dest-r16 INTEGER ::= 32 -- Maximum number of destination for NR sidelink communication and discovery

maxNrofSL-Dest-1-r16 INTEGER ::= 31 -- Highest index of destination for NR sidelink communication and discovery

maxNrofSL-PRS-PerDest-r18 INTEGER ::= 8 -- Max number of SL-PRS transmission supported per destination UE

maxNrofSLRB-r16 INTEGER ::= 512 -- Maximum number of radio bearer for NR sidelink communication per UE without duplication

maxSL-LCID-Plus1-r18 INTEGER ::= 513 -- Maximum number of RLC bearer for NR sidelink communication per UE without duplication plus 1

maxSL-LCID-r18 INTEGER ::= 1024 -- Maximum number of RLC bearer for NR sidelink communication per UE with duplication

maxSL-NonAnchorRBsets INTEGER ::= 4 -- Maximum number of non-anchor RB sets

maxSL-LCID-r16 INTEGER ::= 512 -- Maximum number of RLC bearer for NR sidelink communication per UE

maxSL-SyncConfig-r16 INTEGER ::= 16 -- Maximum number of sidelink Sync configurations

maxNrofRXPool-r16 INTEGER ::= 16 -- Maximum number of Rx resource pool for NR sidelink communication and

 -- discovery

maxNrofTXPool-r16 INTEGER ::= 8 -- Maximum number of Tx resource pool for NR sidelink communication and

 -- discovery

maxNrofPoolID-r16 INTEGER ::= 16 -- Maximum index of resource pool for NR sidelink communication and

 -- discovery

maxNrofSRS-PathlossReferenceRS-r16 INTEGER ::= 64 -- Maximum number of RSs used as pathloss reference for SRS power control.

maxNrofSRS-PathlossReferenceRS-1-r16 INTEGER ::= 63 -- Maximum number of RSs used as pathloss reference for SRS power control

 -- minus 1.

maxNrofSRS-ResourceSets INTEGER ::= 16 -- Maximum number of SRS resource sets in a BWP.

maxNrofSRS-ResourceSets-1 INTEGER ::= 15 -- Maximum number of SRS resource sets in a BWP minus 1.

maxNrofSRS-PosResourceSets-r16 INTEGER ::= 16 -- Maximum number of SRS Positioning resource sets in a BWP.

maxNrofSRS-PosResourceSets-1-r16 INTEGER ::= 15 -- Maximum number of SRS Positioning resource sets in a BWP minus 1.

maxNrofSRS-Resources INTEGER ::= 64 -- Maximum number of SRS resources.

maxNrofSRS-Resources-1 INTEGER ::= 63 -- Maximum number of SRS resources minus 1.

maxNrofSRS-PosResources-r16 INTEGER ::= 64 -- Maximum number of SRS Positioning resources.

maxNrofSRS-PosResources-1-r16 INTEGER ::= 63 -- Maximum number of SRS Positioning resources minus 1.

maxNrofSRS-ResourcesPerSet INTEGER ::= 16 -- Maximum number of SRS resources in an SRS resource set

maxNrofSRS-TriggerStates-1 INTEGER ::= 3 -- Maximum number of SRS trigger states minus 1, i.e., the largest code point.

maxNrofSRS-TriggerStates-2 INTEGER ::= 2 -- Maximum number of SRS trigger states minus 2.

maxRAT-CapabilityContainers INTEGER ::= 8 -- Maximum number of interworking RAT containers (incl NR and MRDC)

maxSimultaneousBands INTEGER ::= 32 -- Maximum number of simultaneously aggregated bands

maxSimultaneousBands-2-r18 INTEGER ::= 30 -- Maximum number of simultaneously aggregated bands minus 2.

maxULTxSwitchingBandPairs INTEGER ::= 32 -- Maximum number of band pairs supporting dynamic UL Tx switching in a band

 -- combination.

maxULTxSwitchingBetweenBandPairs-r18 INTEGER ::= 32 -- Maximum number of combinations of a band pair and another band pair/band

 -- between which dynamic UL Tx switching requires additional switching

 -- period.

maxSchedulingBandCombination-r18 INTEGER ::= 32 -- Maximum number of combinations of scheduling cell and co-scheduled cells

 -- have same or different carrier type.

maxNrofSlotFormatCombinationsPerSet INTEGER ::= 512 -- Maximum number of Slot Format Combinations in a SF-Set.

maxNrofSlotFormatCombinationsPerSet-1 INTEGER ::= 511 -- Maximum number of Slot Format Combinations in a SF-Set minus 1.

maxNrofTrafficPattern-r16 INTEGER ::= 8 -- Maximum number of Traffic Pattern for NR sidelink communication.

maxNrofPUCCH-Resources INTEGER ::= 128

maxNrofPUCCH-Resources-1 INTEGER ::= 127

maxNrofPUCCH-ResourceSets INTEGER ::= 4 -- Maximum number of PUCCH Resource Sets

maxNrofPUCCH-ResourceSets-1 INTEGER ::= 3 -- Maximum number of PUCCH Resource Sets minus 1.

maxNrofPUCCH-ResourcesPerSet INTEGER ::= 32 -- Maximum number of PUCCH Resources per PUCCH-ResourceSet

maxNrofPUCCH-P0-PerSet INTEGER ::= 8 -- Maximum number of P0-pucch present in a p0-pucch set

maxNrofPUCCH-PathlossReferenceRSs INTEGER ::= 4 -- Maximum number of RSs used as pathloss reference for PUCCH power control.

maxNrofPUCCH-PathlossReferenceRSs-1 INTEGER ::= 3 -- Maximum number of RSs used as pathloss reference for PUCCH power control

 -- minus 1.

maxNrofPUCCH-PathlossReferenceRSs-r16 INTEGER ::= 64 -- Maximum number of RSs used as pathloss reference for PUCCH power control

 -- extended.

maxNrofPUCCH-PathlossReferenceRSs-1-r16 INTEGER ::= 63 -- Maximum number of RSs used as pathloss reference for PUCCH power control

 -- minus 1 extended.

maxNrofPUCCH-PathlossReferenceRSs-1-r17 INTEGER ::= 7 -- Maximum number of RSs used as pathloss reference for PUCCH power control

 -- minus 1.

maxNrofPUCCH-PathlossReferenceRSsDiff-r16 INTEGER ::= 60 -- Difference between the extended maximum and the non-extended maximum

maxNrofPUCCH-ResourceGroups-r16 INTEGER ::= 4 -- Maximum number of PUCCH resources groups.

maxNrofPUCCH-ResourcesPerGroup-r16 INTEGER ::= 128 -- Maximum number of PUCCH resources in a PUCCH group.

maxNrofPowerControlSetInfos-r17 INTEGER ::= 8 -- Maximum number of PUCCH power control set infos

maxNrofMultiplePUSCHs-r16 INTEGER ::= 8 -- Maximum number of multiple PUSCHs in PUSCH TDRA list

maxNrofP0-PUSCH-AlphaSets INTEGER ::= 30 -- Maximum number of P0-pusch-alpha-sets (see TS 38.213 [13], clause 7.1)

maxNrofP0-PUSCH-AlphaSets-1 INTEGER ::= 29 -- Maximum number of P0-pusch-alpha-sets minus 1 (see TS 38.213 [13], clause 7.1)

maxNrofPUSCH-PathlossReferenceRSs INTEGER ::= 4 -- Maximum number of RSs used as pathloss reference for PUSCH power control.

maxNrofPUSCH-PathlossReferenceRSs-1 INTEGER ::= 3 -- Maximum number of RSs used as pathloss reference for PUSCH power control

 -- minus 1.

maxNrofPUSCH-PathlossReferenceRSs-r16 INTEGER ::= 64 -- Maximum number of RSs used as pathloss reference for PUSCH power control

 -- extended

maxNrofPUSCH-PathlossReferenceRSs-1-r16 INTEGER ::= 63 -- Maximum number of RSs used as pathloss reference for PUSCH power control

 -- extended minus 1

maxNrofPUSCH-PathlossReferenceRSsDiff-r16 INTEGER ::= 60 -- Difference between maxNrofPUSCH-PathlossReferenceRSs-r16 and

 -- maxNrofPUSCH-PathlossReferenceRSs

maxNrofPathlossReferenceRSs-r17 INTEGER ::= 64 -- Maximum number of RSs used as pathloss reference for PUSCH, PUCCH, SRS

 -- power control for unified TCI state operation

maxNrofPathlossReferenceRSs-1-r17 INTEGER ::= 63 -- Maximum number of RSs used as pathloss reference for PUSCH, PUCCH, SRS

 -- power control for unified TCI state operation minus 1

maxNrofNAICS-Entries INTEGER ::= 8 -- Maximum number of supported NAICS capability set

maxBands INTEGER ::= 1024 -- Maximum number of supported bands in UE capability.

maxBandsMRDC INTEGER ::= 1280

maxBandsEUTRA INTEGER ::= 256

maxCellReport INTEGER ::= 8

maxDRB INTEGER ::= 29 -- Maximum number of DRBs (that can be added in DRB-ToAddModList).

maxFreq INTEGER ::= 8 -- Max number of frequencies.

maxFreqLayers INTEGER ::= 4 -- Max number of frequency layers.

maxFreqPlus1 INTEGER ::= 9 -- Max number of frequencies for Slicing.

maxFreqIDC-r16 INTEGER ::= 128 -- Max number of frequencies for IDC indication.

maxCombIDC-r16 INTEGER ::= 128 -- Max number of reported UL CA for IDC indication.

maxFreqIDC-MRDC INTEGER ::= 32 -- Maximum number of candidate NR frequencies for MR-DC IDC indication

maxNrofCandidateBeams INTEGER ::= 16 -- Max number of PRACH-ResourceDedicatedBFR in BFR config.

maxNrofCandidateBeams-r16 INTEGER ::= 64 -- Max number of candidate beam resources in BFR config.

maxNrofCandidateBeamsExt-r16 INTEGER ::= 48 -- Max number of PRACH-ResourceDedicatedBFR in the CandidateBeamRSListExt

maxNrofPCIsPerSMTC INTEGER ::= 64 -- Maximum number of PCIs per SMTC.

maxNrofQFIs INTEGER ::= 64

maxNrofResourceAvailabilityPerCombination-r16 INTEGER ::= 256

maxNrOfSemiPersistentPUSCH-Triggers INTEGER ::= 64 -- Maximum number of triggers for semi persistent reporting on PUSCH

maxNrofSR-Resources INTEGER ::= 8 -- Maximum number of SR resources per BWP in a cell.

maxNrofSlotFormatsPerCombination INTEGER ::= 256

maxNrofSpatialRelationInfos INTEGER ::= 8

maxNrofSpatialRelationInfos-plus-1 INTEGER ::= 9

maxNrofSpatialRelationInfos-r16 INTEGER ::= 64

maxNrofSpatialRelationInfosDiff-r16 INTEGER ::= 56 -- Difference between maxNrofSpatialRelationInfos-r16 and maxNrofSpatialRelationInfos

maxNrofIndexesToReport INTEGER ::= 32

maxNrofIndexesToReport2 INTEGER ::= 64

maxNrofSSBs-r16 INTEGER ::= 64 -- Maximum number of SSB resources in a resource set.

maxNrofSSBs-1 INTEGER ::= 63 -- Maximum number of SSB resources in a resource set minus 1.

maxNrofS-NSSAI INTEGER ::= 8 -- Maximum number of S-NSSAI.

maxNrofTCI-StatesPDCCH INTEGER ::= 64

maxNrofTCI-States INTEGER ::= 128 -- Maximum number of TCI states.

maxNrofTCI-States-1 INTEGER ::= 127 -- Maximum number of TCI states minus 1.

maxUL-TCI-r17 INTEGER ::= 64 -- Maximum number of TCI states.

maxUL-TCI-1-r17 INTEGER ::= 63 -- Maximum number of TCI states minus 1.

maxNrofAdditionalPCI-r17 INTEGER ::= 7 -- Maximum number of additional PCI

maxNrofAdditionalPRACHConfigs-r18 INTEGER ::= 7 -- Maximum number of additional PRACH configurations for 2TA

maxNrofdelayD-r18 INTEGER ::= 4 -- Maximum number of delayD values.

maxMPE-Resources-r17 INTEGER ::= 64 -- Maximum number of pooled MPE resources

maxNrofUL-Allocations INTEGER ::= 16 -- Maximum number of PUSCH time domain resource allocations.

maxQFI INTEGER ::= 63

maxRA-CSIRS-Resources INTEGER ::= 96

maxRA-OccasionsPerCSIRS INTEGER ::= 64 -- Maximum number of RA occasions for one CSI-RS

maxRA-Occasions-1 INTEGER ::= 511 -- Maximum number of RA occasions in the system

maxRA-SSB-Resources INTEGER ::= 64

maxSCSs INTEGER ::= 5

maxSecondaryCellGroups INTEGER ::= 3

maxNrofServingCellsEUTRA INTEGER ::= 32

maxMBSFN-Allocations INTEGER ::= 8

maxNrofMultiBands INTEGER ::= 8

maxCellSFTD INTEGER ::= 3 -- Maximum number of cells for SFTD reporting

maxReportConfigId INTEGER ::= 64

maxNrofCodebooks INTEGER ::= 16 -- Maximum number of codebooks supported by the UE

maxNrofCSI-RS-ResourcesExt-r16 INTEGER ::= 16 -- Maximum number of codebook resources supported by the UE for eType2/Codebook combo

maxNrofCSI-RS-ResourcesExt-r17 INTEGER ::= 8 -- Maximum number of codebook resources for fetype2R1 and fetype2R2

maxNrofCSI-RS-Resources INTEGER ::= 7 -- Maximum number of codebook resources supported by the UE

maxNrofCSI-RS-ResourcesAlt-r16 INTEGER ::= 512 -- Maximum number of alternative codebook resources supported by the UE

maxNrofCSI-RS-ResourcesAlt-1-r16 INTEGER ::= 511 -- Maximum number of alternative codebook resources supported by the UE minus 1

maxNrofSRI-PUSCH-Mappings INTEGER ::= 16

maxNrofSRI-PUSCH-Mappings-1 INTEGER ::= 15

maxSIB INTEGER::= 32 -- Maximum number of SIBs

maxSI-Message INTEGER::= 32 -- Maximum number of SI messages

maxSIB-MessagePlus1-r17 INTEGER::= 33 -- Maximum number of SIB messages plus 1

maxPO-perPF INTEGER ::= 4 -- Maximum number of paging occasion per paging frame

maxPEI-perPF-r17 INTEGER ::= 4 -- Maximum number of PEI occasion per paging frame

maxAccessCat-1 INTEGER ::= 63 -- Maximum number of Access Categories minus 1

maxBarringInfoSet INTEGER ::= 8 -- Maximum number of access control parameter sets

maxCellEUTRA INTEGER ::= 8 -- Maximum number of E-UTRA cells in SIB list

maxEUTRA-Carrier INTEGER ::= 8 -- Maximum number of E-UTRA carriers in SIB list

maxPLMNIdentities INTEGER ::= 8 -- Maximum number of PLMN identities in RAN area configurations

maxDownlinkFeatureSets INTEGER ::= 1024 -- (for NR DL) Total number of FeatureSets (size of the pool)

maxUplinkFeatureSets INTEGER ::= 1024 -- (for NR UL) Total number of FeatureSets (size of the pool)

maxEUTRA-DL-FeatureSets INTEGER ::= 256 -- (for E-UTRA) Total number of FeatureSets (size of the pool)

maxEUTRA-UL-FeatureSets INTEGER ::= 256 -- (for E-UTRA) Total number of FeatureSets (size of the pool)

maxFeatureSetsPerBand INTEGER ::= 128 -- (for NR) The number of feature sets associated with one band.

maxPerCC-FeatureSets INTEGER ::= 1024 -- (for NR) Total number of CC-specific FeatureSets (size of the pool)

maxFeatureSetCombinations INTEGER ::= 1024 -- (for MR-DC/NR)Total number of Feature set combinations (size of the pool)

maxInterRAT-RSTD-Freq INTEGER ::= 3

maxGIN-r17 INTEGER ::= 24 -- Maximum number of broadcast GINs

maxHRNN-Len-r16 INTEGER ::= 48 -- Maximum length of HRNNs

maxNPN-r16 INTEGER ::= 12 -- Maximum number of NPNs broadcast and reported by UE at establishment

maxSNPN-ConfigCellId-r18 INTEGER ::= 32 -- Maximum number of Cell ID subject for SNPNS for MDT scope

maxSNPN-ConfigID-r18 INTEGER ::= 16 -- Maximum number of SNPNs subject for MDT scope

maxSNPN-ConfigTAI-r18 INTEGER ::= 8 -- Maximum number of TA subject for MDT scope

maxNrOfMinSchedulingOffsetValues-r16 INTEGER ::= 2 -- Maximum number of min. scheduling offset (K0/K2) configurations

maxK0-SchedulingOffset-r16 INTEGER ::= 16 -- Maximum number of slots configured as min. scheduling offset (K0)

maxK2-SchedulingOffset-r16 INTEGER ::= 16 -- Maximum number of slots configured as min. scheduling offset (K2)

maxK0-SchedulingOffset-r17 INTEGER ::= 64 -- Maximum number of slots configured as min. scheduling offset (K0)

maxK2-SchedulingOffset-r17 INTEGER ::= 64 -- Maximum number of slots configured as min. scheduling offset (K2)

maxDCI-2-6-Size-r16 INTEGER ::= 140 -- Maximum size of DCI format 2-6

maxDCI-2-7-Size-r17 INTEGER ::= 43 -- Maximum size of DCI format 2-7

maxDCI-2-6-Size-1-r16 INTEGER ::= 139 -- Maximum DCI format 2-6 size minus 1

maxDCI-2-9-Size-r18 INTEGER ::= 140 -- Maximum DCI format 2-9 size

maxDCI-2-9-Size-1-r18 INTEGER ::= 139 -- Maximum DCI format 2-9 size minus 1

maxNrofUL-Allocations-r16 INTEGER ::= 64 -- Maximum number of PUSCH time domain resource allocations

maxNrofUL-Allocations-1-r18 INTEGER ::= 63 -- Maximum number of PUSCH time domain resource allocations minus 1

maxNrofP0-PUSCH-Set-r16 INTEGER ::= 2 -- Maximum number of P0 PUSCH set(s)

maxOnDemandSIB-r16 INTEGER ::= 8 -- Maximum number of SIB(s) that can be requested on-demand

maxOnDemandPosSIB-r16 INTEGER ::= 32 -- Maximum number of posSIB(s) that can be requested on-demand

maxCI-DCI-PayloadSize-r16 INTEGER ::= 126 -- Maximum number of the DCI size for CI

maxCI-DCI-PayloadSize-1-r16 INTEGER ::= 125 -- Maximum number of the DCI size for CI minus 1

maxUu-RelayRLC-ChannelID-r17 INTEGER ::= 32 -- Maximum value of Uu Relay RLC channel ID

maxWLAN-Id-Report-r16 INTEGER ::= 32 -- Maximum number of WLAN IDs to report

maxWLAN-Name-r16 INTEGER ::= 4 -- Maximum number of WLAN name

maxRAReport-r16 INTEGER ::= 8 -- Maximum number of RA procedures information to be included in the RA report

maxTxConfig-r16 INTEGER ::= 64 -- Maximum number of sidelink transmission parameters configurations

maxTxConfig-1-r16 INTEGER ::= 63 -- Maximum number of sidelink transmission parameters configurations minus 1

maxPSSCH-TxConfig-r16 INTEGER ::= 16 -- Maximum number of PSSCH TX configurations

maxNrofCLI-RSSI-Resources-r16 INTEGER ::= 64 -- Maximum number of CLI-RSSI resources for UE

maxNrofCLI-RSSI-Resources-1-r16 INTEGER ::= 63 -- Maximum number of CLI-RSSI resources for UE minus 1

maxNrofCLI-SRS-Resources-r16 INTEGER ::= 32 -- Maximum number of SRS resources for CLI measurement for UE

maxCLI-Report-r16 INTEGER ::= 8

maxNrofCC-Group-r17 INTEGER ::= 16 -- Maximum number of CC groups for DC location report

maxNrofConfiguredGrantConfig-r16 INTEGER ::= 12 -- Maximum number of configured grant configurations per BWP

maxNrofConfiguredGrantConfig-1-r16 INTEGER ::= 11 -- Maximum number of configured grant configurations per BWP minus 1

maxNrofCG-Type2DeactivationState INTEGER ::= 16 -- Maximum number of deactivation state for type 2 configured grants per BWP

maxNrofConfiguredGrantConfigMAC-1-r16 INTEGER ::= 31 -- Maximum number of configured grant configurations per MAC entity minus 1

maxNrofCSI-ReportSubconfigPerCSI-ReportConfig-r18 INTEGER ::= 8 -- Maximum number of CSI report subconfigurations per CSI report

 -- configuration

maxNrofCSI-ReportSubconfigPerCSI-ReportConfig-1-r18 INTEGER ::= 7 -- Maximum number of CSI report subconfigurations per CSI report

 -- configuration minus 1

maxNrofSPS-Config-r16 INTEGER ::= 8 -- Maximum number of SPS configurations per BWP

maxNrofSPS-Config-1-r16 INTEGER ::= 7 -- Maximum number of SPS configurations per BWP minus 1

maxNrofSPS-DeactivationState INTEGER ::= 16 -- Maximum number of deactivation state for SPS per BWP

maxNrofPPW-Config-r17 INTEGER ::= 4 -- Maximum number of Preconfigured PRS processing windows per DL BWP

maxNrofPPW-ID-1-r17 INTEGER ::= 15 -- Maximum number of Preconfigured PRS processing windows minus 1

maxNrOfTxTEGReport-r17 INTEGER ::= 256 -- Maximum number of UE Tx Timing Error Group Report

maxNrOfTxTEG-ID-1-r17 INTEGER ::= 7 -- Maximum number of UE Tx Timing Error Group ID minus 1

maxNrofPagingSubgroups-r17 INTEGER ::= 8 -- Maximum number of paging subgroups per paging occasion

maxNrofPagingSubgroupsLP-r19 INTEGER ::= [31] -- Maximum number of paging subgroups per paging occasion for LP-WUS

Editor’s NOTE: The maximum subgroup number is to be updated based on RAN1 progress.

maxNrofPUCCH-ResourceGroups-1-r16 INTEGER ::= 3

maxNrofReqComDC-Location-r17 INTEGER ::= 128 -- Maximum number of requested carriers/BWPs combinations for DC location

 -- report

maxNrofServingCellsTCI-r16 INTEGER ::= 32 -- Maximum number of serving cells in simultaneousTCI-UpdateList

maxNrofTxDC-TwoCarrier-r16 INTEGER ::= 64 -- Maximum number of UL Tx DC locations reported by the UE for 2CC uplink CA

maxNrofRB-SetGroups-r17 INTEGER ::= 8 -- Maximum number of RB set groups

maxNrofRB-Sets-r17 INTEGER ::= 8 -- Maximum number of RB sets

maxNrofEnhType3HARQ-ACK-r17 INTEGER ::= 8 -- Maximum number of enhanced type 3 HARQ-ACK codebook

maxNrofEnhType3HARQ-ACK-1-r17 INTEGER ::= 7 -- Maximum number of enhanced type 3 HARQ-ACK codebook minus 1

maxNrofPRS-ResourcesPerSet-r17 INTEGER ::= 64 -- Maximum number of PRS resources for one set

maxNrofPRS-ResourcesPerSet-1-r17 INTEGER ::= 63 -- Maximum number of PRS resources for one set minus 1

maxNrofPRS-ResourceOffsetValue-1-r17 INTEGER ::= 511

maxNrofGapId-r17 INTEGER ::= 8 -- Maximum number of measurement gap ID

maxNrofPreConfigPosGapId-r17 INTEGER ::= 16 -- Maximum number of preconfigured positioning measurement gap

maxNrOfGapPri-r17 INTEGER ::= 16 -- Maximum number of gap priority level

maxCEFReport-r17 INTEGER ::= 4 -- Maximum number of CEF reports by the UE

maxNrofMultiplePDSCHs-r17 INTEGER ::= 8 -- Maximum number of PDSCHs in PDSCH TDRA list

maxSliceInfo-r17 INTEGER ::= 8 -- Maximum number of NSAGs

maxCellSlice-r17 INTEGER ::= 16 -- Maximum number of cells supporting the NSAG

maxNrofTRS-ResourceSets-r17 INTEGER ::= 64 -- Maximum number of TRS resource sets

maxNrofSearchSpaceGroups-1-r17 INTEGER ::= 2 -- Maximum number of search space groups minus 1

maxNrofRemoteUE-r17 INTEGER ::= 32 -- Maximum number of connected L2 U2N Remote UEs

maxDCI-4-2-Size-r17 INTEGER ::= 140 -- Maximum size of DCI format 4-2

maxFreqMBS-r17 INTEGER ::= 16 -- Maximum number of MBS frequencies reported in MBSInterestIndication

maxNrofDRX-ConfigPTM-r17 INTEGER ::= 64 -- Max number of DRX configuration for PTM provided in MBS broadcast in a

 -- cell

maxNrofDRX-ConfigPTM-1-r17 INTEGER ::= 63 -- Max number of DRX configuration for PTM provided in MBS broadcast in a

 -- cell minus 1

maxNrofMBS-ServiceListPerUE-r17 INTEGER ::= 16 -- Maximum number of services which the UE can include in the MBS interest

 -- indication

maxNrofMBS-Session-r17 INTEGER ::= 1024 -- Maximum number of MBS sessions provided in MBS broadcast or multicast in

 -- a cell

maxNrofMTCH-SSB-MappingWindow-r17 INTEGER ::= 16 -- Maximum number of MTCH to SSB beam mapping pattern

maxNrofMTCH-SSB-MappingWindow-1-r17 INTEGER ::= 15 -- Maximum number of MTCH to SSB beam mapping pattern minus 1

maxNrofMRB-Broadcast-r17 INTEGER ::= 4 -- Maximum number of broadcast MRBs configured for one MBS broadcast service

maxNrofPageGroup-r17 INTEGER ::= 32 -- Maximum number of paging groups in a paging message

maxNrofPDSCH-ConfigPTM-r17 INTEGER ::= 16 -- Maximum number of PDSCH configuration groups for PTM

maxNrofPDSCH-ConfigPTM-1-r17 INTEGER ::= 15 -- Maximum number of PDSCH configuration groups for PTM minus 1

maxG-RNTI-r17 INTEGER ::= 16 -- Maximum number of G-RNTI that can be configured for a UE.

maxG-RNTI-1-r17 INTEGER ::= 15 -- Maximum number of G-RNTI that can be configured for a UE minus 1.

maxG-CS-RNTI-r17 INTEGER ::= 8 -- Maximum number of G-CS-RNTI that can be configured for a UE.

maxG-CS-RNTI-1-r17 INTEGER ::= 7 -- Maximum number of G-CS-RNTI that can be configured for a UE minus 1.

maxMRB-r17 INTEGER ::= 32 -- Maximum number of multicast MRBs (that can be added in MRB-ToAddModLIst)

maxFSAI-MBS-r17 INTEGER ::= 64 -- Maximum number of MBS frequency selection area identities

maxNeighCellMBS-r17 INTEGER ::= 8 -- Maximum number of MBS broadcast neighbour cells

maxNrofPdcch-BlindDetectionMixed-1-r16 INTEGER ::= 7 -- Maximum number of combinations of mixed Rel-16 and Rel-15 PDCCH

 -- monitoring capabilities minus 1

maxNrofPdcch-BlindDetection-r17 INTEGER ::= 16 -- Maximum number of combinations of PDCCH blind detection monitoring

 -- capabilities

maxNrofAltitudeRanges-r18 INTEGER ::= 8 -- Maximum number of altitude ranges for altitude-based measurement configurations

maxWayPoint-r18 INTEGER ::= 20 -- Maximum number of flight path information waypoints

maxAltitude-r18 INTEGER ::= 10000 -- Maximum altitude in meters

minAltitude-r18 INTEGER ::= -420 -- Minimum altitude in meters

maxMeasSequence-r18 INTEGER ::= 64 -- Maximum number of configured sequence for measurement

maxNrofHops-1-r18 INTEGER ::= 5 -- Maximum number of Hops that can be configured for Positioning SRS Transmission

maxNrOfCellsInVA-r18 INTEGER ::= 16 -- Maximum number of cells in validity area for Positioning SRS

maxNrOfCellsInVA-Ext-r18 INTEGER ::= 16 -- Maximum number of additional cells in validity area for Positioning SRS

maxNrOfLinkedSRS-PosResourceSet-r18 INTEGER ::= 3 -- Maximum number of linked SRSPosResourceSets that can be aggregated across

 -- CCs

maxNrOfLinkedSRS-PosResSetComb-r18 INTEGER ::= 32 -- Maximum number of combinations of linked SRSPosResourceSets that can be

 -- aggregated in RRC\_CONNECTED state

maxNrOfLinkedSRS-PosResSetCombInactive-r18 INTEGER ::= 16 -- Maximum number of combinations of linked SRSPosResourceSets that can be

 -- aggregated in RRC\_INACTIVE state

maxCBR-ConfigDedSL-PRS-1-r18 INTEGER ::= 7 -- Maximum number of CBR ranges for dedicated SL PRS resource pool

maxCBR-LevelDedSL-PRS-1-r18 INTEGER ::= 15 -- Maximum number of CBR levels for dedicated SL PRS resource pool

maxNrofSL-PRS-TxPool-r18 INTEGER ::= 8 -- Maximum number of Tx dedicated SL-PRS resource pool for NR sidelink positioning

maxNrofSL-PRS-TxConfig-r18 INTEGER ::= 64 -- Maximum number of SL PRS transmission parameter configurations

maxNrOfVA-r18 INTEGER ::= 16 -- Maximum number of validity area

maxNrofLTM-Configs-r18 INTEGER ::= 8 -- Maximum number of LTM candidate cells

maxNrofLTM-Configs-plus1-r18 INTEGER ::= 9 -- Maximum number of LTM candidate cells plus 1

maxNrofLTM-CSI-ReportConfigurations-r18 INTEGER ::= 48 -- Maximum number of LTM CSI reporting configurations

maxNrofLTM-CSI-ReportConfigurations-1-r18 INTEGER ::= 47 -- Maximum number of LTM CSI reporting configurations minus 1

maxNrofLTM-CSI-SSB-ResourcesPerSet-r18 INTEGER ::= 512 -- Maximum number of LTM CSI SSB resource per set

maxNrofLTM-CSI-ResourceConfigurations-r18 INTEGER ::= 112 -- Maximum number of LTM CSI resource configurations

maxNrofLTM-CSI-ResourceConfigurations-1-r18 INTEGER ::= 111 -- Maximum number of LTM CSI resource configurations minus 1

maxNrofCandidateTCI-State-r18 INTEGER ::= 128 -- Maximum number of LTM TCI states

maxNrofCandidateUL-TCI-r18 INTEGER ::= 64 -- Maximum number of LTM UL TCI states

maxSecurityCellSet-r18 INTEGER ::= 9 -- Maximum number of cell sets for subsequent CPAC.

maxSK-Counter-r18 INTEGER ::= 8 -- Maximum number of SK-counters configured for a cell set for subsequent CPAC.

maxNrofThresholdMBS-r18 INTEGER ::= 8 -- Max number of thresholds of MBS sessions for RRC connection resume for a

 -- UE receiving multicast in RRC\_INACTIVE

maxNrofThresholdMBS-1-r18 INTEGER ::= 7 -- Max number of thresholds of MBS sessions for RRC connection resume for a

 -- UE receiving multicast in RRC\_INACTIVE minus 1

maxTN-AreaInfo-r18 INTEGER ::= 32 -- Maximum number of TN coverage areas for which assistance info is

 -- provided in an NTN cell

maxNrofSetsOfCells-r18 INTEGER ::= 4 -- Maximum number of sets of cells for multi-cell PDSCH/PUSCH scheduling

maxNrofSetsOfCells-1-r18 INTEGER ::= 3 -- Maximum number of sets of cells for multi-cell PDSCH/PUSCH scheduling

 -- minus 1

maxNrofCellsInSet-r18 INTEGER ::= 4 -- Maximum number of cells configured in a set of cells for multi-cell

 -- PDSCH/PUSCH scheduling

maxNrofCellsInSet-1-r18 INTEGER ::= 3 -- Maximum number of cells configured in a set of cells for multi-cell

 -- PDSCH/PUSCH scheduling minus 1

maxNrofCellCombos-r18 INTEGER ::= 16 -- Maximum number of combinations of co-scheduled cells for multi-cell

 -- PDSCH/PUSCH scheduling

maxNrofBWPsInSetOfCells-r18 INTEGER ::= 16 -- Maximum number of BWPs configured in a set of cells for multi-cell

 -- PDSCH/PUSCH scheduling

maxLowerMSD-r18 INTEGER ::= 256 -- Maximum number of lower MSD capability sets for a victim band

maxLowerMSDInfo-r18 INTEGER ::= 64 -- Maximum number of lower MSD capability sets for a band combination

maxNrofIntraEndc-Components-r17 INTEGER ::= 4 -- Maximum number of intra-band (NG)EN-DC band components in an inter-band

 -- (NG)EN-DC band combination

-- TAG-MULTIPLICITY-AND-TYPE-CONSTRAINT-DEFINITIONS-STOP

-- ASN1STOP

End of change

Annex E (informative) – RAN2 agreements

Annex F (informative) – RAN1 agreements