**3GPP TSG-RAN WG2 Meeting #130 R2-250xxxx**

**St Julian, Malta, 19th – 23rd May 2025**

**Source: vivo**

**Title: Discussion summary and list of MAC open issues for mobility Enhancements**

**Agenda Item: 8.6.1**

**Document for: Discussion and Decision**

1. Introduction

This document summarizes the discussion of the following email discussion and collects the MAC open issues for mobility Enhancements.

* [POST129b][117][MOB] (Vivo)

**Scope:**

1. Update MAC running CR based on RAN2#129bis progress
2. Essential open issue list in a separate contribution (MAC running CR can keep editor’s notes for readability).

**Intended outcome:** Updated MAC running CR and essential MAC open issue list.

**Deadline: Long email discussion**

Companies are invited to provide comments/additional issues in the below table by 2nd May, 2025

# Discussion

* 1. Part I - Issues related to running CR

**Open issue MAC-1 (essential): Whether the beam specific offset for serving cell Obs is needed for LTM event evaluation**

In the current MAC running CR, there is an EN as below:

Editor’s NOTE: FFS whether the beam specific offset for serving cell Obs is needed. If needed, per-serving cell or per-beam or per-RS type. Similar as other events.

In RAN2#126 meeting, we agreed the beam specific offset is configured for LTM event evaluation:

|  |
| --- |
| 6. For LTM event evaluation, TTT, hysteresis for entering/leaving, and/or beam specific (FFS for cell specific) offset can be applied. FFS on the need of measurement reporting once leaving condition is met. |

In RAN2#129bis meeting, the configuration format for the beam specific offset is agreed as following:

|  |
| --- |
| 1. In L1 reporting configuration, the UE can be configured with a list of candidate IDs. For each listed candidate ID, the network can configure an offset, this offset applies to all the RSs belong the candidate ID that associated with the reporting configuration (the offset value also includes 0dB); If a candidate ID is not provided in the reporting configuration, it means the UE is not required to measure/evaluate the RSs that belonging to the candidate ID for this event, even if these are configured within the L1 resource configuration (to which the L1 reporting configuration points to). |

Current MAC running CR introduce the beam offset for candidate beam as below, while the beam offset for serving cell is FFS. According to the latest agreement, the beam offset is configured in the LTM L1 reporting configuration. The serving cell won’t generally be associated to a LTM L1 reporting configuration, so there is no such beam offset is configured for current beam.

|  |
| --- |
| Inequality LTM3-1 (Entering condition)  *Mn + Obn* *– Hys > Ms + Obs + Off*  Inequality LTM3-2 (Leaving condition)  *Mn + Obn + Hys < Ms + Obs + Off*  The variables in the formula are defined as follows:  ***Mn*** is the beam measurement quantity of the LTM candidate cell based on SS/PBCH block or CSI-RS, not taking into account any offsets.  ***Obn*** is the offset of the LTM candidate cell (i.e. [*beamIndividualOffsetN*] as defined in *LTM-CSI-ReportConfig* for this event). One offset is applied to all beam(s) associated with the LTM candidate cell.  ***Ms*** is the beam measurement quantity of the serving cell based on SS/PBCH block or CSI-RS, not taking into account any offsets. The beam associated with this event is the current beam, i.e corresponding to the RS configured in the indicated TCI state or the RS QCLed with the RS configured in the indicated TCI State indicated by TCI State in the serving cell [as defined in clause 5.1.5 in TS 38.214] in the serving cell.  **[*FFS Obs*** is the offset of the beam of the serving cell (i.e. [*beamIndividualOffsetS*] as defined in *LTM-CSI-ReportConfig* for this event).] |

Thus, rapporteur suggests to discuss whether the beam offset should be introduced for current beam of serving cell for LTM event evaluation, e.g. for LTM2, LTM3 and LTM5.

**Companies are invited to provide your views on whether introducing the beam offset for current beam of serving cell for the LTM event evaluation:**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments, if any** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**If companies agree to introduce the beam offset for current beam of serving cell, companies are invited to provide your preference on the offset granularity, e.g. the beam offset is configured per beam/serving cell/RS type/etc.:**

|  |  |  |
| --- | --- | --- |
| **Company** | **Granularity** | **Comments, if any** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**If companies agree to introduce the beam offset for current beam of serving cell, companies are invited to provide your preference on which LTM event the beam offset is used for, e.g. LTM2, LTM3, LTM5:**

|  |  |  |
| --- | --- | --- |
| **Company** | **LTM2/LTM3/LTM5** | **Comments, if any** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Open issue MAC-2 (essential): How to ensure UE be able to report the event-triggered beam(s) that were not included in the truncated MR MAC CE by the following grant**

In RAN2#129 bis meeting, we have the following agreements for the truncated L1 MR MAC CE, the UE should be able to report the event-triggered beam(s) that were not included in the truncated MR MAC CE by the following grant.

|  |
| --- |
| 1. Intention is that the UE should be able to report the event-triggered beam(s) that were not included in the truncated MR MAC CE by the following grant. Detailed wording can be further discussed as part of the running CR. |

In the current MAC running CR, this agreement was catprued as below, i.e. the triggered L1 MR is cancelled only if the normal MR MAC CE is transmitted, while it is not cancelled if the truncated MAC CE is transmitted.

|  |
| --- |
| 1> if at least one L1 measurement report has been triggered as specified in 5.x.3 and not cancelled:  2> if UL-SCH resources are available for a new transmission in the serving cell and these UL-SCH resources can accommodate the L1 measurement report MAC CE plus its subheader as a result of logical channel prioritization:  3> instruct the Multiplexing and Assembly procedure to generate the L1 measurement report MAC CE;  ….  3> cancel the the triggered L1 measurement report;  2> else if the UL-SCH resources are available for a new transmission in the serving cell and these UL-SCH resources can accommodate the Truncated L1 measurement report MAC CE plus its subheader as a result of logical channel prioritization:  3> instruct the Multiplexing and Assembly procedure to generate the Truncated L1 measurement report MAC CE;  …. |

Rapportuer understands that this could ensure that UE is able to report the event-triggered beam(s) that were not included in the truncated MR MAC CE by the following grant. If the network provides enough grant later, the UE will transmit the whole L1 MR MAC CE, which would include the event-triggered beam(s) that were not included in the truncated MR MAC CE, and maybe also include the parts which have been reported to network via the truncated L1 MR MAC CE before. If the grant provided by network is still not enough later, the UE will continue to transmit the truncated L1 MR MAC CE, which would include the event-triggered beam(s) that were not included in the truncated MR MAC CE before by UE implementation.

Alternatively, if companies prefer to specify this explicitly in the specification, we need to design the model like:

* UE maintains a list for the triggering beam(s); once the measurement quantity of a beam satisfies the trigger event, it will be stored in this list;
* UE maintains a list for the reporting beam(s); once the UE transmits the event triggered L1 MR MAC CE (not truncated MAC CE), the beam(s) in the triggering list will be moved to the reporting list;

If the UE transmits the event triggered truncated L1 MR MAC CE, the beam(s) in the triggering list will be still maintained in the triggering list.

Rapporteur understands the current MAC running CR is enough, or at most we could add some note the clarify the UE behaviour on how to report event-triggered beam(s) after a truncated MR MAC CE before.

**Companies are invited to provide your view on whether the current MAC running CR is enough (may be a note could be added) or not for the above agreement.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Comments** | |
|  |  | |
|  |  | |
|  |  | |
|  |  | |
|  |  |  |

**Open issue MAC-3 (essential):The initial status for Semi-persistent CSI-RS resoruce set for candidate cell**

In the current MAC running CR, there is an EN as below:

Editor’s NOTE: FFS whether the Semi-persistent CSI-RS resource set for candidate cell is initially deactivation upon (re-)configuration by upper layers.

In RAN2#129bis meeting, we have the agreements:

|  |
| --- |
| 1. Introduce new MAC CE to activate/deactivate the semi-persistent CSI-RS resource. 2. The new MAC CE includes: A/D indication, Target configuration id or {SP CSI-RS resource set id and/or candidate id}, TCI state id. |

However there is no conclusion on whether the Semi-persostemt CSI-RS resource set for candidate cell is initial deactivated or not upon (re)configuraiton by upper, rapporteur thinks it is straightforward that it is initial deactivated and will be activated upon receiving the new MAC CE.

**Companies are invited to provide comments on** **whether agree: the Semi-persistent CSI-RS resource set for candidate cell MAC CE is initially deactiated upon (re-)configuration by upper layer or not .**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments, if any** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Open issue MAC-4 (essential): Whethe keep L1-SINR quantity for L1 event triggered MR as FFS..**

In the current MAC running CR, there is an EN as below:

Editor’s NOTE: Beam quantity of SINR is up to RAN1 discussion and decision. Similar for events definition. By now, the conclusion in RAN1 is: *there is no consensus in RAN1 on the support L1-SINR measurement based on CSI-RS for candidate cells.* But there is no concludion on L1-SINR for SSB.

In the corresponding description for the L1 event triggered MR procedure, multiple places are FFS due to this undetermined point.

However, rapporteur understands that RAN1 won’t discuss this issue anymore for CSI-RS, and there is no beam quantity SINR for SSB. Thus, there is no need to keep this open issue in RAN2.

**Companies are invited to provide comments on whether agree RAN2 assumes there is no L1-SINR quantity for L1 event triggered MR.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments, if any** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

* 1. Part I – Other open issue list

**Rapporteur provides the list of open issues as below, and the corresponding suggestions on how to address them. Some of them could be further discussed based on contributions or resoved based on further progress. Companies are invited to provide comments on whether it is open issue and whether the suggestions from reapporteur is accuracy enough.**

|  |  |
| --- | --- |
| **Company** | **Comments, if any** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

### Inter-CU LTM

N/A

### Event triggered L1 measurement

|  |  |  |
| --- | --- | --- |
| **Index** | **Issue description** | **Rapporteur suggestion** |
| MAC-5 | **The content of L1 MR MAC CE triggered by LTM2**  Editor’s NOTE: FFS For MR triggered by LTM2, whether only include the current beam information in the MR MAC CE or the MR can include measurements for LTM candidates. | **Issue Type:** Essential  **How to address it:** based on companies’ contribution |
| MAC-6 | **Truncated L1 MR MAC CE details. E.g.**  **Except the triggered beam, whether any beam should be prioritised to be included in the truncated L1 MR MAC CE?**  **In case the UL grant could include at least 2 beams in truncated L1 MR MAC CE, which beam should be included as the first beam in the truncated L1 MR MAC CE?**  **Based on following agreement:**   * For differential L1-RSRP reporting, the best quality beam among the beams included in L1 MR MAC CE is taken as the reference beam as the first one. The differential L1-RSRP value is derived based on the absolute L1-RSRP of the reference beam. FFS for truncated MAC CE. | **Issue Type:** Not essential  **How to address it:** can be discussed based on companies’ contribution |
| MAC-7 | **Whether one UL TB could include more than one truncated MAC CE or only one?**  For the case more than 1 triggering events are pending, if UL grant is sufficient for one regular L1 MR MAC CE or for two truncated L1 MR MAC CEs but insufficient for two regular L1 MR MAC CEs, the UE behaviour should be discussed. | **Issue Type:** Not essential  **How to address it:** can be discussed based on companies’ contribution |
| MAC-8 | **FFS the coexistence between event triggered report and mTRP, e.g.**  how UE determine the current beam or candidate beam in this case? | **Issue Type:** Not essential  **How to address it:** can be discussed based on companies’ contribution |

### Conditional intra-CU LTM

|  |  |  |
| --- | --- | --- |
| **Index** | **Issue description** | **Rapporteur suggestion** |
| MAC-9 | **In case UE considers RACH-less CLTM is ongoing, i.e., UE has valid TA for CLTM target cell, how UE selectes the valid CG resource for L3 based CLTM?**  Editor’s NOTE: FFS in case UE considers RACH-less CLTM is ongoing, i.e., UE has valid TA for CLTM target cell, how UE selectes the valid CG resource for L3 based CLTM. | **Issue Type:** Essential  **How to address it:** based on companies’ contribution |
| MAC-10 | **Beam selection for L3 based RACH-less CLTM determination**  Editor’s NOTE: FFS how to determine the selected beam in case the CLTM is triggered by L3 event. | **Issue Type:** Essential  **How to address it:** based on companies’ contribution |
| MAC-11 | **In case UE considers RACH-less CLTM is ongoing, i.e., UE has valid TA for LTM target cell, while UE couldn’t obtain valid CG resource, whether UE will fall back to RACH-based LTM?** | **Issue Type:** Not essential but important  **How to address it:** based on companies’ contribution |
| MAC-12 | **How UE selece the CG resource if the selected beam is CSI-RS?**  Editor’s NOTE: This part will be further updated based on RAN1 progress on CSI-RS. E.g. there is no agreeent on CSI-RS associated with CG. | **Issue Type:** Not essential but important  **How to address it:** based on RAN1 inputs |
| MAC-13 | **FFS the coexistence between CLTM and (e)RedCap, CovEnh?**  Editor’s NOTE: Whether/How CLTM could co-exist with (e)RedCap is FFS, i.e. whether follow Rel-18 intra-CU LTM as below.  Editor’s NOTE: Whether/How CLTM could co-exist with CovEnh is FFS, i.e. whether follow Rel-18 intra-CU LTM as below. | **Issue Type:** Not essential but important  **How to address it:** based on companies’ contribution |

### Others, please specify

Companies are invited to describe any other identified open issues not currently included within this document.

|  |  |
| --- | --- |
| **Company** | **Other identified open issues? (please describe) or other comments** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# Conclusion

In this contribution, we collect the open issues for mobility enhancements in MAC as below:

***Inter-CU LTM***

***Event triggered L1 measurement***

***Conditional intra-CU LTM***

# References

1. R2-25xxx, MAC running CR for Mob ph4, vivo.