3GPP RAN WG2 Meeting #130 *R2-25xxxxx*

Malta, Malta, May 19th – 23rd, 2025

Agenda Item: 8.11.1

Source: Huawei, HiSilicon

Title: Remaining RRC open issues in feature SBFD

Document for: Discussion, Decision

# Introduction

The following document includes a list of open issues (and proposals applicable) according to the following email discussion:

* [Post129bis][212][SBFD] Running CR for 38.331 (Huawei)

Intended outcome: Updated running CR based on new agreements for endorsement, open issue list (if needed)

Deadline: Long

Companies are invited to provide feedback on open issue list by: **01 May 2025**

# Remaining open issues for specification RRC

**Open issue number RRC-1: RO indication by RRC signalling, MAC CE or PDCCH indication.**

**Issue description:** In RAN2#129 meeting, there is one FFS regarding the detailed signalling for the NT indicating the RO type for the case of CBRA.

* **For initial RA transmission, the network can indicate the RO type (legacy RO or additional RO) to the SBFD-aware UE for the case of CBRA. Detailed signalling is FFS.**

According to [18], there can be several options which can be compared from the aspects of how dynamic the NT intends this signalling to be, the signalling overhead and the availability of the signalling to the SBFD-aware UEs.

* Option 1) RRC signaling, e.g., additional field in *RACH-ConfigCommon* IE to indicate RO type;
* Option 2) MAC CE using broadcast RNTI; or
* Option 3) PDCCH indication (e.g., DCI scrambled with P-RNTI, similar to time domain PRACH adaptation discussed in NES WI)

Rapporteurs understands that the proponent is open to each option and there are no discussion on this siganlling design from other companies. It is proposed to discuss and try to converge to one option in this email discussion. If there is majority view then no need for contributions for the May meeting.

**Proposed resolution: Discuss and converge to one signalling design option.**

**Proposal : To select one option for RO type indication signalling:**

- **Option 1) RRC signaling, e.g., additional field in RACH-ConfigCommon IE to indicate RO type;**

**- Option 2) MAC CE using broadcast RNTI; or**

**- Option 3) PDCCH indication (e.g., DCI scrambled with P-RNTI, similar to time domain PRACH adaptation discussed in NES WI)**

(only for cases as described above) Companies are invited to provide feedback regarding the above open issue and proposed resolution:

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree to which option?** | **Other comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

[**Summary**]

**Open issue number RRC-2:**

**Issue description:** In RAN2#129-bis meeting, there is one FFS regarding triggering events in SBFD resource.

* **Random access procedure in SBFD symbols is supported for all the existing RACH trigger events except for SI request. FFS for LTM.**

As there was no much discussion about the RACH procedure triggered by the event of ” Early UL synchronization with an LTM candidate cell” and ”RACH-based LTM cell switch” (both are LTM related), it is suggested that companies can discuss whether ” Early UL synchronization with an LTM candidate cell” and/or ”RACH-based LTM” can be supported in symbols in their contributions for May meeting, and if supported, what is the impact on RRC spec (especially for Early UL synchronization case). Rapporteur intends to discuss only the RRC impact here.

**Proposed resolution: Companies discuss whether ” Early UL synchronization with an LTM candidate cell” and/or ”RACH-based LTM” can be supported in symbols in their contributions.**

**Proposal: If RACH triggering event “Early UL sync with an LTM candidate cell” is supported in SBFD symbols, the RO type is indicated in *EarlyUL-SyncConfig*. [2]**

Companies are invited to provide feedback regarding the above open issue and proposed resolution:

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree to proposal?** | **Other comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**[Summary]**

**Open issue number RRC-3:**

In last meeting, RAN2 agrees to support RO-Type change from legacy RO to additional RO in SBFD symbols and assume the threshold is the same with the fallback from additional RO to legacy RO.

* **Issue description: RO-Type change procedure on RO type selection from legacy RO to additional RO in SBFD symbols is supported when the number of PRACH transmission attempts exceed a threshold (we assume it is the same threshold with the fallback from additional RO to legacy RO). If fallback from legacy RO to additional RO occurs, no further fallback to legacy RO is supported.**

The NT indicates this threshold/maximum preamble transmission number to the UE. The possible values for this number needs to be decided.

Rapporteur suggests to solve this signaling issue in this email discussion, no contributions for May meeting are needed for this simple issue.

**Proposed resolution: Decide the preamble transmission number range based on the majority view in this email discussion.**

**Proposal: To choose between:**

**Option 1: {n1, n2, n4, n6, n8, n10, n20, n50, n100, n200}. (same as for *msgA-TransMax* and)** ***preambleTransMax-Msg1-Repetition*)**

**Option 2: {n3, n4, n5, n6, n7, n8, n10, n20, n50, n100, n200}, (same as for *preambleTransMax*).**

Companies are invited to provide feedback regarding the above open issue and proposed resolution:

|  |  |  |
| --- | --- | --- |
| **Company** | **Option** | **Other comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**[Summary]**

**Open issue number RRC-4:**

According to [25] and [30], RAN2 can confirm that the CSI-RS resource configured for a L3 measurement can be in both DL subband of SBFD symbols and non-SBFD DL symbols, and the separate Layer 3 measurement report for CSI-RS resources in SBFD symbol is not supported. [27] has the opposite proposal that to support the separate Layer3 measurement report for CSI-RS resources in SBFD symbol.

Rapporteur understands both sides expect no or minor RRC spec impact and suggests to try to discuss/agree on one way forward and especially on the spec impact. Rapporteur encourages compromise if there is no critical difference between these two approaches.

**Proposed resolution: Try to agree on one way forward, no need for meeting contributions if compromise can be reached.**

**Proposal: RAN2 to select between:**

**Option 1 : The separate Layer 3 measurement report for CSI-RS resources in SBFD symbol is not supported, no RRC spec impact is expected.**

**Option 2: Support the separate Layer3 measurement report for CSI-RS resources in SBFD symbol, please input on the RRC spec impact.**

Companies are invited to provide feedback regarding the above open issue and proposed resolution:

|  |  |  |
| --- | --- | --- |
| **Company** | **Option** | **Other comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**[Summary]**

# Other identified open issues

Companies are invited to describe any other identified open issues not currently included within this document. Further open issues can also be added as well during RRC running CR (including RAN1 higher layer parameter list implementation) review.

|  |  |
| --- | --- |
| **Company** | **Other identified open issues? (please describe)** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

**[Summary]**

# Conclusions

The following proposals have been provided based on feedback to the above document:

[Proposals for easy agreement]

[Proposals for discussion]

# References

1. R2-2501797 Discussion on RACH in SBFD Xiaomi
2. R2-2501849 Random Access in SBFD symbols CATT
3. R2-2501860 Random Access for SBFD Operation NEC
4. R2-2501878 Impacts on the random access by the evolution of duplex operation Huawei, HiSilicon
5. R2-2501945 Discussion on Random Access in SBFD Sharp
6. R2-2502000 Random access in SBFD Samsung
7. R2-2502082 Discussion on random access procedure in SBFD ZTE Corporation
8. R2-2502316 Random Access Operation of SBFD Nokia Corporation
9. R2-2502387 Discussion on random access procedure in SBFD vivo
10. R2-2502394 Remaining issues of SBFD RACH procedure OPPO
11. R2-2502495 Random access for SBFD Operation Sony
12. R2-2502510 Remaining issues for RACH in SBFD Apple
13. R2-2502565 SBFD RA aspects Ericsson
14. R2-2502566 CSI-RS measurements and SBFD operation in CA and DC Ericsson
15. R2-2502588 Views on random access for SBFD Qualcomm Incorporated
16. R2-2502642 Discussion on Random Access operation in SBFD InterDigital, Inc.
17. R2-2502706 Discussion on random access in SBFD CMCC
18. R2-2502850 Discussion on Random Access procedure for SBFD LG Electronics Inc.
19. R2-2502967 Random Access in SBFD Lenovo
20. R2-2501850 Discussion on other aspects of SBFD CATT
21. R2-2501883 Other aspects of SBFD Xiaomi
22. R2-2502083 Discussion on multiple carrier and measurements in SBFD ZTE Corporation
23. R2-2502318 Other impacts by the evolution of duplex operation Huawei, HiSilicon
24. R2-2502388 SBFD other aspects vivo
25. R2-2502395 Discussion on the SBFD related measurement and BFR OPPO
26. R2-2502644 Discussion on resource configuration in SBFD InterDigital, Inc.
27. R2-2502801 Other Aspects of SBFD Samsung
28. R2-2502851 Other aspects on SBFD LG Electronics Inc.
29. R2-2502918 Other aspects of SBFD Nokia
30. R2-2502589 Other aspects of SBFD Qualcomm Incorporated discussion

# Appendix: Agreement of SBFD in RAN2:

# RAN2#127

## Random access in SBFD

* Working assumption: Random access procedure in SBFD symbols is supported for all the existing RACH trigger events.
* RAN2 assume RACH configuration for SBFD via SIB and/or dedicated RRC signalling is supported. Detailed signalling FFS.
* RAN2 to strive for a common SBFD CBRA framework independent of RRC state.
* FFS whether/how early indication is used during a SBFD RA procedure.
* RAN2 focus on 4-step RACH for SBFD RA, FFS on 2-step if needed.

## Other aspects

* Cell-specific SBFD time/frequency configuration is provided by SIB1 (or via dedicated signalling to covey cell specific configuration). FFS on UE specific dedicated RRC configuration if needed, pending on RAN1 progress.

# RAN2#127-bis

## Random access in SBFD

* RAN2 understand that if additional RO is selected by SBFD-aware UE, early identification via Msg1 is possible from NW point of view for this UE without specification impact.
* From R2 point of view, there is no need to introduce SBFD as a new feature combination in the current PRACH preamble partitioning framework.
* Upon initiation of CBRA RACH procedure for a SBFD-aware UE, UE selects one type of ROs between legacy-ROs and additional-ROs based on certain specified/configured conditions/prioritizations, if no additional indication (FFS if there needs to be any) is from network.
* For the PRACH transmission re-attempt in one RACH procedure, after certain (configured) number of times of RACH attempt in SBFD RACH occasions, UE is allowed to switch to legacy RACH occasions. FFS about the case when UE select legacy ROs first.
* The following two RACH configuration options are considered for SBFD based random access:
  + - Option 1: Use one single RACH configuration based on the existing parameters of the single RACH configuration. Can extend the existing parameters if needed.
    - Option 2: Use two separate RACH configurations, including one legacy RACH configuration and one additional RACH configuration
* For RACH configuration Option 2, RAN2 needs to specify RRC signalling for the new SBFD based RACH configuration with a new set of parameters.
* The RACH configuration for SBFD is transmitted via SIB1. FFS dedicated RRC signalling detail. FFS whether NW can provide both configurations.

## Other aspects

* For UL resource muting for PUSCH, the configuration of time and frequency location for UL resource muting should be introduced based on R1 agreement.
* For L1 based UE-to-UE CLI measurement mechanism, the configuration of periodic, semi-persistent or aperiodic UE-to-UE CLI measurement resource (set) should be introduced based on R1 agreement.
* For L1 based UE-to-UE CLI reporting mechanism, the configuration of report quantities should be introduced based on R1 agreement.

# RAN2#128

## Random access in SBFD

CFRA

* The RO type is indicated by NW for CFRA. FFS on signaling (can FFS for the SI request case if needed).

CBRA

* FFS on the following options

**Option 1**

**Upon initiation of RACH procedure for a SBFD-aware UE, network provides the indication on the prioritization of the additional ROs over legacy RO.**

**If there is no such indication from the NW, FFS on the following mechanism**

* **UE select legacy RO or SBFD RO based on SSB RSRP, or**
* **UE select the legacy RO, or**
* **UE select the SBFD RO, or**
* **Other metrics than SSB RSRP.**

**Option 2**

**UE select legacy RO or SBFD RO based on SSB RSRP if such condition is configured, and if not configured, then UE can prioritize one type of the ROs, FFS which one.**

RACH configuration

* Only one RACH configuration option (i.e., either RACH configuration Option 1 with Alt 1-1 or RACH configuration Option 2) is supported in a cell.

## Other aspects

* Prioritization of SBFD cells / frequencies during cell reselection is not considered.
* RAN2 wait for input from the other WGs regarding whether for inter-cell CSI-RS measurements, UE needs to be provided with information of the SBFD configuration of neighbouring cells.

# RAN2#129

## Random access in SBFD

RACH configuration

* **When a SBFD aware UE supporting one or both SBFD RACH configuration options accesses a cell, the UE can apply the supported SBFD RACH configuration option in the cell.**
* **When a SBFD aware UE supporting a SBFD RACH configuration option accesses a cell configured with a different SBFD RACH configuration option, the UE applies the legacy RA operation, and does not apply the SBFD RACH configuration.**

RACH procedure, RO selection criteria

* **For initial RA transmission, the network can indicate the RO type (legacy RO or additional RO) to the SBFD-aware UE for the case of CBRA. Detailed signalling is FFS.**
* **If no RO type indication is provided by the NW, a UE selects RO type based on a SSB RSRP threshold. FFS whether NW can further indicate whether to select the additional RO type below or above this SSB RSRP threshold.**

RACH procedure, RO selection before or after selecting a set of RA resources

* **FFS whether RO type selection is performed before or after the RA type selection.**

RACH procedure, fallback behaviour

* **FFS if switching from the PRACH resources in non-SBFD symbols to the PRACH resources in SBFD symbols is supported.**

## Other aspects

* **A new SP CLI measurement resource set activation/deactivation MAC CE is introduced to activate/deactivate the SP CLI measurement resource.**

# RAN2#129-bis

## Random access in SBFD

Output of email discussion [Post129][217]

* **On RO type signaling for CFRA**

**1. For CFRA triggered by BFR, the RO type is indicated in BeamFailureRecoveryConfig.**

**2. For CFRA triggered by ReconfigurationwithSync, the RO type is indicated in RACH-ConfigDedicated.**

* **When both NW indication on RO type and RSRP threshold are absent, it is up to UE implementation to select the RO type.**
* **Random access procedure in SBFD symbols is supported for all the existing RACH trigger events except for SI request. FFS for LTM.**

On RSRP threshold for RO type selection (e.g., configuration, related procedure, etc.)

* **NW indicate via explicit signaling whether the SBFD RO is selected when SSB RSRP are 'below' or 'above' the configured threshold.**

RO type selection before or after RA type selection

* **Working assumption: For SBFD-aware UE, the selection of RO type is suggested to be performed before the selection of the set of Random Access resources.**

On RO type fallback

* **RO-Type change procedure on RO type selection from legacy RO to additional RO in SBFD symbols is supported when the number of PRACH transmission attempts exceed a threshold (we assume it is the same threshold with the fallback from additional RO to legacy RO). If fallback from legacy RO to additional RO occurs, no further fallback to legacy RO is supported.**

## Other aspects

SBFD in DC

* **Send an LS to RAN1 (CC RAN3 and RAN4) on whether SBFD and DC can be configured simultaneously, and whether there is any issue for such configuration.**

MAC CE design SP CLI Measurement Resource Set Activation/Deactivation

* **Working assumption: The configured SP CLI measurement resource sets are initially deactivated upon (re-) configuration by upper layers and after reconfiguration with sync.**
* **SP CLI measurement resource set activation/deactivation MAC CE includes following fields: A/D, Serving Cell ID, BWP ID, CLI measurement resource set ID (for CLI-RSSI or SRS-RSRP measurement), TCI State IDs.**