|  |  |  |  |
| --- | --- | --- | --- |
| **Company** | **Section/clause/IE** | **Comments/Suggested Change** | **Rapp Response** |
| ZTE | BeamFailureRecoveryConfig | ra-OccasionType-r19 can only indicate SBFD. If gNB indicates non-SBFD RO, gNB can make the field absent. |  |
| ZTE | sbfd-RACH-SingleConfig-r19 | Option 1 should be indicated per RACH-ConfigCommon?  Option 1 and option 2 cannot be configured together for all the RACH-ConfigCommon (including those in the AdditionalRACH-ConfigList-r17), this condition should be added. |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |