|  |  |  |  |
| --- | --- | --- | --- |
| **Company** | **Section/clause/IE** | **Comments/Suggested Change** | **Rapp Response** |
| ZTE | BeamFailureRecoveryConfig | ra-OccasionType-r19 can only indicate SBFD. If gNB indicates non-SBFD RO, gNB can make the field absent. |  |
| ZTE | sbfd-RACH-SingleConfig-r19 | Option 1 should be indicated per RACH-ConfigCommon?  Option 1 and option 2 cannot be configured together for all the RACH-ConfigCommon (including those in the AdditionalRACH-ConfigList-r17), this condition should be added. |  |
| Nokia | sbfd-RACH-SingleConfig-r19 | Same understanding as ZTE |  |
| Nokia | CSI-ReportConfig | The metrics cli-RSSI and cli-SRS-RSRP are not included as part of new reporting metrics within *CSI-ReportConfig* IE. |  |
| Nokia | CSI-ResourceConfig | The definition of the *CSI-ResourceConfig* IE should be updated to indicate that it is also used to define a group of CLI-RSSI or SRS-RSRP resource sets. |  |
| Nokia | CSI-ReportConfig | The definition of *resourcesForChannelMeasurement* should be extended to cover CLI-RSSI and SRS-RSRP resources |  |
| Xiaomi | ASN.1 grammar: there are several places where commas are placed before “]]”. For example:  OPTIONAL, -- Need M  ]] | Remove comma before “]]”. |  |
| Xiaomi | Naming convention is not followed for several field or IE names. | Understand the names might be based on RAN1 parameter list, but proper name should be used in 38.331.  The examples of name corrections:  RACH-configConmonSBFD-r19 🡪 RACH-ConfigConmonSBFD-r19  sbfd-rsrp-ThresholdRO-Type-r19 🡪 sbfd-RSRP-ThresholdRO-Type-r19  … |  |
| Xiaomi | sbfd-RACH-SingleConfig-r19 | In RAN1 parameter list R1-2503155, the IE location (column “Per (UE, cell, TRP, …)”) is empty with yellow background. Not sure whether RAN1 will further update it. Maybe we can have an Editor’s note about the IE location. |  |
| Xiaomi | Relationship between sbfd-RACH-SingleConfig-r19 and sbfd-RACH-DualConfig-r19 | Similar comment as ZTE for sbfd-RACH-SingleConfig-r19.  In RAN1#117 meeting, RAN1 agreed that “Enabling both options at the same time for a UE is not supported”. Suggest to capture the restriction in field description or condition. |  |