3GPP TSG-RAN WG2 #131 R2-250xxxx

**Bengaluru, India, 25-29 August 2025**

**Agenda item:**8.18 (LTE-based 5G Broadcast)

**Source:** Samsung

**Title:** Discussion of [POST130][511][LTE Broadcast] MAC running CR and open issues (Samsung)

**Document for:** Report

# 1. Introduction

This document summarizes the discussion of the following offline discussion.

* [POST130][511][LTE Broadcast] MAC running CR and open issues (Samsung)

 Scope:

* Prepare and review the CR
* List open issues related to the CR

 Intended outcome:

* Running CR for endorsement in the next meeting
* List of open issues for discussion at the next meeting

 Deadline: 01 Aug 2025, 10:00 UTC

Note: Please provide your comments to the MAC CR in this document only (i.e. no bubble comments and no direct changes to the CR)

# 2. Contact information

|  |  |  |
| --- | --- | --- |
| Company | Name  | E-mail |
| Samsung | Vinay Kumar Shrivastava  | shrivastava@samsung.com |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# 3. Review of MAC running CR

* 1. Comments to the MAC running CR v00

**Companies are invited to list their comments on the CR v00, using comment identifier (company ID and number), e.g. SS001. The rapporteur will provide update based on the comments in proper time.**

|  |  |  |  |
| --- | --- | --- | --- |
| Comment identifier | Clause | Comments and/or change suggestions | Rapporteur resolution |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

* 1. Comments to the MAC running CR v01

**Based on companies’ comments in section 3, an updated CR version could be provided by Rapporteur for further review.**

**TBD**

# 4. Discussion on open issues

* 1. Open issue list

**Rapporteur provides the list of open issues as below, and the corresponding suggestions on how to address them. Some of them could be further discussed based on contributions or resolved based on further progress. Companies are invited to provide comments on whether it is open issue and whether the suggestions from rapporteur is accurate enough.**

* + 1. HARQ handling for Time-Interleaved MCH reception

RAN1 made the below agreement in RAN1#121 about the HARQ for time interleaved MCH and sent a LS to RAN2 [2]

|  |
| --- |
| **Agreement****RAN1 asks RAN2 whether/how to address the HARQ handling in the MAC specification for the Rel-19 time-interleaved PMCH transmission with M TBs and N RVs.** |

Time interleaving enhancements for LTE-based 5G Broadcast are based on the reuse of the 3GPP building block behind the HARQ retransmission and combining, which allows spreading the coded bits of a transport block across multiple non-consecutive subframes [RP-242534]. RAN1 discussed the matter and reached the above agreement, and a LS is sent to RAN2 given the HARQ handling is described in MAC specs.



**Fig. 1 Time interleaved MCH [RP-242534]**

In Rapp’s view, similar mechanisms for the HARQ handling have been addressed in MAC specs for SIB reception (TS 36.321, TS 38.321) and NR MBS Broadcast reception (TS 38.321) and it is straight-forward to inherit the approach for time interleaved MCH reception. Accordingly, the two spec changes (Change#1 and Change#2) as required in TS 36.321 to address HARQ handling for M transport blocks and N redundancy versions corresponding to the time interleaved MCH reception should be considered.

**Excerpt from TS 38.321: SIB reception and MR MBS Broadcast reception**

|  |
| --- |
| 5.3.2.2 HARQ process…For each received TB and associated HARQ information, the HARQ process shall:1> if the NDI, when provided, has been toggled compared to the value of the previous received transmission corresponding to this TB; or1> if the HARQ process is equal to the broadcast process, and this is the first received transmission for the TB according to the system information schedule indicated by RRC; or1> if the HARQ process is associated with a transmission indicated with a MCCH-RNTI for MBS broadcast, and this is the first received transmission for the TB according to the broadcast MCCH schedule indicated by RRC; or1> if the HARQ process is associated with a transmission indicated with a Multicast MCCH-RNTI for MBS multicast in RRC\_INACTIVE, and this is the first received transmission for the TB according to the multicast MCCH schedule indicated by RRC; or1> if the HARQ process is associated with a transmission indicated with a G-RNTI for MBS broadcast, and this is the first received transmission for the TB according to the MTCH schedule indicated by RRC or according to the scheduling indicated by DCI as specified in TS 38.214 [7]; or1> if this is the very first received transmission for this TB (i.e. there is no previous NDI for this TB):2> consider this transmission to be a new transmission.1> else:2> consider this transmission to be a retransmission.The MAC entity then shall:1> if this is a new transmission:2> attempt to decode the received data.1> else if this is a retransmission:2> if the data for this TB has not yet been successfully decoded:3> instruct the physical layer to combine the received data with the data currently in the soft buffer for this TB and attempt to decode the combined data.1> if the data which the MAC entity attempted to decode was successfully decoded for this TB; or1> if the data for this TB was successfully decoded before:2> if the HARQ process is equal to the broadcast process:3> deliver the decoded MAC PDU to upper layers.2> else if this is the first successful decoding of the data for this TB:3> deliver the decoded MAC PDU to the disassembly and demultiplexing entity.1> else:2> instruct the physical layer to replace the data in the soft buffer for this TB with the data which the MAC entity attempted to decode.1> if the HARQ process is associated with a transmission indicated with a Temporary C-RNTI and the Contention Resolution is not yet successful (see clause 5.1.5); or1> if the HARQ process is associated with a transmission indicated with a MSGB-RNTI and the Random Access procedure is not yet successfully completed (see clause 5.1.4a); or1> if the HARQ process is equal to the broadcast process; or1> if the HARQ process is associated with a transmission indicated with a MCCH-RNTI or a G-RNTI for MBS broadcast; or1> if the HARQ process is associated with a transmission indicated with a Multicast MCCH-RNTI for MBS multicast; or1> if the HARQ process is associated with a transmission indicated with a G-RNTI or a G-CS-RNTI or a configured downlink assignment for MBS multicast and HARQ feedback is disabled for this G-RNTI or G-CS-RNTI or the corresponding G-CS-RNTI, as specified in clause 18 of TS 38.213 [6]; or1> if the HARQ process is associated with a transmission indicated with a G-RNTI or a G-CS-RNTI or a configured downlink assignment for MBS multicast and NACK only HARQ feedback is used for this G-RNTI or G-CS-RNTI or the corresponding G-CS-RNTI and the data for this TB is successfully decoded and the transmission is not the first transmission of PDSCH where the configured downlink assignment was (re-)initialised; or1> if the *timeAlignmentTimer*, associated with the TAG containing the Serving Cell on which the HARQ feedback is to be transmitted, is stopped or expired, and the Serving Cell is not configured with two TAGs, and if the *cg-SDT-TimeAlignmentTimer*, if configured, is not running; or1> if the Serving Cell on which the HARQ feedback is to be transmitted is configured with two TAGs and if the *timeAlignmentTimer* of the TAG, associated with the TCI state(s) used for transmitting the HARQ feedback, is stopped or expired:2> not instruct the physical layer to generate acknowledgement(s) of the data in this TB. |

**Change#1: HARQ applicability for MTCH corresponding to time interleaved MCH**

|  |
| --- |
| 4.2.1 MAC Entities…Figure 4.2.1-1: MAC structure overview, UE side |

**Change#2: TB decoding and soft combining**

|  |
| --- |
| 5.12a Time interleaved MCH receptionTime interleaved MCH transmission may occur in subframes configured by upper layer for MTCH transmission. For each such subframe, *dataMCS* applies. The transmission of an MCH occurs in a set of subframes defined by *PMCH-Config*. An MCH Scheduling Information MAC control element is included in the first subframe allocated to the MCH within the MCH scheduling period to indicate the position of each MTCH and unused subframes on the MCH. The MAC entity shall assume that the first scheduled MTCH starts at the earliest in the next subframe after the subframe containing the MCCH and/or the MCH Scheduling Information MAC control element, and the other scheduled MTCH(s) start immediately after the previous MTCH, at the earliest in the next subframe (which is not containing MCCH) after the subframe where the previous MTCH stops. Unused part of the subframe, if any, is filled with padding. When the MAC entity needs to receive MCH, the MAC entity shall:- if the HARQ process is associated with a transmission indicated with a M-RNTI for time interleaved MCH: - if this is the first received transmission for the TB according to the MTCH schedule indicated by MSI:- attempt to decode the received data.- else:- if the data for this TB has not yet been successfully decoded:- combine the received data with the data currently in the soft buffer for this TB and attempt to decode the combined data.- if the data which the MAC entity attempted to decode was successfully decoded for this TB; or- if the data for this TB was successfully decoded before:- deliver the decoded MAC PDU to upper layers.- else:- replace the data in the soft buffer for this TB with the data which the MAC entity attempted to decode.- do not indicate the positive or negative acknowledgement to the physical layer.NOTE: The MAC entity should continue receiving MCH until the MTCH is removed from the MCCH. |

**Q1. Are Change#1 and Change#2 appropriately address the HARQ handling for time interleaved MCH in the MAC spec? Provide your comments and suggest changes, if any.**

|  |  |
| --- | --- |
| **Company** | **Comments, if any** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

* 1. Others, please specify

**Companies are invited to describe any other identified open issues not currently included within this document.**

|  |  |
| --- | --- |
| **Company** | **Any other identified open issues? (please describe) or other comments** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# 5. Conclusion

In this contribution, we collected the open issues for LTE-based 5G Broadcast enhancements in MAC. Based on the discussion, the following proposals have been achieved:

**TBD**

# 6. References

1. RAN2#130 Meeting report
2. R2-2504963 (R1-2504922): LS on RAN2 aspects for LTE-based 5G Broadcast Phase 2
3. RP-250238: (RAN#107) Status report for WI LTE-based 5G Broadcast Phase 2
4. RP-251143: (RAN#108) Status report for WI LTE-based 5G Broadcast Phase 2