|  |  |  |  |
| --- | --- | --- | --- |
| **Company** | **Section/clause/IE** | **Comments/Suggested Change** | **Rapp Response** |
| ZTE | BeamFailureRecoveryConfig | ra-OccasionType-r19 can only indicate SBFD. If gNB indicates non-SBFD RO, gNB can make the field absent. | This may be different taste of design. The actual bit is the same (one bit). Rapp think explicit signaling is clearer than implicit signalling (by absence), open for more views from companies. |
| ZTE | sbfd-RACH-SingleConfig-r19 | Option 1 should be indicated per RACH-ConfigCommon?  Option 1 and option 2 cannot be configured together for all the RACH-ConfigCommon (including those in the AdditionalRACH-ConfigList-r17), this condition should be added. | For the first question, yes, the R19 gNB configures Option1 through RACH-ConfigCommon.  For the second question, it is already stated in 300 running CR that “A cell can configure only one RACH configuration option”. Rapp thinks no need to duplicate this restriction in FD. Open to add if majority companies want to add. |
| Nokia | sbfd-RACH-SingleConfig-r19 | Same understanding as ZTE | See above |
| Nokia | CSI-ReportConfig | The metrics cli-RSSI and cli-SRS-RSRP are not included as part of new reporting metrics within *CSI-ReportConfig* IE. | Rapp understands the report quantity is the same as in legacy. |
| Nokia | CSI-ResourceConfig | The definition of the *CSI-ResourceConfig* IE should be updated to indicate that it is also used to define a group of CLI-RSSI or SRS-RSRP resource sets. | Yes. Thanks for spotting this. Will add in the next version. |
| Nokia | CSI-ReportConfig | The definition of *resourcesForChannelMeasurement* should be extended to cover CLI-RSSI and SRS-RSRP resources | The new field resourcesForChannelCLI covers CLI-RSSI and SRS-RSRP resources. |
| Xiaomi | ASN.1 grammar: there are several places where commas are placed before “]]”. For example:  OPTIONAL, -- Need M  ]] | Remove comma before “]]”. | Thanks for spotting this. Two such cases with “rach-ConfigConmonSBFD-r19” to be corrected in the next version. |
| Xiaomi | Naming convention is not followed for several field or IE names. | Understand the names might be based on RAN1 parameter list, but proper name should be used in 38.331.  The examples of name corrections:  RACH-configConmonSBFD-r19 🡪 RACH-ConfigConmonSBFD-r19  sbfd-rsrp-ThresholdRO-Type-r19 🡪 sbfd-RSRP-ThresholdRO-Type-r19  … | Thanks. -rsrp- to be changed to -RSRP-, -config to be changed to -Config. in next version.  Also Conmon to be changed to Common. |
| Xiaomi | sbfd-RACH-SingleConfig-r19 | In RAN1 parameter list R1-2503155, the IE location (column “Per (UE, cell, TRP, …)”) is empty with yellow background. Not sure whether RAN1 will further update it. Maybe we can have an Editor’s note about the IE location. | Will add EN for this in next version. |
| Xiaomi | Relationship between sbfd-RACH-SingleConfig-r19 and sbfd-RACH-DualConfig-r19 | Similar comment as ZTE for sbfd-RACH-SingleConfig-r19.  In RAN1#117 meeting, RAN1 agreed that “Enabling both options at the same time for a UE is not supported”. Suggest to capture the restriction in field description or condition. | See response above. |
| LGE001 | - | Remove unchanged IE and clauses.  Given that RRC spec is large-sized, it is really hard to review unless the running RRC CR only includes essential part. | Rapp started from the full 331 as not clear which sections will be changed.  Indeed it is big and easily freezes in Print Layout mode. One workaround is change to ”Draft mode” immediately after opening the word file then no repagination/freezing issues. |
| LGE002 | sbfd-rsrp-ThresholdMsg1-RepetitionNum2/4/8 IE in RACH-configConmonSBFD | According to RAN1 parameter list, the separated RSRP threshold to determine Msg1 repetition number for SBFD RO is configured for each BWP, not for each RACH partition.  Given that legacy RSRP threshold to determine Msg1 repetition number in legacy RO is configured within BWP-UplinkCommon IE, this separated RSRP threshold should be configured in the same place, i.e., directly within BWP-UplinkCommon IE. There is no need to further configure these thresholds in AdditionalRACH-Config IE.  Suggestion: move sbfd-rsrp-ThresholdMsg1-RepetitionNum2/4/8 to directly in BWP-UplinkCommon IE and remove these from RACH-ConfigCommonSBFD IE. | Indeed those three thresholds are generic parameters, shall be listed together with the legacy thresholds. To be revised in the next version. |
| LGE003 | *sbfd-RACH-SingleConfig* | We may need to further discuss whether the this indication (i.e., indicating whether RACH configuration Option 1 for SBFD random access operation is enabled or not from network side) should be configured for each Cell/BWP or for each RACH configuration). We are okay for companies’ view but given that there is no explicit discussion on this, propose to add an EN to further discuss. | Add one EN on this |
| LGE004 | *sbfd-RACH-SingleConfig* and *sbfd-RACH-DualConfig* in BWP*-UplinkCommon* IE | Similar comment as ZTE.  In RAN2#128 meeting, it is agreed that only one RACH configuration option is supported in a cell:   * Only one RACH configuration option (i.e., either RACH configuration Option 1 with Alt 1-1 or RACH configuration Option 2) is supported in a cell.   Therefore, some network restriction to allow only one RACH configuration option in a cell should be specified, e.g., in field description or in conditional presence. | See response on this comment above. |
| LGE005 | ra-OccasionType in *BeamFailureRecoveryConfig* | In our understanding, this indication is intended to indicate RO type in **CFRA** case:   * **For CFRA** triggered by BFR, the RO type is indicated in BeamFailureRecoveryConfig.   However, in BFR config, it is possible that CFRA resource is not included, while RA prioritization parameter (e.g., ra-Prioritization IE or ra-PrioritizationTwoStep IE) is included in the BFR config. In this case, even though the RA is initiated for Beam failure recovery, CBRA is performed due to no CFRA resource in BFR config. Note that it is different fallback from CFRA to CBRA, which is caused by low channel quality even though CFRA resource is configured for BFR.  In this sense, in order to avoid any confusion on whether the RO type can indicated without CFRA resource configuration, suggest to change the field description of ra-OccasionType-19 as follows:  Indicates the RACH occasion type for CFRA, SBFD or non-SBFD, to be used a SBFD capable UE. | Add “for CFRA” in the next version. |
| LGE006 | ra-OccasionType in *RACH-ConfigDedicated* | Similar comment in LGE005. It should be clarified that this field indicates RO type for **CFRA** cases. Suggest to change the field description of ra-OccasionType-19 as follows:  Indicates the RACH occasion type for CFRA, SBFD or non-SBFD, to be used a SBFD capable UE. | Same as above |
| LGE007 | SchedulingRequestResourceConfigExt-v19xy | SchedulingRequestResourceConfigExt-v19xy is defined, but it is never be used. Similar to other SchedulingRequestResourceConfigExt-v1610/v1700, following configuration may be needed under PUCCH-Config IE, as an optional field:   * schedulingRequestResourceToAddModListExt-v19xy SEQUENCE (SIZE (1..maxNrofSR-Resources)) OF SchedulingRequestResourceConfigExt-v19xy | Thanks for the suggestion, will adopt in the next version. |
| LGE008 | PUCCH-CSI-ResourceExt-v19xy | Similar as LGE007, PUCCH-CSI-ResourceExt-v19xy is never used. Further discussion may be needed on how to configure symbol type for each PUCCH-CSI-Resource, based on RAN1 parameter list. | Add one line with a new field pucch-CSI-ResourceListExt-r19: pucch-CSI-ResourceListExt-r19 SEQUENCE (SIZE (1..maxNrofBWPs)) OF PUCCH-CSI-ResourceExt-v19xy. And one EN on this revision. |
| LGE009 | SCS-SpecificCarrier | Typo: close the square bracket, i.e., ‘]]’ is missing at the end of SCS-SpecificCarrier IE. | Good catch! |
| CMCC | BWP-UplinkCommon | Within table of BWP-UplinkCommon field descriptions, we think that the last sentence of additionalRACH-ConfigList should be revised to “If at least two of rach-ConfigCommon, msgA-ConfigCommon and rach-ConfigCommonSBFD are configured for a specific FeatureCombination, the network always provides them in the same additionalRACH-Config.”. | Rapp thinks this sentence might need further consideration. First, msgA-ConfigCommon will not be present with rach-ConfigCommonSBFD at the same time (SBFD not supported with SBFD). Second, SBFD is not a feature and two same rach-ConfigCommonSBFD are placed as one with rach-ConfigCommon and another within AdditionalRACH-Config-r17. |
| Nokia | BWP-{Downlink,Uplink}Dedicated | On the description of *sbfd-Configuration2-{Reception,Transmission}*, RAN1 specifications specify the behaviour when *sbfd-Configuration2-{Reception, Transmission}* is provided, and do not refer to a ‘configuration 1’ in any case. We think the sentence in the description ‘If not enabled, Configuration 1 is applied for xxx in the given DL BWP’ can be removed | RAN1 explicitly states “If not enabled…” in their FD. Will keep both for clarity (also the need code is Need S now, so specification is needed when this field is not configured/enabled. ) |
| Nokia | ConfiguredGrantConfig, SchedulingRequestResourceConfig, etc.. | Same reasoning as earlier: ‘for SBFD Configuration 1’ can be removed from the description of *symbolType*. It is clear from the second sentence that this is only configured when Configuration 2 is not enabled. | Unless there is strong motivation to remove (error, dupicated texts etc.), Rapp prefers to follow RAN1 FD in their list at least for now. |
| ERI1 | BeamFailureRecoveryConfig | We agree with ZTE very first comment.  Additionally, we typically do not state that certain field is for UE that support certain feature.  We should also avoid “SBFD capable” but instead use “SDFB-aware”, we think this is preferred is in RAN1. This is a general comment, there are some “SBFD capable” in the CR. | On ZTE first comment, since there are multiple support from other companies, the explicit signaling of non-SBFD RO will be removed (also from RACH-ConfigDedicated), i.e. to use implicit signaling via absence of ”SBFD RO type”, in next version of running CR.  Regarding ”SBFD aware” vs. ”SBFD capable”: will add one EN on this term that a unified solution can be used across specs. |
| ERI2 | sbfd-RACH-SsingleConfig-preambleReceivedTargetPower | Field description refers to SBFD RACH Configuration option 1. I do not expect RAN1 spec will clarify these options, we should consider clarify them in 38331, if we at all need them. | There are reminder clause X, clause Y, we can wait for RAN1 spec. This FD is following RAN1 higher layer parameter list, if we want to “clarify them” in 331, the optimal way is to ask RAN1 first. |
| ERI3 | sbfd-Configuration2-Transmission-r19 | General, can use “Config” instead of “Configuration” (many places).  Also, we do not need the word “Transmission”, since this is obvious from an UL BWP?  (Same comments for sbfd-Configuration2-Reception-r19).  If this field is configured always together with next field sbfd-Configuration2-PUSCH-RBOffset-r19, then this can be expressed in ASN.1? | On config vs configuration: Rapp prefer to follow the naming from RAN1 parameter list however will change it to “config” as it is quite long to use “configuration”.  Any suggestion on ASN.1? |
| ERI4 | Gen | In many field descriptions CR uses text similar to “The network does not configure this field if SBFD Configuration 2 is enabled for the UL BWP. (see TS 38.214 [19], clause 7.2)”.  Normally, we prefer to use the field name by wich the feature is enabled.  Question: Is same Config used in both UL and DL? | The FDs are copied from RAN1 parameter list.  Any suggestion on how o optimize on the naming?  The FD and config are based on RAN1 list, so better check with RAN1 on the question.  Is this UL/DL question related to CATT006? |
| ERI5 | resourcesForChannelCLI | Not sure if covered by others, but this field description need more work. | Rapp highlighted FD for this field indicating optimization may be needed. There is no FD for this field from RAN1.  Add one EN for FFS |
| ERI6 | CSI-MeasConfig | (Editorial) Can use Meas instead of Measurement in field names of new fields, such that each definition occupies a single line. | Good suggestion: for all new field and IE, measurement->meas. |
| ERI7 | (General) | (Editorial: Can get cleaner CR by avoiding changes on changes, and by accepting the Word-generated comments for format changes.) | Will do before submission. |
| CATT001 | sbfd-Configuration2-Reception-r19 | sbfd-Configuration2Reception-r19 | As configuration->config, prefer keep this hyphen. |
| CATT002 | sbfd-RACH-DdualConfig-ValidROacrossSymbolTypes-r19 | sbfd-RACH-DdualConfig-ValidRO-acrossSymbolTypes-r19 | RO is capital, shall be no problem here. |
| CATT003 | RACH-ConfigCommonSBFD-r19 = SEQUENCE {  sbfd-RACH-SingleConfig-r19 ENUMERATED {enabled} OPTIONAL, -- Need R  sbfd-RACH-DualConfig-r19 SBFD-RACH-DualConfig-r19 OPTIONAL, -- Need R | RACH-ConfigCommonSBFD-r19 = SEQUENCE {  sbfd-RACH-ConfigCommon CHOICE {  sbfd-RACH-SingleConfig-r19 ENUMERATED {enabled} OPTIONAL, -- Need R  sbfd-RACH-DualConfig-r19 SBFD-RACH-DualConfig-r19 OPTIONAL, -- Need R  }, | Understand the motivation of CHOICE is that gNB only config one option at one cell. However sbfd-RACH-SingleConfig is not config option 1 but only the on/off indicator of config option 1. Also this indicator is optional with Need R, shall be fine as it is. |
| CATT004 | sbfd-RSRP-ThresholdMsg1-RepetitionNum2, sbfd-RSRP-ThresholdMsg1-RepetitionNum4, sbfd-RSRP-ThresholdMsg1-RepetitionNum8  Threshold used by the UE for determining whether to select resources indicating Msg1 repetition number 2, 4 or 8 within the additional-ROs. | There is no definition of additional-ROs in this spec. Additional description is required to align with the description of ***rsrp-ThresholdMsg1-RepetitionNum2.*** Please take the description in to consideration:  The value applies to RACH configurations in SBFD symbols. For a given MSG1 repetition number, ... It is absent otherwise. | The FD is following RAN1 list. We can discuss the FD by first checking with them.  Indeed “addition RO” is not defined, for now Rapp proposed to replace additional RO, additional-RO with SBFD ROs, companies are welcome to comment on this change. Another place for this change is “sbfd-RACH-SingleConfig-preambleReceivedTargetPower” |
| CATT005 | sbfd-RSRP-ThresholdRO-Type-r19 RSRP-Range OPTIONAL, -- Need R  sbfd-RSRP-ThresholdRO-TypeUsage-r19 ENUMERATED {above,below} OPTIONAL -- Need R | According to the agreement as below, RO type can be indicated directly to UE without threshold.   * **For initial RA transmission, the network can indicate the RO type (legacy RO or additional RO) to the SBFD-aware UE for the case of CBRA. Detailed signalling is FFS.** * **NW indicate via explicit signaling whether the SBFD RO is selected when SSB RSRP are 'below' or 'above' the configured threshold.** | The direct RO type indication signalling design is the RRC-01 in the RRC open issue discussion. Once P1 is agreed, will implement this RO type indication signalling in the running CR. |
| CATT006 | *BWP-UplinkDedicated* information element  sbfd-Configuration2-Transmission-r19  Indicates that the PDSCH receptions can be in SBFD symbols and non-SBFD symbols in different slots for the dedicated UL BWP (see TS 38.213 [13], clause x and TS 38.214 [19], clause y).If not enabled, Configuration 1 is applied for PUCCH and PUSCH transmissions in the given UL BWP.  sbfd-Configuration2-PUSCH-RBOffset-r19 | Should be:  sbfd-Configuration2Transmission-r19  Indicates that the PUCCH and PUSCH transmissions can be in SBFD symbols and non-SBFD symbols in different slots for the dedicated UL BWP (see TS 38.213 [13], clause x and TS 38.214 [19], clause y). If not enabled, Configuration 1 is applied for PUCCH and PUSCH transmissions in the given UL BWP.  Should be :  sbfd-Configuration2PUSCH-RB-Offset-r19 | Thanks for catching this copy/paste error.  On the hyphen, no strong opinion but will do no change for now. |
| CATT007 | *CLI-RSSI-MeasurementResource* information element  CLI-RSSI-MeasurementResourceSet-r19 ::= SEQUENCE {  cli-RSSI-MeasurementResourceId-r19 CLI-RSSI-MeasurementResourceId-r19 OPTIONAL, -- Need R  startSymbol-r19 INTEGER (0..13) OPTIONAL, -- Need R  nrofSymbols-r19 INTEGER (0..14) OPTIONAL, -- Need R  startPRB-r19 INTEGER (0..maxNrofPhysicalResourceBlocks-1) OPTIONAL, -- Need R  nrofPRBs-r19 INTEGER (1..maxNrofPhysicalResourceBlocks) OPTIONAL, -- Need R  cli-RSSI-PeriodicityAndOffset-r19 CSI-ReportPeriodicityAndOffset OPTIONAL, -- Need R  qclInfo-Periodic-CLI-RSSI-MeasurementResource-r19 TCI-StateId OPTIONAL, -- Need R  ...  } | CLI-RSSI-MeasurementResource~~Set~~-r19 ::= SEQUENCE {  cli-RSSI-MeasurementResourceId-r19 CLI-RSSI-MeasurementResourceId-r19 OPTIONAL, -- Need R  startSymbol-r19 INTEGER (0..13) OPTIONAL, -- Need R  nrofSymbols-r19 INTEGER (~~0~~1..14) OPTIONAL, -- Need R  startPRB-r19 INTEGER (0..maxNrofPhysicalResourceBlocks-1) OPTIONAL, -- Need R  nrofPRBs-r19 INTEGER (1..maxNrofPhysicalResourceBlocks) OPTIONAL, -- Need R  cli-RSSI-PeriodicityAndOffset-r19 CSI-ReportPeriodicityAndOffset OPTIONAL, -- Need R  qclInfo-Periodic-CLI-RSSI-MeasurementResource-r19 TCI-StateId  OPTIONAL, -- Need R  ...  } | Good catch, appreciated! |
| CATT008 | ***qclInfo-Periodic-CLI-RSSI-MeasurementResource***  Indicates a reference to one TCI-State in TCI-States for providing the QCL source and QCL type for a target periodic CLI-RSSI-MeasurementResource | Indicates ~~a~~the reference to one TCI-State in TCI-States for providing the QCL source and QCL type for ~~a~~the target periodic CLI-RSSI-MeasurementResource | Both “a” are following RAN1 list, can check with RAN1. |
| CATT009 | ***startSymbol***  Indicates starting symbol of the *CLI-RSSI-MeasurementResource* within a slot | Indicates the starting symbol of the *CLI-RSSI-MeasurementResource* within a slot | OK |
| CATT010 | *CLI-RSSI-MeasurementResourceSet* information element  cli-RSSI-MeasurementResourceIdList-r19 SEQUENCE (SIZE (1..maxNrofCLI-RSSI-MeasurementResourcesPerSet-r19) ) OF CLI-RSSI-MeasurementResourceSetId | cli-RSSI-MeasurementResourceIdList-r19 SEQUENCE (SIZE (1..maxNrofCLI-RSSI-MeasurementResourcesPerSet-r19) ) OF CLI-RSSI-MeasurementResource~~Set~~Id | Good catch. |
| CATT011 | *CSI-ResourceConfig* information element  cli-RSSI-MeasurementResourceSetList CHOICE { | cli-RSSI-MeasurementResourceSetList-r19 CHOICE { |  |
| CATT012 | *CSI-MeasConfig* information element  CLI-RSSI-MeasurementResourceList-r19 ::= SEQUENCE (SIZE (1..maxNrofCLI-RSSI-MeasurementResources-r19)) OF CLI-RSSI-MeasurementResource-r19  CLI-RSSI-MeasurementResourceSetList-r19 ::= SEQUENCE (SIZE (1..maxNrofCLI-RSSI-MeasurementResourceSets-r19)) OF CLI-RSSI-MeasurementResourceSet-r19  SRS-RSRP-MeasurementResourceList-r19 ::= SEQUENCE (SIZE (1..maxNrofSRS-RSRP-MeasurementResources-r19)) OF SRS-RSRP-MeasurementResource-r19  SRS-RSRP-MeasurementResourceSetList-r19 ::= SEQUENCE (SIZE (1..maxNrofSRS-RSRP-MeasurementResourceSets-r19)) OF SRS-RSRP-MeasurementResourceSet-r19 | These codes seems not necessary | Those are referred to by “cli-MeasResourceSetList” |
| CATT013 | *sbfd-Configuration2-PUSCH-RBoffset-r19* | sbfd-Configuration2PUSCH-RB-offset-r19 | Same response as above |
| CATT014 | ***resourcesForChannelCLI***  Configures CLI measurement resource set and the list of corresponding references to TCI-States. If the parameter *resourcesForChannelCLI* is configured, the following legacy parameters should not be configured or should be ignored:  *resourcesForChannel,*  *csi-IM-ResourcesForInterference,*  *nzp-CSI-RS-ResourcesForInterference,*  *resourcesForChannel2-r17,*  *resourcesForChannelTDCP-r18,*  *applyIndicatedTCI-State-r18,*  *csi-ReportSubConfigTriggerList-r18.* | -r17 or –r18 will be removed in Field description | Will follow RAN1 Note. Those suffix can be used if specific fields are referred to. |
| Samsung01 | General | The term “additional-ROs” or “SBFD RACH Occasion” should be aligned with RAN1 spec. Suggest to add EN or put under square bracket.  Better to unified the term, to avoid mixed use of “additional-RO” and “SBFD RACH occasion”. | Now all are SBFD ROs. Note “RO” is used in 331 for RACH occasion. |
| Samsung02 | RACH-ConfigCommonSBFD-r19 | The field (“preambleTransMaxRO-Type” in MAC running CR) for max number of preamble transmissions before RO type switching should be captured. | Will capture it after Proposal for RRC-3 is agreed. |
| Samsung03 | RACH-ConfigCommonSBFD-r19 | Explicit NW signalling of RO type for CBRA is not captured. | Will capture it after Proposal for RRC-1 is agreed. |
| Samsung04 | RACH-ConfigCommonSBFD-r19 | sbfd-RSRP-ThresholdRO-Type and sbfd-RSRP-ThresholdRO-TypeUsage should be present together. Can consider add restriction in field description or cond presence. | See above. Will capture it after Proposal for RRC-1 is agreed. |
| Samsung05 | CLI-RSSI-MeasurementResource | IE name of CLI-RSSI-MeasurementResource is captured as CLI-RSSI-MeasurementResource**Set**-r19. The “**Set**” should be removed here. |  |
| Samsung06 | CLI-RSSI-MeasurementResourceSet | cli-RSSI-MeasurementResourceIdList-r19 SEQUENCE (SIZE (1..maxNrofCLI-RSSI-MeasurementResourcesPerSet-r19) ) OF CLI-RSSI-MeasurementResource**~~Set~~**Id | Thanks, See response to CATT 007, 010 |
| Samsung07 | CSI-ReportConfig | We share same concern as Nokia, i.e., “The metrics cli-RSSI and cli-SRS-RSRP are not included as part of new reporting metrics within *CSI-ReportConfig* IE. ” considering the RAN1 agreement “For L1 UE-to-UE CLI measurement and reporting, support two additional report quantities {‘cli-RSSI’, ‘cli-SRS-RSRP’} to the higher layer parameter reportQuantity.”. Suggest to extend report quantity. | Add one EN on how to capture additional report quantities {‘cli-RSSI’, ‘cli-SRS-RSRP’} |
| Samsung08 | *ra-OccasionType* | “Indicates the RACH occasion type for CFRA, SBFD or non-SBFD, to be used **by** a SBFD capable UE.” | Corrected. |
| Charter | sbfd-Configuration2-Transmission-r19 | Agreed with Ericsson to use “Config” instead of Configuration and the word “Transmission” can be dropped as well. Just simply sbfd-Config2-r19. Same comment for the, just use Config. | Ok to use Config but will keep “Transmission” and “Reception” following RAN1 list. |
| Charter | sbfd-Configuration2-PUSCH-RBOffset-r19 | Same comment as above. |  |
| Charter | BeamFailureRecoveryConfig | Agreed with ZTE and Ericsson |  |
| Charter | sbfd-RSRP-ThresholdMsg1-RepetitionNum2, sbfd-RSRP-ThresholdMsg1-RepetitionNum4, sbfd-RSRP-ThresholdMsg1-RepetitionNum8  Threshold used by the UE for determining whether to select resources indicating Msg1 repetition number 2, 4 or 8 within the additional-ROs. | We share the same view as CATT, the definition of additional-ROs should be included in the description. | See the corresponding Rapp response. |
| LGE010 | sbfd-RSRP-ThresholdRO-Type and  sbfd-RSRP-ThresholdRO-TypeUsage | According to current MAC procedure, RO type is selected after the BWP operation and before the RACH partition selection. Therefore, unified RSRP threshold for RO type selection is sufficient for each BWP configuration, which is commonly applied for all RACH configuration within the BWP.  There is no need to define separated RSRP threshold for each RACH configuration, since RACH configuration is selected **after** the RO type selection.  Suggestion: move sbfd-RSRP-ThresholdRO-Type and  sbfd-RSRP-ThresholdRO-TypeUsage to directly in BWP-UplinkCommon IE. | Fine |
| Samsung09 | sbfd-RSRP-ThresholdRO-Type and  sbfd-RSRP-ThresholdRO-TypeUsage | Same suggestion as LGE010 above. |  |
| Rapp01 | Add one EN on how to capture additional report quantities {‘cli-RSSI’, ‘cli-SRS-RSRP’} |  | The additional report quantities {‘cli-RSSI’, ‘cli-SRS-RSRP’} are implemented in the latest version v05 and the related EN is removed.  Note, name “srs-rsrp” is used instead of “cli-SRS-RSRP” in order to reuse/not-to-change the corresponding procedure texts.  Similarly name “reportQuantityCLI” is used instead of “reportQuantity” in RAN1 list. |
| Rapp02 | Change-on-changes |  | In v05, The post 129bis changes are replaced to remove the change-on-changes. |
| Rapp03 |  |  | Editorial/format corrections |
| Rapp04 |  |  | Revise Rapp response to Samsung04 |
| The below changes and comments are post RAN2 130 | | | |
| Rapp05 |  | 1. Revise FD for sbfd-RACHDualConfig according to RAN1#121 agreement. 2. Adding RRC signaling to indicate (per BWP indication) RO type for CBRA sbfd-RO-Type according to meeting agreement. 3. revise FD/need code for sbfd-RSRP-ThresholdRO-TypeUsage according to meeting agreement. 4. move sbfd-RACH-SingleConfig-r19 to per BWP indication according to common understanding during online discussion and delete rach-ConfigCommonSBFD-r19 as no need. 5. Add preambleTransMaxSBFD according to meeting agreement. 6. alternative implementation of reportQuantity-r19 (CATT R2-2503424 TP1) , please comment/compare the two approaches: the current reportQuantityCLI-r19 and reportQuantity-r19. 7. add the missing field mimoParam-v19xy and its type (CATT 3424 TP2) 8. Revise cli-MeasResourceSetList-r19 in CSI-ResourceConfig (CATT 3424 TP3). 9. add cli-RSSI-MeasResourceToAddModList in CSI-MeasConfig (CATT 3424 TP4). |  |
| Rapp06 | In v01 version | 1. editorial changes on font style.  2. revise/shorten FD for sbfd-RSRP-ThresholdRO-TypeUsage .  3. change "SBFD capable UE" to "SBFD aware UE" as RAN1 TP to 38.300 provides reference of "SBFD aware UE". |  |
| Rapp07 | In v02 version | Implement RAN1 parameters and revisions according to R1-2503243 |  |