|  |  |  |  |
| --- | --- | --- | --- |
| Company | Clause | Comment | Rapp Response |
| Xiaomi | 4.2.2 | 1.The following context conflicts with each other, it says U2N relay UE (which may also be intermediate relay UE) contains Uu SRAP entity +PC5 SRAP entity, and it also contains only one PC5 SRAP entity.  On the U2N Relay UE (including the last Relay UE in multi-hop U2N Relay), the SRAP sublayer contains one SRAP entity at Uu interface and a separate collocated SRAP entity at the PC5 interface. On the U2N Remote UE and intermediate Relay UE, the SRAP sublayer contains only one SRAP entity at the PC5 interface. On the U2U Relay UE and U2U Remote UE, the SRAP sublayer contains only one SRAP entity at the PC5 interface. |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |