**3GPP TSG-RAN WG2 Meeting #131  *R2-2506486***

**Bengaluru, India, 25th - 29th August, 2025**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | **38.331** | **CR** | **Draft** | **rev** | **1** | **Current version:** | **18.6.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Introduction of 3Tx UL switching [TxSwitch\_R19] |
|  |  |
| ***Source to WG:*** | MediaTek Inc., Ericsson, T-Mobile USA |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | TEI19 |  | ***Date:*** | 2025-09-01 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-19 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | In RAN2#130 meeting, RAN2 was notified of introducing the further Tx switching enhancement for 2 configured UL bands in Rel-19 TEI as per RAN4 LS in R2-2503333.The corresponding FGs of 3Tx UL switching are included in RAN4 feature list (R4-2511883) on R19 RAN4 UE feature list for NR.This CR proposes to add RRC capability parameters for the above RAN4 FGs of the 3Tx UL switching scenario. |
|  |  |
| ***Summary of change:*** | To introduce the new 3Tx switching capability parameters as per Rel-19 RAN4 feature list. |
|  |  |
| ***Consequences if not approved:*** | UL Tx switching for 3Tx UE will not be enabled. |
|  |  |
| ***Clauses affected:*** | 6.3.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **X** |  |  Other core specifications  | TS 38.306 CR Draft TS 38.331 CR 5411r1 |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | Rev1: Update coversheet and TPs accoridng to the RAN4 Feature list. |

# 6 Protocol data units, formats and parameters (ASN.1)

<Unchanged part is omitted>

## 6.3 RRC information elements

<Unchanged part is omitted>

Beginning of first change

### 6.3.3 UE capability information elements

#### – *BandCombinationList*

The IE *BandCombinationList* contains a list of NR CA, NR non-CA and/or MR-DC band combinations (also including DL only or UL only band).

*BandCombinationList* information element

-- ASN1START

-- TAG-BANDCOMBINATIONLIST-START

BandCombinationList ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination

BandCombinationList-v1540 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1540

BandCombinationList-v1550 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1550

BandCombinationList-v1560 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1560

BandCombinationList-v1570 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1570

BandCombinationList-v1580 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1580

BandCombinationList-v1590 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1590

BandCombinationList-v15g0 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v15g0

BandCombinationList-v15n0 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v15n0

BandCombinationList-v1610 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1610

BandCombinationList-v1630 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1630

BandCombinationList-v1640 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1640

BandCombinationList-v1650 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1650

BandCombinationList-v1680 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1680

BandCombinationList-v1690 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1690

BandCombinationList-v16a0 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v16a0

BandCombinationList-v16j0 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v16j0

BandCombinationList-v1700 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1700

BandCombinationList-v1720 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1720

BandCombinationList-v1730 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1730

BandCombinationList-v1740 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1740

BandCombinationList-v1760 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1760

BandCombinationList-v1770 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1770

BandCombinationList-v1780 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1780

BandCombinationList-v1790 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1790

BandCombinationList-v17b0 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v17b0

BandCombinationList-v1800 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1800

BandCombinationList-v1830 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1830

BandCombinationList-v1840 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1840

BandCombinationList-v1860 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1860

BandCombinationList-UplinkTxSwitch-r16 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-r16

BandCombinationList-UplinkTxSwitch-v1630 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1630

BandCombinationList-UplinkTxSwitch-v1640 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1640

BandCombinationList-UplinkTxSwitch-v1650 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1650

BandCombinationList-UplinkTxSwitch-v1670 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1670

BandCombinationList-UplinkTxSwitch-v1690 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1690

BandCombinationList-UplinkTxSwitch-v16a0 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v16a0

BandCombinationList-UplinkTxSwitch-v16e0 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v16e0

BandCombinationList-UplinkTxSwitch-v16j0 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v16j0

BandCombinationList-UplinkTxSwitch-v1700 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1700

BandCombinationList-UplinkTxSwitch-v1720 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1720

BandCombinationList-UplinkTxSwitch-v1730 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1730

BandCombinationList-UplinkTxSwitch-v1740 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1740

BandCombinationList-UplinkTxSwitch-v1760 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1760

BandCombinationList-UplinkTxSwitch-v1770 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1770

BandCombinationList-UplinkTxSwitch-v1780 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1780

BandCombinationList-UplinkTxSwitch-v1790 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1790

BandCombinationList-UplinkTxSwitch-v17b0 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v17b0

BandCombinationList-UplinkTxSwitch-v1800 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1800

BandCombinationList-UplinkTxSwitch-v1830 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1830

BandCombinationList-UplinkTxSwitch-v1840 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1840

BandCombinationList-UplinkTxSwitch-v1860 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1860

BandCombinationList-UplinkTxSwitch-v19xy ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v19xy

BandCombination ::= SEQUENCE {

 bandList SEQUENCE (SIZE (1..maxSimultaneousBands)) OF BandParameters,

 featureSetCombination FeatureSetCombinationId,

 ca-ParametersEUTRA CA-ParametersEUTRA OPTIONAL,

 ca-ParametersNR CA-ParametersNR OPTIONAL,

 mrdc-Parameters MRDC-Parameters OPTIONAL,

 supportedBandwidthCombinationSet BIT STRING (SIZE (1..32)) OPTIONAL,

 powerClass-v1530 ENUMERATED {pc2} OPTIONAL

}

BandCombination-v1540::= SEQUENCE {

 bandList-v1540 SEQUENCE (SIZE (1..maxSimultaneousBands)) OF BandParameters-v1540,

 ca-ParametersNR-v1540 CA-ParametersNR-v1540 OPTIONAL

}

BandCombination-v1550 ::= SEQUENCE {

 ca-ParametersNR-v1550 CA-ParametersNR-v1550

}

BandCombination-v1560::= SEQUENCE {

 ne-DC-BC ENUMERATED {supported} OPTIONAL,

 ca-ParametersNRDC CA-ParametersNRDC OPTIONAL,

 ca-ParametersEUTRA-v1560 CA-ParametersEUTRA-v1560 OPTIONAL,

 ca-ParametersNR-v1560 CA-ParametersNR-v1560 OPTIONAL

}

BandCombination-v1570 ::= SEQUENCE {

 ca-ParametersEUTRA-v1570 CA-ParametersEUTRA-v1570

}

BandCombination-v1580 ::= SEQUENCE {

 mrdc-Parameters-v1580 MRDC-Parameters-v1580

}

BandCombination-v1590::= SEQUENCE {

 supportedBandwidthCombinationSetIntraENDC BIT STRING (SIZE (1..32)) OPTIONAL,

 mrdc-Parameters-v1590 MRDC-Parameters-v1590

}

BandCombination-v15g0::= SEQUENCE {

 ca-ParametersNR-v15g0 CA-ParametersNR-v15g0 OPTIONAL,

 ca-ParametersNRDC-v15g0 CA-ParametersNRDC-v15g0 OPTIONAL,

 mrdc-Parameters-v15g0 MRDC-Parameters-v15g0 OPTIONAL

}

BandCombination-v15n0::= SEQUENCE {

 mrdc-Parameters-v15n0 MRDC-Parameters-v15n0

}

BandCombination-v1610 ::= SEQUENCE {

 bandList-v1610 SEQUENCE (SIZE (1..maxSimultaneousBands)) OF BandParameters-v1610 OPTIONAL,

 ca-ParametersNR-v1610 CA-ParametersNR-v1610 OPTIONAL,

 ca-ParametersNRDC-v1610 CA-ParametersNRDC-v1610 OPTIONAL,

 powerClass-v1610 ENUMERATED {pc1dot5} OPTIONAL,

 powerClassNRPart-r16 ENUMERATED {pc1, pc2, pc3, pc5} OPTIONAL,

 featureSetCombinationDAPS-r16 FeatureSetCombinationId OPTIONAL,

 mrdc-Parameters-v1620 MRDC-Parameters-v1620 OPTIONAL

}

BandCombination-v1630 ::= SEQUENCE {

 ca-ParametersNR-v1630 CA-ParametersNR-v1630 OPTIONAL,

 ca-ParametersNRDC-v1630 CA-ParametersNRDC-v1630 OPTIONAL,

 mrdc-Parameters-v1630 MRDC-Parameters-v1630 OPTIONAL,

 supportedTxBandCombListPerBC-Sidelink-r16 BIT STRING (SIZE (1..maxBandComb)) OPTIONAL,

 supportedRxBandCombListPerBC-Sidelink-r16 BIT STRING (SIZE (1..maxBandComb)) OPTIONAL,

 scalingFactorTxSidelink-r16 SEQUENCE (SIZE (1..maxBandComb)) OF ScalingFactorSidelink-r16 OPTIONAL,

 scalingFactorRxSidelink-r16 SEQUENCE (SIZE (1..maxBandComb)) OF ScalingFactorSidelink-r16 OPTIONAL

}

BandCombination-v1640 ::= SEQUENCE {

 ca-ParametersNR-v1640 CA-ParametersNR-v1640 OPTIONAL,

 ca-ParametersNRDC-v1640 CA-ParametersNRDC-v1640 OPTIONAL

}

BandCombination-v1650 ::= SEQUENCE {

 ca-ParametersNRDC-v1650 CA-ParametersNRDC-v1650 OPTIONAL

}

BandCombination-v1680 ::= SEQUENCE {

 intrabandConcurrentOperationPowerClass-r16 SEQUENCE (SIZE (1..maxBandComb)) OF IntraBandPowerClass-r16 OPTIONAL

}

BandCombination-v1690 ::= SEQUENCE {

 dummy CA-ParametersNR-v1690 OPTIONAL

}

BandCombination-v16a0 ::= SEQUENCE {

 ca-ParametersNR-v16a0 CA-ParametersNR-v16a0 OPTIONAL,

 ca-ParametersNRDC-v16a0 CA-ParametersNRDC-v16a0 OPTIONAL

}

BandCombination-v16j0::= SEQUENCE {

 ca-ParametersNR-v16j0 CA-ParametersNR-v1690 OPTIONAL,

 ca-ParametersNRDC-v16j0 CA-ParametersNRDC-v16j0 OPTIONAL

}

BandCombination-v1700 ::= SEQUENCE {

 ca-ParametersNR-v1700 CA-ParametersNR-v1700 OPTIONAL,

 ca-ParametersNRDC-v1700 CA-ParametersNRDC-v1700 OPTIONAL,

 mrdc-Parameters-v1700 MRDC-Parameters-v1700 OPTIONAL,

 bandList-v1710 SEQUENCE (SIZE (1..maxSimultaneousBands)) OF BandParameters-v1710 OPTIONAL,

 supportedBandCombListPerBC-SL-RelayDiscovery-r17 BIT STRING (SIZE (1..maxBandComb)) OPTIONAL,

 supportedBandCombListPerBC-SL-NonRelayDiscovery-r17 BIT STRING (SIZE (1..maxBandComb)) OPTIONAL

}

BandCombination-v1720 ::= SEQUENCE {

 ca-ParametersNR-v1720 CA-ParametersNR-v1720 OPTIONAL,

 ca-ParametersNRDC-v1720 CA-ParametersNRDC-v1720 OPTIONAL

}

BandCombination-v1730 ::= SEQUENCE {

 ca-ParametersNR-v1730 CA-ParametersNR-v1730 OPTIONAL,

 ca-ParametersNRDC-v1730 CA-ParametersNRDC-v1730 OPTIONAL,

 bandList-v1730 SEQUENCE (SIZE (1..maxSimultaneousBands)) OF BandParameters-v1730 OPTIONAL

}

BandCombination-v1740 ::= SEQUENCE {

 dummy CA-ParametersNR-v1740 OPTIONAL

}

BandCombination-v1760 ::= SEQUENCE {

 ca-ParametersNR-v1760 CA-ParametersNR-v1760,

 ca-ParametersNRDC-v1760 CA-ParametersNRDC-v1760

}

BandCombination-v1770::= SEQUENCE {

 bandList-v1770 SEQUENCE (SIZE (1..maxSimultaneousBands)) OF BandParameters-v1770,

 mrdc-Parameters-v1770 MRDC-Parameters-v1770 OPTIONAL,

 ca-ParametersNR-v1770 CA-ParametersNR-v1770 OPTIONAL

}

BandCombination-v1780 ::= SEQUENCE {

 ca-ParametersNR-v1780 CA-ParametersNR-v1780 OPTIONAL,

 ca-ParametersNRDC-v1780 CA-ParametersNRDC-v1780 OPTIONAL,

 bandList-v1780 SEQUENCE (SIZE (1..maxSimultaneousBands)) OF BandParameters-v1780 OPTIONAL,

 mrdc-Parameters-v1780 MRDC-Parameters-v1770 OPTIONAL

}

BandCombination-v1790 ::= SEQUENCE {

 supportedIntraENDC-BandCombinationList-r17 SEQUENCE (SIZE (1..maxNrofIntraEndc-Components-r17)) OF SupportedIntraENDC-BandCombination-r17 OPTIONAL

}

BandCombination-v17b0::= SEQUENCE {

 ca-ParametersNR-v17b0 CA-ParametersNR-v1740 OPTIONAL,

 ca-ParametersNRDC-v17b0 CA-ParametersNRDC-v17b0 OPTIONAL

}

BandCombination-v1800 ::= SEQUENCE {

 ca-ParametersNR-v1800 CA-ParametersNR-v1800 OPTIONAL,

 ca-ParametersNRDC-v1800 CA-ParametersNRDC-v1800 OPTIONAL,

 supportedBandCombListPerBC-SL-U2U-RelayDiscovery-r18 BIT STRING (SIZE (1..maxBandComb)) OPTIONAL,

 bandList-v1810 SEQUENCE (SIZE (1..maxSimultaneousBands)) OF BandParameters-v1810 OPTIONAL

}

BandCombination-v1830 ::= SEQUENCE {

 ca-ParametersNR-v1830 CA-ParametersNR-v1830 OPTIONAL,

 ca-ParametersNRDC-v1830 CA-ParametersNRDC-v1830 OPTIONAL

}

BandCombination-v1840 ::= SEQUENCE {

 mrdc-Parameters-v1840 MRDC-Parameters-v1840 OPTIONAL

}

BandCombination-v1860 ::= SEQUENCE {

 ca-ParametersNR-v1860 CA-ParametersNR-v1860 OPTIONAL

}

BandCombination-UplinkTxSwitch-r16 ::= SEQUENCE {

 bandCombination-r16 BandCombination,

 bandCombination-v1540 BandCombination-v1540 OPTIONAL,

 bandCombination-v1560 BandCombination-v1560 OPTIONAL,

 bandCombination-v1570 BandCombination-v1570 OPTIONAL,

 bandCombination-v1580 BandCombination-v1580 OPTIONAL,

 bandCombination-v1590 BandCombination-v1590 OPTIONAL,

 bandCombination-v1610 BandCombination-v1610 OPTIONAL,

 supportedBandPairListNR-r16 SEQUENCE (SIZE (1..maxULTxSwitchingBandPairs)) OF ULTxSwitchingBandPair-r16,

 uplinkTxSwitching-OptionSupport-r16 ENUMERATED {switchedUL, dualUL, both} OPTIONAL,

 uplinkTxSwitching-PowerBoosting-r16 ENUMERATED {supported} OPTIONAL,

 ...,

 [[

 -- R4 16-5 UL-MIMO coherence capability for dynamic Tx switching between 3CC 1Tx-2Tx switching

 uplinkTxSwitching-PUSCH-TransCoherence-r16 ENUMERATED {nonCoherent, fullCoherent} OPTIONAL

 ]]

}

BandCombination-UplinkTxSwitch-v1630 ::= SEQUENCE {

 bandCombination-v1630 BandCombination-v1630 OPTIONAL

}

BandCombination-UplinkTxSwitch-v1640 ::= SEQUENCE {

 bandCombination-v1640 BandCombination-v1640 OPTIONAL

}

BandCombination-UplinkTxSwitch-v1650 ::= SEQUENCE {

 bandCombination-v1650 BandCombination-v1650 OPTIONAL

}

BandCombination-UplinkTxSwitch-v1670 ::= SEQUENCE {

 bandCombination-v15g0 BandCombination-v15g0 OPTIONAL

}

BandCombination-UplinkTxSwitch-v1690 ::= SEQUENCE {

 bandCombination-v1690 BandCombination-v1690 OPTIONAL

}

BandCombination-UplinkTxSwitch-v16a0 ::= SEQUENCE {

 bandCombination-v16a0 BandCombination-v16a0 OPTIONAL

}

BandCombination-UplinkTxSwitch-v16e0 ::= SEQUENCE {

 bandCombination-v15n0 BandCombination-v15n0 OPTIONAL

}

BandCombination-UplinkTxSwitch-v16j0 ::= SEQUENCE {

 bandCombination-v16j0 BandCombination-v16j0 OPTIONAL

}

BandCombination-UplinkTxSwitch-v1700 ::= SEQUENCE {

 bandCombination-v1700 BandCombination-v1700 OPTIONAL,

 -- R4 16-1/16-2/16-3 Dynamic Tx switching between 2CC/3CC 2Tx-2Tx/1Tx-2Tx switching

 supportedBandPairListNR-v1700 SEQUENCE (SIZE (1..maxULTxSwitchingBandPairs)) OF ULTxSwitchingBandPair-v1700 OPTIONAL,

 -- R4 16-6: UL-MIMO coherence capability for dynamic Tx switching between 2Tx-2Tx switching

 uplinkTxSwitchingBandParametersList-v1700 SEQUENCE (SIZE (1.. maxSimultaneousBands)) OF UplinkTxSwitchingBandParameters-v1700 OPTIONAL

}

BandCombination-UplinkTxSwitch-v1720 ::= SEQUENCE {

 bandCombination-v1720 BandCombination-v1720 OPTIONAL,

 uplinkTxSwitching-OptionSupport2T2T-r17 ENUMERATED {switchedUL, dualUL, both} OPTIONAL

}

BandCombination-UplinkTxSwitch-v1730 ::= SEQUENCE {

 bandCombination-v1730 BandCombination-v1730 OPTIONAL

}

BandCombination-UplinkTxSwitch-v1740 ::= SEQUENCE {

 bandCombination-v1740 BandCombination-v1740 OPTIONAL

}

BandCombination-UplinkTxSwitch-v1760 ::= SEQUENCE {

 bandCombination-v1760 BandCombination-v1760 OPTIONAL

}

BandCombination-UplinkTxSwitch-v1770 ::= SEQUENCE {

 bandCombination-v1770 BandCombination-v1770 OPTIONAL

}

BandCombination-UplinkTxSwitch-v1780 ::= SEQUENCE {

 bandCombination-v1780 BandCombination-v1780 OPTIONAL

}

BandCombination-UplinkTxSwitch-v1790 ::= SEQUENCE {

 bandCombination-v1790 BandCombination-v1790 OPTIONAL

}

BandCombination-UplinkTxSwitch-v17b0 ::= SEQUENCE {

 bandCombination-v17b0 BandCombination-v17b0 OPTIONAL

}

BandCombination-UplinkTxSwitch-v1800 ::= SEQUENCE {

 bandCombination-v1800 BandCombination-v1800 OPTIONAL,

 supportedBandPairListNR-r18 SEQUENCE (SIZE (1..maxULTxSwitchingBandPairs)) OF ULTxSwitchingBandPair-r18 OPTIONAL,

 -- R1 49-Y: Minimum separation time for two uplink switching on more than 2 bands within any two consecutive reference slots

 uplinkTxSwitchingMinimumSeparationTime-r18 ENUMERATED {n0us, n500us} OPTIONAL,

 -- R4 38-4: Switching Period for unaffected Band for Dual UL

 uplinkTxSwitchingAdditionalPeriodDualUL-List-r18 SEQUENCE (SIZE (1..maxULTxSwitchingBetweenBandPairs-r18)) OF

 UplinkTxSwitchingAdditionalPeriodDualUL-r18 OPTIONAL,

 -- R4 38-6: Switching period restriction for fallback band combination

 switchingPeriodRestriction-r18 ENUMERATED {true} OPTIONAL

}

BandCombination-UplinkTxSwitch-v1830 ::= SEQUENCE {

 bandCombination-v1830 BandCombination-v1830 OPTIONAL

}

BandCombination-UplinkTxSwitch-v1840 ::= SEQUENCE {

 bandCombination-v1840 BandCombination-v1840 OPTIONAL,

 supportedBandPairListNR-v1840 SEQUENCE (SIZE (1..maxULTxSwitchingBandPairs)) OF ULTxSwitchingBandPair-v1840 OPTIONAL

}

BandCombination-UplinkTxSwitch-v1860 ::= SEQUENCE {

 bandCombination-v1860 BandCombination-v1860 OPTIONAL

}

BandCombination-UplinkTxSwitch-v19xy ::= SEQUENCE {

 supportedBandPairListNR-v19xy SEQUENCE (SIZE (1..maxULTxSwitchingBandPairs)) OF ULTxSwitchingBandPair-v19xy OPTIONAL,

 uplinkTxSwitchingBandParametersList-v19xy SEQUENCE (SIZE (1..maxSimultaneousBands)) OF UplinkTxSwitchingBandParameters-v19xy OPTIONAL

}

ULTxSwitchingBandPair-r16 ::= SEQUENCE {

 bandIndexUL1-r16 INTEGER(1..maxSimultaneousBands),

 bandIndexUL2-r16 INTEGER(1..maxSimultaneousBands),

 uplinkTxSwitchingPeriod-r16 ENUMERATED {n35us, n140us, n210us},

 uplinkTxSwitching-DL-Interruption-r16 BIT STRING (SIZE(1..maxSimultaneousBands)) OPTIONAL

}

ULTxSwitchingBandPair-v1700 ::= SEQUENCE {

 uplinkTxSwitchingPeriod2T2T-r17 ENUMERATED {n35us, n140us, n210us} OPTIONAL

}

ULTxSwitchingBandPair-r18 ::= SEQUENCE {

 bandIndexUL1-r18 INTEGER(1..maxSimultaneousBands),

 bandIndexUL2-r18 INTEGER(1..maxSimultaneousBands),

 -- R1 49-X: Supported switching option for each band pair in the band combination for UL Tx switching across more than 2 bands

 uplinkTxSwitchingOptionForBandPair-r18 ENUMERATED {switchedUL, dualUL, both},

 -- R4 38-1: Switching period for dynamic UL Tx switching across up to 4 bands in case of inter-band CA, SUL up to two TAGs

 uplinkTxSwitchingPeriodForBandPair-r18 SEQUENCE {

 switchingPeriodFor2T-r18 ENUMERATED {n35us, n140us, n210us} OPTIONAL,

 switchingPeriodFor1T-r18 ENUMERATED {n35us, n140us, n210us}

 },

 -- R4 38-2: Application of DL interruptions due to dynamic UL Tx switching

 uplinkTxSwitching-DL-Interruption-r18 BIT STRING (SIZE(1..maxSimultaneousBands)) OPTIONAL,

 -- R4 38-3: Switching Period for unaffected Band for Dual UL

 uplinkTxSwitchingPeriodUnaffectedBandDualUL-List-r18 SEQUENCE (SIZE (1..maxSimultaneousBands-2-r18)) OF

 SwitchingPeriodUnaffectedBandDualUL-r18 OPTIONAL

}

ULTxSwitchingBandPair-v1840 ::= SEQUENCE {

 -- R1 49-Z: Support of 2-band configuration of 1T-1T UL Tx switching by using Rel-18 UL Tx switching configurations

 configured1T1T-OnTwoBands-r18 ENUMERATED {supported} OPTIONAL

}

ULTxSwitchingBandPair-v19xy ::= SEQUENCE {

 -- R4 57-1: Switch period for dynamic UL Tx switching between 2 bands for 3Tx UE with up to 2Tx per band

 uplink3TxSwitchingPeriodUpTo2TPerBandDualUL-v19xy ENUMERATED {n35us, n140us, n210us},

 -- R4 57-2: Application of DL interruptions due to dynamic UL Tx switching between 2 bands for 3Tx UE with up to 2Tx per band

 uplinkTxSwitching-DL-Interruption-DualUL-v19xy BIT STRING (SIZE(1..maxSimultaneousBands)) OPTIONAL

}

UplinkTxSwitchingBandParameters-v1700 ::= SEQUENCE {

 bandIndex-r17 INTEGER(1..maxSimultaneousBands),

 -- R4 38-5: UL-MIMO coherence capability for dynamic Tx switching between 2Tx-2Tx switching among up to 4 bands

 uplinkTxSwitching2T2T-PUSCH-TransCoherence-r17 ENUMERATED {nonCoherent, fullCoherent} OPTIONAL

}

UplinkTxSwitchingAdditionalPeriodDualUL-r18::= SEQUENCE {

 uplinkTxSwitchingBetweenBandPairs-r18 SEQUENCE {

 bandPairIndex1-r18 INTEGER(1.. maxULTxSwitchingBandPairs),

 anotherBandPairOrBand-r18 CHOICE {

 bandPairIndex2-r18 INTEGER(1.. maxULTxSwitchingBandPairs),

 bandIndex-r18 INTEGER(1..maxSimultaneousBands)

 }

 },

 -- R4 38-4: Additional switching Period for switching case across three or four bands for Dual UL

 switchingAdditionalPeriodDualUL-r18 ENUMERATED {n35us, n140us, n210us}

}

UplinkTxSwitchingBandParameters-v19xy ::= SEQUENCE {

 bandIndex-r19 INTEGER(1..maxSimultaneousBands),

 -- R4 57-3: UL-MIMO coherence capability for dynamic UL Tx switching between 2 bands for 3Tx UE with up to 2Tx per band

 uplinkTxSwitching3Tx-PUSCH-TransCoherence-DualUL-v19xy ENUMERATED {nonCoherent, fullCoherent} OPTIONAL

}

SwitchingPeriodUnaffectedBandDualUL-r18::= SEQUENCE {

 bandIndexUnaffected-r18 INTEGER(1..maxSimultaneousBands),

 periodUnaffectedBandDualUL-r18 CHOICE {

 maintainedUL-Trans-r18 NULL,

 periodOnULBands-r18 ENUMERATED {n35us, n140us, n210us}

 }

}

BandParameters ::= CHOICE {

 eutra SEQUENCE {

 bandEUTRA FreqBandIndicatorEUTRA,

 ca-BandwidthClassDL-EUTRA CA-BandwidthClassEUTRA OPTIONAL,

 ca-BandwidthClassUL-EUTRA CA-BandwidthClassEUTRA OPTIONAL

 },

 nr SEQUENCE {

 bandNR FreqBandIndicatorNR,

 ca-BandwidthClassDL-NR CA-BandwidthClassNR OPTIONAL,

 ca-BandwidthClassUL-NR CA-BandwidthClassNR OPTIONAL

 }

}

BandParameters-v1540 ::= SEQUENCE {

 srs-CarrierSwitch CHOICE {

 nr SEQUENCE {

 srs-SwitchingTimesListNR SEQUENCE (SIZE (1..maxSimultaneousBands)) OF SRS-SwitchingTimeNR

 },

 eutra SEQUENCE {

 srs-SwitchingTimesListEUTRA SEQUENCE (SIZE (1..maxSimultaneousBands)) OF SRS-SwitchingTimeEUTRA

 }

 } OPTIONAL,

 srs-TxSwitch SEQUENCE {

 supportedSRS-TxPortSwitch ENUMERATED {t1r2, t1r4, t2r4, t1r4-t2r4, t1r1, t2r2, t4r4, notSupported},

 txSwitchImpactToRx INTEGER (1..32) OPTIONAL,

 txSwitchWithAnotherBand INTEGER (1..32) OPTIONAL

 } OPTIONAL

}

BandParameters-v1610 ::= SEQUENCE {

 srs-TxSwitch-v1610 SEQUENCE {

 supportedSRS-TxPortSwitch-v1610 ENUMERATED {t1r1-t1r2, t1r1-t1r2-t1r4, t1r1-t1r2-t2r2-t2r4, t1r1-t1r2-t2r2-t1r4-t2r4,

 t1r1-t2r2, t1r1-t2r2-t4r4}

 } OPTIONAL

}

BandParameters-v1710 ::= SEQUENCE {

 -- R1 23-8-3 SRS Antenna switching for >4Rx

 srs-AntennaSwitchingBeyond4RX-r17 SEQUENCE {

 -- 1. Support of SRS antenna switching xTyR with y>4

 supportedSRS-TxPortSwitchBeyond4Rx-r17 BIT STRING (SIZE (11)),

 -- 2. Report the entry number of the first-listed band with UL in the band combination that affects this DL

 entryNumberAffectBeyond4Rx-r17 INTEGER (1..32) OPTIONAL,

 -- 3. Report the entry number of the first-listed band with UL in the band combination that switches together with this UL

 entryNumberSwitchBeyond4Rx-r17 INTEGER (1..32) OPTIONAL

 } OPTIONAL

}

BandParameters-v1730 ::= SEQUENCE {

 -- R1 39-3-2 Affected bands for inter-band CA during SRS carrier switching

 srs-SwitchingAffectedBandsListNR-r17 SEQUENCE (SIZE (1..maxSimultaneousBands)) OF SRS-SwitchingAffectedBandsNR-r17

}

BandParameters-v1770 ::= SEQUENCE {

 ca-BandwidthClassDL-NR-r17 CA-BandwidthClassNR-r17 OPTIONAL,

 ca-BandwidthClassUL-NR-r17 CA-BandwidthClassNR-r17 OPTIONAL

}

BandParameters-v1780 ::= SEQUENCE {

 ca-BandwidthClassDL-NR-r17 CA-BandwidthClassNR-r17 OPTIONAL,

 ca-BandwidthClassUL-NR-r17 CA-BandwidthClassNR-r17 OPTIONAL,

 supportedAggBW-FR2-r17 SEQUENCE {

 supportedAggBW-DL-r17 SupportedAggBandwidth-r17 OPTIONAL,

 supportedAggBW-UL-r17 SupportedAggBandwidth-r17 OPTIONAL

 } OPTIONAL

}

BandParameters-v1810 ::= SEQUENCE {

 -- R1 40-5-4: SRS 8 Tx ports-antenna switching

 srs-AntennaSwitching8T8R-r18 SEQUENCE {

 antennaSwitch8T8R-r18 ENUMERATED {noTdm, tdmAndNoTdm} OPTIONAL,

 downgradeConfig-r18 CHOICE {

 empty-r18 NULL,

 downgrade-r18 BIT STRING (SIZE (11))

 } OPTIONAL,

 entryNumberAffect-r18 INTEGER (1..32) OPTIONAL,

 entryNumberSwitch-r18 INTEGER (1..32) OPTIONAL

 } OPTIONAL

}

ScalingFactorSidelink-r16 ::= ENUMERATED {f0p4, f0p75, f0p8, f1}

IntraBandPowerClass-r16 ::= ENUMERATED {pc2, pc3, spare6, spare5, spare4, spare3, spare2, spare1}

SRS-SwitchingAffectedBandsNR-r17 ::= BIT STRING (SIZE (1..maxSimultaneousBands))

SupportedIntraENDC-BandCombination-r17 ::= SEQUENCE {

 supportedBandwidthCombinationSetIntraENDC-v1790 BIT STRING (SIZE (1..32)) OPTIONAL,

 mrdc-Parameters-v1790 MRDC-Parameters-v1790 OPTIONAL

}

-- TAG-BANDCOMBINATIONLIST-STOP

-- ASN1STOP

|  |
| --- |
| *BandCombination* field descriptions |
| ***BandCombinationList-v1540, BandCombinationList-v1550, BandCombinationList-v1560, BandCombinationList-v1570, BandCombinationList-v1580, BandCombinationList-v1590, BandCombinationList-v15g0, BandCombinationList-v15n0, BandCombinationList-v1610*, *BandCombinationList-v1630*, *BandCombinationList-v1640*, *BandCombinationList-v1650, BandCombinationList-v1680, BandCombinationList-v1690, BandCombinationList-v16a0, BandCombinationList-v16j0, BandCombinationList-v1700, BandCombinationList-v1720, BandCombinationList-v1730, BandCombinationList-v1760, BandCombinationList-v1780, BandCombinationList-v1790, BandCombinationList-v17b0, BandCombinationList-v1800, BandCombinationList-v1830, BandCombinationList-v1840, BandCombinationList-v1860***The UE shall include the same number of entries, and listed in the same order, as in *BandCombinationList* (without suffix). If the field is included in *supportedBandCombinationListNEDC-Only-v1610*, the UE shall include the same number of entries, and listed in the same order, as in *BandCombinationList* of *supportedBandCombinationListNEDC-Only* (without suffix) field.If the field is included in *supportedBandCombinationListNEDC-Only-v15a0*, the UE shall include the same number of entries, and listed in the same order, as in *BandCombinationList* (without suffix) of *supportedBandCombinationListNEDC-Only* (without suffix) field. |
| ***BandCombinationList-UplinkTxSwitch-r16, BandCombinationList-UplinkTxSwitch-v1630, BandCombinationList-UplinkTxSwitch-v1640, BandCombinationList-UplinkTxSwitch-v1650, BandCombinationList-UplinkTxSwitch-v1690, BandCombinationList-UplinkTxSwitch-v16a0, BandCombinationList-UplinkTxSwitch-v16e0, BandCombinationList-UplinkTxSwitch-v16j0, BandCombinationList-UplinkTxSwitch-v1700, BandCombinationList-UplinkTxSwitch-v1720, BandCombinationList-UplinkTxSwitch-v1730, BandCombinationList-UplinkTxSwitch-v1760, BandCombinationList-UplinkTxSwitch-v1780, BandCombinationList-UplinkTxSwitch-v1790, BandCombinationList-UplinkTxSwitch-v17b0, BandCombinationList-UplinkTxSwitch-v1800, BandCombinationList-UplinkTxSwitch-v1830, BandCombinationList-UplinkTxSwitch-v1840, BandCombinationList-UplinkTxSwitch-v1860, BandCombinationList-UplinkTxSwitch-v19xy***The UE shall include the same number of entries, and listed in the same order, as in *BandCombinationList-UplinkTxSwitch-r16*.For the field of *supportedBandCombinationList-UplinkTxSwitch-v1700*, if the UE does not support 2Tx-2Tx switching for a given band combination, the field of *supportedBandPairListNR-v1700* in the corresponding entry is absent. |
| ***ca-ParametersNRDC***If the field (without suffix) is included for a band combination in the NR capability container, the field (without suffix) indicates support of NR-DC. Otherwise, the field is absent. If a version of the field (with suffix) is absent for a band combination, *ca-ParametersNR* field version in *BandCombination* corresponding to the *ca-ParametersNR-ForDC* field version in the field (with suffix) is applicable to the UE configured with NR-DC for the band combination. |
| ***featureSetCombinationDAPS***If this field is present for a band combination, it reports the feature set combination supported for the band combination when any DAPS bearer is configured. |
| ***ne-DC-BC***If the field is included for a band combination in the MR-DC capability container, the field indicates support of NE-DC. Otherwise, the field is absent. |
| ***supportedBandPairListNR-r16, supportedBandPairListNR-v1700, supportedBandPairListNR-v19xy***Indicates a list of band pair supporting UL Tx switching as defined in TS 38.101-1 [15] for a given band combination.A UE supporting 2Tx-2Tx switching should include both of *supportedBandPairListNR-r16* and *supportedBandPairListNR-v1700*. And the UE shall include the same number of entries listed in the same order as in *supportedBandPairListNR-r16*.If the UE does not support 2Tx-2Tx switching for a given band pair, the field of *uplinkTxSwitchingPeriod2T2T* in the corresponding entry is absent.A 3Tx UE supporting Tx switching between 2 UL bands with up to 2Tx per band should indicate both of *supportedBandPairListNR-r16* and *supportedBandPairListNR-v19xy*. And the UE shall include the same number of entries listed in the same order as in *supportedBandPairListNR-r16*. |
| ***supportedBandPairListNR-r18*, *supportedBandPairListNR-v1840***Indicates a list of band pair supporting UL Tx switching up to 4 bands as defined in TS 38.101-1 [15] for a given band combination. The UE shall include all the possible band pairs. If *supportedBandPairListNR-v1840* is included, the UE shall include the same number of entries listed in the same order as in *supportedBandPairListNR-r18*.For a band pair only supporting 1Tx-1Tx switching, the UE should include *switchingPeriodFor1T* in *ULTxSwitchingBandPair-r18*.For a band pair supporting 1Tx-2Tx switching, the UE always supports 1Tx-1Tx switching, and the UE should include *switchingPeriodFor1T* in *ULTxSwitchingBandPair-r18*.For a band pair supporting 2Tx-2Tx switching, the UE always supports 1Tx-2Tx switching and 1Tx-1Tx switching, the UE should include *switchingPeriodFor2T* as well as *switchingPeriodFor1T* in *ULTxSwitchingBandPair-r18*. |
| ***srs-SwitchingTimesListNR***Indicates, for a particular pair of NR bands, the RF retuning time when switching between a NR carrier corresponding to this band entry and another (PUSCH-less) NR carrier corresponding to the band entry in the order indicated below:- For the first NR band, the UE shall include the same number of entries for NR bands as in *bandList*, i.e. first entry corresponds to first NR band in *bandList* and so on,- For the second NR band, the UE shall include one entry less, i.e. first entry corresponds to the second NR band in *bandList* and so on- And so on |
| ***srs-SwitchingTimesListEUTRA***Indicates, for a particular pair of E-UTRA bands, the RF retuning time when switching between an E-UTRA carrier corresponding to this band entry and another (PUSCH-less) E-UTRA carrier corresponding to the band entry in the order indicated below:- For the first E-UTRA band, the UE shall include the same number of entries for E-UTRA bands as in *bandList,* i.e. first entry corresponds to first E-UTRA band in *bandList* and so on,- For the second E-UTRA band, the UE shall include one entry less, i.e. first entry corresponds to the second E-UTRA band in *bandList* and so on - And so on |
| ***srs-TxSwitch***Indicates supported SRS antenna switch capability for the associated band. If the UE indicates support of *SRS-SwitchingTimeNR*, the UE is allowed to set this field for a band with associated *FeatureSetUplinkId* set to 0 for SRS carrier switching. |
| ***supportedIntraENDC-BandCombinationList***Indicates BCS and/or spectrum contiguity capability for each entry in a list of intra-band (NG)EN-DC components in an inter-band (NG)EN-DC band combination. The UE shall include the entries in the order corresponding to the order of NR band entries of the intra-band (NG)EN-DC components in the *bandList* in the inter-band (NG)EN-DC band combination (i.e., *BandCombination* without suffix). |
| ***uplinkTxSwitchingBandParametersList-v1700, uplinkTxSwitchingBandParametersList-v19xy***Indicates a list of per band per band combination capabilities for UL Tx switching. |

End of first change

Beginning of second change

#### – *RF-Parameters*

The IE *RF-Parameters* is used to convey RF-related capabilities for NR operation.

*RF-Parameters* information element

-- ASN1START

-- TAG-RF-PARAMETERS-START

RF-Parameters ::= SEQUENCE {

 supportedBandListNR SEQUENCE (SIZE (1..maxBands)) OF BandNR,

 supportedBandCombinationList BandCombinationList OPTIONAL,

 appliedFreqBandListFilter FreqBandList OPTIONAL,

 ...,

 [[

 supportedBandCombinationList-v1540 BandCombinationList-v1540 OPTIONAL,

 srs-SwitchingTimeRequested ENUMERATED {true} OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1550 BandCombinationList-v1550 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1560 BandCombinationList-v1560 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1610 BandCombinationList-v1610 OPTIONAL,

 supportedBandCombinationListSidelinkEUTRA-NR-r16 BandCombinationListSidelinkEUTRA-NR-r16 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-r16 BandCombinationList-UplinkTxSwitch-r16 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1630 BandCombinationList-v1630 OPTIONAL,

 supportedBandCombinationListSidelinkEUTRA-NR-v1630 BandCombinationListSidelinkEUTRA-NR-v1630 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1630 BandCombinationList-UplinkTxSwitch-v1630 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1640 BandCombinationList-v1640 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1640 BandCombinationList-UplinkTxSwitch-v1640 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1650 BandCombinationList-v1650 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1650 BandCombinationList-UplinkTxSwitch-v1650 OPTIONAL

 ]],

 [[

 extendedBand-n77-r16 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 supportedBandCombinationList-UplinkTxSwitch-v1670 BandCombinationList-UplinkTxSwitch-v1670 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1680 BandCombinationList-v1680 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1690 BandCombinationList-v1690 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1690 BandCombinationList-UplinkTxSwitch-v1690 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1700 BandCombinationList-v1700 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1700 BandCombinationList-UplinkTxSwitch-v1700 OPTIONAL,

 supportedBandCombinationListSL-RelayDiscovery-r17 OCTET STRING OPTIONAL, -- Contains PC5 BandCombinationListSidelinkNR-r16

 supportedBandCombinationListSL-NonRelayDiscovery-r17 OCTET STRING OPTIONAL, -- Contains PC5 BandCombinationListSidelinkNR-r16

 supportedBandCombinationListSidelinkEUTRA-NR-v1710 BandCombinationListSidelinkEUTRA-NR-v1710 OPTIONAL,

 sidelinkRequested-r17 ENUMERATED {true} OPTIONAL,

 extendedBand-n77-2-r17 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1720 BandCombinationList-v1720 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1720 BandCombinationList-UplinkTxSwitch-v1720 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1730 BandCombinationList-v1730 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1730 BandCombinationList-UplinkTxSwitch-v1730 OPTIONAL,

 supportedBandCombinationListSL-RelayDiscovery-v1730 BandCombinationListSL-Discovery-r17 OPTIONAL,

 supportedBandCombinationListSL-NonRelayDiscovery-v1730 BandCombinationListSL-Discovery-r17 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1740 BandCombinationList-v1740 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1740 BandCombinationList-UplinkTxSwitch-v1740 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1760 BandCombinationList-v1760 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1760 BandCombinationList-UplinkTxSwitch-v1760 OPTIONAL

 ]],

 [[

 dummy1 BandCombinationList-v1770 OPTIONAL,

 dummy2 BandCombinationList-UplinkTxSwitch-v1770 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1780 BandCombinationList-v1780 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1780 BandCombinationList-UplinkTxSwitch-v1780 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1800 BandCombinationList-v1800 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1800 BandCombinationList-UplinkTxSwitch-v1800 OPTIONAL,

 supportedBandCombinationListSL-U2U-Relay-r18 SEQUENCE {

 supportedBandCombinationListSL-U2U-RelayDiscovery-r18 OCTET STRING OPTIONAL, -- Contains PC5

 -- BandCombinationListSidelinkNR-r16

 supportedBandCombinationListSL-U2U-DiscoveryExt BandCombinationListSL-Discovery-r17 OPTIONAL

 } OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1830 BandCombinationList-v1830 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1830 BandCombinationList-UplinkTxSwitch-v1830 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1840 BandCombinationList-v1840 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1840 BandCombinationList-UplinkTxSwitch-v1840 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1860 BandCombinationList-v1860 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1860 BandCombinationList-UplinkTxSwitch-v1860 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-UplinkTxSwitch-v19xy BandCombinationList-UplinkTxSwitch-v19xy OPTIONAL

 ]]

}

RF-Parameters-v15g0 ::= SEQUENCE {

 supportedBandCombinationList-v15g0 BandCombinationList-v15g0 OPTIONAL

}

RF-Parameters-v16a0 ::= SEQUENCE {

 supportedBandCombinationList-v16a0 BandCombinationList-v16a0 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v16a0 BandCombinationList-UplinkTxSwitch-v16a0 OPTIONAL

}

RF-Parameters-v16c0 ::= SEQUENCE {

 supportedBandListNR-v16c0 SEQUENCE (SIZE (1..maxBands)) OF BandNR-v16c0

}

RF-Parameters-v16j0 ::= SEQUENCE {

 supportedBandCombinationList-v16j0 BandCombinationList-v16j0 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v16j0 BandCombinationList-UplinkTxSwitch-v16j0 OPTIONAL

}

RF-Parameters-v17b0 ::= SEQUENCE {

 supportedBandListNR-v17b0 SEQUENCE (SIZE (1..maxBands)) OF BandNR-v17b0 OPTIONAL,

 supportedBandCombinationList-v17b0 BandCombinationList-v17b0 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v17b0 BandCombinationList-UplinkTxSwitch-v17b0 OPTIONAL

}

BandNR ::= SEQUENCE {

 bandNR FreqBandIndicatorNR,

 modifiedMPR-Behaviour BIT STRING (SIZE (8)) OPTIONAL,

 mimo-ParametersPerBand MIMO-ParametersPerBand OPTIONAL,

 extendedCP ENUMERATED {supported} OPTIONAL,

 multipleTCI ENUMERATED {supported} OPTIONAL,

 bwp-WithoutRestriction ENUMERATED {supported} OPTIONAL,

 bwp-SameNumerology ENUMERATED {upto2, upto4} OPTIONAL,

 bwp-DiffNumerology ENUMERATED {upto4} OPTIONAL,

 crossCarrierScheduling-SameSCS ENUMERATED {supported} OPTIONAL,

 pdsch-256QAM-FR2 ENUMERATED {supported} OPTIONAL,

 pusch-256QAM ENUMERATED {supported} OPTIONAL,

 ue-PowerClass ENUMERATED {pc1, pc2, pc3, pc4} OPTIONAL,

 rateMatchingLTE-CRS ENUMERATED {supported} OPTIONAL,

 channelBWs-DL CHOICE {

 fr1 SEQUENCE {

 scs-15kHz BIT STRING (SIZE (10)) OPTIONAL,

 scs-30kHz BIT STRING (SIZE (10)) OPTIONAL,

 scs-60kHz BIT STRING (SIZE (10)) OPTIONAL

 },

 fr2 SEQUENCE {

 scs-60kHz BIT STRING (SIZE (3)) OPTIONAL,

 scs-120kHz BIT STRING (SIZE (3)) OPTIONAL

 }

 } OPTIONAL,

 channelBWs-UL CHOICE {

 fr1 SEQUENCE {

 scs-15kHz BIT STRING (SIZE (10)) OPTIONAL,

 scs-30kHz BIT STRING (SIZE (10)) OPTIONAL,

 scs-60kHz BIT STRING (SIZE (10)) OPTIONAL

 },

 fr2 SEQUENCE {

 scs-60kHz BIT STRING (SIZE (3)) OPTIONAL,

 scs-120kHz BIT STRING (SIZE (3)) OPTIONAL

 }

 } OPTIONAL,

 ...,

 [[

 maxUplinkDutyCycle-PC2-FR1 ENUMERATED {n60, n70, n80, n90, n100} OPTIONAL

 ]],

 [[

 pucch-SpatialRelInfoMAC-CE ENUMERATED {supported} OPTIONAL,

 powerBoosting-pi2BPSK ENUMERATED {supported} OPTIONAL

 ]],

 [[

 maxUplinkDutyCycle-FR2 ENUMERATED {n15, n20, n25, n30, n40, n50, n60, n70, n80, n90, n100} OPTIONAL

 ]],

 [[

 channelBWs-DL-v1590 CHOICE {

 fr1 SEQUENCE {

 scs-15kHz BIT STRING (SIZE (16)) OPTIONAL,

 scs-30kHz BIT STRING (SIZE (16)) OPTIONAL,

 scs-60kHz BIT STRING (SIZE (16)) OPTIONAL

 },

 fr2 SEQUENCE {

 scs-60kHz BIT STRING (SIZE (8)) OPTIONAL,

 scs-120kHz BIT STRING (SIZE (8)) OPTIONAL

 }

 } OPTIONAL,

 channelBWs-UL-v1590 CHOICE {

 fr1 SEQUENCE {

 scs-15kHz BIT STRING (SIZE (16)) OPTIONAL,

 scs-30kHz BIT STRING (SIZE (16)) OPTIONAL,

 scs-60kHz BIT STRING (SIZE (16)) OPTIONAL

 },

 fr2 SEQUENCE {

 scs-60kHz BIT STRING (SIZE (8)) OPTIONAL,

 scs-120kHz BIT STRING (SIZE (8)) OPTIONAL

 }

 } OPTIONAL

 ]],

 [[

 asymmetricBandwidthCombinationSet BIT STRING (SIZE (1..32)) OPTIONAL

 ]],

 [[

 -- R1 10: NR-unlicensed

 sharedSpectrumChAccessParamsPerBand-r16 SharedSpectrumChAccessParamsPerBand-r16 OPTIONAL,

 -- R1 11-7b: Independent cancellation of the overlapping PUSCHs in an intra-band UL CA

 cancelOverlappingPUSCH-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 14-1: Multiple LTE-CRS rate matching patterns

 multipleRateMatchingEUTRA-CRS-r16 SEQUENCE {

 maxNumberPatterns-r16 INTEGER (2..6),

 maxNumberNon-OverlapPatterns-r16 INTEGER (1..3)

 } OPTIONAL,

 -- R1 14-1a: Two LTE-CRS overlapping rate matching patterns within a part of NR carrier using 15 kHz overlapping with a LTE carrier

 overlapRateMatchingEUTRA-CRS-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 14-2: PDSCH Type B mapping of length 9 and 10 OFDM symbols

 pdsch-MappingTypeB-Alt-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 14-3: One slot periodic TRS configuration for FR1

 oneSlotPeriodicTRS-r16 ENUMERATED {supported} OPTIONAL,

 olpc-SRS-Pos-r16 OLPC-SRS-Pos-r16 OPTIONAL,

 spatialRelationsSRS-Pos-r16 SpatialRelationsSRS-Pos-r16 OPTIONAL,

 simulSRS-MIMO-TransWithinBand-r16 ENUMERATED {n2} OPTIONAL,

 channelBW-DL-IAB-r16 CHOICE {

 fr1-100mhz SEQUENCE {

 scs-15kHz ENUMERATED {supported} OPTIONAL,

 scs-30kHz ENUMERATED {supported} OPTIONAL,

 scs-60kHz ENUMERATED {supported} OPTIONAL

 },

 fr2-200mhz SEQUENCE {

 scs-60kHz ENUMERATED {supported} OPTIONAL,

 scs-120kHz ENUMERATED {supported} OPTIONAL

 }

 } OPTIONAL,

 channelBW-UL-IAB-r16 CHOICE {

 fr1-100mhz SEQUENCE {

 scs-15kHz ENUMERATED {supported} OPTIONAL,

 scs-30kHz ENUMERATED {supported} OPTIONAL,

 scs-60kHz ENUMERATED {supported} OPTIONAL

 },

 fr2-200mhz SEQUENCE {

 scs-60kHz ENUMERATED {supported} OPTIONAL,

 scs-120kHz ENUMERATED {supported} OPTIONAL

 }

 } OPTIONAL,

 rasterShift7dot5-IAB-r16 ENUMERATED {supported} OPTIONAL,

 ue-PowerClass-v1610 ENUMERATED {pc1dot5} OPTIONAL,

 condHandover-r16 ENUMERATED {supported} OPTIONAL,

 condHandoverFailure-r16 ENUMERATED {supported} OPTIONAL,

 condHandoverTwoTriggerEvents-r16 ENUMERATED {supported} OPTIONAL,

 condPSCellChange-r16 ENUMERATED {supported} OPTIONAL,

 condPSCellChangeTwoTriggerEvents-r16 ENUMERATED {supported} OPTIONAL,

 mpr-PowerBoost-FR2-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 11-9: Multiple active configured grant configurations for a BWP of a serving cell

 activeConfiguredGrant-r16 SEQUENCE {

 maxNumberConfigsPerBWP-r16 ENUMERATED {n1, n2, n4, n8, n12},

 maxNumberConfigsAllCC-r16 INTEGER (2..32)

 } OPTIONAL,

 -- R1 11-9a: Joint release in a DCI for two or more configured grant Type 2 configurations for a given BWP of a serving cell

 jointReleaseConfiguredGrantType2-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 12-2: Multiple SPS configurations

 sps-r16 SEQUENCE {

 maxNumberConfigsPerBWP-r16 INTEGER (1..8),

 maxNumberConfigsAllCC-r16 INTEGER (2..32)

 } OPTIONAL,

 -- R1 12-2a: Joint release in a DCI for two or more SPS configurations for a given BWP of a serving cell

 jointReleaseSPS-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 13-19: Simultaneous positioning SRS and MIMO SRS transmission within a band across multiple CCs

 simulSRS-TransWithinBand-r16 ENUMERATED {n2} OPTIONAL,

 trs-AdditionalBandwidth-r16 ENUMERATED {trs-AddBW-Set1, trs-AddBW-Set2} OPTIONAL,

 handoverIntraF-IAB-r16 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 -- R1 22-5a: Simultaneous transmission of SRS for antenna switching and SRS for CB/NCB /BM for intra-band UL CA

 -- R1 22-5c: Simultaneous transmission of SRS for antenna switching and SRS for antenna switching for intra-band UL CA

 simulTX-SRS-AntSwitchingIntraBandUL-CA-r16 SimulSRS-ForAntennaSwitching-r16 OPTIONAL,

 -- R1 10: NR-unlicensed

 sharedSpectrumChAccessParamsPerBand-v1630 SharedSpectrumChAccessParamsPerBand-v1630 OPTIONAL

 ]],

 [[

 handoverUTRA-FDD-r16 ENUMERATED {supported} OPTIONAL,

 -- R4 7-4: Report the shorter transient capability supported by the UE: 2, 4 or 7us

 enhancedUL-TransientPeriod-r16 ENUMERATED {us2, us4, us7} OPTIONAL,

 sharedSpectrumChAccessParamsPerBand-v1640 SharedSpectrumChAccessParamsPerBand-v1640 OPTIONAL

 ]],

 [[

 type1-PUSCH-RepetitionMultiSlots-v1650 ENUMERATED {supported} OPTIONAL,

 type2-PUSCH-RepetitionMultiSlots-v1650 ENUMERATED {supported} OPTIONAL,

 pusch-RepetitionMultiSlots-v1650 ENUMERATED {supported} OPTIONAL,

 configuredUL-GrantType1-v1650 ENUMERATED {supported} OPTIONAL,

 configuredUL-GrantType2-v1650 ENUMERATED {supported} OPTIONAL,

 sharedSpectrumChAccessParamsPerBand-v1650 SharedSpectrumChAccessParamsPerBand-v1650 OPTIONAL

 ]],

 [[

 enhancedSkipUplinkTxConfigured-v1660 ENUMERATED {supported} OPTIONAL,

 enhancedSkipUplinkTxDynamic-v1660 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 maxUplinkDutyCycle-PC1dot5-MPE-FR1-r16 ENUMERATED {n10, n15, n20, n25, n30, n40, n50, n60, n70, n80, n90, n100} OPTIONAL,

 txDiversity-r16 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 -- R1 36-1: Support of 1024QAM for PDSCH for FR1

 pdsch-1024QAM-FR1-r17 ENUMERATED {supported} OPTIONAL,

 -- R4 22-1 support of FR2 HST operation

 ue-PowerClass-v1700 ENUMERATED {pc5, pc6, pc7} OPTIONAL,

 -- R1 24: NR extension to 71GHz (FR2-2)

 fr2-2-AccessParamsPerBand-r17 FR2-2-AccessParamsPerBand-r17 OPTIONAL,

 rlm-Relaxation-r17 ENUMERATED {supported} OPTIONAL,

 bfd-Relaxation-r17 ENUMERATED {supported} OPTIONAL,

 cg-SDT-r17 ENUMERATED {supported} OPTIONAL,

 locationBasedCondHandover-r17 ENUMERATED {supported} OPTIONAL,

 timeBasedCondHandover-r17 ENUMERATED {supported} OPTIONAL,

 eventA4BasedCondHandover-r17 ENUMERATED {supported} OPTIONAL,

 mn-InitiatedCondPSCellChangeNRDC-r17 ENUMERATED {supported} OPTIONAL,

 sn-InitiatedCondPSCellChangeNRDC-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 29-3a: PDCCH skipping

 pdcch-SkippingWithoutSSSG-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 29-3b: 2 search space sets group switching

 sssg-Switching-1BitInd-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 29-3c: 3 search space sets group switching

 sssg-Switching-2BitInd-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 29-3d: 2 search space sets group switching with PDCCH skipping

 pdcch-SkippingWithSSSG-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 29-3e: Support Search space set group switching capability 2 for FR1

 searchSpaceSetGrp-switchCap2-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 26-1: Uplink Time and Frequency pre-compensation and timing relationship enhancements

 uplinkPreCompensation-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 26-4: UE reporting of information related to TA pre-compensation

 uplink-TA-Reporting-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 26-5: Increasing the number of HARQ processes

 max-HARQ-ProcessNumber-r17 ENUMERATED {u16d32, u32d16, u32d32} OPTIONAL,

 -- R1 26-6: Type-2 HARQ codebook enhancement

 type2-HARQ-Codebook-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 26-6a: Type-1 HARQ codebook enhancement

 type1-HARQ-Codebook-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 26-6b: Type-3 HARQ codebook enhancement

 type3-HARQ-Codebook-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 26-9: UE-specific K\_offset

 ue-specific-K-Offset-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 24-1f: Multiple PDSCH scheduling by single DCI for 120kHz in FR2-1

 multiPDSCH-SingleDCI-FR2-1-SCS-120kHz-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 24-1g: Multiple PUSCH scheduling by single DCI for 120kHz in FR2-1

 multiPUSCH-SingleDCI-FR2-1-SCS-120kHz-r17 ENUMERATED {supported} OPTIONAL,

 -- R4 14-4: Parallel PRS measurements in RRC\_INACTIVE state, FR1/FR2 diff

 parallelPRS-MeasRRC-Inactive-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 27-1-2: Support of UE-TxTEGs for UL TDOA

 nr-UE-TxTEG-ID-MaxSupport-r17 ENUMERATED {n1, n2, n3, n4, n6, n8} OPTIONAL,

 -- R1 27-17: PRS processing in RRC\_INACTIVE

 prs-ProcessingRRC-Inactive-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 27-3-2: DL PRS measurement outside MG and in a PRS processing window

 prs-ProcessingWindowType1A-r17 ENUMERATED {option1, option2, option3} OPTIONAL,

 prs-ProcessingWindowType1B-r17 ENUMERATED {option1, option2, option3} OPTIONAL,

 prs-ProcessingWindowType2-r17 ENUMERATED {option1, option2, option3} OPTIONAL,

 -- R1 27-15: Positioning SRS transmission in RRC\_INACTIVE state for initial UL BWP

 srs-AllPosResourcesRRC-Inactive-r17 SRS-AllPosResourcesRRC-Inactive-r17 OPTIONAL,

 -- R1 27-16: OLPC for positioning SRS in RRC\_INACTIVE state - gNB

 olpc-SRS-PosRRC-Inactive-r17 OLPC-SRS-Pos-r16 OPTIONAL,

 -- R1 27-19: Spatial relation for positioning SRS in RRC\_INACTIVE state - gNB

 spatialRelationsSRS-PosRRC-Inactive-r17 SpatialRelationsSRS-Pos-r16 OPTIONAL,

 -- R1 30-1: Increased maximum number of PUSCH Type A repetitions

 maxNumberPUSCH-TypeA-Repetition-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 30-2: PUSCH Type A repetitions based on available slots

 puschTypeA-RepetitionsAvailSlot-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 30-3: TB processing over multi-slot PUSCH

 tb-ProcessingMultiSlotPUSCH-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 30-3a: Repetition of TB processing over multi-slot PUSCH

 tb-ProcessingRepMultiSlotPUSCH-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 30-4: The maximum duration for DM-RS bundling

 maxDurationDMRS-Bundling-r17 SEQUENCE {

 fdd-r17 ENUMERATED {n4, n8, n16, n32} OPTIONAL,

 tdd-r17 ENUMERATED {n2, n4, n8, n16} OPTIONAL

 } OPTIONAL,

 -- R1 30-6: Repetition of PUSCH transmission scheduled by RAR UL grant and DCI format 0\_0 with CRC scrambled by TC-RNTI

 pusch-RepetitionMsg3-r17 ENUMERATED {supported} OPTIONAL,

 sharedSpectrumChAccessParamsPerBand-v1710 SharedSpectrumChAccessParamsPerBand-v1710 OPTIONAL,

 -- R4 25-2: Parallel measurements on cells belonging to a different NGSO satellite than a serving satellite without scheduling restrictions

 -- on normal operations with the serving cell

 parallelMeasurementWithoutRestriction-r17 ENUMERATED {supported} OPTIONAL,

 -- R4 25-5: Parallel measurements on multiple NGSO satellites within a SMTC

 maxNumber-NGSO-SatellitesWithinOneSMTC-r17 ENUMERATED {n1, n2, n3, n4} OPTIONAL,

 -- R1 26-10: K1 range extension

 k1-RangeExtension-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 35-1: Aperiodic CSI-RS for tracking for fast SCell activation

 aperiodicCSI-RS-FastScellActivation-r17 SEQUENCE {

 maxNumberAperiodicCSI-RS-PerCC-r17 ENUMERATED {n8, n16, n32, n48, n64, n128, n255},

 maxNumberAperiodicCSI-RS-AcrossCCs-r17 ENUMERATED {n8, n16, n32, n64, n128, n256, n512, n1024}

 } OPTIONAL,

 -- R1 35-2: Aperiodic CSI-RS bandwidth for tracking for fast SCell activation for 10MHz UE channel bandwidth

 aperiodicCSI-RS-AdditionalBandwidth-r17 ENUMERATED {addBW-Set1, addBW-Set2} OPTIONAL,

 -- R1 28-1a: RRC-configured DL BWP without CD-SSB or NCD-SSB

 bwp-WithoutCD-SSB-OrNCD-SSB-RedCap-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 28-3: Half-duplex FDD operation type A for (e)RedCap UE

 halfDuplexFDD-TypeA-RedCap-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 27-15b: Positioning SRS transmission in RRC\_INACTIVE state configured outside initial UL BWP

 posSRS-RRC-Inactive-OutsideInitialUL-BWP-r17 PosSRS-RRC-Inactive-OutsideInitialUL-BWP-r17 OPTIONAL,

 -- R4 15-3 UE support of CBW for 480kHz SCS

 channelBWs-DL-SCS-480kHz-FR2-2-r17 BIT STRING (SIZE (8)) OPTIONAL,

 channelBWs-UL-SCS-480kHz-FR2-2-r17 BIT STRING (SIZE (8)) OPTIONAL,

 -- R4 15-4 UE support of CBW for 960kHz SCS

 channelBWs-DL-SCS-960kHz-FR2-2-r17 BIT STRING (SIZE (8)) OPTIONAL,

 channelBWs-UL-SCS-960kHz-FR2-2-r17 BIT STRING (SIZE (8)) OPTIONAL,

 -- R4 17-1 UL gap for Tx power management

 ul-GapFR2-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 25-4: One-shot HARQ ACK feedback triggered by DCI format 1\_2

 oneShotHARQ-feedbackTriggeredByDCI-1-2-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 25-5: PHY priority handling for one-shot HARQ ACK feedback

 oneShotHARQ-feedbackPhy-Priority-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 25-6: Enhanced type 3 HARQ-ACK codebook feedback

 enhancedType3-HARQ-CodebookFeedback-r17 SEQUENCE {

 enhancedType3-HARQ-Codebooks-r17 ENUMERATED {n1, n2, n4, n8},

 maxNumberPUCCH-Transmissions-r17 ENUMERATED {n1, n2, n3, n4, n5, n6, n7}

 } OPTIONAL,

 -- R1 25-7: Triggered HARQ-ACK codebook re-transmission

 triggeredHARQ-CodebookRetx-r17 SEQUENCE {

 minHARQ-Retx-Offset-r17 ENUMERATED {n-7, n-5, n-3, n-1, n1},

 maxHARQ-Retx-Offset-r17 ENUMERATED {n4, n6, n8, n10, n12, n14, n16, n18, n20, n22, n24}

 } OPTIONAL

 ]],

 [[

 -- R4 22-2 support of one shot large UL timing adjustment

 ue-OneShotUL-TimingAdj-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 25-2: Repetitions for PUCCH format 0, and 2 over multiple slots with K = 2, 4, 8

 pucch-Repetition-F0-2-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 25-11a: 4-bits subband CQI for NTN and unlicensed

 cqi-4-BitsSubbandNTN-SharedSpectrumChAccess-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 25-16: HARQ-ACK with different priorities multiplexing on a PUCCH/PUSCH

 mux-HARQ-ACK-DiffPriorities-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 25-20a: Propagation delay compensation based on Rel-15 TA procedure for NTN and unlicensed

 ta-BasedPDC-NTN-SharedSpectrumChAccess-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 33-2b: DCI-based enabling/disabling ACK/NACK-based feedback for dynamic scheduling for multicast

 ack-NACK-FeedbackForMulticastWithDCI-Enabler-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 33-2e: Multiple G-RNTIs for group-common PDSCHs

 maxNumberG-RNTI-r17 INTEGER (2..8) OPTIONAL,

 -- R1 33-2f: Dynamic multicast with DCI format 4\_2

 dynamicMulticastDCI-Format4-2-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 33-2i: Supported maximal modulation order for multicast PDSCH

 maxModulationOrderForMulticast-r17 CHOICE {

 fr1-r17 ENUMERATED {qam256, qam1024},

 fr2-r17 ENUMERATED {qam64, qam256}

 } OPTIONAL,

 -- R1 33-3-1: Dynamic Slot-level repetition for group-common PDSCH for TN and licensed

 dynamicSlotRepetitionMulticastTN-NonSharedSpectrumChAccess-r17 ENUMERATED {n8, n16} OPTIONAL,

 -- R1 33-3-1a: Dynamic Slot-level repetition for group-common PDSCH for NTN and unlicensed

 dynamicSlotRepetitionMulticastNTN-SharedSpectrumChAccess-r17 ENUMERATED {n8, n16} OPTIONAL,

 -- R1 33-4-1: DCI-based enabling/disabling NACK-only based feedback for dynamic scheduling for multicast

 nack-OnlyFeedbackForMulticastWithDCI-Enabler-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 33-5-1b: DCI-based enabling/disabling ACK/NACK-based feedback for dynamic scheduling for multicast

 ack-NACK-FeedbackForSPS-MulticastWithDCI-Enabler-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 33-5-1h: Multiple G-CS-RNTIs for SPS group-common PDSCHs

 maxNumberG-CS-RNTI-r17 INTEGER (2..8) OPTIONAL,

 -- R1 33-10: Support group-common PDSCH RE-level rate matching for multicast

 re-LevelRateMatchingForMulticast-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 36-1a: Support of 1024QAM for PDSCH with maximum 2 MIMO layers for FR1

 pdsch-1024QAM-2MIMO-FR1-r17 ENUMERATED {supported} OPTIONAL,

 -- R4 14-3 PRS measurement without MG

 prs-MeasurementWithoutMG-r17 ENUMERATED {cpLength, quarterSymbol, halfSymbol, halfSlot} OPTIONAL,

 -- R4 25-7: The number of target NGSO satellites the UE can monitor per carrier

 maxNumber-NGSO-SatellitesPerCarrier-r17 INTEGER (3..4) OPTIONAL,

 -- R1 27-3-3 DL PRS Processing Capability outside MG - buffering capability

 prs-ProcessingCapabilityOutsideMGinPPW-r17 SEQUENCE (SIZE(1..3)) OF PRS-ProcessingCapabilityOutsideMGinPPWperType-r17 OPTIONAL,

 -- R1 27-15a: Positioning SRS transmission in RRC\_INACTIVE state for initial UL BWP with semi-persistent SRS

 srs-SemiPersistent-PosResourcesRRC-Inactive-r17 SEQUENCE {

 maxNumOfSemiPersistentSRSposResources-r17 ENUMERATED {n1, n2, n4, n8, n16, n32, n64},

 maxNumOfSemiPersistentSRSposResourcesPerSlot-r17 ENUMERATED {n1, n2, n3, n4, n5, n6, n8, n10, n12, n14}

 } OPTIONAL,

 -- R2: UE support of CBW for 120kHz SCS

 channelBWs-DL-SCS-120kHz-FR2-2-r17 BIT STRING (SIZE (8)) OPTIONAL,

 channelBWs-UL-SCS-120kHz-FR2-2-r17 BIT STRING (SIZE (8)) OPTIONAL

 ]],

 [[

 -- R1 30-4a: DM-RS bundling for PUSCH repetition type A

 dmrs-BundlingPUSCH-RepTypeA-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 30-4b: DM-RS bundling for PUSCH repetition type B

 dmrs-BundlingPUSCH-RepTypeB-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 30-4c: DM-RS bundling for TB processing over multi-slot PUSCH

 dmrs-BundlingPUSCH-multiSlot-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 30-4d: DMRS bundling for PUCCH repetitions

 dmrs-BundlingPUCCH-Rep-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 30-4e: Enhanced inter-slot frequency hopping with inter-slot bundling for PUSCH

 interSlotFreqHopInterSlotBundlingPUSCH-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 30-4f: Enhanced inter-slot frequency hopping for PUCCH repetitions with DMRS bundling

 interSlotFreqHopPUCCH-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 30-4g: Restart DM-RS bundling

 dmrs-BundlingRestart-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 30-4h: DM-RS bundling for non-back-to-back transmission

 dmrs-BundlingNonBackToBackTX-r17 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 -- R1 33-5-1e: Dynamic Slot-level repetition for SPS group-common PDSCH for multicast

 maxDynamicSlotRepetitionForSPS-Multicast-r17 ENUMERATED {n8, n16} OPTIONAL,

 -- R1 33-5-1g: DCI-based enabling/disabling NACK-only based feedback for SPS group-common PDSCH for multicast

 nack-OnlyFeedbackForSPS-MulticastWithDCI-Enabler-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 33-5-1i: Multicast SPS scheduling with DCI format 4\_2

 sps-MulticastDCI-Format4-2-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 33-5-2: Multiple SPS group-common PDSCH configuration on PCell

 sps-MulticastMultiConfig-r17 INTEGER (1..8) OPTIONAL,

 -- R1 33-6-1: DL priority indication for multicast in DCI

 priorityIndicatorInDCI-Multicast-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 33-6-1a: DL priority configuration for SPS multicast

 priorityIndicatorInDCI-SPS-Multicast-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 33-6-2: Two HARQ-ACK codebooks simultaneously constructed for supporting HARQ-ACK codebooks with different priorities

 -- for unicast and multicast at a UE

 twoHARQ-ACK-CodebookForUnicastAndMulticast-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 33-6-3: More than one PUCCH for HARQ-ACK transmission for multicast or for unicast and multicast within a slot

 multiPUCCH-HARQ-ACK-ForMulticastUnicast-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 33-9: Supporting unicast PDCCH to release SPS group-common PDSCH

 releaseSPS-MulticastWithCS-RNTI-r17 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 -- R1 41-3-1a UE automomous TA adjustment when cell-reselection happens

 posUE-TA-AutoAdjustment-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 41-3-1: SRS for positioning configuration in multiple cells for UEs in RRC\_INACTIVE state for initial UL BWP

 posSRS-ValidityAreaRRC-InactiveInitialUL-BWP-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 41-3-2: SRS for positioning configuration in multiple cells for UEs in RRC\_INACTIVE state for configured outside

 -- initial UL BWP

 posSRS-ValidityAreaRRC-InactiveOutsideInitialUL-BWP-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 41-5-1:PRS measurement with Rx frequency hopping within a MG and measurement reporting RRC\_CONNECTED for RedCap UEs

 dl-PRS-MeasurementWithRxFH-RRC-ConnectedForRedCap-r18 DL-PRS-MeasurementWithRxFH-RRC-Connected-r18 OPTIONAL,

 -- R1 41-5-2: Support of positioning SRS with Tx frequency hopping in RRC\_CONNECTED for RedCap UEs

 posSRS-TxFH-RRC-ConnectedForRedCap-r18 PosSRS-TxFrequencyHoppingRRC-Connected-r18 OPTIONAL,

 -- R1 41-5-2a: Support of positioning SRS with Tx frequency hopping in RRC\_INACTIVE for RedCap UEs

 posSRS-TxFH-RRC-InactiveForRedCap-r18 PosSRS-TxFrequencyHoppingRRC-Inactive-r18 OPTIONAL,

 -- R1 41-4-8: Support of Positioning SRS bandwidth aggregation in RRC\_INACTIVE

 posSRS-BWA-RRC-Inactive-r18 PosSRS-BWA-RRC-Inactive-r18 OPTIONAL,

 -- R1 41-4-6a support a Rel-17 single DCI scheduling positioning SRS resource sets across the linked carriers

 -- for SRS bandwidth aggregation in RRC\_CONNECTED state

 posJointTriggerBySingleDCI-RRC-Connected-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 41-5-1a PRS measurement with Rx frequency hopping in RRC\_INACTIVE for RedCap UEs

 dl-PRS-MeasurementWithRxFH-RRC-InactiveforRedCap-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 41-5-1b PRS measurement with Rx frequency hopping in RRC\_IDLE for RedCap UEs

 dl-PRS-MeasurementWithRxFH-RRC-IdleforRedCap-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 42-1: Spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s) for periodic CSI reporting

 spatialAdaptation-CSI-Feedback-r18 SEQUENCE {

 csiFeedbackType-r18 ENUMERATED {sdType1, sdType2, both},

 maxNumberLmax-r18 INTEGER (2..4),

 maxNumberCSI-ResourcePerCC-r18 SEQUENCE {

 sdType1-Resource-r18 INTEGER (1..32),

 sdType2-Resource-r18 INTEGER (1..32)

 },

 maxNumberTotalCSI-ResourcePerCC-r18 SEQUENCE {

 sdType1-Resource-r18 ENUMERATED {n8, n16, n24, n32, n64, n128},

 sdType2-Resource-r18 ENUMERATED {n8, n16, n24, n32, n64, n128}

 },

 totalNumberCSI-Reporting-r18 INTEGER (2..4)

 } OPTIONAL,

 -- R1 42-1a: Spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s) for periodic CSI

 -- reporting on PUSCH

 spatialAdaptation-CSI-FeedbackPUSCH-r18 SEQUENCE {

 csiFeedbackType-r18 ENUMERATED {sdType1, sdType2, both},

 maxNumberLmax-r18 INTEGER (2..8),

 subReportCSI-r18 INTEGER (2..4),

 maxNumberCSI-ResourcePerCC-r18 INTEGER (1..32),

 maxNumberTotalCSI-ResourcePerCC-r18 ENUMERATED {n8, n16, n24, n32, n64, n128},

 totalNumberCSI-Reporting-r18 INTEGER (2..12)

 } OPTIONAL,

 -- R1 42-1b: Spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s) for aperiodic CSI reporting

 spatialAdaptation-CSI-FeedbackAperiodic-r18 SEQUENCE {

 csiFeedbackType-r18 ENUMERATED {sdType1, sdType2, both},

 maxNumberLmax-r18 INTEGER (2..8),

 subReportCSI-r18 INTEGER (2..4),

 maxNumberCSI-ResourcePerCC-r18 SEQUENCE {

 sdType1-Resource-r18 INTEGER (1..32),

 sdType2-Resource-r18 INTEGER (1..32)

 },

 maxNumberTotalCSI-ResourcePerCC-r18 SEQUENCE {

 sdType1-Resource-r18 ENUMERATED {n8, n16, n24, n32, n64, n128},

 sdType2-Resource-r18 ENUMERATED {n8, n16, n24, n32, n64, n128}

 },

 totalNumberCSI-Reporting-r18 INTEGER (2..12)

 } OPTIONAL,

 -- R1 42-1c: Spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s) for semi-persistent

 -- CSI reporting on PUCCH

 spatialAdaptation-CSI-FeedbackPUCCH-r18 SEQUENCE {

 csiFeedbackType-r18 ENUMERATED {sdType1, sdType2, both},

 maxNumberLmax-r18 INTEGER (2..4),

 subReportCSI-r18 INTEGER (2..4),

 maxNumberCSI-ResourcePerCC-r18 INTEGER (1..32),

 maxNumberTotalCSI-ResourcePerCC-r18 ENUMERATED {n8, n16, n24, n32, n64, n128},

 totalNumberCSI-Reporting-r18 INTEGER (2..4)

 } OPTIONAL,

 -- R1 42-2: Power domain adaptation with CSI feedback based on CSI report sub-configuration(s) for periodic CSI reporting

 powerAdaptation-CSI-Feedback-r18 SEQUENCE {

 maxNumberLmax-r18 INTEGER (2..4),

 maxNumberCSI-ResourcePerCC-r18 INTEGER (1..32),

 maxNumberTotalCSI-ResourcePerCC-r18 ENUMERATED {n8, n16, n24, n32, n64, n128},

 totalNumberCSI-Reporting-r18 INTEGER (2..4)

 } OPTIONAL,

 -- R1 42-2a: Power domain adaptation with CSI feedback based on CSI report sub-configuration(s) for semi-persistent CSI

 -- reporting on PUSCH

 powerAdaptation-CSI-FeedbackPUSCH-r18 SEQUENCE {

 maxNumberLmax-r18 INTEGER (2..8),

 subReportCSI-r18 INTEGER (2..4),

 maxNumberCSI-ResourcePerCC-r18 INTEGER (1..32),

 maxNumberTotalCSI-ResourcePerCC-r18 ENUMERATED {n8, n16, n24, n32, n64, n128},

 totalNumberCSI-Reporting-r18 INTEGER (2..12)

 } OPTIONAL,

 -- R1 42-2b: Power domain adaptation with CSI feedback based on CSI report sub-configuration(s) for aperiodic CSI reporting

 powerAdaptation-CSI-FeedbackAperiodic-r18 SEQUENCE {

 maxNumberLmax-r18 INTEGER (2..8),

 subReportCSI-r18 INTEGER (2..4),

 maxNumberCSI-ResourcePerCC-r18 INTEGER (1..32),

 maxNumberTotalCSI-ResourcePerCC-r18 ENUMERATED {n8, n16, n24, n32, n64, n128},

 totalNumberCSI-Reporting-r18 INTEGER (2..12)

 } OPTIONAL,

 -- R1 42-2c: Power domain adaptation with CSI feedback based on CSI report sub-configuration(s) for semi-persistent CSI

 -- reporting on PUCCH

 powerAdaptation-CSI-FeedbackPUCCH-r18 SEQUENCE {

 maxNumberLmax-r18 INTEGER (2..4),

 subReportCSI-r18 INTEGER (2..4),

 maxNumberCSI-ResourcePerCC-r18 INTEGER (1..32),

 maxNumberTotalCSI-ResourcePerCC-r18 ENUMERATED {n8, n16, n24, n32, n64, n128},

 totalNumberCSI-Reporting-r18 INTEGER (2..4)

 } OPTIONAL,

 -- R1 42-4: Cell DTX and/or DRX operation based on RRC configuration

 nes-CellDTX-DRX-r18 ENUMERATED {cellDTXonly, cellDRXonly, both} OPTIONAL,

 -- R1 42-5: Cell DTX/DRX operation triggered by DCI format 2\_9

 nes-CellDTX-DRX-DCI2-9-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 42-7: Mixed codebook combination for spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s),

 -- each containing one port subset configuration

 mixCodeBookSpatialAdaptation-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 42-8: the number of CSI report(s) for which the UE can measure and process reference signals simultaneously in a CC of the

 -- band for which this capability is provided.

 simultaneousCSI-SubReportsPerCC-r18 INTEGER (1..8) OPTIONAL,

 -- R1 44-2: NTN DMRS bundling enhancement for PUSCH in NGSO scenarios

 ntn-DMRS-BundlingNGSO-r18 ENUMERATED {n4, n8, n16, n32} OPTIONAL,

 -- R1 45-3: Beam indication with joint DL/UL LTM TCI states

 ltm-BeamIndicationJointTCI-r18 SEQUENCE {

 maxNumberJointTCI-PerCell-r18 ENUMERATED {n8,n12,n16,n24,n32,n48,n64,n128},

 qcl-Resource-r18 ENUMERATED {ssb, trs, both},

 maxNumberJointTCI-AcrossCells-r18 INTEGER (1..128),

 maxNumberCells-r18 INTEGER (1..8)

 } OPTIONAL,

 dummy-ltm-MAC-CE-JointTCI-r18 SEQUENCE {

 qcl-Resource-r18 ENUMERATED {ssb, trs, both},

 maxNumberJointTCI-PerCell-r18 INTEGER (1..16),

 maxNumberJointTCI-AcrossCells-r18 ENUMERATED {n1,n2,n3,n4,n8,n16,n32}

 } OPTIONAL,

 -- R1 45-4: Beam indication with separate DL/UL LTM TCI states

 ltm-BeamIndicationSeparateTCI-r18 SEQUENCE {

 maxNumberDL-TCI-PerCell-r18 ENUMERATED {n4,n8,n12,n16,n24,n32,n48,n64,n128},

 maxNumberUL-TCI-PerCell-r18 ENUMERATED {n4,n8,n12,n16,n24,n32,n48,n64},

 qcl-Resource-r18 ENUMERATED {ssb, trs, both},

 maxNumberDL-TCI-AcrossCells-r18 INTEGER (1..128),

 maxNumberUL-TCI-AcrossCells-r18 INTEGER (1..64),

 maxNumberCells-r18 INTEGER (1..8)

 } OPTIONAL,

 dummy-ltm-MAC-CE-SeparateTCI-r18 SEQUENCE {

 qcl-Resource-r18 ENUMERATED {ssb, trs, both},

 maxNumberDL-TCI-PerCell-r18 INTEGER (1..8),

 maxNumberUL-TCI-PerCell-r18 INTEGER (1..8),

 maxNumberDL-TCI-AcrossCells-r18 ENUMERATED {n1,n2,n4,n8,n16},

 maxNumberUL-TCI-AcrossCells-r18 ENUMERATED {n1,n2,n4,n8,n16}

 } OPTIONAL,

 -- R1 45-5: RACH-based early TA acquisition

 rach-EarlyTA-Measurement-r18 INTEGER (1..8) OPTIONAL,

 -- R1 45-6: UE-based TA measurement

 ue-TA-Measurement-r18 INTEGER (1..8) OPTIONAL,

 -- R1 45-7: TA indication in cell switch command

 ta-IndicationCellSwitch-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 49-8: Triggered HARQ-ACK codebook re-transmission for DCI format 1\_3

 triggeredHARQ-CodebookRetxDCI-1-3-r18 SEQUENCE {

 minHARQ-Retx-Offset-r18 ENUMERATED {n-7, n-5, n-3, n-1, n1},

 maxHARQ-Retx-Offset-r18 ENUMERATED {n4, n6, n8, n10, n12, n14, n16, n18, n20, n22, n24}

 } OPTIONAL,

 -- R1 49-12: Unified TCI with joint DL/UL TCI update by DCI format 1\_3 for intra-cell and inter-cell beam management with more than

 -- one MAC-CE activated joint TCI state per CC

 unifiedJointTCI-MultiMAC-CE-DCI-1-3-r18 SEQUENCE {

 minBeamApplicationTime-r18 CHOICE {

 fr1-r18 SEQUENCE {

 scs-15kHz-r18 ENUMERATED {sym1, sym2, sym4, sym7, sym14, sym28, sym42, sym56, sym70} OPTIONAL,

 scs-30kHz-r18 ENUMERATED {sym1, sym2, sym4, sym7, sym14, sym28, sym42, sym56, sym70} OPTIONAL,

 scs-60kHz-r18 ENUMERATED {sym1, sym2, sym4, sym7, sym14, sym28, sym42, sym56, sym70} OPTIONAL

 },

 fr2-r18 SEQUENCE {

 scs-60kHz-r18 ENUMERATED {sym1, sym2, sym4, sym7, sym14, sym28, sym42, sym56, sym70,

 sym84, sym98, sym112, sym224, sym336} OPTIONAL,

 scs-120kHz-r18 ENUMERATED {sym1, sym2, sym4, sym7, sym14, sym28, sym42, sym56, sym70,

 sym84, sym98, sym112, sym224, sym336} OPTIONAL

 }

 },

 maxActivatedTCI-PerCC-r18 INTEGER (2..8) OPTIONAL

 } OPTIONAL,

 -- R1 49-12a: Unified TCI with separate DL/UL TCI update by DCI format 1\_3 for intra-cell beam management with more than

 -- one MAC-CE activated separate TCI state per CC

 unifiedSeparateTCI-MultiMAC-CE-IntraCell-r18 SEQUENCE {

 minBeamApplicationTime-r18 CHOICE {

 fr1-r18 SEQUENCE {

 scs-15kHz-r18 ENUMERATED {sym1, sym2, sym4, sym7, sym14, sym28, sym42, sym56, sym70,

 sym84, sym98, sym112, sym224, sym336} OPTIONAL,

 scs-30kHz-r18 ENUMERATED {sym1, sym2, sym4, sym7, sym14, sym28, sym42, sym56, sym70,

 sym84, sym98, sym112, sym224, sym336} OPTIONAL,

 scs-60kHz-r18 ENUMERATED {sym1, sym2, sym4, sym7, sym14, sym28, sym42, sym56, sym70,

 sym84, sym98, sym112, sym224, sym336} OPTIONAL

 },

 fr2-r18 SEQUENCE {

 scs-60kHz-r18 ENUMERATED {sym1, sym2, sym4, sym7, sym14, sym28, sym42, sym56, sym70,

 sym84, sym98, sym112, sym224, sym336} OPTIONAL,

 scs-120kHz-r18 ENUMERATED {sym1, sym2, sym4, sym7, sym14, sym28, sym42, sym56, sym70,

 sym84, sym98, sym112, sym224, sym336} OPTIONAL

 }

 },

 maxActivatedDL-TCI-PerCC-r18 INTEGER (2..8) OPTIONAL,

 maxActivatedUL-TCI-PerCC-r18 INTEGER (2..8) OPTIONAL

 } OPTIONAL,

 -- R1 50-1: Multi-PUSCHs for Configured Grant

 multiPUSCH-CG-r18 ENUMERATED {n16, n32} OPTIONAL,

 -- R1 50-1a: Multiple active multi-PUSCHs configured grant configurations for a BWP of a serving cell

 multiPUSCH-ActiveConfiguredGrant-r18 SEQUENCE {

 maxNumberConfigsPerBWP ENUMERATED {n1, n2, n4, n8, n12},

 maxNumberConfigsAllCC-FR1 INTEGER (2..32),

 maxNumberConfigsAllCC-FR2 INTEGER (2..32)

 } OPTIONAL,

 -- R1 50-1b: Joint release in a DCI for two or more configured grant Type 2 configurations, including multi-PUSCH CG

 -- configuration(s), for a given BWP of a serving cell

 jointReleaseDCI-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 50-2: UCI indication of unused CG-PUSCH transmission occasions

 cg-PUSCH-UTO-UCI-Ind-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 50-3: PDCCH monitoring resumption after UL NACK

 pdcch-MonitoringResumptionAfterUL-NACK-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 51-1: Support for 3 MHz symmetric channel bandwidth in DL and UL

 support3MHz-ChannelBW-Symmetric-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 51-1a: Support for 3 MHz channel bandwidth in uplink with larger than 3 MHz channel BW in DL

 support3MHz-ChannelBW-Asymmetric-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 51-2a: support 12 PRB CORESET0

 support12PRB-CORESET0-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 52-1: Reception of NR PDCCH candidates overlapping with LTE CRS REs

 nr-PDCCH-OverlapLTE-CRS-RE-r18 SEQUENCE {

 overlapInRE-r18 ENUMERATED {oneSymbolNoOverlap, someOrAllSymOverlap},

 overlapInSymbol-r18 ENUMERATED {symbol2,symbol1And2}

 } OPTIONAL,

 -- R1 52-1a: Reception of NR PDCCH candidates overlapping with LTE CRS REs with multiple non-overlapping CRS rate matching patterns

 nr-PDCCH-OverlapLTE-CRS-RE-MultiPatterns-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 52-1b: NR PDCCH reception that overlaps with LTE CRS within a single span of 3 consecutive OFDM symbols that is within the

 -- first 4 OFDM symbols in a slot

 nr-PDCCH-OverlapLTE-CRS-RE-Span-3-4-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 52-2: Two LTE-CRS overlapping rate matching patterns within NR 15 kHz carrier overlapping with LTE carrier (regardless of

 -- support or configuration of multi-TRP)

 twoRateMatchingEUTRA-CRS-patterns-3-4-r18 SEQUENCE {

 maxNumberPatterns-r18 INTEGER (2..6),

 maxNumberNon-OverlapPatterns-r18 INTEGER (1..3)

 } OPTIONAL,

 -- R1 52-2a: Two LTE-CRS overlapping rate matching patterns with two different values of coresetPoolIndex within NR 15 kHz carrier

 -- overlapping with LTE carrier

 overlapRateMatchingEUTRA-CRS-Patterns-3-4-Diff-CS-Pool-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 53-3: Support RLM/BM/BFD measurements based on NCD-SSB within active BWP

 ncd-SSB-BWP-Wor-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 53-4: Support Support RLM/BM/BFD measurements based on CSI-RS when CD-SSB is outside active BWP

 rlm-BM-BFD-CSI-RS-OutsideActiveBWP-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 54-1: PRACH coverage enhancements

 prach-CoverageEnh-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 54-1a: PRACH repetitions with less than N symbols gap

 prach-Repetition-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 54-3: Dynamic waveform switching

 dynamicWaveformSwitch-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 54-3a: PHR enhancement for dynamic waveform switching

 dynamicWaveformSwitchPHR-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 54-3b: Dynamic waveform switching for intra-band UL CA

 dynamicWaveformSwitchIntraCA-r18 INTEGER (2..8) OPTIONAL,

 -- R1 55-3: Multiple PUSCHs scheduling by single DCI for non-consecutive slots in FR1

 multiPUSCH-SingleDCI-NonConsSlots-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 55-2d: single-symbol DL-PRS used in RTT-based Propagation delay compensation

 pdc-maxNumberPRS-ResourceProcessedPerSlot-r18 SEQUENCE {

 fr1-r18 SEQUENCE {

 scs-15kHz-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24, n32, n48, n64} OPTIONAL,

 scs-30kHz-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24, n32, n48, n64} OPTIONAL,

 scs-60kHz-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24, n32, n48, n64} OPTIONAL

 },

 fr2-r18 SEQUENCE {

 scs-60kHz-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24, n32, n48, n64} OPTIONAL,

 scs-120kHz-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24, n32, n48, n64} OPTIONAL

 }

 } OPTIONAL,

 -- R1 57-2: Intra-slot TDM-ed unicast PDSCH and group-common PDSCH for multicast in RRC\_INACTIVE state

 intraSlot-PDSCH-MulticastInactive-r18 BOOLEAN OPTIONAL,

 -- R1 57-1: Dynamic scheduling for multicast in RRC\_INACTIVE state

 multicastInactive-r18 ENUMERATED {supported} OPTIONAL,

 thresholdBasedMulticastResume-r18 ENUMERATED {supported} OPTIONAL,

 -- R4 27-2: LowerMSD for inter-band NR CA and EN-DC

 lowerMSD-r18 SEQUENCE (SIZE (1..maxLowerMSD-r18)) OF LowerMSD-r18 OPTIONAL,

 lowerMSD-ENDC-r18 SEQUENCE (SIZE (1..maxLowerMSD-r18)) OF LowerMSD-r18 OPTIONAL,

 -- R4 28-1: Enhanced channel raster

 enhancedChannelRaster-r18 ENUMERATED {supported} OPTIONAL,

 -- R4 30-2: Fast beam sweeping for layer-1 measurement when the UE is in multi-Rx operation

 fastBeamSweepingMultiRx-r18 ENUMERATED {n2,n4,n6} OPTIONAL,

 -- R4 31-2 Beam sweeping factor reduction for FR2 unknown SCell activation

 beamSweepingFactorReduction-r18 SEQUENCE {

 reduceForCellDetection ENUMERATED {n1, n2, n4, n6},

 reduceForSSB-L1-RSRP-Meas INTEGER (0..7)

 } OPTIONAL,

 -- R4 34-1: Support of NR FR2 HST with simultaneous DL reception with two different QCL TypeD RSs

 simultaneousReceptionTwoQCL-r18 ENUMERATED {supported} OPTIONAL,

 -- R4 34-2: Enhanced FR2 HST RRM requirements for intra-band CA and inter-frequency measurements in connected mode

 measEnhCAInterFreqFR2-r18 ENUMERATED {supported} OPTIONAL,

 -- R4 34-4: Support of enhanced MAC CE for TCI state switch indication for FR2 HST

 tci-StateSwitchInd-r18 ENUMERATED {supported} OPTIONAL,

 -- R4 35-2: the requirements defined for ATG UE with antenna array or omni-direction antenna requirements.

 antennaArrayType-r18 ENUMERATED {supported} OPTIONAL,

 locationBasedCondHandoverATG-r18 ENUMERATED {supported} OPTIONAL,

 -- R4 35-3: rated maximum output power value range from 23dBm to 40dBm with 1dB as granularity at maximum modulation order and full

 -- PRB configurations.

 maxOutputPowerATG-r18 INTEGER (1..18) OPTIONAL,

 -- R4 39-6: Fast processing of LTM candidate cell RRC configuration

 ltm-FastProcessingConfig-r18 SEQUENCE {

 maxNumberStoredConfigCells-r18 ENUMERATED {n2,n3,n4,n5,n6,n7,n8,n9,n10,n11,n12,n16},

 maxNumberConfigs-r18 INTEGER (1..4)

 } OPTIONAL,

 -- R4 39-8: Measurement validation based on EMR measurement during connection setup/resume

 measValidationReportEMR-r18 ENUMERATED {supported} OPTIONAL,

 -- R4 39-9: Measurement validation based on reselection measurement during connection setup/resume

 measValidationReportReselectionMeasurements-r18 ENUMERATED {supported} OPTIONAL,

 eventA4BasedCondHandoverNES-r18 ENUMERATED {supported} OPTIONAL,

 nesBasedCondHandoverWithDCI-r18 ENUMERATED {supported} OPTIONAL,

 rach-LessHandoverCG-r18 ENUMERATED {supported} OPTIONAL,

 rach-LessHandoverDG-r18 ENUMERATED {supported} OPTIONAL,

 locationBasedCondHandoverEMC-r18 ENUMERATED {supported} OPTIONAL,

 mt-CG-SDT-r18 ENUMERATED {supported} OPTIONAL,

 posSRS-PreconfigureRRC-InactiveInitialUL-BWP-r18 ENUMERATED {supported} OPTIONAL,

 posSRS-PreconfigureRRC-InactiveOutsideInitialUL-BWP-r18 ENUMERATED {supported} OPTIONAL,

 cg-SDT-PeriodicityExt-r18 ENUMERATED {supported} OPTIONAL,

 -- R2: 2Rx XR UEs

 supportOf2RxXR-r18 ENUMERATED {supported} OPTIONAL,

 condHandoverWithCandSCG-change-r18 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 mac-ParametersPerBand-r18 MAC-ParametersPerBand-r18 OPTIONAL,

 channelBW-DL-NCR-r18 CHOICE {

 fr1-100mhz SEQUENCE {

 scs-15kHz ENUMERATED {supported} OPTIONAL,

 scs-30kHz ENUMERATED {supported} OPTIONAL,

 scs-60kHz ENUMERATED {supported} OPTIONAL

 },

 fr2-200mhz SEQUENCE {

 scs-60kHz ENUMERATED {supported} OPTIONAL,

 scs-120kHz ENUMERATED {supported} OPTIONAL

 }

 } OPTIONAL,

 channelBW-UL-NCR-r18 CHOICE {

 fr1-100mhz SEQUENCE {

 scs-15kHz ENUMERATED {supported} OPTIONAL,

 scs-30kHz ENUMERATED {supported} OPTIONAL,

 scs-60kHz ENUMERATED {supported} OPTIONAL

 },

 fr2-200mhz SEQUENCE {

 scs-60kHz ENUMERATED {supported} OPTIONAL,

 scs-120kHz ENUMERATED {supported} OPTIONAL

 }

 } OPTIONAL,

 ncr-PDSCH-64QAM-FR2-r18 ENUMERATED {supported} OPTIONAL,

 ltm-MCG-IntraFreq-r18 ENUMERATED {supported} OPTIONAL,

 ltm-SCG-IntraFreq-r18 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 -- R1 45-3a: MAC-CE activated joint LTM TCI states

 ltm-MAC-CE-JointTCI-r18 SEQUENCE {

 qcl-Resource-r18 ENUMERATED {ssb, trs, both},

 maxNumberJointTCI-PerCell-r18 INTEGER (1..16),

 maxNumberJointTCI-AcrossCells-r18 INTEGER (1..32)

 } OPTIONAL,

 -- R1 45-4a: MAC-CE activated DL/UL LTM TCI states

 ltm-MAC-CE-SeparateTCI-r18 SEQUENCE {

 qcl-Resource-r18 ENUMERATED {ssb, trs, both},

 maxNumberDL-TCI-PerCell-r18 INTEGER (1..8),

 maxNumberUL-TCI-PerCell-r18 INTEGER (1..8),

 maxNumberDL-TCI-AcrossCells-r18 INTEGER (1..32),

 maxNumberUL-TCI-AcrossCells-r18 INTEGER (1..32)

 } OPTIONAL

 ]]

}

BandNR-v16c0 ::= SEQUENCE {

 pusch-RepetitionTypeA-v16c0 ENUMERATED {supported} OPTIONAL,

 ...

}

BandNR-v17b0 ::= SEQUENCE {

 mimo-ParametersPerBand-v17b0 MIMO-ParametersPerBand-v17b0 OPTIONAL,

 ...

}

LowerMSD-r18 ::= SEQUENCE {

 aggressorband1-r18 CHOICE {

 nr FreqBandIndicatorNR,

 eutra FreqBandIndicatorEUTRA

 },

 aggressorband2-r18 FreqBandIndicatorNR OPTIONAL,

 msd-Information-r18 SEQUENCE (SIZE (1..maxLowerMSDInfo-r18)) OF MSD-Information-r18

}

MSD-Information-r18 ::= SEQUENCE {

 msd-Type-r18 ENUMERATED {harmonic, harmonicMixing, crossBandIsolation, imd2, imd3, imd4, imd5, all, spare8, spare7,

 spare6, spare5,spare4, spare3, spare2, spare1},

 msd-PowerClass-r18 ENUMERATED {pc1dot5, pc2, pc3},

 msd-Class-r18 ENUMERATED {classI, classII, classIII, classIV, classV, classVI, classVII, classVIII }

}

-- TAG-RF-PARAMETERS-STOP

-- ASN1STOP

|  |
| --- |
| *RF-Parameters* field descriptions |
| ***appliedFreqBandListFilter***In this field the UE mirrors the *FreqBandList* that the NW provided in the capability enquiry, if any, as described in clause 5.6.1.4. The UE filtered the band combinations in the *supportedBandCombinationList* in accordance with this *appliedFreqBandListFilter*. The UE does not include this field if the UE capability is requested by E-UTRAN and the network request includes the field *eutra-nr-only* [10]. |
| ***dummy1, dummy2, dummy-ltm-MAC-CE-JointTCI-r18, dummy-ltm-MAC-CE-SeparateTCI-r18***The fields are not used in the specification and the network ignores the received values. |
| ***supportedBandCombinationList***A list of band combinations that the UE supports for NR (and NR-DC, if requested). The *FeatureSetCombinationId*:s in this list refer to the *FeatureSetCombination* entries in the *featureSetCombinations* list in the *UE-NR-Capability* IE. The UE does not include this field if the UE capability is requested by E-UTRAN and the network request includes the field *eutra-nr-only* [10]. |
| ***supportedBandCombinationListSidelinkEUTRA-NR***A list of band combinations that the UE supports for NR sidelink communication only, for joint NR sidelink communication and V2X sidelink communication, or for V2X sidelink communication only. The UE does not include this field if the UE capability is requested by E-UTRAN (see TS 36.331[10]) and the network request includes the field *eutra-nr-only*. |
| ***supportedBandCombinationListSL-NonRelayDiscovery***A list of band combinations that the UE supports for NR sidelink non-relay discovery. The encoding is defined in PC5 *BandCombinationListSidelinkNR-r16.* |
| ***supportedBandCombinationListSL-RelayDiscovery***A list of band combinations that the UE supports for NR sidelink relay discovery. The encoding is defined in PC5 *BandCombinationListSidelinkNR-r16.* |
| ***supportedBandCombinationListSL-U2U-DiscoveryExt***This field indicates the band parameter in *BandCombinationListSL-Discovery-r17* that the UE supports for NR U2U sidelink relay discovery in a band included in *supportedBandCombinationListSL-U2U-RelayDiscovery*. |
| ***supportedBandCombinationListSL-U2U-RelayDiscovery***A list of band combinations that the UE supports for NR U2U sidelink relay discovery. The encoding is defined in PC5 *BandCombinationListSidelinkNR-r16.* |
| ***supportedBandCombinationList-UplinkTxSwitch***A list of band combinations that the UE supports dynamic uplink Tx switching for NR UL CA and SUL. The *FeatureSetCombinationId*:s in this list refer to the *FeatureSetCombination* entries in the *featureSetCombinations* list in the *UE-NR-Capability* IE. The UE does not include this field if the UE capability is requested by E-UTRAN and the network request includes the field *eutra-nr-only* [10]. |
| ***supportedBandListNR***A list of NR bands supported by the UE. If *supportedBandListNR-v16c0* is included, the UE shall include the same number of entries, and listed in the same order, as in *supportedBandListNR* (without suffix). |

End of second change