**3GPP TSG RAN WG2 #131 R2-250xxxx**

**Bangalore, India, Aug 25th – 29th, 2025**

**Title:** Draft LS on two-TA configuration and UE-initiated CSI reporting

**Response to:** -

**Release:** Rel-19

**Work Items:** NR\_MIMO\_Ph5

**Source:** Samsung (to be RAN WG2)

**To:** RAN WG1

**CC:** -

**Contact Person:**

#### Name: Shiyang Leng

E-mail Address: shiyang.leng@samsung.com

**Send any reply LS to: 3GPP Liaisons Coordinator,** [**mailto:3GPPLiaison@etsi.org**](mailto:3GPPLiaison@etsi.org)

**Attachments: None**

**1. Overall Description:**

Regarding Rel-19 two-TA configuration and UE-initiated CSI reporting, RAN2 made the following agreements.

* RAN2 clarifies that the parameter that enables Rel-19 two-TA configuration (singleDCI-MultiTRP-2TA) is applied for both Rel-19 intra-cell 2TA without mDCI mTRP (including asymmetric TRP and symmetric TRP) and inter-cell 2TA without mDCI mTRP (i.e., ICBM). The corresponding parameter name and its field description will be updated to capture this agreement, and the agreement will be informed to RAN1 by LS.
* **UE does not transmit PUCCH and PUSCH for mode-B if either PUCCH or PUSCH (first valid type-1 CG occasion) is outside DRX Active Time, and if the PUCCH has been transmitted, UE does not transmit the PUSCH if type-1 CG occasion is outside DRX Active time. Inform RAN1 about this conclusion.**

**2. Actions:**

**To RAN WG1**

**ACTION:** RAN2 respectfully asks RAN1 to take the above agreements into account for future work.

**3. Dates of Next RAN WG2 Meetings:**

TSG RAN2 Meeting #131bis 13th – 17rd October, 2025 Prague, CZ

TSG RAN2 Meeting #132 17th – 21st November, 2025 Dallas, US