**3GPP TSG-CT WG1 Meeting #148C1-242779**

**Changsha, China, 15 -19 April 2024**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **24.583** | **CR** |  | **rev** | **1** | **Current version:** | **18.0.0** |  |
|  |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Resolve EN on UE identity |
|  |  |
| ***Source to WG:*** | vivo |
| ***Source to TSG:*** | C1 |
|  |  |
| ***Work item code:*** | PINAPP |  | ***Date:*** | 2024-04-07 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | The following EN is on UE identity:Editor’s note: The coding of UE identity should be revisited since the UE identity may contain "identity token", which is depending on SA3 and SA6 coordination.As per SA6 requirement, UE identity can be set both a UE identity or a identity token. The identity token is a pre-configured security token for PINAPP. It should be treated as a string from the protocol perspective. Hence the EN can be resolved. Please note that the XML body has already supported the UE identity as a string. So there is no impact on XML body. |
|  |  |
| ***Summary of change:*** | Remove the EN on UE identity |
|  |  |
| ***Consequences if not approved:*** | EN on UE identity is not resloved. |
|  |  |
| ***Clauses affected:*** | 7.2.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

**\* \* \* First Change \* \* \***

### 7.2.1 UE identity

This parameter is used to carry the UE identity contained in a PINAPP protocol message. The format of the UE identity is encoded as:

a) if GPSI is included: same as GPSI (see clause 28.8 of 3GPP TS 23.003 [x]); or

b) if identity token is included: a string with a variable length.

**\* \* \* End of Changes \* \* \***