**3GPP TSG-RAN WG2 Meeting # *R2-2505222***

**Bengaluru, India, Aug 25th –**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.3* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** | **0439** | **rev** |  | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Introduction of UAV mobility enhancements [UAV\_Mobility] | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | CATT, NTT DOCOMO, LG Electronics Inc., Kyocera, LGU+, China Telecom, NEC, SK Telecom, Qualcomm Incorporated, Ericsson, Nokia | | | | | | | | | |
| ***Source to TSG:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | 19 | | | | |  | ***Date:*** | | | 2025-08-15 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | B |  | | | | | ***Release:*** | | |  |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)  Rel-20 (Release 20)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | To introudce idle/inactive enhancement for UAV | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | To support the following mobility enhancements for UAV:   1. Altitude based SSB measurement for idle/inactive UE 2. UAV dedicated frequency for cell reselection | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Idle/inactive enhancements are not supported for UAV. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 3.1, 3.2, 5.2.4.1, 5.2.4.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | | **X** |  | Other core specifications | | | | TS 38.306 CR 1319  TS 38.300 CR 1004  TS 38.331 CR 5399 | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

|  |
| --- |
| CHANGE START |

## 3.1 Definitions

For the purposes of the present document, the following terms and definitions apply:

**2Rx XR UE**:two antenna port XR UE as specified in TS 38.101-1 [15].

**Acceptable Cell**: A cell that satisfies certain conditions as specified in 4.5.

**Allowed CAG list**: A per-PLMN list of CAG Identifiers the UE is allowed to access (see TS 23.501 [10])**.**

**Available PLMN(s)**: One or more PLMN(s) for which the UE has found at least one cell and read its PLMN identity(ies).

**Available SNPN(s)**: One or more SNPN(s) for which the UE has found at least one cell and read its SNPN identity(ies).

**Barred Cell**: A cell a UE is not allowed to camp on.

**CAG cell**: A cell broadcasting at least one Closed Access Group Identifier.

**Camped on a cell**: UE has completed the cell selection/reselection process and has chosen a cell. The UE monitors system information and (in most cases) paging information.

**Camped on any cell**: UE is in idle mode and has completed the cell selection/reselection process and has chosen a cell irrespective of PLMN identity.

**Closed Access Group Identifier**: Identifier of a CAG within a PLMN.

**Commercial Mobile Alert System**: Public Warning System that delivers *Warning Notifications* provided by *Warning Notification Providers* to CMAS capable UEs.

**Earth-fixed cell:** An NTN cell fixed with respect to a certain geographic area on the earth all the time. It can be provisioned by beam(s) continuously covering the same geographical areas all the time (e.g., the case of GSO satellites).

**Earth-moving cell**: An NTN cell moving on the ground. It can be provisioned by beam(s) whose coverage area slides over the Earth surface (e.g., the case of NGSO satellites generating fixed or non-steerable beams).

**eCall Only Mode**: A UE configuration option that allows the UE to register at 5GC and register in IMS to perform only eCall Over IMS, and a non-emergencyIMS call for test and/or terminal reconfiguration services.

**EHPLMN**:Any of the PLMN entries contained in the Equivalent HPLMN list TS 23.122 [9].

**Equivalent PLMN list**:List of PLMNs considered as equivalent by the UE for cell selection, cell reselection, and handover according to the information provided by the NAS.

**Equivalent SNPN list**:List of SNPNs considered as equivalent by the UE for cell selection, cell reselection, and handover according to the information provided by the NAS.

**eRedCap UE**:A UE with enhanced reduced capabilities as specified in clause 4.2.22 in TS 38.306 [24].

**Home PLMN**: A PLMN where the Mobile Country Code (MCC) and Mobile Network Code (MNC) of the PLMN identity are the same as the MCC and MNC of the IMSI.

**HSDN cell**: A cell that has higher priority than other cells for cell reselection for HSDN capable UE in a High-mobility state.

**Mobile-IAB cell**: As defined in TS 38.300 [2].

**Network Identifier**: Identifier of an SNPN in combination with a PLMN ID (TS 23.501 [10]).

**Non-Public Network**: A network deployed for non-public use, as defined in TS 22.261 [12].

**Non-terrestrial network**: An NG-RAN consisting of gNBs, which provides non-terrestrial NR access to UEs by means of an NTN payload embarked on an airborne or space-borne NTN vehicle and an NTN Gateway.

**NR sidelink communication**: AS functionality enabling at least V2X Communication as defined in TS 23.287 [16] and/or A2X Communication as defined in TS 23.256 [26], and ProSe communication (including ProSe non-Relay, UE-to-Network Relay communication and, UE-to-UE Relay communication including UE-to-UE Relay communication with integrated discovery) as defined in TS 23.304 [22], between two or more nearby UEs, using NR technology but not traversing any network node.

**NR sidelink discovery**: AS functionality enabling ProSe non-Relay Discovery, ProSe UE-to-Network Relay discovery and ProSe UE-to-UE Relay discovery for Proximity based Services as defined in TS 23.304 [22] between two or more nearby UEs, using NR technology but not traversing any network node.

**Process**: A local action in the UE invoked by an RRC procedure or an RRC\_IDLE or RRC\_INACTIVE state procedure.

**Quasi-Earth fixed cell**: An NTN cell fixed with respect to a certain geographic area on the earth during a certain time duration. It can be provisioned by beam(s) covering one geographic area for a limited period and a different geographic area during another period (e.g., the case of NGSO satellites generating steerable beams).

**Radio Access Technology**: Type of technology used for radio access, for instance NR or E-UTRA.

**Ranging/Sidelink Positioning**: AS functionality enabling ranging-based services and sidelink positioning as defined in TS 23.586 [25].

**RedCap UE:** A UE with reduced capabilities as specified in clause 4.2.21 in TS 38.306 [24].

**Registration Area**: (NAS) registration area is an area in which the UE may roam without a need to perform location registration, which is a NAS procedure.

**Registered PLMN**: This is the PLMN on which certain Location Registration outcomes have occurred, as specified in TS 23.122 [9].

**Registered SNPN**: This is the SNPN on which certain Location Registration outcomes have occurred, as specified in TS 23.122 [9].

**Reserved Cell**: A cell on which camping is not allowed, except for particular UEs, if so indicated in the system information.

**Selected PLMN**: This is the PLMN that has been selected by the NAS, either manually or automatically.

**Selected SNPN**: This is the SNPN that has been selected by the NAS, either manually or automatically.

**Serving cell**: The cell on which the UE is camped.

**Sidelink**: UE to UE interface for V2X sidelink communication defined in TS 23.287[16].

**SNPN Access Mode**: Mode of operation wherein UE only selects SNPNs (as defined in TS 23.501 [10]).

**SNPN identity**: An identifier of an SNPN comprising of a PLMN ID and an NID combination.

**Strongest cell**: The cell on a particular frequency that is considered strongest according to the layer 1 cell search procedure (TS 38.213 [4], TS 38.215 [11]).

**Suitable Cell**: This is a cell on which a UE may camp. For NR cell, the criteria are defined in clause 4.5, for E-UTRA cell in TS 36.304 [7].

**U2N Relay UE**: a UE that provides functionality to support connectivity to the network for U2N Remote UE(s).

**U2N Remote UE**: a UE that communicates with the network via a U2N Relay UE.

**U2U Relay UE**: a UE that provides functionality to support connectivity for U2U Remote UE(s).

**U2U Remote UE**: a UE that communicates with other UE(s) via a U2U Relay UE.

**V2X sidelink communication**: AS functionality enabling V2X Communication as defined in TS 23.285 [17], between nearby UEs, using E-UTRA technology but not traversing any network node.

**UAV Frequency**: A frequency that may have higher priority than other frequencies for cell reselection for Aerial UE.

## 3.2 Abbreviations

For the purposes of the present document, the abbreviations given in TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in TR 21.905 [1].

AS Access Stratum

ATG Air To Ground

CAG Closed Access Group

CAG-ID Closed Access Group Identifier

CMAS Commercial Mobile Alert System

CN Core Network

DCI Downlink Control Information

DRX Discontinuous Reception

DTX Discontinuous Transmission

eDRX Extended DRX

ETWS Earthquake and Tsunami Warning System

E-UTRA Evolved UMTS Terrestrial Radio Access

E-UTRAN Evolved UMTS Terrestrial Radio Access Network

GIN Group ID for Network selection

H-SFN Hyper System Frame Number

HRNN Human-Readable Network Name

HSDN High Speed Dedicated Network

IAB Integrated Access and Backhaul

IMSI International Mobile Subscriber Identity

L2 Layer-2

MBS Multicast/Broadcast Services

MBS FSAI MBS Frequency Selection Area Identity

MCC Mobile Country Code

MCCH MBS Control Channel

MICO Mobile Initiated Connection Only

MRB MBS Radio Bearer

MTCH MBS Traffic Channel

NAS Non-Access Stratum

NCR Network-Controlled Repeater

NCR-Fwd NCR Forwarding

NCR-MT NCR Mobile Termination

NES Network Energy Savings

NID Network Identifier

NPN Non-Public Network

NR NR Radio Access

NSAG Network Slice AS Group

NTN Non-Terrestrial Network

PEI Paging Early Indication

PEI-O Paging Early Indication-Occasion

PH Paging Hyperframe

PLMN Public Land Mobile Network

PTW Paging Time Window

RAT Radio Access Technology

RNA RAN-based Notification Area

RNAU RAN-based Notification Area Update

RRC Radio Resource Control

SDT Small Data Transmission

SL Sidelink

SNPN Stand-alone Non-Public Network

TN Terrestrial Network

TRS Tracking Reference Signal

U2N UE-to-Network

U2U UE-to-UE

UAC Unified Access Control

UAV Uncrewed Aerial Vehicles

UE User Equipment

UMTS Universal Mobile Telecommunications System

VSAT Very Small Aperture Terminal

V2X Vehicle to Everything

|  |
| --- |
| NEXT CHANGE |

#### 5.2.4.1 Reselection priorities handling

Absolute priorities of different NR frequencies or inter-RAT frequencies may be provided to the UE in the system information, in the *RRCRelease* message, or by inheriting from another RAT at inter-RAT cell (re)selection. In the case of system information, an NR frequency or inter-RAT frequency may be listed without providing a priority (i.e. the field *cellReselectionPriority* is absent for that frequency). If any fields with *cellReselectionPriority* or *nsag-CellReselectionPriority* are provided in dedicated signalling, the UE shall ignore any fields with *cellReselectionPriority* and *nsag-CellReselectionPriority* provided in system information.

When UE is in camped normally state, if it supports slice-based cell reselection and has received the network slice(s) and NSAG information from NAS to be used for cell reselection, UE shall derive reselection priorities according to clause 5.2.4.11.

NOTE 00: UE derives reselection priorities according to clause 5.2.4.11 also in case *SIB16* (see TS 38.331 [3]) is not broadcast in the camped cell.

If UE is in *camped on any cell* state, UE shall only apply the priorities provided by system information from current cell, and the UE preserves priorities provided by dedicated signalling and *deprioritisationReq* received in *RRCRelease* unless specified otherwise. When the UE in camped normally state, has only dedicated priorities other than for the current frequency, the UE shall consider the current frequency to be the lowest priority frequency (i.e. lower than any of the network configured values). When the HSDN capable UE is in High-mobility state, the UE shall always consider the HSDN cells to be the highest priority (i.e., higher than any other network configured priorities). When the HSDN capable UE is not in High-mobility state, the UE shall always consider HSDN cells to be the lowest priority (i.e., lower than any other network configured priorities). The Aerial UE may consider the frequency to be the highest priority (i.e., higher than any other network configured priorities) if the frequency is configured with *uav-Frequency* without *uav-FrequencyAltitudeRange*. The Aerial UE may consider the frequency to be the highest priority if the frequency is configured with *uav-Frequency* and *uav-FrequencyAltitudeRange,* and if the Aerial UE is within the corresponding altitude range. If the UE is configured to perform both NR sidelink communication and V2X sidelink communication, the UE may consider the frequency providing both NR sidelink communication configuration and V2X sidelink communication configuration to be the highest priority. If the UE is configured to perform NR sidelink communication and not perform V2X communication, the UE may consider the frequency providing NR sidelink communication configuration to be the highest priority. If the UE is configured to perform V2X sidelink communication and not perform NR sidelink communication, the UE may consider the frequency providing V2X sidelink communication configuration to be the highest priority. If the UE is configured to perform ranging/sidelink positioning, the UE may consider the frequency providing ranging/sidelink positioning configuration to be the highest priority.

A UE on a vehicle with a mobile-IAB cell may consider the frequency for which a mobile-IAB cell is the best cell to be the highest priority. The UE identifies a mobile-IAB cell by *mobileIAB-Cell* in SIB1 (see TS 38.331 [3]). The UE may narrow its search scope for mobile-IAB cell(s) by *mobileIAB-CellList* if broadcasted in SIB4 (see TS 38.331 [3]). A non-mobile-IAB cell may be excluded from this mobile IAB frequency prioritization for up to 300 seconds.

NOTE 0a: The frequency only providing the anchor frequency configuration should not be prioritized for V2X service during cell reselection, as specified in TS 38.331[3].

NOTE 0b: When UE is configured to perform NR sidelink communication or V2X sidelink communication performs cell reselection, it may consider the frequencies providing the intra-carrier and inter-carrier configuration have equal priority in cell reselection.

NOTE 0c: The prioritization among the frequencies which UE considers to be the highest priority frequency is left to UE implementation unless otherwise stated.

NOTE 0d: The UE is configured to perform V2X sidelink communication or NR sidelink communication, if it has the capability and is authorized for the corresponding sidelink operation.

NOTE 0e: When UE is configured to perform both NR sidelink communication and V2X sidelink communication, but cannot find a frequency which can provide both NR sidelink communication configuration and V2X sidelink communication configuration, UE may consider the frequency providing either NR sidelink communication configuration or V2X sidelink communication configuration to be the highest priority.

NOTE 0f: Void.

NOTE 0g: How the UE determines itself to be on a vehicle with a mobile-IAB cell is left to the UE's implementation.

The UE shall only perform cell reselection evaluation for NR frequencies and inter-RAT frequencies that are given in system information and for which the UE has a priority provided.

If the MBS broadcast capable UE is receiving or interested to receive an MBS broadcast service(s) and can only receive this MBS broadcast service(s) by camping on a frequency on which it is provided, the UE may consider that frequency to be the highest priority during the MBS broadcast session as specified in TS 38.300 [2] as long as the two following conditions are fulfilled:

1) SIB1 scheduling information of the cell reselected by the UE due to frequency prioritization for MBS contains SIB20;

2) Either:

- One or more MBS FSAI(s) of that frequency is indicated in SIB21 of the serving cell and the same MBS FSAI(s) is also indicated for this MBS broadcast service in MBS User Service Description (USD) as specified in TS 26.517 [20], or

- SIB21 is not provided in the serving cell and that frequency is included in the USD of this service, or

- SIB21 is provided in the serving cell but does not provide the frequency mapping for the concerned service, and that frequency is included in the USD of this service.

NOTE 0g: It is up to UE implementation which frequency to select, when the USD provides multiple frequencies for the service the UE is interested in.

If the MBS broadcast capable UE is receiving or interested to receive an MBS broadcast service, the UE may consider cell reselection candidate frequencies at which it cannot receive the MBS broadcast service to be of the lowest priority during the MBS broadcast session as specified in TS 38.300 [2], as long as SIB1 scheduling information of the cell contains SIB20 on the MBS frequency which the UE monitors and as long as the condition 2) above is fulfilled for the serving cell.

NOTE 0h: Example scenarios in which such down-prioritisation may be needed include the cases where camping is not possible for the UE on the MBS broadcast frequency (e.g. the MBS broadcast frequency belongs to a PLMN different from UE's registered PLMN) while the UE can receive the MBS broadcast service when camped on another frequency than the MBS broadcast frequency or current frequency.

NOTE 0i: The frequency prioritization for MBS broadcast, NR sidelink communication, or V2X sidelink communication may override the re-selection priorities for slice-based cell reselection.

In case UE receives *RRCRelease* with *deprioritisationReq*, UE shall consider current frequency and stored frequencies due to the previously received *RRCRelease* with *deprioritisationReq* or all the frequencies of NR to be the lowest priority frequency (i.e. lower than any of the network configured values) while T325 is running irrespective of camped RAT. The UE shall delete the stored deprioritisation request(s) when a PLMN selection or SNPN selection is performed on request by NAS (TS 23.122 [9]).

NOTE 1: UE should search for a higher priority layer for cell reselection as soon as possible after the change of priority. The minimum related performance requirements specified in TS 38.133 [8] are still applicable.

NOTE 1a: The UE does not consider MBS broadcast, NR sidelink communication or V2X sidelink communication functionality to replace cell reselection priorities caused by HSDN, UAV or *deprioritisationReq* functionality.

The UE shall delete priorities provided by dedicated signalling when:

- the UE enters a different RRC state; or

- the optional validity time of dedicated priorities (T320) expires; or

- the UE receives an *RRCRelease* message with the field *cellReselectionPriorities* absent; or

- a PLMN selection or SNPN selection is performed on request by NAS (TS 23.122 [9]).

NOTE 2: Equal priorities between RATs are not supported.

The UE shall not consider any exclude-listed cells as candidate for cell reselection.

The UE shall consider only the allow-listed cells, if configured, as candidates for cell reselection.

NCR-MT may be configured with additional allowed cell list and/or forbidden cell list, see TS 38.300 [2]. The NCR-MT shall consider only the allowed cell list, if configured by OAM as candidates for cell reselection (ignore above exclude-listed cells and/or allow-listed cells). The NCR-MT shall not consider the cells for cell reselection in the forbidden cell list, if configured by OAM.

The UE in RRC\_IDLE state shall inherit the priorities provided by dedicated signalling and the remaining validity time (i.e. T320 in NR and E-UTRA), if configured, at inter-RAT cell (re)selection.

NOTE 3: The network may assign dedicated cell reselection priorities for frequencies not configured by system information.

#### 5.2.4.2 Measurement rules for cell re-selection

Following rules are used by the UE to limit needed measurements:

- If the serving cell fulfils Srxlev> SIntraSearchP and Squal > SIntraSearchQ:

- If *distanceThresh* and *referenceLocation* are broadcasted in *SIB19*, and if UE supports location-based measurement initiation for NTN (quasi-)Earth-fixed cell and has obtained its location information:

- If the distance between UE and the serving cell reference location *referenceLocation* is shorter than *distanceThresh*, the UE may not perform intra-frequency measurements;

- Else, the UE shall perform intra-frequency measurements;

- else if *distanceThresh* and *movingReferenceLocation* are broadcasted in *SIB19*, and if UE supports location-based measurement initiation for NTN Earth-moving cell and has obtained its location information:

- if the distance between UE's location and the serving cell reference location determined based on *movingReferenceLocation* is shorter than *distanceThresh*, the UE may not perform intra-frequency measurements;

- else, the UE shall perform intra-frequency measurements;

- Else, the UE may not perform intra-frequency measurements;

- Else, the UE shall perform intra-frequency measurements.

- The UE shall apply the following rules for NR inter-frequencies and inter-RAT frequencies which are indicated in system information and for which the UE has priority provided as defined in 5.2.4.1:

- For a NR inter-frequency or inter-RAT frequency with a reselection priority higher than the reselection priority of the current NR frequency, the UE shall perform measurements of higher priority NR inter-frequency or inter-RAT frequencies according to TS 38.133 [8].

- For a NR inter-frequency with an equal or lower reselection priority than the reselection priority of the current NR frequency and for inter-RAT frequency with lower reselection priority than the reselection priority of the current NR frequency:

- If the serving cell fulfils Srxlev > SnonIntraSearchP and Squal > SnonIntraSearchQ:

- If *distanceThresh* and *referenceLocation* are broadcasted in *SIB19*, and if UE supports location-based measurement initiation for NTN (quasi-)Earth-fixed cell and has obtained its UE location information:

- If the distance between UE and the serving cell reference location *referenceLocation* is shorter than *distanceThresh*, the UE may choose not to perform measurements of NR inter-frequency cells of equal or lower priority, or inter-RAT frequency cells of lower priority;

- Else, the UE shall perform measurements of NR inter-frequency cells of equal or lower priority, or inter-RAT frequency cells of lower priority according to TS 38.133 [8];

- else if *distanceThresh* and *movingReferenceLocation* are broadcasted in *SIB19*, and if UE supports location-based measurement initiation for NTN Earth-moving cell and has obtained its location information:

- if the distance between UE's location and the serving cell reference location determined based on *movingReferenceLocation* is shorter than *distanceThresh*, the UE may not perform measurements of NR inter-frequency cells of equal or lower priority, or inter-RAT frequency cells of lower priority;

- else, the UE shall perform measurements of NR inter-frequency cells of equal or lower priority, or inter-RAT frequency cells of lower priority according to TS 38.133 [8];

- Else, the UE may choose not to perform measurements of NR inter-frequency cells of equal or lower priority, or inter-RAT frequency cells of lower priority;

- Else,the UE shall perform measurements of NR inter-frequency cells of equal or lower priority, or inter-RAT frequency cells of lower priority according to TS 38.133 [8].

- If the UE supports relaxed measurement and *relaxedMeasurement* is present in *SIB2*, the UE may further relax the needed measurements, as specified in clause 5.2.4.9.

- For UE camping on NTN cell, if the UE supports skipping TN measurement, and the UE has obtained its location information, and if *coverageAreaInfoList* and *tn-AreaIdList* are broadcast in system information, the UE may not perform measurements of a TN frequency when UE is not in the coverage of that frequency provided via *tn-AreaIdList*, regardless of the frequency priority.

- For Aerial UE, if *ssb-ToMeasureAltitudeBasedList-19* is configured for the measurement frequency, when the UE is within an altitude range indicated by corresponding *altitudeRange-r18* in *ssb-ToMeasureAltitudeBasedList-r19*, it may prioritize the measurements on the SSB(s) configured in *ssb-ToMeasure-r18* *in ssb-ToMeasureAltitudeBasedList-r19.* Otherwise (i.e., the UE is within an altitude range indicated by corresponding *altitudeRange-r18* and *ssb-ToMeasure-r18* is absent in *ssb-ToMeasureAltitudeBasedList-r19*) it measures on all SS-blocks. When the UE is outside all the altitude ranges indicated by corresponding *altitudeRange-r18* (if any) in *ssb-ToMeasureAltitudeBasedList-r19*, *ssb-ToMeasure* (without suffix) applies.

If the *t-Service* of the serving cell is present in *SIB19*, and if UE supports time-based measurement initiation, the UE shall perform intra-frequency, inter-frequency or inter-RAT measurements before the *t-Service*, regardless of the distance between UE and the serving cell reference location or whether the serving cell fulfils Srxlev > SIntraSearchP and Squal > SIntraSearchQ, or Srxlev > SnonIntraSearchP and Squal > SnonIntraSearchQ, The exact time to start measurement before *t-Service* is up to UE implementation. UE shall perform measurements of higher priority NR inter-frequency or inter-RAT frequencies according to TS 38.133 [8] regardless of the remaining service time of the serving cell (i.e. time remaining until *t-Service*).

NOTE 1: When evaluating the distance between UE and the serving cell reference location, it is up to UE implementation to obtain UE location information.

NOTE 2: In the Earth-moving cell, it is up to UE implementation to maintain a valid serving cell reference location, which is derived based on the serving satellite ephemeris, *epochTime* and *movingReferenceLocation*.

|  |
| --- |
| CHANGE END |