**3GPP TSG-RAN WG3 Meeting #129-bisR3-257223**

Prague, Czech Republic, 13th ~17th Oct, 2025

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.3* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.423** | **CR** | **1583** | **Rev** | **1** | **Current version:** | **19.0.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **x** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Correction on CSI-RS Resource Set and CSI IM Resource Transfer for inter-CU LTM | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei, Jio Platforms, CATT, China Telecom, Lenovo, Nokia | | | | | | | | | |
| ***Source to TSG:*** | R3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** |  | | | | |  | ***Date:*** | | | 2025-10-14 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-19 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19) Rel-20 (Release 20)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | The following three IEs in the RRC LTM-Candidate IE needs further refined:   * ltm-NZP-CSI-RS-ResourceSet * ltm-CSI-IM-Resource * ltm-CSI-IM-ResourceSet   LTM modification is not supported in Rel-19 inter-CU LTM, while some redundant IEs for that function are still existing in the spec. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Toremove the magical words from the IEs in ASN.1.   * ltm-NZP-CSI-RS-ResourceSet * ltm-CSI-IM-Resource for periodic and semi-persistent * ltm-CSI-IM-ResourceSet for periodic and semi-persistent   To remove the “to Released List” related IEs for CSI-RS resource and CSI-IM resource. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Some functions of inter-CU LTM are not workable. Redundant IEs exist in the specification. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 9.2.3.224, 9.2.3.225, 9.2.3.226, 9.2.3.227, 9.3.5 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | | **x** |  | Other core specifications | | | | TS38.473 CR1633  TS/TR ... CR ... | | |
| ***affected:*** | |  | **x** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **x** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | v0, R3-257128, submission. | | | | | | | | |

**<< Start of Changes >>**

#### 9.2.3.224 CSI-RS Resource Configuration

This IE contains the CSI resource configuration used for LTM.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Periodic NZP CSI-RS Resource Configuration | O |  | 9.2.3.225 |  |
| Semi-Persistent NZP CSI-RS Resource Configuration | O |  | 9.2.3.225 |  |
| Periodic NZP CSI-RS Resource Set Configuration | O |  | 9.2.3.226 |  |
| Semi-Persistent NZP CSI-RS Resource Set Configuration | O |  | 9.2.3.226 |  |
| Periodic CSI-IM Resource Configuration | O |  | 9.2.3.227 |  |
| Semi-Persistent CSI-IM Resource Configuration | O |  | 9.2.3.227 |  |

#### 9.2.3.225 NZP CSI-RS Resource Configuration

This IE contains the CSI-RS resource configuration used for LTM.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| CSI-RS Resource to AddMod List | O |  | OCTET STRING | Includes the*ltm-NZP-CSI-RS-ResourceToAddModList* as defined in TS 38.331 [10]. |

#### 9.2.3.226 NZP CSI-RS Resource Set Configuration

This IE contains the CSI-RS resource set configuration used for LTM.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| CSI-RS Resource Set to AddMod List | O |  | OCTET STRING | Includes *ltm-NZP-CSI-RS-ResourceSetToAddModList* contained in the *LTM-Config* IE as defined in TS 38.331 [10]. |

#### 9.2.3.227 CSI-IM Resource Configuration

This IE contains the CSI-IM resource configuration used for LTM.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| CSI-IM Resource to AddMod List | O |  | OCTET STRING | Includes *ltm-CSI-IM-ResourceToAddModList* contained in the *LTM-Config* IE as defined in TS 38.331 [10]. |
| CSI-IM ResourceSet to AddMod List | O |  | OCTET STRING | Includes *ltm-CSI-IM-*ResourceSetToAddModList contained in the *LTM-Config* IE as defined in TS 38.331 [10]. |

**<< Next Change >>**

CSI-RSResourceConfiguration ::= SEQUENCE {

periodicNZP-CSI-RS-ResourceConfiguration NZP-CSI-RS-ResourceConfiguration OPTIONAL,

semiPersistentNZP-CSI-RS-ResourceConfiguration NZP-CSI-RS-ResourceConfiguration OPTIONAL,

periodicNZP-CSI-RS-ResourceSetConfiguration NZP-CSI-RS-ResourceSetConfiguration OPTIONAL,

semiPersistentNZP-CSI-RS-ResourceSetConfiguration NZP-CSI-RS-ResourceSetConfiguration OPTIONAL,

periodicCSI-IM-ResourceConfiguration CSI-IM-ResourceConfiguration OPTIONAL,

semiPersistentCSI-IM-ResourceConfiguration CSI-IM-ResourceConfiguration OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { CSI-RSResourceConfiguration-ExtIEs} } OPTIONAL,

...

}

CSI-RSResourceConfiguration-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

**<< Next Change >>**

NZP-CSI-RS-ResourceConfiguration ::= SEQUENCE {

cSI-RSResourceToAddModList OCTET STRING OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { NZP-CSI-RS-ResourceConfiguration-ExtIEs} } OPTIONAL,

...

}

NZP-CSI-RS-ResourceConfiguration-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

NZP-CSI-RS-ResourceSetConfiguration ::= SEQUENCE {

cSI-RSResourceSetToAddModList OCTET STRING OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { NZP-CSI-RS-ResourceSetConfiguration-ExtIEs} } OPTIONAL,

...

}

NZP-CSI-RS-ResourceSetConfiguration-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

CSI-IM-ResourceConfiguration ::= SEQUENCE { cSI-IMResourceToAddModList OCTET STRING OPTIONAL,

cSI-IMResourceSetToAddModList OCTET STRING OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { CSI-IM-ResourceConfiguration-ExtIEs} } OPTIONAL,

...

}

CSI-IM-ResourceConfiguration-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

...

}

**<< End of Changes >>**