**3GPP TSG-RAN3 Meeting #129-bis R3-257297**

**Prague, CZ, 13 - 17 Oct 2025**

**Agenda item: 13.3**

**Source: Xiaomi, Huawei, Samsung,** **Nokia, Nokia Shanghai Bell, ZTE**

**Title: TP to TR38.765 for basic sensing call flow**

**Document for: Other**

# 1 Introduction

This TP provide the call flow for sensing reporting based on the following online guidance and offline discussion in R3-257299.

**- Introduce basic/general call flow using 6529 as baseline, with Editor’s Notes, FFSes, refinements, etc.**

# 2 TP to TR 38.765

<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<change starts>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>

## 8.x Sensing Reporting

Editor’s Note: the detailed signaling procedure is to be formulated, e.g., the message name, the information included in the message, as well as other signalling messages etc.



Figure 8.x-1: Message flow for sensing reporting

1. The SF sends sensing request to the gNB.

2. The gNB sends sensing response to the SF.

3. If requested in Step 1, the gNB sends sensing report to the SF.

<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<change ends>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>