**3GPP TSG-RAN WG4 Meeting # 110bis R4-2406105**

**Changsha, China, Apr. 15th – 19th, 2024**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | **38.141-1** | **CR** |  | **rev** | **-** | **Current version:** | **18.5.0** |  |
|  |
| *For* ***[HELP](http://www.3gpp.org/3G_Specs/CRs.htm%22%20%5Cl%20%22_blank)*** *on using this form: comprehensive instructions can be found at <http://www.3gpp.org/Change-Requests>.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Clarify the CA requirements for ATG BS in R18 |
|  |  |
| ***Source to WG:*** | ZTE Corporation |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_ATG-Perf |  | ***Date:*** | 2024-04-08 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | In R18, CA feature is not supported for ATG BS, which was already clarified in TR38.876.For the requirements, the existing NR BS requirements are applied to ATG BS. However, the existing NR BS requirements includes the features of single carrier, CA, multi-band operation and NB-IoT. For multi-band operation and NB-IoT requirements, it was already clarified that the related requirements are not applied in the spec. However, for CA requirement, there is no such clarification, instead only TAE requirements are not applied to ATG BS due to CA is not supported. For other requirements, such as transmitter OFF power, ACLR, OBW etc, also incorporate the CA requirements. So it shall be clarified that the CA requirements are not applied to ATG BS in Rel-18.Note that CA will be supported for ATG BS in Rel-19. |
|  |  |
| ***Summary of change:*** | Clarify the CA requirements are not applied to ATG BS in Rel-18. |
|  |  |
| ***Consequences if not approved:*** | It is unclear whether CA requirements are not applied to ATG BS in Rel-18 spec. |
|  |  |
| ***Clauses affected:*** | 4.10 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This draft CR is revise from R4-2406105. |
|  |  |
| ***This CR's revision history:*** |  |

## << Start of changes >>

## 4.10 Requirements for contiguous and non-contiguous spectrum

A spectrum allocation where a BS operates can either be contiguous or non-contiguous. Unless otherwise stated, the requirements in the present specification apply for BS configured for both contiguous spectrum operation and non-contiguous spectrum operation.

For BS operation in non-contiguous spectrum, some requirements apply both at the Base Station RF Bandwidth edges and inside the sub-block gaps. For each such requirement, it is stated how the limits apply relative to the Base Station RF Bandwidth edges and the sub-block edges respectively.

There are no CA requirements for ATG BS in the present specification.

<< End of changes >>