**3GPP TSG-RAN WG4 Meeting #116 R4-2511180**

**Bengaluru, India, 25th August – 29th August 2025**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.3* | | | | | | | | |
| **DRAFT CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **-1** | **CR** |  | **rev** |  | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | draft CR 38.101-1 adding 2DL BCS 4 and 5 configurations | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | , AT&T | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_CADC\_SUL\_R19 | | | | |  | ***Date:*** | | | 2025-08-15 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | B |  | | | | | ***Release:*** | | | Rel-19 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)  Rel-20 (Release 20)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Adding new configurations | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Adding BCS 4 and 5 configurations for:  CA\_n2A-n30A  CA\_n2(2A)-n30A  CA\_n5A-n30A  CA\_n14A-n30A  CA\_n30A-n66A  CA\_n30A-n66(2A)  CA\_n30A-n77A  CA\_n30A-n77(2A)  CA\_n66(3A)-n77(2A)  **Technical analysis for CA\_n2-n30 BCS 4 and 5**  For band n2 channel BW 25, 30, 35 and 40 are added compared to previous BCS’s  For band n30 no new channel BW’s are added compared to previous BCS’s  In current specification, there is no MSD defined for cross band isolation, harmonic or harmonic mixing for this band combination.  **Technical analysis for CA\_n5-n30 BCS 4 and 5**  For band n5 channel BW 3, 5 and 25 are added compared to previous BCS’s  For band n30 no new channel BW’s are added compared to previous BCS’s  In current specification, there is no MSD defined for cross band isolation, harmonic or harmonic mixing for this band combination.  **Technical analysis for CA\_n14-n30 BCS 4 and 5**  For band n14 no new channel BW’s are added compared to previous BCS’s For band n30 no new channel BW’s are added compared to previous BCS’s  In current specification, there is no MSD defined for cross band isolation, harmonic or harmonic mixing for this band combination.  **Technical analysis for CA\_n30-n66 BCS 4 and 5**  For band n30 no new channel BW’s are added compared to previous BCS’s For band n66 channel BW 35 and 45 are added compared to previous BCS’s  In current specification there are MSD defined for cross band isolation for this band combination, but not for harmonic or harmonic mixing.  **Technical analysis for CA\_n66-n77 BCS 4 and 5**  All lower order combinations to CA\_n66(3A)-n77(2A) already have BCS 4 and 5 defined. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Configurations are not added | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.5A.3 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | | **X** |  | Test specifications | | | | TS 38.521-1 | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

---Start of changes---

Table 5.5A.3.1-1b: NR CA configurations and bandwidth combinations  
sets defined for inter-band CA (two bands)

| NR CA configuration | Uplink CA configuration or single uplink carrier10 | NR Band | Channel bandwidth (MHz) (NOTE 3) | Bandwidth combination set |
| --- | --- | --- | --- | --- |
| CA\_n2A-n5A | n28  CA\_n2A-n5A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  | CA\_n2A-n5A | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n5B | CA\_n2A-n5A  CA\_n5B | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | CA\_n5B\_BCS0 |  |
|  |  | n2 | See n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | CA\_n5B\_BCS 4 and 5 |  |
| CA\_n2(2A)-n5A | CA\_n2A-n5A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n2 | CA\_n2(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n5 | See n5 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n5B | CA\_n2A-n5A  CA\_n5B | n2 | CA\_n2(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n5 | CA\_n5B\_BCS 4 and 5 |  |
| CA\_n2A-n7A | CA\_n2A-n7A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n2A-n7(2A) | CA\_n2A-n7A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n7 | CA\_n7(2A)\_BCS0 |  |
| CA\_n2(2A)-n7A | CA\_n2A-n7A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n2A-n12A | CA\_n2A-n12A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
| CA\_n2(2A)-n12A | CA\_n2A-n12A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n12 | 5, 10, 15 |  |
| CA\_n2A-n14A | n28  n148  CA\_n2A-n14A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n2 | See n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n14 | See n14 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n14A | CA\_n2A-n14A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n2 | CA\_n2(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n14 | See n14 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n29A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
| CA\_n2(2A)-n29A | - | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n29 | 5, 10 |  |
| CA\_n2A-n30A | CA\_n2A-n30A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n2 | See n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n30 | See n30 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n30A | CA\_n2A-n30A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n2 | CA\_n2(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n30 | See n30 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n38A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n38 | 5, 10, 15, 20, 40 |  |
| CA\_n2A-n41A | CA\_n2A-n41A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n2(2A)-n41A | CA\_n2A-n41A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n48A | CA\_n2A-n48A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 40, 506, 606, 806, 906, 1006 |  |
|  |  | n2 | 5, 10, 15, 20 | 1 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 506, 606,706, 806, 906, 1006 |  |
|  | n28  CA\_n48B  CA\_n2A-n48A  CA\_n2A-n48B | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  | CA\_n2A-n48A | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n48B | CA\_n48B  CA\_n2A-n48A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n2 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n2 | See n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | CA\_n48B\_BCS 4 and 5 |  |
| CA\_n2A-n48C | CA\_n2A-n48A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
| CA\_n2A-n48(2A) | CA\_n2A-n48A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n2 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n2 | See n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | CA\_n48(2A)\_BCS 4 and 5 |  |
| CA\_n2A-n48(A-B) | CA\_n2A-n48A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(A-B)\_BCS0 |  |
|  |  | n2 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48(A-B)\_BCS1 |  |
|  |  | n2 | See n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | CA\_n48(A-B)\_BCS 4 and 5 |  |
| CA\_n2(2A)-n48A | CA\_n2A-n48A | n2 | CA\_n2(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n48 | See n48 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n48B | CA\_n48B  CA\_n2A-n48A  CA\_n2A-n48B | n2 | CA\_n2(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n48 | CA\_n48B\_BCS 4 and 5 |  |
| CA\_n2(2A)-n48(2A) | CA\_n2A-n48A | n2 | CA\_n2(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n48 | CA\_n48(2A)\_BCS 4 and 5 |  |
| CA\_n2(3A)-n48A | CA\_n2A-n48A | n2 | CA\_n2(3A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n48 | See n48 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n66A | n28  n668 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  | n28  n668  CA\_n2A-n66A | n2 | 5, 10, 15, 20 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  | CA\_n2A-n66A | n2 | See n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | See n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n66A | CA\_n2A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n2 | CA\_n2(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | See n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n66(2A) | CA\_n2A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n2 | See n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
| CA\_n2(2A)-n66(2A) | CA\_n2A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n2 | CA\_n2(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
| CA\_n2(2A)-n66(3A) | CA\_n2A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n2A-n66(3A) | CA\_n2A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n2A-n66B | CA\_n2A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66B\_BCS0 |  |
| CA\_n2A-n71A | CA\_n2A-n71A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | - | n2 | See n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | See n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n71A | CA\_n2A-n71A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | - | n2 | CA\_n2(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | See n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n77A | n28  n778,9  CA\_n2A-n77A8,13,14 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n77(2A) | n778,9  CA\_n2A-n77A8  CA\_n77(2A)7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n2 | 5, 10, 15, 20 | 1 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n2A-n77B | CA\_n2A-n77A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n77 | CA\_n77B\_BCS0 |  |
|  | - | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77B\_BCS 4 and 5 |  |
| CA\_n2A-n77C | n778, 9  CA\_n77C  CA\_n2A-n77A8 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  | n778, 9  CA\_n77C  CA\_n2A-n77A8  CA\_n2A-n77C | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77C\_BCS 4 and 5 |  |
| CA\_n2(2A)-n77A | n778, 9  CA\_n2A-n77A8 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | CA\_n2(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n77B | CA\_n2A-n77A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n77 | CA\_n77B\_BCS0 |  |
|  | - | n2 | CA\_n2(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | CA\_n77B\_BCS 4 and 5 |  |
| CA\_n2(2A)-n77(2A) | n778,9  CA\_n2A-n77A8  CA\_n77(2A)7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n2 | CA\_n2(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n2A-n77(3A) | CA\_n2A-n77A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
|  |  | n2 | 5, 10, 15, 20 | 1 |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n2(2A)-n77C | n778, 9  CA\_n77C  CA\_n2A-n77A8 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  | n778, 9  CA\_n77C  CA\_n2A-n77A  CA\_n2A-n77C | n2 | CA\_n2(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | CA\_n77C\_BCS 4 and 5 |  |
| CA\_n2(3A)-n77A | CA\_n2A-n77A | n2 | CA\_n2(3A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | See n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n78A | CA\_n2A-n78A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n2 | 5, 10, 15, 20 | 1 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | See n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n78(2A) | CA\_n2A-n78A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS1 |  |
|  |  | n2 | 5, 10, 15, 20 | 1 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n2 | See n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |

---Text omitted---

Table 5.5A.3.1-1d: NR CA configurations and bandwidth combinations  
sets defined for inter-band CA (two bands)

| NR CA configuration | Uplink CA configuration or single uplink carrier10 | NR Band | Channel bandwidth (MHz) (NOTE 3) | Bandwidth combination set |
| --- | --- | --- | --- | --- |
| CA\_n5A-n7A | CA\_n5A-n7A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n7B | CA\_n5A-n7A  CA\_n7B | n5 | 5, 10, 15, 20 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
| CA\_n5A-n8A15 | - | n5 | 5, 10 | 0 |
|  |  | n8 | 5, 10 |  |
| CA\_n5A-n12A | CA\_n5A-n12A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
| CA\_n5B-n12A | CA\_n5A-n12A  CA\_n5B | n5 | CA\_n5B\_BCS0 | 0 |
|  |  | n12 | 5, 10, 15 |  |
| CA\_n5A-n13A | CA\_n5A-n13A | n5 | 5, 10, 15, 20 | 4 and 5 |
|  |  | n13 | 5, 10 |  |
| CA\_n5B-n13A | CA\_n5A-n13A | n5 | CA\_n5B\_BCS0 | 0 |
|  |  | n13 | 5, 10 |  |
| CA\_n5A-n14A | CA\_n5A-n14A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
| CA\_n5B-n14A | CA\_n5A-n14A  CA\_n5B | n5 | CA\_n5B\_BCS0 | 0 |
|  |  | n14 | 5, 10 |  |
| CA\_n5A-n25A | CA\_n5A-n25A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n25(2A) | CA\_n5A-n25A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
| CA\_n5A-n28A | CA\_n5A-n28A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
| CA\_n5A-n29A | - | n5 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n29 | n29 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5B-n29A | CA\_n5B | n5 | CA\_n5B\_BCS0 | 0 |
|  |  | n29 | 5, 10 |  |
| CA\_n5A-n30A | CA\_n5A-n30A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n30 | n30 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n40A | CA\_n5A-n40A | n5 | 5, 10, 15, 20, 251 | 0 |
|  |  | n40 | 55, 10, 15, 20, 25, 30, 40, 50, 60, 70, 80,90,100 |  |
| CA\_n5A-n41A | CA\_n5A-n41A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n48A | CA\_n5A-n48A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 40, 506, 606, 806, 906, 1006 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 506, 606,706, 806, 906, 1006 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n48(2A) | CA\_n5A-n48A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | CA\_n48(2A)\_BCS 4 and 5 |  |
| CA\_n5A-n48B | CA\_n48B  CA\_n5A-n48A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  | CA\_n48B  CA\_n5A-n48A  CA\_n5A-n48B | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | CA\_n48B\_BCS 4 and 5 |  |
| CA\_n5A-n48C | CA\_n5A-n48A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
| CA\_n5A-n48(A-B) | CA\_n5A-n48A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(A-B)\_BCS0 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48(A-B)\_BCS1 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | CA\_n48(A-B)\_BCS 4 and 5 |  |
| CA\_n5B-n48A | CA\_n5B  CA\_n5A-n48A  CA\_n5B-n48A | n5 | CA\_n5B\_BCS 4 and 5 | 4 and 5 |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5B-n48B | CA\_n5B  CA\_n48B  CA\_n5A-n48A  CA\_n5A-n48B | n5 | CA\_n5B\_BCS 4 and 5 | 4 and 5 |
|  |  | n48 | CA\_n48B\_BCS 4 and 5 |  |
| CA\_n5B-n48(2A) | CA\_n5B  CA\_n5A-n48A | n5 | CA\_n5B\_BCS 4 and 5 | 4 and 5 |
|  |  | n48 | CA\_n48(2A)\_BCS 4 and 5 |  |
| CA\_n5A-n66A | n668  CA\_n5A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n66B | CA\_n5A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66B\_BCS0 |  |
| CA\_n5B-n66A | CA\_n5A-n66A  CA\_n5B | n5 | CA\_n5B\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n5 | CA\_n5B\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5B-n66B | CA\_n5A-n66A | n5 | CA\_n5B\_BCS0 | 0 |
|  |  | n66 | CA\_n66B\_BCS0 |  |
| CA\_n5A-n66(2A) | CA\_n5A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
| CA\_n5A-n66(3A) | CA\_n5A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n5B-n66(2A) | CA\_n5A-n66A  CA\_n5B | n5 | CA\_n5B\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n5 | CA\_n5B\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
| CA\_n5A-n71A | - | n5 | 5, 10, 15, 20 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n77A | n778,9  CA\_n5A-n77A8,13,14 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n77B | CA\_n5A-n77A  n778,9 | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77B\_BCS 4 and 5 |  |
| CA\_n5A-n77(2A) | n778,9  CA\_n5A-n77A8  CA\_n77(2A)8 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n5A-n77(3A) | n778,9  CA\_n77(2A)8  CA\_n5A-n77A8 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77(3A)\_BCS4 and 5 |  |
| CA\_n5(2A)-n77A | n778,9  CA\_n5A-n77A8 | n5 | CA\_n5(2A)\_BCS0 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n77C | n778,9  CA\_n5A-n77A8  CA\_n77C | n5 | 5, 10, 15, 20 | 0 |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  | CA\_n5A-n77A  CA\_n77C  CA\_n5A-n77C | n5 | See n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77C\_BCS 4 and 5 |  |
| CA\_n5(2A)-n77C | n778,9  CA\_n77C  CA\_n5A-n77A8 | n5 | CA\_n5(2A)\_BCS0 | 0 |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n5 | CA\_n5(2A)\_BCS0 | 1 |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n5B-n77A | n778,9  CA\_n5A-n77A8  CA\_n5B | n5 | CA\_n5B\_BCS0 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n5A-n77A  CA\_n5B | n5 | CA\_n5B\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5B-n77C | n778,9  CA\_n5A-n77A8  CA\_n5B  CA\_n77C | n5 | CA\_n5B\_BCS0 | 0 |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n5 | CA\_n5B\_BCS0 | 1 |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  | CA\_n5A-n77A  CA\_n5B  CA\_n77C  CA\_n5A-n77C | n5 | CA\_n5B\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | CA\_n77C\_BCS 4 and 5 |  |
| CA\_n5A-n78A | n788,9  CA\_n5A-n78A8 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n5 | See n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n78(2A) | n788,9  CA\_n5A-n78A8  CA\_n78(2A)8 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n5 | See n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n5A-n78C | CA\_n5A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78C\_BCS0 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n78 | CA\_n78C\_BCS1 |  |
|  | CA\_n78C  CA\_n5A-n78C | n5 | See n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | CA\_n78C\_BCS4 and 5 |  |
| CA\_n5A-n78(A-C) | CA\_n78C  CA\_n5A-n78A | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n78 | CA\_n78(A-C)\_BCS1 |  |
| CA\_n5A-n79A | CA\_n5A-n79A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n5 | See n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n79C | CA\_n5A-n79A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n79 | CA\_n79C\_BCS0 |  |
|  |  | n5 | See n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | CA\_n79C\_BCS4 and 5 |  |
| CA\_n5A-n105A | CA\_n5A-n105A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |

---Text omitted---

Table 5.5A.3.1-1f: NR CA configurations and bandwidth combinations  
sets defined for inter-band CA (two bands)

| NR CA configuration | Uplink CA configuration or single uplink carrier10 | NR Band | Channel bandwidth (MHz) (NOTE 3) | Bandwidth combination set |
| --- | --- | --- | --- | --- |
| CA\_n12A-n25A | CA\_n12A-n25A | n12 | 5, 10, 15 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n12 | n12 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n12A-n30A | CA\_n12A-n30A | n12 | 5, 10, 15 | 0 |
|  |  | n30 | 5, 10 |  |
| CA\_n12A-n41A | - | n12 | 5, 10, 15 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n12 | n12 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n12A-n48A | - | n12 | 5, 10, 15 | 0 |
|  |  | n48 | 10, 15, 20, 30, 40 |  |
| CA\_n12A-n66A | CA\_n12A-n66A | n12 | 5, 10, 15 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n12 | n12 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n12A-n66(2A) | CA\_n12A-n66A | n12 | 5, 10, 15 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n12A-n66(3A) | CA\_n12A-n66A | n12 | 5, 10, 15 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n12A-n71A | - | n12 | 5, 10, 15 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n12A-n77A | n778, 9  CA\_n12A-n77A8 | n12 | 5, 10, 15 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n12 | n12 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n12A-n77B | CA\_n12A-n77A | n12 | n12 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77B\_BCS 4 and 5 |  |
| CA\_n12A-n77C | CA\_n12A-n77A | n12 | n12 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77C\_BCS 4 and 5 |  |
| CA\_n12A-n77(2A) | n778, 9  CA\_n12A-n77A8 | n12 | 5, 10, 15 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n12A-n78A | CA\_n12A-n78A | n12 | 5, 10, 15 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n12A-n78(2A) | CA\_n12A-n78A | n12 | 5, 10, 15 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n13A-n25A | CA\_n13A-n25A | n13 | 5, 10 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n13A-n66A | CA\_n13A-n66A | n13 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n13 | 5, 10, | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n13A-n66B | CA\_n13A-n66A | n13 | 5, 10 | 0 |
|  |  | n66 | CA\_n66B\_BCS0 |  |
| CA\_n13A-n66(2A) | CA\_n13A-n66A | n13 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n13A-n77A | n778, 9  CA\_n13A-n77A8 | n13 | 5, 10 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n13A-n77(2A) | n778,9  CA\_n77(2A)8  CA\_n13A-n77A8 | n13 | 5, 10 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n13A-n77C | n778,9  CA\_n77C  CA\_n13A-n77A8 | n13 | 5, 10 | 0 |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n14A-n30A | n148  CA\_n14A-n30A | n14 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n14 | n14 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n30 | n30 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n14A-n66A | n148  n668  CA\_n14A-n66A | n14 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n14 | n14 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n14A-n66(2A) | CA\_n14A-n66A | n14 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n14 | n14 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
| CA\_n14A-n66(3A) | CA\_n14A-n66A | n14 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n14A-n77A | n148  n778, 9  CA\_n14A-n77A8 | n14 | 5, 10 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n14 | n14 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n14A-n77(2A) | n778, 9  CA\_n14A-n77A8 | n14 | 5, 10 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n14 | n14 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n18A-n28A | CA\_n18A-n28A | n18 | 5, 10, 15 | 0 |
|  |  | n28 | 5, 10 |  |
| CA\_n18A-n40A | CA\_n18A-n40A | n18 | 5, 10, 15 | 0 |
|  |  | n40 | 10, 15, 20, 30, 40 |  |
| CA\_n18A-n41A | n418  CA\_n18A-n41A8 | n18 | 5, 10, 15 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n18A-n74A | CA\_n18A-n74A | n18 | 5, 10, 15 | 0 |
|  |  | n74 | 5, 10, 15, 20 |  |
| CA\_n18A-n77A | n778  CA\_n18A-n77A8 | n18 | 5, 10, 15 | 0 |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n18 | See n18 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | See n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n18A-n77(2A) | n778  CA\_n18A-n77A8 | n18 | 5, 10, 15 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n18 | See n18 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n18A-n77(3A) | CA\_n18A-n77A8 | n18 | 5, 10, 15 | 0 |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n18A-n78A | CA\_n18A-n78A | n18 | 5, 10, 15 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n18 | See n18 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n18A-n78(2A) | CA\_n18A-n78A | n18 | 5, 10, 15 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n18 | See n18 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |

---Text omitted---

Table 5.5A.3.1-1i: NR CA configurations and bandwidth combinations sets defined for inter-band CA (two bands)

| NR CA configuration | Uplink CA configuration or single uplink carrier10 | NR Band | Channel bandwidth (MHz) (NOTE 3) | Bandwidth combination set |
| --- | --- | --- | --- | --- |
| CA\_n30A-n66A | CA\_n30A-n66A | n30 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n30 | See n30 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | See n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n30A-n66(2A) | CA\_n30A-n66A | n30 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n30 | See n30 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
| CA\_n30A-n66(3A) | CA\_n30A-n66A | n30 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n30A-n77A | n778, 9  CA\_n30A-n77A8 | n30 | 5, 10 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n30 | See n30 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | See n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n30A-n77(2A) | n778, 9  CA\_n77(2A)  CA\_n30A-n77A8 | n30 | 5, 10 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  | n778, 9  CA\_n30A-n77A8 | n30 | See n30 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n34A-n39A | n348,9  n398  CA\_n34A-n39A8 | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n34A-n40A | n348,9  n408,9  CA\_n34A-n40A8 | n34 | 5, 10, 15 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n34A-n41A | n348,9  n418,9  CA\_n34A-n41A8 | n34 | 5, 10, 15 | 0 |
|  |  | n41 | 10, 15, 20, 30 ,40 ,50, 60, 70, 80, 90, 100 |  |
|  |  | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n34A-n41C | CA\_n41C  CA\_n34A-n41A  CA\_n34A-n41C | n34 | 5, 10, 15 | 0 |
|  |  | n41 | CA\_n41C\_BCS1 |  |
|  |  | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS4 and 5 |  |
| CA\_n34A-n79A | n348,9  n798,9  CA\_n34A-n79A8 | n34 | 5, 10, 15 | 0 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n34A-n79C | CA\_n34A-n79A | n34 | 5, 10, 15 | 0 |
|  |  | n79 | CA\_n79C\_BCS0 |  |
|  | CA\_n79C  CA\_n34A-n79C | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | CA\_n79C\_BCS4 and 5 |  |
| CA\_n38A-n40A | - | n38 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n40 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n38A-n66A | CA\_n38A-n66A | n38 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 30, 40 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n38A-n66(2A) | CA\_n38A-n66A | n38 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n38A-n71A | - | n38 | 5, 10, 15, 20 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n38A-n78A | CA\_n38A-n78A | n38 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n38 | See n38 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n38A-n78(2A) | CA\_n38A-n78A | n38 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  |  | n38 | 5, 10, 15, 20 | 1 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n38 | See n38 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n38A-n79A | - | n38 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n38 | See n38 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n38A-n79C | - | n38 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n79 | CA\_n79C\_BCS0 |  |
|  |  | n38 | See n38 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | CA\_n79C\_BCS4 and 5 |  |
| CA\_n39A-n40A | n398  n408,9  CA\_n39A-n40A8 | n39 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n39A-n41A | n398  n418,9  CA\_n39A-n41A8 | n39 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n39A-n41C | n398  n418,9  CA\_n41C8  CA\_n39A-n41A8  CA\_n39A-n41C8 | n39 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | CA\_n41C\_BCS0 |  |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS4 and 5 |  |
| CA\_n39A-n41(2A) | CA\_n39A-n41A | n39 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS0 |  |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A)\_BCS4 and 5 |  |
| CA\_n39A-n79A | n398  n798,9  CA\_n39A-n79A8 | n39 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n39A-n79C | CA\_n79C  CA\_n39A-n79A  CA\_n39A-n79C | n39 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n79 | CA\_n79C\_BCS0 |  |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | CA\_n79C\_BCS4 and 5 |  |
| CA\_n40A-n41A | n408,9  n418,9  CA\_n40A-n41A8 | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 40, 50, 60 |  |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n40A-n41C | CA\_n41C  CA\_n40A-n41A  CA\_n40A-n41C | n40 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | CA\_n41C\_BCS0 |  |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS4 and 5 |  |
| CA\_n40A-n71A | CA\_n40A-n71A | n40 | n40 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n40A-n77A | n408,9  n778,9  CA\_n40A-n77A8 | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 704,80, 904, 100 |  |
| CA\_n40A-n77(2A) | CA\_n40A-n77A | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n40A-n77C | - | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n40B-n77A | n778  CA\_n40A-n77A | n40 | CA\_n40B\_BCS1 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 704,80, 904, 100 |  |
| CA\_n40B-n77(2A) | CA\_n40A-n77A | n40 | CA\_n40B\_BCS1 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n40B-n77C | CA\_n40A-n77A | n40 | CA\_n40B\_BCS1 | 0 |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n40A-n78A | n408,9  n788,9  CA\_n40A-n78A8 | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 1 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n40A-n78(2A) | CA\_n40A-n78A | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS1 |  |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n40A-n78C | CA\_n40A-n78A | n40 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n40B-n78A | - | n40 | CA\_n40B\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n40A-n78A | n40 | CA\_n40B\_BCS1 | 1 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n40B-n78(2A) | CA\_n40A-n78A | n40 | CA\_n40B\_BCS1 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n40 | CA\_n40B\_BCS 4 and 5 | 4 and 5 |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n40B-n78C | CA\_n40A-n78A | n40 | CA\_n40B\_BCS1 | 0 |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n40A-n79A | n408,9  n798,9  CA\_n40A-n79A8 | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 | 0 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n40A-n79C | n408,9  n798,9  CA\_n79C8  CA\_n40A-n79A8 | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 | 0 |
|  |  | n79 | CA\_n79C\_BCS0 |  |
|  | CA\_n79C  CA\_n40A-n79A  CA\_n40A-n79C | n40 | See n40 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n40A-n105A | CA\_n40A-n105A | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |

---Text omitted---

Table 5.5A.3.1-1m: NR CA configurations and bandwidth combinations sets defined for inter-band CA (two bands)

| NR CA configuration | Uplink CA configuration or single uplink carrier10 | NR Band | Channel bandwidth (MHz) (NOTE 3) | Bandwidth combination set |
| --- | --- | --- | --- | --- |
| CA\_n66A-n70A | n668  n708 | n66 | 5, 10, 15, 20, 40 | 0 |
|  |  | n70 | 5, 10, 15, 201,251 |  |
|  | - | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n70 | n70 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66B-n70A | n668  n708 | n66 | CA\_n66B\_BCS0 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n66(2A)-n70A | n668  n708 | n66 | CA\_n66(2A)\_BCS0 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  | - | n66 | CA\_n66(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n70 | n70 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66(3A)-n70A | n668  n708 | n66 | CA\_n66(3A)\_BCS0 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n66A-n71A | n668  n718  CA\_n66A-n71A8 | n66 | 5, 10, 15, 20, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66A-n71B | n668  n718  CA\_n66A-n71A8 | n66 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | CA\_n71B\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n66A-n71(2A) | n668  n718  CA\_n66A-n71A8 | n66 | 5, 10, 15, 20, 40 | 0 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
| CA\_n66(2A)-n71A | n668  n718  CA\_n66A-n71A8 | n66 | CA\_n66(2A)\_BCS0 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 | 1 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66(2A)-n71B | n668  n718  CA\_n66A-n71A8 | n66 | CA\_n66(2A)\_BCS1 | 0 |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n66(2A)-n71(2A) | n668  n718  CA\_n66A-n71A8 | n66 | CA\_n66(2A)\_BCS1 | 0 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
| CA\_n66(3A)-n71A | n668  n718  CA\_n66A-n71A | n66 | CA\_n66(3A)\_BCS0 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n66 | CA\_n66(3A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66(3A)-n71(2A) | CA\_n66A-n71A | n66 | CA\_n66(3A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
| CA\_n66B-n71A | n668  n718  CA\_n66A-n71A | n66 | CA\_n66B\_BCS0 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n66A-n77A | n668  n778,9  CA\_n66A-n77A8,13,14 | n66 | 5, 10, 15, 20, 40 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66A-n77B | CA\_n66A-n77A | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77B\_BCS 4 and 5 |  |
| CA\_n66(2A)-n77A | n668  n778,9  CA\_n66A-n77A8 | n66 | CA\_n66(2A)\_BCS1 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 | 1 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66(2A)-n77B | CA\_n66A-n77A | n66 | CA\_n66(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | CA\_n77B\_BCS 4 and 5 |  |
| CA\_n66A-n77(2A) | n668  n778,9  CA\_n66A-n77A8,13,14  CA\_n77(2A)8 | n66 | 5, 10, 15, 20, 40 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n66(3A)-n77A | n668  n778,9  CA\_n66A-n77A8 | n66 | CA\_n66(3A)\_BCS0 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n66A-n77A | n66 | CA\_n66(3A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66(2A)-n77(2A) | n668  n778,9  CA\_n66A-n77A8  CA\_n77(2A) | n66 | CA\_n66(2A)\_BCS0 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 | 1 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n66(3A)-n77(2A) | n778,9  CA\_n66A-n77A8 | n66 | CA\_n66(3A)\_BCS0 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n66 | CA\_n66(3A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n66A-n77C | n778,9  CA\_n77C  CA\_n66A-n77A8 | n66 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  | CA\_n77C  CA\_n66A-n77A  CA\_n66A-n77C | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77C\_BCS 4 and 5 |  |
| CA\_n66A-n77(3A) | n778,9  CA\_n77(2A)8  CA\_n66A-n77A8 | n66 | 5, 10, 15, 20, 40 | 0 |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77(3A)\_BCS4 and 5 |  |
| CA\_n66(2A)-n77(3A) | CA\_n77(2A)  CA\_n66A-n77A | n66 | CA\_n66(2A)\_BCS0 | 0 |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n66(2A)-n77C | n778,9  CA\_n77C  CA\_n66A-n77A8 | n66 | CA\_n66(2A)\_BCS0 | 0 |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 | 1 |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  | CA\_n77C  CA\_n66A-n77A  CA\_n66A-n77C | n66 | CA\_n66(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | CA\_n77C\_BCS 4 and 5 |  |
| CA\_n66(3A)-n77C | n778,9  CA\_n77C CA\_n66A-n77A8 | n66 | CA\_n66(3A)\_BCS0 | 0 |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n66B-n77A | n668  n778,9  CA\_n66A-n77A8 | n66 | CA\_n66B\_BCS0 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n66B-n77C | n778,9  CA\_n77C  CA\_n66A-n77A8 | n66 | CA\_n66B\_BCS0 | 0 |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n66 | CA\_n66B\_BCS0 | 1 |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n66A-n78A | n788,9  CA\_n66A-n78A8 | n66 | 5, 10, 15, 20, 40 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | See n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66A-n78(2A) | n788,9  CA\_n66A-n78A8 | n66 | 5, 10, 15, 20, 30, 40 | 0 |
|  | CA\_n78(2A)8 | n78 | CA\_n78(2A)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n66 | See n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n66(2A)-n78A | n788,9  CA\_n66A-n78A8 | n66 | CA\_n66(2A)\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 | 1 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66(2A)-n78(2A) | n788,9  CA\_n66A-n78A8 | n66 | CA\_n66(2A)\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 | 1 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n66A-n85A | n668  CA\_n66A-n85A8 | n66 | See n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n85 | See n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66(2A)-n85A | CA\_n66A-n85A | n66 | CA\_n66(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n85 | See n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n67A-n78A | - | n67 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n67A-n78(2A) | CA\_n78(2A) | n67 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |

---End of changes---