**3GPP TSG- Meeting #**

**Bengaluru, India, August 25th – 29th, 2025**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.3* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** |  | **rev** | **-** | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | draftCR on CSI-RS based RLM evaluation period requirements with SBFD | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** |  | | | | | | | | | |
| ***Source to TSG:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_duplex\_evo-Core | | | | |  | ***Date:*** | | |  |
|  |  | | | |  | |  | | |  |
| ***Category:*** |  |  | | | | | ***Release:*** | | |  |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)  Rel-20 (Release 20)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Based on CR work split in WF R4-2504904, the requirements on CSI-RS based RLM evaluation period needs to be updated for impact of SBFD operation. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Introduce updated CSI-RS based RLM evaluation period requirements due to the impact of SBFD operation. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The CSI-RS based RLM evaluation period requirements with SBFD are missing. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 8.1.3.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

Start of Change 1

#### 8.1.3.2 Minimum requirement

UE shall be able to evaluate whether the downlink radio link quality on the configured RLM-RS resource estimated over the last TEvaluate\_out\_CSI-RS period becomes worse than the threshold Qout\_CSI-RS within TEvaluate\_out\_CSI-RS evaluation period.

UE shall be able to evaluate whether the downlink radio link quality on the configured RLM-RS resource estimated over the last TEvaluate\_in\_CSI-RS ms period becomes better than the threshold Qin\_CSI-RS within TEvaluate\_in\_CSI-RS ms evaluation period.

- TEvaluate\_out\_CSI-RS and TEvaluate\_in\_CSI-RS are defined in table 8.1.3.2-1 for FR1.

- TEvaluate\_out\_CSI-RS and TEvaluate\_in\_CSI-RS are defined in table 8.1.3.2-2 for FR2 with scaling factor N=1.

- TEvaluate\_out\_CSI-RS and TEvaluate\_in\_CSI-RS are defined in table 8.1.3.2-3 for FR1 (deactivated PSCell).

- TEvaluate\_out\_CSI-RS and TEvaluate\_in\_CSI-RS are defined in table 8.1.3.2-4 for FR2 (deactivated PSCell) with scaling factor N=1.

The requirements of TEvaluate\_out\_CSI-RS and TEvaluate\_in\_CSI-RS apply provided that the CSI-RS for RLM is not in a resource set configured with repetition ON. The requirements do not apply when the CSI-RS resource in the active TCI state of CORESET is the same CSI-RS resource for RLM and the TCI state information of the CSI-RS resource is not given, wherein the TCI state information means QCL Type-D to SSB for L1-RSRP or CSI-RS with repetition ON.

For the value of L1Out and L1In,

1> If the UE does not support *supportSBFD* or SBFD is not configured by the network,

2> L1Out = 0;

2> L1In = 0;

1> Else if the UE supports *supportSBFD* and SBFD is configured by the network,

2> If DRX is not configured,

3> L1Out is the number of occasions of the CSI-RS resource for RLM that are overlapping with dynamic UL transmission on SBFD symbols during TEvaluate\_Out\_CSI-RS;

3> L1In is the number of occasions of the CSI-RS resource for RLM that are overlapping with dynamic UL transmission on SBFD symbols during TEvaluate\_In\_CSI-RS, when DRX is not configured

2> If DRX is configured,

3> L1Out is the number of DRX cycles in which at least one occasion of the CSI-RS resource for RLM is overlapping with dynamic UL transmission on SBFD symbols during TEvaluate\_Out\_CSI-RS;

3> L1In is the number of DRX cycles in which at least one occasion of the CSI-RS resource for RLM is overlapping with dynamic UL transmission on SBFD symbols during TEvaluate\_In\_CSI-RS;

If the UE supports *supportSBFD* and SBFD is configured by the network, the requirements in this clause apply provided that all the occasions of the CSI-RS resource are in the same type (i.e., SBFD or non-SBFD) of symbols.

For a UE supporting *concurrentMeasGapsPreMG-r18* and when concurrent measurement gap(s) with Pre-MG(s) are configured, or a UE supporting *concurrentMeasGapsNCSG-r18* and when concurrent measurement gap(s) with NCSG(s) are configured, or a UE supporting *concurrentMeasGap-r17* or *musim-GapPreference-r17* or both *concurrentMeasGap-r17* and *musim-GapPreference-r17,* and when concurrent measurement gaps or periodic MUSIM gaps or both concurrent GAPs and periodic MUSIM gaps are are configured,

- an RLM-RS resource occasion is not considered to be overlapped by a gap occasion if the gap occasion is dropped according to clauses 9.1.8 and 9.1.10,

- P value for an RLM-RS resource to be measured is defined as

- Ntotal / Noutside\_MG in FR1

- Psharing factor \* Ntotal / Noutside\_MG in FR2 with Navailable = 0

- Ntotal / Navailable in FR2 with Navailable > 0

- For a window W of duration max(TL1, xRP\_max), where xRP\_max is the maximum xRP across all configured per-UE measurement gaps or periodic MUSIM gap(s) or NCSGs and per-FR measurement gaps or NCSGs, and, in case of Pre-MG, all activated per-UE measurement gaps and per-FR measurement gaps, within the same FR as serving cell, and starting at the beginning of any RLM-RS resource occasion:

- Ntotal is the total number of RLM-RS resource occasions within the window W, including those overlapped with GAP occasions, MUSIM gap occasions or SMTC occasions within the window W, and

- Noutside\_MG is the number of RLM-RS resource occasions that are not overlapped with any non-dropped GAP occasion nor non-dropped MUSIM gap occasion within the window W, and

- Navailable is the number of RLM-RS resource occasions that are not overlapped with any non-dropped GAP occasion, nor non-dropped MUSIM gap occasion, nor any SMTC occasion within the window W, and

- an RLM-RS resource occasion is considered to be overlapped with the MUSIM gap if it overlaps a MUSIM gap occasion, and

- TL1 is periodicity of the target RLM-RS.

- xRP = MGRP when configured GAP is activated Pre-MG or MG, and xRP = VIRP when configured GAP is NCSG.

Otherwise, for a UE neither supporting *concurrentMeasGap-r17* nor *concurrentMeasGapsPreMG-r18* nor *concurrentMeasGapsNCSG-r18* nor supporting *musim-GapPreference-r17* or when neither of the above configurations applies, i.e. concurrent measurement gaps, concurrent measurement gap(s) with Pre-MG(s), concurrent measurement gap(s) with NCSG(s), and periodic MUSIM gaps,

For FR1,

- , when in the monitored cell there are GAPs configured for intra-frequency, inter-frequency or inter-RAT measurements, and these GAPs] are overlapping with some but not all occasions of the CSI-RS; and

- P=1 when in the monitored cell there are no GAPs overlapping with any occasion of the CSI-RS.

For FR2,

- P=1, when the RLM-RS resource is not overlapped with measurement gap and also not overlapped with SMTC occasion.

- , when the RLM-RS resource is partially overlapped with GAP and the RLM-RS resource is not overlapped with SMTC occasion (TCSI-RS < xRP)

- , when the RLM-RS resource is not overlapped with GAP and the RLM-RS resource is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod).

- P = Psharing factor, when the RLM-RS resource is not overlapped with GAP and RLM-RS resource is fully overlapped with SMTC occasion (TCSI-RS = TSMTCperiod).

- , when the RLM-RS resource is partially overlapped with GAP and the RLM-RS resource is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is not overlapped with GAP and

- TSMTCperiod ≠ xRP or

- TSMTCperiod = xRP and TCSI-RS < 0.5 × TSMTCperiod

- , when the RLM-RS resource is partially overlapped with GAP and the RLM-RS resource is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is not overlapped with GAP and TSMTCperiod = xRP and TCSI-RS = 0.5 × TSMTCperiod

- , when the RLM-RS resource is partially overlapped with GAP and the RLM-RS resource is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is partially or fully overlapped with GAP

- , when the RLM-RS resource is partially overlapped with GAP and the RLM-RS resource is fully overlapped with SMTC occasion (TCSI-RS = TSMTCperiod) and SMTC occasion is partially overlapped with GAP (TSMTCperiod < xRP)

where,

- Psharing factor = 1, if the RLM-RS resource outside GAP is

- not overlapped with the SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol before each consecutive SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol after each consecutive SSB symbols indicated by *SSB-ToMeasure*, given that *SSB-ToMeasure* is configured, where the *SSB-ToMeasure* is the union set of *SSB-ToMeasure* from all the configured measurement objects merged on the same serving carrier, and,

- not overlapped by the RSSI symbols indicated by *ss-RSSI-Measurement* and 1 data symbol before each RSSI symbol indicated by *ss-RSSI-Measurement* and 1 data symbol after each RSSI symbol indicated by *ss-RSSI-Measurement*, given that *ss-RSSI-Measurement* is configured.

- Psharing factor = 3, otherwise.

- If the higher layer in TS 38.331 [2] signalling of *smtc2*is present, TSMTCperiod follows *smtc2*; Otherwise TSMTCperiod follows *smtc1.* TSMTCperiod is the shortest SMTC period among all CCs in the same FR2 band, provided the SMTC offset of all CCs in FR2 have the same offset.

- When a GAP is configured only and the GAP is not NCSG,

- an RLM-RS resource or an SMTC occasion is considered to be overlapped with the GAP if it overlaps a GAP occasion, and

- xRP = MGRP

- Otherwise, when NCSG is configured,

- an RLM-RS resource or an SMTC occasion is considered to be overlapped with the GAP if

- it overlaps the VIL1 or VIL2 of NCSG, or

- it overlaps the ML of NCSG in FR2, and there exists a target carrier to be measured within NCSG that is intra-frequency carrier or inter-frequency carrier in the same band as the serving cell, or inter-frequency carrier in different band as the serving cell and UE does not support IBM between the target carrier and the serving cell,

- and

- xRP = VIRP

If the UE is configured with Pre-MG only, an RLM-RS resource or an SMTC occasion is only considered to be overlapped by the Pre-MG if the Pre-MG is activated.

When concurrent gaps or concurrent measurement gap(s) with Pre-MG(s) or concurrent measurement gap(s) with NCSG(s) are configured , an RLM-RS resource or an SMTC occasion is not considered to be overlapped by a GAP occasion if the GAP occasion is dropped according to clause 9.1.8, clause 9.1.12, clause 9.1.13, respectively.

If the higher layer in TS 38.331 [2] signalling of *smtc2*is present, TSMTCperiod follows *smtc2*; Otherwise TSMTCperiod follows *smtc1.*

NOTE: The overlap between CSI-RS for RLM and SMTC means that CSI-RS based RLM is within the SMTC window duration.

Longer evaluation period would be expected if the combination of RLM-RS resource, SMTC occasion and GAP configurations does not meet previous conditions.

When the configured aperiodic MUSIM gap is overlapping with RLM-RS resource occasion, longer evaluation period would be expected.

When UE is configured with MUSIM gap(s), and if RLM-RS resource occasions are fully overlapped with MUSIM gap(s) or the union of MUSIM gap(s) and GAPs, no requirement applies for CSI-RS based RLM.

For either an FR1 or FR2 serving cell, longer evaluation period would be expected during the period Tidentify\_CGI when the UE is requested to decode an NR CGI.

For either an FR1 or FR2 serving cell, longer evaluation period would be expected during the period Tidentify\_CGI,E-UTRAN when the UE is requested to decode an LTE CGI.

The values of Mout and Min used in table 8.1.3.2-1, table 8.1.3.2-2, table 8.1.3.2-3 and table 8.1.3.2-4 are defined as:

- Mout = 20 and Min = 10, if the CSI-RS resource configured for RLM is transmitted with higher layer CSI-RS parameter *density* [6, clause 7.4.1] set to 3 and over the bandwidth ≥ 24 PRBs.

If the UE supports *supportSBFD* and SBFD is configured by the network, the requirements in this clause apply provided that the CSI-RS resource configured for RLM is transmitted with higher layer CSI-RS parameter *density* [6, clause 7.4.1] set to 3 and over the bandwidth ≥ 24 PRBs in at least one DL subband.

Table 8.1.3.2-1: Evaluation period TEvaluate\_out\_CSI-RS and TEvaluate\_in\_CSI-RS for FR1

|  |  |  |
| --- | --- | --- |
| Configuration | TEvaluate\_out\_CSI-RS (ms) | TEvaluate\_in\_CSI-RS (ms) |
| no DRX | Max(200, Ceil((Mout+ L1Out)×P)×max(TCSI-RS, Tproc) | Max(100, Ceil((Min+ L1In)×P) × max(TCSI-RS, Tproc)) |
| DRX ≤ 320 ms | Max(200, Ceil(1.5×(Mout+ L1Out)×P)× Max(TDRX, TCSI-RS, Tproc)) | Max(100, Ceil(1.5×(Min+ L1In)×P)× Max(TDRX, TCSI-RS, Tproc)) |
| DRX > 320 ms | Ceil((Mout+ L1Out)×P) × TDRX | Ceil((Min+ L1In)×P) × TDRX |
| NOTE 1: TCSI-RS is the periodicity of the CSI-RS resource configured for RLM. The requirements in this table apply for TCSI-RS equal to 5 ms, 10 ms, 20 ms or 40 ms. TDRX is the DRX cycle length.  NOTE 2: If UE indicates *needForScaledCSIProcTimeDualDL* and the CSI-RS resource for RLM is across 2 DL subbands, Tproc = 8ms; otherwise Tproc = 0. | | |

Table 8.1.3.2-2: Evaluation period TEvaluate\_out\_CSI-RS and TEvaluate\_in\_CSI-RS for FR2

|  |  |  |
| --- | --- | --- |
| Configuration | TEvaluate\_out\_CSI-RS (ms) | TEvaluate\_in\_CSI-RS (ms) |
| no DRX | Max(200, Ceil((Mout+ L1Out)×P×N)× max(TCSI-RS, Tproc)) | Max(100, Ceil((Min+ L1In)×P×N) × max(TCSI-RS, Tproc)) |
| DRX ≤ 320 ms | Max(200, Ceil(1.5×(Mout+ L1Out)×P×N)× Max(TDRX, TCSI-RS, Tproc)) | Max(100, Ceil(1.5×(Min+ L1In)×P×N)× Max(TDRX, TCSI-RS, Tproc)) |
| DRX > 320 ms | Ceil((Mout+ L1Out)×P×N) × TDRX | Ceil((Min+ L1In)×P×N) × TDRX |
| NOTE 1: TCSI-RS is the periodicity of the CSI-RS resource configured for RLM. The requirements in this table apply for TCSI-RS equal to 5 ms, 10 ms, 20 ms or 40 ms. TDRX is the DRX cycle length.  NOTE 2: If UE indicates *needForScaledCSIProcTimeDualDL* and the CSI-RS resource for RLM is across 2 DL subbands, Tproc = 8ms; otherwise Tproc = 0. | | |

Table 8.1.3.2-3: Evaluation period TEvaluate\_out\_CSI-RS and TEvaluate\_in\_CSI-RS for FR1 (deactivated PSCell)

|  |  |  |
| --- | --- | --- |
| Configuration | TEvaluate\_out\_CSI-RS (ms) | TEvaluate\_in\_CSI-RS (ms) |
| no DRX | Ceil(Mout×P) × measCyclePSCell | Ceil(Min×P) × measCyclePSCell |
| DRX ≤ 320 ms | Ceil(1.5 ×Mout×P) × Max(TDRX, measCyclePSCell) | Ceil(1.5 ×Min×P) × Max(TDRX, measCyclePSCell) |
| DRX > 320 ms | Ceil(Mout×P) × Max(TDRX, measCyclePSCell) | Ceil(Min×P) × Max(TDRX, measCyclePSCell) |
| NOTE: TDRX is the DRX cycle length of SCG. measCyclePSCell is the measurement cycle length of the deactivated PSCell. | | |

Table 8.1.3.2-4: Evaluation period TEvaluate\_out\_CSI-RS and TEvaluate\_in\_CSI-RS for FR2 (deactivated PSCell)

|  |  |  |
| --- | --- | --- |
| Configuration | TEvaluate\_out\_CSI-RS (ms) | TEvaluate\_in\_CSI-RS (ms) |
| no DRX | Ceil(Mout×P×N) × measCyclePSCell | Ceil(Min×P×N) × measCyclePSCell |
| DRX ≤ 320 ms | Ceil(1.5 × Mout×P×N) × Max(TDRX, measCyclePSCell) | Ceil(1.5 × Min×P×N) × Max(TDRX, measCyclePSCell) |
| DRX > 320 ms | Ceil(Mout×P×N) × Max(TDRX, measCyclePSCell) | Ceil(Min×P×N) × Max(TDRX, measCyclePSCell) |
| NOTE: TDRX is the DRX cycle length of SCG. measCyclePSCell is the measurement cycle length of the deactivated PSCell. | | |

End of Change 1