3GPP TSG RAN WG4 Meeting #116 R4-2512596

Bangalore, India, August 25th – 29th , 2025

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.3* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** |  | **rev** | **1** | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **x** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | BigCR to TS 38.141-1 on support for LP-WUS | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | CATT | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** |  | | | | |  | ***Date:*** | | |  |
|  |  | | | |  | |  | | |  |
| ***Category:*** |  |  | | | | | ***Release:*** | | |  |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)  Rel-20 (Release 20)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | This is a formal CR based on the endorsed draftCR R4-2508666 with addition of declarations for LP-WUS support with two different declaration items according to WF R4-2502305, and also alignment with the endorsed draftCR R4-2508777, R4-2508772 for TS 38.104.  And both BS type 1-C and 1-H could be considered according to WF R4-2416589. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | 1. Add declaration item D.126 on LP-WUS support  2. Add declaration item D.127 on the minimum power boosting level  3. Add abbrievation of LP-WUS  4. Add applicability of unwanted emission and Tx IMD | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | LP-WUS is not supported | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 3.3, 4.6, 6.6.3.1, 6.6.4.1, 6.6.5.1, 6.7.5.1.1 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **x** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **x** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **x** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

<Start of changes>

## 3.3 Abbreviations

For the purposes of the present document, the abbreviations given in TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in TR 21.905 [1].

AAS Active Antenna System

ACLR Adjacent Channel Leakage Ratio

ACS Adjacent Channel Selectivity

ATG Air to Ground

AWGN Additive White Gaussian Noise

BS Base Station

BW Bandwidth

CA Carrier Aggregation

CACLR Cumulative ACLR

CP-OFDM Cyclic Prefix-OFDM

CW Continuous Wave

DFT-s-OFDM Discrete Fourier Transform-spread-OFDM

DM-RS Demodulation Reference Signal

E-UTRA Evolved UTRA

EVM Error Vector Magnitude

FDD Frequency Division Duplex

FR Frequency Range

GSCN Global Synchronization Channel Number

GSM Global System for Mobile communications

HAPS High Altitude Platform Station

ITU‑R Radiocommunication Sector of the International Telecommunication Union

ICS In-Channel Selectivity

LA Local Area

LNA Low Noise Amplifier

LP-WUS Low-Power Wake-Up Signal

MR Medium Range

NB-IoT Narrowband – Internet of Things

NR New Radio

NR-ARFCN NR Absolute Radio Frequency Channel Number

OBUE Operating Band Unwanted Emissions

OCC Orthogonal Covering Code

OTA Over The Air

RB Resource Block

RDN Radio Distribution Network

REFSENS Reference Sensitivity

RF Radio Frequency

RIB Radiated Interface Boundary

RMR Railway Mobile Radio

RMS Root Mean Square (value)

RS Reference Signal

RV Redundancy Version

RX Receiver

SCS Sub-Carrier Spacing

SDL Supplementary Downlink

SSB Synchronization Signal Block

SUL Supplementary Uplink

TAB Transceiver Array Boundary

TAE Time Alignment Error

TDD Time division Duplex

TDL Tapped Delay Line

TX Transmitter

TT Test Tolerance

UCI Uplink Control Information

ZF Zero Forcing

<Next change>

## 4.6 Manufacturer declarations

The following BS declarations listed in table 4.6-1, when applicable to the BS under test, are required to be provided by the manufacturer for the conducted requirements testing of the *BS type 1-C* and *BS type 1-H*.

For the *BS type 1-H* declarations required for the radiated requirements testing, refer to TS 38.141-2 [3].

Table 4.6-1 Manufacturer declarations for *BS type 1-C* and *BS type 1-H* conducted test requirements

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Declaration identifier | Declaration | Description | Applicability | |
|  |  |  | *BS type 1-C* | *BS type 1-H* |
| D.1 | BS requirements set | Declaration of one of the NR base station *requirement's set* as defined for *BS type 1-C*, or *BS type 1-H*. | x | x |
| D.2 | BS class | BS class of the BS, declared as Wide Area BS, Medium Range BS, or Local Area BS. | x | x |
| D.3 | *Operating bands* and frequency ranges | List of NR *operating band(s)* supported by *single-band connector(s)* and/or *multi-band connector(s)* of the BS and if applicable, frequency range(s) within the *operating band(s)* that the BS can operate in.  Declarations shall be made per *antenna connector* for *BS type 1-C*, or *TAB connector* for *BS type 1-H*. | x | x |
| D.4 | Spurious emission category | Declare the BS spurious emission category as either category A or B with respect to the limits for spurious emissions, as defined in Recommendation ITU-R SM.329 [5]. | x | x |
| D.5 | Additional operating band unwanted emissions | The manufacturer shall declare whether the BS under test is intended to operate in geographic areas where the additional operating band unwanted emission limits defined in clause 6.6.4.5.6 apply. (Note 3, Note 6). | x | x |
| D.6 | Co-existence with other systems | The manufacturer shall declare whether the BS under test is intended to operate in geographic areas where one or more of the systems GSM850, GSM900, DCS1800, PCS1900, UTRA FDD, UTRA TDD, E-UTRA, PHS and/or NR operating in another band are deployed. | x | x |
| D.7 | Co-location with other base stations | The manufacturer shall declare whether the BS under test is intended to operate co-located with Base Stations of one or more of the systems GSM850, GSM900, DCS1800, PCS1900, UTRA FDD, UTRA TDD, E-UTRA and/or NR operating in another band. | x | x |
| D.8 | *Single band connector* or *multi-band connector* | Declaration of the single band or multi-band capability of *single band connector(s)* or *multi-band connector(s),* declared for every connector. | x | x |
| D.9 | Contiguous or non-contiguous spectrum operation support | Ability to support contiguous or non-contiguous (or both) frequency distribution of carriers when operating multi-carrier. Declared per *single band connector* or *multi-band connector*, per *operating band*. | x | x |
| D.10 | void | void | x | x |
| D.11 | Maximum *Base Station RF Bandwidth* | Maximum *Base Station RF Bandwidth* in the *operating band* for single-band operation. Declared per supported *operating band,* per *antenna connector* for *BS type 1-C*, or *TAB connector* for *BS type 1-H.* (Note 2) | x | x |
| D.12 | Maximum *Base Station RF Bandwidth* for multi-band operation | Maximum *Base Station RF Bandwidth* for multi-band operation. Declared per supported *operating band,* per *antenna connector* for *BS type 1-C*, or *TAB connector* for *BS type 1-H.* | x | x |
| D.13 | Total RF bandwidth (BWtot) | Total RF bandwidth BWtot of transmitter and receiver, declared per the band combinations (D.27). | x | x |
| D.14 | NR supported channel bandwidths and SCS | NR supported SCS and channel bandwidths per supported SCS. Declared per supported *operating band,* per *antenna connector* for *BS type 1-C*, or *TAB connector* for *BS type 1-H.* | x | x |
| D.15 | CA only operation | Declaration of CA-only operation (with equal power spectral density among carriers) but not multiple carriers, declared per *operating band* per *antenna connector* for *BS type 1-C*, or *TAB connector* for *BS type 1-H*. | x | x |
| D.16 | Single or multiple carrier | Capable of operating with a single carrier (only) or multiple carriers. Declared per supported *operating band*, per *antenna connector* for *BS type 1-C*, or *TAB connector* for *BS type 1-H.* | x | x |
| D.17 | Maximum number of supported carriers per operating band in single band operation | Maximum number of supported carriers per supported *operation band* in single band operation*.* Declared per supported *operating band*, per *antenna connector* for *BS type 1-C*, or *TAB connector* for *BS type 1-H.* (Note 2) | x | x |
| D.18 | Maximum number of supported carriers per operating band in multi-band operation | Maximum number of supported carriers per supported *operation band* in multi-band operation. (Note 2) | x | x |
| D.19 | Total maximum number of supported carriers in multi-band operation | Maximum number of supported carriers for all supported *operating bands* in multi-band operation*.* Declared for all connectors (D.18)*.* | x | x |
| D.20 | Other band combination multi-band restrictions | Declare any other limitations under simultaneous operation in the declared band combinations (D.27) for each *multi-band connector* which have any impact on the test configuration generation.  Declared for every *multi-band connector*. | x | x |
| D.21 | Rated carrier output power(Prated,c,AC, or Prated,c,TABC) | Conducted rated carrier output power, per *single band connector* or *multi-band connector.*  Declared per supported *operating band*, per *antenna connector* for *BS type 1-C*, or *TAB connector* for *BS type 1-H*. (Note 1, 2, 7) | x | x |
| D.22 | R*ated total output power* (Prated,t,AC, or Prated,t,TABC) | Conducted total rated output power*.*  Declared per supported *operating band*, per *antenna connector* for *BS type 1-C*, or *TAB connector* for *BS type 1-H.*  For *multi-band connectors* declared for each supported *operating band* in each supported band combination. (Note 1, 2, 7) | x | x |
| D.23 | Rated multi-band total output power, Prated,MB,TABC | Conducted multi-band rated total output power*.*  Declared per supported operating band combinations, per *multi-band connector*. (Note 1, 7) | x | x |
| D.24 | Ncells | Number corresponding to the minimum number of cells that can be transmitted by a BS in a particular *operating band* with transmission on all *TAB connectors* supporting the *operating band*. |  | x |
| D.25 | Maximum supported power difference between carriers | Maximum supported power difference between carriers. Declared per supported *operating band*, per *antenna connector* for *BS type 1-C*, or *TAB connector* for *BS type 1-H.* | x | x |
| D.26 | Maximum supported power difference between carriers is different *operating bands* | Supported power difference between any two carriers in any two different supported *operating bands.* Declared per supported operating band combination, per *multi-band connector.* | x | x |
| D.27 | Operating band combination support | List of operating bands combinations supported by *single-band connector(s)* and/or *multi-band connector(s)* of the BS. Declared per *antenna connector* for *BS type 1-C*, or *TAB connector* for *BS type 1-H.* | x | x |
| D.28 | void | void | x | x |
| D.29 | Intra-system interfering signal declaration list | List of *single band connector(s)* or *multi-band connector(s)* for which an intra-system interfering signal level is required to be declared. Declaration is required if the intra-system interfering signal level is larger than the co-location interfering signal level. |  | x |
| D.30 | Intra-system interfering signal level | The interfering signal level in dBm. Declared per supported *operating band*, per *TAB connector* for *BS type 1-H* covered by D.29. |  | x |
| D.31 | TAE groups | Set of declared *TAB connector beam forming groups* on which the TAE requirements apply.  *All TAB connectors* belong to at least one *TAB connector beam forming group* (even if it's a *TAB connector beam forming group* consisting of one connector).  The smallest possible number of *TAB connector beam forming groups* need to be declared such that there is no *TAB connector* not contained in at least one of the declared *TAB connector beam forming groups*.  Declared per supported *operating band*. |  | x |
| D.32 | Equivalent connectors | List of *antenna connectors* of *BS type 1-C*, or *TAB connector* of *BS type 1-H*, which have been declared equivalent.  Equivalent connectors imply that the *antenna connector* of *BS type 1-C*, or *TAB connector* of *BS type 1-H*, are expected to behave in the same way when presented with identical signals under the same operating conditions. All declarations made for the *antenna connector* of *BS type 1-C*, or *TAB connector* of *BS type 1-H* are identical and the transmitter unit and/or receiver unit driving the *antenna connector* of *BS type 1-C* or *TAB connector* of *BS type 1-H* are of identical design. | x | x |
| D.33 | *TAB connector RX min cell group* | Declared as a group of *TAB connectors* to which RX requirements are applied. This declaration corresponds to group of *TAB connectors* which are responsible for receiving a cell when the *BS type 1-H* setting corresponding to the declared minimum number of cells (Ncells) with transmission on all *TAB connectors* supporting an *operating band*. |  | x |
| D.34 | *TAB connector TX min cell group* | Declared group of *TAB connectors* to which TX requirements are applied. This declaration corresponds to group of *TAB connectors* which are responsible for transmitting a cell when the *BS type 1-H* setting corresponding to the declared minimum number of cells (Ncells) with transmission on all *TAB connectors* supporting an *operating band*. |  | x |
| D.35 | Connecting network loss range for BS testing with ancillary RF amplifiers | Declaration of the range of connecting network losses (in dB) for *BS type 1-C* testing with ancillary Tx RF amplifier only, or with Rx RF amplifier only, or with combined Tx/Rx RF amplifiers. (Note 4) | x |  |
| D.36 | Relation between supported maximum RF bandwidth, number of carriers and Rated total output power | If the rated total output power and total number of supported carriers are not simultaneously supported, the manufacturer shall declare the following additional parameters:  - The reduced number of supported carriers at the rated total output power;  - The reduced total output power at the maximum number of supported carriers. | x | x |
| D.37 | *TAB connectors* used for performance requirement testing | To reduce test complexity, declaration of a representative (sub)set of *TAB connectors* to be used for performance requirement test purposes. At least one *TAB connector* mapped to each *demodulation branch* is declared. |  | x |
| D.38 | Inter-band CA | Band combinations declared to support inter-band CA (per CA capable *multi-band connector(s)*, as in D.15).  Declared for every *multi-band connector* which support CA. | x | x |
| D.39 | Intra-band contiguous CA | Bands declared to support intra-band contiguous CA (per CA capable *single band connector(s)* or *multi-band connector(s)*, as in D.15).  Declared per *antenna connector* for *BS type 1-C*, or *TAB connector* for *BS type 1-H*. | x | x |
| D.40 | Intra-band non-contiguous CA | Bands declared to support intra-band non-contiguous CA (per CA capable *single band connector(s)* or *multi-band connector(s)*, as in D.15).  Declared per *antenna connector* for *BS type 1-C*, or *TAB connector* for *BS type 1-H*. | x | x |
| D.41 | NB-IoT operation | Manufacturer shall declare the support of NB-IoT operation in NR in-band and the number of supported NB-IoT carriers in total and for each supported band, frequency range and channel bandwidth. | x |  |
| D.42 | NB-IoT sub-carrier spacing | If the BS supports NB-IoT operation in NR in-band, manufacturer shall declare if it supports 15 kHz sub-carrier spacing, 3.75 kHz sub-carrier spacing, or both for NPUSCH. | x |  |
| D.43 | NB-IoT power dynamic range | If the BS supports NB-IoT operation in NR in-band, manufacturer shall declare the maximum power dynamic range it could support with a minimum of +6dB or +3dB as specified in clause 6.3.4 of TS 38.104 [2] (Note 5). | x |  |
| D.100 | PUSCH mapping type | Declaration of the supported PUSCH mapping type as specified in TS 38.211 [17], i.e., type A, type B or both. | x | x |
| D.101 | PUSCH additional DM-RS positions | Declaration of the supported additional DM-RS position(s), i.e., pos0, pos1 or both. |  |  |
| D.102 | PUCCH format | Declaration of the supported PUCCH format(s) as specified in TS 38.211 [17], i.e., format 0, format 1, format 2, format 3, format 4. | x | x |
| D.103 | PRACH format and SCS | Declaration of the supported PRACH format(s) as specified in TS 38.211 [17], i.e., format: 0, A1, A2, A3, B4, C0, C2.  Declaration of the supported SCS(s) per supported PRACH format with short sequence, as specified in TS 38.211 [17], i.e., 15 kHz, 30 kHz or both. | x | x |
| D.104 | Additional DM-RS for PUCCH format 3 | Declaration of the supported additional DM-RS for PUCCH format 3: without additional DM-RS, with additional DM-RS or both. | x | x |
| D.105 | Additional DM-RS for PUCCH format 4 | Declaration of the supported additional DM-RS for PUCCH format 4: without additional DM-RS, with additional DM-RS or both. | x | x |
| D.106 | PUCCH multi-slot | Declaration of multi-slot PUCCH support. | x | x |
| D.107 | UL CA | For the highest supported SCS, declaration of the carrier combination with the largest aggregated bandwidth. If there is more than one combination, the carrier combination with the largest number of carriers shall be declared. | x | x |
| D.108 | High speed train | Declaration of high speed train scenario support, i.e. HST support or no HST support | x | x |
| D.109 | Maximum speed of high speed train for PUSCH | Declaration of supported maximum speed for high speed train scenario, i.e. 350 km/h or 500 km/h.  This declaration is applicable to PUSCH for high speed train and UL timing adjustment only if BS declares to support high speed train in D.108. | x | X |
| D.110 | PRACH format for high speed train | Declaration of supported PRACH format(s) for high speed train scenario, i.e. format 0 restricted set type A, format 0 restricted set type B, format A2, format B4, format C2.  This declaration is applicable to PRACH for high speed train only if BS declares to support high speed train in D.108. | x | x |
| D.111 | Interlaced formats | Declaration of support of interlaced PUSCH and PUCCH formats. | x | x |
| D.112 | PRACH format with LRA = 1151 for 15 kHz SCS and LRA = 571 for 30 kHz SCS | Declaration of the supported PRACH format(s) as specified in TS 38.211 [17], i.e., format: A2, B4, C2.    Declaration of the supported SCS(s) per supported PRACH format as specified in TS 38.211 [17], i.e., 15 kHz, 30 kHz or both. | x | x |
| D.113 | CG-UCI | Declaration of support of GC-UCI multiplexed on PUSCH as specified in TS 38.211 [17]. | x | x |
| D.114 | 2-step RA | Declaration of support of 2-step RA type. | x | x |
| D.115 | PUSCH 256QAM | Declaration of PUSCH 256QAM support | x | x |
| D.116 | PUCCH sub-slot based repetition formats | Declaration of PUCCH sub-slot based repetition formats | x | x |
| D.117 | PUSCH TB over Multi-slots | BS support TBoMS over physical consecutive UL slots | x | x |
| D.118 | PUSCH TB over Multi-slots | BS support TBoMS over physical non-consecutive UL slots | x | x |
| D.119 | Supported SCS for TDD PUSCH DM-RS bundling and PUCCH DM-RS bundling | Declaration of supported SCS for TDD PUSCH DM-RS bundling and and PUCCH DM-RS bundling and, i.e. {15kHz, 30kHz, 60kHz 120kHz} | x | x |
| D.120 | Supported FDD PUSCH DM-RS bundling and and PUCCH DM-RS bundling and | Declaration of supporting FDD PUSCH DM-RS bundling and PUCCH DM-RS bundling | x | x |
| D.121 | MCS index table 3 | Declaration of support MCS index table 3 as specified in TS 38.214 [18]. | x | x |
| D.122 | PUSCH repetition type A | Declaration of support PUSCH repetition type A | x | x |
| D.123 | Air-to-ground scenario | Declaration of air-to-ground scenario support, i.e., ATG support or no ATG support | x | x |
| D.124 | PUSCH with enhanced DM-RS | Declaration of support for *enhanced-dmrs-Type r18* as specified in TS 38.211 [17]. | x | x |
| D.125 | PRACH format for HAPS scenario | Declaration of supported PRACH format(s) for HAPS scenario, i.e., format 1. | x | x |
| [D.126] | LP-WUS operation | Declaration of support for LP-WUS. | x | x |
| [D.127] | LP-WUS power boosting | Declaration of support for power boosting for LP-WUS with a minimum of +3dB which is applicable to CBWs equal to or larger than 50 MHz, different boosting levels may be declared for smaller CBWs. | x | x |
| NOTE 1: If a BS is capable of 1024QAM DL operation then up to three rated output power declarations may be made. One declaration is applicable when configured for 1024QAM transmissions, a different declaration is applicable when configured 256QAM transmissions and the other declaration is applicable when configured neither for 256QAM nor 1024QAM transmissions.  NOTE 2: Parameters for contiguous or non-contiguous spectrum operation in the operating band are assumed to be the same unless they are separately declared. When separately declared, they shall still use the same declaration identifier.  NOTE 3: If BS is declared to support Band n20 (D.3), the manufacturer shall declare if the BS may operate in geographical areas allocated to broadcasting (DTT). Additionally, related declarations of the emission levels and maximum output power shall be declared.  NOTE 4: This manufacturer declaration is optional.  NOTE 5: This manufacturer may declare two values, one with a minimum of +6dB and the other with a minimum of +3dB.  NOTE 6: If BS is declared to support Band n24 (D.3), the manufacturer shall declare if the BS may operate in geographical areas where FCC regulations apply. Additionally, related declarations of the emission levels and maximum output power shall be declared.  NOTE 7: If a BS is capable of 256QAM DL operation but not capable of 1024QAM DL operation then up to two rated output power declarations may be made. One declaration is applicable when configured for 256QAM transmissions, and the other declaration is applicable when not configured for 256QAM transmissions | | | | |

<Next change>

#### 6.6.3.1 Definition and applicability

Adjacent Channel Leakage power Ratio (ACLR) is the ratio of the filtered mean power centred on the assigned channel frequency to the filtered mean power centred on an adjacent channel frequency.

The requirements shall apply outside the Base Station RF Bandwidth or Radio Bandwidth whatever the type of transmitter considered (single carrier or multi-carrier) and for all transmission modes foreseen by the manufacturer's specification.

The requirements shall also apply if the BS supports NB-IoT operation in NR in-band.

The requirements shall also apply if the BS supports LP-WUS operation

For a BS operating in non-contiguous spectrum, the ACLR or the CACLR requirement in Tables 6.6.3.5.2-3 to 6.6.3.5.2.4a shall apply in *sub block gaps*, depending on the *operating band* and the *sub-block* *gap size* (Wgap) where the limit applies.

For a *multi-band connector*, the ACLR or the CACLR requirement in Tables 6.6.3.5.2-3 to 6.6.3.5.2.4a shall apply in *Inter RF Bandwidth gaps*, depending on the *operating band* and the *Inter RF Bandwidth gap size* (Wgap) where the limit applies.

The requirement applies during the *transmitter ON period*.

< Next change>

#### 6.6.4.1 Definition and applicability

Unless otherwise stated, the operating band unwanted emission (OBUE) limits in FR1 are defined from ΔfOBUE below the lowest frequency of each supported downlink *operating band* up to ΔfOBUE above the highest frequency of each supported downlink *operating band*. The values of ΔfOBUE are defined in table 6.6.1‑1 for the NR *operating bands*.

The requirements shall apply whatever the type of transmitter considered and for all transmission modes foreseen by the manufacturer's specification. In addition, for a BS operating in non-contiguous spectrum, the requirements apply inside any sub-block gap. In addition, for a BS operating in multiple bands, the requirements apply inside any Inter RF Bandwidth gap.

B*asic limits* are specified in the tables below, where:

- Δf is the separation between the channel edge frequency and the nominal -3 dB point of the measuring filter closest to the carrier frequency.

- f\_offset is the separation between the channel edge frequency and the centre of the measuring filter.

- f\_offsetmax is the offset to the frequency ΔfOBUE outside the downlink *operating band*, where ΔfOBUE is defined in table 6.6.1-1.

- Δfmax is equal to f\_offsetmax minus half of the bandwidth of the measuring filter.

For a *multi-band connector* inside any *Inter RF Bandwidth gaps* with Wgap < 2\*ΔfOBUE, a combined *basic* limit shall be applied which is the cumulative sum of the *basic limit*s specified at the *Base Station RF Bandwidth edges* on each side of the *Inter RF Bandwidth gap*. The *basic limit* for *Base Station RF Bandwidth edge* is specified in the clauses 6.6.4.5.2 to 6.6.4.5.5below, where in this case:

- Δf is the separation between the *Base Station RF Bandwidth edge* frequency and the nominal -3 dB point of the measuring filter closest to the *Base Station RF Bandwidth edge*.

- f\_offset is the separation between the *Base Station RF Bandwidth edge* frequency and the centre of the measuring filter.

- f\_offsetmax is equal to the *Inter RF Bandwidth gap* minus half of the bandwidth of the measuring filter.

- Δfmax is equal to f\_offsetmax minus half of the bandwidth of the measuring filter.

For a *multi-band connector*, the operating band unwanted emission *basic limits* apply also in a supported operating band without any carrier transmitted, in the case where there are carrier(s) transmitted in another supported operating band. In this case, no cumulative *basic limit* is applied in the *inter-band gap* between a supported downlink operating band with carrier(s) transmitted and a supported downlink operating band without any carrier transmitted and

- In case the *inter-band gap* between a supported downlink operating band with carrier(s) transmitted and a supported downlink operating band without any carrier transmitted is less than 2\*ΔfOBUE, f\_offsetmax shall be the offset to the frequency ΔfOBUE MHz outside the outermost edges of the two supported downlink operating bands and the operating band unwanted emission *basic limit* of the band where there are carriers transmitted, as defined in the tables of the present clause, shall apply across both downlink bands.

- In other cases, the operating band unwanted emission *basic limits* of the band where there are carriers transmitted, as defined in the tables of the present clause for the largest frequency offset (Δfmax), shall apply from ΔfOBUE MHz below the lowest frequency, up to ΔfOBUE MHz above the highest frequency of the supported downlink operating band without any carrier transmitted.

For a multicarrier *single-band connector* or a *single-band connector* configured for intra-band contiguous or non-contiguous carrier aggregation the definitions above apply to the lower edge of the carrier transmitted at the lowest carrier frequency and the upper edge of the carrier transmitted at the highest carrier frequency within a specified frequency band.

In addition inside any sub-block gap for a *single-band connector* operating in non-contiguous spectrum, a combined *basic limit* shall be applied which is the cumulative sum of the *basic limit*s specified for the adjacent sub blocks on each side of the sub block gap. The *basic limit* for each sub block is specified in the subcluases 6.6.4.5.2 to 6.6.4.5.5below, where in this case:

- Δf is the separation between the sub block edge frequency and the nominal -3 dB point of the measuring filter closest to the sub block edge.

- f\_offset is the separation between the sub block edge frequency and the centre of the measuring filter.

- f\_offsetmax is equal to the sub block gap bandwidth minus half of the bandwidth of the measuring filter.

- Δfmax is equal to f\_offsetmax minus half of the bandwidth of the measuring filter.

For Wide Area BS, the requirements of either clause 6.6.4.5.2 (Category A limits) or clause 6.6.4.5.3 (Category B limits) shall apply.

For Medium Range BS, the requirements in clause 6.6.4.5.4 shall apply (Category A and B).

For Local Area BS, the requirements of clause 6.6.4.5.5 shall apply (Category A and B).

The requirements shall also apply if the BS supports NB-IoT operation in NR in-band.

The requirements shall also apply if the BS supports LP-WUS operation.

The application of either Category A or Category B *basic limits* shall be the same as for transmitter spurious emissions in clause 6.6.5.

<Next change>

#### 6.6.5.1 Definition and applicability

The transmitter spurious emission limits shall apply from 9 kHz to 12.75 GHz, excluding the frequency range from ΔfOBUE below the lowest frequency of each supported downlink *operating band*, up to ΔfOBUE above the highest frequency of each supported downlink *operating band*, where the ΔfOBUE is defined in table 6.6.1. For some *operating bands*, the upper limit is higher than 12.75 GHz in order to comply with the 5th harmonic limit of the downlink *operating band*, as specified in ITU-R recommendation SM.329 [5].

For a *multi-band connector*, each supported *operating band* together with ΔfOBUE around the band is excluded from the transmitter spurious emissions requirement.

The requirements shall apply whatever the type of transmitter considered (single carrier or multi-carrier). It applies for all transmission modes foreseen by the manufacturer's specification.

The requirements shall apply to BS that support NR or NR with NB-IoT operation in NR in-band.

The requirements shall also apply if the BS supports LP-WUS operation.

Unless otherwise stated, all requirements are measured as mean power (RMS).

For operation in region 2, where the FCC guidance for MIMO systems in FCC Title 47 [13] is applicable, NTXU,countedpercell shall be equal to one for the purposes of calculating the spurious emissions limits in clauses 6.6.5. For all other unwanted emissions requirements, NTXU,countedpercell shall be the value calculated according to clause 6.1.

<Next change>

##### 6.7.5.1.1 Co-location minimum requirements

For *BS type 1-C*, the wanted signal and interfering signal centre frequency is specified in table 6.7.5.1.1-1, where interfering signal level is *rated total output power* (Prated,t,AC) at *antenna connector* in the *operating band* – 30 dB.

The requirement is applicable outside the Base Station RF Bandwidth or Radio Bandwidth. The interfering signal offset is defined relative to the Base Station RF Bandwidth edges or Radio Bandwidth edges.

For a BS operating in non-contiguous spectrum, the requirement is also applicable inside a sub-block gap for interfering signal offsets where the interfering signal falls completely within the sub-block gap. The interfering signal offset is defined relative to the sub-block edges.

For a *multi-band connector*, the requirement shall apply relative to the Base Station RF Bandwidth edges of each supported operating band. In case the Inter RF Bandwidth gap is less than 3\*BWChannel MHz (where BWChannel is the minimal *BS channel bandwidth* of the band), the requirement in the gap shall apply only for interfering signal offsets where the interfering signal falls completely within the Inter RF Bandwidth gap.

The transmitter intermodulation level shall not exceed the unwanted emission limits in clauses 6.6.3, 6.6.4 and 6.6.5 in the presence of an NR interfering signal according to table 6.7.5.1.1-1.

The requirements shall also apply if the BS supports LP-WUS operation.

<End of changes>