# FS\_XRM\_Ph2 KI#6 Summary

Agreeable principle

Needs more discussion

## Wireline access

|  |  |  |
| --- | --- | --- |
| **ECN marking in** | **Supported by W-AGF**  **(N2 Signaling)** | **Supported by 5G-RG**  **(N1 Signaling)** |
| W-AGF | Indication of ECN marking for L4S | NA |
| Wireline nodes | Mapping between 5G QoS and wireline QoS for DL | Mapping between 5G QoS and wireline QoS for UL |
| 5G-RG | NA | Indication of ECN marking for L4S |

## Untrusted/trusted access

|  |  |
| --- | --- |
| **ECN marking in** | **Supported by N3IWF/TNGF (N2 Signaling)** |
| N3IWF/TNGF | Indication of ECN marking for L4S |
| WLAN | Establishing a dedicated child SA for L4S |