**3GPP TSG-SA3 Meeting #115 *draft\_S3-240698-r2***

Athens, Greece, 26th February - 1st March 2024

**Source: Samsung, KDDI, THALES, IDEMIA**

**Title: Permanent secret key length (K)**

**Document for: Approval**

**Agenda Item: 5.5**

# 1 Decision/action requested

***It is proposed to approve this key issue on long-term key K entropy to study potential solutions.***

# 2 References

[1] [S3‑235091](https://www.3gpp.org/ftp/tsg_sa/WG3_Security/TSGS3_113_Chicago/docs/S3-235091.zip) New SID on study on enabling a cryptographic algorithm transition to 256 bits

[2] 3GPP TS 31.102 Characteristics of the Universal Subscriber Identity Module (USIM) application (Release 18)

[3] 3GPP TS 33.102 3G Security; Security architecture (Release 17)

[4] 3GPP TS 33.501 Security architecture and procedures for 5G system (Release 18)

# 3 Rationale

In SA3#113 meeting, a SID to study on enabling a cryptographic algorithm transition to 256 bits was agreed. Based on the objectives in [S3‑235091](https://www.3gpp.org/ftp/tsg_sa/WG3_Security/TSGS3_113_Chicago/docs/S3-235091.zip) [1], it is proposed to study the challenges in supporting both 128 bits and 256 bits key.

According to the below excerpt from TS 31.102 [2], it is evident that the USIM supports subscription with permanent secret key length of 128 bits or 256 bits.

## 6.1 Authentication and key agreement procedure

…………

A permanent secret key K is used in this procedure. This key K has a length of 128 bits or 256 bits and is stored within the USIM for use in the algorithms described below. Also more than one secret key K can be stored in the USIM. The active key to be used by the algorithms is signalled within the AMF field in the AUTN.

………….

Following are the length of authentication parameters as specified in TS 33.102 [3].

………….

### 6.3.7 Length of authentication parameters

The authentication key (K) shall have a length of 128 bits or 256 bits.

NOTE: Examples of algorithm set for 3GPP authentication and key agreement functions allow either an authentication key K with only a length of 128 bits, or an authentication key K with a length of 128 bits or 256 bits. Depending on the chosen algorithm set, the operator may have the choice of the length of the authentication key K (128 bits or 256 bits).

The random challenge (RAND) shall have a length of 128 bits.

Sequence numbers (SQN) shall have a length of 48 bits.

The anonymity key (AK) shall have a length of 48 bits.

The authentication management field (AMF) shall have a length of 16 bits.

The message authentication codes MAC in AUTN and MAC‑S in AUTS shall have a length of 64 bits.

The cipher key (CK) shall have a length of 128 bits.

The integrity key (IK) shall have a length of 128 bits.

The authentication response (RES) shall have a variable length of 4‑16 octets.

………….

According to the above excerpt, CK and IK shall have a length of 128 bits (combining gives 256 bits). Further based on the key derivation and distribution as specified in clause 6.2.2 in TS 33.501 [4], NAS and AS keys are truncated to 128 bits for 128 bits algorithm. If UE and network negotiate and agree to use 256 bits security algorithm, the derived NAS and AS keys would be used without truncation.

Following are the scenarios when a permanent key (K) in the USIM has 256 bits or 128 bits key length, respectively:

**Permanent key length (K) is 256 bits**

If UE and network negotiate and agree to use either 256 bits or 128 bits security algorithm, it provides sufficient entropy in both cases.

**Permanent key length (K) is 128 bits**

If UE and network negotiate and agree to use 128 bits security algorithm, it provides sufficient entropy.

But in case if UE and network negotiate and agree to use 256 bits security algorithm, it does not provide sufficient entropy.

**Observation:** The security algorithm negotiation between UE and the network to select either 128 bits or 256 bits security algorithm without considering the permanent key length will result in insufficient entropy in case when 128 bits K is used and 256 bit algorithm is selected.

# 4 Detailed proposal

\*\*\* Start of 1st Change \*\*\*

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

 [xx] 3GPP TS 33.501: "Security architecture and procedures for 5G system".

\*\*\* Start of 2nd Change \*\*\*

## 5.X Key Issue #X: Key Issue on using different permanent secret key lengths

### 5.X.1 Key issue details

As per TS 33.501 [xx], the long-term key K length could be either 128 bits or 256 bits long. If the long-term key K length is 128 bits, it does not have any security benefit to use 256 bits algorithm.

According to TS 33.501 [xx], the NAS and AS keys are truncated to 128 bits for 128 bits algorithm. If UE and the network negotiate and agree to use 256 bits algorithm, the derived NAS and AS keys would be used without truncation.

The length of the permanent secret key to be taken into account when selecting the algorithms.

### 5.X.2 Security threats

Not applicable

### 5.X.3 Potential security requirements

The 5G system shall support the negotiation of security algorithm (either 128 bits or 256 bits) based on the permanent secret key length (K).

\*\*\* End of Changes \*\*\*