**3GPP TSG-SA3 Meeting #115 *draft\_S3-240909-r3***

Athens, Greece, 26th February - 1st March 2024

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** | **1934** | **rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **x** |

|  |
| --- |
|  |
| ***Title:***  | Details of the DNS security mechanism in EDGE computing (roaming) |
|  |  |
| ***Source to WG:*** | Nokia, Nokia Shanghai Bell |
| ***Source to TSG:*** | S3 |
|  |  |
| ***Work item code:*** | EDGE\_Ph2 |  | ***Date:*** | 2024-02-19 |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | To provide details of the DNS security mechanism (DNS over TLS, namely DoT) in the context of EDGE computing. DoT has been agreed to be specified as protection mechanism for more secure and private DNS resolution process between UE and V-EASDF in EDGE architecture as defined by 3GPP. IETF RFCs 7858 and 8310 specify DoT and usage profiles for DoT respectively, including several configuration options. This CR is intended to profile the mechanism by selecting the options of Strict Privacy profile. |
|  |  |
| ***Summary of change:*** | Providing details for DoT specified security mechanism |
|  |  |
| ***Consequences if not approved:*** | Specification would be incomplete, and may cause interoperability issues.  |
|  |  |
| ***Clauses affected:*** | Annex T |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  |  |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  |  |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  |  |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\*\*\*\*\* FIRST CHANGE\*\*\*\*\*\*

# T.4 Security of EAS discovery procedure via V-EASDF in roaming Scenario

DNS over TLS and Strict Privacy usage profile as specified in IETF RFC 7858 [83] and RFC 8310 [84] should be supported by the UE and the V-EASDF. The DNS connection shall be authenticated and encrypted.

NOTE X: Other DNS protection mechanisms are subject to implementation.

The security information of the V-EASDF can be preconfigured in the UE by using out of band mechanisms or if the core network is used to configure the security information, the V-SMF is preconfigured with the V-EASDF security information (authentication information, supported security mechanisms, port number, etc.) and provides the security information to the UE as follows:

- In the case of LBO roaming, the V-SMF provides the V-EASDF security information to the UE via PCO.

- In the case of HR with Session Breakout (HR-SBO) roaming scenarios, during the PDU session establishment or modification procedure, the V-SMF provides the V-EASDF security information via Nsmf\_PDUSession\_Create/ Nsmf\_PDUSession\_Update to H-SMF when the V-SMF determines to use a V-EASDF for EAS discovery, and the H-SMF provides the V-EASDF security information to UE via PCO if HR SBO is authorized.

NOTE: The security information of V-EASDF provided to the UE is only related with the VPLMN parameter.

According to the clause 6.4.1.3 of TS 24.501, upon receiving the DNS server security information, the UE passes it to the upper layer. The UE uses this information to send the DNS over TLS. Additionally, the clause 10.5.6.3 of TS 24.008 provides the configuration of the different options of DNS over TLS specified in the RFC 7858 [83].

\*\*\*\*\* END of FIRST CHANGE\*\*\*\*\*\*