**3GPP TSG-SA3 Meeting #115 *S3-240851-r1***

**Athens, February 26 - March 01, 2024**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **33.122** | **CR** | **0067** | **rev** | **1** | **Current version:** | **18.2.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Update for CAPIF 8 |
|  |  |
| ***Source to WG:*** | Xiaomi |
| ***Source to TSG:*** | S3 |
|  |  |
| ***Work item code:*** | SNAAPPY |  | ***Date:*** | 2024-2-05 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | According to clause 6.2.3 of TS 23.222, the interaction between Resource Owner Client and CCF over CAPIF-8 is not specified in the current release of the specification.However, clause 4.8 of TS 33.122 states that CAPIF-8 interface is not in scope of 3GPP. Therefore, there is a misalignment between TS 23.222 and TS 33.122. |
|  |  |
| ***Summary of change:*** | The following statement is captured.CAPIF-8 interface is not in scope of this specification.  |
|  |  |
| ***Consequences if not approved:*** | CAPIF-8 will be treated as not in the scope of 3GPP. |
|  |  |
| ***Clauses affected:*** | 4.8 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*Start of the Change \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

## 4.8 Security requirements on the CAPIF-8 reference points

CAPIF-8 interface is not in scope of this specification. Nevertheless, integrity and confidentiality protection, protection against replay attacks, privacy of the resource owner, authentication between the resource owner and the CCF need to be addressed by mechanism(s) which are out of 3GPP scope.\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*End of the Changes \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*