**3GPP TSG-SA5 Meeting #154 *S5-241855***

**Changsha, CHINA, 15 Apr - 19 Apr 2024**  Revision of S5-241610

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **32.290** | **CR** | **0223** | **rev** | **1** | **Current version:** | **18.5.0** |  |
|  |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Rel-18 CR 32.290 Correction on the threshold based re-authorization triggers |
|  |  |
| ***Source to WG:*** | Huawei |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** | TEI18 |  | ***Date:*** | 2024-04-17 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | Based on the conclusion of TR 28.826, NF consumer allows the service to continue whilst the re-authorization is progress, until the remaining part had been used up. However, how to handle the consumed remaining granted quotas during the re-authorization, be reported later or not, how to handle the remaing part if receiving a charging data response from CHF is not described. the corresponding mechanism should be clarified. |
|  |  |
| ***Summary of change:*** | Correct the description for the threshold based re-authorization triggers. |
|  |  |
| ***Consequences if not approved:*** | The description about the Threshold based re-authorization triggers is unclear. |
|  |  |
| ***Clauses affected:*** | 5.4.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ... |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

|  |
| --- |
| **First change** |

### 5.4.2 Threshold based re-authorization triggers

The CHF (NF Service Producer) may optionally include an indication to the NF Service Consumer of the remaining quota threshold that shall trigger a quota re-authorization.

If received quota threshold based re-authorization triggers (i.e. timeQuotaThreshold, volumeQuotaThreshold, unitQuotaThreshold), the NF Service Consumer shall seek re-authorization for the quota when the quota contents fall below the supplied threshold. The NF Service Consumer allows the service to continue whilst the re-authorization is progress, until the remaining part had been used up or receiving a Charging Data Response from CHF.

If the remaining part is exhausted before receiving a Charging Data Response:

- NF Service Consumer stops the service delivery and waits for the Charging Data Response.

If the Charging Data Response with new quota is received before the quota is exhausted:

- NF Service Consumer continues the service delivery, deducting the used units from the new granted quota.

If the Charging Data Response without new quota before the quota is exhausted:

- the NF Service Consumermay continue the service delivery until the quota is exhausted or stop the service delivery and reports the used unit.

|  |
| --- |
| **End of change** |