**3GPP TSG- Meeting # *d1***

**, , -**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.3* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** |  | | | | | | | | | |
| ***Source to TSG:*** | S5 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** |  | | | | |  | ***Date:*** | | |  |
|  |  | | | |  | |  | | |  |
| ***Category:*** |  |  | | | | | ***Release:*** | | |  |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)  Rel-20 (Release 20)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | CR S5-240243 was approved in meeting SA5#153 to remove definition of the fault management Mns from TS 28.532 , since it has been moved to TS 28.111, voiding clauses that are used as reference in other TS’s without adding any information that fault management Mns can now be found in 28.111. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Add clause 11.2.a with refererences to 28.111 for generic fault management Mns | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | lead to incorrect and incomplete implementation. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 2 and 11.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | S5-240243 | | | | | | | | |

|  |
| --- |
| **Start of modification** |

# 2 References

- The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] Void

[3] 3GPP TS 28.541: "Management and orchestration ; 5G Network Resource Model (NRM); Stage 2 and stage3".

[4] ITU-T Recommendation X.733 (02/92): "Information technology - Open Systems Interconnection - Systems Management: Alarm reporting function".

[5] 3GPP TS 28.531: "Management and orchestration ; Provisioning; ".

[6] 3GPP TS 28.554: "Management and orchestration ; 5G end to end Key Performance Indicators (KPI)".

[7] Void

[8] Void

[9] Void

[10] Void

[11] 3GPP TS 28.622: "Telecommunication management; Generic Network Resource Model (NRM) Integration Reference Point (IRP); Information Service (IS)".

[12] Void

[13] 3GPP TS 28.533: "Management and orchestration; Architecture framework"

[14] Void

[15] 3GPP TS 32.158: "Management and orchestration; Design rules for REpresentational State Transfer (REST) Solution Sets (SS)".

[16] Void

[17] Void

[18] 3GPP TS 28.552: "Management and orchestration; 5G performance measurements".

[19] 3GPP TS 32.401: "Telecommunication management; Perfomance Measurement (PM); Concept and requirements".

[20] ISO 8601:2004: "Data elements and interchange formats – Information interchange – Representation of dates and times".

[21] Void.

[22] Void.

[23] Void.

[24] Void.

[25] 3GPP TS 32.300: "Telecommunication management; Configuration Management (CM); Name convention for Managed Objects ".

[26] W3C REC-xmlschema-0-20010502: "XML Schema Part 0: Primer".

[27] W3C REC-xmlschema-1-20010502: "XML Schema Part 1: Structures".

[28] W3C REC-xmlschema-2-20010502: "XML Schema Part 2: Datatypes".

[29] W3C REC-xml-names-19990114: "Namespaces in XML".

[30] Void.

[31] Void.

[32] IETF RFC 6241 "Network Configuration Protocol (NETCONF)".

[33] 3GPP TS 32.160 " Management and orchestration; Management service template ".

[34] IETF RFC 7950 "The YANG 1.1 Data Modeling Language".

[35] Void

[36] IETF RFC 6902: "JavaScript Object Notation (JSON) Patch".

[37] IETF RFC 7396: "JSON Merge Patch".

[38] 3GPP TS 32.422: "Telecommunication management; Subscriber and equipment trace; Trace control and configuration management".

[39] 3GPP TS 32.423: "Telecommunication management; Subscriber and equipment trace; Trace data definition and management".

[40] IETF RFC 6455: "The WebSocket Protocol".

[41] IETF RFC 793: "Transmission Control Protocol".

[42] 3GPP TS 28.550: "Management and orchestration; Performance assurance".

[43] Void

[44] 3GPP TS 28.623: "Telecommunication management; Generic Network Resource Model (NRM) Integration Reference Point (IRP); Solution Set (SS) definitions".

[45] Text Attribution: Creator: ONAP, under Creative Commons Attribution 4.0 International License, https://creativecommons.org/licenses/by/4.0/, URI to access the text: <https://github.com/onap/vnfrqts-requirements/blob/05f26fac2b941513a7d0e856b99fd8c61d688299/docs/Chapter8/ves7_1spec.rst#resource-structure>.

[46] Void

[47] 3GPP TS 32.404: "Performance Management (PM); Performance measurements; Definitions and template".

[48] Void

[49] IETF RFC 8040: "RESTCONF protocol".

[50] IETF RFC 7951: " JSON Encoding of Data Modeled with YANG".

[51] IETF RFC 6243: "With-defaults Capability for NETCONF".

[52] IETF RFC 3339: " Date and Time on the Internet: Timestamps".

[53] 3GPP SA5 FORGE OpenAPI definitions: <https://forge.3gpp.org/rep/sa5>

[X] 3GPP TS 28.111: "Management and orchestration; Study on Network Slice Management Enhancement".

|  |
| --- |
| **Next modification** |

## 11.2 Void

## 11.2a Generic fault supervision management service

See TS 28.111 [x] for more information on Generic fault supervision management service.

|  |
| --- |
| **End of modification** |