**3GPP TSG-SA5 Meeting #154 *S5-242052d1***

Changsha, China, 15 - 19 April 2024

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **28.312** | **CR** | **0224**  | **rev** | **1** | **Current version:** | 18.3.0 |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Rel-18 CR TS 28.312 Correction of Expectation Targets |
|  |  |
| ***Source to WG:*** | China Unicom |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** | IDMS\_MN\_ph2 |  | ***Date:*** | 2024-03-25 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | There is a misunderstanding of examples of Expectation Targets for different Objects in Table 4.5.2-1. Each row represents an example of expectation, not an expectation Target. |
|  |  |
| ***Summary of change:*** | Correct Table 4.5.2-1: Examples of Expectation Targets for different Objects. |
|  |  |
| ***Consequences if not approved:*** | Table 4.5.2-1 may cause misunderstanding. |
|  |  |
| ***Clauses affected:*** | 4.5.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

|  |
| --- |
| **1st Change** |

### 4.5.2 Expectation Targets

For a given intent expectation, the desired characteristics of the object(s) are the expectation targets to be achieved. The expectation targets may include the metrics that characterize the performance of the object(s) or some abstract index that expresses the behaviour of the object(s). A given intent expectation may include multiple expectation targets on the same object or on different objects with the same properties. A consumer may for example require for the Network Slice object(s) that User throughput > 5Mbps and latency < 1ms. The expectation targets may also be context specific, i.e. the intent may require a specific expectation targets given a specific target context. As such with the characteristics as a combination of expectation targets and target contexts, the intent expectation may be stated as:

"ensure that for

 Expectation Object O,

 Expectation Target\_1 is T\_1, Target Context\_1 is C\_1

 ….,

 Expectation Target\_m is T\_m, Target Context\_k is C\_k;

Each expectation target expresses an aspect of the characteristics of the object under consideration, i.e. it expresses a desired characteristics on a specific object. Each of the object characteristic may be desired to be equivalent to a specific value or constrained to a value or a range of values, e.g. as listed in Table 4.5.2-1. The combination of the name of characteristic (or simply the targetName), the condition constraining the characteristic and the value or value range for the characteristic is the target, i.e. the Expectation Target is the tuple:

 Expectation Target = [targetName, condition, value range]

Table 4.5.2-1: Examples of Expectation Objects and Targets for different Intent expectations

|  |  |  |
| --- | --- | --- |
| Example of Intent Expectations | ExpectationObject | Example of Expectation Targets |
| targetName | Condition | Value range |
| example 1 | Network Slice | Coverage area | Is greater than | 40 km radius |
| example 2 | Communication Service | User throughput | Is greater than | 2 Mbps |

|  |
| --- |
| **End of Change** |