**3GPP TSG-SA5 Meeting #154 *S5-242161***

**Changsha, Hunan Province, China, 15th Apr 2024 - 19th Apr 2024**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | **28.541** | **CR** | **1192** | **rev** | **1** | **Current version:** | **17.14.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **x** | Core Network | **x** |

|  |
| --- |
|  |
| ***Title:***  | Rel-17 CR TS 28.541 Remove presence definition from support qualifier condition in NetworkSliceSubnet IOC |
|  |  |
| ***Source to WG:*** | Nokia |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** | TEI15 |  | ***Date:*** | 2024-04-04 |
|  |  |  |  |  |
| ***Category:*** | **A** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | The attribute condition defined for the conditional mandatory attribute nsInfo of NetworkSliceSubnet IOC describes when the attribute shall be absent, i.e., it is describing the condition for presence or absance of the attribute and not the constriant for support qualifier.  |
|  |  |
| ***Summary of change:*** | Corrected the support qualifier condition for attribute attribute nsInfo of NetworkSliceSubnet IOC |
|  |  |
| ***Consequences if not approved:*** | Inconsistent specification leads to confusion and incorrect implementation.  |
|  |  |
| ***Clauses affected:*** | 6.3.2.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This is a mirror of Rel-15 CR 1190 |
|  |  |
| ***This CR's revision history:*** | S5-241194 is revised to S5-242161 |

|  |
| --- |
| **1st Change** |

#### 6.3.2.3 Attribute constraints

|  |  |
| --- | --- |
| Name | Definition |
| nsInfo Support Qualifier | Condition: It shall be supported if the NetworkSliceSubnet instance is realized in the virtualized environment.  |

|  |
| --- |
| **End of change** |