**3GPP TSG-SA5 Meeting #162 *S5-253762***

Goteborg, Sweden, 25 - 29 August 2025

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | **32.298** | **CR** | **1055** | **rev** | 1 | **Current version:** | **19.2.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Rel-19 CR TS 32.298 Add a new field in IMS CDR to record the timestamp of last ACR |
|  |  |
| ***Source to WG:*** | CSCN |
| ***Source to TSG:*** | SA5 |
|  |  |
| ***Work item code:*** | TEI19 |  | ***Date:*** | 2025-08-25 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-19 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | For ACR[Stop] lost scenario, it is required to record the timestamp of last ACR[Interim] in incomplete CDR to get the valid call duration. |
|  |  |
| ***Summary of change:*** | Change IMS CDR to add the field “lastACRInterimTimeStamp” |
|  |  |
| ***Consequences if not approved:*** | Operators’ revenue loss in ACR[Stop] lost scenario since incomplete CDR can not provide valid call duration. |
|  |  |
| ***Clauses affected:*** | 5.1.3.1.X |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ... |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | Revision of S5-253624 |

|  |
| --- |
| **First change** |

5.1.3.1.X ACR Interim Time Stamp

This field records the event time stamp carried in the latest ACR[Interim] CDF receives. It is Present only in session related charging .

The content of this field corresponds to the *Event-TimeStamp* AVP of the latest ACR[Interim] message.

|  |
| --- |
| **End of change** |