**3GPP TSG RAN WG1 #122bis R1-25nnnnn**

**Prague, Czech Republic, October 13th –17th, 2025**

**Source: Ad-Hoc Chair (AT&T)**

**Title: Session Notes of AI 9.13**

**Agenda Item: 9.13**

**Document for: Endorsement**

### 9.13 UE features for LTE based 5G broadcast Phase 2

**Agreement: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 3. LTE\_terr\_bcast\_Ph2 | 3-1a | Cyclic shift of PMCH – ~~fixed~~ alpha1 | 1. Support of cyclic shift for the bit sequence in Section 6.3.1 of TS 36.211 for the i^th subframe of the time-interleaved TB by X\_i bits | 3-1 | Yes | N/A | UE is not able to support time-interleaving with the cyclic shift and alpha1 | Per band | No | N/A | , with   * + - is the number of bits in the codeblock within a subframe (as defined in TS 36.212) | Optional with capability signalling |

**Agreement: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 3. LTE\_terr\_bcast\_Ph2 | 3-1b | Cyclic shift of PMCH – alpha2 | 1. Support of cyclic shift for the bit sequence in Section 6.3.1 of TS 36.211 for the i^th subframe of the time-interleaved TB by X\_i bits | 3-1 | Yes | N/A | UE is not able to support time-interleaving with the cyclic shift and alpha2 | Per band | No | N/A | , with   * + - denotes the number of OFDM symbols within a subframe     - denotes the number of CBs in the time-interleaved (scaled) TB     - is the number of bits in the codeblock within a subframe (as defined in TS 36.212) | Optional with capability signalling |

**Agreement: Introduce the following Rel. 19 UE FGs (yellow highlighting, if any, shows text that’s not yet agreed)**

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 3. LTE\_terr\_bcast\_Ph2 | 3-1c | Cyclic shift of PMCH - alpha3 | 1. Support of cyclic shift for the bit sequence in Section 6.3.1 of TS 36.211 for the i^th subframe of the time-interleaved TB by X\_i bits | 3-1 | Yes | N/A | UE is not able to support time-interleaving with the cyclic shift and alpha3 | Per band | No | N/A | where   * the pseudo-random sequence is defined by clause 7.2 and shall be initialized with at the beginning of each radio frame for which , * is the number of subcarriers available in one OFDM symbol for PMCH, * is the modulation order, * denotes the subframe to which the transport block is mapped,   - is the number of subframes to which the transport block is mapped | Optional with capability signalling |

**Agreement: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 3. LTE\_terr\_bcast\_Ph2 | 3-1 | Time-interleaving | 1. Support of PMCH transmission pattern, excluding MCCH and MSI, with time interleaving for a set of PMCH numerologies  2. Support of TBS determination for the scaled TB up to a maximum TBS  3. Support of determining the starting point for reading from the circular buffer (k0) for each subframe  4. Support of the extended MSI periodicities | Support of fembmsDedicatedCell | Yes | N/A | UE is not able to support time-interleaving for LTE-based 5G broadcast | Per band | No | N/A | For component 1, the UE indicates a bitmap [b15, b7dot5, b2dot5, b1dot25] where each bit indicates whether the UE supports time-interleaving for the corresponding numerology  For component 2, the maximum TBS a UE supports for the scaled TB is derived based on the UE’s unicast capability  Note: One TB is mapped to N non-consecutive subframes. Two transmissions of the same TB are separated by (M-1) subframes. | Optional with capability signalling |

R1-2506915 Discussion on UE features for LTE based 5G broadcast ZTE Corporation, Sanechips

R1-2506977 UE features for LTE based 5G broadcast Xiaomi

R1-2507241 UE features for LTE broadcast Samsung

R1-2507709 UE features for LTE based 5G broadcast Phase 2 Qualcomm Incorporated

R1-2507742 Summary of UE features for LTE based 5G broadcast Phase 2 Moderator (AT&T)