3GPP TSG-RAN WG3 Meeting #129 R3-25xxxx

Bengaluru, India, 25 – 29 August, 2025

**Title: [Draft] LS on the handling of inter-DU L2 reset for LTM**

**Response to:**

**Release:** Release 18

**Work Item:** NR\_Mob\_enh2-Core

**Source:** Ericsson [to be RAN3]

**To:** RAN2

**CC:**

**Contact Person:**

#### **Name: Liwei Qiu**

**E-mail Address:** liwei.qiu@ericsson.com

**Send any reply LS to: 3GPP Liaisons Coordinator,** [**mailto:3GPPLiaison@etsi.org**](mailto:3GPPLiaison@etsi.org)

**Attachments: None**

**1. Overall Description:**

RAN3 has discussed the handling of L2 reset in the context of inter-DU LTM. The common understanding within RAN3 is that L2 reset is always performed for a UE when the serving DU changes from one DU to another, as part of inter-DU LTM.

RAN3 kindly asks RAN2 to clarify whether any issue is identified with the above understanding.

**2. To RAN2**

**ACTION:** RAN3 kindly requests RAN2 to confirm whether any issue is foreseen with the above common understanding.

**3. Dates of Next TSG-RAN WG3 Meetings:**

TSG-RAN WG3 Meeting #129-bis 13 - 17 October 2025 Prague, CZ

TSG-RAN WG3 Meeting #130 17 - 21 November 2025 Dallas, US