**3GPP TSG-RAN4 Meeting # *R4-25***

**Prague, Czech Republic, 13th – 17th October 2025**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.3* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.101-1** | **CR** | **-** | **rev** | **-** | **Current version:** | **19.3.1** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Draft CR for TS38.101-1 Rel-19 Adding BCS4 and 5 into 4 band NR CA combinations | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Qualcomm, KDDI | | | | | | | | | |
| ***Source to TSG:*** | RAN4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** |  | | | | |  | ***Date:*** | | | 2025-10-03 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-19 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)  Rel-20 (Release 20)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | BCS4 and 5 is added into some 4 band NR CA combinations | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Adding BCS 4 and 5 support into following combinations:  CA\_n3A-n18A-n28A-n41A with UL CA\_n3A-n18A/CA\_n3A-n28A/CA\_n3A-n41A/CA\_n18A-n28A/CA\_n18A-n41A/CA\_n28A-n41A  CA\_n3A-n18A-n28A-n77A with UL CA\_n3A-n18A/CA\_n3A-n28A/CA\_n3A-n77A/CA\_n18A-n28A/CA\_n18A-n77A/CA\_n28A-n77A  CA\_n3A-n18A-n41A-n77A with UL CA\_n3A-n18A/CA\_n3A-n41A/CA\_n3A-n77A/CA\_n18A-n41A/CA\_n18A-n77A/CA\_n41A-n77A  CA\_n3A-n28A-n41A-n77A with UL CA\_n3A-n28A/CA\_n3A-n41A/CA\_n3A-n77A/CA\_n28A-n41A/CA\_n28A-n77A/CA\_n41A-n77A  CA\_n18A-n28A-n41A-n77A with UL CA\_n18A-n28A/CA\_n18A-n41A/CA\_n18A-n77A/CA\_n28A-n41A/CA\_n28A-n77A/CA\_n41A-n77A  CA\_n3A-n28A-n41A-n77(2A) with UL CA\_n3A-n28A/CA\_n3A-n41A/CA\_n3A-n77A/CA\_n28A-n41A/CA\_n28A-n77A/CA\_n41A-n77A/CA\_n77(2A) | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | BCS 4 and 5 are not supported for these combinations | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.5A.3.3 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | | **X** |  | Test specifications | | | | TS/TR ... CR ... 38.521-1 | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

<START OF CHANGE>

#### 5.5A.3.3 Configurations for inter-band CA (four bands)

Table 5.5A.3.3-1: Void

##### Table 5.5A.3.3-1a

Table 5.5A.3.3-1a: NR CA configurations and bandwidth combinations sets defined for inter-band CA (four bands)

| NR CA configuration | Uplink CA configuration  or single uplink carrier 4 | NR Band | Channel bandwidth (MHz) (NOTE 3) | Bandwidth combination set |
| --- | --- | --- | --- | --- |
| CA\_n1A-n3A-n5A-n7A | CA\_n1A-n3A  CA\_n1A-n5A  CA\_n1A-n7A  CA\_n3A-n5A  CA\_n3A-n7A  CA\_n5A-n7A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n1A-n3A-n5A-n7B | CA\_n1A-n3A  CA\_n1A-n5A  CA\_n1A-n7A  CA\_n3A-n5A  CA\_n3A-n7A  CA\_n5A-n7A  CA\_n7B | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
| CA\_n1A-n3A-n5A-n28A | CA\_n1A-n3A  CA\_n1A-n5A  CA\_n1A-n28A  CA\_n3A-n5A  CA\_n3A-n28A  CA\_n5A-n28A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n5A-n78A | CA\_n1A-n3A  CA\_n1A-n5A  CA\_n1A-n78A  CA\_n3A-n5A  CA\_n3A-n78A  CA\_n5A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n7A-n8A | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n8A  CA\_n3A-n7A  CA\_n3A-n8A  CA\_n7A-n8A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
| CA\_n1A-n3(2A)-n7A-n8A | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n8A  CA\_n3A-n7A  CA\_n3A-n8A  CA\_n7A-n8A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
| CA\_n1A-n3A-n7(2A)-n8A | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n8A  CA\_n3A-n7A  CA\_n3A-n8A  CA\_n7A-n8A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n7 | CA\_n7(2A)\_BCS0 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
| CA\_n1A-n3(2A)-n7(2A)-n8A | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n8A  CA\_n3A-n7A  CA\_n3A-n8A  CA\_n7A-n8A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS0 |  |
|  |  | n7 | CA\_n7(2A)\_BCS0 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
| CA\_n1A-n3A-n7A-n20A | n35  n75  CA\_n1A-n3A5  CA\_n1A-n7A5  CA\_n1A-n20A  CA\_n3A-n7A5  CA\_n3A-n20A5  CA\_n7A-n20A5 | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n7A-n26A | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n26A  CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
| CA\_n1A-n3B-n7A-n26A | CA\_n3B  CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n26A  CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
|  | CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 1 |
|  |  | n3 | CA\_n3B\_BCS1 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
| CA\_n1A-n3A-n7B-n26A | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n26A  CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A  CA\_n7B | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
| CA\_n1A-n3B-n7B-n26A | CA\_n7B  CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n26A  CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
|  | CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 1 |
|  |  | n3 | CA\_n3B\_BCS1 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
| CA\_n1A-n3A-n7A-n26(2A) | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n26A  CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A | n1 | 5, 10, 15, 20 | 0 |
|  | CA\_n26(2A) | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
| CA\_n1A-n3B-n7A-n26(2A) | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n26A  CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A | n1 | 5, 10, 15, 20 | 0 |
|  | CA\_n26(2A) | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  | CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 1 |
|  |  | n3 | CA\_n3B\_BCS1 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
| CA\_n1A-n3A-n7B-n26(2A) | CA\_n7B  CA\_n26(2A)  CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n26A  CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
| CA\_n1A-n3B-n7B-n26(2A) | CA\_n7B  CA\_n26(2A)  CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n26A  CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  | CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 1 |
|  |  | n3 | CA\_n3B\_BCS1 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
| CA\_n1A-n3A-n7A-n28A | n35  n75 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  | n35  n75  CA\_n1A-n3A5  CA\_n1A-n7A5  CA\_n1A-n28A  CA\_n3A-n7A5  CA\_n3A-n28A5  CA\_n7A-n28A5 | n1 | 5, 10, 15, 20 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 202 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n7B-n28A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n28A  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n7A-n28A  CA\_n7B | n1 | 5, 10, 15, 20 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
| CA\_n1A-n3B-n7A-n28A | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n28A  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n7A-n28A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  | CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 1 |
|  |  | n3 | CA\_n3B\_BCS1 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
| CA\_n1A-n3B-n7B-n28A | CA\_n7B  CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n28A  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n7A-n28A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  | CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 1 |
|  |  | n3 | CA\_n3B\_BCS1 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
| CA\_n1A-n3A-n7A-n38A7 | - | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1(2A)-n3A-n7A-n38A7 | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1A-n3B-n7A-n38A7 | - | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1(2A)-n3B-n7A-n38A7 | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1A-n3(2A)-n7A-n38A7 | - | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS1 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1(2A)-n3(2A)-n7A-n38A7 | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS1 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1A-n3A-n7A-n40A | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n40A  CA\_n3A-n7A  CA\_n3A-n40A  CA\_n7A-n40A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n7A-n67A | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n3A-n7A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n7A-n75A | - | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n3A-n7A | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n75 | n75 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n7A-n78A | n35  n75  n785,6  CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A5  CA\_n3A-n7A  CA\_n3A-n78A5  CA\_n7A-n78A5 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 2 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3B-n7A-n78A | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 1 |
|  |  | n3 | CA\_n3B\_BCS1 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3B-n7B-n78A | CA\_n7B  CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 1 |
|  |  | n3 | CA\_n3B\_BCS1 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n7A-n78(2A) | n35  n75  n785,6  CA\_n78(2A)5  CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A5  CA\_n3A-n7A  CA\_n3A-n78A5  CA\_n7A-n78A5 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS 4 and 5 |  |
| CA\_n1A-n3A-n7A-n78C | CA\_n78C  CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n1A-n3A-n7B-n78A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A  CA\_n7B | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3B-n7A-n78(2A) | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  | CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 1 |
|  |  | n3 | CA\_n3B\_BCS1 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  | CA\_n78(2A) | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | CA\_n3B\_BCS 4 and 5 |  |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS 4 and 5 |  |
| CA\_n1A-n3B-n7A-n78C | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A  CA\_n78C | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
|  | CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 1 |
|  |  | n3 | CA\_n3B\_BCS1 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n1A-n3A-n7B-n78(2A) | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A  CA\_n7B | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  | CA\_n7B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A CA\_n78(2A) | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n7 | CA\_n7B\_BCS 4 and 5 |  |
|  |  | n78 | CA\_n78(2A)\_BCS 4 and 5 |  |
| CA\_n1A-n3A-n7B-n78C | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A  CA\_n7B  CA\_n78C | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
|  | CA\_n7B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
|  | CA\_n3A-n7A  CA\_n78C  CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n78A  CA\_n7A-n78A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n7 | CA\_n7B\_BCS 4 and 5 |  |
|  |  | n78 | CA\_n78C\_BCS 4 and 5 |  |
| CA\_n1A-n3B-n7B-n78(2A) | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A  CA\_n7B | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  | CA\_n3B  CA\_n7B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 1 |
|  |  | n3 | CA\_n3B\_BCS1 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A  CA\_n78(2A) | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | CA\_n3B\_BCS 4 and 5 |  |
|  |  | n7 | CA\_n7B\_BCS 4 and 5 |  |
|  |  | n78 | CA\_n78(2A)\_BCS 4 and 5 |  |
| CA\_n1A-n3B-n7B-n78C | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A  CA\_n7B  CA\_n78C | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
|  | CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 1 |
|  |  | n3 | CA\_n3B\_BCS1 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n1A-n3(2A)-n7A-n78A | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n7(2A)-n78A | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n7 | CA\_n7(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3(2A)-n7(2A)-n78A | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS0 |  |
|  |  | n7 | CA\_n7(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n7A-n79A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n3A-n7A-n79C | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1(2A)-n3A-n7A-n79A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1(2A)-n3A-n7A-n79C | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1A-n3B-n7A-n79A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n3B-n7A-n79C | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1(2A)-n3B-n7A-n79A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1(2A)-n3B-n7A-n79C | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1A-n3(2A)-n7A-n79A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n3(2A)-n7A-n79C | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1(2A)-n3(2A)-n7A-n79A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1(2A)-n3(2A)-n7A-n79C | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1A-n3A-n7A-n105A | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n105A  CA\_n3A-n7A  CA\_n3A-n105A  CA\_n7A-n105A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n105 | 5, 10,15, 20, 25, 30, 35 |  |
| CA\_n1A-n3A-n8A-n40A | CA\_n1A-n3A  CA\_n1A-n8A  CA\_n1A-n40A  CA\_n3A-n8A  CA\_n3A-n40A  CA\_n8A-n40A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n8 | n8 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n8A-n41A | CA\_n1A-n3A  CA\_n1A-n8A  CA\_n1A-n41A  CA\_n3A-n8A  CA\_n3A-n41A  CA\_n8A-n41A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n8 | n8 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n8A-n77A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n3A-n8A-n77(2A) | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n1A-n3A-n8A-n78A | CA\_n1A-n3A  CA\_n1A-n8A  CA\_n1A-n78A  CA\_n3A-n8A  CA\_n3A-n78A  CA\_n8A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 901, 100 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n8 | n8 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3(2A)-n8A-n78A | CA\_n1A-n3A  CA\_n1A-n8A  CA\_n1A-n78A  CA\_n3A-n8A  CA\_n3A-n78A  CA\_n8A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS0 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n8A-n78C | CA\_n1A-n3A  CA\_n1A-n8A  CA\_n1A-n78A  CA\_n1A-n78C  CA\_n3A-n8A  CA\_n3A-n78A  CA\_n3A-n78C  CA\_n8A-n78A  CA\_n8A-n78C | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n1A-n3(2A)-n8A-n78C | CA\_n1A-n3A  CA\_n1A-n8A  CA\_n1A-n78A  CA\_n1A-n78C  CA\_n3A-n8A  CA\_n3A-n78A  CA\_n3A-n78C  CA\_n8A-n78A  CA\_n8A-n78C | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS0 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n1A-n3A-n18A-n28A | CA\_n1A-n3A  CA\_n1A-n18A  CA\_n1A-n28A  CA\_n3A-n18A  CA\_n3A-n28A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20 |  |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n28 | 5, 10 |  |
| CA\_n1A-n3A-n18A-n41A | n415  CA\_n1A-n3A  CA\_n1A-n18A  CA\_n1A-n41A5  CA\_n3A-n18A  CA\_n3A-n41A5  CA\_n18A-n41A5 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20 |  |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n3A-n18A-n77A | n775  CA\_n1A-n3A  CA\_n1A-n18A  CA\_n1A-n77A5  CA\_n3A-n18A  CA\_n3A-n77A5  CA\_n18A-n77A5 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20 |  |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n18A-n77(2A) | n775  CA\_n1A-n3A  CA\_n1A-n18A  CA\_n1A-n77A5  CA\_n3A-n18A  CA\_n3A-n77A5  CA\_n18A-n77A5 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20 |  |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
| CA\_n1A-n3A-n20A-n41A | CA\_n1A-n3A  CA\_n1A-n20A  CA\_n1A-n41A  CA\_n3A-n20A  CA\_n3A-n41A  CA\_n20A-n41A | n1 | 5, 10,15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10,15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n20 | 5, 10,15, 20 |  |
|  |  | n41 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n20A-n67A | CA\_n1A-n3A  CA\_n1A-n20A  CA\_n3A-n20A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n20A-n71A | CA\_n1A-n3A  CA\_n1A-n20A  CA\_n1A-n71A  CA\_n3A-n20A  CA\_n3A-n71A  CA\_n20A-n71A | n1 | 5, 10,15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10,15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n20 | 5, 10,15, 20 |  |
|  |  | n71 | 5, 10,15, 20, 25, 30, 35 |  |
| CA\_n1A-n3A-n20A-n77A | CA\_n1A-n3A  CA\_n1A-n20A  CA\_n1A-n77A  CA\_n3A-n20A  CA\_n3A-n77A  CA\_n20A-n77A | n1 | 5, 10,15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10,15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n20 | 5, 10,15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n20A-n77(2A) | CA\_n1A-n3A  CA\_n1A-n20A  CA\_n1A-n77A  CA\_n3A-n20A  CA\_n3A-n77A  CA\_n20A-n77A | n1 | 5, 10,15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10,15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n20 | 5, 10,15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n1A-n3A-n20A-n78A | CA\_n1A-n3A  CA\_n1A-n20A  CA\_n1A-n78A  CA\_n3A-n20A  CA\_n3A-n78A  CA\_n20A-n78A | n1 | 5, 10,15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10,15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n20 | 5, 10,15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n1A-n3A  CA\_n1A-n20A  CA\_n1A-n78A  CA\_n3A-n20A  CA\_n3A-n78A  CA\_n20A-n78A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n20A-n78(2A) | CA\_n1A-n3A  CA\_n1A-n20A  CA\_n1A-n78A  CA\_n3A-n20A  CA\_n3A-n78A  CA\_n20A-n78A  CA\_n78(2A) | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS 4 and 5 |  |
| CA\_n1A-n3A-n26A-n78A | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n26(2A)-n78A | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  | CA\_n26(2A) | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n26A-n78(2A) | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  | CA\_n78(2A) | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n26 | n26 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n1A-n3A-n26A-n78C | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A  CA\_n78C | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n1A-n3A-n26(2A)-n78(2A) | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  | CA\_n26(2A)  CA\_n78(2A) | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n1A-n3A-n26(2A)-n78C | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A  CA\_n26(2A)  CA\_n78C | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n1A-n3B-n26A-n78A | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 1 |
|  |  | n3 | CA\_n3B\_BCS1 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3B-n26(2A)-n78A | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  | CA\_n26(2A) | n3 | CA\_n3B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 1 |
|  |  | n3 | CA\_n3B\_BCS1 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3B-n26A-n78(2A) | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  | CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 1 |
|  |  | n3 | CA\_n3B\_BCS1 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  | CA\_n78(2A) | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | CA\_n3B\_BCS 4 and 5 |  |
|  |  | n26 | n26 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS 4 and 5 |  |
| CA\_n1A-n3B-n26A-n78C | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A  CA\_n78C | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
|  | CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 1 |
|  |  | n3 | CA\_n3B\_BCS1 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n1A-n3B-n26(2A)-n78(2A) | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  | CA\_n26(2A)  CA\_n78(2A) | n3 | CA\_n3B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  | CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 1 |
|  |  | n3 | CA\_n3B\_BCS1 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n3B-n26(2A)-n78C | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A  CA\_n26(2A)  CA\_n78C | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
|  | CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 1 |
|  |  | n3 | CA\_n3B\_BCS1 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n1A-n3A-n28A-n38A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1A-n3A-n28A-n40A | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n40A  CA\_n3A-n28A  CA\_n3A-n40A  CA\_n28A-n40A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n28A-n41A | n415,6  CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n41A5  CA\_n3A-n28A  CA\_n3A-n41A5  CA\_n28A-n41A5 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20 |  |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  | n415,6  CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n41A5  CA\_n3A-n28A  CA\_n3A-n41A5  CA\_n28A-n41A5 | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n28A-n77A | n775,6  CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n77A5  CA\_n3A-n28A  CA\_n3A-n77A5  CA\_n28A-n77A5 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  | n775  CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n77A  CA\_n3A-n28A  CA\_n3A-n77A  CA\_n28A-n77A | n1 | 5, 10, 15, 20 | 1 |
|  |  | n3 | 5, 10, 15, 20 |  |
|  |  | n28 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n77A  CA\_n3A-n28A  CA\_n3A-n77A  CA\_n28A-n77A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n28A-n77(2A) | n775,6  CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n77A5  CA\_n3A-n28A  CA\_n3A-n77A5  CA\_n28A-n77A5  CA\_n77(2A)5 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n77A  CA\_n3A-n28A  CA\_n3A-n77A  CA\_n28A-n77A  CA\_n77(2A) | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
| CA\_n1A-n3A-n28A-n77(3A) | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n77A  CA\_n3A-n28A  CA\_n3A-n77A  CA\_n28A-n77A  CA\_n77(2A) | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
| CA\_n1A-n3A-n28A-n78A | n35  n785,6 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n28 | 5, 10, 15, 202 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 901, 100 |  |
|  | n35  n785,6  CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n78A5  CA\_n3A-n28A  CA\_n3A-n78A5  CA\_n28A-n78A5 | n1 | 5, 10, 15, 20 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n28 | 5, 10, 15, 202 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 2 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 202,302 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n28A-n78(2A) | n35  n785,6  CA\_n78(2A) 5  CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n78A5  CA\_n3A-n28A  CA\_n3A-n78A5  CA\_n28A-n78A5 | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 202, 302 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS 4 and 5 |  |
| CA\_n1A-n3A-n28A-n78C | CA\_n78C  CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n28A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 202, 302 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n1A-n3B-n28A-n78A | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n28A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 1 |
|  |  | n3 | CA\_n3B\_BCS1 |  |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3B-n28A-n78(2A) | CA\_n78(2A)  CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n28A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  | CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 1 |
|  |  | n3 | CA\_n3B\_BCS1 |  |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n3B-n28A-n78C | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n28A-n78A  CA\_n78C | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
|  | CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 1 |
|  |  | n3 | CA\_n3B\_BCS1 |  |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n1A-n3A-n28A-n79A | n795,6  CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n79A5  CA\_n3A-n28A  CA\_n3A-n79A5  CA\_n28A-n79A5 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25,30 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n79A  CA\_n3A-n28A  CA\_n3A-n79A  CA\_n28A-n79A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n38A-n78A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n40A-n41A | CA\_n1A-n3A  CA\_n1A-n40A  CA\_n1A-n41A  CA\_n3A-n40A  CA\_n3A-n41A  CA\_n40A-n41A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n40A-n77A | CA\_n1A-n3A  CA\_n1A-n40A  CA\_n1A-n77A  CA\_n3A-n40A  CA\_n3A-n77A  CA\_n40A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20 |  |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n40A-n77(2A) | CA\_n1A-n3A  CA\_n1A-n40A  CA\_n1A-n77A  CA\_n3A-n40A  CA\_n3A-n77A  CA\_n40A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
| CA\_n1A-n3A-n40A-n78A | CA\_n1A-n3A  CA\_n1A-n40A  CA\_n1A-n78A  CA\_n3A-n40A  CA\_n3A-n78A  CA\_n40A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n40A-n79A | CA\_n1A-n3A  CA\_n1A-n79A  CA\_n1A-n40A  CA\_n3A-n79A  CA\_n3A-n40A  CA\_n40A-n79A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  |  |  |  |
| CA\_n1A-n3A-n40A-n105A | CA\_n1A-n3A  CA\_n1A-n40A  CA\_n1A-n105A  CA\_n3A-n40A  CA\_n3A-n105A  CA\_n40A-n105A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20 |  |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n1A-n3A-n41A-n71A | CA\_n1A-n3A  CA\_n1A-n41A  CA\_n1A-n71A  CA\_n3A-n41A  CA\_n3A-n71A  CA\_n41A-n71A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n1A-n3A-n41A-n77A | n415,6  n775,6  CA\_n1A-n3A  CA\_n1A-n41A5  CA\_n1A-n77A5  CA\_n3A-n41A5  CA\_n3A-n77A5  CA\_n41A-n77A5 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n41A-n77(2A) | n415,6  n775,6  CA\_n1A-n3A  CA\_n1A-n41A5  CA\_n1A-n77A5  CA\_n3A-n41A5  CA\_n3A-n77A5  CA\_n41A-n77A5 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
| CA\_n1A-n3A-n41A-n78A | CA\_n1A-n3A  CA\_n1A-n41A  CA\_n1A-n78A  CA\_n3A-n41A  CA\_n3A-n78A  CA\_n41A-n78A | n1 | 5, 10,15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10,15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n41 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50, 60, 70, 80, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n41A-n78C | CA\_n1A-n3A  CA\_n1A-n41A  CA\_n1A-n78A  CA\_n1A-n78C  CA\_n3A-n41A  CA\_n3A-n78A  CA\_n3A-n78C  CA\_n41A-n78A  CA\_n41A-n78C | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n1A-n3(2A)-n41A-n78A | CA\_n1A-n3A  CA\_n1A-n41A  CA\_n1A-n78A  CA\_n3A-n41A  CA\_n3A-n78A  CA\_n41A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS0 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3(2A)-n41A-n78C | CA\_n1A-n3A  CA\_n1A-n41A  CA\_n1A-n78A  CA\_n1A-n78C  CA\_n3A-n41A  CA\_n3A-n78A  CA\_n3A-n78C  CA\_n41A-n78A  CA\_n41A-n78C | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS0 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n1A-n3A-n41A-n79A | CA\_n1A-n3A  CA\_n1A-n41A  CA\_n1A-n79A  CA\_n3A-n41A  CA\_n3A-n79A  CA\_n41A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n3A-n67A-n78A | CA\_n1A-n3A  CA\_n1A-n78A  CA\_n3A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n67A-n78(2A) | CA\_n1A-n3A  CA\_n1A-n78A  CA\_n3A-n78A  CA\_n78(2A) | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n1A-n3A-n71A-n77A | CA\_n1A-n3A  CA\_n1A-n71A  CA\_n1A-n77A  CA\_n3A-n71A  CA\_n3A-n77A  CA\_n71A-n77A | n1 | 5, 10,15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10,15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n71 | 5, 10,15, 20, 25, 30, 35 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n71A-n77(2A) | CA\_n1A-n3A  CA\_n1A-n71A  CA\_n1A-n77A  CA\_n3A-n71A  CA\_n3A-n77A  CA\_n71A-n77A | n1 | 5, 10,15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10,15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n71 | 5, 10,15, 20, 25, 30, 35 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n1A-n3A-n71A-n78A | CA\_n1A-n3A  CA\_n1A-n71A  CA\_n1A-n78A  CA\_n3A-n71A  CA\_n3A-n78A  CA\_n71A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n71A-n78C | CA\_n1A-n3A  CA\_n1A-n71A  CA\_n1A-n78A  CA\_n1A-n78C  CA\_n3A-n71A  CA\_n3A-n78A  CA\_n3A-n78C  CA\_n71A-n78A  CA\_n71A-n78C | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n1A-n3(2A)-n71A-n78A | CA\_n1A-n3A  CA\_n1A-n71A  CA\_n1A-n78A  CA\_n3A-n71A  CA\_n3A-n78A  CA\_n71A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS0 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3(2A)-n71A-n78C | CA\_n1A-n3A  CA\_n1A-n71A  CA\_n1A-n78A  CA\_n3A-n71A  CA\_n3A-n78A  CA\_n71A-n78A  CA\_n71A-n78C | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS0 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n1A-n3A-n75A-n78A | CA\_n1A-n3A  CA\_n1A-n78A  CA\_n3A-n78A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n75 | n75 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n77A-n79A | n775,6  n795,6  CA\_n1A-n3A  CA\_n1A-n77A5  CA\_n1A-n79A5  CA\_n3A-n77A5  CA\_n3A-n79A5  CA\_n77A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25,30 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  | CA\_n1A-n3A  CA\_n1A-n77A  CA\_n1A-n79A  CA\_n3A-n77A  CA\_n3A-n79A  CA\_n77A-n79A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n77(2A)-n79A | CA\_n1A-n3A  CA\_n1A-n77A  CA\_n1A-n79A  CA\_n3A-n77A  CA\_n3A-n79A  CA\_n77A-n79A  CA\_n77(2A) | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25,30 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n77(3A)-n79A | CA\_n1A-n3A  CA\_n1A-n77A  CA\_n1A-n79A  CA\_n3A-n77A  CA\_n3A-n79A  CA\_n77A-n79A  CA\_n77(2A) | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25,30 |  |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n3A-n78A-n105A | CA\_n1A-n3A  CA\_n1A-n78A  CA\_n1A-n105A  CA\_n3A-n78A  CA\_n3A-n105A  CA\_n78A-n105A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25,30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25,30, 35 |  |
| CA\_n1A-n5A-n7A-n40A | CA\_n1A-n5A CA\_n1A-n7A CA\_n1A-n40A CA\_n5A-n7A CA\_n5A-n40A CA\_n7A-n40A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n5A-n7A-n78A | CA\_n1A-n5A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n5A-n7A  CA\_n5A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n5A-n7B-n78A | CA\_n1A-n5A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n5A-n7A  CA\_n5A-n78A  CA\_n7A-n78A  CA\_n7B | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n5A-n7A-n105A | CA\_n1A-n5A CA\_n1A-n7A CA\_n1A-n105A CA\_n5A-n7A CA\_n5A-n105A CA\_n7A-n105A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n1A-n5A-n28A-n78A | CA\_n1A-n5A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n5A-n28A  CA\_n5A-n78A  CA\_n28A-n78A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n5A-n28A-n79A | CA\_n1A-n5A  CA\_n1A-n28A  CA\_n1A-n79A  CA\_n5A-n28A  CA\_n5A-n79A  CA\_n28A-n79A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n5A-n40A-n78A | CA\_n1A-n5A  CA\_n1A-n40A  CA\_n1A-n78A  CA\_n5A-n40A  CA\_n5A-n78A  CA\_n40A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n5A-n40A-n105A | CA\_n1A-n5A CA\_n1A-n40A CA\_n1A-n105A CA\_n5A-n40A CA\_n5A-n105A CA\_n40A-n105A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n1A-n5A-n78A-n79A | CA\_n1A-n5A  CA\_n1A-n78A  CA\_n1A-n79A  CA\_n5A-n78A  CA\_n5A-n79A  CA\_n78A-n79A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n5A-n78A-n105A | CA\_n1A-n5A CA\_n1A-n78A CA\_n1A-n105A CA\_n5A-n78A CA\_n5A-n105A CA\_n78A-n105A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40 , 50 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n1A-n7A-n8A-n40A | CA\_n1A-n7A  CA\_n1A-n8A  CA\_n1A-n40A  CA\_n7A-n8A  CA\_n7A-n40A  CA\_n8A-n40A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n8 | n8 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n7A-n8A-n78A | CA\_n1A-n7A  CA\_n1A-n8A  CA\_n1A-n78A  CA\_n7A-n8A  CA\_n7A-n78A  CA\_n8A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n7(2A)-n8A-n78A | CA\_n1A-n7A  CA\_n1A-n8A  CA\_n1A-n78A  CA\_n7A-n8A  CA\_n7A-n78A  CA\_n8A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | CA\_n7(2A)\_BCS0 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n7A-n20A-n67A | CA\_n1A-n7A  CA\_n1A-n20A  CA\_n7A-n20A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n7A-n20A-n78A | CA\_n1A-n7A  CA\_n1A-n20A  CA\_n1A-n78A  CA\_n7A-n20A  CA\_n7A-n78A  CA\_n20A-n78A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n7A-n20A-n78(2A) | CA\_n1A-n7A  CA\_n1A-n20A  CA\_n1A-n78A  CA\_n7A-n20A  CA\_n7A-n78A  CA\_n20A-n78A  CA\_n78(2A) | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS 4 and 5 |  |
| CA\_n1A-n7A-n26A-n78A | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n7B-n26A-n78A | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n7A-n26(2A)-n78A | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  | CA\_n26(2A) | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n7A-n26A-n78(2A) | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  | CA\_n78(2A) | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n26 | n26 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS 4 and 5 |  |
| CA\_n1A-n7A-n26A-n78C | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n78C | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n1A-n7A-n26(2A)-n78(2A) | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  | CA\_n26(2A)  CA\_n78(2A) | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n1A-n7A-n26(2A)-n78C | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n26(2A)  CA\_n78C | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n1A-n7B-n26(2A)-n78A | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B | n1 | 5, 10, 15, 20 | 0 |
|  | CA\_n26(2A) | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n7B-n26A-n78(2A) | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  | CA\_n78(2A) | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | CA\_n7B\_BCS 4 and 5 |  |
|  |  | n26 | n26 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS 4 and 5 |  |
| CA\_n1A-n7B-n26A-n78C | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B  CA\_n78C | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n1A-n7B-n26(2A)-n78(2A) | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B | n1 | 5, 10, 15, 20 | 0 |
|  | CA\_n26(2A) | n7 | CA\_n7B\_BCS0 |  |
|  | CA\_n78(2A) | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n1A-n7B-n26(2A)-n78C | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B  CA\_n26(2A)  CA\_n78C | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n1A-n7A-n28A-n38A7 | - | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1A-n7A-n28A-n78A | n75  n785,6  CA\_n1A-n7A  CA\_n1A-n28A  CA\_n1A-n78A5  CA\_n7A-n28A  CA\_n7A-n78A5  CA\_n28A-n78A5 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n7B-n28A-n78A | CA\_n1A-n7A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n7B  CA\_n28A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n7B-n28A-n78(2A) | CA\_n7B  CA\_n78(2A)  CA\_n1A-n7A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n7B-n28A-n78C | CA\_n7B  CA\_n78C  CA\_n1A-n7A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n1A-n7A-n28A-n78(2A) | n75  n785,6  CA\_n78(2A) 5  CA\_n1A-n7A  CA\_n1A-n28A  CA\_n1A-n78A5  CA\_n7A-n28A  CA\_n7A-n78A5  CA\_n28A-n78A5 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 202 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS 4 and 5 |  |
| CA\_n1A-n7A-n28A-n78C | CA\_n78C  CA\_n1A-n7A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 202 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n1A-n7A-n38A-n78A7 | - | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n7A-n40A-n78A | CA\_n1A-n7A  CA\_n1A-n40A  CA\_n1A-n78A  CA\_n7A-n40A  CA\_n7A-n78A  CA\_n40A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n7A-n40A-n79A | CA\_n1A-n7A  CA\_n1A-n79A  CA\_n1A-n40A  CA\_n7A-n79A  CA\_n7A-n40A  CA\_n40A-n79A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n7A-n40A-n105A | CA\_n1A-n7A  CA\_n1A-n40A  CA\_n1A-n105A  CA\_n7A-n40A  CA\_n7A-n105A  CA\_n40A-n105A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n1A-n7A-n67A-n78A | CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n7A-n67A-n78(2A) | CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n78A  CA\_n78(2A) | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n1A-n7A-n75A-n78A | CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n78A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n75 | n75 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n7A-n78A-n105A | CA\_n1A-n7A  CA\_n1A-n78A  CA\_n1A-n105A  CA\_n7A-n78A  CA\_n7A-n105A  CA\_n78A-n105A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n1A-n8A-n28A-n40A | CA\_n1A-n8A  CA\_n1A-n28A  CA\_n1A-n40A  CA\_n8A-n28A  CA\_n8A-n40A  CA\_n28A-n40A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n8 | n8 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n8A-n40A-n78A | CA\_n1A-n8A  CA\_n1A-n40A  CA\_n1A-n78A  CA\_n8A-n40A  CA\_n8A-n78A  CA\_n40A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n8 | n8 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n8A-n40A-n79A | CA\_n1A-n8A  CA\_n1A-n40A  CA\_n1A-n79A  CA\_n8A-n40A  CA\_n8A-n79A  CA\_n40A-n79A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n8 | n8 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n8A-n41A-n78A | CA\_n1A-n8A  CA\_n1A-n41A  CA\_n1A-n78A  CA\_n8A-n41A  CA\_n8A-n78A  CA\_n41A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n8A-n41A-n78C | CA\_n1A-n8A  CA\_n1A-n41A  CA\_n1A-n78A  CA\_n1A-n78C  CA\_n8A-n41A  CA\_n8A-n78A  CA\_n8A-n78C  CA\_n41A-n78A  CA\_n41A-n78C | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n1A-n8A-n78A-n79A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n8A-n78(2A)-n79A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS1 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n18A-n28A-n41A | n415  CA\_n1A-n18A  CA\_n1A-n28A  CA\_n1A-n41A5  CA\_n18A-n28A  CA\_n18A-n41A5  CA\_n28A-n41A5 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n18A-n28A-n77A | n775  CA\_n1A-n18A  CA\_n1A-n28A  CA\_n1A-n77A5  CA\_n18A-n28A  CA\_n18A-n77A5  CA\_n28A-n77A5 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n28 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n18A-n41A-n77A | n415  n775  CA\_n1A-n18A  CA\_n1A-n41A5  CA\_n1A-n77A5  CA\_n18A-n41A5  CA\_n18A-n77A5  CA\_n41A-n77A5 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n20A-n41A-n71A | CA\_n1A-n20A  CA\_n1A-n41A  CA\_n1A-n71A  CA\_n20A-n41A  CA\_n20A-n71A  CA\_n41A-n71A | n1 | 5, 10,15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n20 | 5, 10,15, 20 |  |
|  |  | n41 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50, 60, 70, 80, 90, 100 |  |
|  |  | n71 | 5, 10,15, 20, 25, 30, 35 |  |
| CA\_n1A-n20A-n41A-n77A | CA\_n1A-n20A  CA\_n1A-n41A  CA\_n1A-n77A  CA\_n20A-n41A  CA\_n20A-n77A  CA\_n41A-n77A | n1 | 5, 10,15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n20 | 5, 10,15, 20 |  |
|  |  | n41 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n20A-n41A-n77(2A) | CA\_n1A-n20A  CA\_n1A-n41A  CA\_n1A-n77A  CA\_n20A-n41A  CA\_n20A-n77A  CA\_n41A-n77A | n1 | 5, 10,15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n20 | 5, 10,15, 20 |  |
|  |  | n41 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n1A-n20A-n41A-n78A | CA\_n1A-n20A  CA\_n1A-n41A  CA\_n1A-n78A  CA\_n20A-n41A  CA\_n20A-n78A  CA\_n41A-n78A | n1 | 5, 10,15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n20 | 5, 10,15, 20 |  |
|  |  | n41 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50, 60, 70, 80, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n20A-n67A-n78A | CA\_n1A-n20A  CA\_n1A-n78A  CA\_n20A-n78A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n20A-n67A-n78(2A) | CA\_n1A-n20A  CA\_n1A-n78A  CA\_n20A-n78A  CA\_n78(2A) | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n1A-n20A-n71A-n78A | CA\_n1A-n20A  CA\_n1A-n71A  CA\_n1A-n78A  CA\_n20A-n71A  CA\_n20A-n78A  CA\_n71A-n78A | n1 | 5, 10,15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n20 | 5, 10,15, 20 |  |
|  |  | n71 | 5, 10,15, 20, 25, 30, 35 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n28A-n38A-n78A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n28A-n40A-n41A | CA\_n1A-n28A  CA\_n1A-n40A  CA\_n1A-n41A  CA\_n28A-n40A  CA\_n28A-n41A  CA\_n40A-n41A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n28A-n40A-n77A | CA\_n1A-n28A  CA\_n1A-n40A  CA\_n1A-n77A  CA\_n28A-n40A  CA\_n28A-n77A  CA\_n40A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n28A-n40A-n77(2A) | CA\_n1A-n28A  CA\_n1A-n40A  CA\_n1A-n77A  CA\_n28A-n40A  CA\_n28A-n77A  CA\_n40A-n77A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n1A-n28A-n40A-n78A | CA\_n1A-n28A  CA\_n1A-n40A  CA\_n1A-n78A  CA\_n28A-n40A  CA\_n28A-n78A  CA\_n40A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n28A-n40B-n78A | CA\_n1A-n28A  CA\_n1A-n40A  CA\_n1A-n78A  CA\_n28A-n40A  CA\_n28A-n78A  CA\_n40A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n40 | CA\_n40B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n28A-n40A-n79A | CA\_n1A-n28A  CA\_n1A-n40A  CA\_n1A-n79A  CA\_n28A-n40A  CA\_n28A-n79A  CA\_n40A-n79A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n28A-n41A-n77A | n41**5,6**  n775,6  CA\_n1A-n28A  CA\_n1A-n41A5  CA\_n1A-n77A5  CA\_n28A-n41A5  CA\_n28A-n77A5  CA\_n41A-n77A5 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n28A-n41A-n77(2A) | n415,6  n775,6  CA\_n1A-n28A  CA\_n1A-n41A5  CA\_n1A-n77A5  CA\_n28A-n41A5  CA\_n28A-n77A5  CA\_n41A-n77A5 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
| CA\_n1A-n28A-n41A-n79A | CA\_n1A-n28A  CA\_n1A-n41A  CA\_n1A-n79A  CA\_n28A-n41A  CA\_n28A-n79A  CA\_n41A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n28A-n75A-n78A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n75 | 5, 10, 15, 20, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n28A-n77A-n79A | n775,6  n795,6  CA\_n1A-n28A  CA\_n1A-n77A5  CA\_n1A-n79A5  CA\_n28A-n77A5  CA\_n28A-n79A5  CA\_n77A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  | CA\_n1A-n28A  CA\_n1A-n77A  CA\_n1A-n79A  CA\_n28A-n77A  CA\_n28A-n79A  CA\_n77A-n79A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n28A-n78A-n79A | n785,6  n795,6  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n1A-n79A  CA\_n28A-n78A  CA\_n28A-n79A  CA\_n78A-n79A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n28A-n77(2A)-n79A | CA\_n1A-n28A  CA\_n1A-n77A  CA\_n1A-n79A  CA\_n28A-n77A  CA\_n28A-n79A  CA\_n77A-n79A  CA\_n77(2A) | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n28A-n77(3A)-n79A | CA\_n1A-n28A  CA\_n1A-n77A  CA\_n1A-n79A  CA\_n28A-n77A  CA\_n28A-n79A  CA\_n77A-n79A  CA\_n77(2A) | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n40A-n78A-n79A | CA\_n1A-n40A  CA\_n1A-n78A  CA\_n1A-n79A  CA\_n40A-n78A  CA\_n40A-n79A  CA\_n78A-n79A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n40A-n78A-n105A | CA\_n1A-n40A  CA\_n1A-n78A  CA\_n1A-n105A  CA\_n40A-n78A  CA\_n40A-n105A  CA\_n78A-n105A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n1A-n41A-n71A-n77A | CA\_n1A-n41A  CA\_n1A-n71A  CA\_n1A-n77A  CA\_n41A-n71A  CA\_n41A-n77A  CA\_n71A-n77A | n1 | 5, 10,15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n41 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50, 60, 70, 80, 90, 100 |  |
|  |  | n71 | 5, 10,15, 20, 25, 30, 35 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n41A-n71A-n77(2A) | CA\_n1A-n41A  CA\_n1A-n71A  CA\_n1A-n77A  CA\_n41A-n71A  CA\_n41A-n77A  CA\_n71A-n77A | n1 | 5, 10,15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n41 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50, 60, 70, 80, 90, 100 |  |
|  |  | n71 | 5, 10,15, 20, 25, 30, 35 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n1A-n41A-n71A-n78A | CA\_n1A-n41A  CA\_n1A-n71A  CA\_n1A-n78A  CA\_n41A-n71A  CA\_n41A-n78A  CA\_n71A-n78A | n1 | 5, 10, 15, 20, 30, 40, 50 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n41A-n71A-n78C | CA\_n1A-n41A  CA\_n1A-n71A  CA\_n1A-n78A  CA\_n1A-n78C  CA\_n41A-n71A  CA\_n41A-n78A  CA\_n41A-n78C  CA\_n71A-n78A  CA\_n71A-n78C | n1 | 5, 10, 15, 20, 30, 40, 50 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n1A-n41A-n77A-n79A | CA\_n1A-n41A  CA\_n1A-n77A  CA\_n1A-n79A  CA\_n41A-n77A  CA\_n41A-n79A  CA\_n77A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n41A-n77(2A)-n79A | CA\_n1A-n41A  CA\_n1A-n77A  CA\_n1A-n79A  CA\_n41A-n77A  CA\_n41A-n79A  CA\_n77A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n2A-n5A-n30A-n66A | CA\_n2A-n5A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n5A-n30A  CA\_n5A-n66A  CA\_n30A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 10, 15, 20, 25, 30, 40 |  |
| CA\_n2(2A)-n5A-n30A-n66A | CA\_n2A-n5A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n5A-n30A  CA\_n5A-n66A  CA\_n30A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  | n5 | 5, 10, 15, 20 |
|  | n30 | 5, 10 |
|  | n66 | 10, 15, 20, 25, 30, 40 |
| CA\_n2A-n5A-n30A-n66(2A) | CA\_n2A-n5A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n5A-n30A  CA\_n5A-n66A  CA\_n30A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  | n5 | 5, 10, 15, 20 |
|  | n30 | 5, 10 |
|  | n66 | CA\_n66(2A)\_BCS1 |
| CA\_n2A-n5A-n30A-n77A | n775,6  CA\_n2A-n5A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n5A-n30A  CA\_n5A-n77A5  CA\_n30A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n30 | n30 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n5A-n30A-n77A | n775,6  CA\_n2A-n5A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n5A-n30A  CA\_n5A-n77A5  CA\_n30A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n5A-n30A-n77(2A) | n775,6  CA\_n2A-n5A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n5A-n30A  CA\_n5A-n77A5  CA\_n30A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n5A-n30A-n77(2A) | n775,6  CA\_n2A-n5A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n5A-n30A  CA\_n5A-n77A5  CA\_n30A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n30 | n30 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n2A-n5A-n48A-n66A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 508, 608, 708, 808, 908, 1008 |  |
|  |  | n66 | 10, 15, 20, 25, 30, 40 |  |
|  | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 508, 608, 708, 808, 908, 1008 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n5A-n48A-n66A | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n2 | CA\_n2(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n5A-n48A-n66(2A) | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
| CA\_n2(2A)-n5A-n48A-n66(2A) | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n2 | CA\_n2(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
| CA\_n2A-n5A-n48(2A)-n66(2A) | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n48 | CA\_n48(2A)\_BCS 4 and 5 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
| CA\_n2A-n5A-n48B-n66(2A) | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n48B  CA\_n5A-n48A  CA\_n5A-n48B  CA\_n5A-n66A  CA\_n48A-n66A  CA\_n48B-n66A  CA\_n48B | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n48 | CA\_n48B\_BCS 4 and 5 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
| CA\_n2A-n5A-n48B-n66A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n66 | 10, 15, 20, 25, 30, 40 |  |
|  | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 2 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 3 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  | CA\_n48B  CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n48B  CA\_n2A-n66A  CA\_n5A-n48A  CA\_n5A-n48B  CA\_n5A-n66A  CA\_n48A-n66A | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  | CA\_n48B-n66A | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n48 | CA\_n48B\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n5B-n48B-n66A | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n48B  CA\_n2A-n66A  CA\_n5A-n48A  CA\_n5A-n48B  CA\_n5A-n66A  CA\_n48A-n66A  CA\_n48B-n66A  CA\_n48B | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  | CA\_n5B | n5 | CA\_n5B\_BCS 4 and 5 |  |
|  |  | n48 | CA\_n48B\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n5A-n48(2A)-n66A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n66 | 10, 15, 20, 25, 30, 40 |  |
|  | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 2 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n48 | CA\_n48(2A)\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n5B-n48A-n66A | CA\_n5B  CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n48A  CA\_n5A-n66A  CA\_n5A-n48A  CA\_n48A-n66A | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | CA\_n5B\_BCS 4 and 5 |  |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n5B-n48A-n66A | CA\_n5B  CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n2 | CA\_n2(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n5 | CA\_n5B\_BCS 4 and 5 |  |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n5B-n48(2A)-n66A | CA\_n5B  CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | CA\_n5B\_BCS 4 and 5 |  |
|  |  | n48 | CA\_n48(2A)\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n5B-n48A-n66(2A) | CA\_n5B  CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | CA\_n5B\_BCS 4 and 5 |  |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
| CA\_n2(2A)-n5A-n48(2A)-n66A | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n2 | CA\_n2(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n48 | CA\_n48(2A)\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n5A-n48B-n66A | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n48B  CA\_n2A-n66A  CA\_n5A-n48A  CA\_n5A-n48B  CA\_n5A-n66A  CA\_n48A-n66A  CA\_n48B-n66A  CA\_n48B | n2 | CA\_n2(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n48 | CA\_n48B\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n5A-n48(A-B)-n66A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48(A-B)\_BCS1 |  |
|  |  | n66 | 10, 15, 20, 25, 30, 40 |  |
|  | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n48 | CA\_n48(A-B)\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n5A-n48A-n77A | n775,6 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 508, 608, 708, 808, 908, 1008 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | n775,6  CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n77A5  CA\_n5A-n48A  CA\_n5A-n77A5 | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 508, 608, 708, 808, 908, 1008 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n77A  CA\_n5A-n48A  CA\_n5A-n77A | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n5A-n48A-n77A | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n77A  CA\_n5A-n48A  CA\_n5A-n77A | n2 | CA\_n2(2A) \_BCS 4 and 5 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n5A-n48(2A)-n77A | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n77A  CA\_n5A-n48A  CA\_n5A-n77A | n2 | CA\_n2(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n48 | CA\_n48(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n5B-n48A-n77A | CA\_n5B  CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n77A  CA\_n5A-n48A  CA\_n5A-n77A | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | CA\_n5B\_BCS 4 and 5 |  |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n5B-n48A-n77A | CA\_n5B  CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n77A  CA\_n5A-n48A  CA\_n5A-n77A | n2 | CA\_n2(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n5 | CA\_n5B\_BCS 4 and 5 |  |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n5B-n48(2A)-n77A | CA\_n5B  CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n77A  CA\_n5A-n48A  CA\_n5A-n77A | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | CA\_n5B\_BCS 4 and 5 |  |
|  |  | n48 | CA\_n48(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n5A-n48A-n77C | n775,6  CA\_n77C  CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n77A5  CA\_n5A-n48A  CA\_n5A-n77A5 | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 508, 608, 708, 808, 908, 1008 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  | n775,6 | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  | CA\_n77C  CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n77A  CA\_n2A-n77C  CA\_n5A-n48A  CA\_n5A-n77A  CA\_n5A-n77C | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77C\_BCS 4 and 5 |  |
| CA\_n2(2A)-n5A-n48A-n77C | CA\_n77C  CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n77A  CA\_n2A-n77C  CA\_n5A-n48A  CA\_n5A-n77A  CA\_n5A-n77C | n2 | CA\_n2(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77C\_BCS 4 and 5 |  |
| CA\_n2A-n5B-n48A-n77C | CA\_n5B  CA\_n77C  CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n77A  CA\_n2A-n77C  CA\_n5A-n48A  CA\_n5A-n77A  CA\_n5A-n77C | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | CA\_n5B\_BCS 4 and 5 |  |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77C\_BCS 4 and 5 |  |
| CA\_n2A-n5A-n48B-n77A | n775,6 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | n775,6  CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n77A5  CA\_n5A-n48A  CA\_n5A-n77A5 | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 2 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 3 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n48B  CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n48B  CA\_n2A-n77A  CA\_n5A-n48A  CA\_n5A-n48B  CA\_n5A-n77A | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n48 | CA\_n48B\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n5A-n48B-n77A | CA\_n48B  CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n48B  CA\_n2A-n77A  CA\_n5A-n48A  CA\_n5A-n48B  CA\_n5A-n77A | n2 | CA\_n2(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n48 | CA\_n48B\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n5B-n48B-n77A | CA\_n5B  CA\_n48B  CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n48B  CA\_n2A-n77A  CA\_n5A-n48A  CA\_n5A-n48B  CA\_n5A-n77A | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | CA\_n5B\_BCS 4 and 5 |  |
|  |  | n48 | CA\_n48B\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n5A-n48B-n77C | CA\_n48B  CA\_n77C  CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n48B  CA\_n2A-n77A  CA\_n2A-n77C  CA\_n5A-n48A  CA\_n5A-n48B  CA\_n5A-n77A | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  | CA\_n5A-n77C | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n48 | CA\_n48B\_BCS 4 and 5 |  |
|  |  | n77 | CA\_n77C\_BCS 4 and 5 |  |
| CA\_n2A-n5A-n48(2A)-n77A | n775,6 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | n775,6  CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n77A5  CA\_n5A-n48A  CA\_n5A-n77A5 | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 2 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n77A  CA\_n5A-n48A  CA\_n5A-n77A | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n48 | CA\_n48(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n5A-n48(2A)-n77C | CA\_n77C  CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n77A  CA\_n2A-n77C  CA\_n5A-n48A  CA\_n5A-n77A | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  | CA\_n5A-n77C | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n48 | CA\_n48(2A)\_BCS 4 and 5 |  |
|  |  | n77 | CA\_n77C\_BCS 4 and 5 |  |
| CA\_n2A-n5A-n66A-n77A | n775,6  CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n66A-n77A | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n5B-n66A-n77A | CA\_n5B  CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n66A-n77A | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | CA\_n5B\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n5B-n66(2A)-n77A | CA\_n5B  CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n66A-n77A | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | CA\_n5B\_BCS 4 and 5 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n5A-n66A-n77A | n775,6  CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n66A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30,40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n66A-n77A | n2 | CA\_n2(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n5A-n66(2A)-n77A | CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n66A-n77A | n2 | CA\_n2(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n5B-n66A-n77A | CA\_n5B  CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n66A-n77A | n2 | CA\_n2(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n5 | CA\_n5B\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n5A-n66A-n77C | CA\_n77C  CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n2A-n77C  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n5A-n77C  CA\_n66A-n77A  CA\_n66A-n77C | n2 | CA\_n2(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77C\_BCS 4 and 5 |  |
| CA\_n2A-n5A-n66(2A)-n77A | n775,6  CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n66A-n77A | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n5A-n66A-n77(2A) | n775,6  CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n2A-n5A-n66(2A)-n77(2A) | n775,6  CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2(2A)-n5A-n66A-n77(2A) | n775,6  CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n66A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n5A-n66A-n77C | n775,6  CA\_n77C  CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n5A-n77A5  CA\_n5A-n66A  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  | CA\_n77C  CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n2A-n77C  CA\_n5A-n77A  CA\_n5A-n77C  CA\_n5A-n66A  CA\_n66A-n77A | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  | CA\_n66A-n77C | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77C\_BCS 4 and 5 |  |
| CA\_n2A-n5A-n66(2A)-n77C | CA\_n77C  CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n2A-n77C  CA\_n5A-n77A  CA\_n5A-n66A  CA\_n5A-n77C  CA\_n66A-n77A | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  | CA\_n66A-n77C | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n77 | CA\_n77C\_BCS 4 and 5 |  |
| CA\_n2A-n5B-n66A-n77C | CA\_n5B  CA\_n77C  CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n2A-n77C  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n5A-n77C  CA\_n66A-n77A | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  | CA\_n66A-n77C | n5 | CA\_n5B\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77C\_BCS 4 and 5 |  |
| CA\_n2A-n12A-n30A-n66A | CA\_n2A-n12A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n12A-n30A  CA\_n12A-n66A  CA\_n30A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2(2A)-n12A-n30A-n66A | CA\_n2A-n12A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n12A-n30A  CA\_n12A-n66A  CA\_n30A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2A-n12A-n30A-n66(2A) | CA\_n2A-n12A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n12A-n30A  CA\_n12A-n66A  CA\_n30A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n2A-n12A-n30A-n77A | n775,6  CA\_n2A-n12A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n12A-n30A  CA\_n12A-n77A5  CA\_n30A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n12A-n30A-n77A | n775,6  CA\_n2A-n12A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n12A-n30A  CA\_n12A-n77A5  CA\_n30A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n12A-n30A-n77(2A) | n775,6  CA\_n2A-n12A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n12A-n30A  CA\_n12A-n77A5  CA\_n30A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2(2A)-n12A-n30A-n77(2A) | n775,6  CA\_n2A-n12A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n12A-n30A  CA\_n12A-n77A5  CA\_n30A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n12A-n66A-n77A | n775,6  CA\_n2A-n12A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n12A-n66A  CA\_n12A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n12A-n66A-n77A | n775,6  CA\_n2A-n12A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n12A-n66A  CA\_n12A-n77A5  CA\_n66A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n12A-n66(2A)-n77A | n775,6  CA\_n2A-n12A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n12A-n66A  CA\_n12A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n12A-n66A-n77(2A) | n775,6  CA\_n2A-n12A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n12A-n66A  CA\_n12A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n12A-n66(2A)-n77(2A) | n775,6  CA\_n2A-n12A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n12A-n66A  CA\_n12A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2(2A)-n12A-n66A-n77(2A) | n775,6  CA\_n2A-n12A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n12A-n66A  CA\_n12A-n77A5  CA\_n66A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n14A-n30A-n66A | CA\_n2A-n14A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n14A-n30A  CA\_n14A-n66A  CA\_n30A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2(2A)-n14A-n30A-n66A | CA\_n2A-n14A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n14A-n30A  CA\_n14A-n66A  CA\_n30A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  | n14 | 5, 10 |
|  | n30 | 5, 10 |
|  | n66 | 5, 10, 15, 20, 25, 30, 40 |
| CA\_n2A-n14A-n30A-n66(2A) | CA\_n2A-n14A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n14A-n30A  CA\_n14A-n66A  CA\_n30A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  | n14 | 5, 10 |
|  | n30 | 5, 10 |
|  | n66 | CA\_n66(2A)\_BCS1 |
| CA\_n2A-n14A-n30A-n77A | n775,6  CA\_n2A-n14A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n14A-n30A  CA\_n14A-n77A5  CA\_n30A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n14 | n14 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n30 | n30 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n14A-n30A-n77A | n775,6  CA\_n2A-n14A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n14A-n30A  CA\_n14A-n77A5  CA\_n30A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n14A-n30A-n77(2A) | n775,6  CA\_n2A-n14A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n14A-n30A  CA\_n14A-n77A5  CA\_n30A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n14 | n14 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n30 | n30 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n2(2A)-n14A-n30A-n77(2A) | n775,6  CA\_n2A-n14A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n14A-n30A  CA\_n14A-n77A5  CA\_n30A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n14A-n66A-n77A | n775,6  CA\_n2A-n14A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n14A-n66A  CA\_n14A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n14 | n14 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n14A-n66A-n77A | n775,6  CA\_n2A-n14A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n14A-n66A  CA\_n14A-n77A5  CA\_n66A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n14A-n66(2A)-n77A | n775,6  CA\_n2A-n14A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n14A-n66A  CA\_n14A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n14A-n66A-n77(2A) | n775,6  CA\_n2A-n14A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n14A-n66A  CA\_n14A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n14 | n14 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n2A-n14A-n66(2A)-n77(2A) | n775,6  CA\_n2A-n14A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n14A-n66A  CA\_n14A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2(2A)-n14A-n66A-n77(2A) | n775,6  CA\_n2A-n14A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n14A-n66A  CA\_n14A-n77A5  CA\_n66A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n29A-n30A-n66A | CA\_n2A-n30A  CA\_n2A-n66A  CA\_n30A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2(2A)-n29A-n30A-n66A | CA\_n2A-n30A  CA\_n2A-n66A  CA\_n30A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2A-n29A-n30A-n66(2A) | CA\_n2A-n30A  CA\_n2A-n66A  CA\_n30A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n2A-n29A-n30A-n77A | n775,6  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n30A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n29A-n30A-n77A | n775,6  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n30A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n29A-n30A-n77(2A) | n775,6  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n30A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2(2A)-n29A-n30A-n77(2A) | n775,6  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n30A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n29A-n66A-n77A | n775,6  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n29A-n66A-n77A | n775,6  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n66A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n29A-n66(2A)-n77A | n775,6  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n29A-n66A-n77(2A) | n775,6  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2(2A)-n29A-n66A-n77(2A) | n775,6  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n66A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n29A-n66(2A)-n77(2A) | n775,6  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n30A-n66A-n77A | n775,6  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n30 | n30 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n30A-n66A-n77A | n775,6  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n30A-n66(2A)-n77A | n775,6  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n30A-n66A-n77(2A) | n775,6  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n30 | n30 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n2A-n30A-n66(2A)-n77(2A) | n775,6  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2(2A)-n30A-n66A-n77(2A) | n775,6  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n41A-n66A-n71A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n2A-n48A-n66A-n77A | n775,6 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 508, 608, 708, 808, 908, 1008 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | n775,6  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n48A-n66A  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 508, 608, 708, 808, 908, 1008 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n48A-n66A  CA\_n66A-n77A | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n48A-n66A-n77A | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n48A-n66A  CA\_n66A-n77A | n2 | CA\_n2(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n48B-n66A-n77A | n775,6 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | n775,6  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n48A-n66A  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 2 |
|  |  | n48 | CA\_n48B\_BCS1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 3 |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n48B  CA\_n2A-n48A  CA\_n2A-n48B  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n48A-n66A  CA\_n48B-n66A  CA\_n66A-n77A | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | CA\_n48B\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n48B-n66A-n77A | CA\_n48B  CA\_n2A-n48A  CA\_n2A-n48B  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n48A-n66A  CA\_n48B-n66A  CA\_n66A-n77A | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n48 | CA\_n48B\_BCS4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n48(2A)-n66A-n77A | n775,6 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | n775,6  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n48A-n66A  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 2 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n48A-n66A  CA\_n66A-n77A | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | CA\_n48(2A)\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n48A-n66(2A)-n77A | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n48A-n66A  CA\_n66A-n77A | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n48(2A)-n66A-n77A | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n48A-n66A  CA\_n66A-n77A | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n48 | CA\_n48(2A)\_BCS4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n48A-n66(2A)-n77A | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n48A-n66A  CA\_n66A-n77A | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n48B-n66(2A)-n77A | CA\_n48B  CA\_n2A-n48A  CA\_n2A-n48B  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n48A-n66A  CA\_n48B-n66A  CA\_n66A-n77A | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | CA\_n48B\_BCS4 and 5 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n48(2A)-n66(2A)-n77A | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n48A-n66A  CA\_n66A-n77A | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | CA\_n48(2A)\_BCS 4 and 5 |  |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n48A-n66A-n77C | n775,6 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 508, 608, 708, 808, 908, 1008 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  | n775,6  CA\_n77C  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n48A-n66A  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 508, 608, 708, 808, 908, 1008 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 2 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 508, 608, 708, 808, 908, 1008 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  | CA\_n77C  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n2A-n77C  CA\_n48A-n66A  CA\_n66A-n77A | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  | CA\_n66A-n77C | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77C\_BCS 4 and 5 |  |
| CA\_n2(2A)-n48A-n66A-n77C | CA\_n77C  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n2A-n77C  CA\_n48A-n66A  CA\_n66A-n77A  CA\_n66A-n77C | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77C\_BCS 4 and 5 |  |
| CA\_n2A-n48B-n66A-n77C | CA\_n48B  CA\_n77C  CA\_n2A-n48A  CA\_n2A-n48B  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n2A-n77C  CA\_n48A-n66A  CA\_n48B-n66A  CA\_n66A-n77A | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  | CA\_n66A-n77C | n48 | CA\_n48B\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77C\_BCS 4 and 5 |  |
| CA\_n2A-n48(2A)-n66A-n77C | CA\_n77C  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n2A-n77C  CA\_n48A-n66A  CA\_n66A-n77A | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  | CA\_n66A-n77C | n48 | CA\_n48(2A)\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77C\_BCS 4 and 5 |  |
| CA\_n2A-n48A-n66(2A)-n77C | CA\_n77C  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n2A-n77C  CA\_n48A-n66A  CA\_n66A-n77A  CA\_n66A-n77C | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n77 | CA\_n77C\_BCS 4 and 5 |  |
| CA\_n2A-n66A-n71A-n77A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n66A-n71A-n77(2A) | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n66A-n71A-n78A | - | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n66A-n71A-n78(2A) | - | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3A-n5A-n7A-n78A | - | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n3A-n5A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n5A-n7A  CA\_n5A-n78A  CA\_n7A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n5A-n7B-n78A | - | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n3A-n5A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n5A-n7A  CA\_n5A-n78A  CA\_n7A-n78A  CA\_n7B | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n5A-n28A-n78A | CA\_n3A-n5A  CA\_n3A-n28A  CA\_n3A-n79A  CA\_n5A-n28A  CA\_n5A-n79A  CA\_n28A-n79A | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n5A-n28A-n79A | CA\_n3A-n5A  CA\_n3A-n28A  CA\_n3A-n79A  CA\_n5A-n28A  CA\_n5A-n79A  CA\_n28A-n79A | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n7A-n8A-n40A | CA\_n3A-n7A  CA\_n3A-n8A  CA\_n3A-n40A  CA\_n7A-n8A  CA\_n7A-n40A  CA\_n8A-n40A | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n8 | n8 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n7A-n8A-n78A | CA\_n3A-n7A  CA\_n3A-n8A  CA\_n3A-n78A  CA\_n7A-n8A  CA\_n7A-n78A  CA\_n8A-n78A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n3(2A)-n7A-n8A-n78A | CA\_n3A-n7A  CA\_n3A-n8A  CA\_n3A-n78A  CA\_n7A-n8A  CA\_n7A-n78A  CA\_n8A-n78A | n3 | CA\_n3(2A)\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n7(2A)-n8A-n78A | CA\_n3A-n7A  CA\_n3A-n8A  CA\_n3A-n78A  CA\_n7A-n8A  CA\_n7A-n78A  CA\_n8A-n78A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n7 | CA\_n7(2A)\_BCS0 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3(2A)-n7(2A)-n8A-n78A | CA\_n3A-n7A  CA\_n3A-n8A  CA\_n3A-n78A  CA\_n7A-n8A  CA\_n7A-n78A  CA\_n8A-n78A | n3 | CA\_n3(2A)\_BCS0 | 0 |
|  |  | n7 | CA\_n7(2A)\_BCS0 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n7A-n20A-n67A | CA\_n3A-n7A  CA\_n3A-n20A  CA\_n7A-n20A | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n7A-n20A-n78A | CA\_n3A-n7A  CA\_n3A-n20A  CA\_n3A-n78A  CA\_n7A-n20A  CA\_n7A-n78A  CA\_n20A-n78A | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n7A-n20A-n78(2A) | CA\_n3A-n7A  CA\_n3A-n20A  CA\_n3A-n78A  CA\_n7A-n20A  CA\_n7A-n78A  CA\_n20A-n78A  CA\_n78(2A) | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS 4 and 5 |  |
| CA\_n3A-n7A-n26A-n78A | CA\_n3A-n7A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n7A-n78A  CA\_n26A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n7B-n26A-n78A | CA\_n3A-n7A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n7A-n78A  CA\_n26A-n78A  CA\_n7B | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n7A-n26(2A)-n78A | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  | CA\_n26(2A) | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n7A-n26A-n78(2A) | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  | CA\_n78(2A) | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n26 | n26 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS 4 and 5 |  |
| CA\_n3A-n7A-n26A-n78C | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n78C | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n3A-n7A-n26(2A)-n78(2A) | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  | CA\_n26(2A) | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  | CA\_n78(2A) | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n3A-n7A-n26(2A)-n78C | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n26(2A)  CA\_n78C | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n3A-n7B-n26(2A)-n78A | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  | CA\_n26(2A) | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n7B-n26A-n78(2A) | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | n26 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A) \_BCS0 |  |
|  | CA\_n78(2A) | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | CA\_n7B\_BCS 4 and 5 |  |
|  |  | n26 | n26 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS 4 and 5 |  |
| CA\_n3A-n7B-n26A-n78C | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B  CA\_n78C | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n3A-n7B-n26(2A)-n78(2A) | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  | CA\_n26(2A) )  CA\_n78(2A) | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n3A-n7B-n26(2A)-n78C | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B  CA\_n26(2A)  CA\_n78C | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n3B-n7A-n26A-n78A | CA\_n3A-n7A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n7A-n78A  CA\_n26A-n78A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3B-n7A-n26(2A)-n78A | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A | n3 | CA\_n3B\_BCS0 | 0 |
|  | CA\_n26(2A) | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3B-n7A-n26A-n78(2A) | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  | CA\_n78(2A) | n3 | CA\_n3B\_BCS 4 and 5 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n26 | n26 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS 4 and 5 |  |
| CA\_n3B-n7A-n26A-n78C | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n78C | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n3B-n7A-n26(2A)-n78(2A) | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n26(2A)  CA\_n78(2A) | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3B-n7A-n26(2A)-n78C | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n26(2A)  CA\_n78C | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n3B-n7B-n26A-n78A | CA\_n3A-n7A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n7A-n78A  CA\_n26A-n78A  CA\_n7B | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3B-n7B-n26(2A)-n78A | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B | n3 | CA\_n3B\_BCS0 | 0 |
|  | CA\_n26(2A) | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3B-n7B-n26A-n78(2A) | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  | CA\_n78(2A) | n3 | CA\_n3B\_BCS 4 and 5 | 4 and 5 |
|  |  | n7 | CA\_n7B\_BCS 4 and 5 |  |
|  |  | n26 | n26 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS 4 and 5 |  |
| CA\_n3B-n7B-n26A-n78C | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B  CA\_n78C | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n3B-n7B-n26(2A)-n78(2A) | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B | n3 | CA\_n3B\_BCS0 | 0 |
|  | CA\_n26(2A) | n7 | CA\_n7B\_BCS0 |  |
|  | CA\_n78(2A) | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3B-n7B-n26(2A)-n78C | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B  CA\_n26(2A)  CA\_n78C | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n3A-n7A-n28A-n38A7 | - | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n3A-n7A-n28A-n78A | n35  n75  n785,6 | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | n35  n75  n785,6  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n3A-n78A5  CA\_n7A-n28A  CA\_n7A-n78A5  CA\_n28A-n78A5 | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 202 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n7A-n28A-n78(2A) | n35  n75  n785,6  CA\_n78(2A)5  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n3A-n78A5  CA\_n7A-n28A  CA\_n7A-n78A5  CA\_n28A-n78A5 | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 202 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS 4 and 5 |  |
| CA\_n3A-n7A-n28A-n78C | CA\_n78C  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 202 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n3A-n7B-n28A-n78A | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n3A-n7A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n7B  CA\_n28A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n7B-n28A-n78(2A) | CA\_n7B  CA\_n78(2A)  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3A-n7B-n28A-n78C | CA\_n7B  CA\_n78C  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n3B-n7A-n28A-n78A | CA\_n3A-n7A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3B-n7A-n28A-n78(2A) | CA\_n78(2A)  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3B-n7B-n28A-n78A | CA\_n7B  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3B-n7B-n28A-n78(2A) | CA\_n7B  CA\_n78(2A)  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3B-n7B-n28A-n78C | CA\_n7B  CA\_n78C  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n3B-n7A-n28A-n78C | CA\_n78C  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n3A-n7A-n38A-n78A7 | - | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n7A-n40A-n78A | CA\_n3A-n7A  CA\_n3A-n40A  CA\_n3A-n78A  CA\_n7A-n40A  CA\_n7A-n78A  CA\_n40A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n7A-n40A-n79A | CA\_n3A-n7A  CA\_n3A-n79A  CA\_n3A-n40A  CA\_n7A-n79A  CA\_n7A-n40A  CA\_n40A-n79A | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n7A-n40A-n105A | CA\_n3A-n7A  CA\_n3A-n40A  CA\_n3A-n105A  CA\_n7A-n40A  CA\_n7A-n105A  CA\_n40A-n105A | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n3A-n7A-n67A-n78A | CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n7A-n67A-n78(2A) | CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A  CA\_n78(2A) | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n3A-n7A-n75A-n78A | CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n75 | n75 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n7A-n78A-n105A | CA\_n3A-n7A  CA\_n3A-n78A  CA\_n3A-n105A  CA\_n7A-n78A  CA\_n7A-n105A  CA\_n78A-n105A | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n3A-n8A-n28A-n40A | CA\_n3A-n8A  CA\_n3A-n28A  CA\_n3A-n40A  CA\_n8A-n28A  CA\_n8A-n40A  CA\_n28A-n40A | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n8 | n8 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n8A-n39A-n41A | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 35, 40 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n3A-n8A-n39A-n79A | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 35, 40 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n3A-n8A-n40A-n78A | CA\_n3A-n8A  CA\_n3A-n40A  CA\_n3A-n78A  CA\_n8A-n40A  CA\_n8A-n78A  CA\_n40A-n78A | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n8 | n8 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n8A-n40A-n79A | CA\_n3A-n8A  CA\_n3A-n40A  CA\_n3A-n79A  CA\_n8A-n40A  CA\_n8A-n79A  CA\_n40A-n79A | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n8 | n8 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n8A-n41A-n78A | CA\_n3A-n8A  CA\_n3A-n41A  CA\_n3A-n78A  CA\_n8A-n41A  CA\_n8A-n78A  CA\_n41A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n78 | 10, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n8A-n41A-n78C | CA\_n3A-n8A  CA\_n3A-n41A  CA\_n3A-n78A  CA\_n3A-n78C  CA\_n8A-n41A  CA\_n8A-n78A  CA\_n8A-n78C  CA\_n41A-n78A  CA\_n41A-n78C | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n3A-n8A-n41A-n79A | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n3A-n18A-n28A-n41A | n415  CA\_n3A-n18A  CA\_n3A-n28A  CA\_n3A-n41A5  CA\_n18A-n28A  CA\_n18A-n41A5  CA\_n28A-n41A5 | n3 | 5, 10, 15, 20 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n18 | n18 channel bandwidths in Table 5.3.5-1 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |
| CA\_n3A-n18A-n28A-n77A | n775  CA\_n3A-n18A  CA\_n3A-n28A  CA\_n3A-n41A5  CA\_n18A-n28A  CA\_n18A-n41A5  CA\_n28A-n41A5 | n3 | 5, 10, 15, 20 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n28 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n18 | n18 channel bandwidths in Table 5.3.5-1 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |
| CA\_n3A-n18A-n41A-n77A | n415  n775  CA\_n3A-n18A  CA\_n3A-n41A5  CA\_n3A-n77A5  CA\_n18A-n41A5  CA\_n18A-n77A5  CA\_n41A-n77A5 | n3 | 5, 10, 15, 20 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n18 | n18 channel bandwidths in Table 5.3.5-1 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |
| CA\_n3A-n20A-n41A-n71A | CA\_n3A-n20A  CA\_n3A-n41A  CA\_n3A-n71A  CA\_n20A-n41A  CA\_n20A-n71A  CA\_n41A-n71A | n3 | 5, 10,15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n20 | 5, 10,15, 20 |  |
|  |  | n41 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50, 60, 70, 80, 90, 100 |  |
|  |  | n71 | 5, 10,15, 20, 25, 30, 35 |  |
| CA\_n3A-n20A-n41A-n77A | CA\_n3A-n20A  CA\_n3A-n41A  CA\_n3A-n77A  CA\_n20A-n41A  CA\_n20A-n77A  CA\_n41A-n77A | n3 | 5, 10,15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n20 | 5, 10,15, 20 |  |
|  |  | n41 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n20A-n41A-n77(2A) | CA\_n3A-n20A  CA\_n3A-n41A  CA\_n3A-n77A  CA\_n20A-n41A  CA\_n20A-n77A  CA\_n41A-n77A | n3 | 5, 10,15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n20 | 5, 10,15, 20 |  |
|  |  | n41 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n3A-n20A-n41A-n78A | CA\_n3A-n20A  CA\_n3A-n41A  CA\_n3A-n78A  CA\_n20A-n41A  CA\_n20A-n78A  CA\_n41A-n78A | n3 | 5, 10,15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n20 | 5, 10,15, 20 |  |
|  |  | n41 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50, 60, 70, 80, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n20A-n67A-n78A | CA\_n3A-n20A  CA\_n3A-n78A  CA\_n20A-n78A | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n20A-n67A-n78(2A) | CA\_n3A-n20A  CA\_n3A-n78A  CA\_n20A-n78A  CA\_n78(2A) | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS 4 and 5 |  |
| CA\_n3A-n20A-n71A-n78A | CA\_n3A-n20A  CA\_n3A-n71A  CA\_n3A-n78A  CA\_n20A-n71A  CA\_n20A-n78A  CA\_n71A-n78A | n3 | 5, 10,15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n20 | 5, 10,15, 20 |  |
|  |  | n71 | 5, 10,15, 20, 25, 30, 35 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n28A-n38A-n78A | - | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n28A-n40A-n41A | CA\_n3A-n28A  CA\_n3A-n40A  CA\_n3A-n41A  CA\_n28A-n40A  CA\_n28A-n41A  CA\_n40A-n41A | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n28A-n40A-n77A | CA\_n3A-n28A  CA\_n3A-n40A  CA\_n3A-n77A  CA\_n28A-n40A  CA\_n28A-n77A  CA\_n40A-n77A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n40 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n28A-n40A-n77(2A) | CA\_n3A-n28A  CA\_n3A-n40A  CA\_n3A-n77A  CA\_n28A-n40A  CA\_n28A-n77A  CA\_n40A-n77A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n40 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
| CA\_n3A-n28A-n40A-n78A | CA\_n3A-n28A  CA\_n3A-n40A  CA\_n3A-n78A  CA\_n28A-n40A  CA\_n28A-n78A  CA\_n40A-n78A | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n28A-n40A-n79A | CA\_n3A-n28A  CA\_n3A-n40A  CA\_n3A-n79A  CA\_n28A-n40A  CA\_n28A-n79A  CA\_n40A-n79A | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n28A-n41A-n77A | n415,6  n775,6  CA\_n3A-n28A  CA\_n3A-n41A5  CA\_n3A-n77A5  CA\_n28A-n41A5  CA\_n28A-n77A5  CA\_n41A-n77A5 | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |
| CA\_n3A-n28A-n41B-n77A | CA\_n3A-n28A  CA\_n3A-n41A  CA\_n3A-n77A  CA\_n28A-n41A  CA\_n28A-n77A  CA\_n41A-n77A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n28A-n41A-n77(2A) | n415,6  n775,6  CA\_n3A-n28A  CA\_n3A-n41A5  CA\_n3A-n77A5  CA\_n28A-n41A5  CA\_n28A-n77A5  CA\_n41A-n77A5 | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  | n415,6  n775,6  CA\_n3A-n28A  CA\_n3A-n41A5  CA\_n3A-n77A5  CA\_n28A-n41A5  CA\_n28A-n77A5  CA\_n41A-n77A5 | n3 | 5, 10, 15, 20 | 1 |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  | n415,6  n775,6  CA\_n3A-n28A  CA\_n3A-n41A5  CA\_n3A-n77A5  CA\_n28A-n41A5  CA\_n28A-n77A5  CA\_n41A-n77A5  CA\_n77(2A) | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |
| CA\_n3A-n28A-n41B-n77(2A) | CA\_n3A-n28A  CA\_n3A-n41A  CA\_n3A-n77A  CA\_n28A-n41A  CA\_n28A-n77A  CA\_n41A-n77A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
| CA\_n3A-n28A-n41A-n78A | CA\_n3A-n28A  CA\_n3A-n41A  CA\_n3A-n78A  CA\_n28A-n41A  CA\_n28A-n78A  CA\_n41A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n28A-n41A-n78(2A) | CA\_n3A-n28A  CA\_n3A-n41A  CA\_n3A-n78A  CA\_n28A-n41A  CA\_n28A-n78A  CA\_n41A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3A-n28A-n41A-n79A | n415,6  n795,6  CA\_n3A-n28A  CA\_n3A-n41A5  CA\_n3A-n79A5  CA\_n28A-n41A5  CA\_n28A-n79A5  CA\_n41A-n79A5 | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n3A-n28A-n77A-n79A | n775,6  n795,6  CA\_n3A-n28A  CA\_n3A-n77A5  CA\_n3A-n79A5  CA\_n28A-n77A5  CA\_n28A-n79A5  CA\_n77A-n79A5 | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 80, 100 |  |
|  | CA\_n3A-n28A  CA\_n3A-n77A  CA\_n3A-n79A  CA\_n28A-n77A  CA\_n28A-n79A  CA\_n77A-n79A | n3 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n28A-n77(2A)-n79A | CA\_n3A-n28A  CA\_n3A-n77A  CA\_n3A-n79A  CA\_n28A-n77A  CA\_n28A-n79A  CA\_n77A-n79A  CA\_n77(2A) | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n79 | 40, 50, 80, 100 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n28A-n77(3A)-n79A | CA\_n3A-n28A  CA\_n3A-n77A  CA\_n3A-n79A  CA\_n28A-n77A  CA\_n28A-n79A  CA\_n77A-n79A  CA\_n77(2A) | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
|  |  | n79 | 40, 50, 80, 100 |  |
| CA\_n3A-n39A-n41A-n79A | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 35, 40 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n3A-n40A-n78A-n79A | CA\_n3A-n40A  CA\_n3A-n78A  CA\_n3A-n79A  CA\_n40A-n78A  CA\_n40A-n79A  CA\_n78A-n79A | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n40A-n78A-n105A | CA\_n3A-n40A  CA\_n3A-n78A  CA\_n3A-n105A  CA\_n40A-n78A  CA\_n40A-n105A  CA\_n78A-n105A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25,30, 35 |  |
| CA\_n3A-n41A-n71A-n77A | CA\_n3A-n41A  CA\_n3A-n71A  CA\_n3A-n77A  CA\_n41A-n71A  CA\_n41A-n77A  CA\_n71A-n77A | n3 | 5, 10,15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n41 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50, 60, 70, 80, 90, 100 |  |
|  |  | n71 | 5, 10,15, 20, 25, 30, 35 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n41A-n71A-n77(2A) | CA\_n3A-n41A  CA\_n3A-n71A  CA\_n3A-n77A  CA\_n41A-n71A  CA\_n41A-n77A  CA\_n71A-n77A | n3 | 5, 10,15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n41 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50, 60, 70, 80, 90, 100 |  |
|  |  | n71 | 5, 10,15, 20, 25, 30, 35 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n3A-n41A-n71A-n78A | CA\_n3A-n41A  CA\_n3A-n71A  CA\_n3A-n78A  CA\_n41A-n71A  CA\_n41A-n78A  CA\_n71A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n71 | 5, 10, 15, 20, |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n41A-n71A-n78C | CA\_n3A-n41A  CA\_n3A-n71A  CA\_n3A-n78A  CA\_n3A-n78C  CA\_n41A-n71A  CA\_n41A-n78A  CA\_n41A-n78C  CA\_n71A-n78A  CA\_n71A-n78C | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n71 | 5, 10, 15, 20, |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n3A-n41A-n77A-n79A | n415,6  n775,6  n795,6  CA\_n3A-n41A5  CA\_n3A-n77A5  CA\_n3A-n79A5  CA\_n41A-n77A5  CA\_n41A-n79A5  CA\_n77A-n79A5 | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n3A-n41A-n77(2A)-n79A | CA\_n3A-n41A  CA\_n3A-n77A  CA\_n3A-n79A  CA\_n41A-n77A  CA\_n41A-n79A  CA\_n77A-n79A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |

##### Table 5.5A.3.3-1b

Table 5.5A.3.3-1b: NR CA configurations and bandwidth combinations sets defined for inter-band CA (four bands)

| NR CA configuration | Uplink CA configuration  or single uplink carrier 4 | NR Band | Channel bandwidth (MHz) (NOTE 3) | Bandwidth combination set |
| --- | --- | --- | --- | --- |
| CA\_n5A-n7A-n40A-n78A | CA\_n5A-n7A CA\_n5A-n40A CA\_n5A-n78A CA\_n7A-n40A CA\_n7A-n78A CA\_n40A-n78A | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n7A-n40A-n105A | CA\_n5A-n7A CA\_n5A-n40A CA\_n5A-n105A CA\_n7A-n40A CA\_n7A-n105A CA\_n40A-n105A | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n5A-n7A-n66A-n77A | CA\_n5A-n7A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n7A-n66A  CA\_n7A-n77A  CA\_n66A-n77A | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n7A-n66A-n77(2A) | CA\_n77(2A)  CA\_n5A-n7A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n7A-n66A  CA\_n7A-n77A  CA\_n66A-n77A | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n5A-n7A-n66A-n77(3A) | CA\_n5A-n7A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n7A-n66A  CA\_n7A-n77A  CA\_n66A-n77A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n66 | 5, 10, 15, 20, 30, 40 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(3A)\_BCS4 and 5 |  |
| CA\_n5A-n7A-n78A-n105A | CA\_n5A-n7A CA\_n5A-n78A CA\_n5A-n105A CA\_n7A-n78A CA\_n7A-n105A CA\_n78A-n105A | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n5A-n25A-n29A-n66A | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n25A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 30, 40 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n29 | n29 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n25A-n66A-n77A | n775,6  CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n66A-n77A5 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n25(2A)-n66A-n77A | n775,6  CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n66A-n77A5 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n25A-n66(2A)-n77A | n775,6  CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n66A-n77A5 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n25A-n66A-n77(2A) | n775,6  CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n66A-n77A5 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n25A-n66A-n77(3A) | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 30, 40 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(3A)\_BCS4 and 5 |  |
| CA\_n5A-n25(2A)-n66(2A)-n77A | n775,6  CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n66A-n77A5 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n25(2A)-n66A-n77(2A) | n775,6  CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n66A-n77A5 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n25A-n66(2A)-n77(2A) | n775,6  CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n66A-n77A5 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n25(2A)-n66(2A)-n77(2A) | n775,6  CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n66A-n77A5 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n25A-n66A-n78A | n785  CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n78A5  CA\_n25A-n66A  CA\_n25A-n78A5  CA\_n66A-n78A5 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n25(2A)-n66A-n78A | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n25A-n66(2A)-n78A | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n25A-n66A-n78(2A) | n785  CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n78A5  CA\_n25A-n66A  CA\_n25A-n78A5  CA\_n66A-n78A5 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n5A-n25(2A)-n66(2A)-n78A | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n25(2A)-n66A-n78(2A) | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n5A-n25A-n66(2A)-n78(2A) | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n5A-n25(2A)-n66(2A)-n78(2A) | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n5A-n28A-n78A-n79A | CA\_n5A-n28A  CA\_n5A-n78A  CA\_n5A-n79A  CA\_n28A-n78A  CA\_n28A-n79A  CA\_n78A-n79A | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n30A-n66A-n77A | n775,6  CA\_n5A-n30A  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n30 | n30 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n30A-n66(2A)-n77A | n775,6  CA\_n5A-n30A  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n30A-n66(2A)-n77(2A) | n775,6  CA\_n5A-n30A  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n30A-n66A-n77(2A) | n775,6CA\_n5A-n30A  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n30 | n30 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n5A-n40A-n78A-n105A | CA\_n5A-n40A CA\_n5A-n78A CA\_n5A-n105A CA\_n40A-n78A CA\_n40A-n105A CA\_n78A-n105A | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n5A-n48A-n66A-n77A | n775,6 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 508, 608, 708, 808, 908, 1008 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | n775,6  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n48A-n66A  CA\_n66A-n77A5 | n5 | 5, 10, 15, 20, 25 | 1 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 508, 608, 708, 808, 908, 1008 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n48A-n66A  CA\_n66A-n77A | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n48(2A)-n66(2A)-n77A | CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n48A-n66A  CA\_n66A-n77A | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | CA\_n48(2A)\_BCS4 and 5 |  |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n48A-n66A-n77C | n775,6  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n48A-n66A  CA\_n66A-n77A5 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 508, 608, 708, 808, 908, 1008 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  | CA\_n77C  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n5A-n77AC  CA\_n48A-n66A  CA\_n66A-n77A | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  | CA\_n66A-n77C | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77C\_BCS 4 and 5 |  |
| CA\_n5A-n48A-n66(2A)-n77C | CA\_n77C  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n5A-n77C  CA\_n48A-n66A  CA\_n66A-n77A  CA\_n66A-n77C | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 |  |
|  |  | n77 | CA\_n77C\_BCS 4 and 5 |  |
| CA\_n5B-n48A-n66A-n77A | CA\_n5B  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n48A-n66A  CA\_n66A-n77A | n5 | CA\_n5B\_BCS 4 and 5 | 4 and 5 |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5B-n48(2A)-n66A-n77A | CA\_n5B  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n48A-n66A  CA\_n66A-n77A | n5 | CA\_n5B\_BCS 4 and 5 | 4 and 5 |
|  |  | n48 | CA\_n48(2A)\_BCS4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5B-n48A-n66(2A)-n77A | CA\_n5B  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n48A-n66A  CA\_n66A-n77A | n5 | CA\_n5B\_BCS 4 and 5 | 4 and 5 |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5B-n48A-n66A-n77C | CA\_n5B  CA\_n77C  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n5A-n77C  CA\_n48A-n66A  CA\_n66A-n77A  CA\_n66A-n77C | n5 | CA\_n5B\_BCS4 and 5 | 4 and 5 |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77C\_BCS 4 and 5 |  |
| CA\_n5A-n48B-n66A-n77A | n775,6 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | n775,6  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n48A-n66A  CA\_n66A-n77A5 | n5 | 5, 10, 15, 20, 25 | 1 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n5 | 5, 10, 15, 20, 25 | 2 |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n5 | 5, 10, 15, 20, 25 | 3 |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n48B  CA\_n5A-n48A  CA\_n5A-n48B  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n48A-n66A  CA\_n48B-n66A  CA\_n66A-n77A | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | CA\_n48B\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5B-n48B-n66A-n77A | CA\_n5B  CA\_n48B  CA\_n5A-n48A  CA\_n5A-n48B  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n48A-n66A  CA\_n48B-n66A  CA\_n66A-n77A | n5 | CA\_n5B\_BCS4 and 5 | 4 and 5 |
|  |  | n48 | CA\_n48B\_BCS4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n48B-n66(2A)-n77A | CA\_n48B  CA\_n5A-n48A  CA\_n5A-n48B  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n48A-n66A  CA\_n48B-n66A  CA\_n66A-n77A | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | CA\_n48B\_BCS4 and 5 |  |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n48B-n66A-n77C | CA\_n48B  CA\_n77C  CA\_n5A-n48A  CA\_n5A-n48B  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n5A-n77C  CA\_n48A-n66A  CA\_n48B-n66A  CA\_n66A-n77A | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  | CA\_n66A-n77C | n48 | CA\_n48B\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77C\_BCS 4 and 5 |  |
| CA\_n5A-n48(2A)-n66A-n77A | n775,6 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | n775,6  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n48A-n66A  CA\_n66A-n77A5 | n5 | 5, 10, 15, 20, 25 | 1 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n5 | 5, 10, 15, 20, 25 | 2 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n48A-n66A  CA\_n66A-n77A | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | CA\_n48(2A)\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n48A-n66(2A)-n77A | CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n48A-n66A  CA\_n66A-n77A | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n48(2A)-n66A-n77C | CA\_n77C  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n5A-n77C  CA\_n48A-n66A  CA\_n66A-n77A | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  | CA\_n66A-n77C | n48 | CA\_n48(2A)\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77C\_BCS 4 and 5 |  |
| CA\_n7A-n8A-n28A-n40A | CA\_n7A-n8A  CA\_n7A-n28A  CA\_n7A-n40A  CA\_n8A-n28A  CA\_n8A-n40A  CA\_n28A-n40A | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n8 | n8 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n8A-n40A-n78A | CA\_n7A-n8A  CA\_n7A-n40A  CA\_n7A-n78A  CA\_n8A-n40A  CA\_n8A-n78A  CA\_n40A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n8 | n8 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n8A-n40A-n79A | CA\_n7A-n8A  CA\_n7A-n40A  CA\_n7A-n79A  CA\_n8A-n40A  CA\_n8A-n79A  CA\_n40A-n79A | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n8 | n8 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n12A-n25A-n66A | - | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n12 | n12 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n20A-n67A-n78A | CA\_n7A-n20A  CA\_n7A-n78A  CA\_n20A-n78A | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n20A-n67A-n78(2A) | CA\_n7A-n20A  CA\_n7A-n78A  CA\_n20A-n78A  CA\_n78(2A) | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS 4 and 5 |  |
| CA\_n7A-n25A-n29A-n77A | CA\_n7A-n25A  CA\_n7A-n77A  CA\_n25A-n77A | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n29 | n29 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n25A-n29A-n77(2A) | CA\_n7A-n25A  CA\_n7A-n77A  CA\_n25A-n77A  CA\_n77(2A) | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n25 | n29 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n29 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n7A-n25A-n29A-n77(3A) | CA\_n7A-n25A  CA\_n7A-n77A  CA\_n25A-n77A  CA\_n77(2A) | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n25 | n29 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n29 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(3A)\_BCS4 and 5 |  |
| CA\_n7A-n25A-n66A-n71A | - | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n25A-n66A-n77A | n775,6  CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n66A-n77A5 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n25A-n66A-n77A | n775,6  CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n66A-n77A5 | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n25(2A)-n66A-n77A | n775,6  CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n66A-n77A5 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n25A-n66(2A)-n77A | n775,6  CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n66A-n77A5 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n25A-n66A-n77(2A) | n775,6  CA\_n77(2A)5  CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n66A-n77A5 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7A-n25A-n66A-n77(3A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 30, 40 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(3A)\_BCS4 and 5 |  |
| CA\_n7(2A)-n25(2A)-n66A-n77A | n775,6  CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n66A-n77A5 | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n25A-n66(2A)-n77A | n775,6  CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n66A-n77A5 | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n25A-n66A-n77(2A) | n775,6  CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n66A-n77A5 | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7A-n25(2A)-n66(2A)-n77A | n775,6  CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n66A-n77A5 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n25(2A)-n66A-n77(2A) | n775,6  CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n66A-n77A5 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7A-n25A-n66(2A)-n77(2A) | n775,6  CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n66A-n77A5 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7(2A)-n25(2A)-n66(2A)-n77A | n775,6  CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n66A-n77A5 | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n25A-n66(2A)-n77(2A) | n775,6  CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n66A-n77A5 | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7(2A)-n25(2A)-n66A-n77(2A) | n775,6  CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n66A-n77A5 | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7A-n25(2A)-n66(2A)-n77(2A) | n775,6  CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n66A-n77A5 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7(2A)-n25(2A)-n66(2A)-n77(2A) | n775,6  CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n66A-n77A5 | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7A-n25A-n66A-n78A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n25(2A)-n66A-n78A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n25A-n66(2A)-n78A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n25A-n66A-n78(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7(2A)-n25A-n66A-n78A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n25(2A)-n66A-n78(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7A-n25(2A)-n66(2A)-n78A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n25A-n66(2A)-n78(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7(2A)-n25(2A)-n66A-n78A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n25A-n66(2A)-n78A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n25A-n66A-n78(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7A-n25(2A)-n66(2A)-n78(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7(2A)-n25(2A)-n66A-n78(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7(2A)-n25(2A)-n66(2A)-n78A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n25A-n66(2A)-n78(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7(2A)-n25(2A)-n66(2A)-n78(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7A-n28A-n38A-n78A7 | - | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n28A-n40A-n78A | CA\_n7A-n28A  CA\_n7A-n40A  CA\_n7A-n78A  CA\_n28A-n40A  CA\_n28A-n78A  CA\_n40A-n78A | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n28A-n40A-n79A | CA\_n7A-n28A  CA\_n7A-n40A  CA\_n7A-n79A  CA\_n28A-n40A  CA\_n28A-n79A  CA\_n40A-n79A | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n29A-n66A-n77A | CA\_n7A-n66A  CA\_n7A-n77A  CA\_n66A-n77A | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n29 | n29 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n29A-n66A-n77(2A) | CA\_n7A-n66A  CA\_n7A-n77A  CA\_n66A-n77A  CA\_n77(2A) | n7 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n29 | n29 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n7A-n29A-n66A-n77(3A) | CA\_n7A-n66A  CA\_n7A-n77A  CA\_n66A-n77A  CA\_n77(2A) | n7 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n29 | n29 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(3A)\_BCS4 and 5 |  |
| CA\_n7A-n40A-n78A-n79A | CA\_n7A-n40A  CA\_n7A-n78A  CA\_n7A-n79A  CA\_n40A-n78A  CA\_n40A-n79A  CA\_n78A-n79A | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n40A-n78A-n105A | CA\_n7A-n40A  CA\_n7A-n78A  CA\_n7A-n105A  CA\_n40A-n78A  CA\_n40A-n105A  CA\_n78A-n105A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n78 | 10, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n7A-n66A-n71A-n77A | CA\_n7A-n66A  CA\_n7A-n71A  CA\_n7A-n77A  CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n66A-n71A-n77(2A) | CA\_n7A-n66A  CA\_n7A-n71A  CA\_n7A-n77A  CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n7A-n66A-n71A-n77(3A) | CA\_n7A-n66A  CA\_n7A-n71A  CA\_n7A-n77A  CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | 5, 10, 15, 20, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20, 25, 30, 35 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(3A)\_BCS4 and 5 |  |
| CA\_n8A-n20A-n28A-n75A | CA\_n8A-n20A  CA\_n8A-n28A  CA\_n20A-n28A | n8 | 5, 10, 15, 20 | 0 |
|  |  | n20 | 5, 10, 15, 20 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n75 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n8A-n28A-n40A-n78A | CA\_n8A-n28A  CA\_n8A-n40A  CA\_n8A-n78A  CA\_n28A-n40A  CA\_n28A-n78A  CA\_n40A-n78A | n8 | n8 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n8A-n28A-n40A-n79A | CA\_n8A-n28A  CA\_n8A-n40A  CA\_n8A-n79A  CA\_n28A-n40A  CA\_n28A-n79A  CA\_n40A-n79A | n8 | n8 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n8A-n39A-n41A-n79A | - | n8 | 5, 10, 15, 20 | 0 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n8A-n40A-n78A-n79A | CA\_n8A-n40A  CA\_n8A-n78A  CA\_n8A-n79A  CA\_n40A-n78A  CA\_n40A-n79A  CA\_n78A-n79A | n8 | n8 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n12A-n30A-n66A-n77A | n775,6  CA\_n12A-n30A  CA\_n12A-n66A  CA\_n12A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | n12 | 5, 10,15 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n12A-n30A-n66(2A)-n77A | n775,6  CA\_n12A-n30A  CA\_n12A-n66A  CA\_n12A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | n12 | 5, 10,15 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n12A-n30A-n66A-n77(2A) | n775,6  CA\_n12A-n30A  CA\_n12A-n66A  CA\_n12A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | n12 | 5, 10,15 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n12A-n30A-n66(2A)-n77(2A) | n775,6  CA\_n12A-n30A  CA\_n12A-n66A  CA\_n12A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | n12 | 5, 10,15 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n13A-n25A-n66A-n77A | n775,6  CA\_n13A-n25A  CA\_n13A-n66A  CA\_n13A-n77A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n66A-n77A5 | n13 | 5, 10 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n13A-n25A-n66A-n77(2A) | n775,6  CA\_n77(2A)  CA\_n13A-n25A  CA\_n13A-n66A  CA\_n13A-n77A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n66A-n77A5 | n13 | 5, 10 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n14A-n30A-n66A-n77A | n775,6  CA\_n14A-n30A  CA\_n14A-n66A  CA\_n14A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | n14 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n14 | n14 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n30 | n30 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n14A-n30A-n66(2A)-n77A | n775,6  CA\_n14A-n30A  CA\_n14A-n66A  CA\_n14A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | n14 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n14A-n30A-n66A-n77(2A) | n775,6  CA\_n14A-n30A  CA\_n14A-n66A  CA\_n14A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | n14 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n14 | n14 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n30 | n30 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n14A-n30A-n66(2A)-n77(2A) | n775,6  CA\_n14A-n30A  CA\_n14A-n66A  CA\_n14A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | n14 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n18A-n28A-n41A-n77A | n415  n775  CA\_n18A-n28A  CA\_n18A-n41A5  CA\_n18A-n77A5  CA\_n28A-n41A5  CA\_n28A-n77A5  CA\_n41A-n77A5 | n18 | 5, 10, 15 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n18 | n18 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |
| CA\_n20A-n41A-n71A-n78A | CA\_n20A-n41A  CA\_n20A-n71A  CA\_n20A-n78A  CA\_n41A-n71A  CA\_n41A-n78A  CA\_n71A-n78A | n20 | 5, 10,15, 20 | 0 |
|  |  | n41 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50, 60, 70, 80, 90, 100 |  |
|  |  | n71 | 5, 10,15, 20, 25, 30, 35 |  |
|  |  | n78 | 10,15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25A-n29A-n66A-n77A | CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n29 | n29 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n29A-n66A-n77(2A) | CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A  CA\_n77(2A) | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n29 | n29 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n25A-n29A-n66A-n77(3A) | CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A  CA\_n77(2A) | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n29 | n29 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(3A)\_BCS4 and 5 |  |
| CA\_n25A-n38A-n66A-n78A | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25(2A)-n38A-n66A-n78A | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25A-n38A-n66(2A)-n78A | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25A-n38A-n66A-n78(2A) | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25(2A)-n38A-n66(2A)-n78A | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25(2A)-n38A-n66A-n78(2A) | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25A-n38A-n66(2A)-n78(2A) | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25(2A)-n38A-n66(2A)-n78(2A) | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25A-n41A-n66A-n71A | - | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | n255  n415,6  n665  n715  CA\_n25A-n41A5  CA\_n25A-n66A5  CA\_n25A-n71A5  CA\_n41A-n66A5  CA\_n41A-n71A5  CA\_n66A-n71A5 | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(A-C)-n66A-n71A | n255  n415,6  n665  n715  CA\_n25A-n41A5  CA\_n25A-n41C  CA\_n25A-n66A5  CA\_n25A-n71A5  CA\_n41A-n66A5  CA\_n41C-n66A  CA\_n41A-n71A5  CA\_n41C-n71A  CA\_n41C5  CA\_n66A-n71A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(A-C)\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n66(2A)-n71A | n255  n415,6  n665  n715  CA\_n25A-n41A5  CA\_n25A-n66A5  CA\_n25A-n71A5  CA\_n41A-n66A5  CA\_n41A-n71A5  CA\_n66A-n71A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n66(2A)-n71(2A) | n415,6  CA\_n25A-n41A5 CA\_n25A-n66A CA\_n25A-n71A CA\_n41A-n66A5 CA\_n41A-n71A5 CA\_n66A-n71A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
| CA\_n25A-n41A-n66(2A)-n71B | n415,6  CA\_n25A-n41A5 CA\_n25A-n66A CA\_n25A-n71A CA\_n41A-n66A5 CA\_n41A-n71A5 CA\_n66A-n71A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n25A-n41A-n66A-n71(2A) | n255  n415,6  n665  n715  CA\_n25A-n41A5  CA\_n25A-n66A5  CA\_n25A-n71A5  CA\_n41A-n66A5  CA\_n41A-n71A5  CA\_n66A-n71A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
| CA\_n25A-n41A-n66A-n71B | n255  n415,6  n665  n715  CA\_n25A-n41A5  CA\_n25A-n66A5  CA\_n25A-n71A5  CA\_n41A-n66A5  CA\_n41A-n71A5  CA\_n66A-n71A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n25A-n41(2A)-n66A-n71A | - | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | n255  n415,6  n665  n715  CA\_n25A-n41A5  CA\_n25A-n66A5  CA\_n25A-n71A5  CA\_n41A-n66A5  CA\_n41A-n71A5  CA\_n66A-n71A5 | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A)\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(2A)-n66A-n71(2A) | n255  n415,6  n665  n715  CA\_n25A-n41A5  CA\_n25A-n66A5  CA\_n25A-n71A5  CA\_n41A-n66A5  CA\_n41A-n71A5  CA\_n66A-n71A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A)\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
| CA\_n25A-n41(2A)-n66A-n71B | n255  n415,6  n665  n715  CA\_n25A-n41A5  CA\_n25A-n66A5  CA\_n25A-n71A5  CA\_n41A-n66A5  CA\_n41A-n71A5  CA\_n66A-n71A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A)\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n25A-n41(2A)-n66(2A)-n71A | n255  n415,6  n665  n715  CA\_n25A-n41A5  CA\_n25A-n66A5  CA\_n25A-n71A5  CA\_n41A-n66A5  CA\_n41A-n71A5  CA\_n66A-n71A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A)\_BCS 4 and 5 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41C-n66A-n71A | - | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | CA\_n41C\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | n255  n415,6  n665  n715  CA\_n25A-n41A5  CA\_n25A-n41C  CA\_n25A-n66A5  CA\_n25A-n71A5  CA\_n41A-n66A5  CA\_n41C-n66A  CA\_n41A-n71A5  CA\_n41C-n71A  CA\_n41C5  CA\_n66A-n71A5 | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | CA\_n41C\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41C-n66A-n71(2A) | n255  n415,6  n665  n715  CA\_n25A-n41A5  CA\_n25A-n41C  CA\_n25A-n66A5  CA\_n25A-n71A5  CA\_n41A-n66A5  CA\_n41C-n66A  CA\_n41A-n71A5  CA\_n41C-n71A  CA\_n41C5  CA\_n66A-n71A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
| CA\_n25A-n41C-n66A-n71B | n255  n415,6  n665  n715  CA\_n25A-n41A5  CA\_n25A-n41C  CA\_n25A-n66A5  CA\_n25A-n71A5  CA\_n41A-n66A5  CA\_n41C-n66A  CA\_n41A-n71A5  CA\_n41C-n71A  CA\_n41C5  CA\_n66A-n71A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n25A-n41C-n66(2A)-n71A | n255  n415,6  n665  n715  CA\_n25A-n41A5  CA\_n25A-n41C  CA\_n25A-n66A5  CA\_n25A-n71A5  CA\_n41A-n66A5  CA\_n41C-n66A  CA\_n41A-n71A5  CA\_n41C-n71A  CA\_n41C5  CA\_n66A-n71A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41A-n66A-n71A | n255  n415,6  n665  n715  CA\_n25A-n41A5  CA\_n25A-n66A5  CA\_n25A-n71A5  CA\_n41A-n66A5  CA\_n41A-n71A5  CA\_n66A-n71A5 | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41A-n66A-n71(2A) | n415,6  CA\_n25A-n41A5 CA\_n25A-n66A CA\_n25A-n71A CA\_n41A-n66A5 CA\_n41A-n71A5 CA\_n66A-n71A | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
| CA\_n25(2A)-n41A-n66A-n71B | n415,6  CA\_n25A-n41A5 CA\_n25A-n66A CA\_n25A-n71A CA\_n41A-n66A5 CA\_n41A-n71A5 CA\_n66A-n71A | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n25(2A)-n41A-n66(2A)-n71A | n415,6  CA\_n25A-n41A5 CA\_n25A-n66A CA\_n25A-n71A CA\_n41A-n66A5 CA\_n41A-n71A5 CA\_n66A-n71A | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41(2A)-n66A-n71A | n255  n415,6  n665  n715  CA\_n25A-n41A5  CA\_n25A-n66A5  CA\_n25A-n71A5  CA\_n41A-n66A5  CA\_n41A-n71A5  CA\_n66A-n71A5 | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(2A)\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41C-n66A-n71A | n255  n415,6  n665  n715  CA\_n25A-n41A5  CA\_n25A-n41C  CA\_n25A-n66A5  CA\_n25A-n71A5  CA\_n41A-n66A5  CA\_n41C-n66A  CA\_n41A-n71A5  CA\_n41C-n71A  CA\_n41C5  CA\_n66A-n71A5 | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(3A)-n66A-n71A | n255  n415,6  n665  n715  CA\_n25A-n41A5 CA\_n25A-n66A5 CA\_n25A-n71A5 CA\_n41A-n66A5 CA\_n41A-n71A5 CA\_n66A-n71A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(3A)\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n66A-n77A | n255  n415,6  n665  n775,6  CA\_n25A-n41A5  CA\_n25A-n66A5  CA\_n25A-n77A5  CA\_n41A-n66A5  CA\_n41A-n77A5,6  CA\_n66A-n77A5 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(A-C)-n66A-n77A | n415,6  n775,6  CA\_n25A-n41A5  CA\_n25A-n41C  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n41C5  CA\_n41A-n66A5  CA\_n41C-n66A  CA\_n41A-n77A5  CA\_n41C-n77A  CA\_n66A-n77A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(A-C)\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41C-n66A-n77A | n255  n415,6  n665  n775,6  CA\_n25A-n41A5  CA\_n25A-n41C  CA\_n25A-n66A5  CA\_n25A-n77A5  CA\_n41A-n66A5  CA\_n41A-n77A5  CA\_n41C5  CA\_n41C-n66A  CA\_n41C-n77A  CA\_n66A-n77A5 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | CA\_n41C\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41C-n66A-n77(2A) | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n41C  CA\_n41A-n66A  CA\_n41A-n77A  CA\_n66A-n77A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n25A-n41C-n66(2A)-n77A | n255  n415,6  n665  n775,6  CA\_n25A-n41A5 CA\_n25A-n41C  CA\_n25A-n66A5 CA\_n25A-n77A5 CA\_n41A-n66A5 CA\_n41C-n66A  CA\_n41A-n77A5 CA\_n41C-n77A  CA\_n41C5 CA\_n66A-n77A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(2A)-n66A-n77A | n255  n415,6  n665  n775,6  CA\_n25A-n41A5  CA\_n25A-n66A5  CA\_n25A-n77A5  CA\_n41A-n66A5  CA\_n41A-n77A5  CA\_n66A-n77A5 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A)\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(2A)-n66A-n77(2A) | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n41A-n66A  CA\_n41A-n77A  CA\_n66A-n77A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A)\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n25A-n41(3A)-n66A-n77A | n415,6  n775,6  CA\_n25A-n41A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n41A-n66A5  CA\_n41A-n77A5  CA\_n66A-n77A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(3A)\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n66(2A)-n77A | n255  n415,6  n665  n775,6  CA\_n25A-n41A5  CA\_n25A-n66A5  CA\_n25A-n77A5  CA\_n41A-n66A5  CA\_n41A-n77A5  CA\_n66A-n77A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n66A-n77(2A) | n415,6  n775,6  CA\_n25A-n41A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n41A-n66A5  CA\_n41A-n77A5  CA\_n66A-n77A5 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n25A-n41A-n66(2A)-n77(2A) | n415,6  n775,6  CA\_n25A-n41A5 CA\_n25A-n66A CA\_n25A-n77A5 CA\_n41A-n66A5 CA\_n41A-n77A5 CA\_n66A-n77A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n25A-n41(2A)-n66(2A)-n77A | n255  n415,6  n665  n775,6  CA\_n25A-n41A5 CA\_n25A-n66A5 CA\_n25A-n77A5 CA\_n41A-n66A5 CA\_n41A-n77A5 CA\_n66A-n77A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A)\_BCS 4 and 5 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41A-n66A-n77A | n255  n415,6  n665  n775,6  CA\_n25A-n41A5  CA\_n25A-n66A5  CA\_n25A-n77A5  CA\_n41A-n66A5  CA\_n41A-n77A5  CA\_n66A-n77A5 | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41A-n66A-n77(2A) | n415,6  n775,6  CA\_n25A-n41A5 CA\_n25A-n66A CA\_n25A-n77A5 CA\_n41A-n66A5 CA\_n41A-n77A5 CA\_n66A-n77A5 | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n25(2A)-n41A-n66(2A)-n77A | n255  n415,6  n665  n775,6  CA\_n25A-n41A5  CA\_n25A-n66A5  CA\_n25A-n77A5  CA\_n41A-n66A5  CA\_n41A-n77A5  CA\_n66A-n77A5 | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41C-n66A-n77A | n255  n415,6  n665  n775,6  CA\_n25A-n41A5 CA\_n25A-n41C  CA\_n25A-n66A5 CA\_n25A-n77A5 CA\_n41A-n66A5 CA\_n41C-n66A  CA\_n41A-n77A5 CA\_n41C-n77A  CA\_n66A-n77A5  CA\_n41C5 | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41(2A)-n66A-n77A | n255  n415,6  n665  n775,6  CA\_n25A-n41A5 CA\_n25A-n66A5 CA\_n25A-n77A5 CA\_n41A-n66A5 CA\_n41A-n77A5 CA\_n66A-n77A5 | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(2A)\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n66A-n78A | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n41A-n66A  CA\_n41A-n78A  CA\_n66A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25A-n41A-n66A-n78(2A) | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n41A-n66A  CA\_n41A-n78A  CA\_n66A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25A-n41A-n66A-n85A | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n25A-n85A  CA\_n41A-n66A  CA\_n41A-n85A  CA\_n66A-n85A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n71A-n77A | n255  n415,6  n715  n775,6  CA\_n25A-n41A5  CA\_n25A-n71A5  CA\_n25A-n77A5  CA\_n41A-n71A5  CA\_n41A-n77A5,6  CA\_n71A-n77A5 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n71A-n77(2A) | n415,6  n775,6  CA\_n25A-n41A5  CA\_n25A-n71A  CA\_n25A-n77A5  CA\_n41A-n71A5  CA\_n41A-n77A5  CA\_n71A-n77A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n25A-n41A-n71B-n77A | n255  n415,6  n715  n775,6  CA\_n25A-n41A5  CA\_n25A-n71A5  CA\_n25A-n77A5  CA\_n41A-n71A5  CA\_n41A-n77A5  CA\_n71A-n77A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n71B-n77(2A) | n415,6  n775,6  CA\_n25A-n41A5 CA\_n25A-n71A CA\_n25A-n77A5 CA\_n41A-n71A5 CA\_n41A-n77A5 CA\_n71A-n77A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n25A-n41A-n71(2A)-n77A | n255  n415,6  n715  n775,6  CA\_n25A-n41A5  CA\_n25A-n71A5  CA\_n25A-n77A5  CA\_n41A-n71A5  CA\_n41A-n77A5  CA\_n71A-n77A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n71(2A)-n77(2A) | n415,6  n775,6  CA\_n25A-n41A5 CA\_n25A-n71A CA\_n25A-n77A5 CA\_n41A-n71A5 CA\_n41A-n77A5 CA\_n71A-n77A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n25A-n41(A-C)-n71A-n77A | n415,6  n775,6  CA\_n25A-n41A5  CA\_n25A-n41C  CA\_n25A-n71A  CA\_n25A-n77A5  CA\_n41C5  CA\_n41A-n71A5  CA\_n41C-n71A  CA\_n41A-n77A5  CA\_n41C-n77A  CA\_n71A-n77A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(A-C)\_BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41C-n71A-n77A | n255  n415,6  n715  n775,6  CA\_n25A-n41A5  CA\_n25A-n41C  CA\_n25A-n71A5  CA\_n25A-n77A5  CA\_n41A-n71A5  CA\_n41A-n77A5  CA\_n41C5  CA\_n41C-n71A  CA\_n41C-n77A  CA\_n71A-n77A5 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | CA\_n41C\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41C-n71A-n77(2A) | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n25A-n77A  CA\_n41C  CA\_n41A-n71A  CA\_n41A-n77A  CA\_n71A-n77A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n25A-n41C-n71B-n77A | n255  n415,6  n715  n775,6  CA\_n25A-n41A5 CA\_n25A-n41C  CA\_n25A-n71A5 CA\_n25A-n77A5 CA\_n41A-n71A5 CA\_n41C-n71A  CA\_n41A-n77A5 CA\_n41C-n77A  CA\_n41C5 CA\_n71A-n77A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41C-n71(2A)-n77A | n255  n415,6  n715  n775,6  CA\_n25A-n41A5 CA\_n25A-n41C  CA\_n25A-n71A5 CA\_n25A-n77A5 CA\_n41A-n71A5 CA\_n41C-n71A  CA\_n41A-n77A5 CA\_n41C-n77A  CA\_n41C5 CA\_n71A-n77A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(2A)-n71A-n77A | n255  n415,6  n715  n775,6  CA\_n25A-n41A5  CA\_n25A-n71A5  CA\_n25A-n77A5  CA\_n41A-n71A5  CA\_n41A-n77A5  CA\_n71A-n77A5 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A)\_BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(2A)-n71A-n77(2A) | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n25A-n77A  CA\_n41A-n71A  CA\_n41A-n77A  CA\_n71A-n77A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A)\_BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n25A-n41(3A)-n71A-n77A | n415,6  n775,6  CA\_n25A-n41A5  CA\_n25A-n71A  CA\_n25A-n77A5  CA\_n41A-n71A5  CA\_n41A-n77A5  CA\_n71A-n77A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(3A)\_BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(2A)-n71B-n77A | n255  n415,6  n715  n775,6  CA\_n25A-n41A5 CA\_n25A-n71A5 CA\_n25A-n77A5 CA\_n41A-n71A5 CA\_n41A-n77A5 CA\_n71A-n77A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A)\_BCS 4 and 5 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(2A)-n71(2A)-n77A | n255  n415,6  n715  n775,6  CA\_n25A-n41A5 CA\_n25A-n71A5 CA\_n25A-n77A5 CA\_n41A-n71A5 CA\_n41A-n77A5 CA\_n71A-n77A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A)\_BCS 4 and 5 |  |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41A-n71A-n77A | n255  n415,6  n715  n775,6  CA\_n25A-n41A5  CA\_n25A-n71A5  CA\_n25A-n77A5  CA\_n41A-n71A5  CA\_n41A-n77A5  CA\_n71A-n77A5 | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41A-n71(2A)-n77A | n255  n415,6  n715  n775,6  CA\_n25A-n41A5  CA\_n25A-n71A5  CA\_n25A-n77A5  CA\_n41A-n71A5  CA\_n41A-n77A5  CA\_n71A-n77A5 | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41A-n71B-n77A | n255  n415,6  n715  n775,6  CA\_n25A-n41A5  CA\_n25A-n71A5  CA\_n25A-n77A5  CA\_n41A-n71A5  CA\_n41A-n77A5  CA\_n71A-n77A5 | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41A-n71A-n77(2A) | n415,6  n775,6  CA\_n25A-n41A5 CA\_n25A-n71A CA\_n25A-n77A5 CA\_n41A-n71A5 CA\_n41A-n77A5 CA\_n71A-n77A5 | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n25(2A)-n41C-n71A-n77A | n255  n415,6  n715  n775,6  CA\_n25A-n41A5 CA\_n25A-n41C  CA\_n25A-n71A5 CA\_n25A-n77A5 CA\_n41A-n71A5 CA\_n41C-n71A  CA\_n41A-n77A5 CA\_n41C-n77C  CA\_n71A-n77A5  CA\_n41C5 | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41(2A)-n71A-n77A | n255  n415,6  n715  n775,6  CA\_n25A-n41A5 CA\_n25A-n71A5 CA\_n25A-n77A5 CA\_n41A-n71A5 CA\_n41A-n77A5 CA\_n71A-n77A5 | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(2A)\_BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n71A-n78A | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n25A-n78A  CA\_n41A-n71A  CA\_n41A-n78A  CA\_n71A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25A-n41A-n71A-n85A | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n25A-n85A  CA\_n41A-n71A  CA\_n41A-n85A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n77A-n85A | CA\_n25A-n41A CA\_n25A-n77A CA\_n25A-n85A CA\_n41A-n77A CA\_n41A-n85A CA\_n77A-n85A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n66A-n71A-n77A | n255  n665  n715  n775,6  CA\_n25A-n66A5  CA\_n25A-n71A5  CA\_n25A-n77A5  CA\_n66A-n71A5  CA\_n66A-n77A5  CA\_n71A-n77A5 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n66(2A)-n71A-n77A | n255  n665  n715  n775,6  CA\_n25A-n66A5  CA\_n25A-n71A5  CA\_n25A-n77A5  CA\_n66A-n71A5  CA\_n66A-n77A5  CA\_n71A-n77A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n66(2A)-n71A-n77(2A) | n775,6  CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n77A5  CA\_n66A-n71A  CA\_n66A-n77A5  CA\_n71A-n77A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n25A-n66A-n71B-n77A | n255  n665  n715  n775,6  CA\_n25A-n66A5  CA\_n25A-n71A5  CA\_n25A-n77A5  CA\_n66A-n71A5  CA\_n66A-n77A5  CA\_n71A-n77A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n66A-n71(2A)-n77A | n255  n665  n715  n775,6  CA\_n25A-n66A5  CA\_n25A-n71A5  CA\_n25A-n77A5  CA\_n66A-n71A5  CA\_n66A-n77A5  CA\_n71A-n77A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n66A-n71A-n77(2A) | n775,6  CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n77A5  CA\_n66A-n71A  CA\_n66A-n77A5  CA\_n71A-n77A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n25A-n66A-n71A-n77(3A) | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n77A  CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20, 25, 30, 35 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(3A)\_BCS 4 and 5 |  |
| CA\_n25A-n66A-n71(2A)-n77(2A) | n775,6  CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n77A5  CA\_n66A-n71A  CA\_n66A-n77A5  CA\_n71A-n77A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n25A-n66A-n71B-n77(2A) | n775,6  CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n77A5  CA\_n66A-n71A  CA\_n66A-n77A5  CA\_n71A-n77A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n25A-n66(2A)-n71(2A)-n77A | n775,6  CA\_n25A-n66A CA\_n25A-n71A CA\_n25A-n77A5 CA\_n66A-n71A CA\_n66A-n77A5 CA\_n71A-n77A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n66(2A)-n71B-n77A | n775,6  CA\_n25A-n66A CA\_n25A-n71A CA\_n25A-n77A5 CA\_n66A-n71A CA\_n66A-n77A5 CA\_n71A-n77A5 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n66A-n71A-n77A | n255  n665  n715  n775,6  CA\_n25A-n66A5  CA\_n25A-n71A5  CA\_n25A-n77A5  CA\_n66A-n71A5  CA\_n66A-n77A5  CA\_n71A-n77A5 | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n66A-n71A-n77(2A) | n775,6  CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n77A5  CA\_n66A-n71A  CA\_n66A-n77A5  CA\_n71A-n77A5 | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n25(2A)-n66A-n71(2A)-n77A | n775,6  CA\_n25A-n66A CA\_n25A-n71A CA\_n25A-n77A5 CA\_n66A-n71A CA\_n66A-n77A5 CA\_n71A-n77A5 | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n66A-n71B-n77A | n775,6  CA\_n25A-n66A CA\_n25A-n71A CA\_n25A-n77A5 CA\_n66A-n71A CA\_n66A-n77A5 CA\_n71A-n77A5 | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n66(2A)-n71A-n77A | n775,6  CA\_n25A-n66A CA\_n25A-n71A CA\_n25A-n77A5 CA\_n66A-n71A CA\_n66A-n77A5 CA\_n71A-n77A5 | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n66A-n71A-n78A | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n78A  CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25A-n66(2A)-n71A-n78A | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n78A  CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25A-n66A-n71A-n78(2A) | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n78A  CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25A-n66(2A)-n71A-n78(2A) | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n78A  CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25A-n66A-n71A-n85A | CA\_n25A-n66A CA\_n25A-n71A CA\_n25A-n85A CA\_n66A-n71A CA\_n66A-n85A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n66A-n77A-n85A | CA\_n25A-n66A  CA\_n25A-n77A  CA\_n25A-n85A  CA\_n66A-n77A  CA\_n66A-n85A  CA\_n77A-n85A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n28A-n40A-n71A-n77A | CA\_n28A-n40A  CA\_n28A-n77A  CA\_n40A-n71A  CA\_n40A-n77A  CA\_n71A-n77A | n28 | n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n28A-n40A-n78A-n79A | CA\_n28A-n40A  CA\_n28A-n78A  CA\_n28A-n79A  CA\_n40A-n78A  CA\_n40A-n79A  CA\_n78A-n79A | n28 | n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n28A-n41A-n75A-n78A | - | n28 | 5,10, 15, 20, 25,30 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n75 | 5,10, 15, 20, 25,30,40,50 |  |
|  |  | n78 | 10, 15, 20, 25,30,40, 50, 60,70, 80, 90, 100 |  |
| CA\_n28A-n41A-n77A-n79A | n415,6  n775,6  n795,6  CA\_n28A-n41A5  CA\_n28A-n77A5  CA\_n28A-n79A5  CA\_n41A-n77A5  CA\_n41A-n79A5  CA\_n77A-n79A5 | n28 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n28A-n41A-n77(2A)-n79A | CA\_n28A-n41A  CA\_n28A-n77A  CA\_n28A-n79A  CA\_n41A-n77A  CA\_n41A-n79A  CA\_n77A-n79A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n29A-n30A-n66A-n77A | n775,6  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | n29 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n29A-n30A-n66(2A)-n77A | n775,6  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | n29 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n29A-n30A-n66A-n77(2A) | n775,6  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | n29 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n29A-n30A-n66(2A)-n77(2A) | n775,6  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | n29 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n29A-n66A-n70A-n71A | n665  n705  n715  CA\_n66A-n71A  CA\_n70A-n71A | n29 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | CA\_n66A-n71A  CA\_n70A-n71A | n29 | n29 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n70 | n70 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n29A-n66(2A)-n70A-n71A | n665  n705  n715  CA\_n66A-n71A  CA\_n70A-n71A | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | CA\_n66A-n71A  CA\_n70A-n71A | n29 | n29 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n70 | n70 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n29A-n66A-n70A-n71(2A) | CA\_n66A-n71A CA\_n70A-n71A | n29 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 35, 40 |  |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
| CA\_n41A-n66A-n70A-n78A | CA\_n41A-n66A  CA\_n41A-n70A  CA\_n41A-n78A  CA\_n66A-n78A  CA\_n70A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 10, 15, 20, 25, 30, 40 |  |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n41A-n66A-n71A-n77A | n415,6  n665  n715  n775,6  CA\_n41A-n66A5  CA\_n41A-n71A5  CA\_n41A-n77A5,6  CA\_n66A-n71A5  CA\_n66A-n77A5  CA\_n71A-n77A5 | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n66A-n71B-n77A | n415,6  n665  n715  n775,6  CA\_n41A-n66A5  CA\_n41A-n71A5  CA\_n41A-n77A5  CA\_n66A-n71A5  CA\_n66A-n77A5  CA\_n71A-n77A5 | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n66A-n71B-n77(2A) | n415,6  n775,6  CA\_n41A-n66A5  CA\_n41A-n71A5  CA\_n41A-n77A5  CA\_n66A-n71A  CA\_n66A-n77A5  CA\_n71A-n77A5 | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n41A-n66A-n71(2A)-n77A | n415,6  n665  n715  n775,6  CA\_n41A-n66A5  CA\_n41A-n71A5  CA\_n41A-n77A5  CA\_n66A-n71A5  CA\_n66A-n77A5  CA\_n71A-n77A5 | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n66A-n71(2A)-n77(2A) | n415,6  n775,6  CA\_n41A-n66A5 CA\_n41A-n71A5 CA\_n41A-n77A5 CA\_n66A-n71A CA\_n66A-n77A5 CA\_n71A-n77A5 | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n41A-n66(2A)-n71A-n77(2A) | n415,6  n775,6  CA\_n41A-n66A5 CA\_n41A-n71A5 CA\_n41A-n77A5 CA\_n66A-n71A CA\_n66A-n77A5 CA\_n71A-n77A5 | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n41(A-C)-n66A-n71A-n77A | n415,6  n775,6  CA\_n41C5  CA\_n41A-n66A5  CA\_n41C-n66A  CA\_n41A-n71A5  CA\_n41C-n71A  CA\_n41A-n77A5  CA\_n41C-n77A  CA\_n66A-n71A  CA\_n66A-n77A5  CA\_n71A-n77A5 | n41 | CA\_n41(A-C)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n66A-n71A-n77A | n415,6  n665  n715  n775,6  CA\_n41A-n66A5  CA\_n41A-n71A5  CA\_n41A-n77A5  CA\_n41C5  CA\_n41C-n66A  CA\_n41C-n71A  CA\_n41C-n77A  CA\_n66A-n71A5  CA\_n66A-n77A5  CA\_n71A-n77A5 | n41 | CA\_n41C\_BCS1 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n66A-n71A-n77(2A) | CA\_n41C  CA\_n41A-n66A  CA\_n41A-n71A  CA\_n41A-n77A  CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n41 | CA\_n41C\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n41C-n66A-n71B-n77A | n415,6  n665  n715  n775,6  CA\_n41C5  CA\_n41A-n66A5 CA\_n41C-n66A  CA\_n41A-n71A5 CA\_n41C-n71A  CA\_n41A-n77A5 CA\_n41C-n77A  CA\_n66A-n71A5 CA\_n66A-n77A5 CA\_n71A-n77A5 | n41 | CA\_n41C\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n66A-n71(2A)-n77A | n415,6  n665  n715  n775,6  CA\_n41C5  CA\_n41A-n66A5 CA\_n41C-n66A  CA\_n41A-n71A5 CA\_n41C-n71A  CA\_n41A-n77A5 CA\_n41C-n77A  CA\_n66A-n71A5 CA\_n66A-n77A5 CA\_n71A-n77A5 | n41 | CA\_n41C\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n66(2A)-n71A-n77A | n415,6  n665  n715  n775,6  CA\_n41C5  CA\_n41A-n66A5 CA\_n41C-n66A  CA\_n41A-n71A5 CA\_n41C-n71A  CA\_n41A-n77A5 CA\_n41C-n77A  CA\_n66A-n71A5 CA\_n66A-n77A5 CA\_n71A-n77A5 | n41 | CA\_n41C\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n66A-n71A-n77(2A) | CA\_n41A-n66A  CA\_n41A-n71A  CA\_n41A-n77A  CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n41 | CA\_n41(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n41(3A)-n66A-n71A-n77A | n415,6  n775,6  CA\_n41A-n66A5  CA\_n41A-n71A5  CA\_n41A-n77A5  CA\_n66A-n71A  CA\_n66A-n77A5  CA\_n71A-n77A5 | n41 | CA\_n41(3A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n66A-n71A-n77A | n415,6  n665  n715  n775,6  CA\_n41A-n66A5  CA\_n41A-n71A5  CA\_n41A-n77A5  CA\_n66A-n71A5  CA\_n66A-n77A5  CA\_n71A-n77A5 | n41 | CA\_n41(2A)\_BCS1 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | CA\_n41(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n66A-n71B-n77A | n415,6  n66A5  n71A5  n775,6  CA\_n41A-n66A5 CA\_n41A-n71A5 CA\_n41A-n77A5 CA\_n66A-n71A5 CA\_n66A-n77A5 CA\_n71A-n77A5 | n41 | CA\_n41(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n66A-n71(2A)-n77A | n415,6  n665  n715  n775,6  CA\_n41A-n66A5 CA\_n41A-n71A5 CA\_n41A-n77A5 CA\_n66A-n71A5 CA\_n66A-n77A5 CA\_n71A-n77A5 | n41 | CA\_n41(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n66(2A)-n71A-n77A | n415,6  n665  n715  n775,6  CA\_n41A-n66A5 CA\_n41A-n71A5 CA\_n41A-n77A5 CA\_n66A-n71A5 CA\_n66A-n77A5 CA\_n71A-n77A5 | n41 | CA\_n41(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n66(2A)-n71A-n77A | n415,6  n665  n715  n775,6  CA\_n41A-n66A5  CA\_n41A-n71A5  CA\_n41A-n77A5  CA\_n66A-n71A5  CA\_n66A-n77A5  CA\_n71A-n77A5 | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n66(2A)-n71(2A)-n77A | n415,6  n66A5  n71A5  n775,6  CA\_n41A-n66A5  CA\_n41A-n71A5  CA\_n41A-n77A5  CA\_n66A-n71A5  CA\_n66A-n77A5  CA\_n71A-n77A5 | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n66(2A)-n71B-n77A | n415,6  n665  n715  n775,6  CA\_n41A-n66A5  CA\_n41A-n71A5  CA\_n41A-n77A5  CA\_n66A-n71A5  CA\_n66A-n77A5  CA\_n71A-n77A5 | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n66A-n71A-n77(2A) | n415,6  n775,6  CA\_n41A-n66A5  CA\_n41A-n77A5  CA\_n41A-n71A5  CA\_n66A-n71A  CA\_n66A-n77A5  CA\_n71A-n77A5 | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n41A-n66A-n71A-n78A | CA\_n41A-n66A  CA\_n41A-n71A  CA\_n41A-n78A  CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n41A-n66(2A)-n71A-n78A | CA\_n41A-n66A  CA\_n41A-n71A  CA\_n41A-n78A  CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n41A-n66A-n71A-n78(2A) | CA\_n41A-n66A  CA\_n41A-n71A  CA\_n41A-n78A  CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n41A-n66(2A)-n71A-n78(2A) | CA\_n41A-n66A  CA\_n41A-n71A  CA\_n41A-n78A  CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n41A-n66A-n71A-n85A | CA\_n41A-n66A  CA\_n41A-n71A  CA\_n41A-n85A  CA\_n66A-n71A  CA\_n66A-n85A | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n66A-n77A-n85A | CA\_n41A-n66A CA\_n41A-n77A CA\_n41A-n85A CA\_n66A-n77A CA\_n66A-n85A CA\_n77A-n85A | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n48A-n66A-n70A-n71A | CA\_n48A-n66A CA\_n48A-n70A CA\_n48A-n71A CA\_n66A-n71A CA\_n70A-n71A | n48 | 5, 10, 15, 20, 30, 40, 508, 608, 708, 808, 908, 1008 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 35, 40 |  |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48A-n66A-n70A-n77A | CA\_n48A-n66A CA\_n48A-n70A CA\_n66A-n77A CA\_n70A-n77A | n48 | 5, 10, 15, 20, 30, 40, 508, 608, 708, 808, 908, 1008 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 35, 40 |  |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48A-n66(2A)-n70A-n77A | CA\_n48A-n66A  CA\_n48A-n70A  CA\_n66A-n77A  CA\_n70A-n77A | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48(2A)-n66(2A)-n70A-n77A | CA\_n48A-n66A CA\_n48A-n70A CA\_n66A-n77A CA\_n70A-n77A | n48 | CA\_n48(2A)\_BCS1 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48A-n66(3A)-n70A-n77A | CA\_n48A-n66A CA\_n48A-n70A CA\_n66A-n77A CA\_n70A-n77A | n48 | 5, 10, 15, 20, 30, 40, 508, 608, 708, 808, 908, 1008 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48(2A)-n66A-n70A-n77A | CA\_n48A-n66A  CA\_n48A-n70A  CA\_n66A-n77A  CA\_n70A-n77A | n48 | CA\_n48(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 35, 40 |  |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48(3A)-n66A-n70A-n77A | CA\_n48A-n66A CA\_n48A-n70A CA\_n66A-n77A CA\_n70A-n77A | n48 | CA\_n48(3A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 35, 40 |  |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48A-n66A-n71A-n77A | CA\_n48A-n66A CA\_n48A-n71A CA\_n66A-n71A CA\_n66A-n77A CA\_n71A-n77A | n48 | 5, 10, 15, 20, 30, 40, 508, 608, 708, 808, 908, 1008 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 35, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48(2A)-n66A-n71A-n77A | CA\_n48A-n66A CA\_n48A-n71A CA\_n66A-n71A CA\_n66A-n77A CA\_n71A-n77A | n48 | CA\_n48(2A)\_BCS1 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 35, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48(2A)-n66A-n71(2A)-n77A | CA\_n48A-n66A CA\_n48A-n71A CA\_n66A-n71A CA\_n66A-n77A CA\_n71A-n77A | n48 | CA\_n48(2A)\_BCS1 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 35, 40 |  |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48A-n66(2A)-n71A-n77A | CA\_n48A-n66A CA\_n48A-n71A CA\_n66A-n71A CA\_n66A-n77A CA\_n71A-n77A | n48 | 5, 10, 15, 20, 30, 40, 508, 608, 708, 808, 908, 1008 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 508, 608, 708, 808, 908, 1008 | 1 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48A-n66(3A)-n71A-n77A | CA\_n48A-n66A CA\_n48A-n71A CA\_n66A-n71A CA\_n66A-n77A CA\_n71A-n77A | n48 | 5, 10, 15, 20, 30, 40, 508, 608, 708, 808, 908, 1008 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48A-n66A-n71(2A)-n77A | CA\_n48A-n66A CA\_n48A-n71A CA\_n66A-n71A CA\_n66A-n77A CA\_n71A-n77A | n48 | 5, 10, 15, 20, 30, 40, 508, 608, 708, 808, 908, 1008 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 35, 40 |  |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48A-n70A-n71A-n77A | CA\_n48A-n70A CA\_n48A-n71A CA\_n70A-n71A CA\_n70A-n77A CA\_n71A-n77A | n48 | 5, 10, 15, 20, 30, 40, 508, 608, 708, 808, 908, 1008 | 0 |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48(2A)-n70A-n71A-n77A | CA\_n48A-n70A CA\_n48A-n71A CA\_n70A-n71A CA\_n70A-n77A CA\_n71A-n77A | n48 | CA\_n48(2A)\_BCS1 | 0 |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48A-n70A-n71(2A)-n77A | CA\_n48A-n70A CA\_n48A-n71A CA\_n70A-n71A CA\_n70A-n77A CA\_n71A-n77A | n48 | 5, 10, 15, 20, 30, 40, 508, 608, 708, 808, 908, 1008 | 0 |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48(2A)-n70A-n71(2A)-n77A | CA\_n48A-n70A CA\_n48A-n71A CA\_n70A-n71A CA\_n70A-n77A CA\_n71A-n77A | n48 | CA\_n48(2A)\_BCS1 | 0 |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n66A-n70A-n71A-n77A | CA\_n66A-n71A CA\_n66A-n77A CA\_n70A-n71A CA\_n70A-n77A CA\_n71A-n77A | n66 | 5, 10, 15, 20, 25, 30, 35, 40 | 0 |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |

The following notes are applied to the above tables.

NOTE 1: This UE channel bandwidth is optional in this release of the specification.

NOTE 2: For the 20 MHz bandwidth, the minimum requirements are specified for NR UL carrier frequencies confined to either 713-723 MHz or 728-738 MHz. For the 30MHz bandwidth, the minimum requirements are specified for NR UL transmission bandwidth configuration confined to either 703-733 or 718-748 MHz.

NOTE 3: For each channel bandwidth of each component carrier, refer to Table 5.3.5-1 for the applicable SCSs. For a given band, not all UE channel bandwidths support the same SCSs.

NOTE 4: Only single uplink carriers with power class other than PC3 are listed.

NOTE 5: Minimum requirements for Power Class 2 are applicable for this uplink combination or single uplink carrier in this downlink/uplink combination.

NOTE 6: Minimum requirements for Power Class 1.5 are applicable for this uplink combination or single uplink carrier in this downlink/uplink combination.

NOTE 7: For a band combination which includes band n7 and n38 simultaneously, carriers in band n7 and n38 can only be configured as downlink carriers. Power imbalance between downlink carriers on Band n7 and Band n38 is assumed to be within 6dB.

NOTE 8: For this bandwidth, the minimum requirements are restricted to operation when carrier is configured as a downlink SCell part of CA configuration

<END OF CHANCE>