**3GPP TSG-RAN WG4 Meeting #116-bis R4-2514359**

**Prague, Czech Republic, 13 – 17 October 2025**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.3* | | | | | | | | |
| **DRAFT CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **-1** | **CR** |  | **rev** |  | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | draft CR 38.101-1 to add PC2 and PC1.5 2BUL CA for 3BDL combinations | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | , Verizon | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | HPUE\_NR\_CADC\_SUL\_R19 | | | | |  | ***Date:*** | | | 2025-10-13 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | B |  | | | | | ***Release:*** | | | Rel-19 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)  Rel-20 (Release 20)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | To add PC2 and PC1.5 2BUL CA | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | To add PC2 and PC1.5 2BUL CA for the following 3BDL combinations:  CA\_n2A-n5A-n77A  CA\_n2A-n48A-n77A  CA\_n2A-n66A-n77A  The MSD values are drived using look-up tables. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | New PC2 and PC1.5 UL Configurations are not included in the specification. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.5A.3.2, 7.3A.5 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | | **X** |  | Test specifications | | | | TS 38.521-1 | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

---Start of changes---

##### Table 5.5A.3.2-1a

Table 5.5A.3.2-1a: NR CA configurations and bandwidth combinations sets defined for inter-band CA (three bands)

| NR CA configuration | Uplink CA configuration  or single uplink carrier6 | NR Band | Channel bandwidth (MHz) (NOTE 3) | Bandwidth combination set |
| --- | --- | --- | --- | --- |
| CA\_n1A-n3A-n5A | CA\_n1A-n3A  CA\_n1A-n5A  CA\_n3A-n5A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n5 | 5, 10, 15, 20 |  |
| CA\_n1A-n3A-n7A | n37  n77  CA\_n1A-n3A7  CA\_n1A-n7A7  CA\_n3A-n7A7 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n1 | 5, 10, 15, 20 | 2 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n7B | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n3A-n7A  CA\_n7B | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
| CA\_n1A-n3A-n7(2A) | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n3A-n7A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n7 | CA\_n7(2A)\_BCS0 |  |
| CA\_n1A-n3(2A)-n7A | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n3A-n7A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS1 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n1A-n3(2A)-n7(2A) | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n3A-n7A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS0 |  |
|  |  | n7 | CA\_n7(2A)\_BCS0 |  |
| CA\_n1(2A)-n3A-n7A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n1A-n3B-n7A | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n3A-n7A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  | CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 1 |
|  |  | n3 | CA\_n3B\_BCS1 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
| CA\_n1(2A)-n3B-n7A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n1(2A)-n3(2A)-n7A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS1 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n1A-n3B-n7B | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n3A-n7A  CA\_n7B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  | CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 1 |
|  |  | n3 | CA\_n3B\_BCS1 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
| CA\_n1A-n3A-n8A | CA\_n1A-n3A  CA\_n1A-n8A  CA\_n3A-n8A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n8 | n8 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3(2A)-n8A | CA\_n1A-n3A  CA\_n1A-n8A  CA\_n3A-n8A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS0 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 1 |
|  |  | n3 | CA\_n3(2A)\_BCS 4 and 5 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
| CA\_n1A-n3A-n18A | CA\_n1A-n3A  CA\_n1A-n18A  CA\_n3A-n18A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n18 | 5, 10, 15 |  |
| CA\_n1A-n3A-n20A | n37  CA\_n1A-n3A7  CA\_n1A-n20A  CA\_n3A-n20A7 | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n20 | 5, 10, 15, 20 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n26A | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n3A-n26A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
| CA\_n1A-n3A-n26(2A) | CA\_n26(2A)  CA\_n1A-n3A  CA\_n1A-n26A  CA\_n3A-n26A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
| CA\_n1A-n3B-n26A | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n3A-n26A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  | CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 1 |
|  |  | n3 | CA\_n3B\_BCS1 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
| CA\_n1A-n3B-n26(2A) | CA\_n26(2A)  CA\_n1A-n3A  CA\_n1A-n26A  CA\_n3A-n26A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  | CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 1 |
|  |  | n3 | CA\_n3B\_BCS1 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
| CA\_n1A-n3A-n28A | n37 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n28 | 5, 10, 15, 202 |  |
|  | n37  CA\_n1A-n3A7  CA\_n1A-n28A  CA\_n3A-n28A7 | n1 | 5, 10, 15, 20 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 2 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 201, 301 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3B-n28A | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n3A-n28A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  | CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 1 |
|  |  | n3 | CA\_n3B\_BCS1 |  |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
| CA\_n1A-n3A-n38A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1A-n3B-n38A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1(2A)-n3A-n38A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1(2A)-n3B-n38A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1A-n3(2A)-n38A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS1 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1(2A)-n3(2A)-n38A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS1 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1A-n3A-n40A | CA\_n1A-n3A  CA\_n1A-n40A  CA\_n3A-n40A | n1 | 5, 10, 15, 20, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 30, 35, 40, 45, 50 |  |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n41A | n417,9  CA\_n1A-n3A  CA\_n1A-n41A7  CA\_n3A-n41A7 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n1A-n3A  CA\_n1A-n41A  CA\_n3A-n41A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3(2A)-n41A | CA\_n1A-n3A  CA\_n1A-n41A  CA\_n3A-n41A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS0 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n3A-n67A | CA\_n1A-n3A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n71A | CA\_n1A-n3A  CA\_n1A-n71A  CA\_n3A-n71A | n1 | 5,10,15,20,25,30,40,45,50 | 0 |
|  |  | n3 | 5,10,15,20,25,30,35,40,45,50 |  |
|  |  | n71 | 5,10,15,20 |  |
| CA\_n1A-n3(2A)-n71A | CA\_n1A-n3A  CA\_n1A-n71A  CA\_n3A-n71A | n1 | 5,10,15,20,25,30,40,45,50 | 0 |
|  |  | n3 | CA\_n3(2A)­\_BCS 4 and 5 |  |
|  |  | n71 | 5,10,15,20 |  |
| CA\_n1A-n3A-n75A | CA\_n1A-n3A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n75 | n75 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n77A | n777,9  CA\_n1A-n3A  CA\_n1A-n77A7  CA\_n3A-n77A7 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20 | 2 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35,40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n1A-n3A  CA\_n1A-n77A  CA\_n3A-n77A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n77(2A) | n777,9  CA\_n1A-n3A  CA\_n1A-n77A7  CA\_n3A-n77A7  CA\_n77(2A)7 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  | n777,9  CA\_n1A-n3A  CA\_n1A-n77A7  CA\_n3A-n77A7  CA\_n77(2A)7 | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n1A-n3A-n77(3A) | n777,9  CA\_n1A-n3A  CA\_n1A-n77A7  CA\_n3A-n77A7  CA\_n77(2A) | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
|  | n777,9  CA\_n1A-n3A  CA\_n1A-n77A7  CA\_n3A-n77A7  CA\_n77(2A) | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(3A)\_BCS4 and 5 |  |
| CA\_n1A-n3A-n78A | n37  n787,9  CA\_n1A-n3A  CA\_n1A-n78A7,13, 14  CA\_n3A-n78A7,13, 14 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20 | 2 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n78C | n787,9  CA\_n1A-n3A  CA\_n1A-n78A7  CA\_n3A-n78A7  CA\_n78C | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
|  | CA\_n1A-n3A  CA\_n1A-n78A14  CA\_n1A-n78C  CA\_n3A-n78A14  CA\_n3A-n78C  CA\_n78C | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 4 and 5 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78C\_BCS4 and 5 |  |
| CA\_n1A-n3(2A)-n78A | n787,9  CA\_n1A-n3A  CA\_n1A-n78A7  CA\_n3A-n78A7 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n1A-n3A  CA\_n1A-n78A  CA\_n3A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 4 and 5 |
|  |  | n3 | CA\_n3(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3(2A)-n78C | CA\_n1A-n3A  CA\_n1A-n78A  CA\_n1A-n78C  CA\_n3A-n78A  CA\_n3A-n78C  CA\_n78C | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 4 and 5 |
|  |  | n3 | CA\_n3(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78C\_BCS4 and 5 |  |
| CA\_n1A-n3A-n78(2A) | n37  n787,9  CA\_n1A-n3A  CA\_n1A-n78A7,13, 14  CA\_n3A-n78A7,13, 14  CA\_n78(2A)7 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n1A-n3A-n78(A-C) | n787,9  CA\_n1A-n3A  CA\_n1A-n78A7  CA\_n3A-n78A7  CA\_n78C7 | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n78 | CA\_n78(A-C)\_BCS1 |  |
| CA\_n1A-n3B-n78A | CA\_n1A-n3A  CA\_n1A-n78A14  CA\_n3A-n78A14 | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 1 |
|  |  | n3 | CA\_n3B\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3B-n78(2A) | n787,9  CA\_n1A-n3A  CA\_n1A-n78A7,14  CA\_n3A-n78A7,14 | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  | CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 1 |
|  |  | n3 | CA\_n3B\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  | CA\_n78(2A) | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | CA\_n3B\_BCS4 and 5 |  |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n1A-n3B-n78C | CA\_n78C  CA\_n1A-n3A  CA\_n1A-n78A14  CA\_n3A-n78A14 | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
|  | CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 1 |
|  |  | n3 | CA\_n3B\_BCS1 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n1A-n3A-n79A | n797,9  CA\_n1A-n3A  CA\_n1A-n79A7  CA\_n3A-n79A7 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  | CA\_n1A-n3A  CA\_n1A-n79A  CA\_n3A-n79A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1(2A)-n3A-n79A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n3A-n79C | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1(2A)-n3A-n79C | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1A-n3B-n79A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n3B-n79C | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1(2A)-n3B-n79A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1(2A)-n3B-n79C | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1A-n3(2A)-n79A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS1 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n3(2A)-n79C | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS1 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1(2A)-n3(2A)-n79A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS1 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1(2A)-n3(2A)-n79C | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS1 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1A-n3A-n105A | CA\_n1A-n3A  CA\_n1A-n105A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  | CA\_n3A-n105A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n1A-n5A-n7A | CA\_n1A-n5A  CA\_n1A-n7A  CA\_n5A-n7A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n1A-n5A-n7B | CA\_n1A-n5A  CA\_n1A-n7A  CA\_n5A-n7A  CA\_n7B | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
| CA\_n1A-n5A-n8A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
| CA\_n1A-n5A-n28A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  | CA\_n1A-n5A  CA\_n1A-n28A  CA\_n5A-n28A | n1 | See n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | See n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n28 | See n28 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n5A-n40A | CA\_n1A-n5A  CA\_n1A-n40A  CA\_n5A-n40A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 1 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n1A-n5A-n78A | CA\_n1A-n5A  CA\_n1A-n78A  CA\_n5A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 90, 100 |  |
|  |  | n1 | See n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | See n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n5A-n78(2A) | CA\_n1A-n5A  CA\_n1A-n78A  CA\_n5A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n5A-n78(A-C) | CA\_n78C  CA\_n1A-n5A  CA\_n1A-n78A  CA\_n5A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n78 | CA\_n78(A-C)\_BCS1 |  |
| CA\_n1A-n5A-n78C | CA\_n78C  CA\_n1A-n5A  CA\_n1A-n78A  CA\_n5A-n78A | n1 | See n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | See n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78C\_BCS4 and 5 |  |
| CA\_n1A-n5A-n79A | CA\_n1A-n5A  CA\_n1A-n79A  CA\_n5A-n79A | n1 | See n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | See n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n5A-n105A | CA\_n1A-n5A  CA\_n1A-n105A  CA\_n5A-n105A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n1A-n7A-n8A | CA\_n1A-n7A  CA\_n1A-n8A  CA\_n7A-n8A | n1 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
| CA\_n1A-n7(2A)-n8A | CA\_n1A-n7A  CA\_n1A-n8A  CA\_n7A-n8A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | CA\_n7(2A)\_BCS0 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
| CA\_n1A-n7A-n20A | n77  CA\_n1A-n7A7  CA\_n1A-n20A  CA\_n7A-n20A7 | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n7A-n26A | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n7A-n26A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
| CA\_n1A-n7A-n26(2A) | CA\_n26(2A)  CA\_n1A-n26A  CA\_n1A-n7A  CA\_n7A-n26A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
| CA\_n1A-n7B-n26A | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n7A-n26A  CA\_n7B | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
| CA\_n1A-n7B-n26(2A) | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n7A-n26A  CA\_n7B  CA\_n26(2A) | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
| CA\_n1A-n7A-n28A | n77  CA\_n1A-n7A7  CA\_n1A-n28A  CA\_n7A-n28A7 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n1 | See n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | See n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n28 | See n28 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n7B-n28A | CA\_n1A-n28A  CA\_n1A-n7A  CA\_n7A-n28A  CA\_n7B | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
| CA\_n1A-n7A-n38A10 | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1(2A)-n7A-n38A10 | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1A-n7A-n40A | CA\_n1A-n7A  CA\_n1A-n40A  CA\_n7A-n40A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n7A-n67A | CA\_n1A-n7A | n1 | 5, 10, 15, 20, 30, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n7A-n75A | CA\_n1A-n7A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n75 | n75 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n7A-n78A | n77  n787,9  CA\_n1A-n7A  CA\_n1A-n78A7,13, 14  CA\_n7A-n78A7,13, 14 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 901,100 |  |
|  |  | n1 | 5, 10, 15, 20 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 901, 100 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n7A-n78(A-C) | CA\_n78C  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n78 | CA\_n78(A-C)\_BCS1 |  |
| CA\_n1A-n7B-n78A | n787,9  CA\_n1A-n78A7,14  CA\_n1A-n7A  CA\_n7A-n78A7,14  CA\_n7B | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 90, 100 |  |
| CA\_n1A-n7B-n78(2A) | n787,9  CA\_n1A-n78A7,14  CA\_n1A-n7A  CA\_n7A-n78A7,14  CA\_n7B  CA\_n78(2A) 7 | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  | CA\_n78(2A) | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | CA\_n7B\_BCS4 and 5 |  |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n1A-n7A-n78(2A) | n77  n787,9  CA\_n1A-n7A  CA\_n1A-n78A7,13, 14  CA\_n7A-n78A7,13, 14 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  | n77  n787,9  CA\_n78(2A) 7  CA\_n1A-n7A  CA\_n1A-n78A7,13, 14  CA\_n7A-n78A7, 13, ,14 | n1 | 5, 10, 15, 20 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n1A-n7A-n78C | n787,9  CA\_n78C7  CA\_n1A-n7A  CA\_n1A-n78A7,14  CA\_n7A-n78A7,14 | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n1A-n7B-n78C | n787,9  CA\_n7B  CA\_n1A-n7A  CA\_n1A-n78A7,14  CA\_n7A-n78A7,14  CA\_n78C7 | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n1A-n7(2A)-n78A | CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | CA\_n7(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n7A-n79A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n7A-n79C | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1(2A)-n7A-n79A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1(2A)-n7A-n79C | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1A-n7A-n105A | CA\_n1A-n7A  CA\_n1A-n105A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  | CA\_n7A-n105A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n1A-n8A-n28A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n28 | 10, 15, 20 |  |
| CA\_n1A-n8A-n40A | CA\_n1A-n8A  CA\_n1A-n40A  CA\_n8A-n40A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n8 | n8 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n8A-n41A | CA\_n1A-n8A  CA\_n1A-n41A  CA\_n8A-n41A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 100 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n8 | n8 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n8A-n77A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n8A-n77(2A) | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n1A-n8A-n78A | CA\_n1A-n8A  CA\_n1A-n78A  CA\_n8A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  | - | n1 | 5, 10, 15, 20 | 1 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n1A-n8A  CA\_n1A-n78A  CA\_n8A-n78A | n1 | See n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n8 | See n8 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n8A-n78C | CA\_n78C  CA\_n1A-n8A  CA\_n1A-n78A  CA\_n1A-n78C  CA\_n8A-n78A  CA\_n8A-n78C | n1 | See n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n8 | See n8 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78C\_BCS4 and 5 |  |
| CA\_n1A-n8A-n78(2A) | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS1 |  |
|  | CA\_n1A-n8A  CA\_n1A-n78A  CA\_n8A-n78A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n8 | n8 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS 4 and 5 |  |
| CA\_n1A-n8A-n79A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n18A-n28A | CA\_n1A-n18A  CA\_n1A-n28A  CA\_n18A-n28A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n28 | 5, 10 |  |
| CA\_n1A-n18A-n41A | n417,9  CA\_n1A-n18A  CA\_n1A-n41A7  CA\_n18A-n41A7 | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n18A-n77A | n777,9  CA\_n1A-n18A  CA\_n1A-n77A7  CA\_n18A-n77A7 | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n18A-n77(2A) | n777,9  CA\_n1A-n18A  CA\_n1A-n77A7  CA\_n18A-n77A7  CA\_n77(2A) | n1 | 5, 10, 15, 20 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n1A-n18A-n77(3A) | n777  CA\_n1A-n18A  CA\_n1A-n77A7  CA\_n18A-n77A7  CA\_n77(2A) | n1 | 5, 10, 15, 20 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n1A-n20A-n41A | CA\_n1A-n20A  CA\_n1A-n41A  CA\_n20A-n41A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n20 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 25, 30, 35, 40, 45, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n20A-n67A | CA\_n1A-n20A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n20 | 5, 10, 15, 20 |  |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n20A-n71A | CA\_n1A-n20A  CA\_n1A-n71A  CA\_n20A-n71A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n20 | 5, 10, 15, 20 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n1A-n20A-n77A | CA\_n1A-n20A  CA\_n1A-n77A  CA\_n20A-n77A | n1 | 5,10,15,20,25,30,40,45,50 | 4 and 5 |
|  |  | n20 | 5,10,15,20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n20A-n77(2A) | CA\_n1A-n20A  CA\_n1A-n77A  CA\_n20A-n77A | n1 | 5,10,15,20,25,30,40,45,50 | 4 and 5 |
|  |  | n20 | 5,10,15,20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n1A-n20A-n78A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n20 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n1A-n20A  CA\_n1A-n78A  CA\_n20A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 1 |
|  |  | n20 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n20A-n78(2A) | CA\_n1A-n20A  CA\_n1A-n78A  CA\_n20A-n78A  CA\_n78(2A) | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n1A-n26A-n78A | n787,9  CA\_n1A-n26A  CA\_n1A-n78A7,14  CA\_n26A-n78A7,14 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n26 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n26A-n78C | n787,9  CA\_n78C7  CA\_n1A-n26A  CA\_n1A-n78A7,14  CA\_n26A-n78A7,14 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n26 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n1A-n26A-n78(A-C) | CA\_n78C  CA\_n1A-n26A  CA\_n1A-n78A  CA\_n26A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(A-C)\_BCS1 |  |
| CA\_n1A-n26(2A)-n78A | n787,9  CA\_n1A-n26A  CA\_n1A-n78A7,14  CA\_n26A-n78A7,14  CA\_n26(2A) | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n26A-n78(2A) | n787,9  CA\_n1A-n26A  CA\_n1A-n78A7,14  CA\_n26A-n78A7,14  CA\_n78(2A)7 | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  | CA\_n78(2A) | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n26 | n26 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n1A-n26(2A)-n78(2A) | n787,9  CA\_n1A-n26A  CA\_n1A-n78A7,14  CA\_n26A-n78A7,14  CA\_n26(2A)  CA\_n78(2A)7 | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n1A-n26(2A)-n78C | n787,9  CA\_n26(2A)  CA\_n78C7  CA\_n1A-n26A  CA\_n1A-n78A7,14  CA\_n26A-n78A7,14 | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n1A-n28A-n38A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1A-n28A-n40A | CA\_n1A-n28A  CA\_n1A-n40A  CA\_n28A-n40A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n1 | 5, 10, 15, 20 | 1 |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n28A-n40B | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n40 | CA\_n40B\_BCS0 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | CA\_n40B\_BCS4 and 5 |  |
| CA\_n1A-n28A-n41A | n417,9  CA\_n1A-n28A  CA\_n1A-n41A7  CA\_n28A-n41A7 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n1A-n28A  CA\_n1A-n41A  CA\_n28A-n41A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n28A-n46A | CA\_n1A-n28A  CA\_n1A-n46A  CA\_n28A-n46A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n46 | 10, 20, 40, 60, 80 |  |
| CA\_n1A-n28A-n46C | CA\_n1A-n28A  CA\_n1A-n46A  CA\_n28A-n46A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n46 | CA\_n46C\_BCS0 |  |
| CA\_n1A-n28A-n46D | CA\_n1A-n28A  CA\_n1A-n46A  CA\_n28A-n46A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n46 | CA\_n46D\_BCS0 |  |
| CA\_n1A-n28A-n46(2A) | CA\_n1A-n28A  CA\_n1A-n46A  CA\_n28A-n46A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n46 | CA\_n46(2A)\_BCS0 |  |
| CA\_n1A-n28A-n75A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n75 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n1A-n28A-n77A | n777,9  CA\_n1A-n28A  CA\_n1A-n77A7  CA\_n28A-n77A7 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20 | 1 |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n1A-n28A  CA\_n1A-n77A  CA\_n28A-n77A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n28A-n77(2A) | n777,9  CA\_n1A-n28A  CA\_n1A-n77A7  CA\_n28A-n77A7  CA\_n77(2A)7 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n1 | 5, 10, 15, 20 | 1 |
|  |  | n28 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  | CA\_n1A-n28A  CA\_n1A-n77A  CA\_n28A-n77A  CA\_n77(2A) | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n1A-n28A-n77(3A) | n777,9  CA\_n1A-n28A  CA\_n1A-n77A7  CA\_n28A-n77A7  CA\_n77(2A)7 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
|  | CA\_n1A-n28A  CA\_n1A-n77A  CA\_n28A-n77A  CA\_n77(2A) | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(3A)\_BCS4 and 5 |  |
| CA\_n1A-n28A-n78A | n787,9  CA\_n1A-n28A  CA\_n1A-n78A7,13, 14  CA\_n28A-n78A7,13, 14 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 202 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20 | 1 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 2 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n28A-n78(2A) | n787,9  CA\_n1A-n28A  CA\_n1A-n78A7,13, 14  CA\_n28A-n78A7,13, 14  CA\_n78(2A)7 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n1A-n28A-n78C | n787,9  CA\_n1A-n28A  CA\_n1A-n78A7,14  CA\_n28A-n78A7,14 | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  | CA\_n78C7 | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n1A-n28A-n78(A-C) | CA\_n78C  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n28A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(A-C)\_BCS1 |  |
| CA\_n1A-n28A-n79A | n797,9  CA\_n1A-n28A  CA\_n1A-n79A7  CA\_n28A-n79A7 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  | CA\_n1A-n28A  CA\_n1A-n79A  CA\_n28A-n79A | n1 | n1 channel bandwidths in Table 5.3.5.1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5.1 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n28A-n102A | CA\_n1A-n28A  CA\_n1A-n102A  CA\_n28A-n102A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n1A-n28A-n102B | CA\_n1A-n28A  CA\_n1A-n102A  CA\_n1A-n102B  CA\_n28A-n102A  CA\_n28A-n102B | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n1A-n28A-n102C | CA\_n1A-n28A  CA\_n1A-n102A  CA\_n1A-n102C  CA\_n28A-n102A  CA\_n28A-n102C | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n1A-n28A-n102D | CA\_n1A-n28A  CA\_n1A-n102A  CA\_n28A-n102A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n1A-n28A-n102E | CA\_n1A-n28A  CA\_n1A-n102A  CA\_n28A-n102A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n1A-n28A-n102(2A) | CA\_n1A-n28A  CA\_n1A-n102A  CA\_n28A-n102A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n1A-n38A-n78A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n40A-n41A | CA\_n1A-n40A  CA\_n1A-n41A  CA\_n40A-n41A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n40A-n77A | CA\_n1A-n40A  CA\_n1A-n77A  CA\_n40A-n77A | n1 | 5, 10, 15, 20, 30, 40, 45, 50 | 0 |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n40A-n77(2A) | CA\_n1A-n40A  CA\_n1A-n77A  CA\_n40A-n77A | n1 | 5, 10, 15, 20, 30, 40, 45, 50 | 0 |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n1A-n40A-n78A | CA\_n1A-n40A  CA\_n1A-n78A  CA\_n40A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20 | 1 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20 | 2 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n40B-n78A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n40 | CA\_n40B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | CA\_n40B\_BCS 4 and 5 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n40A-n79A | CA\_n1A-n40A  CA\_n1A-n79A  CA\_n40A-n79A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n40A-n105A | CA\_n1A-n40A  CA\_n1A-n105A  CA\_n40A-n105A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n1A-n41A-n71A | CA\_n1A-n41A  CA\_n1A-n71A  CA\_n41A-n71A | n1 | 5,10,15,20,25,30,40,45,50 | 0 |
|  |  | n41 | 5,10,15,20,25,30,35,40,45,50,60,70,80,90,100 |  |
|  |  | n71 | 5,10,15,20 |  |
| CA\_n1A-n41A-n77A | n417,9  n777,9  CA\_n1A-n41A7  CA\_n1A-n77A7  CA\_n41A-n77A7 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n41A-n77(2A) | n417,9  n777,9  CA\_n1A-n41A7  CA\_n1A-n77A7  CA\_n41A-n77A7  CA\_n77(2A) | n1 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n1A-n41A-n77(3A) | CA\_n1A-n41A  CA\_n1A-n77A  CA\_n41A-n77A  CA\_n77(2A) | n1 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n1A-n41A-n78A | CA\_n1A-n41A  CA\_n1A-n78A  CA\_n41A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 100 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n41A-n78C | CA\_n78C  CA\_n1A-n41A  CA\_n1A-n78A  CA\_n1A-n78C  CA\_n41A-n78A  CA\_n41A-n78C | n1 | 5,10,15,20,25,30,40,45,50 | 0 |
|  |  | n41 | 5,10,15,20,25,30,35,40,45,50,60,70,80,90,100 |  |
|  |  | n78 | CA\_n78C\_BCS4 and 5 |  |
| CA\_n1A-n41A-n79A | CA\_n1A-n41A  CA\_n1A-n79A  CA\_n41A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n46A-n78A | CA\_n1A-n46A  CA\_n1A-n78A  CA\_n46A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | 10, 20, 40, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n46C-n78A | CA\_n1A-n46A  CA\_n1A-n78A  CA\_n46A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | CA\_n46C\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n46D-n78A | CA\_n1A-n46A  CA\_n1A-n78A  CA\_n46A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | CA\_n46D\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n46(2A)-n78A | CA\_n1A-n46A  CA\_n1A-n78A  CA\_n46A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | CA\_n46(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n46A-n78(2A) | CA\_n1A-n46A  CA\_n1A-n78A  CA\_n46A-n78A  CA\_n78(2A) | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | 10, 20, 40, 60, 80 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n46C-n78(2A) | CA\_n1A-n46A  CA\_n1A-n78A  CA\_n46A-n78A  CA\_n78(2A) | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | CA\_n46C\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n46D-n78(2A) | CA\_n1A-n46A  CA\_n1A-n78A  CA\_n46A-n78A  CA\_n78(2A) | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | CA\_n46D\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n46(2A)-n78(2A) | CA\_n1A-n46A  CA\_n1A-n78A  CA\_n46A-n78A  CA\_n78(2A) | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | CA\_n46(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n67A-n78A | CA\_n1A-n78A | n1 | 5, 10, 15, 20, 30, 40, 45, 50 | 0 |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n67A-n78(2A) | CA\_n1A-n78A  CA\_n78(2A) | n1 | 5, 10, 15, 20, 30, 40, 45, 50 | 0 |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n1A-n71A-n77A | CA\_n1A-n71A  CA\_n1A-n77A  CA\_n71A-n77A | n1 | 5,10,15,20,25,30,40,45,50 | 0 |
|  |  | n71 | 5,10,15,20 |  |
|  |  | n77 | 10,15,20,25,30,40,50,60,70,80,90,100 |  |
| CA\_n1A-n71A-n77(2A) | CA\_n1A-n71A  CA\_n1A-n77A  CA\_n71A-n77A | n1 | 5,10,15,20,25,30,40,45,50 | 0 |
|  |  | n71 | 5,10,15,20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n1A-n71A-n78A | CA\_n1A-n71A  CA\_n1A-n78A  CA\_n71A-n78A | n1 | 5,10,15,20,25,30,40,45,50 | 0 |
|  |  | n71 | 5,10,15,20 |  |
|  |  | n78 | 10,15,20,25,30,40,50,60,70,80,90,100 |  |
| CA\_n1A-n71A-n78C | CA\_n78C  CA\_n1A-n71A  CA\_n1A-n78A  CA\_n1A-n78C  CA\_n71A-n78A  CA\_n71A-n78C | n1 | 5,10,15,20,25,30,40,45,50 | 0 |
|  |  | n71 | 5,10,15,20 |  |
|  |  | n78 | CA\_n78C\_BCS 4 and 5 |  |
| CA\_n1A-n75A-n78A | CA\_n1A-n78A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n75 | n75 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n77A-n79A4 | n777,9  n797,9  CA\_n1A-n77A7  CA\_n1A-n79A7  CA\_n77A-n79A7 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n77(2A)-n79A4 | n777,9  n797,9  CA\_n1A-n77A7  CA\_n1A-n79A7  CA\_n77A-n79A7  CA\_n77(2A)7 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n77(3A)-n79A4 | CA\_n1A-n77A  CA\_n1A-n79A  CA\_n77A-n79A  CA\_n77(2A) | n1 | 5, 10, 15, 20 | 0 |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77(3A)\_BCS4 and 5 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n78A-n79A5 | n787,9  n797,9  CA\_n1A-n78A  CA\_n1A-n79A  CA\_n78A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n1 | 5, 10, 15, 20 | 1 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n78(2A)-n79A | n787,9  n797,9  CA\_n1A-n78A  CA\_n1A-n79A  CA\_n78A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS1 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n78A-n102A | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n78A-n102A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n1A-n78A-n102B | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n1A-n102B  CA\_n78A-n102A  CA\_n78A-n102B | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n1A-n78A-n102C | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n1A-n102C  CA\_n78A-n102A  CA\_n78A-n102C | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n1A-n78A-n102D | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n78A-n102A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n1A-n78A-n102E | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n78A-n102A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n1A-n78A-n102(2A) | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n78A-n102A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n1A-n78(2A)-n102A | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n78A-n102A  CA\_n78(2A) | n1 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n1A-n78(2A)-n102B | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n1A-n102B  CA\_n78A-n102A  CA\_n78A-n102B  CA\_n78(2A) | n1 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n1A-n78(2A)-n102C | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n1A-n102C  CA\_n78A-n102A  CA\_n78A-n102C  CA\_n78(2A) | n1 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n1A-n78(2A)-n102D | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n78A-n102A  CA\_n78(2A) | n1 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n1A-n78(2A)-n102E | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n78A-n102A  CA\_n78(2A) | n1 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n1A-n78(2A)-n102(2A) | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n78A-n102A  CA\_n78(2A) | n1 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n1A-n78A-n105A | CA\_n1A-n78A  CA\_n1A-n105A  CA\_n78A-n105A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n2A-n5A-n30A | CA\_n2A-n5A  CA\_n2A-n30A  CA\_n5A-n30A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n30 | n30 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n5A-n41A | CA\_n2A-n5A  CA\_n2A-n41A  CA\_n5A-n41A | n2 | 5, 10, 15, 20, 25, 30, 35, 40 | 0 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n2A-n5A-n48A | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n5A-n48A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n5A-n48A | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n5A-n48A | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n5A-n48B | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n48B  CA\_n5A-n48A  CA\_n5A-n48B  CA\_n48B | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n48 | CA\_n48B\_BCS4 and 5 |  |
| CA\_n2A-n5B-n48A | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n5A-n48A  CA\_n5B | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | CA\_n5B\_BCS4 and 5 |  |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n5A-n48B | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n48B  CA\_n5A-n48A  CA\_n5A-n48B  CA\_n48B | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n2 | 5, 10, 15, 20 | 1 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n2 | 5, 10, 15, 20 | 2 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n48 | CA\_n48B\_BCS4 and 5 |  |
| CA\_n2A-n5B-n48B | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n48B  CA\_n5A-n48A  CA\_n5A-n48B  CA\_n5B  CA\_n48B | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | CA\_n5B\_BCS4 and 5 |  |
|  |  | n48 | CA\_n48B\_BCS4 and 5 |  |
| CA\_n2A-n5A-n48(2A) | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n5A-n48A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n2 | 5, 10, 15, 20 | 1 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n48 | CA\_n48(2A)\_BCS4 and 5 |  |
| CA\_n2(2A)-n5A-n48(2A) | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n5A-n48A | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n48 | CA\_n48(2A)\_BCS4 and 5 |  |
| CA\_n2(2A)-n5B-n48A | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n5A-n48A  CA\_n5B | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n5 | CA\_n5B\_BCS4 and 5 |  |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n5B-n48B | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n48B  CA\_n5A-n48A  CA\_n5A-n48B  CA\_n5B  CA\_n48B | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n5 | CA\_n5B\_BCS4 and 5 |  |
|  |  | n48 | CA\_n48B\_BCS4 and 5 |  |
| CA\_n2A-n5B-n48(2A) | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n5A-n48A  CA\_n5B | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | CA\_n5B\_BCS4 and 5 |  |
|  |  | n48 | CA\_n48(2A)\_BCS4 and 5 |  |
| CA\_n2(2A)-n5B-n48(2A) | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n5A-n48A  CA\_n5B | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n5 | CA\_n5B\_BCS4 and 5 |  |
|  |  | n48 | CA\_n48(2A)\_BCS4 and 5 |  |
| CA\_n2A-n5A-n48(A-B) | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n5A-n48A | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n5 | 5, 10, 15, 20, 251 |  |
|  |  | n48 | CA\_n48(A-B)\_BCS0 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n5 | 5, 10, 15, 20, 251 |  |
|  |  | n48 | CA\_n48(A-B)\_BCS1 |  |
|  |  | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n48 | CA\_n48(A-B)\_BCS4 and 5 |  |
| CA\_n2(2A)-n5A-n30A | CA\_n2A-n5A  CA\_n2A-n30A  CA\_n5A-n30A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n30 | 5, 10 |  |
| CA\_n2A-n5A-n66A | CA\_n2A-n5A  CA\_n2A-n66A  CA\_n5A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n5A-n66A | CA\_n2A-n5A  CA\_n2A-n66A  CA\_n5A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n5A-n66(2A) | CA\_n2A-n5A  CA\_n2A-n66A  CA\_n5A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n2 | CA\_n2(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 |  |
| CA\_n2A-n5A-n66(2A) | CA\_n2A-n5A  CA\_n2A-n66A  CA\_n5A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
|  |  | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 |  |
| CA\_n2A-n5A-n66(3A) | CA\_n2A-n5A  CA\_n2A-n66A  CA\_n5A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n2A-n5B-n66A | CA\_n2A-n5A  CA\_n2A-n66A  CA\_n5A-n66A  CA\_n5B | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | CA\_n5B\_BCS4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n5B-n66(2A) | CA\_n2A-n5A  CA\_n2A-n66A  CA\_n5A-n66A  CA\_n5B | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | CA\_n5B\_BCS4 and 5 |  |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 |  |
| CA\_n2(2A)-n5B-n66A | CA\_n2A-n5A  CA\_n2A-n66A  CA\_n5A-n66A  CA\_n5B | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n5 | CA\_n5B\_BCS4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n5B-n66(2A) | CA\_n2A-n5A  CA\_n2A-n66A  CA\_n5A-n66A  CA\_n5B | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n5 | CA\_n5B\_BCS4 and 5 |  |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 |  |
| CA\_n2A-n5A-n77A | n777,9  CA\_n2A-n5A  CA\_n2A-n77A7,13,14  CA\_n5A-n77A7,13,14 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | n777,9  CA\_n2A-n5A  CA\_n2A-n77A7,13,14  CA\_n5A-n77A7,13,14 | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n5B-n77A | n777,9  CA\_n2A-n5A  CA\_n2A-n77A7,13,14  CA\_n5A-n77A7,13,14  CA\_n5B | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | CA\_n5B\_BCS4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n5A-n77C | n777,9  CA\_n2A-n5A  CA\_n2A-n77A7,13,14  CA\_n5A-n77A7,13,14  CA\_n77C | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n5 | 5, 10, 15, 20, 251 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n5 | 5, 10, 15, 20, 251 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  | n777,9  CA\_n2A-n5A  CA\_n2A-n77A7,13,14  CA\_n2A-n77C7,13,14  CA\_n5A-n77A7,13,14  CA\_n5A-n77C7,13,14  CA\_n77C | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77C\_BCS4 and 5 |  |
| CA\_n2A-n5B-n77C | n777,9  CA\_n2A-n5A  CA\_n2A-n77A7,13,14  CA\_n2A-n77C7,13,14  CA\_n5B  CA\_n5A-n77A7,13,14  CA\_n5A-n77C7,13,14  CA\_n77C | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | CA\_n5B\_BCS4 and 5 |  |
|  |  | n77 | CA\_n77C\_BCS4 and 5 |  |
| CA\_n2A-n5A-n77(2A) | n777,9  CA\_n2A-n5A  CA\_n2A-n77A7  CA\_n5A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n2(2A)-n5A-n77A | n777,9  CA\_n2A-n5A  CA\_n2A-n77A7,13,14  CA\_n5A-n77A7,13,14 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | n777,9  CA\_n2A-n5A  CA\_n2A-n77A7,13,14  CA\_n5A-n77A7,13,14 | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n5A-n77C | n777,9  CA\_n2A-n5A  CA\_n2A-n77A7,13,14  CA\_n2A-n77C7,13,14  CA\_n5A-n77A7,13,14  CA\_n5A-n77C7,13,14  CA\_n77C | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77C\_BCS4 and 5 |  |
| CA\_n2(2A)-n5A-n77(2A) | n777,9  CA\_n2A-n5A  CA\_n2A-n77A7  CA\_n5A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n2(2A)-n5B-n77A | n777,9  CA\_n2A-n5A  CA\_n2A-n77A7,13,14  CA\_n5A-n77A7,13,14  CA\_n5B | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n5 | CA\_n5B\_BCS4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n5B-n77C | n777,9  CA\_n2A-n5A  CA\_n2A-n77A7,13,14  CA\_n2A-n77C7,13,14  CA\_n5A-n77A7,13,14  CA\_n5A-n77C7,13,14  CA\_n5B  CA\_n77C | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n5 | CA\_n5B\_BCS4 and 5 |  |
|  |  | n77 | CA\_n77C\_BCS4 and 5 |  |
| CA\_n2A-n7A-n12A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n12 | 5, 10, 15 |  |
| CA\_n2A-n7A-n66A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
| CA\_n2A-n7A-n71A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n2A-n7A-n77A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n12A-n30A | CA\_n2A-n12A  CA\_n2A-n30A  CA\_n12A-n30A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n30 | 5, 10 |  |
| CA\_n2(2A)-n12A-n30A | CA\_n2A-n12A  CA\_n2A-n30A  CA\_n12A-n30A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n30 | 5, 10 |  |
| CA\_n2A-n12A-n41A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n2A-n12A-n66A | CA\_n2A-n12A  CA\_n2A-n66A  CA\_n12A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2(2A)-n12A-n66A | CA\_n2A-n12A  CA\_n2A-n66A  CA\_n12A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2A-n12A-n66(2A) | CA\_n2A-n12A  CA\_n2A-n66A  CA\_n12A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n2(2A)-n12A-n66(2A) | CA\_n2A-n12A  CA\_n2A-n66A  CA\_n12A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n2A-n12A-n66(3A) | CA\_n2A-n12A  CA\_n2A-n66A  CA\_n12A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n2A-n12A-n71A | CA\_n2A-n12A  CA\_n2A-n71A | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n2A-n12A-n77A | n777,9  CA\_n2A-n12A  CA\_n2A-n77A7  CA\_n12A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n12A-n77A | n777,9  CA\_n2A-n12A  CA\_n2A-n77A7  CA\_n12A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n12A-n77(2A) | n777,9  CA\_n2A-n12A  CA\_n2A-n77A7  CA\_n12A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2(2A)-n12A-n77(2A) | n777,9  CA\_n2A-n12A  CA\_n2A-n77A7  CA\_n12A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n14A-n30A | CA\_n2A-n14A  CA\_n2A-n30A  CA\_n14A-n30A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n14 | n14 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n30 | n30 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n14A-n30A | CA\_n2A-n14A  CA\_n2A-n30A  CA\_n14A-n30A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
| CA\_n2A-n14A-n66A | CA\_n2A-n14A  CA\_n2A-n66A  CA\_n14A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n14 | n14 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n14A-n66A | CA\_n2A-n14A  CA\_n2A-n66A  CA\_n14A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n14 | n14 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n14A-n66(2A) | CA\_n2A-n14A  CA\_n2A-n66A  CA\_n14A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n14 | n14 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 |  |
| CA\_n2A-n14A-n66(2A) | CA\_n2A-n14A  CA\_n2A-n66A  CA\_n14A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n14 | n14 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 |  |
| CA\_n2A-n14A-n66(3A) | CA\_n2A-n14A  CA\_n2A-n66A  CA\_n14A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n2A-n14A-n77A | n777,9  CA\_n2A-n14A  CA\_n2A-n77A7  CA\_n14A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n14 | n14 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n14A-n77(2A) | n777,9  CA\_n2A-n14A  CA\_n2A-n77A7  CA\_n14A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n14 | n14 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n2(2A)-n14A-n77A | n777,9  CA\_n2A-n14A  CA\_n2A-n77A7  CA\_n14A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n14 | n14 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n14A-n77(2A) | n777,9  CA\_n2A-n14A  CA\_n2A-n77A7  CA\_n14A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n14 | n14 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n2A-n29A-n30A | CA\_n2A-n30A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
| CA\_n2(2A)-n29A-n30A | CA\_n2A-n30A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
| CA\_n2A-n29A-n66A | CA\_n2A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2(2A)-n29A-n66A | CA\_n2A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2A-n29A-n66(2A) | CA\_n2A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n2(2A)-n29A-n66(2A) | CA\_n2A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n2A-n29A-n77A | n777,9  CA\_n2A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n29A-n77A | n777,9  CA\_n2A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n29A-n77(2A) | n777,9  CA\_n2A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2(2A)-n29A-n77(2A) | n777,9  CA\_n2A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n30A-n66A | CA\_n2A-n30A  CA\_n2A-n66A  CA\_n30A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n30 | n30 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n30A-n66A | CA\_n2A-n30A  CA\_n2A-n66A  CA\_n30A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
| CA\_n2(2A)-n30A-n66(2A) | CA\_n2A-n30A  CA\_n2A-n66A  CA\_n30A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n2A-n30A-n66(2A) | CA\_n2A-n30A  CA\_n2A-n66A  CA\_n30A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
| CA\_n2A-n30A-n66(3A) | CA\_n2A-n30A  CA\_n2A-n66A  CA\_n30A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n2A-n30A-n77A | n777,9  CA\_n2A-n30A  CA\_n2A-n77A7  CA\_n30A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n30 | n30 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n30A-n77(2A) | n777,9  CA\_n2A-n30A  CA\_n2A-n77A7  CA\_n30A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n30 | n30 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n2(2A)-n30A-n77A | n777,9  CA\_n2A-n30A  CA\_n2A-n77A7  CA\_n30A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | CA\_n2(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n30 | n30 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n30A-n77(2A) | n777,9  CA\_n2A-n30A  CA\_n2A-n77A7  CA\_n30A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n2 | CA\_n2(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n30 | n30 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n2A-n41A-n66A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
| CA\_n2A-n41A-n71A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n2A-n48A-n66A | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n48A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n48A-n66A | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n48A-n66A | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n48B-n66A | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n48B  CA\_n48A-n66A  CA\_n48B-n66A  CA\_n48B | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n48 | CA\_n48B\_BCS4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n48(A-B)-n66A | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n48A-n66A | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n48 | CA\_n48(A-B)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | CA\_n48(A-B)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | CA\_n48(A-B)\_BCS4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n48B-n66A | CA\_n48B  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n48B  CA\_n48A-n66A  CA\_n48B-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n2 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n2 | 5, 10, 15, 20 | 2 |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | CA\_n48B\_BCS4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n48(2A)-n66A | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n48A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n2 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | CA\_n48(2A)\_BCS4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n48A-n66(2A) | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n48A-n66A | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 |  |
| CA\_n2A-n48B-n66(2A) | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n48B  CA\_n48A-n66A  CA\_n48B-n66A  CA\_n48B | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | CA\_n48B\_BCS4 and 5 |  |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 |  |
| CA\_n2(2A)-n48(2A)-n66A | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n48A-n66A | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n48 | CA\_n48(2A)\_BCS4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n48A-n66(2A) | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n48A-n66A | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 |  |
| CA\_n2A-n48(2A)-n66(2A) | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n48A-n66A | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | CA\_n48(2A)\_BCS4 and 5 |  |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 |  |
| CA\_n2(2A)-n48B-n66(2A) | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n48B  CA\_n48A-n66A  CA\_n48B-n66A  CA\_n48B | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n48 | CA\_n48B\_BCS4 and 5 |  |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 |  |
| CA\_n2(2A)-n48(2A)-n66(2A) | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n48A-n66A | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n48 | CA\_n48(2A)\_BCS4 and 5 |  |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 |  |
| CA\_n2A-n48A-n77A | n777,9  CA\_n2A-n48A  CA\_n2A-n77A7,13,14 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | n777,9  CA\_n2A-n48A  CA\_n2A-n77A7,13,14 | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n48A-n77C | n777,9  CA\_n2A-n48A  CA\_n2A-n77A7,13,14  CA\_n77C | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  | n777,9  CA\_n2A-n48A  CA\_n2A-n77A7,13,14  CA\_n2A-n77C7,13,14  CA\_n77C | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77C\_BCS4 and 5 |  |
| CA\_n2A-n48(2A)-n77C | n777,9  CA\_n2A-n48A  CA\_n2A-n77A7,13,14 | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  | n777,9  CA\_n77C  CA\_n2A-n48A  CA\_n2A-n77A7,13,14  CA\_n2A-n77C7,13,14 | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | CA\_n48(2A)\_BCS4 and 5 |  |
|  |  | n77 | CA\_n77C\_BCS4 and 5 |  |
| CA\_n2A-n48B-n77A | n777,9  CA\_n48B  CA\_n2A-n48A  CA\_n2A-n77A7,13,14 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | 5, 10, 15, 20 | 2 |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | n777,9  CA\_n48B  CA\_n2A-n48A  CA\_n2A-n48B  CA\_n2A-n77A7,13,14 | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | CA\_n48B\_BCS4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n48B-n77C | n777,9  CA\_n48B  CA\_n2A-n48A  CA\_n2A-n77A7,13,14 | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  | n777,9  CA\_n48B  CA\_n77C  CA\_n2A-n48A  CA\_n2A-n48B  CA\_n2A-n77A7,13,14  CA\_n2A-n77C7,13,14 | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | CA\_n48B\_BCS4 and 5 |  |
|  |  | n77 | CA\_n77C\_BCS4 and 5 |  |
| CA\_n2(2A)-n48B-n77A | n777,9  CA\_n2A-n48A  CA\_n2A-n48B  CA\_n2A-n77A7,13,14  CA\_n48B | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n48 | CA\_n48B\_BCS4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n48(2A)-n77A | n777,9  CA\_n2A-n48A  CA\_n2A-n77A7,13,14 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | n777,9  CA\_n2A-n48A  CA\_n2A-n77A7,13,14 | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | CA\_n48(2A)\_BCS4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n48A-n77A | n777,9  CA\_n2A-n48A  CA\_n2A-n77A7,13,14 | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n48(2A)-n77A | n777,9  CA\_n2A-n48A  CA\_n2A-n77A7,13,14 | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n48 | CA\_n48(2A)\_BCS4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n48A-n77C | n777,9  CA\_n2A-n48A  CA\_n2A-n77A7,13,14  CA\_n2A-n77C7,13,14  CA\_n77C | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77C\_BCS4 and 5 |  |
| CA\_n2(2A)-n48(2A)-n77C | n777,9  CA\_n2A-n48A  CA\_n2A-n77A7,13,14  CA\_n2A-n77C7,13,14  CA\_n77C | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n48 | CA\_n48(2A)\_BCS4 and 5 |  |
|  |  | n77 | CA\_n77C\_BCS4 and 5 |  |
| CA\_n2(2A)-n48B-n77C | n777,9  CA\_n2A-n48A  CA\_n2A-n48B  CA\_n2A-n77A7,13,14  CA\_n2A-n77C7,13,14  CA\_n48B  CA\_n77C | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n48 | CA\_n48B\_BCS4 and 5 |  |
|  |  | n77 | CA\_n77C\_BCS4 and 5 |  |
| CA\_n2A-n66A-n71A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n2A-n66A-n77A | n777,9  CA\_n2A-n66A  CA\_n2A-n77A7,13,14  CA\_n66A-n77A7,13,14 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | n777,9  CA\_n2A-n66A  CA\_n2A-n77A7,13,14  CA\_n66A-n77A7,13,14 | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n66A-n77A | n777,9  CA\_n2A-n66A  CA\_n2A-n77A7,13,14  CA\_n66A-n77A7,13,14 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | n777,9  CA\_n2A-n66A  CA\_n2A-n77A7,13,14  CA\_n66A-n77A7,13,14 | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n66A-n77C | n777,9  CA\_n2A-n66A  CA\_n2A-n77A7,13,14  CA\_n2A-n77C7,13,14  CA\_n66A-n77A7,13,14  CA\_n66A-n77C7,13,14  CA\_n77C | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77C\_BCS4 and 5 |  |
| CA\_n2A-n66(2A)-n77A | n777,9  CA\_n2A-n66A  CA\_n2A-n77A7,13,14  CA\_n66A-n77A7,13,14 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | n777,9  CA\_n2A-n66A  CA\_n2A-n77A7,13,14  CA\_n66A-n77A7,13,14 | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2A-n66(2A)-n77C | n777,9  CA\_n2A-n66A  CA\_n2A-n77A7,13,14  CA\_n2A-n77C7,13,14  CA\_n66A-n77A7,13,14  CA\_n66A-n77C7,13,14  CA\_n77C | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 |  |
|  |  | n77 | CA\_n77C\_BCS4 and 5 |  |
| CA\_n2A-n66A-n77C | n777,9  CA\_n2A-n66A  CA\_n2A-n77A7,13,14  CA\_n66A-n77A7,13,14 | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  | n777,9  CA\_n77C  CA\_n2A-n66A  CA\_n2A-n77A7,13,14  CA\_n2A-n77C7,13,14  CA\_n66A-n77A7,13,14  CA\_n66A-n77C7,13,14 | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77C\_BCS4 and 5 |  |
| CA\_n2A-n66A-n77(2A) | n777,9  CA\_n2A-n66A  CA\_n2A-n77A7  CA\_n66A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n2(2A)-n66(2A)-n77A | n777,9  CA\_n2A-n66A  CA\_n66A-n77A7,13,14  CA\_n2A-n77A7,13,14 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | n777,9  CA\_n2A-n66A  CA\_n66A-n77A7,13,14  CA\_n2A-n77A7,13,14 | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n2(2A)-n66(2A)-n77C | n777,9  CA\_n2A-n66A  CA\_n66A-n77A7,13,14  CA\_n66A-n77C7,13,14  CA\_n2A-n77A7,13,14  CA\_n2A-n77C7,13,14  CA\_n77C | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 |  |
|  |  | n77 | CA\_n77C\_BCS4 and 5 |  |
| CA\_n2(2A)-n66(2A)-n77(2A) | n777,9  CA\_n2A-n66A  CA\_n2A-n77A7  CA\_n66A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2(2A)-n66A-n77(2A) | n777,9  CA\_n2A-n66A  CA\_n66A-n77A7  CA\_n2A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n2 | CA\_n2(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n2A-n66(2A)-n77(2A) | n777,9  CA\_n2A-n66A  CA\_n66A-n77A7  CA\_n2A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n2 | n2 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 |  |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n2A-n66(3A)-n77A | n777,9  CA\_n2A-n66A  CA\_n66A-n77A7  CA\_n2A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n66(3A)-n77(2A) | n777,9  CA\_n2A-n66A  CA\_n2A-n77A7  CA\_n66A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n66A-n78A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n66A-n78(2A) | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n2A-n71A-n77A | CA\_n2A-n71A  CA\_n2A-n77A  CA\_n71A-n77A | n2 | 5, 10, 15, 20, 25, 30, 35, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20, 25, 30, 35 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n71A-n77(2A) | CA\_n2A-n71A  CA\_n2A-n77A  CA\_n71A-n77A | n2 | 5, 10, 15, 20, 25, 30, 35, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20, 25, 30, 35 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n71A-n78A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n71A-n78(2A) | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3A-n5A-n7A | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40 |  |
|  | CA\_n3A-n5A  CA\_n3A-n7A  CA\_n5A-n7A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n3A-n5A-n7B | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  | CA\_n3A-n5A  CA\_n3A-n7A  CA\_n5A-n7A  CA\_n7B | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
| CA\_n3A-n5A-n8A | - | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
| CA\_n3A-n5A-n28A | - | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  | CA\_n3A-n5A  CA\_n3A-n28A  CA\_n5A-n28A | n3 | See n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | See n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n28 | See n28 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n5A-n78A | CA\_n3A-n5A  CA\_n3A-n78A  CA\_n5A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n5A-n78(2A) | CA\_n3A-n5A  CA\_n3A-n78A  CA\_n5A-n78A | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3A-n5A-n78C | CA\_n78C  CA\_n3A-n5A  CA\_n3A-n78A  CA\_n5A-n78A | n3 | See n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | See n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78C\_BCS4 and 5 |  |
| CA\_n3A-n5A-n78(A-C) | CA\_n78C  CA\_n3A-n5A  CA\_n3A-n78A  CA\_n5A-n78A | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n78 | CA\_n78(A-C)\_BCS1 |  |
| CA\_n3A-n5A-n79A | CA\_n3A-n5A  CA\_n3A-n79A  CA\_n5A-n79A | n3 | See n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | See n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n7A-n8A | CA\_n3A-n7A  CA\_n3A-n8A  CA\_n7A-n8A | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n8 | 5, 10, 15, 20, 35 |  |
| CA\_n3A-n7(2A)-n8A | CA\_n3A-n7A  CA\_n3A-n8A  CA\_n7A-n8A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n7 | CA\_n7(2A)\_BCS0 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
| CA\_n3(2A)-n7A-n8A | CA\_n3A-n7A  CA\_n3A-n8A  CA\_n7A-n8A | n3 | CA\_n3(2A)\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
| CA\_n3(2A)-n7(2A)-n8A | CA\_n3A-n7A  CA\_n3A-n8A  CA\_n7A-n8A | n3 | CA\_n3(2A)\_BCS0 | 0 |
|  |  | n7 | CA\_n7(2A)\_BCS0 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
| CA\_n3A-n7A-n20A | n37  n77  CA\_n3A-n7A7  CA\_n3A-n20A  CA\_n7A-n20A7 | n3 | See n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | See n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n20 | See n20 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n7A-n26A | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n7A-n26A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
| CA\_n3A-n7A-n26(2A) | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n7A-n26A  CA\_n26(2A) | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
| CA\_n3A-n7B-n26A | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n7A-n26A  CA\_n7B | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
| CA\_n3A-n7B-n26(2A) | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n7A-n26A  CA\_n7B  CA\_n26(2A) | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
| CA\_n3B-n7A-n26A | CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
| CA\_n3B-n7A-n26(2A) | CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A  CA\_n26(2A) | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
| CA\_n3B-n7B-n26A | CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A  CA\_n7B | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
| CA\_n3B-n7B-n26(2A) | CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A  CA\_n7B  CA\_n26(2A) | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
| CA\_n3A-n7A-n28A | n37  n77 | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  | n37  n77  CA\_n3A-n7A7  CA\_n3A-n28A7  CA\_n7A-n28A7 | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 2 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n7B-n28A | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  | CA\_n3A-n7A  CA\_n3A-n28A  CA\_n7A-n28A  CA\_n7B | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
| CA\_n3B-n7A-n28A | CA\_n3A-n7A  CA\_n3A-n28A  CA\_n7A-n28A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
| CA\_n3B-n7B-n28A | CA\_n7B  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n7A-n28A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
| CA\_n3A-n7A-n38A10 | - | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n3B-n7A-n38A10 | - | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n3(2A)-n7A-n38A10 | - | n3 | CA\_n3(2A)\_BCS1 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n3A-n7A-n40A | CA\_n3A-n7A  CA\_n3A-n40A  CA\_n7A-n40A | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n7A-n67A | CA\_n3A-n7A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n7A-n75A | CA\_n3A-n7A | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n75 | n75 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n7A-n77A | CA\_n3A-n7A CA\_n3A-n77A CA\_n7A-n77A | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n7A-n77(2A) | CA\_n77(2A)  CA\_n3A-n7A CA\_n3A-n77A CA\_n7A-n77A | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n3A-n7A-n78A | n37  n77  n787,9  CA\_n3A-n7A  CA\_n3A-n78A7,13, 14  CA\_n7A-n78A7,13, 14 | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 90, 100 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n7A-n78C | n787,9  CA\_n78C7  CA\_n3A-n7A  CA\_n3A-n78A7,14  CA\_n7A-n78A7,14 | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n3A-n7A-n78(A-C) | CA\_n78C  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n78 | CA\_n78(A-C)\_BCS1 |  |
| CA\_n3A-n7B-n78A | n787,9 | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  | n787,9  CA\_n3A-n7A  CA\_n3A-n78A7,14  CA\_n7A-n78A7,14  CA\_n7B | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 90, 100 |  |
| CA\_n3A-n7B-n78(2A) | n787,9  CA\_n3A-n7A  CA\_n3A-n78A7,14  CA\_n7A-n78A7,14  CA\_n7B | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  | CA\_n78(2A) 7 | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  | CA\_n78(2A) | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | CA\_n7B\_BCS4 and 5 |  |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n3A-n7B-n78C | n787,9  CA\_n3A-n7A  CA\_n3A-n78A7,14  CA\_n7A-n78A7,14  CA\_n7B  CA\_n78C7 | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n3A-n7A-n78(2A) | n37  n77  n787,9  CA\_n78(2A) 7  CA\_n3A-n7A  CA\_n3A-n78A7,13, 14  CA\_n7A-n78A7,13, 14 | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n3A-n7(2A)-n78A | CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n7 | CA\_n7(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3B-n7A-n78A | n787,9  CA\_n3A-n7A  CA\_n3A-n78A7,14  CA\_n7A-n78A7,14 | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3B-n7A-n78(2A) | n787,9  CA\_n78(2A) 7  CA\_n3A-n7A  CA\_n3A-n78A7,14  CA\_n7A-n78A7,14 | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  | CA\_n78(2A) | n3 | CA\_n3B\_BCS4 and 5 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n3B-n7A-n78C | n787,9  CA\_n3A-n7A  CA\_n3A-n78A7,14  CA\_n7A-n78A7,14  CA\_n78C7 | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n3B-n7B-n78A | n787,9  CA\_n3A-n7A  CA\_n3A-n78A7,14  CA\_n7A-n78A7,14  CA\_n7B | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3B-n7B-n78(2A) | n787,9  CA\_n3A-n7A  CA\_n3A-n78A7,14  CA\_n7A-n78A7,14  CA\_n7B | n3 | CA\_n3B\_BCS0 | 0 |
|  | CA\_n78(2A) 7 | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  | CA\_n78(2A) | n3 | CA\_n3B\_BCS4 and 5 | 4 and 5 |
|  |  | n7 | CA\_n7B\_BCS4 and 5 |  |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n3B-n7B-n78C | n787,9  CA\_n3A-n7A  CA\_n3A-n78A7,14  CA\_n7A-n78A7,14  CA\_n7B  CA\_n78C7 | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n3(2A)-n7A-n78A | CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | n3 | CA\_n3(2A)\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3(2A)-n7(2A)-n78A | CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | n3 | CA\_n3(2A)\_BCS0 | 0 |
|  |  | n7 | CA\_n7(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n7A-n79A | - | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n7A-n79C | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n3B-n7A-n79A | - | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3(2A)-n7A-n79A | - | n3 | CA\_n3(2A)\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3B-n7A-n79C | - | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n3(2A)-n7A-n79C | - | n3 | CA\_n3(2A)\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n3A-n7A-n105A | CA\_n3A-n7A  CA\_n3A-n105A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  | CA\_n7A-n105A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n3A-n8A-n28A | - | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n8 | 5, 10, 15, 20, 35 |  |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
| CA\_n3A-n8A-n39A | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 35, 40 |  |
| CA\_n3A-n8A-n40A | CA\_n3A-n8A  CA\_n3A-n40A  CA\_n8A-n40A | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n8 | n8 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n8A-n41A | CA\_n3A-n8A  CA\_n3A-n41A  CA\_n8A-n41A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n8 | n8 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n8A-n77A | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n3A-n8A-n77(2A) | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n3A-n8A-n78A | CA\_n3A-n8A  CA\_n3A-n78A  CA\_n8A-n78A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n8 | n8 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n8A-n78(2A) | CA\_n3A-n8A  CA\_n3A-n78A  CA\_n8A-n78A | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n8 | n8 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS 4 and 5 |  |
| CA\_n3(2A)-n8A-n78A | CA\_n3A-n8A  CA\_n3A-n78A  CA\_n8A-n78A | n3 | CA\_n3(2A)\_BCS0 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3(2A)-n8A-n78C | CA\_n3A-n8A  CA\_n3A-n78A  CA\_n3A-n78C  CA\_n8A-n78A  CA\_n8A-n78C | n3 | CA\_n3(2A)\_BCS0 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n3A-n8A-n78C | CA\_n78C  CA\_n3A-n8A  CA\_n3A-n78A  CA\_n3A-n78C  CA\_n8A-n78A  CA\_n8A-n78C | n3 | 5,10,15,20,25,30,35,40,45,50 | 4 and 5 |
|  |  | n8 | 5,10,15,20 |  |
|  |  | n78 | CA\_n78C\_BCS 4 and 5 |  |
| CA\_n3A-n8A-n79A | CA\_n3A-n8A  CA\_n3A-n79A  CA\_n8A-n79A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n3A-n18A-n28A | CA\_n3A-n18A  CA\_n3A-n28A  CA\_n18A-n28A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n28 | 5, 10 |  |
| CA\_n3A-n18A-n41A | n417,9  CA\_n3A-n41A7  CA\_n3A-n18A  CA\_n18A-n41A7 | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n3A-n18A-n77A | n777  CA\_n3A-n18A  CA\_n3A-n77A7  CA\_n18A-n77A7 | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n3A-n18A-n77(2A) | n777  CA\_n3A-n18A  CA\_n3A-n77A7  CA\_n18A-n77A7  CA\_n77(2A) | n3 | 5, 10, 15, 20 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n3A-n18A-n77(3A) | n777  CA\_n3A-n18A  CA\_n3A-n77A7  CA\_n18A-n77A7  CA\_n77(2A) | n3 | 5, 10, 15, 20 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n3A-n20A-n67A | n37  CA\_n3A-n20A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n20 | 5, 10, 15, 20 |  |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n20A-n28A | CA\_n3A-n20A  CA\_n3A-n28A  CA\_n20A-n28A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n20 | 5, 10, 15, 20 |  |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
| CA\_n3A-n20A-n41A | CA\_n3A-n20A  CA\_n3A-n41A  CA\_n20A-n41A | n3 | 5, 10, 15, 20, 25, 30, 45, 40, 45, 50 | 0 |
|  |  | n20 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 25, 30, 35, 40, 45, 50, 60, 70, 80, 90, 100 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n20A-n71A | CA\_n3A-n20A  CA\_n3A-n71A  CA\_n20A-n71A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n20 | 5, 10, 15, 20 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n3A-n20A-n77A | CA\_n3A-n20A  CA\_n3A-n77A  CA\_n20A-n77A | n3 | 5,10,15,20,25,30,35,40,45,50 | 0 |
|  |  | n20 | 5,10,15,20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n20A-n77(2A) | CA\_n3A-n20A  CA\_n3A-n77A  CA\_n20A-n77A | n3 | 5,10,15,20,25,30,35,40,45,50 | 0 |
|  |  | n20 | 5,10,15,20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n3A-n20A-n78A | CA\_n3A-n20A CA\_n3A-n78A CA\_n20A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n20 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n20A-n78(2A) | CA\_n3A-n20A CA\_n3A-n78A CA\_n20A-n78A  CA\_n78(2A) | n3 | See n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n20 | See n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n3A-n26A-n78A | n787,9  CA\_n3A-n26A  CA\_n3A-n78A7,14  CA\_n26A-n78A7,14 | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n26 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n26A-n78(2A) | n787,9  CA\_n3A-n26A  CA\_n3A-n78A7,14  CA\_n26A-n78A7,14  CA\_n78(2A)7 | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  | CA\_n78(2A) | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n26 | n26 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n3A-n26A-n78C | n787,9  CA\_n3A-n26A  CA\_n3A-n78A7,14  CA\_n26A-n78A7,14  CA\_n78C7 | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n3A-n26A-n78(A-C) | CA\_n78C  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(A-C)\_BCS1 |  |
| CA\_n3A-n26(2A)-n78A | n787,9  CA\_n3A-n26A  CA\_n3A-n78A7,14  CA\_n26A-n78A7,14  CA\_n26(2A) | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n26(2A)-n78(2A) | n787,9  CA\_n3A-n26A  CA\_n3A-n78A7,14  CA\_n26A-n78A7,14  CA\_n26(2A)  CA\_n78(2A)7 | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n3A-n26(2A)-n78C | n787,9  CA\_n3A-n26A  CA\_n3A-n78A7,14  CA\_n26A-n78A7,14  CA\_n26(2A)  CA\_n78C7 | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n3B-n26A-n78A | n787,9  CA\_n3A-n26A  CA\_n26A-n78A7,14  CA\_n3A-n78A7,14 | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3B-n26A-n78(2A) | n787,9  CA\_n3A-n26A  CA\_n3A-n78A7,14  CA\_n26A-n78A7,14  CA\_n78(2A)7 | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  | CA\_n78(2A) | n3 | CA\_n3B\_BCS4 and 5 | 4 and 5 |
|  |  | n26 | n26 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n3B-n26A-n78C | n787,9  CA\_n3A-n26A  CA\_n3A-n78A7,14  CA\_n26A-n78A7,14  CA\_n78C7 | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n3B-n26(2A)-n78A | n787,9  CA\_n3A-n26A  CA\_n3A-n78A7,14  CA\_n26A-n78A7,14  CA\_n26(2A) | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3B-n26(2A)-n78(2A) | n787,9  CA\_n3A-n26A  CA\_n3A-n78A7,14  CA\_n26A-n78A7,14  CA\_n26(2A)  CA\_n78(2A)7 | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3B-n26(2A)-n78C | n787,9  CA\_n3A-n26A  CA\_n3A-n78A7,14  CA\_n26A-n78A7,14  CA\_n26(2A)  CA\_n78C7 | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n3A-n28A-n38A | - | n3 | 5, 10, 15, 20, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n38 | 5, 10, 15, 20, 30, 40 |  |
| CA\_n3A-n28A-n40A | CA\_n3A-n28A  CA\_n3A-n40A  CA\_n28A-n40A | n3 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n40 | 20, 40 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35,40 | 1 |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n28A-n41A | n417,9  CA\_n3A-n28A  CA\_n3A-n41A7  CA\_n28A-n41A7 | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n3A-n28A  CA\_n3A-n41A  CA\_n28A-n41A | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n28A-n41B | CA\_n3A-n28A  CA\_n3A-n41A  CA\_n28A-n41A | n3 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | CA\_n41B\_BCS0 |  |
| CA\_n3A-n28A-n77A | n777,9  CA\_n3A-n28A  CA\_n3A-n77A7  CA\_n28A-n77A7 | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35,40 | 2 |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n28A-n77(2A) | n777,9  CA\_n3A-n28A  CA\_n3A-n77A7  CA\_n28A-n77A7  CA\_n77(2A)7 | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n3A-n28A-n77(3A) | n777,9  CA\_n3A-n28A  CA\_n3A-n77A7  CA\_n28A-n77A7  CA\_n77(2A) | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(3A)\_BCS4 and 5 |  |
| CA\_n3A-n28A-n78A | n37  n787,9  CA\_n3A-n28A  CA\_n3A-n78A7,13, 14  CA\_n28A-n78A7,13, 14 | n3 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 202 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n28 | 5, 10, 15, 202 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 | 2 |
|  |  | n28 | 5, 10 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n28A-n78C | n787,9  CA\_n78C7  CA\_n3A-n28A  CA\_n3A-n78A7,14  CA\_n28A-n78A7,14 | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n3A-n28A-n78(2A) | n37  n787,9  CA\_n3A-n28A  CA\_n3A-n78A7,13, 14  CA\_n28A-n78A7,13, 14 | n3 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 202 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n28 | 5, 10 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  | n37  n787,9  CA\_n78(2A) 7  CA\_n3A-n28A  CA\_n3A-n78A7,13, 14  CA\_n28A-n78A7,13, 14 | n3 | 5, 10, 15, 20, 25, 30, 40 | 2 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n3A-n28A-n78(A-C) | CA\_n78C  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n28A-n78A | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(A-C)\_BCS1 |  |
| CA\_n3B-n28A-n78A | n787,9  CA\_n3A-n28A  CA\_n3A-n78A7,14  CA\_n28A-n78A7,14 | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3B-n28A-n78(2A) | n787,9  CA\_n78(2A) 7  CA\_n3A-n28A  CA\_n3A-n78A7,14  CA\_n28A-n78A7,14 | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3B-n28A-n78C | n787,9  CA\_n78C7  CA\_n3A-n28A  CA\_n3A-n78A7,14  CA\_n28A-n78A7,14 | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
|  | CA\_n3B | n3 | CA\_n3B\_BCS1 | 1 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n3A-n28A-n79A | n797,9  CA\_n3A-n28A  CA\_n3A-n79A7  CA\_n28A-n79A7 | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n79 | 40, 50, 80, 100 |  |
|  | CA\_n3A-n28A  CA\_n3A-n79A  CA\_n28A-n79A | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n3A-n34A-n41A | CA\_n3A-n34A  CA\_n3A-n41A  CA\_n34A-n41A | n3 | See n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n34 | See n34 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n34A-n41C | CA\_n3A-n34A  CA\_n3A-n41A  CA\_n34A-n41A | n3 | See n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n34 | See n34 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
| CA\_n3A-n34A-n79A | CA\_n3A-n34A  CA\_n3A-n79A  CA\_n34A-n79A | n3 | See n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n34 | See n34 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n38A-n40A | - | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n38A-n78A | - | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n39A-n41A | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 35, 40 |  |
|  |  | n41 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n39A-n79A | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 35, 40 |  |
|  |  | n79 | 10, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n40A-n78A | CA\_n3A-n40A  CA\_n3A-n78A  CA\_n40A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n40A-n105A | CA\_n3A-n40A  CA\_n3A-n105A  CA\_n40A-n105A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n3A-n41A-n71A | CA\_n3A-n41A  CA\_n3A-n71A  CA\_n41A-n71A | n3 | 5,10,15,20,25,30,35,40,45,50 | 0 |
|  |  | n41 | 5,10,15,20,25,30,35,40,45,50,60,70,80,90,100 |  |
|  |  | n71 | 5,10,15,20 |  |
| CA\_n3A-n41A-n78C | CA\_n78C  CA\_n3A-n41A  CA\_n3A-n78A  CA\_n3A-n78C  CA\_n41A-n78A  CA\_n41A-n78C | n3 | 5,10,15,20,25,30,35,40,45,50 | 4 and 5 |
|  |  | n41 | 5,10,15,20,25,30,35,40,45,50,60,70,80,90,100 |  |
|  |  | n78 | CA\_n78C\_BCS4 and 5 |  |
| CA\_n3(2A)-n41A-n78A | CA\_n3A-n41A  CA\_n3A-n78A  CA\_n41A-n78A | n3 | CA\_n3(2A)\_BCS0 | 4 and 5 |
|  |  | n41 | 5,10,15,20,25,30,35,40,45,50,60,70,80,90,100 |  |
|  |  | n78 | 10,15,20,25,30,40,50,60,70,80,90,100 |  |
| CA\_n3(2A)-n41A-n78C | CA\_n3A-n41A  CA\_n3A-n78A  CA\_n41A-n78A  CA\_n41A-n78C | n3 | CA\_n3(2A)\_BCS0 | 4 and 5 |
|  |  | n41 | 5,10,15,20,25,30,35,40,45,50,60,70,80,90,100 |  |
|  |  | n78 | CA\_n78C\_BCS4 and 5 |  |
| CA\_n3A-n71A-n78A | CA\_n3A-n71A  CA\_n3A-n78A  CA\_n71A-n78A | n3 | 5,10,15,20,25,30,35,40,45,50 | 4 and 5 |
|  |  | n71 | 5,10,15,20 |  |
|  |  | n78 | 10,15,20,25,30,40,50,60,70,80,90,100 |  |
| CA\_n3(2A)-n71A-n78A | C A\_n3A-n71A  CA\_n3A-n78A  CA\_n71A-n78A | n3 | CA\_n3(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | 5,10,15,20 |  |
|  |  | n78 | 10,15,20,25,30,40,50,60,70,80,90,100 |  |
| CA\_n3(2A)-n71A-n78C | CA\_n78C  CA\_n3A-n71A  CA\_n3A-n78A  CA\_n3A-n78C  CA\_n71A-n78A  CA\_n71A-n78C | n3 | CA\_n3(2A)\_BCS0 | 0 |
|  |  | n71 | 5,10,15,20 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n3A-n71A-n78C | CA\_n78C  CA\_n3A-n71A  CA\_n3A-n78A  CA\_n3A-n78C  CA\_n71A-n78A  CA\_n71A-n78C | n3 | 5,10,15,20,25,30,35,40,45,50 | 4 and 5 |
|  |  | n71 | 5,10,15,20 |  |
|  |  | n78 | CA\_n78C\_BCS 4 and 5 |  |
| CA\_n3A-n77A-n79A4 | n777,9  n797,9  CA\_n3A-n77A7  CA\_n3A-n79A7  CA\_n77A-n79A7 | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n77(2A)-n79A4 | n777,9  n797,9  CA\_n77(2A)  CA\_n3A-n77A7  CA\_n3A-n79A7  CA\_n77A-n79A7 | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n77(3A)-n79A4 | CA\_n77(2A)  CA\_n3A-n77A  CA\_n3A-n79A  CA\_n77A-n79A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77(3A)\_BCS4 and 5 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n40A-n41A | CA\_n3A-n40A  CA\_n3A-n41A  CA\_n40A-n41A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n3 | See n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n40A-n41C | CA\_n3A-n40A  CA\_n3A-n41A  CA\_n40A-n41A | n3 | See n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | CA\_n41C\_BCS4 and 5 |  |
| CA\_n3A-n40A-n77A | CA\_n3A-n40A  CA\_n3A-n77A  CA\_n40A-n77A | n3 | 5, 10, 15, 20, 30, 35, 40, 45, 50 | 0 |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n40A-n77(2A) | CA\_n3A-n40A  CA\_n3A-n77A  CA\_n40A-n77A | n3 | 5, 10, 15, 20, 30, 35, 40, 45, 50 | 0 |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n3A-n40A-n79A | CA\_n3A-n40A  CA\_n3A-n79A  CA\_n40A-n79A | n3 | See n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n41A-n77A | n417,9  n777,9  CA\_n3A-n41A7  CA\_n3A-n77A7  CA\_n41A-n77A7 | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | - | n3 | See n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | See n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n41B-n77A | CA\_n3A-n41A  CA\_n3A-n77A  CA\_n41A-n77A | n3 | 5, 10, 15, 20 | 0 |
|  |  | n41 | CA\_n41B\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n41A-n77(2A) | n417,9  n777,9  CA\_n3A-n41A7  CA\_n3A-n77A7  CA\_n41A-n77A7  CA\_n77(2A)7 | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  | - | n3 | See n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n3A-n41A-n77(3A) | n417,9  n777,9  CA\_n3A-n41A7  CA\_n3A-n77A7  CA\_n41A-n77A7  CA\_n77(2A) | n3 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n3A-n41A-n78A | - | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n3A-n41A  CA\_n3A-n78A  CA\_n41A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n3A-n41A-n78(2A) | CA\_n3A-n41A  CA\_n3A-n78A  CA\_n41A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3A-n41A-n79A | n3  n417, 9  n797, 9  CA\_n3A-n41A7  CA\_n3A-n79A7  CA\_n41A-n79A7 | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30 | 1 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30 | 2 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n3 | See n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n41A-n79C | CA\_n3A-n41A  CA\_n3A-n79A  CA\_n41A-n79A | n3 | See n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | CA\_n79C\_BCS4 and 5 |  |
| CA\_n3A-n41C-n79A | CA\_n41C  CA\_n3A-n41A  CA\_n3A-n79A  CA\_n41A-n79A | n3 | See n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS4 and 5 |  |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n41C-n79C | CA\_n3A-n41A  CA\_n3A-n79A  CA\_n41A-n79A | n3 | See n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS4 and 5 |  |
|  |  | n79 | CA\_n79C\_BCS4 and 5 |  |
| CA\_n3A-n67A-n78A | CA\_n3A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n67A-n78(2A) | CA\_n78(2A)  CA\_n3A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n3A-n71A-n77A | CA\_n3A-n71A  CA\_n3A-n77A  CA\_n71A-n77A | n3 | 5,10,15,20,25,30,35,40,45,50 | 0 |
|  |  | n71 | 5,10,15,20 |  |
|  |  | n77 | 10,15,20,25,30,40,50,60,70,80,90,100 |  |
| CA\_n3A-n71A-n77(2A) | CA\_n3A-n71A  CA\_n3A-n77A  CA\_n71A-n77A | n3 | 5,10,15,20,25,30,35,40,45,50 | 0 |
|  |  | n71 | 5,10,15,20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n3A-n75A-n78A | CA\_n3A-n78A | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n75 | n75 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n78A-n79A5 | n787,9 | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  | n797  CA\_n3A-n78A7  CA\_n3A-n79A7  CA\_n78A-n79A5,7 | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  | CA\_n3A-n78A CA\_n3A-n79A  CA\_n78A-n79A | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n78A-n79C | - | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n3B-n78A-n79A | - | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n3B-n78A-n79C | - | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n3(2A)-n78A-n79A | - | n3 | CA\_n3(2A)\_BCS1 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n3(2A)-n78A-n79C | - | n3 | CA\_n3(2A)\_BCS1 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n3A-n78A-n105A | CA\_n3A-n78A  CA\_n3A-n105A  CA\_n78A-n105A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n5A-n7A-n25A | CA\_n5A-n7A  CA\_n5A-n25A  CA\_n7A-n25A | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 35, 40, 45 |  |
| CA\_n5A-n7A-n25(2A) | CA\_n5A-n7A  CA\_n5A-n25A  CA\_n7A-n25A | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
| CA\_n5A-n7A-n28A | - | n5 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
| CA\_n5A-n7A-n40A | CA\_n5A-n7A  CA\_n5A-n40A  CA\_n7A-n40A | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n7A-n66A | CA\_n5A-n7A  CA\_n5A-n66A  CA\_n7A-n66A | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 35, 40, 45 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n7A-n77A | n777,9  CA\_n5A-n7A  CA\_n5A-n77A7  CA\_n7A-n77A7 | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n5 | See n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | See n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | See n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n7A-n77(2A) | n777,9  CA\_n77(2A)7  CA\_n5A-n7A  CA\_n5A-n77A7  CA\_n7A-n77A7 | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n5 | See n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | See n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n5A-n7A-n77(3A) | n777,9  CA\_n77(2A)7  CA\_n5A-n7A  CA\_n5A-n77A7  CA\_n7A-n77A7 | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
| CA\_n5A-n7A-n78A | n787,9  CA\_n5A-n78A7  CA\_n7A-n78A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n5A-n7A  CA\_n5A-n78A  CA\_n7A-n78A | n5 | 5, 10, 15, 20 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n7A-n78(2A) | CA\_n5A-n7A  CA\_n5A-n78A  CA\_n7A-n78A | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n5A-n7A-n78C | CA\_n78C  CA\_n5A-n7A  CA\_n5A-n78A  CA\_n7A-n78A | n5 | See n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | See n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78C\_BCS4 and 5 |  |
| CA\_n5A-n7A-n78(A-C) | CA\_n78C  CA\_n5A-n7A  CA\_n5A-n78A  CA\_n7A-n78A | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n78 | CA\_n78(A-C)\_BCS1 |  |
| CA\_n5A-n7B-n78A | n787,9  CA\_n5A-n78A7  CA\_n7A-n78A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n5A-n7A  CA\_n5A-n78A  CA\_n7A-n78A  CA\_n7B | n5 | 5, 10, 15, 20 | 1 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 90, 100 |  |
| CA\_n5A-n7A-n105A | CA\_n5A-n7A  CA\_n5A-n105A  CA\_n7A-n105A | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n5A-n12A-n77A | n777  CA\_n5A-n12A  CA\_n5A-n77A7  CA\_n12A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n12A-n77(2A) | n777  CA\_n5A-n12A CA\_n5A-n77A7 CA\_n12A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n14A-n77A | n777  CA\_n5A-n14A  CA\_n5A-n77A7  CA\_n14A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n14A-n77(2A) | n777  CA\_n5A-n14A CA\_n5A-n77A7 CA\_n14A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n25A-n29A | CA\_n5A-n25A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n29 | 5, 10 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n29 | n29 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n25A-n41A | CA\_n5A-n25A  CA\_n5A-n41A  CA\_n25A-n41A | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 35, 40, 45 |  |
|  |  | n41 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
| CA\_n5A-n25(2A)-n41A | CA\_n5A-n25A  CA\_n5A-n41A  CA\_n25A-n41A | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n25 | CA\_n25(2A) |  |
|  |  | n41 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
| CA\_n5A-n25A-n66A | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n25A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n25(2A)-n66A | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n25A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n5A-n25A-n66(2A) | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n25A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n5A-n25(2A)-n66(2A) | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n25A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n5A-n25A-n77A | n777,9  CA\_n5A-n25A | n5 | 5, 10, 15, 20 | 0 |
|  | CA\_n5A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  | CA\_n25A-n77A7 | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n25(2A)-n77A | n777,9  CA\_n5A-n25A  CA\_n5A-n77A7  CA\_n25A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n25A-n77(2A) | n777,9  CA\_n77(2A)7  CA\_n5A-n25A  CA\_n5A-n77A7  CA\_n25A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n25A-n77(3A) | n777,9  CA\_n77(2A)7  CA\_n5A-n25A  CA\_n5A-n77A7  CA\_n25A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n5A-n25(2A)-n77(2A) | n777,9  CA\_n5A-n25A  CA\_n5A-n77A7  CA\_n25A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n25A-n78A | n787,9  CA\_n5A-n25A  CA\_n5A-n78A7  CA\_n25A-n78A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n25(2A)-n78A | n787,9  CA\_n5A-n25A  CA\_n5A-n78A7  CA\_n25A-n78A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n25A-n78(2A) | n787,9  CA\_n5A-n25A  CA\_n5A-n78A7  CA\_n25A-n78A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n5A-n25(2A)-n78(2A) | n787,9  CA\_n5A-n25A  CA\_n5A-n78A7  CA\_n25A-n78A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n5A-n28A-n78A | CA\_n5A-n28A  CA\_n5A-n78A  CA\_n28A-n78A | n5 | See n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | See n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n28A-n79A | CA\_n5A-n28A  CA\_n5A-n79A  CA\_n28A-n79A | n5 | See n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | See n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n28A-n105A | CA\_n5A-n28A  CA\_n5A-n105A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n5A-n29A-n66A | CA\_n5A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n29 | n29 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n29A-n77A | n777  CA\_n5A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n29A-n77(2A) | n777  CA\_n5A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n30A-n66A | CA\_n5A-n30A  CA\_n5A-n66A  CA\_n30A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n30 | n30 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n30A-n66(2A) | CA\_n5A-n30A  CA\_n5A-n66A  CA\_n30A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
| CA\_n5A-n30A-n66(3A) | CA\_n5A-n30A  CA\_n5A-n66A  CA\_n30A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n5A-n30A-n77A | n777,9  CA\_n5A-n30A  CA\_n5A-n77A7  CA\_n30A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n30 | n30 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n30A-n77(2A) | n777,9  CA\_n5A-n30A CA\_n5A-n77A7 CA\_n30A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n30 | n30 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n5A-n40A-n78A | CA\_n5A-n40A  CA\_n5A-n78A  CA\_n40A-n78A | n5 | 5, 10, 15, 20, 251 | 0 |
|  |  | n40 | 58, 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90,100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90,100 |  |
| CA\_n5A-n40A-n105A | CA\_n5A-n40A CA\_n5A-n105A CA\_n40A-n105A | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n5A-n41A-n66A | CA\_n5A-n41A CA\_n5A-n66A CA\_n41A-n66A | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 35, 40, 45 |  |
| CA\_n5A-n41A-n77A | CA\_n5A-n41A  CA\_n5A-n77A  CA\_n41A-n77A | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n41 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n41A-n77(2A) | CA\_n5A-n41A  CA\_n5A-n77A  CA\_n41A-n77A | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n41 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
| CA\_n5A-n48A-n66A | CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5B-n48A-n66A | CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A  CA\_n5B | n5 | CA\_n5B\_BCS4 and 5 | 4 and 5 |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n48(A-B)-n66A | CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n5 | 5, 10, 15, 20, 251 | 0 |
|  |  | n48 | CA\_n48(A-B)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n5 | 5, 10, 15, 20, 251 | 1 |
|  |  | n48 | CA\_n48(A-B)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | CA\_n48(A-B)\_BCS4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n48B-n66A | CA\_n48B  CA\_n5A-n48A  CA\_n5A-n48B  CA\_n5A-n66A  CA\_n48A-n66A  CA\_n48B-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n5 | 5, 10, 15, 20 | 2 |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | CA\_n48B\_BCS4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5B-n48B-n66A | CA\_n48B  CA\_n5A-n48A  CA\_n5A-n48B  CA\_n5A-n66A  CA\_n5B  CA\_n48A-n66A  CA\_n48B-n66A | n5 | CA\_n5B\_BCS4 and 5 | 4 and 5 |
|  |  | n48 | CA\_n48B\_BCS4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n48(2A)-n66A | CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | CA\_n48(2A)\_BCS4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5B-n48(2A)-n66A | CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5B  CA\_n48A-n66A | n5 | CA\_n5B\_BCS4 and 5 | 4 and 5 |
|  |  | n48 | CA\_n48(2A)\_BCS4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n48A-n66(2A) | CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 |  |
| CA\_n5A-n48B-n66(2A) | CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5A-n48B  CA\_n48A-n66A  CA\_n48B-n66A  CA\_n48B | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | CA\_n48B\_BCS4 and 5 |  |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 |  |
| CA\_n5A-n48(2A)-n66(2A) | CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | CA\_n48(2A)\_BCS4 and 5 |  |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 |  |
| CA\_n5B-n48A-n66(2A) | CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5B  CA\_n48A-n66A | n5 | CA\_n5B\_BCS4 and 5 | 4 and 5 |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 |  |
| CA\_n5B-n48(2A)-n66(2A) | CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5B  CA\_n48A-n66A | n5 | CA\_n5B\_BCS4 and 5 | 4 and 5 |
|  |  | n48 | CA\_n48(2A)\_BCS4 and 5 |  |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 |  |
| CA\_n5B-n48B-n66(2A) | CA\_n5A-n48A  CA\_n5A-n48B  CA\_n5A-n66A  CA\_n5B  CA\_n48A-n66A  CA\_n48B-n66A  CA\_n48B | n5 | CA\_n5B\_BCS4 and 5 | 4 and 5 |
|  |  | n48 | CA\_n48B\_BCS4 and 5 |  |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 |  |
| CA\_n5A-n48A-n77A | n777,9  CA\_n5A-n48A  CA\_n5A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n5A-n48A  CA\_n5A-n77A | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5B-n48A-n77A | CA\_n5A-n48A  CA\_n5A-n77A  CA\_n5B | n5 | CA\_n5B\_BCS4 and 5 | 4 and 5 |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n48A-n77C | n777,9  CA\_n5A-n48A  CA\_n5A-n77A7  CA\_n77C | n5 | 5, 10, 15, 20, 251 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n5 | 5, 10, 15, 20, 251 | 1 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  | CA\_n5A-n48A  CA\_n5A-n77A  CA\_n5A-n77C  CA\_n77C | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77C\_BCS4 and 5 |  |
| CA\_n5A-n48B-n77A | n777,9  CA\_n5A-n48A  CA\_n5A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n5 | 5, 10, 15, 20 | 2 |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n5A-n48A  CA\_n5A-n48B  CA\_n5A-n77A  CA\_n48B | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | CA\_n48B\_BCS4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n48B-n77C | n777,9  CA\_n5A-n48A  CA\_n5A-n77A7  CA\_n77C | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  |  | n5 | 5, 10, 15, 20 | 2 |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n5 | 5, 10, 15, 20 | 3 |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  | CA\_n5A-n48A  CA\_n5A-n48B  CA\_n5A-n77A  CA\_n5A-n77C  CA\_n48B  CA\_n77C | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | CA\_n48B\_BCS4 and 5 |  |
|  |  | n77 | CA\_n77C\_BCS4 and 5 |  |
| CA\_n5A-n48(2A)-n77A | n777,9  CA\_n5A-n48A  CA\_n5A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n5A-n48A  CA\_n5A-n77A | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | CA\_n48(2A)\_BCS4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n48(2A)-n77C | n777,9  CA\_n5A-n48A  CA\_n5A-n77A7  CA\_n77C | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  |  | n5 | 5, 10, 15, 20 | 2 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n5 | 5, 10, 15, 20 | 3 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  | CA\_n5A-n48A  CA\_n5A-n77A  CA\_n5A-n77C  CA\_n77C | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | CA\_n48(2A)\_BCS4 and 5 |  |
|  |  | n77 | CA\_n77C\_BCS4 and 5 |  |
| CA\_n5B-n48A-n77C | CA\_n5A-n48A  CA\_n5A-n77A  CA\_n5A-n77C  CA\_n5B  CA\_n77C | n5 | CA\_n5B\_BCS4 and 5 | 4 and 5 |
|  |  | n48 | n48 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77C\_BCS4 and 5 |  |
| CA\_n5B-n48(2A)-n77A | CA\_n5A-n48A  CA\_n5A-n77A  CA\_n5B | n5 | CA\_n5B\_BCS4 and 5 | 4 and 5 |
|  |  | n48 | CA\_n48(2A)\_BCS4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5B-n48(2A)-n77C | CA\_n5A-n48A  CA\_n5A-n77A  CA\_n5A-n77C  CA\_n5B  CA\_n77C | n5 | CA\_n5B\_BCS4 and 5 | 4 and 5 |
|  |  | n48 | CA\_n48(2A)\_BCS4 and 5 |  |
|  |  | n77 | CA\_n77C\_BCS4 and 5 |  |
| CA\_n5B-n48B-n77A | CA\_n5A-n48A  CA\_n5A-n48B  CA\_n5A-n77A  CA\_n5B  CA\_n48B | n5 | CA\_n5B\_BCS4 and 5 | 4 and 5 |
|  |  | n48 | CA\_n48B\_BCS4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5B-n48B-n77C | CA\_n5A-n48A  CA\_n5A-n48B  CA\_n5A-n77A  CA\_n5A-n77C  CA\_n5B  CA\_n48B  CA\_n77C | n5 | CA\_n5B\_BCS4 and 5 | 4 and 5 |
|  |  | n48 | CA\_n48B\_BCS4 and 5 |  |
|  |  | n77 | CA\_n77C\_BCS4 and 5 |  |
| CA\_n5A-n66A-n77A | n777,9  CA\_n5A-n66A  CA\_n5A-n77A7  CA\_n66A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5B-n66A-n77A | CA\_n5A-n66A  CA\_n5A-n77A  CA\_n66A-n77A  CA\_n5B | n5 | CA\_n5B\_BCS4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n66(2A)-n77A | n777,9  CA\_n5A-n66A  CA\_n5A-n77A7  CA\_n66A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n5A-n66A  CA\_n5A-n77A  CA\_n66A-n77A | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n66(2A)-n77C | CA\_n5A-n66A  CA\_n5A-n77A  CA\_n5A-n77C  CA\_n66A-n77A  CA\_n66A-n77C  CA\_n77C | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 |  |
|  |  | n77 | CA\_n77C\_BCS4 and 5 |  |
| CA\_n5B-n66(2A)-n77A | CA\_n5A-n66A  CA\_n5A-n77A  CA\_n66A-n77A  CA\_n5B | n5 | CA\_n5B\_BCS4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5B-n66(2A)-n77C | CA\_n5A-n66A  CA\_n5A-n77A  CA\_n5A-n77C  CA\_n5B  CA\_n66A-n77A  CA\_n66A-n77C  CA\_n77C | n5 | CA\_n5B\_BCS4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 |  |
|  |  | n77 | CA\_n77C\_BCS4 and 5 |  |
| CA\_n5A-n66(2A)-n77(2A) | n777,9  CA\_n5A-n66A  CA\_n5A-n77A7  CA\_n66A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 |  |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n5A-n66(3A)-n77A | n777,9  CA\_n5A-n66A  CA\_n66A-n77A7  CA\_n5A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n66(3A)-n77(2A) | n777,9  CA\_n5A-n66A  CA\_n66A-n77A7  CA\_n5A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n66A-n77C | n777,9  CA\_n5A-n66A  CA\_n5A-n77A7  CA\_n66A-n77A7  CA\_n77C | n5 | 5, 10, 15, 20, 251 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n5 | 5, 10, 15, 20, 251 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  | CA\_n5A-n66A  CA\_n5A-n77A  CA\_n5A-n77C  CA\_n66A-n77A  CA\_n66A-n77C  CA\_n77C | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77C\_BCS4 and 5 |  |
| CA\_n5B-n66A-n77C | CA\_n5A-n66A  CA\_n5A-n77A  CA\_n5A-n77C  CA\_n5B  CA\_n66A-n77A  CA\_n66A-n77C  CA\_n77C | n5 | CA\_n5B\_BCS4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77C\_BCS4 and 5 |  |
| CA\_n5A-n66A-n77(2A) | n777,9  CA\_n5A-n66A  CA\_n5A-n77A7  CA\_n66A-n77A7  CA\_n77(2A)7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n66 | 5, 10, 15, 20, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n5A-n66A-n77(3A) | CA\_n77(2A)  CA\_n5A-n66A  CA\_n5A-n77A7  CA\_n66A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(3A)\_BCS4 and 5 |  |
| CA\_n5A-n66A-n78A | CA\_n5A-n66A  CA\_n5A-n78A  CA\_n66A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n66(2A)-n78A | CA\_n5A-n66A CA\_n5A-n78A CA\_n66A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n66A-n78(2A) | CA\_n5A-n66A CA\_n5A-n78A CA\_n66A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n5A-n66(2A)-n78(2A) | CA\_n5A-n66A CA\_n5A-n78A CA\_n66A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n5A-n78A-n79A | CA\_n5A-n78A  CA\_n5A-n79A  CA\_n78A-n79A | n5 | See n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n78A-n105A | CA\_n5A-n78A CA\_n5A-n105A CA\_n78A-n105A | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n7A-n8A-n28A | - | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
| CA\_n7A-n8A-n40A | CA\_n7A-n8A  CA\_n7A-n40A  CA\_n8A-n40A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n8 | n8 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n8A-n78A | CA\_n7A-n8A  CA\_n7A-n78A  CA\_n8A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n8A-n78A | CA\_n7A-n8A  CA\_n7A-n78A  CA\_n8A-n78A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n12A-n25A | - | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n12 | n12 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n12A-n66A | - | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 35, 40, 45 |  |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n12 | n12 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n12A-n71A | CA\_n7A-n12A  CA\_n7A-n71A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n7A-n12A-n77A | - | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n12 | n12 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n20A-n67A | CA\_n7A-n20A | n7 | See n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n20 | See n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n67 | See n67 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n20A-n78A | CA\_n7A-n20A CA\_n7A-n78A CA\_n20A-n78A | n7 | See n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n20 | See n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n20A-n78(2A) | CA\_n7A-n20A CA\_n7A-n78A CA\_n20A-n78A  CA\_n78(2A) | n7 | See n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n20 | See n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n7A-n25A-n29A | CA\_n7A-n25A | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n29 | n29 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n25A-n66A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n25A-n66A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n25(2A)-n66A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n25A-n66A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n7A-n25(2A)-n66(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n25A-n66A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n7A-n25A-n66(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n25A-n66A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n7(2A)-n25A-n66A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n25A-n66A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n7(2A)-n25(2A)-n66A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n25A-n66A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n7(2A)-n25A-n66(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n25A-n66A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n7(2A)-n25(2A)-n66(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n25A-n66A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n7A-n25A-n71A | - | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n25A-n77A | n777,9  CA\_n7A-n25A  CA\_n7A-n77A7  CA\_n25A-n77A7 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n7A-n25A  CA\_n7A-n77A  CA\_n25A-n77A | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n25(2A)-n77A | n777,9  CA\_n7A-n25A  CA\_n7A-n77A7  CA\_n25A-n77A7 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n25A-n77(2A) | n777,9  CA\_n77(2A)7  CA\_n7A-n25A  CA\_n7A-n77A7  CA\_n25A-n77A7 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  | CA\_n77(2A)  CA\_n7A-n25A  CA\_n7A-n77A  CA\_n25A-n77A | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n7A-n25A-n77(3A) | n777,9  CA\_n77(2A)7  CA\_n7A-n25A  CA\_n7A-n77A7  CA\_n25A-n77A7 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
|  | CA\_n77(2A)  CA\_n7A-n25A  CA\_n7A-n77A  CA\_n25A-n77A | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(3A)\_BCS4 and 5 |  |
| CA\_n7A-n25(2A)-n77(2A) | n777,9  CA\_n7A-n25A  CA\_n7A-n77A7  CA\_n25A-n77A7 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7(2A)-n25A-n77A | n777,9  CA\_n7A-n25A  CA\_n7A-n77A7  CA\_n25A-n77A7 | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n25(2A)-n77A | n777,9  CA\_n7A-n25A  CA\_n7A-n77A7  CA\_n25A-n77A7 | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n25A-n77(2A) | n777,9  CA\_n7A-n25A  CA\_n7A-n77A7  CA\_n25A-n77A7 | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7(2A)-n25(2A)-n77(2A) | n777,9  CA\_n7A-n25A  CA\_n7A-n77A7  CA\_n25A-n77A7 | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7A-n25A-n78A | CA\_n7A-n25A  CA\_n7A-n78A  CA\_n25A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 904, 100 |  |
| CA\_n7(2A)-n25A-n78A | - | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 904, 100 |  |
| CA\_n7A-n25(2A)-n78A | - | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 904, 100 |  |
| CA\_n7(2A)-n25(2A)-n78A | - | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 904, 100 |  |
| CA\_n7A-n25A-n78(2A) | CA\_n7A-n25A  CA\_n7A-n78A  CA\_n25A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7(2A)-n25A-n78(2A) | - | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n7A-n25(2A)-n78(2A) | - | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n7(2A)-n25(2A)-n78(2A) | - | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n7A-n26A-n78A | n787,9  CA\_n7A-n26A  CA\_n7A-n78A7,14  CA\_n26A-n78A7,14 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n26 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n26A-n78(2A) | n787,9  CA\_n78(2A) 7  CA\_n7A-n26A  CA\_n7A-n78A7,14  CA\_n26A-n78A7,14 | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  | CA\_n78(2A) | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n26 | n26 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n7A-n26A-n78C | n787,9  CA\_n7A-n26A  CA\_n7A-n78A7,14  CA\_n26A-n78A7,14  CA\_n78C7 | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n7A-n26A-n78(A-C) | CA\_n78C  CA\_n7A-n26A  CA\_n7A-n78A  CA\_n26A-n78A | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(A-C)\_BCS1 |  |
| CA\_n7A-n26(2A)-n78A | n787,9  CA\_n7A-n26A  CA\_n7A-n78A7,14  CA\_n26A-n78A7,14  CA\_n26(2A) | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n26(2A)-n78(2A) | n787,9  CA\_n78(2A) 7  CA\_n7A-n26A  CA\_n7A-n78A7,14  CA\_n26A-n78A7,14  CA\_n26(2A) | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n7A-n26(2A)-n78C | n787,9  CA\_n7A-n26A  CA\_n7A-n78A7,14  CA\_n26A-n78A7,14  CA\_n26(2A)  CA\_n78C7 | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n7B-n26A-n78A | n787,9  CA\_n7A-n26A  CA\_n7A-n78A7,14  CA\_n26A-n78A7,14  CA\_n7B | n7 | CA\_n7B\_BCS0 | 0 |
|  |  | n26 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7B-n26A-n78(2A) | n787,9  CA\_n78(2A) 7  CA\_n7A-n26A  CA\_n7A-n78A7,14  CA\_n7B  CA\_n26A-n78A7,14 | n7 | CA\_n7B\_BCS0 | 0 |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  | CA\_n78(2A) | n7 | CA\_n7B\_BCS4 and 5 | 4 and 5 |
|  |  | n26 | n26 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n7B-n26A-n78C | n787,9  CA\_n7A-n26A  CA\_n7A-n78A7,14  CA\_n7B  CA\_n26A-n78A7,14  CA\_n78C7 | n7 | CA\_n7B\_BCS0 | 0 |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n7B-n26(2A)-n78A | n787,9  CA\_n7A-n26A  CA\_n7A-n78A7,14  CA\_n26A-n78A7,14  CA\_n7B  CA\_n26(2A) | n7 | CA\_n7B\_BCS0 | 0 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7B-n26(2A)-n78(2A) | n787,9  CA\_n78(2A) 7  CA\_n7A-n26A  CA\_n7A-n78A7,14  CA\_n26A-n78A7,14  CA\_n7B  CA\_n26(2A) | n7 | CA\_n7B\_BCS0 | 0 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n7B-n26(2A)-n78C | n787,9  CA\_n7A-n26A  CA\_n7A-n78A7,14  CA\_n26A-n78A7,14  CA\_n7B  CA\_n26(2A)  CA\_n78C7 | n7 | CA\_n7B\_BCS0 | 0 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n7A-n28A-n38A11 | - | n7 | 5, 10, 15, 20, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n38 | 5, 10, 15, 20, 30, 40 |  |
| CA\_n7A-n28A-n40A | CA\_n7A-n28A  CA\_n7A-n40A  CA\_n28A-n40A | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n28A-n78A | n77  n787,9  CA\_n7A-n78A7,14  CA\_n28A-n78A7,14 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  | n77  n787,9  CA\_n7A-n28A  CA\_n7A-n78A7,14  CA\_n28A-n78A7,14 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 90, 100 |  |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n28A-n78(2A) | n77  n787,9  CA\_n7A-n28A  CA\_n7A-n78A7,14  CA\_n28A-n78A7,14  CA\_n78(2A)7 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n7A-n28A-n78C | n787,9  CA\_n78C7  CA\_n7A-n28A  CA\_n7A-n78A7,14  CA\_n28A-n78A7,14 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n7A-n28A-n78(A-C) | CA\_n78C  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(A-C)\_BCS1 |  |
| CA\_n7B-n28A-n78A | n787,9  CA\_n7A-n78A7,14  CA\_n28A-n78A7,14 | n7 | CA\_n7B\_BCS0 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n7A-n28A  CA\_n7A-n78A7,14  CA\_n28A-n78A7,14  CA\_n7B | n7 | CA\_n7B\_BCS0 | 1 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 90, 100 |  |
| CA\_n7B-n28A-n78(2A) | n787,9  CA\_n7B  CA\_n7A-n28A  CA\_n7A-n78A7,14  CA\_n28A-n78A7,14  CA\_n78(2A)7 | n7 | CA\_n7B\_BCS0 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7B-n28A-n78C | n787  CA\_n7B  CA\_n78C7  CA\_n7A-n28A  CA\_n7A-n78A7,14  CA\_n28A-n78A7,14 | n7 | CA\_n7B\_BCS0 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n7A-n29A-n66A | CA\_n7A-n66A | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n29 | n29 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n29A-n77A | CA\_n7A-n77A | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n29 | n29 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n29A-n77(2A) | CA\_n7A-n77A  CA\_n77(2A) | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n29 | n29 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n7A-n29A-n77(3A) | CA\_n7A-n77A  CA\_n77(2A) | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n29 | n29 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(3A)\_BCS4 and 5 |  |
| CA\_n7A-n38A-n78A10 | - | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n40A-n78A | CA\_n7A-n40A  CA\_n7A-n78A  CA\_n40A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n40 | 5, 10, 15, 20, 30, 40, 50, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n40A-n79A | CA\_n7A-n40A  CA\_n7A-n79A  CA\_n40A-n79A | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n40A-n105A | CA\_n7A-n40A  CA\_n7A-n105A  CA\_n40A-n105A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n40 | 5,10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n7A-n46A-n78A | CA\_n7A-n46A CA\_n7A-n78A CA\_n46A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | 20, 40, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n46C-n78A | CA\_n7A-n46A CA\_n7A-n78A CA\_n46A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | CA\_n46C\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n46D-n78A | CA\_n7A-n46A CA\_n7A-n78A CA\_n46A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | CA\_n46D\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n46(2A)-n78A | CA\_n7A-n46A CA\_n7A-n78A CA\_n46A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | CA\_n46(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n46(2A)-n78(2A) | CA\_n7A-n46A CA\_n7A-n78A CA\_n46A-n78A  CA\_n78(2A) | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | CA\_n46(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7A-n46A-n78(2A) | CA\_n7A-n46A CA\_n7A-n78A CA\_n46A-n78A  CA\_n78(2A) | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | 20, 40, 60, 80 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7A-n46C-n78(2A) | CA\_n7A-n46A CA\_n7A-n78A CA\_n46A-n78A  CA\_n78(2A) | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | CA\_n46C\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7A-n46D-n78(2A) | CA\_n7A-n46A CA\_n7A-n78A CA\_n46A-n78A  CA\_n78(2A) | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | CA\_n46D\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7A-n66A-n71A | CA\_n7A-n66A  CA\_n7A-n71A  CA\_n66A-n71A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n66A-n77A | n777,9  CA\_n7A-n66A  CA\_n7A-n77A7  CA\_n66A-n77A7 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n66(2A)-n77A | n777,9  CA\_n7A-n66A  CA\_n7A-n77A7  CA\_n66A-n77A7 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n66A-n77(2A) | n777,9  CA\_n77(2A)  CA\_n7A-n66A CA\_n7A-n77A7 CA\_n66A-n77A7 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n7A-n66A-n77(3A) | n777,9  CA\_n77(2A)7  CA\_n77(2A) 7  CA\_n7A-n66A  CA\_n7A-n77A7  CA\_n66A-n77A7 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(3A)\_BCS4 and 5 |  |
| CA\_n7A-n66(2A)-n77(2A) | n777,9  CA\_n7A-n66A CA\_n7A-n77A7 CA\_n66A-n77A7 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7(2A)-n66A-n77A | n777,9  CA\_n7A-n66A CA\_n7A-n77A7 CA\_n66A-n77A7 | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n66(2A)-n77A | n777,9  CA\_n7A-n66A CA\_n7A-n77A7 CA\_n66A-n77A7 | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n66A-n77(2A) | n777,9  CA\_n7A-n66A CA\_n7A-n77A7 CA\_n66A-n77A7 | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7(2A)-n66(2A)-n77(2A) | n777,9  CA\_n7A-n66A CA\_n7A-n77A7 CA\_n66A-n77A7 | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7A-n66A-n78A | n787,9  CA\_n7A-n66A  CA\_n7A-n78A7  CA\_n66A-n78A7 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n66A-n78(2A) | CA\_n7A-n66A  CA\_n7A-n78A  CA\_n66A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS1 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7(2A)-n66A-n78A | CA\_n7A-n66A  CA\_n7A-n78A  CA\_n66A-n78A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n66(2A)-n78A | CA\_n7A-n66A  CA\_n7A-n78A  CA\_n66A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n66(2A)-n78A | CA\_n7A-n66A  CA\_n7A-n78A  CA\_n66A-n78A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n66(2A)-n78(2A) | CA\_n7A-n66A  CA\_n7A-n78A  CA\_n66A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7(2A)-n66A-n78(2A) | CA\_n7A-n66A  CA\_n7A-n78A  CA\_n66A-n78A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7(2A)-n66(2A)-n78(2A) | CA\_n7A-n66A  CA\_n7A-n78A  CA\_n66A-n78A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7A-n67A-n78A | CA\_n7A-n78A | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n67A-n78(2A) | CA\_n7A-n78A CA\_n78(2A) | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n7A-n71A-n77A | n777,9  CA\_n7A-n71A  CA\_n7A-n77A7  CA\_n71A-n77A7 | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n71 | 5, 10, 15, 20, 25, 30, 35 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n7 | See n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | See n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | See n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n71A-n77(2A) | n777,9  CA\_n77(2A)7  CA\_n7A-n71A  CA\_n7A-n77A7  CA\_n71A-n77A7 | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n71 | 5, 10, 15, 20, 25, 30, 35 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n7 | See n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | See n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n7A-n71A-n77(3A) | n777,9  CA\_n77(2A)7  CA\_n7A-n71A  CA\_n7A-n77A7  CA\_n71A-n77A7 | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n71 | 5, 10, 15, 20, 25, 30, 35 |  |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
| CA\_n7A-n75A-n78A | CA\_n7A-n78A | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n75 | n75 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n78A-n79A | CA\_n7A-n78A  CA\_n7A-n79A  CA\_n78A-n79A | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n78A-n102A | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n78A-n102A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n7A-n78A-n102B | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n7A-n102B  CA\_n78A-n102A  CA\_n78A-n102B | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n7A-n78A-n102C | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n7A-n102C  CA\_n78A-n102A  CA\_n78A-n102C | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n7A-n78A-n102D | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n78A-n102A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n7A-n78A-n102E | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n78A-n102A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n7A-n78A-n102(2A) | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n78A-n102A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n7A-n78(2A)-n102A | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n78A-n102A  CA\_n78(2A) | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n7A-n78(2A)-n102B | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n7A-n102B  CA\_n78A-n102A  CA\_n78A-n102B  CA\_n78(2A) | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n7A-n78(2A)-n102C | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n7A-n102C  CA\_n78A-n102A  CA\_n78A-n102C  CA\_n78(2A) | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n7A-n78(2A)-n102D | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n78A-n102A  CA\_n78(2A) | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n7A-n78(2A)-n102E | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n78A-n102A  CA\_n78(2A) | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n7A-n78(2A)-n102(2A) | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n78A-n102A  CA\_n78(2A) | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n7A-n78A-n105A | CA\_n7A-n78A  CA\_n7A-n105A  CA\_n78A-n105A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |

---Unchanged texts are omitted ---

### 7.3A.5 Reference sensitivity exceptions due to intermodulation interference due to 2UL CA

---Unchanged texts are omitted ---

Table 7.3A.5-2a: 3DL/2UL interband Reference sensitivity QPSK PREFSENS and uplink/downlink configurations for PC2 CA

| Band / Channel bandwidth / NRB / Duplex mode | | | | | | | | Source of IMD |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| NR CA band combination | NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | Duplex mode |  |
| CA\_n1-n3-n77 | n1 | 1950 | 5 | 25 | 2140 | N/A | FDD | N/A |
|  | n3 | N/A | 5 | N/A | 1807.5 | 37.5 | FDD | IMD21,2 |
|  | n77 | 3757.5 | 10 | 50 | 3757.5 | N/A | TDD | N/A |
|  | n1 | N/A | 5 | N/A | 2140 | 37.0 | FDD | IMD21 |
|  | n3 | 1775 | 5 | 25 | 1870 | N/A | FDD | N/A |
|  | n77 | 3915 | 10 | 50 | 3915 | N/A | TDD | N/A |
| CA\_n1-n3-n28 | n3 | 1780 | 5 | 25 | 1875 | N/A | FDD | N/A |
|  | n28 | 710.5 | 5 | 25 | 765.5 | N/A | FDD | N/A |
|  | n1 | N/A | 5 | N/A | 2139 | 22.7 | FDD | IMD4 |
| CA\_n1-n3-n78 | n1 | 1950 | 5 | 25 | 2140 | N/A | FDD | N/A |
|  | n3 | N/A | 5 | N/A | 1830 | 33.9 | FDD | IMD2 |
|  | n78 | 3780 | 10 | 50 | 3780 | N/A | TDD | N/A |
| CA\_n1-n3-n79 | n3 | 1750 | 5 | 25 | 1845 | N/A | FDD | N/A |
|  | n79 | 4860 | 40 | 216 | 4860 | N/A | TDD | N/A |
|  | n1 | N/A | 5 | N/A | 2140 | 18.7 | FDD | IMD5 |
| CA\_n1-n7-n20 | n1 | 1940 | 5 | 25 | 2130 | N/A | FDD | N/A |
|  | n7 | 2510 | 10 | 50 | 2630 | N/A | FDD | N/A |
|  | n20 | N/A | 5 | N/A | 800 | 17.7 | FDD | IMD5 |
| CA\_n1-n7-n28 | n1 | 1935 | 5 | 25 | 2125 | N/A | FDD | N/A |
|  | n7 | 2510 | 10 | 50 | 2630 | N/A | FDD | N/A |
|  | n28 | N/A | 10 | N/A | 785 | 17,7 | FDD | IMD5 |
| CA\_n1-n7-n78 | n1 | 1977.5 | 5 | 25 | 2167.5 | N/A | FDD | N/A |
|  | n7 | N/A | 5 | N/A | 2627.5 | 20.6 | FDD | IMD4 |
|  | n78 | 3305 | 10 | 50 | 3305 | N/A | TDD | N/A |
|  | n1 | N/A | 5 | N/A | 2140 | 20.1 | FDD | IMD4 |
|  | n7 | 2510 | 10 | 50 | 2630 | N/A | FDD | N/A |
|  | n78 | 3580 | 10 | 50 | 3580 | N/A | TDD | N/A |
| CA\_n1-n18-n41 | n1 | 1960 | 5 | 25 | 2150 | N/A | FDD | N/A |
|  | n41 | 2505 | 10 | 50 | 2505 | N/A | TDD | N/A |
|  | n18 | N/A | 5 | N/A | 870 | 12.4 | FDD | IMD5 |
| CA\_n1-n18-n77 | n1 | 1970 | 5 | 25 | 2160 | N/A | FDD | N/A |
|  | n77 | 3390 | 10 | 50 | 3390 | N/A | TDD | N/A |
|  | n18 | N/A | 5 | N/A | 870 | 18.6 | FDD | IMD5 |
|  | n1 | N/A | 5 | N/A | 2120 | 25.4 | FDD | IMD3 |
|  | n18 | 825 | 5 | 25 | 870 | N/A | FDD | N/A |
|  | n77 | 3770 | 10 | 50 | 3770 | N/A | TDD | N/A |
| CA\_n1-n26-n78 | n1 | N/A | 5 | N/A | 2122 | 27.0 | FDD | IMD3 |
|  | n26 | 829 | 5 | 25 | 874 | N/A | FDD | N/A |
|  | n78 | 3780 | 10 | 50 | 3780 | N/A | TDD | N/A |
|  | n1 | 1975 | 5 | 25 | 2165 | N/A | FDD | N/A |
|  | n26 | N/A | 5 | N/A | 885 | 15.3 | FDD | IMD5 |
|  | n78 | 3405 | 10 | 50 | 3405 | N/A | TDD | N/A |
| CA\_n1-n28-n41 | n1 | 1923 | 5 | 25 | 2113 | N/A | FDD | N/A |
|  | n28 | N/A | 5 | N/A | 762 | 36.6 | FDD | IMD21 |
|  | n41 | 2685 | 10 | 50 | 2685 | N/A | TDD | N/A |
| CA\_n1-n28-n77 | n1 | 1950 | 5 | 25 | 2140 | N/A | FDD | N/A |
|  | n77 | 3320 | 10 | 50 | 3320 | N/A | TDD | N/A |
|  | n28 | N/A | 5 | N/A | 790 | 16.5 | FDD | IMD5 |
|  | n28 | 740 | 5 | 25 | 795 | N/A | FDD | N/A |
|  | n77 | 3630 | 10 | 50 | 3630 | N/A | TDD | N/A |
|  | n1 | N/A | 5 | N/A | 2150 | 24.7 | FDD | IMD3 |
| CA\_n1-n28-n78 | n1 | N/A | 5 | N/A | 2150 | 24.6 | FDD | IMD3 |
|  | n28 | 740 | 5 | 25 | 795 | N/A | FDD | N/A |
|  | n78 | 3630 | 10 | 50 | 3630 | N/A | TDD | N/A |
|  | n1 | 1970 | 5 | 25 | 2160 | N/A | FDD | N/A |
|  | n28 | N/A | 5 | N/A | 794 | 17.2 | FDD | IMD5 |
|  | n78 | 3352 | 10 | 50 | 3352 | N/A | TDD | N/A |
| CA\_n1-n28-n79 | n1 | 1930 | 5 | 25 | 2120 | N/A | FDD | N/A |
|  | n79 | 4648 | 40 | 216 | 4648 | N/A | TDD | N/A |
|  | n28 | N/A | 5 | N/A | 788 | 24.2 | FDD | IMD32 |
|  | n28 | 745.5 | 5 | 25 | 800.5 | N/A | FDD | N/A |
|  | n79 | 4420 | 40 | 216 | 4420 | N/A | TDD | N/A |
|  | n1 | N/A | 5 | N/A | 2167.5 | 13.4 | FDD | IMD41 |
| CA\_n1-n77-n79 | n1 | 1950 | 5 | 25 | 2140 | 24.6 | FDD | IMD31,2 |
|  | n77 | 3400 | 10 | 50 | 3400 | N/A | TDD | N/A |
|  | n79 | 4660 | 40 | 216 | 4660 | N/A | TDD | N/A |
| CA\_n1-n41-n77 | n1 | 1970 | 5 | 25 | 2160 | N/A | FDD | N/A |
|  | n41 | 2650 | 10 | 50 | 2650 | N/A | TDD | N/A |
|  | n77 | N/A | 10 | N/A | 3330 | 28.2 | TDD | IMD31,2 |
|  | n1 | 1975 | 5 | 10 | 2165 | N/A | FDD | N/A |
|  | n77 | 3410 | 10 | 50 | 3410 | N/A | TDD | N/A |
|  | n41 | N/A | 10 | N/A | 2515 | 22.0 | TDD | IMD41 |
|  | n41 | 2640 | 10 | 50 | 2640 | N/A | TDD | N/A |
|  | n77 | 3710 | 10 | 50 | 3710 | N/A | TDD | N/A |
|  | n1 | N/A | 5 | N/A | 2140 | 21.4 | FDD | IMD4 |
| CA\_n1-n78-n79 | n1 | 1950 | 5 | 25 | 2140 | N/A | FDD | N/A |
|  | n78 | 3410 | 10 | 50 | 3410 | N/A | TDD | N/A |
|  | n79 | N/A | 40 | N/A | 4870 | 24.9 | TDD | IMD31,3 |
|  | n1 | 1950 | 5 | 25 | 2140 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3490 | 17 | TDD | IMD53 |
|  | n79 | 4670 | 40 | 216 | 4670 | N/A | TDD | N/A |
|  | n1 | N/A | 5 | N/A | 2140 | 24.6 | FDD | IMD31 |
|  | n78 | 3400 | 10 | 50 | 3400 | N/A | TDD | N/A |
|  | n79 | 4660 | 40 | 216 | 4660 | N/A | TDD | N/A |
|  | n1 | N/A | 5 | N/A | 2140 | 3.8 | FDD | IMD41 |
|  | n78 | 3590 | 10 | 50 | 3590 | N/A | TDD | N/A |
|  | n79 | 4660 | 40 | 216 | 4660 | N/A | TDD | N/A |
| CA\_n2-n5-n77 | n2 | 1907.5 | 5 | 25 | 1987.5 | N/A | FDD | N/A |
|  | n5 | N/A | 5 | N/A | 887.5 | 13.6 | FDD | IMD55 |
|  | n77 | 3305 | 10 | 50 | 3305 | N/A | TDD | N/A |
|  | n2 | N/A | 5 | N/A | 1987 | 24.8 | FDD | IMD35 |
|  | n5 | 846.5 | 5 | 25 | 891.5 | N/A | FDD | N/A |
|  | n77 | 3680 | 10 | 50 | 3680 | N/A | TDD | N/A |
| CA\_n2-n12-n77 | n2 | N/A | 5 | N/A | 1960 | 24,8 | FDD | IMD32,5 |
|  | n12 | 707.5 | 5 | 25 | 737.5 | N/A | FDD | N/A |
|  | n77 | 3375 | 10 | 50 | 3375 | N/A | TDD | N/A |
| CA\_n2-n14-n77 | n2 | N/A | 5 | N/A | 1954 | 24.8 | FDD | IMD3 |
|  | n14 | 793 | 5 | 25 | 763 | N/A | FDD | N/A |
|  | n77 | 3540 | 10 | 50 | 3540 | N/A | TDD | N/A |
| CA\_n2-n30-n77 | n2 | N/A | 5 | N/A | 1986 | 19.3 | FDD | IMD45 |
|  | n30 | 2312 | 5 | 25 | 2357 | N/A | FDD | N/A |
|  | n77 | 3305 | 10 | 50 | 3305 | N/A | TDD | N/A |
|  | n2 | 1905 | 5 | 25 | 1985 | N/A | FDD | N/A |
|  | n30 | N/A | 5 | N/A | 2354 | 22.2 | FDD | IMD45 |
|  | n77 | 3361 | 10 | 50 | 3361 | N/A | TDD | N/A |
|  | n2 | 1860 | 5 | 25 | 1940 | N/A | FDD | N/A |
|  | n30 | N/A | 5 | N/A | 2354 | 12.9 | FDD | IMD5 |
|  | n77 | 3967 | 10 | 50 | 3967 | N/A | TDD | N/A |
| CA\_n2-n66-n77 | n2 | 1855 | 5 | 25 | 1935 | N/A | FDD | N/A |
|  | n66 | N/A | 5 | N/A | 2115 | 34.7 | FDD | IMD21,2 |
|  | n77 | 3970 | 10 | 50 | 3970 | N/A | TDD | N/A |
|  | n2 | N/A | 5 | N/A | 1960 | 37.6 | FDD | IMD21,2 |
|  | n66 | 1760 | 5 | 25 | 2160 | N/A | FDD | N/A |
|  | n77 | 3720 | 10 | 50 | 3720 | N/A | TDD | N/A |
|  | n2 | N/A | 5 | 25 | 1950 | 24.3 | FDD | IMD3 |
|  | n66 | 1775 | 5 | 25 | 2195 | N/A | FDD | N/A |
|  | n77 | 3300 | 100 | 1 (RBstart=203) | 3300 | N/A | TDD | N/A |
|  |  | 3400 | 100 | 1 (RBstart=67) | 3400 |  |  |  |
| CA\_n3-n7-n20 | n3 | 1747 | 5 | 25 | 1842 | N/A | FDD | N/A |
|  | n7 | 2543 | 10 | 50 | 2663 | N/A | FDD | N/A |
|  | n20 | N/A | 5 | N/A | 796 | 26.0 | FDD | IMD2 |
|  | n3 | 1780 | 5 | 25 | 1875 | N/A | FDD | N/A |
|  | n7 | N/A | 10 | N/A | 2625 | 35.0 | FDD | IMD2 |
|  | n20 | 845 | 5 | 25 | 804 | N/A | FDD | N/A |
|  | n3 | 1750 | 5 | 25 | 1845 | N/A | FDD | N/A |
|  | n7 | N/A | 5 | 25 | N/A | 25.9 | FDD | IMD3 |
|  | n20 | 835 | 5 | 25 | 794 | N/A | FDD | N/A |
| CA\_n3-n7-n28 | n3 | 1747 | 5 | 25 | 1842 | N/A | FDD | N/A |
|  | n7 | 2543 | 5 | 25 | 2663 | N/A | FDD | N/A |
|  | n28 | N/A | 5 | N/A | 796 | 26.0 | FDD | IMD2 |
|  | n3 | 1712.5 | 5 | 25 | 1807.5 | N/A | FDD | N/A |
|  | n7 | N/A | 5 | N/A | 2682 | 25.9 | FDD | IMD3 |
|  | n28 | 743 | 5 | 25 | 798 | N/A | FDD | N/A |
|  | n3 | N/A | 5 | N/A | 1832.5 | 32 | FDD | IMD2 |
|  | n7 | 2543 | 5 | 25 | 2663 | N/A | FDD | N/A |
|  | n28 | 710.5 | 5 | 25 | 765.5 | N/A | FDD | N/A |
| CA\_n3-n7-n78 | n3 | N/A | 5 | N/A | 1820 | 26.6 | FDD | IMD3 |
|  | n7 | 2565 | 5 | 25 | 2685 | N/A | FDD | N/A |
|  | n78 | 3310 | 10 | 50 | 3310 | N/A | TDD | N/A |
|  | n3 | N/A | 5 | N/A | 1820 | 17 | FDD | IMD4 |
|  | n7 | 2565 | 5 | 25 | 2685 | N/A | FDD | N/A |
|  | n78 | 3475 | 10 | 50 | 3475 | N/A | TDD | N/A |
| CA\_n3-n18-n41 | n18 | N/A | 5 | N/A | 865 | 34.9 | FDD | IMD2 |
|  | n3 | 1765 | 5 | 25 | 1860 | N/A | FDD | N/A |
|  | n41 | 2630 | 10 | 50 | 2630 | N/A | TDD | N/A |
|  | n18 | N/A | 5 | N/A | 875 | 28 | FDD | IMD3 |
|  | n3 | 1725 | 5 | 25 | 1820 | N/A | FDD | N/A |
|  | n41 | 2670 | 5 | 25 | 2670 | N/A | TDD | N/A |
|  | n3 | N/A | 5 | N/A | 1850 | 34.8 | FDD | IMD2 |
|  | n41 | 2670 | 10 | 50 | 2670 | N/A | TDD | N/A |
|  | n18 | 820 | 5 | 25 | 865 | N/A | FDD | N/A |
| CA\_n3-n18-n77 | n18 | 820 | 5 | 25 | 865 | N/A | TDD | N/A |
|  | n3 | N/A | 5 | N/A | 1865 | 24.2 | FDD | IMD3 |
|  | n77 | 3505 | 10 | 50 | 3505 | N/A | TDD | N/A |
| CA\_n3-n26-n78 | n3 | N/A | 5 | N/A | 1862 | 24.6 | FDD | IMD3 |
|  | n26 | 839 | 5 | 25 | 884 | N/A | FDD | N/A |
|  | n78 | 3540 | 10 | 50 | 3540 | N/A | TDD | N/A |
| CA\_n3-n28-n41 | n3 | 1720 | 5 | 25 | 1815 | N/A | FDD | N/A |
|  | n28 | N/A | 5 | N/A | 790 | 32 | FDD | IMD24 |
|  | n41 | 2510 | 5 | 25 | 2510 | N/A | TDD | N/A |
|  | n3 | N/A | 5 | N/A | 1832.5 | 32 | FDD | IMD2 |
|  | n28 | 710.5 | 5 | 25 | 765.5 | N/A | FDD | N/A |
|  | n41 | 2543 | 10 | 50 | 2543 | N/A | TDD | N/A |
| CA\_n3-n28-n77 | n3 | 1712.5 | 5 | 25 | 1807.5 | N/A | FDD | N/A |
|  | n28 | N/A | 5 | N/A | 770 | 24.2 | FDD | IMD3 |
|  | n77 | 4195 | 10 | 50 | 4195 | N/A | TDD | N/A |
|  | n3 | N/A | 5 | N/A | 1850 | 25.8 | FDD | IMD32 |
|  | n28 | 735 | 5 | 25 | 790 | N/A | FDD | N/A |
|  | n77 | 3320 | 10 | 50 | 3320 | N/A | TDD | N/A |
| CA\_n3-n28-n78 | n3 | N/A | 5 | N/A | 1850 | 29.2 | FDD | IMD3 |
|  | n28 | 735 | 5 | 25 | 790 | N/A | FDD | N/A |
|  | n78 | 3320 | 10 | 50 | 3320 | N/A | TDD | N/A |
| CA\_n3-n28-n79 | n3 | 1770 | 5 | 25 | 1865 | N/A | FDD | N/A |
|  | n79 | 4530 | 40 | 216 | 4530 | N/A | TDD | N/A |
|  | n28 | N/A | 5 | N/A | 780 | 21.5 | FDD | IMD4  |3\*fBn3-fBn79| |
|  | n28 | 725 | 5 | 25 | 780 | N/A | FDD | N/A |
|  | n79 | 4770 | 40 | 216 | 4770 | N/A | TDD | N/A |
|  | n3 | N/A | 5 | N/A | 1870 | 20.5 | FDD | IMD5  |4\*fBn28-fBn79| |
| CA\_n3-n41-n77 | n3 | 1720 | 5 | 25 | 1815 | N/A | FDD | N/A |
|  | n41 | 2580 | 5 | 25 | 2580 | N/A | TDD | N/A |
|  | n77 | N/A | 10 | N/A | 3440 | 25.6 | TDD | IMD31 |
|  | n3 | N/A | 5 | N/A | 1840 | 25.1 | FDD | IMD32 |
|  | n41 | 2620 | 5 | 25 | 2620 | N/A | TDD | N/A |
|  | n77 | 3400 | 10 | 50 | 3400 | N/A | TDD | N/A |
|  | n3 | 1720 | 5 | 25 | 1815 | N/A | FDD | N/A |
|  | n41 | N/A | 5 | N/A | 2640 | 13 | TDD | IMD5 |
|  | n77 | 3900 | 10 | 50 | 3900 | N/A | TDD | N/A |
| CA\_n3-n41-n79 | n3 | 1755 | 5 | 25 | 1850 | 35.4 | FDD | IMD21 |
|  | n41 | 2570 | 10 | 50 | 2570 | N/A | TDD | N/A |
|  | n79 | 4420 | 40 | 216 | 4420 | N/A | TDD | N/A |
|  | n3 | 1770 | 5 | 25 | 1865 | N/A | FDD | N/A |
|  | n41 | 2670 | 10 | 50 | 2670 | 36.2 | TDD | IMD21 |
|  | n79 | 4440 | 40 | 216 | 4440 | N/A | TDD | N/A |
|  | n3 | 1770 | 5 | 25 | 1865 | N/A | FDD | N/A |
|  | n41 | 2670 | 10 | 50 | 2670 | N/A | TDD | N/A |
|  | n79 | 4440 | 40 | 216 | 4440 | 36.8 | TDD | IMD21 |
| CA\_n3-n77-n79 | n77 | 3350 | 10 | 50 | 3350 | N/A | FDD | N/A |
|  | n79 | 4840 | 40 | 216 | 4840 | N/A | TDD | N/A |
|  | n3 | 1765 | 5 | 25 | 1860 | 24.2 | TDD | IMD31, 2  |2\*fBn77-fBn79| |
| CA\_n3-n78-n79 | n3 | 1780 | 5 | 25 | 1875 | N/A | FDD | N/A |
|  | n78 | 3320 | 10 | 50 | 3320 | N/A | TDD | N/A |
|  | n79 | N/A | 10 | N/A | 4860 | 22.1 | TDD | IMD3 |
|  | n3 | 1780 | 5 | 25 | 1875 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3480 | 8.5 | TDD | IMD5 |
|  | n79 | 4410 | 10 | 50 | 4410 | N/A | TDD | N/A |
|  | n3 | 1765 | 5 | 25 | 1860 | 24.7 | FDD | IMD31 |
|  | n78 | 3350 | 10 | 50 | 3350 | N/A | TDD | N/A |
|  | n79 | 4840 | 10 | 50 | 4840 | N/A | TDD | N/A |
|  | n3 | 1745 | 5 | 25 | 1840 | 11.5 | FDD | IMD4 |
|  | n78 | 3780 | 10 | 50 | 3780 | N/A | TDD | N/A |
|  | n79 | 4700 | 10 | 50 | 4700 | N/A | TDD | N/A |
| CA\_n5-n7-n77 | n5 | N/A | 5 | N/A | 879 | 35.2 | FDD | IMD21,4 |
|  | n7 | 2550 | 5 | 25 | 2670 | N/A | FDD | N/A |
|  | n77 | 3429 | 10 | 50 | 3429 | N/A | TDD | N/A |
|  | n5 | 844 | 5 | 25 | 889 | N/A | FDD | N/A |
|  | n7 | N/A | 5 | N/A | 2645 | 35.1 | FDD | IMD2 |
|  | n77 | 3489 | 10 | 50 | 3489 | N/A | TDD | N/A |
| CA\_n5-n7-n78 | n5 | N/A | 5 | N/A | 879 | 35.2 | FDD | IMD21 |
|  | n7 | 2550 | 5 | 25 | 2670 | N/A | FDD | N/A |
|  | n78 | 3429 | 10 | 50 | 3429 | N/A | TDD | N/A |
|  | n5 | 844 | 5 | 25 | 889 | N/A | FDD | N/A |
|  | n7 | N/A | 5 | N/A | 2645 | 35.1 | FDD | IMD2 |
|  | n78 | 3489 | 10 | 50 | 3489 | N/A | TDD | N/A |
| CA\_n5-n12-n77 | n5 | N/A | 5 | N/A | 880 | 14.0 | FDD | IMD5 |
|  | n12 | 707.5 | 5 | 25 | 737.5 | N/A | FDD | N/A |
|  | n77 | 3710 | 10 | 50 | 3710 | N/A | TDD | N/A |
|  | n5 | 835 | 5 | 25 | 880 | N/A | FDD | N/A |
|  | n12 | N/A | 5 | N/A | 740 | 14.9 | FDD | IMD55 |
|  | n77 | 4080 | 10 | 50 | 4080 | N/A | TDD | N/A |
| CA\_n5-n14-n77 | n5 | N/A | 5 | N/A | 880 | 14.0 | FDD | IMD55 |
|  | n14 | 793 | 5 | 25 | 763 | N/A | FDD | N/A |
|  | n77 | 4052 | 10 | 50 | 4052 | N/A | TDD | N/A |
|  | n5 | 846.5 | 5 | 25 | 891.5 | N/A | FDD | N/A |
|  | n14 | N/A | 5 | N/A | 765.5 | 20.3 | FDD | IMD41.5 |
|  | n77 | 3305 | 10 | 50 | 3305 | N/A | TDD | N/A |
| CA\_n5-n25-n77 | n5 | N/A | 5 | N/A | 889 | 13.6 | FDD | IMD55 |
|  | n25 | 1907 | 5 | 25 | 1987 | N/A | FDD | N/A |
|  | n77 | 3305 | 10 | 50 | 3305 | N/A | TDD | N/A |
|  | n5 | 846.5 | 5 | 25 | 891.5 | N/A | FDD | N/A |
|  | n25 | N/A | 5 | N/A | 1987 | 24.8 | FDD | IMD3 |
|  | n77 | 3680 | 10 | 25 | 3680 | N/A | TDD | N/A |
| CA\_n5-n25-n78 | n5 | N/A | 5 | N/A | 889 | 13.6 | FDD | IMD5 |
|  | n25 | 1907 | 5 | 25 | 1987 | N/A | FDD | N/A |
|  | n78 | 3305 | 10 | 50 | 3305 | N/A | TDD | N/A |
|  | n5 | 846.5 | 5 | 25 | 891.5 | N/A | FDD | N/A |
|  | n25 | N/A | 5 | N/A | 1987 | 24.8 | FDD | IMD3 |
|  | n78 | 3680 | 10 | 50 | 3680 | N/A | TDD | N/A |
| CA\_n5-n29-n77 | n5 | 835 | 5 | 25 | 880 | N/A | FDD | N/A |
|  | n29 | N/A | 5 | N/A | 722 | 14.9 | FDD | IMD55 |
|  | n77 | 4062 | 10 | 50 | 4062 | N/A | TDD | N/A |
| CA\_n5-n30-n77 | n5 | N/A | 5 | N/A | 880 | 23.5 | FDD | IMD31 |
|  | n30 | 2310 | 5 | 25 | 2355 | N/A | FDD | N/A |
|  | n77 | 3740 | 10 | 50 | 3740 | N/A | TDD | N/A |
|  | n5 | 835 | 5 | 25 | 880 | N/A | FDD | N/A |
|  | n30 | N/A | 5 | N/A | 2355 | 21.4 | FDD | IMD35 |
|  | n77 | 4025 | 10 | 50 | 4025 | N/A | TDD | N/A |
| CA\_n5-n66-n77 | n5 | 826.5 | 5 | 25 | 871.5 | N/A | FDD | N/A |
|  | n66 | N/A | 5 | N/A | 2142 | 22.2 | FDD | IMD3 |
|  | n77 | 3795 | 10 | 50 | 3795 | N/A | TDD | N/A |
| CA\_n7-n25-n77 | n7 | 2550 | 5 | 25 | 2670 | N/A | FDD | N/A |
|  | n25 | N/A | 5 | N/A | 1950 | 20.0 | FDD | IMD4 |
|  | n77 | 3525 | 10 | 50 | 3525 | N/A | TDD | N/A |
|  | n7 | N/A | 5 | N/A | 2640 | 18.8 | FDD | IMD5 |
|  | n25 | 1870 | 5 | 25 | 1950 | N/A | FDD | N/A |
|  | n77 | 4125 | 10 | 50 | 4125 | N/A | TDD | N/A |
| CA\_n7-n66-n77 | n7 | 2550 | 5 | 25 | 2670 | N/A | FDD | N/A |
|  | n66 | N/A | 5 | N/A | 2150 | 20.5 | FDD | IMD4 |
|  | n77 | 3625 | 10 | 50 | 3625 | N/A | TDD | N/A |
|  | n7 | N/A | 5 | N/A | 2640 | 18.8 | FDD | IMD5 |
|  | n66 | 1720 | 5 | 25 | 2120 | N/A | FDD | N/A |
|  | n77 | 3900 | 10 | 50 | 3900 | N/A | TDD | N/A |
| CA\_n7-n71-n77 | n7 | N/A | 5 | N/A | 2670 | 34.6 | FDD | IMD2 |
|  | n71 | 680 | 5 | 25 | 634 | N/A | FDD | N/A |
|  | n77 | 3350 | 10 | 50 | 3350 | N/A | TDD | N/A |
| CA\_n7-n26-n78 | n7 | 2550 | 5 | 25 | 2670 | N/A | FDD | N/A |
|  | n26 | N/A | 5 | N/A | 879 | 36.2 | FDD | IMD2 |
|  | n78 | 3429 | 10 | 50 | 3429 | N/A | TDD | N/A |
|  | n7 | 2525 | 5 | 25 | 2645 | N/A | FDD | N/A |
|  | n26 | N/A | 5 | N/A | 875 | 15.7 | FDD | IMD5 |
|  | n78 | 3350 | 10 | 50 | 3350 | N/A | TDD | N/A |
|  | n7 | N/A | 5 | N/A | 2645 | 36.1 | FDD | IMD2 |
|  | n26 | 844 | 5 | 25 | 889 | N/A | FDD | N/A |
|  | n78 | 3489 | 10 | 50 | 3489 | N/A | TDD | N/A |
| CA\_n7-n28-n78 | n7 | 2567.5 | 5 | 25 | 2687.5 | N/A | FDD | N/A |
|  | n28 | N/A | 5 | N/A | 782.5 | 33.8 | FDD | IMD21 |
|  | n78 | 3350 | 10 | 50 | 3350 | N/A | TDD | N/A |
|  | n7 | N/A | 5 | N/A | 2650 | 35.5 | FDD | IMD2 |
|  | n28 | 740 | 5 | 25 | 795 | N/A | FDD | N/A |
|  | n78 | 3390 | 10 | 50 | 3390 | N/A | TDD | N/A |
| CA\_n7-n66-n78 | n7 | 2540 | 5 | 25 | 2660 | N/A | FDD | N/A |
|  | n66 | 1760 | 5 | 25 | 2160 | 20.5 | FDD | IMD4 |
|  | n78 | 3620 | 10 | 50 | 3620 | N/A | TDD | N/A |
| CA\_n12-n30-n77 | n12 | N/A | 5 | N/A | 740 | 23.5 | FDD | IMD31 |
|  | n30 | 2310 | 5 | 25 | 2355 | N/A | FDD | N/A |
|  | n77 | 3880 | 10 | 50 | 3880 | N/A | TDD | N/A |
|  | n12 | 707.5 | 5 | 25 | 737.5 | N/A | FDD | N/A |
|  | n30 | N/A | 5 | N/A | 2355 | 21.4 | FDD | IMD3 |
|  | n77 | 3770 | 10 | 50 | 3770 | N/A | TDD | N/A |
| CA\_n12-n66-n77 | n12 | N/A | 5 | N/A | 740 | 23.5 | FDD | IMD35 |
|  | n66 | 1720 | 5 | 25 | 2120 | N/A | FDD | N/A |
|  | n77 | 4180 | 10 | 50 | 4180 | N/A | TDD | N/A |
|  | n12 | 707 | 5 | 25 | 737 | N/A | FDD | N/A |
|  | n66 | N/A | 5 | N/A | 2126 | 21.4 | FDD | IMD3 |
|  | n77 | 3540 | 10 | 50 | 3540 | N/A | TDD | N/A |
| CA\_n13-n25-n77 | n13 | 782 | 5 | 25 | 751 | N/A | FDD | N/A |
|  | n25 | N/A | 5 | N/A | 1960 | 24.0 | FDD | IMD3 |
|  | n77 | 3524 | 10 | 50 | 3524 | N/A | TDD | N/A |
| CA\_n13-n66-n77 | n13 | 782 | 5 | 25 | 751 | N/A | FDD | N/A |
|  | n66 | N/A | 5 | N/A | 2146 | 26.0 | FDD | IMD3 |
|  | n77 | 3710 | 10 | 50 | 3710 | N/A | TDD | N/A |
|  | n13 | N/A | 5 | N/A | 750 | 24.1 | FDD | IMD3 |
|  | n66 | 1710 | 5 | 25 | 2110 | N/A | FDD | N/A |
|  | n77 | 4170 | 10 | 50 | 4170 | N/A | TDD | N/A |
| CA\_n14-n30-n77 | n14 | N/A | 5 | N/A | 763 | 23.5 | FDD | IMD31 |
|  | n30 | 2310 | 5 | 25 | 2355 | N/A | FDD | N/A |
|  | n77 | 3857 | 10 | 50 | 3857 | N/A | TDD | N/A |
|  | n14 | 793 | 5 | 25 | 763 | N/A | FDD | N/A |
|  | n30 | N/A | 5 | N/A | 2355 | 21.4 | FDD | IMD3 |
|  | n77 | 3941 | 10 | 50 | 3941 | N/A | TDD | N/A |
| CA\_n14-n66-n77 | n14 | N/A | 5 | N/A | 763 | 23.5 | FDD | IMD35 |
|  | n66 | 1712.5 | 5 | 25 | 2112.5 | N/A | FDD | N/A |
|  | n77 | 4188 | 10 | 50 | 4188 | N/A | TDD | N/A |
|  | n14 | 793 | 5 | 25 | 763 | N/A | FDD | N/A |
|  | n66 | N/A | 5 | N/A | 2155 | 21.4 | FDD | IMD3 |
|  | n77 | 3741 | 10 | 50 | 3741 | N/A | TDD | N/A |
| CA\_n18-n28-n41 | n18 | 825 | 5 | 25 | 870 | N/A | FDD | N/A |
|  | n41 | 2505 | 10 | 50 | 2505 | N/A | TDD | N/A |
|  | n28 | N/A | 5 | N/A | 795 | 16.9 | FDD | IMD5 |
| CA\_n18-n28-n77 | n18 | 820 | 5 | 25 | 865 | N/A | FDD | N/A |
|  | n28 | N/A | 5 | N/A | 778 | 17.5 | FDD | IMD5 |
|  | n77 | 4058 | 10 | 50 | 4058 | N/A | TDD | N/A |
|  | n18 | N/A | 5 | N/A | 865 | 12.1 | FDD | IMD5 |
|  | n28 | 723 | 5 | 25 | 778 | N/A | FDD | N/A |
|  | n77 | 3757 | 10 | 50 | 3757 | N/A | TDD | N/A |
| CA\_n18-n41-n77 | n18 | 820 | 5 | 25 | 865 | N/A | FDD | N/A |
|  | n41 | 2570 | 5 | 25 | 2570 | N/A | TDD | N/A |
|  | n77 | N/A | 10 | N/A | 3390 | 33.0 | TDD | IMD22,4 |
|  | n18 | 820 | 5 | 25 | 865 | N/A | FDD | N/A |
|  | n41 | N/A | 5 | N/A | 2630 | 32.6 | TDD | IMD24 |
|  | n77 | 3450 | 10 | 50 | 3450 | N/A | TDD | N/A |
|  | n18 | N/A | 5 | N/A | 870 | 33.8 | FDD | IMD21,4 |
|  | n41 | 2590 | 10 | 50 | 2590 | N/A | TDD | N/A |
|  | n77 | 3460 | 10 | 50 | 3460 | N/A | TDD | N/A |
| CA\_n25-n41-n66 | n25 | N/A | 5 | N/A | 1940 | 23.0 | FDD | IMD4 |
|  | n41 | 2685 | 10 | 50 | 2685 | N/A | TDD | N/A |
|  | n66 | 1715 | 5 | 25 | 2115 | N/A | FDD | N/A |
| CA\_n25-n41-n77 | n25 | 1870 | 5 | 25 | 1950 | N/A | FDD | N/A |
|  | n41 | 2670 | 5 | 25 | 2670 | N/A | TDD | N/A |
|  | n77 | N/A | 10 | N/A | 3470 | 24.3 | TDD | IMD3 |
|  | n25 | 1900 | 5 | 25 | 1980 | N/A | FDD | N/A |
|  | n41 | 2525 | 5 | 25 | 2645 | N/A | TDD | N/A |
|  | n77 | N/A | 10 | N/A | 3775 | 16.6 | TDD | IMD5 |
|  | n25 | 1870 | 5 | 25 | 1950 | N/A | FDD | N/A |
|  | n41 | N/A | 5 | N/A | 2640 | 18.1 | TDD | IMD55 |
|  | n77 | 4125 | 10 | 50 | 4125 | N/A | TDD | N/A |
|  | n25 | N/A | 5 | N/A | 1950 | 26.6 | FDD | IMD35 |
|  | n41 | 2675 | 5 | 25 | 2675 | N/A | TDD | N/A |
|  | n77 | 3400 | 10 | 50 | 3400 | N/A | TDD | N/A |
|  | n25 | N/A | 5 | N/A | 1950 | 19.6 | FDD | IMD4 |
|  | n41 | 2550 | 5 | 25 | 2685 | N/A | TDD | N/A |
|  | n77 | 3525 | 10 | 50 | 3525 | N/A | TDD | N/A |
| CA\_n25-n66-n77 | n25 | 1855 | 5 | 25 | 1935 | N/A | FDD | N/A |
|  | n66 | N/A | 5 | N/A | 2115 | 35.2 | FDD | IMD2 |
|  | n77 | 3970 | 10 | 50 | 3970 | N/A | TDD | N/A |
|  | n25 | 1900 | 5 | 25 | 1980 | N/A | FDD | N/A |
|  | n66 | N/A | 5 | N/A | 2160 | 22.4 | FDD | IMD4 |
|  | n77 | 3540 | 10 | 50 | 3540 | N/A | TDD | N/A |
|  | n25 | 1900 | 5 | 25 | 1980 | N/A | FDD | N/A |
|  | n66 | N/A | 5 | N/A | 2160 | 16.4 | FDD | IMD5 |
|  | n77 | 3930 | 10 | 50 | 3930 | N/A | TDD | N/A |
|  | n25 | N/A | 5 | N/A | 1960 | 38.1 | FDD | IMD2 |
|  | n66 | 1760 | 5 | 25 | 2160 | N/A | FDD | N/A |
|  | n77 | 3720 | 10 | 50 | 3720 | N/A | TDD | N/A |
|  | n25 | N/A | 5 | N/A | 1960 | 21.1 | FDD | IMD45 |
|  | n66 | 1770 | 5 | 25 | 2170 | N/A | FDD | N/A |
|  | n77 | 3350 | 10 | 50 | 3350 | N/A | TDD | N/A |
|  | n25 | N/A | 5 | N/A | 1960 | 13.0 | FDD | IMD55 |
|  | n66 | 1760 | 5 | 25 | 2160 | N/A | FDD | N/A |
|  | n77 | 3620 | 10 | 50 | 3620 | N/A | TDD | N/A |
|  | n25 | 1880 | 5 | 25 | 1960 | N/A | FDD | N/A |
|  | n66 | 1740 | 5 | 25 | 2140 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3620 | 35.4 | TDD | IMD25 |
|  | n25 | 1880 | 5 | 25 | 1960 | N/A | FDD | N/A |
|  | n66 | 1740 | 5 | 25 | 2140 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3900 | 19.9 | TDD | IMD4 |
| CA\_n25-n66-n78 | n25 | 1880 | 5 | 25 | 1960 | M/A | FDD | N/A |
|  | n66 | 1740 | 5 | 25 | 2140 | 21.1 | FDD | IMD4 |
|  | n78 | 3500 | 10 | 50 | 3500 | N/A | TDD | N/A |
|  | n25 | 1880 | 5 | 25 | 1960 | 37.6 | FDD | IMD21,2 |
|  | n66 | 1760 | 5 | 25 | 2160 | N/A | FDD | N/A |
|  | n78 | 3720 | 10 | 50 | 3720 | N/A | TDD | N/A |
| CA\_n25-n71-n77 | n25 | 1907.5 | 5 | 25 | 1987.5 | N/A | FDD | N/A |
|  | n71 | 695.5 | 5 | 25 | 649.5 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3305 | 16.1 | TDD | IMD31,2,5 |
|  | n25 | N/A | 5 | N/A | 1954 | 25.5 | FDD | IMD32,5 |
|  | n71 | 693 | 5 | 25 | 647 | N/A | FDD | N/A |
|  | n77 | 3340 | 10 | 50 | 3340 | N/A | TDD | N/A |
| CA\_n28-n41-n74 | n28 | N/A | 5 | N/A | 782 | 17.5 | FDD | IMD5 |
|  | n41 | 2569 | 10 | 50 | 2569 | N/A | TDD | N/A |
|  | n74 | 1452 | 5 | 25 | 1500 | N/A | FDD | N/A |
| CA\_n28-n41-n77 | n28 | 743 | 5 | 25 | 798 | N/A | FDD | N/A |
|  | n41 | 2580 | 5 | 25 | 2580 | N/A | TDD | N/A |
|  | n77 | N/A | 10 | N/A | 3323 | 34.2 | TDD | IMD22,4 |
|  | n28 | N/A | 5 | N/A | 798 | 36.8 | FDD | IMD21,4 |
|  | n41 | 2642 | 5 | 25 | 2642 | N/A | TDD | N/A |
|  | n77 | 3440 | 10 | 50 | 3440 | N/A | TDD | N/A |
|  | n28 | 738 | 5 | 25 | 793 | N/A | FDD | N/A |
|  | n41 | N/A | 5 | N/A | 2642 | 35.5 | TDD | IMD24 |
|  | n77 | 3380 | 10 | 50 | 3380 | N/A | TDD | N/A |
| CA\_n28-n41-n79 | n28 | 725 | 5 | 25 | 780 | 22 | FDD | IMD31 |
|  | n41 | 2600 | 10 | 50 | 2600 | N/A | TDD | N/A |
|  | n79 | 4600 | 40 | 216 | 4600 | N/A | TDD | N/A |
|  | n28 | 720 | 5 | 25 | 780 | N/A | FDD | N/A |
|  | n41 | 2600 | 10 | 50 | 2600 | N/A | TDD | N/A |
|  | n79 | 4480 | 40 | 216 | 4600 | 19.1 | TDD | IMD32 |
|  | n28 | 735 | 5 | 25 | 790 | N/A | FDD | N/A |
|  | n41 | 2645 | 10 | 50 | 2645 | 22.4 | TDD | IMD4 |
|  | n79 | 4850 | 40 | 216 | 4850 | N/A | TDD | N/A |
| CA\_n28-n74-n77 | n28 | 730 | 5 | 25 | 785 | N/A | FDD | N/A |
|  | n74 | N/A | 5 | 25 | 1500 | 20.7 | FDD | IMD4 |
|  | n77 | 3690 | 10 | 50 | 3690 | N/A | TDD |  |
|  | n28 | N/A | 5 | 25 | 785 | 27.7 | FDD | IMD3 |
|  | n74 | 1452 | 5 | 25 | 1500 | N/A | FDD | N/A |
|  | n77 | 3689 | 10 | 50 | 1818.5 | N/A | FDD | N/A |
|  | n28 | N/A | 5 | 25 | 785 | 25.1 | FDD | IMD4 |
|  | n74 | 1458 | 5 | 25 | 1516 | N/A | FDD | N/A |
|  | n77 | 3589 | 10 | 50 | 1818.5 | N/A | FDD | N/A |
| CA\_n28-n77-n79 | n77 | 3620 | 10 | 50 | 3620 | N/A | TDD | N/A |
|  | n79 | 4420 | 40 | 216 | 4420 | N/A | TDD | N/A |
|  | n28 | 745 | 5 | 25 | 800 | 22.7 | FDD | IMD21, 2 |
| CA\_n28-n78-n79 | n28 | 740 | 5 | 25 | 795 | N/A | FDD | N/A |
|  | n78 | 3700 | 10 | 50 | 3700 | N/A | TDD | N/A |
|  | n79 | N/A | 40 | N/A | 4440 | 32.2 | TDD | IMD23,4 |
|  | n28 | 740 | 5 | 25 | 795 | N/A | FDD | N/A |
|  | n78 | 3320 | 10 | 50 | 3320 | N/A | TDD | N/A |
|  | n79 | N/A | 40 | N/A | 4440 | 5.7 | TDD | IMD53,4 |
|  | n28 | 740 | 5 | 25 | 795 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3700 | 32.9 | TDD | IMD23 |
|  | n79 | 4440 | 40 | 216 | 4440 | N/A | TDD | N/A |
|  | n28 | 740 | 5 | 25 | 795 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3420 | 16.8 | TDD | IMD33 |
|  | n79 | 4900 | 40 | 216 | 4900 | N/A | TDD | N/A |
|  | n28 | N/A | 5 | N/A | 800 | 22.2 | FDD | IMD2 |
|  | n78 | 3620 | 10 | 50 | 3620 | N/A | TDD | N/A |
|  | n79 | 4420 | 40 | 216 | 4420 | N/A | TDD | N/A |
|  | n28 | N/A | 5 | N/A | 790 | 5.7 | FDD | IMD5 |
|  | n78 | 3530 | 10 | 50 | 3530 | N/A | TDD | N/A |
|  | n79 | 4900 | 40 | 216 | 4900 | N/A | TDD | N/A |
| CA\_n29-n30-n77 | n29 | N/A | 5 | N/A | 722 | 23.5 | FDD | IMD31 |
|  | n30 | 2310 | 5 | 25 | 2355 | N/A | FDD | N/A |
|  | n77 | 3898 | 10 | 50 | 3898 | N/A | TDD | N/A |
| CA\_n29-n66-n77 | n29 | N/A | 5 | N/A | 722 | 23.5 | FDD | IMD35 |
|  | n66 | 1734 | 5 | 25 | 2134 | N/A | FDD | N/A |
|  | n77 | 4190 | 10 | 50 | 4190 | N/A | TDD | N/A |
| CA\_n30-n66-n77 | n30 | N/A | 5 | N/A | 2355 | 34.2 | FDD | IMD25 |
|  | n66 | 1745 | 5 | 25 | 2145 | N/A | FDD | N/A |
|  | n77 | 4100 | 10 | 50 | 4100 | N/A | TDD | N/A |
|  | n30 | N/A | 5 | N/A | 2355 | 12.9 | FDD | IMD5 |
|  | n66 | 1735 | 5 | 25 | 2135 | N/A | FDD | N/A |
|  | n77 | 3780 | 10 | 50 | 3780 | N/A | TDD | N/A |
|  | n30 | 2310 | 5 | 25 | 2355 | N/A | FDD | N/A |
|  | n66 | N/A | 5 | N/A | 2160 | 19.2 | FDD | IMD45 |
|  | n77 | 3390 | 10 | 50 | 3390 | N/A | TDD | N/A |
| CA\_n41-n66-n77 | n41 | 2600 | 5 | 25 | 2600 | N/A | TDD | N/A |
|  | n66 | 1730 | 5 | 25 | 2130 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3470 | 25.1 | TDD | IMD31,2 |
|  | n41 | N/A | 5 | N/A | 2670 | 18.0 | TDD | IMD55 |
|  | n66 | 1715 | 5 | 25 | 2115 | N/A | FDD | N/A |
|  | n77 | 4190 | 10 | 50 | 4190 | N/A | TDD | N/A |
|  | n41 | 2640 | 5 | 25 | 2640 | N/A | TDD | N/A |
|  | n66 | N/A | 5 | N/A | 2160 | 21.0 | FDD | IMD4 |
|  | n77 | 3720 | 10 | 50 | 3720 | N/A | TDD | N/A |
| CA\_n41-n71-n77 | n41 | 2615 | 5 | 25 | 2615 | N/A | TDD | N/A |
|  | n71 | 693 | 5 | 25 | 647 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3308 | 35.1 | TDD | IMD21,5 |
|  | n41 | 2564 | 5 | 25 | 2564 | N/A | TDD | N/A |
|  | n71 | 693 | 5 | 25 | 647 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3950 | 25.3 | TDD | IMD31 |
|  | n41 | 2580 | 5 | 25 | 2580 | N/A | TDD | N/A |
|  | n71 | 693 | 5 | 25 | 647 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3774 | 22.4 | TDD | IMD41 |
|  | n41 | N/A | 5 | N/A | 2615 | 34.7 | TDD | IMD25 |
|  | n71 | 693 | 5 | 25 | 647 | N/A | FDD | N/A |
|  | n77 | 3308 | 10 | 50 | 3308 | N/A | TDD | N/A |
|  | n41 | N/A | 5 | N/A | 2564 | 24.5 | TDD | IMD3 |
|  | n71 | 693 | 5 | 25 | 647 | N/A | FDD | N/A |
|  | n77 | 3950 | 10 | 50 | 3950 | N/A | TDD | N/A |
|  | 41 | 2680 | 5 | 25 | 2680 | N/A | TDD | N/A |
|  | n71 | N/A | 5 | N/A | 640 | 36.8 | FDD | IMD25 |
|  | n77 | 3320 | 10 | 50 | 3320 | N/A | TDD | N/A |
| CA\_n41-n74-n77 | n41 | 2650 | 10 | 50 | 2650 | N/A | TDD | N/A |
|  | n74 | N/A | 5 | N/A | 1500 | 35.2 | FDD | IMD22 |
|  | n77 | 4150 | 10 | 50 | 4150 | NA | TDD | N/A |
|  | n41 | 2525 | 10 | 50 | 2525 | N/A | TDD | N/A |
|  | n74 | N/A | 5 | N/A | 1500 | 24 | FDD | IMD3 |
|  | n77 | 3550 | 10 | 50 | 3550 | N/A | TDD | N/A |
|  | n41 | N/A | 10 | N/A | 2650 | 34 | TDD | IMD2 |
|  | n74 | 1450 | 5 | 25 | 1500 | N/A | FDD | N/A |
|  | n77 | 4100 | 10 | 50 | 4150 | N/A | TDD | N/A |
|  | n41 | N/A | 10 | N/A | 2518 | 13.9 | TDD | IMD5 |
|  | n74 | 1454 | 5 | 25 | 1502 | N/A | FDD | N/A |
|  | n77 | 3440 | 10 | 50 | 3440 | N/A | TDD | N/A |
|  | n41 | 2650 | 10 | 50 | 2650 | N/A | TDD | N/A |
|  | n74 | 1450 | 5 | 25 | 1500 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 4100 | 33 | TDD | IMD2 |
|  | n41 | 2525 | 10 | 50 | 2525 | N/A | TDD | N/A |
|  | n74 | 1450 | 5 | 25 | 1498 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3600 | 23 | TDD | IMD31 |
| CA\_n66-n71-n77 | n66 | 1720 | 5 | 25 | 2120 | N/A | FDD | N/A |
|  | n71 | 668 | 5 | 25 | 622 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 4108 | 24.9 | TDD | IMD31,2,5 |
|  | n66 | N/A | 5 | N/A | 2150 | 24.5 | FDD | IMD32 |
|  | n71 | 690 | 5 | 25 | 644 | N/A | FDD | N/A |
|  | n77 | 3530 | 10 | 50 | 3530 | N/A | TDD | N/A |
|  | n66 | 1720 | 5 | 25 | 2120 | N/A | FDD | N/A |
|  | n71 | N/A | 5 | N/A | 640 | 24.3 | FDD | IMD35 |
|  | n77 | 4080 | 10 | 50 | 4080 | N/A | TDD | N/A |
| NOTE 1: This band is subject to IMD5 also which MSD is not specified.  NOTE 2: This band is subject to IMD4 also which MSD is not specified.  NOTE 3: The requirements only apply for UEs supporting inter-band carrier aggregation with simultaneous Rx/Tx capability. Simultaneous Rx/Tx capability does not apply for UEs supporting band n78 with a n77 implementation.  NOTE 4: This band is subject to IMD3 also which MSD is not specified.  NOTE 5: For a UE which supports this band combination only when the Band n77 frequency range restriction defined in NOTE 12 of Table 5.2-1 applies, the MSD test point(s) cannot be verified for the band combination and the test point(s) can be skipped.  NOTE 6: Both of the transmitters shall be set min(+23 dBm, PCMAX\_L,f,c) as defined in clause 6.2A.4  NOTE 7: This band supports intra-band non-contiguous uplink configuration.  NOTE 8: In Japan, n77 band is restricted to 3400 – 4100 MHz frequency range, and there are no valid MSD test points when using this restricted frequency range | | | | | | | | |

Table 7.3A.5-2b: 3DL/2UL inter-band Reference sensitivity QPSK PREFSENS and uplink/downlink configurations for PC1.5 CA

| Band / Channel bandwidth / NRB / Duplex mode | | | | | | | | | | Source of IMD |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| NR CA  Configuration | NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | | Duplex mode | |  |
| CA\_n1-n3-n78 | n1 | 1950 | 5 | 25 | 2140 | N/A | | FDD | | N/A |
|  | n3 | N/A | 5 | N/A | 1830 | 38.7 | | FDD | | IMD2 |
|  | n78 | 3780 | 10 | 50 | 3780 | N/A | | TDD | | N/A |
| CA\_n1-n7-n78 | n1 | 1977.5 | 5 | 25 | 2167.5 | N/A | | FDD | | N/A |
|  | n7 | N/A | 5 | N/A | 2627.5 | 25.2 | | FDD | | IMD4 |
|  | n78 | 3305 | 10 | 50 | 3305 | N/A | | TDD | | N/A |
|  | n1 | N/A | 5 | N/A | 2140 | 29.5 | FDD | | IMD4 | |
|  | n7 | 2510 | 10 | 50 | 2630 | N/A | FDD | | N/A | |
|  | n78 | 3580 | 10 | 50 | 3580 | N/A | TDD | | N/A | |
| CA\_n1-n26-n78 | n1 | N/A | 5 | N/A | 2122 | 31.9 | | FDD | | IMD3 |
|  | n26 | 829 | 5 | 25 | 874 | N/A | | FDD | | N/A |
|  | n78 | 3780 | 10 | 50 | 3780 | N/A | | TDD | | N/A |
|  | n1 | 1975 | 5 | 25 | 2165 | N/A | | FDD | | N/A |
|  | n26 | N/A | 5 | N/A | 885 | 23.9 | | FDD | | IMD5 |
|  | n78 | 3405 | 10 | 50 | 3405 | N/A | | TDD | | N/A |
| CA\_n1-n28-n78 | n1 | N/A | 5 | N/A | 2150 | 29.4 | | FDD | | IMD3 |
|  | n28 | 740 | 5 | 25 | 795 | N/A | | FDD | | N/A |
|  | n78 | 3630 | 10 | 50 | 3630 | N/A | | TDD | | N/A |
|  | n1 | 1970 | 5 | 25 | 2160 | N/A | | FDD | | N/A |
|  | n28 | N/A | 5 | N/A | 794 | 21.3 | | FDD | | IMD5 |
|  | n78 | 3352 | 10 | 50 | 3352 | N/A | | TDD | | N/A |
| CA\_n2-n5-n77 | n2 | 1907.5 | 5 | 25 | 1987.5 | N/A | | FDD | | N/A |
|  | n5 | N/A | 5 | N/A | 887.5 | 30.3 | | FDD | | IMD55 |
|  | n77 | 3305 | 10 | 50 | 3305 | N/A | | TDD | | N/A |
|  | n2 | N/A | 5 | N/A | 1987 | 34.5 | | FDD | | IMD35 |
|  | n5 | 846.5 | 5 | 25 | 891.5 | N/A | | FDD | | N/A |
|  | n77 | 3680 | 10 | 50 | 3680 | N/A | | TDD | | N/A |
| CA\_n2-n66-n77 | n2 | 1855 | 5 | 25 | 1935 | N/A | | FDD | | N/A |
|  | n66 | N/A | 5 | N/A | 2115 | 41.2 | | FDD | | IMD21,2 |
|  | n77 | 3970 | 10 | 50 | 3970 | N/A | | TDD | | N/A |
|  | n2 | N/A | 5 | N/A | 1960 | 44.1 | | FDD | | IMD21,2 |
|  | n66 | 1760 | 5 | 25 | 2160 | N/A | | FDD | | N/A |
|  | n77 | 3720 | 10 | 50 | 3720 | N/A | | TDD | | N/A |
|  | n2 | N/A | 5 | 25 | 1950 | 33.3 | | FDD | | IMD3 |
|  | n66 | 1775 | 5 | 25 | 2195 | N/A | | FDD | | N/A |
|  | n77 | 3300 | 100 | 1 (RBstart=203) | 3300 | N/A | | TDD | | N/A |
|  |  | 3400 | 100 | 1 (RBstart=67) | 3400 |  | |  | |  |
| CA\_n3-n7-n78 | n3 | N/A | 5 | N/A | 1820 | 31.4 | FDD | | IMD3 | |
|  | n7 | 2565 | 5 | 25 | 2685 | N/A | FDD | | N/A | |
|  | n78 | 3310 | 10 | 50 | 3310 | N/A | TDD | | N/A | |
|  | n3 | N/A | 5 | N/A | 1820 | 29.4 | FDD | | IMD4 | |
|  | n7 | 2565 | 5 | 25 | 2685 | N/A | FDD | | N/A | |
|  | n78 | 3475 | 10 | 50 | 3475 | N/A | TDD | | N/A | |
| CA\_n3-n26-n78 | n3 | N/A | 5 | N/A | 1862 | 29.4 | | FDD | | IMD3 |
|  | n26 | 839 | 5 | 25 | 884 | N/A | | FDD | | N/A |
|  | n78 | 3540 | 10 | 50 | 3540 | N/A | | TDD | | N/A |
| CA\_n3-n28-n78 | n3 | N/A | 5 | N/A | 1850 | 31 | | FDD | | IMD3 |
|  | n28 | 735 | 5 | 25 | 790 | N/A | | FDD | | N/A |
|  | n78 | 3320 | 10 | 50 | 3320 | N/A | | TDD | | N/A |
| CA\_n7-n26-n78 | n7 | 2550 | 5 | 25 | 2670 | N/A | | FDD | | N/A |
|  | n26 | N/A | 5 | N/A | 879 | 41 | | FDD | | IMD2 |
|  | n78 | 3429 | 10 | 50 | 3429 | N/A | | TDD | | N/A |
|  | n7 | 2525 | 5 | 25 | 2645 | N/A | | FDD | | N/A |
|  | n26 | N/A | 5 | N/A | 875 | 24.3 | | FDD | | IMD5 |
|  | n78 | 3350 | 10 | 50 | 3350 | N/A | | TDD | | N/A |
|  | n7 | N/A | 5 | N/A | 2645 | 40.9 | FDD | | IMD2 | |
|  | n26 | 844 | 5 | 25 | 889 | N/A | FDD | | N/A | |
|  | n78 | 3489 | 10 | 50 | 3489 | N/A | TDD | | N/A | |
| CA\_n7-n28-n78 | n7 | 2567.5 | 5 | 25 | 2687.5 | N/A | FDD | | N/A | |
|  | n28 | N/A | 5 | N/A | 782.5 | 39.6 | FDD | | IMD21 | |
|  | n78 | 3350 | 10 | 50 | 3350 | N/A | TDD | | N/A | |
|  | n7 | N/A | 5 | N/A | 2650 | 41.3 | | FDD | | IMD2 |
|  | n28 | 740 | 5 | 25 | 795 | N/A | | FDD | | N/A |
|  | n78 | 3390 | 10 | 50 | 3390 | N/A | | TDD | | N/A |
| CA\_n25-n41-n66 | n25 | N/A | 5 | N/A | 1940 | 35.0 | | FDD | | IMD4 |
|  | n41 | 2685 | 10 | 50 | 2685 | N/A | | TDD | | N/A |
|  | n66 | 1715 | 5 | 25 | 2115 | N/A | | FDD | | N/A |
| CA\_n25-n41-n77 | n25 | 1870 | 5 | 25 | 1950 | N/A | | FDD | | N/A |
|  | n41 | 2670 | 5 | 25 | 2670 | N/A | | TDD | | N/A |
|  | n77 | N/A | 10 | N/A | 3470 | 32.8 | | TDD | | IMD3 |
|  | n25 | 1900 | 5 | 25 | 1980 | N/A | | FDD | | N/A |
|  | n41 | 2525 | 5 | 25 | 2645 | N/A | | TDD | | N/A |
|  | n77 | N/A | 10 | N/A | 3775 | 31.4 | | TDD | | IMD5 |
|  | n25 | 1870 | 5 | 25 | 1950 | N/A | | FDD | | N/A |
|  | n41 | N/A | 5 | N/A | 2640 | 33.0 | | TDD | | IMD55 |
|  | n77 | 4125 | 10 | 50 | 4125 | N/A | | TDD | | N/A |
|  | n25 | N/A | 5 | N/A | 1950 | 35.6 | | FDD | | IMD35 |
|  | n41 | 2675 | 5 | 25 | 2675 | N/A | | TDD | | N/A |
|  | n77 | 3400 | 10 | 50 | 3400 | N/A | | TDD | | N/A |
|  | n25 | N/A | 5 | N/A | 1950 | 31.4 | | FDD | | IMD4 |
|  | n41 | 2550 | 5 | 25 | 2685 | N/A | | TDD | | N/A |
|  | n77 | 3525 | 10 | 50 | 3525 | N/A | | TDD | | N/A |
| CA\_n25-n66-n77 | n25 | 1855 | 5 | 25 | 1935 | N/A | FDD | | N/A | |
|  | n66 | N/A | 5 | N/A | 2115 | 41.2 | FDD | | IMD2 | |
|  | n77 | 3970 | 10 | 50 | 3970 | N/A | TDD | | N/A | |
|  | n25 | 1900 | 5 | 25 | 1980 | N/A | FDD | | N/A | |
|  | n66 | N/A | 5 | N/A | 2160 | 34.4 | FDD | | IMD4 | |
|  | n77 | 3540 | 10 | 50 | 3540 | N/A | TDD | | N/A | |
|  | n25 | 1900 | 5 | 25 | 1980 | N/A | FDD | | N/A | |
|  | n66 | N/A | 5 | N/A | 2160 | 31.2 | FDD | | IMD5 | |
|  | n77 | 3930 | 10 | 50 | 3930 | N/A | TDD | | N/A | |
|  | n25 | N/A | 5 | N/A | 1960 | 44.1 | FDD | | IMD2 | |
|  | n66 | 1760 | 5 | 25 | 2160 | N/A | FDD | | N/A | |
|  | n77 | 3720 | 10 | 50 | 3720 | N/A | TDD | | N/A | |
|  | n25 | N/A | 5 | N/A | 1960 | 33.1 | FDD | | IMD45 | |
|  | n66 | 1770 | 5 | 25 | 2170 | N/A | FDD | | N/A | |
|  | n77 | 3350 | 10 | 50 | 3350 | N/A | TDD | | N/A | |
|  | n25 | N/A | 5 | N/A | 1960 | 27.6 | FDD | | IMD55 | |
|  | n66 | 1760 | 5 | 25 | 2160 | N/A | FDD | | N/A | |
|  | n77 | 3620 | 10 | 50 | 3620 | N/A | TDD | | N/A | |
| CA\_n25-n71-n77 | n25 | N/A | 5 | N/A | 1954 | 34.5 | FDD | | IMD32,5 | |
|  | n71 | 693 | 5 | 25 | 647 | N/A | FDD | | N/A | |
|  | n77 | 3340 | 10 | 50 | 3340 | N/A | TDD | | N/A | |
| CA\_n41-n66-n77 | n41 | 2600 | 5 | 25 | 2600 | N/A | TDD | | N/A | |
|  | n66 | 1730 | 5 | 25 | 2130 | N/A | FDD | | N/A | |
|  | n77 | N/A | 10 | N/A | 3470 | 34.1 | TDD | | IMD31,2 | |
|  | n41 | N/A | 5 | N/A | 2670 | 32.9 | TDD | | IMD55 | |
|  | n66 | 1715 | 5 | 25 | 2115 | N/A | FDD | | N/A | |
|  | n77 | 4190 | 10 | 50 | 4190 | N/A | TDD | | N/A | |
|  | n41 | 2640 | 5 | 25 | 2640 | N/A | TDD | | N/A | |
|  | n66 | N/A | 5 | N/A | 2160 | 33.0 | FDD | | IMD4 | |
|  | n77 | 3720 | 10 | 50 | 3720 | N/A | TDD | | N/A | |
| CA\_n41-n71-n77 | n41 | 2615 | 5 | 25 | 2615 | N/A | | TDD | | N/A |
|  | n71 | 693 | 5 | 25 | 647 | N/A | | FDD | | N/A |
|  | n77 | N/A | 10 | N/A | 3308 | 41.1 | | TDD | | IMD21,5 |
|  | n41 | 2564 | 5 | 25 | 2564 | N/A | | TDD | | N/A |
|  | n71 | 693 | 5 | 25 | 647 | N/A | | FDD | | N/A |
|  | n77 | N/A | 10 | N/A | 3950 | 34.3 | | TDD | | IMD31 |
|  | n41 | 2580 | 5 | 25 | 2580 | N/A | | TDD | | N/A |
|  | n71 | 693 | 5 | 25 | 647 | N/A | | FDD | | N/A |
|  | n77 | N/A | 10 | N/A | 3774 | 34.3 | | TDD | | IMD41 |
|  | n41 | N/A | 5 | N/A | 2615 | 40.7 | | TDD | | IMD25 |
|  | n71 | 693 | 5 | 25 | 647 | N/A | | FDD | | N/A |
|  | n77 | 3308 | 10 | 50 | 3308 | N/A | | TDD | | N/A |
|  | n41 | N/A | 5 | N/A | 2564 | 33.5 | | TDD | | IMD3 |
|  | n71 | 693 | 5 | 25 | 647 | N/A | | FDD | | N/A |
|  | n77 | 3950 | 10 | 50 | 3950 | N/A | | TDD | | N/A |
|  | 41 | 2680 | 5 | 25 | 2680 | N/A | | TDD | | N/A |
|  | n71 | N/A | 5 | N/A | 640 | 42.8 | | FDD | | IMD25 |
|  | n77 | 3320 | 10 | 50 | 3320 | N/A | | TDD | | N/A |
| CA\_n66-n71-n77 | n66 | N/A | 5 | N/A | 2150 | 33.5 | | FDD | | IMD32 |
|  | n71 | 690 | 5 | 25 | 644 | N/A | | FDD | | N/A |
|  | n77 | 3530 | 10 | 50 | 3530 | N/A | | TDD | | N/A |
|  | n66 | 1720 | 5 | 25 | 2120 | N/A | | FDD | | N/A |
|  | n71 | N/A | 5 | N/A | 640 | 33.3 | | FDD | | IMD35 |
|  | n77 | 4080 | 10 | 50 | 4080 | N/A | | TDD | | N/A |
| NOTE 1: This band is subject to IMD5 also which MSD is not specified.  NOTE 2: This band is subject to IMD4 also which MSD is not specified.  NOTE 3: The requirements only apply for UEs supporting inter-band carrier aggregation with simultaneous Rx/Tx capability. Simultaneous Rx/Tx capability does not apply for UEs supporting band n78 with a n77 implementation.  NOTE 4: This band is subject to IMD3 also which MSD is not specified.  NOTE 5: For a UE which supports this band combination only when the Band n77 frequency range restriction defined in NOTE 12 of Table 5.2-1 applies, the MSD test point(s) cannot be verified for the band combination and the test point(s) can be skipped  NOTE 6: This band combination is specified with support of two band inter-band UL CA with UL MIMO or Tx diversity capabilities, and the transmitter shall be set at min (+23 dBm, PCMAX\_L,f,c) for the UL band with single Tx antenna connector as defined in clause 6.2A.4, and set at min (+27.8 dBm, PCMAX\_L,f,c) for the UL band with 2Tx antenna connectors as defined in clause 6.2H.3.4 or 6.2L.3.4. | | | | | | | | | | |

---End of changes---