**3GPP TSG-RAN4 Meeting #116-bis *R4-2514168***

**Prague, Czech Republic, 13 – 17 October, 2025**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** | xxxx | **rev** | - | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | draftCR on RRM requirements for LP-WUR |
|  |  |
| ***Source to WG:*** | Huawei, HiSilicon |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_LPWUS-Core |  | ***Date:*** | 2025-09-28 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** | Rel-19 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | There is one open issue in MR serving cell measurement requirements, i.e. the separation between measurment samples used for filtering when MR is relaxation mode. Currently the separation is defined as “either 8 DRX cycles or DRX cycle/2”. |
|  |  |
| ***Summary of change:*** | Clarify that the separation between measurment samples used for filtering when MR is relaxation mode is 8 DRX cycles. |
|  |  |
| ***Consequences if not approved:*** | The MR serving cell measurement requirements are not fully complete. |
|  |  |
| ***Clauses affected:*** | 4.8.2.3.1, 4.8.2.3.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

<Start of Change 1>

4.8.2.3.1 Requirements for evaluation of cell selection criterion

When LP-WUS UE is not in relaxed measurement mode as defined in [1], the requirements in clause 4.2.2.2 shall apply.

When LP-WUS UE is in relaxed measurement mode as defined in [1], the UE shall measure the SS-RSRP and SS-RSRQ level of the serving cell and evaluate the cell selection criterion S defined in TS 38.304 [1] for the serving cell at least once every N1\*16 DRX cycle.

The LP-WUS UE shall filter the SS-RSRP and SS-RSRQ measurements of the serving cell using at least 2 measurements. Within the set of measurements used for the filtering, at least two measurements shall be spaced by 8 DRX cycles.

If the LP-WUS UE has evaluated according to table 4.8.2.3.1-1 in 16\*Nserv consecutive DRX cycles that the serving cell does not fulfil the cell selection criterion S, the LP-WUS UE shall initiate the measurements of all neighbour cells indicated by the serving cell, regardless of the measurement rules currently limiting LP-WUS UE measurement activities.

If the LP-WUS UE in RRC\_IDLE has not found any new suitable cell based on searches and measurements using the intra-frequency, inter-frequency and inter-RAT information indicated in the system information during the time T, the LP-WUS UE shall initiate cell selection procedures for the selected PLMN as defined in TS 38.304 [1], where T= 10s.

**Table 4.8.2.3.1-1: Nserv**

|  |  |  |
| --- | --- | --- |
| **DRX cycle length [s]** | **Scaling Factor (N1)** | **Nserv [number of 16\*DRX cycles]** |
| **FR1** | **FR2-1Note1** |
| 0.32 | 1 | 8 | N1\*4 |
| 0.64 | 5 | N1\*4 |
| 1.28 | 4 | N1\*2 |
| 2.56 | 3 | N1\*2 |
| NOTE 1: Applies for UE supporting FR2-1 power class 2&3&4. For UE supporting FR2-1 power class 1 or 5, N1 = 8 for all DRX cycle length. |

4.8.2.3.2 Requirements for evaluation of LP-WUS related conditions

When LP-WUS UE is in relaxed measurement mode as defined in [1], the LP-WUS UE shall measure the SS-RSRP and SS-RSRQ level of the serving cell and evaluate the following LP-WUR related conditions defined in TS 38.304 [1], if configured, for the serving cell at least once every N1\*16 DRX cycle.

*-* exit condition for relaxed measurement mode

The LP-WUS UE shall filter the SS-RSRP and SS-RSRQ measurements of the serving cell using at least 2 measurements. Within the set of measurements used for the filtering, at least two measurements shall be spaced by 8 DRX cycles.

If the LP-WUS UE has evaluated according to table 4.8.2.3.2-1 in 16\*Nserv consecutive DRX cycles that the serving cell fulfils the exit condition for relaxed measurement mode, the LP-WUS UE shall perform corresponding actions as defined in clause 5.2.4.x in [1].

**Table 4.8.2.3.2-1: Nserv when UE is in relaxed measurement mode**

|  |  |  |
| --- | --- | --- |
| **DRX cycle length [s]** | **Scaling Factor (N1)** | **Nserv [number of 16\*DRX cycles]** |
| **FR1** | **FR2-1Note1** |
| 0.32 | 1 | 8 | N1\*4 |
| 0.64 | 5 | N1\*4 |
| 1.28 | 4 | N1\*2 |
| 2.56 | 3 | N1\*2 |
| NOTE 1: Applies for UE supporting FR2-1 power class 2&3&4. For UE supporting FR2-1 power class 1 or 5, N1 = 8 for all DRX cycle length. |

<End of Change 1>