**3GPP TSG-RAN4 Meeting #116-bis *R4-2515145***

**Prague, Czech Republic, 13 – 17 October, 2025**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** | xxxx | **rev** | 1 | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | draftCR on RRM requirements for RedCap UE in NTN |
|  |  |
| ***Source to WG:*** | Huawei, HiSilicon |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_NTN\_Ph3-Core |  | ***Date:*** | 2025-09-28 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** | Rel-19 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | There are some issues with cell reselection requirements:* In the table for eDRX, there are some notes related to PTW, DRX cycle based measurement and M2. This is confusing because there is no PTW and the measurement is always based on eDRX cycle, and M2 is not used in the requirements.
* The definition of K\_multi\_SMTC is duplicated for RedCap NTN. This is redundant because there is already a reference to existing NTN clause.
* The definition of Ttrigger in inter-frequency requirements is based on HST requirements for normal UE, which are more stringent than the enhanced requirements for RedCap NTN.
 |
|  |  |
| ***Summary of change:*** | Correct cell reselection requirements for RedCap NTN:* Remove the notes in tables for eDRX that are related to PTW, DRX cycle based measurement and M2 .
* Remove the definition of K\_multi\_SMTC
* Update the definition of Ttrigger in inter-frequency requirements such that it is based on the enhanced requirements for RedCap NTN.
* Correct some errors in reference number to the tables.
 |
|  |  |
| ***Consequences if not approved:*** | Cell reselection requirements for RedCap NTN are not fully correct. |
|  |  |
| ***Clauses affected:*** | 4.2E.2.2, 4.2E.2.3, 4.2E.2.4 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

<Start of Change 1>

4.2E.2.2 Measurement and evaluation of serving cell for RedCap UEs

The RedCap UE shall measure the SS-RSRP and SS-RSRQ level of the serving cell and evaluate the cell selection criterion S defined in TS 38.304 [1] for the serving cell at least once every M1\*N1 DRX cycle; where:

- M1=2 if SMTC periodicity (TSMTC) > 20 ms and DRX cycle ≤ 0.64 second and NSMTC =1, upon one SMTC configured at the UE,

- M1=2.5 if SMTC periodicity (TSMTC) > 20 ms and DRX cycle ≤ 0.64 second and 1<NSMTC ≤ 4,

- otherwise M1=1.

Where, NSMTC is the number of SMTCs configured by SAN.

The UE shall filter the SS-RSRP and SS-RSRQ measurements of the serving cell using at least 2 measurements. Within the set of measurements used for the filtering, at least two measurements shall be spaced by, at least eDRX\_IDLE cycle/2, when the RedCap UE is configured with eDRX cycle ≤10.24s; otherwise, DRX cycle/2.

If the UE is not configured with eDRX\_IDLE cycle and the UE has evaluated according to table 4.2C.2.2-1 (only FR1) for both 1Rx RedCap and 2Rx RedCap in Nserv\_RedCap consecutive DRX cycles that the serving cell does not fulfil the cell selection criterion S, the UE shall initiate the measurements of all neighbour cells indicated by the serving cell, regardless of the measurement rules currently limiting UE measurement activities. In this case the UE shall not relax measurements on any of the neighbour cells even if UE has fulfilled the criteria for meeting the relaxed measurement requirements defined clauses 4.2E.2.7 and 4.2E.2.8.

If the UE is configured with eDRX\_IDLE cycle and has evaluated according to table 4.2E.2.2-1, in Nserv\_RedCap consecutive eDRX cycles, the UE shall initiate the measurements of all neighbour cells indicated by the serving cell, regardless of the measurement rules currently limiting UE measurement activities. In this case the UE shall not relax measurements on any of the neighbour cells even if UE has fulfilled the criteria for meeting the relaxed measurement requirements defined clauses 4.2E.2.7 and 4.2E.2.8.

For the UE configured with eDRX\_IDLE cycle, Nserv\_RedCap is specified in table 4.2E.2.2-1 for 1 Rx RedCap and 2 Rx RedCap in FR1.Additionally, if the UE is configured with ‘*t-service*’ [2], the UE shall start measurements of the neighbour cells indicated by the serving cell before ‘*t-service*’ is reached according to the requirements provided in clauses 4.2E.2.3 and 4.2E.2.4.

Also,

- if *distanceThresh* and *referenceLocation* are configured by the network [2] and the UE supports location-based measurement initiation and has obtained its location information, the UE shall initiate the measurements of all neighbour cells indicated by the serving cell if the distance between UE and the serving cell reference location – *referenceLocation ­–* is larger than *distanceThresh.* The requirements apply provided that the distance exceeds the *distanceThresh* by a margin of 50 m.

- if *distanceThresh* and *movingReferenceLocation* are configured by the network [2] and the UE supports location-based measurement initiation and has obtained its location information, the UE shall initiate the measurements of all neighbour cells indicated by the serving cell if the distance between UE and the serving cell moving reference location – *movingReferenceLocation ­–* is larger than *distanceThresh.* The requirements apply provided that the distance exceeds the *distanceThresh* by a margin of 80 m.

If the UE is not configured with*‘t-Service*’ [2] in the serving cell and if the UE in RRC\_IDLE has not found any new suitable cell based on searches and measurements using the intra-frequency, inter-frequency and inter-RAT information indicated in the system information during the time T, the UE shall initiate cell selection procedures for the selected PLMN as defined in TS 38.304 [1], where

- T= 10 s if the UE is not configured with eDRX\_IDLE cycle, or

- T= MAX (10 s, one eDRX\_IDLE cycle) if the UE is configured with eDRX\_IDLE cycle in FR1

If the UE is configured with ‘*t-Service*’ in the serving cell then the UE shall initiate cell selection procedures for the selected PLMN as defined in TS 38.304 [1] when any of the following conditions is fulfilled:

- If the UE in RRC\_IDLE has not found any new suitable cell based on searches and measurements using the intra-frequency, inter-frequency and inter-RAT information indicated in the system information within T since time instance T1 provided that ‘*t-Service*’ > T1 or

- If the UE in RRC\_IDLE has not found any new suitable cell based on searches and measurements using the intra-frequency, inter-frequency and inter-RAT information indicated in the system information within T since the time instance ‘*t-Service*’.

- Where, T1 is the time instance in seconds when the UE has determined that the serving cell does not fulfil the cell selection criterion S.

**Table 4.2E.2.2-1: Nserv\_RedCap for UE configured with eDRX\_IDLE cycle (Frequency range FR1)**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **eDRX\_IDLE cycle length [s]** | **DRX cycle length [s]** | **PTW length [s] (number of 1.28 s periods)** | **Scaling Factor (N1)** | **Nserv\_RedCap [number of eDRX cycles]** |
| 2.56 | N/A  | N/A | 1 | N1\*2 |
| 5.12 | N/A  | N/A | N1\*2 |
| 10.24 | N/A  | N/A | N1\*2 |
| NOTE 1: Void.NOTE 2: The eDRX\_IDLE cycle lengths are as specified in section 10.5.5.32 of TS 24.008 [42].NOTE 3: Void.NOTE 4: Void |

4.2E.2.3 Measurements of intra-frequency NR cells for RedCap UE

The UE shall be able to identify new intra-frequency cells and perform SS-RSRP and SS-RSRQ measurements of the identified intra-frequency cells without an explicit intra-frequency neighbour list containing physical layer cell identities.

If Srxlev > SIntraSearchP and Squal > SIntraSearchQ, and the distance between UE and serving cell reference location or serving cell moving reference location is smaller than *distanceThresh* if the *distanceThresh* is configured (see TS 38.304[1]) and UE has location information, then the UE is not required to perform measurement of intra-frequency.

The UE shall be able to evaluate whether a newly detectable intra-frequency cell meets the reselection criteria defined in TS 38.304 [1] within Kmulti\_SMTC \* Tdetect,NR\_Intrawhen that Treselection= 0 if the UE does not support *Enhanced RRM requirements for measurements in IDLE and INACTIVE modes* defined in TS 38.306 [14] or if the *enhancedMeasurementNGSO-r17* is not enabled, or within Kmulti\_SMTC \* Tdetect,NR\_Intra\_enhif the UE supports *Enhanced RRM requirements for measurements in IDLE and INACTIVE modes* defined in TS 38.306 [14] and the *enhancedMeasurementNGSO-r17* is enabled. An intra-frequency cell is considered to be detectable according to the conditions defined in annex B.1.6 for a corresponding Band.

The UE shall measure SS-RSRP and SS-RSRQ at least every Kmulti\_SMTC \* Tmeasure,NR\_Intra if the UE does not support *Enhanced RRM requirements for measurements in IDLE and INACTIVE modes* defined in TS 38.306 [14] or if the *enhancedMeasurementNGSO-r17* is not enabled, or every Kmulti\_SMTC \* Tmeasure,NR\_Intra\_enh if the UE supports *Enhanced RRM requirements for measurements in IDLE and INACTIVE modes* defined in TS 38.306 [14] and the *enhancedMeasurementNGSO-r17* is enabled, for intra-frequency cells that are identified and measured according to the measurement rules.The UE shall filter SS-RSRP and SS-RSRQ measurements of each measured intra-frequency cell using at least 2 measurements. Within the set of measurements used for the filtering, at least two measurements shall be spaced by at least Tmeasure,NR\_Intra/2. The UE shall not consider an NR neighbour cell for cell reselection, if it is indicated as not allowed in the measurement control system information of the serving cell.

The parameter Kmulti\_SMTC is the scaling factor for measurements of multiple SMTCs or multiple satellites, which refers to clause 4.2C.2.3.

For an intra-frequency cell that has been already detected, but that has not been reselected to, the filtering shall be such that the UE shall be capable of evaluating that the intra-frequency cell has met reselection criterion defined in TS 38.304 [1] within Kmulti\_SMTC \* Tevaluate,NR\_Intra if the UE does not support *Enhanced RRM requirements for measurements in IDLE and INACTIVE modes* defined in TS 38.306 [14] or if the *enhancedMeasurementNGSO-r17* is not enabled, or within Kmulti\_SMTC \* Tevaluate,NR\_Intra\_enh if the UE supports *Enhanced RRM requirements for measurements in IDLE and INACTIVE modes* defined in TS 38.306 [14] and the *enhancedMeasurementNGSO-r17* is enabled, when Treselection = 0as specified in table 4.2C.2.3-1(with FR1), table 4.2E.2.3-1 or table 4.2E.2.3-2 provided that:

- when *rangeToBestCell* is not configured:

- the cell is at least 3 dB better ranked in FR1 for 2Rx RedCap, or

- the cell is at least 4 dB better ranked in FR1 for 1Rx RedCap.

- when *rangeToBestCell* is configured:

- the cell has the highest number of beams above the threshold *absThreshSS-BlocksConsolidation* among all detected cells whose cell-ranking criterion R value in TS 38.304 [1] is within *rangeToBestCell* of the cell-ranking criterion R value of the highest ranked cell.

- if there are multiple such cells, the cell has the highest rank among them.

- the cell is at least 3 dB better ranked in FR1 if the current serving cell is among them for 2 Rx RedCap.

- the cell is at least 4 dB better ranked in FR1 if the current serving cell is among them for 1 Rx RedCap.

The 1 Rx RedCap UE applies *absThreshSS-BlocksConsolidation* as the signalled value of *absThreshSS-BlocksConsolidation* [2] + 1 dB.

When evaluating cells for reselection, the SSB side conditions apply to both serving and non-serving intra-frequency cells.

If Treselection timer has a nonzero value and the intra-frequency cell is satisfied with the reselection criteria which are defined in TS 38.304 [1], the UE shall evaluate this intra-frequency cell for the Treselection time. If this cell remains satisfied with the reselection criteria within this duration, then the UE shall reselect that cell.

For both 1Rx RedCap and 2Rx RedCap not configured with eDRX\_IDLE cycle, Tdetect,NR\_Intra\_RedCap, Tmeasure,NR\_Intra\_RedCap and Tevaluate,NR\_Intra\_RedCap are specified in table 4.2C.2.3-1.

For 1 Rx RedCap and 2 Rx RedCap configured with eDRX\_IDLE cycle, Tdetect,NR\_Intra\_RedCap, Tmeasure,NR\_Intra\_RedCap and Tevaluate,NR\_Intra\_RedCap are specified in table 4.2E.2.3-1 for FR1, where the requirements apply provided that the serving cell is configured with eDRX\_IDLE.

For both 1Rx RedCap and 2Rx RedCap, Tdetect,NR\_Intra\_enh\_RedCap ,Tmeasure,NR\_Intra\_enh\_RedCap and Tevaluate,NR\_Intra\_enh\_RedCap are defined in table 4.2E.2.3-2.

**Table 4.2E.2.3-1: Tdetect,NR\_Intra\_RedCap, Tmeasure,NR\_Intra\_RedCap and Tevaluate,NR\_Intra\_RedCap for UE configured with eDRX\_IDLE cycle (Frequency range FR1)**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **eDRX\_IDLE cycle length [s]** | **DRX cycle length [s]** | **PTW length [s] (number of 1.28 s periods)** | **Tdetect,NR\_Intra\_RedCap [s] (number of eDRX cycles)** | **Tmeasure,NR\_Intra\_RedCap [s] (number of eDRX cycles)** | **Tevaluate,NR\_Intra\_RedCap [s] (number of eDRX cycles)** |
| 2.56 | - | - | 58.88 (23) | 2.56 (1) | 7.68 (3) |
| 5.12 | - | - | 117.76 (23) | 5.12 (1) | 10.24 (2) |
| 10.24 | - | - | 235.52 (23) | 10.24 (1) | 20.48 (2) |
| NOTE 1: VoidNOTE 2: The eDRX\_IDLE cycle lengths are as specified in section 10.5.5.32 of TS 24.008 [42].NOTE 3: Void NOTE 4: VoidNOTE 5: Void |

**Table 4.2E.2.3-2: Tdetect,NR\_Intra\_enh\_RedCap, Tmeasure,NR\_Intra\_enh\_RedCap and Tevaluate,NR\_Intra\_enh\_RedCap**

|  |  |  |  |
| --- | --- | --- | --- |
| **DRX cycle length [s]** | **Tdetect,NR\_Intra\_enh\_RedCap [s] (number of DRX cycles)** | **Tmeasure,NR\_Intra\_enh\_RedCap [s] (number of DRX cycles)** | **Tevaluate,NR\_Intra\_enh\_RedCap [s] (number of DRX cycles)** |
|
| 0.32 |  3.2 x M2 (10 x M2)Note 1 | 0.32 x M3 (1 x M3) Note 1 | 0.96 x M4 (3 x M4) Note 1 |
| 0.64 | 6.4 (10) | 0.64 (1) | 1.92 (3) |
| 1.28 | 11.52 (9) | 1.28 (1) | 3.84 (3) |
| 2.56 | 64 (25) | 2.56 (1) | 7.68 (3) |
| NOTE 1: When SMTC < = 40 ms, M2 = M3 = M4 = 1; and when SMTC > 40 ms, M2 = 2, M3 = M4 = 2.5 |

For any requirement in this section, when the UE transitions between any two states when being configured with eDRX\_IDLE, changing eDRX\_IDLE cycle length, the UE shall meet the transition requirement, which is the less stringent requirement of the two requirements corresponding to the first state and the second state, during the transition time interval which is the time corresponding to the transition requirement. After the transition time interval, the UE shall meet the requirement corresponding to the second state.

If ‘*t-Service*’ is broadcasted and applicable, UE shall be able to detect, measure, and evaluate neighbour cells before the serving cell stops serving the area regardless of whether the distance condition based on serving cell reference location or serving cell moving reference location is met or the legacy Srxlev/Squal condition are met, and when to start the detection, measurement and evaluation on neighbour cells is up to UE implementation. This requirement does not apply when the time span from the last slot of SI transmission within SI modification period where the broadcasting of the last updated value for t-Service is acquired by the UE for the first time to the first slot when the cell is scheduled to stop serving the area according to the broadcasted information is less than Ttrigger.

 Ttrigger = max(Kmulti\_SMTC\*Tdetect,NR\_Intra, Kmulti\_SMTC\*Kcarrier\* Tdetect,NR\_Inter),

where

- Kcarrier is the number of NR inter-frequency carriers indicated by the serving cell,

- Tdetect,NR\_Intra\_RedCap refers to intra-frequency cell detection delay in IDLE/INACTIVE mode defined in tables 4.2C.2.3-1(with FR1) and 4.2E.2.3-1,

- Tdetect,NR\_Inter\_RedCap refers to inter-frequency cell detection delay in IDLE/INACTIVE mode defined in table 4.2C.2.4-1(with FR1) and 4.2E.2.4-1.

The requirements in this clause apply provided that the number of SMTCs for intra-frequency carrier does not exceed the *parallelSMTC-r17*, otherwise UE may select one or subset of all the configured SMTCs sequentially for performing the measurements until all of the SMTCs can be measured. The selection of SMTCs to be used is up to UE implementation, and in this case, measurement period longer than the corresponding measurement period specified in tables 4.2C.2.3-1 (with FR1), 4.2E.2.3-1 and table 4.2E.2.3-2 is expected.

4.2E.2.4 Measurements of inter-frequency NR cells for RedCap UE

The UE shall be able to identify new inter-frequency cells and perform SS-RSRP or SS-RSRQ measurements of identified inter-frequency cells if carrier frequency information is provided by the serving cell, even if no explicit neighbour list with physical layer cell identities is provided.

If Srxlev > SnonIntraSearchP and Squal > SnonIntraSearchQ, and the distance between UE and serving cell reference location or serving cell moving reference location is smaller than *distanceThresh* if *distanceThresh* is configured and UE has location information, then the UE shall search for inter-frequency layers of higher priority at least every Thigher\_priority\_search where Thigher\_priority\_search is described in clause 4.2E.2.9.

If Srxlev ≤ SnonIntraSearchP or Squal ≤ SnonIntraSearchQ, or the distance between UE and serving cell reference location or serving cell moving reference location is larger than *distanceThresh* if *distanceThresh* is configured and UE has location information, then the UE shall search for and measure inter-frequency layers of higher, equal or lower priority in preparation for possible reselection. The requirements apply provided that the distance exceeds the *distanceThresh* by a margin of 50 m when *referenceLocation* is configured by the network or 80 m when *movingReferenceLocation* is configured by the network. In this scenario, the minimum rate at which the UE is required to search for and measure higher priority layers shall be the same as that defined below in this clause.

The UE shall be able to evaluate whether a newly detectable inter-frequency cell meets the reselection criteria defined in TS 38.304 [1] within $K\_{carrier}\*K\_{multi\\_SMTC}\*T\_{detect,NR\_{Inter\\_RedCap}}$ if the UE does not support t *Enhanced RRM requirements for measurements in IDLE and INACTIVE modes* defined in TS 38.306 [14] or if the *enhancedMeasurementLEO-r17* is not enabled, or within $K\_{carrier}\*K\_{multi\\_SMTC}\*T\_{detect,NR\\_Inter\\_RedCap\\_enh}$ if the UE supports *Enhanced RRM requirements for measurements in IDLE and INACTIVE modes* defined in TS 38.306 [14] and the *enhancedMeasurementLEO-r17* is enabled, if at least carrier frequency information is provided for inter-frequency neighbour cells by the serving cells when Treselection = 0 provided that the reselection criteria is met:

 For 2 Rx RedCap by a margin of at least

 5 dB in FR1 for reselections based on ranking or

 6 dB in FR1 for SS-RSRP reselections based on absolute priorities or

 4 dB in FR1 for SS-RSRQ reselections based on absolute priorities

 For 1 Rx RedCap by a margin of at least

 6 dB in FR1 for reselections based on ranking or

 7 dB in FR1 for SS-RSRP reselections based on absolute priorities or

 5 dB in FR1 for SS-RSRQ reselections based on absolute priorities.

The parameter Kcarrier is the number of NR inter-frequency carriers indicated by the serving cell.

The parameter Kmulti\_SMTC is the scaling factor for measurement of multiple SMTCs or multiple satellites, which refers to clause 4.2C.2.4.

An inter-frequency cell is considered to be detectable according to the conditions defined in Annex B.1.7 for a corresponding Band.

When higher priority cells are found by the higher priority search, they shall be measured at least every Tmeasure,NR\_Inter. If, after detecting a cell in a higher priority search, it is determined that reselection has not occurred then the UE is not required to continuously measure the detected cell to evaluate the ongoing possibility of reselection. However, the minimum measurement filtering requirements specified later in this clause shall still be met by the UE before it makes any determination that it may stop measuring the cell. If the UE detects on a NR carrier a cell whose physical identity is indicated as not allowed for that carrier in the measurement control system information of the serving cell, the UE is not required to perform measurements on that cell.

The UE shall measure SS-RSRP or SS-RSRQ at least every $K\_{carrier}\*K\_{multi\\_SMTC}\*T\_{measure,NR\\_Inter\\_RedCap}$ if the UE does not support *Enhanced RRM requirements for measurements in IDLE and INACTIVE modes* defined in TS 38.306 [14] or if the *enhancedMeasurementLEO-r17* is not enabled, or every $K\_{carrier}\*K\_{multi\\_SMTC}\*T\_{measure,NR\\_Inter\\_RedCap\\_enh}$ if the UE supports *Enhanced RRM requirements for measurements in IDLE and INACTIVE modes* defined in TS 38.306 [14] and the *enhancedMeasurementLEO-r17*is enabled, for identified lower or equal priority inter-frequency cells. If the UE detects on a NR carrier a cell whose physical identity is indicated as not allowed for that carrier in the measurement control system information of the serving cell, the UE is not required to perform measurements on that cell.

The UE shall filter SS-RSRP or SS-RSRQ measurements of each measured higher, lower and equal priority inter-frequency cell using at least 2 measurements. Within the set of measurements used for the filtering, at least two measurements shall be spaced by at least Tmeasure,NR\_Inter\_RedCap/2.

The UE shall not consider a NR neighbour cell in cell reselection, if it is indicated as not allowed in the measurement control system information of the serving cell.

For an inter-frequency cell that has been already detected, but that has not been reselected to, the filtering shall be such that the UE shall be capable of evaluating that the inter-frequency cell has met reselection criterion defined TS 38.304 [1] within $K\_{carrier}\*K\_{multi\\_SMTC}\*T\_{evaluate,NR\\_Inter\\_RedCap}$ if the UE does not support *Enhanced RRM requirements for measurements in IDLE and INACTIVE modes* defined in TS 38.306 [14] or if the *enhancedMeasurementLEO-r17* is not enabled, or within $K\_{carrier}\*K\_{multi\\_SMTC}\*T\_{evaluate,NR\\_Inter\\_RedCap\\_enh }$ if the UE supports *Enhanced RRM requirements for measurements in IDLE and INACTIVE modes* defined in TS 38.306 [14] and the *enhancedMeasurementLEO-r17* is enabled, when Treselection = 0as specified in tables 4.2C.2.4-1(with FR1) and 4.2E.2.4-1 provided that the reselection criteria is met by

- the condition when performing equal priority reselection and

- when *rangeToBestCell* is not configured:

- the cell is at least 5 dB better ranked in FR1 for 2 Rx RedCap.

- the cell is at least 6 dB better ranked in FR1 for 1 Rx RedCap.

- when *rangeToBestCell* is configured:

- the cell has the highest number of beams above the threshold *absThreshSS-BlocksConsolidation* among all detected cells whose cell-ranking criterion R value defined in TS 38.304 [1] is within *rangeToBestCell* of the cell-ranking criterion R value of the highest ranked cell.

- if there are multiple such cells, the cell has the highest rank among them

- the cell is at least 5 dB better ranked in FR1 if the current serving cell is among them, or 6 dB in FR1 for SS-RSRP reselections based on absolute priorities for 2 Rx RedCap or 4 dB in FR1 for SS-RSRQ reselections based on absolute priorities for 2 Rx RedCap.

- the cell is at least 6 dB better ranked in FR1 if the current serving cell is among them, or 7 dB in FR1 for SS-RSRP reselections based on absolute priorities or 5 dB in FR1 for SS-RSRQ reselections based on absolute priorities for 1 Rx RedCap.

The 1 Rx RedCap UE applies *absThreshSS-BlocksConsolidation* as the signalled value of *absThreshSS-BlocksConsolidation* [2] + 1 dB.

When evaluating cells for reselection, the SSB side conditions apply to both serving and inter-frequency cells.

If Treselection timer has a non-zero value and the inter-frequency cell is satisfied with the reselection criteria, the UE shall evaluate this inter-frequency cell for the Treselection time. If this cell remains satisfied with the reselection criteria within this duration, then the UE shall reselect that cell.

The UE is not expected to meet the measurement requirements for an inter-frequency carrier under DRX cycle=320 ms defined in table 4.2C.2.4-1(with FR1) under the following conditions:

- TSMTC\_intra = TSMTC\_inter = 160 ms; where

- TSMTC\_intra is the periodicity of the SMTC configured for the intra-frequency carrier if no identified intra-frequency cell is in the PCI list of *smtc2-LP* on this intra-frequency carrier; TSMTC\_intra is the periodicity of the *smtc2-LP* configured for the intra-frequency carrier if at least one identified intra-frequency cell is in the PCI list of *smtc2-LP* on this intra-frequency carrier. During PSS/SSS detection, the periodicity of the SMTC configured for the intra-frequency carrier is assumed for TSMTC\_intra. If the actual SSB transmission periodicity is greater than the SMTC configured for the intra-frequency carrier, longer Tdetect, NR\_intra is expected.

- TSMTC\_inter is the actual SMTC periodicity used by the inter-frequency cell being identified. During PSS/SSS detection, the periodicity of the SMTC configured for the inter-frequency carrier is assumed for TSMTC\_inter. If the actual SSB transmission periodicity is greater than the SMTC configured for the inter-frequency carrier, longer Tdetect, NR\_inter is expected.

- SMTC occasions configured for the inter-frequency carrier occur up to 1 ms before the start or up to 1 ms after the end of the SMTC occasions configured for the intra-frequency carrier, and

- SMTC occasions configured for the intra-frequency carrier and for the inter-frequency carrier occur up to 1 ms before the start or up to 1 ms after the end of the paging occasion in TS 38.304 [1].

For 1 Rx RedCap and 2 Rx RedCap not configured with eDRX\_IDLE cycle, Tdetect,NR\_Inter\_RedCap, Tmeasure,NR\_ Inter \_RedCap and Tevaluate,NR\_ Inter \_RedCap are specified in table 4.2C.2.4-1 (with FR1).

For 1 Rx RedCap and 2 Rx RedCap configured with eDRX\_IDLE cycle, Tdetect,NR\_ Inter \_RedCap, Tmeasure,NR\_ Inter \_RedCap and Tevaluate,NR\_ Inter \_RedCap are specified in table 4.2E.2.4-1 for FR1.

For both 1Rx RedCap and 2Rx RedCap, Tdetect,NR\_Inter\_RedCap\_enh ,Tmeasure,NR\_Intra\_RedCap\_enh and Tevaluate,NR\_Intra\_RedCap\_enh refer to table 4.2E.2.4-2.

**Table 4.2E.2.4-1: Tdetect,NR\_Inter\_RedCap, Tmeasure,NR\_Inter\_RedCap and Tevaluate,NR\_Inter\_RedCap for UE configured with eDRX\_IDLE cycle (Frequency range FR1)**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **eDRX\_IDLE cycle length [s]** | **DRX cycle length [s]** | **PTW length [s] (number of 1.28 s periods)** | **Tdetect,NR\_Inter\_RedCap [s] (number of eDRX cycles)** | **Tmeasure,NR\_Inter\_RedCap [s] (number of eDRX cycles)** | **Tevaluate,NR\_Inter\_RedCap [s] (number of eDRX cycles)** |
|
| 2.56 | - | - | 58.88 (23) | 2.56 (1) | 7.68 (3) |
| 5.12 | - | - | 117.76 (23) | 5.12 (1) | 10.24 (2) |
| 10.24 | - | - | 235.52 (23) | 10.24 (1) | 20.48 (2) |
| NOTE 1: VoidNOTE 2: The eDRX\_IDLE cycle lengths are as specified in section 10.5.5.32 of TS 24.008 [42].NOTE 3: Void NOTE 4: Void |

**Table 4.2E.2.4-2: Tdetect,NR\_Inter\_RedCap\_enh, Tmeasure,NR\_Inter\_RedCap\_enh and Tevaluate,NR\_Inter\_RedCap\_enh**

|  |  |  |  |
| --- | --- | --- | --- |
| **DRX cycle length [s]** | **Tdetect,NR\_Inter\_RedCap\_enh [s] (number of DRX cycles)** | **Tmeasure,NR\_Inter\_RedCap\_enh [s] (number of DRX cycles)** | **Tevaluate,NR\_Inter\_RedCap\_enh [s] (number of DRX cycles)** |
|
| 0.32 | 3.84 x M2 (12 x M2) Note 1 | 0.32 x M3 (1 x M3) Note 1 | 0.96 x M4 (3 x M4) Note 1 |
| 0.64 | 7.68 (12) | 0.64 (1) | 1.92 (3) |
| 1.28 | 12.8 (10) | 1.28 (1) | 3.84 (3) |
| 2.56 | 64 (25) | 2.56 (1) | 7.68 (3) |
| NOTE 1: When SMTC < = 40 ms, M2 = M3 = M4 = 1; and when SMTC > 40 ms, M2 = 1.5, M3 = M4 = 2 |

If *t-Service* is broadcasted and applicable, UE shall be able to detect, measure, and evaluate neighbour cells before the serving cell stops serving the area regardless of whether the distance condition based on serving cell reference location or serving cell moving reference location or the legacy Srxlev/Squal condition are met, and when to start detection, measurement, and evaluation is up to UE implementation. This requirement does not apply when the time span from the last slot of SI transmission within SI modification period where the broadcasting of the last updated value for t-Service is acquired by the UE for the first time to the first slot when the cell is scheduled to stop serving the area according to the broadcasted information is less than Ttrigger, and Ttrigger = max(Kmulti\_SMTC\*Tdetect,NR\_Intra, Kmulti\_SMTC\*Kcarrier\* Tdetect,NR\_Inter) when serving cell is below the search threshold, and Ttrigger = max(Kmulti\_SMTC\*Tdetect,NR\_Intra, Nlayer\* 60 s) when serving cell is above the search threshold, where

- Kcarrier is the number of NR inter-frequency carriers indicated by the serving cell,

- Nlayer is the total number of higher priority NR carrier frequencies broadcasted in system information,

- Tdetect,NR\_Intra refers to enhanced intra-frequency cell detection delay in IDLE/INACTIVE mode defined table 4.2E.2.3-2,

- Tdetect,NR\_Inter refers to enhanced inter-frequency cell detection delay in IDLE/INACTIVE mode defined table 4.2E.2.4-2.

The requirements in this clause apply provided that the number of SMTCs for any inter-frequency carrier does not exceed the values indicated by *parallelSMTC-r17*, otherwise UE may select one or subset of all the configured SMTCs sequentially until all of the SMTCs can be measured, the selection of SMTCs to be used is up to UE implementation, and longer measurement delay than the corresponding measurement period specified in tables 4.2C.2.4-1 (with FR1), table 4.2E.2.4-1 and table 4.2C.2.4-2 is expected.

The requirements in this clause apply provided that the valid information for the satellite serving the target cell has been provided by the serving cell.

The requirements in this clause apply provided that SSB of neighbour cells are within the time shifted SMTC.

<End of Change 1>