**3GPP TSG-RAN WG4 Meeting #116 R4-2510480**

**Bengaluru, India, August 25th – 29th, 2025**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.3* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.101-1** | **CR** |  | **Rev** | **-** | **Current version:** | **19.2.0** |  |
|  | | | | | | | | |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Draft CR for adding some new 2DL NR-CA band combinations to TS 38.101-1 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | KDDI, Samsung | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_CADC\_SUL\_R19-Core | | | | |  | ***Date:*** | | | 2025-08-08 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-19 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)  Rel-20 (Release 20)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | To introduce specific requirements a 2-band combination in the category of Objective #2: NR\_CADC\_R19\_2BDL\_yBUL (y=1,2) for TS 38.101-1.  Relevant two-band fallback configuration has been submitted to this Meeting in TP rev\_R4-2510054 (will be updated to a new Tdoc number). Therefore, this combination can be introduced through this draft CR. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | * UL CA\_n77(2A) for DL CA\_n18A-n77(3A) is added to TS 38.101-1 Version 19.2.0 | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The above mentioned combination is not supported in the specification. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.5A.3.1 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | | **X** |  | Test specifications | | | | TS 38.521-1 | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

## **<<Start of Change>>**

#### 5.5A.3.1 Configurations for inter-band CA (Two bands)

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* Unchanged Tables/parts Omitted \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

##### Table 5.5A.3.1-1f

Table 5.5A.3.1-1f: NR CA configurations and bandwidth combinations  
sets defined for inter-band CA (two bands)

| NR CA configuration | Uplink CA configuration or single uplink carrier10 | NR Band | Channel bandwidth (MHz) (NOTE 3) | Bandwidth combination set |
| --- | --- | --- | --- | --- |
| CA\_n18A-n77A | n778  CA\_n18A-n77A8 | n18 | 5, 10, 15 | 0 |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n18 | See n18 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | See n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n18A-n77(2A) | n778  CA\_n18A-n77A8 | n18 | 5, 10, 15 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n18 | See n18 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n18A-n77(3A) | CA\_n18A-n77A8  CA\_n77(2A) | n18 | 5, 10, 15 | 0 |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n18A-n78A | CA\_n18A-n78A | n18 | 5, 10, 15 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n18 | See n18 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* Unchanged Tables/parts Omitted \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

## **<<End of Change>>**