**3GPP TSG-RAN WG4 Meeting # 116**  **R4-25xxx**

**Bengaluru, India, August 25th - 29th, 2025**

**Agenda item:** 7.26.1

**Source:** Moderator (Nokia)

**Title:** UE feature list for NR\_XR\_Ph3

**Document for:** Approval

# UE feature list for XR

#### Issue 1-5-1: UE capabilities for XR - tables

* Proposals
  + Option 1 (vivo):

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 57.NR\_XR\_Ph3 | 53-1 | Recommended ratio of gap occasions for cancelation | Indicates the UE is capable of reporting recommended ratio of measurement gap occasions for cancelation | 64-1 | Yes | N/A | The UE does not support reporting recommended ratio for gap cancelation | Per UE | no | no |  |  | Optional with capability signalling |

* Recommended WF
  + Tentative agreement on Option 1
* Agreement

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 53.NR\_XR\_Ph3 | 53-1 | Recommended ratio of gap occasions for cancelation | Indicates the UE is capable of reporting recommended ratio of measurement gap occasions for cancelation | 64-1 | Yes | N/A | The UE does not support reporting recommended ratio for gap cancelation | Per UE | no | no |  |  | Optional with capability signalling |