**3GPP TSG-SA3 Meeting #124 S3-253570r1**

Wuhan, China, 14 – 18 October 2025 merger of 570 and 601

**Source: China Mobile, Vodafone, AT&T, T-Mobile US, Verizon, Charter Communication, KDDI, Telecom Italia, China Telecom**

**Title: proposal to introduce security related events - replay attack**

**Document for: Approval**

**Agenda item: 5.1.1**

**Spec: 3GPP TS 33.502**

**Version: 0.1.0**

**Work Item: SECHAND**

**Comments**

It proposes template to specify details security related events .

\* \* \* First Change \* \* \* \*

# 6 Security related Events

Editor’s Note: This clause addresses the list and description of the events as well as naming convention for the events.

6.x Security related events

6.x.y Replay attacks

* *Description:* NF collects information when any NF detects replay requests/responses.
* The information elements for this type shall consist following:
* Content: { replayed messages, source NF ID and FQDN when available}

\* \* \* End of Changes \* \* \* \*