**3GPP TSG-SA3 Meeting #124 S3-253795r2**

Wuhan, China, 14 – 18 October 2025 merger of 569, 589, 6.z of 580 and 2 in 623

**Source: China Mobile, Vodafone, AT&T, T-Mobile US, Verizon, Charter Communication, KDDI, Telecom Italia, China Telecom, Samsung?, Ericsson?, IIT Bombay?, Nokia?**

**Title: proposal to introduce security related events - failed authorization**

**Document for: Approval**

**Agenda item: 5.1.1**

**Spec: 3GPP TS 33.502**

**Version: 0.1.0**

**Work Item: SECHAND**

**Comments**

It proposes template to specify details security related events .

\* \* \* First Change \* \* \* \*

# 6 Security related Events

Editor’s Note: This clause addresses the list and description of the events as well as naming convention for the events.

6.x Security events related to Authorization Failure

*Description:* The NF collects information about failed authorization attempts from inbound connections on the SBA layer.

The information elements for this type shall consist following:

* Message: Full message which fails to pass authorization
* NF consumer name: NF instance ID where unauthorized message comes from.

\* \* \* End of Changes \* \* \* \*